Product ID=2c, Serial#=TV109091204, SWVersion=(See Log Data), HWVersion=(See Log Data)
-------------------------------------------------------------
LOG ID 17 (Encrypted Significant Event Text) 7474 total bytes
-------------------------------------------------------------
     UTC Time             Tril Time          Err              Descr
07/24/2012 10:55:54  07/24/2012 07:04:54 E-00107     0 65535  ERR_SPEAKER_2_FAILURE  URGENT_SERVICE  <UTC:1343127354_00>
07/24/2012 10:55:53  07/24/2012 07:04:53 E-00264     0 65535  ERR_MENU_BYPASS_ACTIVATED  KEYPRESS  <UTC:1343127353_00>
07/24/2012 10:55:48  07/24/2012 07:04:48 E-16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1343127348_00>
07/24/2012 10:55:48  07/24/2012 07:04:48 E-00294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1343127348_00>
07/24/2012 10:55:47  07/24/2012 07:04:47 E-00293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1343127347_00>
07/24/2012 10:55:45  07/24/2012 07:04:45 E-00072     0 65535  ERR_MMC_SD_CARD_INSERTED  BEEP_ONLY  <UTC:1343127345_00>
07/24/2012 10:53:03  07/24/2012 07:02:03 E-00197     0 65535  ERR_INT_LI_ION_NOT_PRESENT  URGENT_SERVICE  <UTC:1343127183_00>
07/24/2012 10:52:52  07/24/2012 07:01:52 E-00195     0 65535  ERR_BATT_LOW_STATE_OF_HEALTH_INT_LI_ION  URGENT_SERVICE  <UTC:1343127172_00>
07/24/2012 10:52:50  07/24/2012 07:01:50 E-00166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1343127170_00>
07/24/2012 10:52:44  07/24/2012 07:01:44 E-00290   195 65535  ERR_URGENT_REMINDER  URGENT_SERVICE  <UTC:1343127164_00>
07/24/2012 10:52:44  07/24/2012 07:01:44 E-00185     0 65535  ERR_LAST_BATT_INT_LI_ION_LOW  MED_ALARM  <UTC:1343127164_00>
07/24/2012 10:52:42  07/24/2012 07:01:42 E-00196     0 65535  ERR_BATT_LOW_STATE_OF_HEALTH_DET_LI_ION  LOW_ALARM  <UTC:1343127162_00>
07/24/2012 10:52:41  07/24/2012 07:01:41 E-00195     0 65535  ERR_BATT_LOW_STATE_OF_HEALTH_INT_LI_ION  URGENT_SERVICE  <UTC:1343127161_00>
07/24/2012 10:52:40  07/24/2012 07:01:40 E-16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1343127160_00>
07/24/2012 10:52:40  07/24/2012 07:01:40 E-00324     3 65535  ERR_POWER_ON  KEYPRESS  <UTC:1343127160_00>
07/24/2012 10:52:39  07/24/2012 07:01:39 E-00252     0 65535  ERR_INT_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1343127159_00>
07/24/2012 10:52:39  07/24/2012 07:01:39 E-00251     0 65535  ERR_DET_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1343127159_00>
07/23/2012 22:58:27  07/23/2012 19:07:27 E-16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1343084307_00>
07/23/2012 22:50:26  07/23/2012 18:59:26 E-00290   106  3600  ERR_URGENT_REMINDER  URGENT_SERVICE  <UTC:1343083826_00>
07/23/2012 22:44:29  07/23/2012 18:53:29 E-00188     0 65535  ERR_LAST_BATT_INT_LI_ION_NEARLY_DEPLETED  HIGH_ALARM  <UTC:1343083469_00>
07/23/2012 22:37:24  07/23/2012 18:46:24 E-00185     0 65535  ERR_LAST_BATT_INT_LI_ION_LOW  MED_ALARM  <UTC:1343083044_00>
07/23/2012 22:29:37  07/23/2012 18:38:37 E-00281     0 65535  ERR_PWR_REDUCTION_DET_LI_ION_DEPLETED  INFO_ALARM  <UTC:1343082577_00>
07/23/2012 22:29:17  07/23/2012 18:38:17 E-00286     0 65535  ERR_PWR_UPGRADE_DET_LI_ION_IN_USE  BEEP_ONLY  <UTC:1343082557_00>
07/23/2012 22:08:33  07/23/2012 18:17:33 E-00281     0 65535  ERR_PWR_REDUCTION_DET_LI_ION_DEPLETED  INFO_ALARM  <UTC:1343081313_00>
07/23/2012 22:08:14  07/23/2012 18:17:14 E-00286     0 65535  ERR_PWR_UPGRADE_DET_LI_ION_IN_USE  BEEP_ONLY  <UTC:1343081294_00>
07/23/2012 22:02:08  07/23/2012 18:11:08 E-00195     0 65535  ERR_BATT_LOW_STATE_OF_HEALTH_INT_LI_ION  URGENT_SERVICE  <UTC:1343080928_00>
07/23/2012 21:53:03  07/23/2012 18:02:03 E-00281     0 65535  ERR_PWR_REDUCTION_DET_LI_ION_DEPLETED  INFO_ALARM  <UTC:1343080383_00>
07/23/2012 21:52:42  07/23/2012 18:01:42 E-00286     0 65535  ERR_PWR_UPGRADE_DET_LI_ION_IN_USE  BEEP_ONLY  <UTC:1343080362_00>
07/23/2012 21:50:26  07/23/2012 17:59:26 E-00290   106  3600  ERR_URGENT_REMINDER  URGENT_SERVICE  <UTC:1343080226_00>
07/23/2012 21:42:01  07/23/2012 17:51:01 E-00281     0 65535  ERR_PWR_REDUCTION_DET_LI_ION_DEPLETED  INFO_ALARM  <UTC:1343079721_00>
07/23/2012 21:41:42  07/23/2012 17:50:42 E-00286     0 65535  ERR_PWR_UPGRADE_DET_LI_ION_IN_USE  BEEP_ONLY  <UTC:1343079702_00>
07/23/2012 21:34:45  07/23/2012 17:43:45 E-00281     0 65535  ERR_PWR_REDUCTION_DET_LI_ION_DEPLETED  INFO_ALARM  <UTC:1343079285_00>
07/23/2012 21:34:23  07/23/2012 17:43:23 E-00286     0 65535  ERR_PWR_UPGRADE_DET_LI_ION_IN_USE  BEEP_ONLY  <UTC:1343079263_00>
07/23/2012 21:31:02  07/23/2012 17:40:02 E-00281     0 65535  ERR_PWR_REDUCTION_DET_LI_ION_DEPLETED  INFO_ALARM  <UTC:1343079062_00>
07/23/2012 20:50:26  07/23/2012 16:59:26 E-00290   106  3600  ERR_URGENT_REMINDER  URGENT_SERVICE  <UTC:1343076626_00>
07/23/2012 20:01:07  07/23/2012 16:10:07 E-00195     0 65535  ERR_BATT_LOW_STATE_OF_HEALTH_INT_LI_ION  URGENT_SERVICE  <UTC:1343073667_00>
07/23/2012 20:01:06  07/23/2012 16:10:06 E-00166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1343073666_00>
07/23/2012 20:01:04  07/23/2012 16:10:04 E-00179     0 65535  ERR_PWR_REDUCTION_AC_DISCONNECTED  MED_ALARM  <UTC:1343073664_00>
07/23/2012 20:01:00  07/23/2012 16:10:00 E-00195     0 65535  ERR_BATT_LOW_STATE_OF_HEALTH_INT_LI_ION  URGENT_SERVICE  <UTC:1343073660_00>
07/23/2012 20:00:58  07/23/2012 16:09:58 E-00166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1343073658_00>
07/23/2012 19:50:45  07/23/2012 15:59:45 E-00196     0 65535  ERR_BATT_LOW_STATE_OF_HEALTH_DET_LI_ION  LOW_ALARM  <UTC:1343073045_00>
07/23/2012 19:50:26  07/23/2012 15:59:26 E-00290   106  3600  ERR_URGENT_REMINDER  URGENT_SERVICE  <UTC:1343073026_00>
07/23/2012 18:50:45  07/23/2012 14:59:45 E-00196     0 65535  ERR_BATT_LOW_STATE_OF_HEALTH_DET_LI_ION  LOW_ALARM  <UTC:1343069445_00>
07/23/2012 18:50:26  07/23/2012 14:59:26 E-00290   106  3600  ERR_URGENT_REMINDER  URGENT_SERVICE  <UTC:1343069426_00>
07/23/2012 17:50:45  07/23/2012 13:59:45 E-00196     0 65535  ERR_BATT_LOW_STATE_OF_HEALTH_DET_LI_ION  LOW_ALARM  <UTC:1343065845_00>
07/23/2012 17:50:26  07/23/2012 13:59:26 E-00290   106  3600  ERR_URGENT_REMINDER  URGENT_SERVICE  <UTC:1343065826_00>
07/23/2012 16:50:46  07/23/2012 12:59:46 E-00195     0 65535  ERR_BATT_LOW_STATE_OF_HEALTH_INT_LI_ION  URGENT_SERVICE  <UTC:1343062246_00>
07/23/2012 16:50:45  07/23/2012 12:59:45 E-00166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1343062245_00>
07/23/2012 16:50:26  07/23/2012 12:59:26 E-00290   106  3600  ERR_URGENT_REMINDER  URGENT_SERVICE  <UTC:1343062226_00>
07/23/2012 16:46:14  07/23/2012 12:55:14 E-00195     0 65535  ERR_BATT_LOW_STATE_OF_HEALTH_INT_LI_ION  URGENT_SERVICE  <UTC:1343061974_00>
07/23/2012 16:46:12  07/23/2012 12:55:12 E-00166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1343061972_00>
07/23/2012 16:46:10  07/23/2012 12:55:10 E-00196     0 65535  ERR_BATT_LOW_STATE_OF_HEALTH_DET_LI_ION  LOW_ALARM  <UTC:1343061970_00>
07/23/2012 16:46:08  07/23/2012 12:55:08 E-00251     0 65535  ERR_DET_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1343061968_00>
07/23/2012 16:46:07  07/23/2012 12:55:07 E-00195     0 65535  ERR_BATT_LOW_STATE_OF_HEALTH_INT_LI_ION  URGENT_SERVICE  <UTC:1343061967_00>
07/23/2012 16:45:58  07/23/2012 12:54:58 E-00195     0 65535  ERR_BATT_LOW_STATE_OF_HEALTH_INT_LI_ION  URGENT_SERVICE  <UTC:1343061958_00>
07/23/2012 16:45:56  07/23/2012 12:54:56 E-00166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1343061956_00>
07/23/2012 16:45:54  07/23/2012 12:54:54 E-00174     0 65535  ERR_LOSS_OF_COMM_CHARGER  URGENT_SERVICE  <UTC:1343061954_00>
07/23/2012 16:45:54  07/23/2012 12:54:54 E-00282     0 65535  ERR_INT_LI_ION_DEPLETED  HIGH_ALARM  <UTC:1343061954_00>
07/23/2012 16:42:50  07/23/2012 12:51:50 E-00195     0 65535  ERR_BATT_LOW_STATE_OF_HEALTH_INT_LI_ION  URGENT_SERVICE  <UTC:1343061770_00>
07/23/2012 16:42:48  07/23/2012 12:51:48 E-00166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1343061768_00>
07/23/2012 16:42:46  07/23/2012 12:51:46 E-00196     0 65535  ERR_BATT_LOW_STATE_OF_HEALTH_DET_LI_ION  LOW_ALARM  <UTC:1343061766_00>
07/23/2012 16:42:44  07/23/2012 12:51:44 E-00251     0 65535  ERR_DET_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1343061764_00>
07/23/2012 16:42:38  07/23/2012 12:51:38 E-00195     0 65535  ERR_BATT_LOW_STATE_OF_HEALTH_INT_LI_ION  URGENT_SERVICE  <UTC:1343061758_00>
07/23/2012 16:42:33  07/23/2012 12:51:33 E-00284     0 65535  ERR_PWR_UPGRADE_AC_IN_USE  BEEP_ONLY  <UTC:1343061753_00>
07/23/2012 16:31:14  07/23/2012 12:40:14 E-00195     0 65535  ERR_BATT_LOW_STATE_OF_HEALTH_INT_LI_ION  URGENT_SERVICE  <UTC:1343061074_00>
07/23/2012 16:31:12  07/23/2012 12:40:12 E-00166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1343061072_00>
07/23/2012 16:31:11  07/23/2012 12:40:11 E-00281     0 65535  ERR_PWR_REDUCTION_DET_LI_ION_DEPLETED  INFO_ALARM  <UTC:1343061071_00>
07/23/2012 16:31:10  07/23/2012 12:40:10 E-00196     0 65535  ERR_BATT_LOW_STATE_OF_HEALTH_DET_LI_ION  LOW_ALARM  <UTC:1343061070_00>
07/23/2012 16:31:10  07/23/2012 12:40:10 E-00179     0 65535  ERR_PWR_REDUCTION_AC_DISCONNECTED  MED_ALARM  <UTC:1343061070_00>
07/23/2012 16:30:58  07/23/2012 12:39:58 E-00195     0 65535  ERR_BATT_LOW_STATE_OF_HEALTH_INT_LI_ION  URGENT_SERVICE  <UTC:1343061058_00>
07/23/2012 16:30:55  07/23/2012 12:39:55 E-00252     0 65535  ERR_INT_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1343061055_00>
07/23/2012 16:30:49  07/23/2012 12:39:49 E-00197     0 65535  ERR_INT_LI_ION_NOT_PRESENT  URGENT_SERVICE  <UTC:1343061049_00>
07/23/2012 16:30:46  07/23/2012 12:39:46 E-00251     0 65535  ERR_DET_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1343061046_00>
07/23/2012 15:51:09  07/23/2012 12:00:09 E-00284     0 65535  ERR_PWR_UPGRADE_AC_IN_USE  BEEP_ONLY  <UTC:1343058669_00>
07/23/2012 15:51:04  07/23/2012 12:00:04 E-00286     0 65535  ERR_PWR_UPGRADE_DET_LI_ION_IN_USE  BEEP_ONLY  <UTC:1343058664_00>
07/23/2012 15:51:03  07/23/2012 12:00:03 E-00251     0 65535  ERR_DET_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1343058663_00>
07/23/2012 15:50:58  07/23/2012 11:59:58 E-00166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1343058658_00>
07/23/2012 15:50:56  07/23/2012 11:59:56 E-00181     0 65535  ERR_PWR_REDUCTION_DET_LI_ION_DISCONNECTED  INFO_ALARM  <UTC:1343058656_00>
07/23/2012 15:50:56  07/23/2012 11:59:56 E-00166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1343058656_00>
07/23/2012 15:50:54  07/23/2012 11:59:54 E-00179     0 65535  ERR_PWR_REDUCTION_AC_DISCONNECTED  MED_ALARM  <UTC:1343058654_00>
07/23/2012 15:50:48  07/23/2012 11:59:48 E-00251     0 65535  ERR_DET_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1343058648_00>
07/23/2012 15:50:42  07/23/2012 11:59:42 E-00284     0 65535  ERR_PWR_UPGRADE_AC_IN_USE  BEEP_ONLY  <UTC:1343058642_00>
07/23/2012 15:50:42  07/23/2012 11:59:42 E-00166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1343058642_00>
07/23/2012 15:50:38  07/23/2012 11:59:38 E-00181     0 65535  ERR_PWR_REDUCTION_DET_LI_ION_DISCONNECTED  INFO_ALARM  <UTC:1343058638_00>
07/23/2012 15:50:32  07/23/2012 11:59:32 E-00166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1343058632_00>
07/23/2012 15:50:31  07/23/2012 11:59:31 E-00179     0 65535  ERR_PWR_REDUCTION_AC_DISCONNECTED  MED_ALARM  <UTC:1343058631_00>
07/23/2012 15:50:29  07/23/2012 11:59:29 E-00166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1343058629_00>
07/23/2012 15:50:26  07/23/2012 11:59:26 E-00290   106  3600  ERR_URGENT_REMINDER  URGENT_SERVICE  <UTC:1343058626_00>
07/23/2012 15:50:23  07/23/2012 11:59:23 E-00107     0 65535  ERR_SPEAKER_2_FAILURE  URGENT_SERVICE  <UTC:1343058623_00>
07/23/2012 15:50:23  07/23/2012 11:59:23 E-00106     0 65535  ERR_SPEAKER_1_FAILURE  URGENT_SERVICE  <UTC:1343058623_00>
07/23/2012 15:50:23  07/23/2012 11:59:23 E-16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1343058623_00>
07/23/2012 15:50:23  07/23/2012 11:59:23 E-00324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1343058623_00>
07/23/2012 15:50:21  07/23/2012 11:59:21 E-16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1343058621_00>
07/23/2012 15:50:21  07/23/2012 11:59:21 E-00294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1343058621_00>
07/23/2012 15:50:21  07/23/2012 11:59:21 E-00293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1343058621_00>
07/23/2012 15:42:08  07/23/2012 11:51:08 E-00290   106  3600  ERR_URGENT_REMINDER  URGENT_SERVICE  <UTC:1343058128_00>
07/23/2012 15:42:06  07/23/2012 11:51:06 E-00107     0 65535  ERR_SPEAKER_2_FAILURE  URGENT_SERVICE  <UTC:1343058126_00>
07/23/2012 15:42:06  07/23/2012 11:51:06 E-00290   106  3600  ERR_URGENT_REMINDER  URGENT_SERVICE  <UTC:1343058126_00>
07/23/2012 15:42:06  07/23/2012 11:51:06 E-00106     0 65535  ERR_SPEAKER_1_FAILURE  URGENT_SERVICE  <UTC:1343058126_00>
07/23/2012 15:42:05  07/23/2012 11:51:05 E-16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1343058125_00>
07/23/2012 15:42:05  07/23/2012 11:51:05 E-00324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1343058125_00>

--------------------------------------------------------------
LOG ID 18 (Encrypted Engineering Debug Text) 80464 total bytes
--------------------------------------------------------------
     UTC Time           Err Descr
07/23/2012 13:06:48 E-00096  ERR_CALIBRATION_CONTROL  LOG_ONLY  <UTC:1343048808_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2929 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=99 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=EXIT
07/23/2012 15:42:06 E-00106  ERR_SPEAKER_1_FAILURE  URGENT_SERVICE  <UTC:1343058126_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2927 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=54 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Speaker On    Note:2638 Alarm:16 Volume: 1 VPwrFail: 4680
07/23/2012 15:42:06 E-00107  ERR_SPEAKER_2_FAILURE  URGENT_SERVICE  <UTC:1343058126_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2927 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=54 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Speaker On  Note:2638 Alarm:16 Volume: 1 VPwrFail: 4727
07/23/2012 15:42:07 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343058127_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2927 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=54 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1625262
07/23/2012 15:42:15 E-00108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1343058135_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2927 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=CP:348  
07/23/2012 15:45:41 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343058341_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2926 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=4
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 15:45:54 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343058354_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2926 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1270
07/23/2012 15:50:23 E-00106  ERR_SPEAKER_1_FAILURE  URGENT_SERVICE  <UTC:1343058623_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2926 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Speaker On    Note:2638 Alarm:16 Volume: 1 VPwrFail: 4664
07/23/2012 15:50:23 E-00107  ERR_SPEAKER_2_FAILURE  URGENT_SERVICE  <UTC:1343058623_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2926 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Speaker On  Note:2638 Alarm:16 Volume: 1 VPwrFail: 4680
07/23/2012 15:50:24 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343058624_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2926 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 15:50:24 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343058624_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2926 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1
07/23/2012 15:50:30 E-00108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1343058630_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2926 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=CP:345  
07/23/2012 15:50:38 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343058638_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2926 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=00 Capacity(LA=0 IntLi=100 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=DET removed
07/23/2012 15:50:41 E-00249  ERR_AC_CONNECTED  LOG_ONLY  <UTC:1343058641_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2926 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=80 Capacity(LA=0 IntLi=100 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=
07/23/2012 15:50:57 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343058657_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2926 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=00 Capacity(LA=0 IntLi=100 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=5
                         Reserved(Offset=52)=00
                         Opt.Text=DET removed
07/23/2012 15:51:08 E-00249  ERR_AC_CONNECTED  LOG_ONLY  <UTC:1343058668_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2926 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=5
                         Reserved(Offset=52)=00
                         Opt.Text=
07/23/2012 15:51:51 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343058711_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2926 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 15:51:57 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343058717_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2926 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 646
07/23/2012 15:52:38 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343058758_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2926 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 15:53:10 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343058790_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2926 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 3228
07/23/2012 15:55:14 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343058914_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2927 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 15:55:25 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343058925_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2927 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1049
07/23/2012 15:57:02 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343059022_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2927 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=4
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 15:57:06 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343059026_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2927 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 354
07/23/2012 16:00:17 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343059217_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2926 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=5
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 16:01:08 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343059268_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2926 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 5092
07/23/2012 16:01:08 E-00108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1343059268_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2926 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=CP:343  
07/23/2012 16:03:18 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343059398_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2926 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 16:03:25 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343059405_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2926 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 785
07/23/2012 16:08:25 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343059705_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2926 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=4
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 16:08:52 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343059732_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2926 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2726
07/23/2012 16:09:33 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343059773_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2926 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 16:09:57 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343059797_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2926 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=1
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2465
07/23/2012 16:10:38 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343059838_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2926 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=1
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 16:10:46 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343059846_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2926 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=1
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 877
07/23/2012 16:11:21 E-00108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1343059881_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2926 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=CP:349  
07/23/2012 16:12:00 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343059920_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2926 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 16:12:03 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343059923_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2926 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 262
07/23/2012 16:12:43 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343059963_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2926 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 16:12:58 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343059978_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2926 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1465
07/23/2012 16:16:57 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343060217_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2926 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=4
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 16:17:03 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343060223_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2926 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 603
07/23/2012 16:21:11 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343060471_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2926 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 16:21:19 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343060479_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2926 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 772
07/23/2012 16:21:31 E-00108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1343060491_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2926 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=CP:350  
07/23/2012 16:27:12 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343060832_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2926 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 16:27:28 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343060848_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2926 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1633
07/23/2012 16:30:09 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343061009_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=5
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 16:30:18 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343061018_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 882
07/23/2012 16:30:42 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343061042_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=80 Capacity(LA=0 IntLi=100 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=DET removed
07/23/2012 16:30:48 E-00335  ERR_RE_SEALED_DET_LI_ION  LOG_ONLY  <UTC:1343061048_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=30) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=OpStatus=0x8403
07/23/2012 16:30:58 E-00195  ERR_BATT_LOW_STATE_OF_HEALTH_INT_LI_ION  URGENT_SERVICE  <UTC:1343061058_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=30) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=SOH=48 FCC=1985 RemCap=1985 Cycle=226 SN=2C01
07/23/2012 16:30:58 E-00334  ERR_RE_SEALED_INT_LI_ION  LOG_ONLY  <UTC:1343061058_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=30) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=OpStatus=0x8443
07/23/2012 16:31:10 E-00196  ERR_BATT_LOW_STATE_OF_HEALTH_DET_LI_ION  LOW_ALARM  <UTC:1343061070_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=SOH=46 FCC=1828 RemCap=0 Cycle=287 SN=101397
07/23/2012 16:31:10 E-00221  ERR_TDA_RSC_LOW_DET_LI_ION  LOG_ONLY  <UTC:1343061070_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=V0=16419 V1=13997 V2=80 FCC0=1985 FCC1=1828 SN0=2C01 SN1=101397 Cyc0=226 C
07/23/2012 16:31:11 E-00281  ERR_PWR_REDUCTION_DET_LI_ION_DEPLETED  INFO_ALARM  <UTC:1343061071_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=V0=16419 V1=13997 V2=40 FCC0=1985 FCC1=1828 RM0=1985 RM1=0 SN0=2C01 SN1=10
07/23/2012 16:31:14 E-00195  ERR_BATT_LOW_STATE_OF_HEALTH_INT_LI_ION  URGENT_SERVICE  <UTC:1343061074_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=SOH=49 FCC=2011 RemCap=2011 Cycle=226 SN=2C01
07/23/2012 16:31:49 E-00108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1343061109_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=4
                         Reserved(Offset=52)=00
                         Opt.Text=CP:349  
07/23/2012 16:36:26 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343061386_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=98 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 16:36:33 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343061393_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=98 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 722
07/23/2012 16:37:43 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343061463_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2926 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=4
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 16:38:13 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343061493_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2926 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=96 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 3010
07/23/2012 16:39:31 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343061571_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=95 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 16:39:33 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343061573_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2926 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=95 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 148
07/23/2012 16:40:43 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343061643_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=94 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 16:41:09 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343061669_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=92 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2608
07/23/2012 16:42:20 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343061740_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=91 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 16:42:25 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343061745_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=91 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 411
07/23/2012 16:42:25 E-00108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1343061745_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=91 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=CP:350  
07/23/2012 16:42:33 E-00249  ERR_AC_CONNECTED  LOG_ONLY  <UTC:1343061753_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=91 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=
07/23/2012 16:42:36 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343061756_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=80 Capacity(LA=0 IntLi=91 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=DET removed
07/23/2012 16:42:38 E-00195  ERR_BATT_LOW_STATE_OF_HEALTH_INT_LI_ION  URGENT_SERVICE  <UTC:1343061758_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=80 Capacity(LA=0 IntLi=91 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=SOH=44 FCC=1798 RemCap=1622 Cycle=226 SN=2C01
07/23/2012 16:42:46 E-00196  ERR_BATT_LOW_STATE_OF_HEALTH_DET_LI_ION  LOW_ALARM  <UTC:1343061766_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=91 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=SOH=46 FCC=1828 RemCap=0 Cycle=287 SN=109397
07/23/2012 16:42:47 E-00221  ERR_TDA_RSC_LOW_DET_LI_ION  LOG_ONLY  <UTC:1343061767_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=91 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=V0=16111 V1=14609 V2=80 FCC0=1798 FCC1=1828 SN0=2C01 SN1=101397 Cyc0=226 C
07/23/2012 16:42:50 E-00195  ERR_BATT_LOW_STATE_OF_HEALTH_INT_LI_ION  URGENT_SERVICE  <UTC:1343061770_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=91 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=SOH=44 FCC=1798 RemCap=1622 Cycle=226 SN=2C01
07/23/2012 16:43:49 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343061829_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=91 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 16:44:09 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343061849_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=91 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1977
07/23/2012 16:44:49 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343061889_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=91 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 16:44:51 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343061891_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=91 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 162
07/23/2012 16:45:54 E-00282  ERR_INT_LI_ION_DEPLETED  HIGH_ALARM  <UTC:1343061954_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=91 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Src=3 V0=16147 V1=14981 V2=120 FCC0=1798 FCC1=1828 RM0=1622 RM1=0 SN0=2C01
07/23/2012 16:45:57 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343061957_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=91 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 16:45:58 E-00195  ERR_BATT_LOW_STATE_OF_HEALTH_INT_LI_ION  URGENT_SERVICE  <UTC:1343061958_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=91 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=SOH=44 FCC=1798 RemCap=1622 Cycle=226 SN=2C01
07/23/2012 16:46:05 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343061965_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=80 Capacity(LA=0 IntLi=91 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=DET removed
07/23/2012 16:46:07 E-00195  ERR_BATT_LOW_STATE_OF_HEALTH_INT_LI_ION  URGENT_SERVICE  <UTC:1343061967_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=80 Capacity(LA=0 IntLi=91 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=SOH=44 FCC=1798 RemCap=1622 Cycle=226 SN=2C01
07/23/2012 16:46:10 E-00196  ERR_BATT_LOW_STATE_OF_HEALTH_DET_LI_ION  LOW_ALARM  <UTC:1343061970_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=91 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=SOH=46 FCC=1828 RemCap=0 Cycle=287 SN=101397
07/23/2012 16:46:10 E-00221  ERR_TDA_RSC_LOW_DET_LI_ION  LOG_ONLY  <UTC:1343061970_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=91 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=V0=16150 V1=14763 V2=120 FCC0=1798 FCC1=1828 SN0=2C01 SN1=101397 Cyc0=226 
07/23/2012 16:46:14 E-00195  ERR_BATT_LOW_STATE_OF_HEALTH_INT_LI_ION  URGENT_SERVICE  <UTC:1343061974_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=91 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=SOH=44 FCC=1798 RemCap=1622 Cycle=226 SN=2C01
07/23/2012 16:46:26 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343061986_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=91 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2912
07/23/2012 16:47:43 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343062063_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=91 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=5
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 16:48:04 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343062084_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=91 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2193
07/23/2012 16:48:45 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343062125_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=91 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=1
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 16:48:55 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343062135_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=91 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=1
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1046
07/23/2012 16:50:16 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343062216_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=91 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=4
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 16:50:46 E-00195  ERR_BATT_LOW_STATE_OF_HEALTH_INT_LI_ION  URGENT_SERVICE  <UTC:1343062246_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=91 DetLi=1) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=SOH=44 FCC=1798 RemCap=1622 Cycle=226 SN=2C01
07/23/2012 16:51:08 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343062268_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=91 DetLi=2) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 5195
07/23/2012 16:55:34 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343062534_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=91 DetLi=10) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 16:55:38 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343062538_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=91 DetLi=10) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 480
07/23/2012 16:57:02 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343062622_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=91 DetLi=13) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 16:57:04 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343062624_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=91 DetLi=13) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 195
07/23/2012 17:00:11 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343062811_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=91 DetLi=18) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 17:00:26 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343062826_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=91 DetLi=19) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1477
07/23/2012 17:01:57 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343062917_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=91 DetLi=22) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 17:01:58 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343062918_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=91 DetLi=22) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 158
07/23/2012 17:05:25 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343063125_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=91 DetLi=28) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 17:05:59 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343063159_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=91 DetLi=29) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 3451
07/23/2012 17:07:01 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343063221_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=91 DetLi=31) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=4
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 17:07:09 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343063229_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=91 DetLi=31) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 830
07/23/2012 17:11:56 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343063516_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=91 DetLi=40) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 17:12:10 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343063530_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=91 DetLi=40) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1409
07/23/2012 17:14:05 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343063645_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=91 DetLi=44) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=5
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 17:14:09 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343063649_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=91 DetLi=44) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 374
07/23/2012 17:15:33 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343063733_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=91 DetLi=46) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 17:16:03 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343063763_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=91 DetLi=47) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 3006
07/23/2012 17:18:34 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343063914_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=91 DetLi=52) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=4
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 17:18:51 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343063931_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=91 DetLi=52) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1728
07/23/2012 17:19:48 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343063988_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=91 DetLi=54) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 17:20:02 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343064002_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=91 DetLi=55) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1395
07/23/2012 17:20:42 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343064042_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=91 DetLi=56) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 17:20:54 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343064054_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=91 DetLi=56) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=1
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1118
07/23/2012 17:23:00 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343064180_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=91 DetLi=60) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 17:23:26 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343064206_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=91 DetLi=61) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2571
07/23/2012 17:26:43 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343064403_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=91 DetLi=66) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 17:26:55 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343064415_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=91 DetLi=67) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1123
07/23/2012 17:27:35 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343064455_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=92 DetLi=68) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 17:28:06 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343064486_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=92 DetLi=68) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 3090
07/23/2012 17:29:06 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343064546_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=92 DetLi=70) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 17:29:09 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343064549_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=92 DetLi=70) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 319
07/23/2012 17:30:00 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343064600_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2924 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=92 DetLi=71) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 17:30:15 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343064615_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2925 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=92 DetLi=72) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1493
07/23/2012 17:33:13 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343064793_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2924 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=94 DetLi=76) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 17:33:38 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343064818_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2924 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=94 DetLi=76) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2544
07/23/2012 17:36:25 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343064985_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2924 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=80) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=4
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 17:36:33 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343064993_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2924 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=80) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 843
07/23/2012 17:38:47 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343065127_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2924 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=97 DetLi=83) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 17:39:00 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343065140_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2924 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=97 DetLi=83) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1269
07/23/2012 17:42:34 E-00108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1343065354_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2924 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=98 DetLi=86) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=5
                         Reserved(Offset=52)=00
                         Opt.Text=CP:355  
07/23/2012 17:45:01 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343065501_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2924 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=99 DetLi=88) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=4
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 17:45:21 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343065521_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2924 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=99 DetLi=89) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2044
07/23/2012 17:46:01 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343065561_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2924 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=99 DetLi=89) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=1
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 17:46:21 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343065581_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2924 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=99 DetLi=89) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=1
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1954
07/23/2012 17:47:52 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343065672_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2924 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=90) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 17:48:04 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343065684_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2924 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=90) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1149
07/23/2012 17:50:32 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343065832_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2924 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=92) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=6
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 17:50:45 E-00196  ERR_BATT_LOW_STATE_OF_HEALTH_DET_LI_ION  LOW_ALARM  <UTC:1343065845_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2924 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=92) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=4
                         Reserved(Offset=52)=00
                         Opt.Text=SOH=46 FCC=1828 RemCap=1669 Cycle=287 SN=101397
07/23/2012 17:51:08 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343065868_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2924 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=92) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 3576
07/23/2012 17:56:19 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343066179_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2923 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=94) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=4
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 17:57:03 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343066223_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2923 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=94) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 4386
07/23/2012 17:57:43 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343066263_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2923 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=95) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 17:58:08 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343066288_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2923 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=95) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=1
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2487
07/23/2012 18:01:43 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343066503_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2923 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=96) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 18:01:54 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343066514_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2923 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=96) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1145
07/23/2012 18:02:35 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343066555_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2923 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=96) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 18:02:57 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343066577_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2923 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=96) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=1
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2196
07/23/2012 18:03:51 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343066631_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2923 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=96) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 18:03:51 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343066631_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2923 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=96) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 32
07/23/2012 18:04:32 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343066672_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2923 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=97) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 18:04:33 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343066673_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2923 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=97) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 180
07/23/2012 18:08:21 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343066901_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2923 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=4
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 18:08:33 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343066913_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2923 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1284
07/23/2012 18:11:46 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343067106_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2923 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=4
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 18:11:53 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343067113_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2923 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 714
07/23/2012 18:14:28 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343067268_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2923 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=4
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 18:15:16 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343067316_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2923 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 4842
07/23/2012 18:15:57 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343067357_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2923 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 18:16:02 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343067362_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2923 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 532
07/23/2012 18:17:04 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343067424_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2923 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 18:17:48 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343067468_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2923 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 4409
07/23/2012 18:19:28 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343067568_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2922 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 18:19:39 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343067579_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2923 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1106
07/23/2012 18:20:36 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343067636_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2922 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 18:20:37 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343067637_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2922 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 73
07/23/2012 18:22:41 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343067761_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2922 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 18:22:52 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343067772_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2922 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1058
07/23/2012 18:27:51 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343068071_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2922 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=4
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 18:27:52 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343068072_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2922 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 160
07/23/2012 18:29:28 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343068168_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2922 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=4
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 18:29:29 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343068169_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2922 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 38
07/23/2012 18:32:49 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343068369_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2922 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 18:33:25 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343068405_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2922 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 3605
07/23/2012 18:37:14 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343068634_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2922 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 18:37:20 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343068640_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2922 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 526
07/23/2012 18:38:00 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343068680_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2922 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 18:38:01 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343068681_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2922 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 113
07/23/2012 18:39:41 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343068781_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2922 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=6
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 18:39:52 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343068792_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2922 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1158
07/23/2012 18:41:31 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343068891_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2922 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=4
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 18:41:58 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343068918_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2922 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2667
07/23/2012 18:42:39 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343068959_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2922 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 18:42:47 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343068967_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2922 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 827
07/23/2012 18:42:48 E-00108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1343068968_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2922 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=CP:354  
07/23/2012 18:49:40 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343069380_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2922 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 18:50:17 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343069417_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2922 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 3699
07/23/2012 18:50:45 E-00196  ERR_BATT_LOW_STATE_OF_HEALTH_DET_LI_ION  LOW_ALARM  <UTC:1343069445_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2921 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=6
                         Reserved(Offset=52)=00
                         Opt.Text=SOH=46 FCC=1828 RemCap=1828 Cycle=287 SN=101397
07/23/2012 18:51:46 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343069506_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2921 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=4
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 18:52:09 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343069529_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2921 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2317
07/23/2012 18:55:09 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343069709_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2921 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=4
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 18:55:21 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343069721_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2921 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1272
07/23/2012 18:58:05 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343069885_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2921 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 18:58:06 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343069886_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2921 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 115
07/23/2012 19:03:30 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343070210_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2921 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=4
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 19:04:01 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343070241_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2921 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 3071
07/23/2012 19:08:00 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343070480_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2921 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=4
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 19:09:10 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343070550_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2920 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 7024
07/23/2012 19:11:35 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343070695_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2920 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 19:11:48 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343070708_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2920 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1308
07/23/2012 19:16:14 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343070974_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2920 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 19:16:56 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343071016_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2920 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 4115
07/23/2012 19:19:52 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343071192_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2920 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 19:19:55 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343071195_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2920 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 327
07/23/2012 19:20:35 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343071235_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2920 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 19:21:12 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343071272_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2920 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 3639
07/23/2012 19:25:33 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343071533_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2919 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=4
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 19:26:37 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343071597_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2919 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 6382
07/23/2012 19:27:17 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343071637_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2919 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 19:27:35 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343071655_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2919 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1763
07/23/2012 19:28:30 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343071710_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2919 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 19:28:36 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343071716_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2919 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 597
07/23/2012 19:30:16 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343071816_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2919 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 19:30:23 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343071823_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2919 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 628
07/23/2012 19:33:18 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343071998_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2919 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=4
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 19:33:33 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343072013_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2919 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1575
07/23/2012 19:34:40 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343072080_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2919 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 19:34:48 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343072088_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2919 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 791
07/23/2012 19:35:44 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343072144_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2919 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 19:36:02 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343072162_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2919 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1850
07/23/2012 19:40:02 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343072402_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2918 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 19:40:10 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343072410_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2919 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 774
07/23/2012 19:41:33 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343072493_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2918 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 19:42:03 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343072523_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2918 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2975
07/23/2012 19:43:02 E-00108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1343072582_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2918 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=CP:354  
07/23/2012 19:45:18 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343072718_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2918 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 19:45:38 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343072738_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2918 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1910
07/23/2012 19:47:05 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343072825_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2918 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=56 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 19:47:15 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343072835_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2918 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 997
07/23/2012 19:50:18 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343073018_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2918 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=4
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 19:50:23 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343073023_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2918 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 589
07/23/2012 19:50:45 E-00196  ERR_BATT_LOW_STATE_OF_HEALTH_DET_LI_ION  LOW_ALARM  <UTC:1343073045_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2918 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=55 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=SOH=46 FCC=1828 RemCap=1826 Cycle=287 SN=101397
07/23/2012 19:51:58 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343073118_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2918 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=54 Meas.BreathRate=4
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 19:52:24 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343073144_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2918 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=54 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2601
07/23/2012 19:55:01 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343073301_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2917 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=54 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 19:55:41 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343073341_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2917 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=54 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 4060
07/23/2012 19:56:32 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343073392_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2917 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 19:56:40 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343073400_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2917 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 833
07/23/2012 19:57:49 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343073469_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2917 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 19:58:20 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343073500_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2917 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 3085
07/23/2012 19:59:52 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343073592_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2917 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 20:00:20 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343073620_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2917 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2874
07/23/2012 20:01:00 E-00195  ERR_BATT_LOW_STATE_OF_HEALTH_INT_LI_ION  URGENT_SERVICE  <UTC:1343073660_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2917 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=4
                         Reserved(Offset=52)=00
                         Opt.Text=SOH=44 FCC=1798 RemCap=1798 Cycle=226 SN=2C01
07/23/2012 20:01:07 E-00195  ERR_BATT_LOW_STATE_OF_HEALTH_INT_LI_ION  URGENT_SERVICE  <UTC:1343073667_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2917 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=4
                         Reserved(Offset=52)=00
                         Opt.Text=SOH=44 FCC=1798 RemCap=1798 Cycle=226 SN=2C01
07/23/2012 20:02:53 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343073773_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2917 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=4
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 20:03:00 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343073780_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2917 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 659
07/23/2012 20:03:47 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343073827_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2917 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 20:04:00 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343073840_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2917 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1362
07/23/2012 20:05:44 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343073944_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2916 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=97) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=4
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 20:06:02 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343073962_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2916 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=97) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1803
07/23/2012 20:11:45 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343074305_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2916 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=93) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 20:12:05 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343074325_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2916 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=92) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2010
07/23/2012 20:14:07 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343074447_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2916 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=92) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=5
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 20:14:15 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343074455_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2916 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=92) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 783
07/23/2012 20:15:58 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343074558_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2916 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=91) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 20:16:09 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343074569_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2916 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=91) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1102
07/23/2012 20:18:06 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343074686_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2916 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=89) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 20:18:30 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343074710_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2916 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=89) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=1
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2453
07/23/2012 20:19:32 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343074772_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2916 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=88) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 20:19:53 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343074793_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2916 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=88) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2100
07/23/2012 20:21:03 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343074863_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2916 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=87) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 20:21:13 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343074873_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2915 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=87) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1002
07/23/2012 20:24:18 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343075058_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2915 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=85) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 20:24:28 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343075068_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2915 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=85) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 950
07/23/2012 20:25:31 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343075131_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2915 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=84) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 20:25:46 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343075146_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2915 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=84) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1541
07/23/2012 20:33:36 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343075616_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2915 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=79) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=4
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 20:34:17 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343075657_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2915 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=79) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 4109
07/23/2012 20:36:42 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343075802_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2915 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=77) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=4
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 20:36:52 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343075812_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2915 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=77) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 987
07/23/2012 20:41:01 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343076061_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2914 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=68) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 20:41:05 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343076065_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2914 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=68) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 362
07/23/2012 20:43:29 E-00108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1343076209_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2914 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=66) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=CP:345  
07/23/2012 20:45:08 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343076308_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2914 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=65) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 20:45:28 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343076328_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2914 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=65) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1995
07/23/2012 20:50:46 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343076646_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2914 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=60) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 20:50:57 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343076657_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2914 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=60) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1124
07/23/2012 20:52:25 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343076745_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2914 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=59) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 20:52:32 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343076752_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2914 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=59) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 714
07/23/2012 20:53:50 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343076830_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2913 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=57) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=4
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 20:54:03 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343076843_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2913 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=57) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1237
07/23/2012 20:55:35 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343076935_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2913 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=56) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 20:55:44 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343076944_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2913 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=56) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 827
07/23/2012 20:56:24 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343076984_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2913 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=55) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 20:56:58 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343077018_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2913 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=54) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 3375
07/23/2012 20:59:38 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343077178_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2913 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=60) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 20:59:50 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343077190_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2913 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=60) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1187
07/23/2012 21:01:31 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343077291_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2913 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=59) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 21:01:34 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343077294_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2913 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=59) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 372
07/23/2012 21:02:59 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343077379_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2913 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=58) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 21:03:01 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343077381_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2913 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=58) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 180
07/23/2012 21:07:05 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343077625_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2913 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=55) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=4
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 21:07:17 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343077637_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2913 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=55) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1158
07/23/2012 21:10:27 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343077827_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2913 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=52) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 21:10:47 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343077847_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2913 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=52) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=1
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2026
07/23/2012 21:11:32 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343077892_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2913 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=51) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 21:11:40 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343077900_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2913 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=51) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 760
07/23/2012 21:12:20 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343077940_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2913 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=51) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 21:12:30 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343077950_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2913 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=51) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 937
07/23/2012 21:13:10 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343077990_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2913 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=50) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 21:13:18 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343077998_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2913 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=50) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 829
07/23/2012 21:15:31 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343078131_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2913 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=49) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=4
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 21:16:04 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343078164_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2913 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=48) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 3304
07/23/2012 21:20:21 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343078421_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2913 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=45) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 21:21:06 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343078466_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2913 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=44) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 4580
07/23/2012 21:21:48 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343078508_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2912 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=44) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=4
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 21:22:14 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343078534_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2912 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=43) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2618
07/23/2012 21:27:20 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343078840_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2912 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=39) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=4
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 21:27:36 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343078856_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2912 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=39) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1683
07/23/2012 21:30:45 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343079045_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2912 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=36) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=4
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 21:30:53 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343079053_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2912 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=36) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 786
07/23/2012 21:31:02 E-00221  ERR_TDA_RSC_LOW_DET_LI_ION  LOG_ONLY  <UTC:1343079062_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2912 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=36) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=V0=16218 V1=13183 V2=80 FCC0=2015 FCC1=3213 SN0=2C01 SN1=101397 Cyc0=226 C
07/23/2012 21:31:02 E-00211  ERR_TDA_CELL_UNDER_VOLTAGE_DET_LI_ION  LOG_ONLY  <UTC:1343079062_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2912 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=36) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=V=13183 C1=2317 C2=3620 C3=3623 C4=3623 C=36 FCC=3213 SN=101397 Cyc=287
07/23/2012 21:31:02 E-00281  ERR_PWR_REDUCTION_DET_LI_ION_DEPLETED  INFO_ALARM  <UTC:1343079062_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2912 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=36) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=V0=16180 V1=13183 V2=80 FCC0=2015 FCC1=3213 RM0=2012 RM1=1149 SN0=2C01 SN1
07/23/2012 21:31:59 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343079119_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2912 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=99 DetLi=36) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 21:32:21 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343079141_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2912 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=99 DetLi=36) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2188
07/23/2012 21:34:45 E-00221  ERR_TDA_RSC_LOW_DET_LI_ION  LOG_ONLY  <UTC:1343079285_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2912 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=34) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=5
                         Reserved(Offset=52)=00
                         Opt.Text=V0=16191 V1=13132 V2=80 FCC0=2019 FCC1=3131 SN0=2C01 SN1=101397 Cyc0=226 C
07/23/2012 21:34:45 E-00211  ERR_TDA_CELL_UNDER_VOLTAGE_DET_LI_ION  LOG_ONLY  <UTC:1343079285_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2912 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=34) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=5
                         Reserved(Offset=52)=00
                         Opt.Text=V=13132 C1=2212 C2=3639 C3=3641 C4=3641 C=34 FCC=3131 SN=101397 Cyc=287
07/23/2012 21:34:45 E-00281  ERR_PWR_REDUCTION_DET_LI_ION_DEPLETED  INFO_ALARM  <UTC:1343079285_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2912 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=34) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=5
                         Reserved(Offset=52)=00
                         Opt.Text=V0=16056 V1=13132 V2=80 FCC0=2019 FCC1=3131 RM0=1945 RM1=1060 SN0=2C01 SN1
07/23/2012 21:36:04 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343079364_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2912 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=96 DetLi=34) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 21:36:23 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343079383_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2912 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=95 DetLi=34) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1918
07/23/2012 21:38:25 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343079505_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2912 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=93 DetLi=34) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=4
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 21:38:46 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343079526_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2912 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=93 DetLi=34) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2101
07/23/2012 21:42:01 E-00221  ERR_TDA_RSC_LOW_DET_LI_ION  LOG_ONLY  <UTC:1343079721_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2912 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=89 DetLi=34) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=7
                         Reserved(Offset=52)=00
                         Opt.Text=V0=15851 V1=13074 V2=40 FCC0=2018 FCC1=3121 SN0=2C01 SN1=101397 Cyc0=226 C
07/23/2012 21:42:01 E-00211  ERR_TDA_CELL_UNDER_VOLTAGE_DET_LI_ION  LOG_ONLY  <UTC:1343079721_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2912 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=89 DetLi=34) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=7
                         Reserved(Offset=52)=00
                         Opt.Text=V=13074 C1=2142 C2=3643 C3=3645 C4=3645 C=34 FCC=3121 SN=101397 Cyc=287
07/23/2012 21:42:01 E-00281  ERR_PWR_REDUCTION_DET_LI_ION_DEPLETED  INFO_ALARM  <UTC:1343079721_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2912 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=89 DetLi=34) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=7
                         Reserved(Offset=52)=00
                         Opt.Text=V0=15851 V1=13074 V2=80 FCC0=2018 FCC1=3121 RM0=1792 RM1=1043 SN0=2C01 SN1
07/23/2012 21:43:34 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343079814_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2912 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=88 DetLi=34) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=4
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 21:43:46 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343079826_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2912 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=87 DetLi=34) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1133
07/23/2012 21:43:46 E-00108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1343079826_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2912 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=87 DetLi=34) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=CP:354  
07/23/2012 21:47:52 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343080072_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2912 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=83 DetLi=34) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=5
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 21:47:56 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343080076_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2912 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=83 DetLi=34) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 377
07/23/2012 21:48:52 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343080132_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2912 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=82 DetLi=34) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 21:49:00 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343080140_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2912 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=82 DetLi=34) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 842
07/23/2012 21:53:02 E-00221  ERR_TDA_RSC_LOW_DET_LI_ION  LOG_ONLY  <UTC:1343080382_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=78 DetLi=34) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=4
                         Reserved(Offset=52)=00
                         Opt.Text=V0=15664 V1=13163 V2=80 FCC0=2219 FCC1=3112 SN0=2C01 SN1=101397 Cyc0=226 C
07/23/2012 21:53:02 E-00211  ERR_TDA_CELL_UNDER_VOLTAGE_DET_LI_ION  LOG_ONLY  <UTC:1343080382_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=78 DetLi=34) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=4
                         Reserved(Offset=52)=00
                         Opt.Text=V=13163 C1=2222 C2=3646 C3=3648 C4=3647 C=34 FCC=3112 SN=101397 Cyc=287
07/23/2012 21:53:03 E-00281  ERR_PWR_REDUCTION_DET_LI_ION_DEPLETED  INFO_ALARM  <UTC:1343080383_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=80 DetLi=34) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=4
                         Reserved(Offset=52)=00
                         Opt.Text=V0=15650 V1=13163 V2=80 FCC0=2219 FCC1=3112 RM0=1764 RM1=1028 SN0=2C01 SN1
07/23/2012 21:55:37 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343080537_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=77 DetLi=34) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=4
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 21:55:42 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343080542_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=77 DetLi=34) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 525
07/23/2012 21:59:00 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343080740_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=74 DetLi=34) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 21:59:35 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343080775_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=73 DetLi=34) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 3471
07/23/2012 22:01:10 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343080870_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=72 DetLi=34) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=4
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 22:01:31 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343080891_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=71 DetLi=34) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2177
07/23/2012 22:02:08 E-00195  ERR_BATT_LOW_STATE_OF_HEALTH_INT_LI_ION  URGENT_SERVICE  <UTC:1343080928_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=68 DetLi=34) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=SOH=49 FCC=2035 RemCap=1376 Cycle=226 SN=2C01
07/23/2012 22:04:10 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343081050_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=66 DetLi=34) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=4
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 22:04:27 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343081067_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=66 DetLi=34) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1688
07/23/2012 22:06:45 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343081205_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=63 DetLi=34) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 22:06:51 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343081211_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=63 DetLi=34) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 635
07/23/2012 22:08:33 E-00221  ERR_TDA_RSC_LOW_DET_LI_ION  LOG_ONLY  <UTC:1343081313_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=66 DetLi=35) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=V0=15338 V1=13095 V2=80 FCC0=2288 FCC1=3209 SN0=2C01 SN1=101397 Cyc0=226 C
07/23/2012 22:08:33 E-00211  ERR_TDA_CELL_UNDER_VOLTAGE_DET_LI_ION  LOG_ONLY  <UTC:1343081313_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=66 DetLi=35) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=V=13095 C1=2151 C2=3647 C3=3649 C4=3648 C=35 FCC=3209 SN=101397 Cyc=287
07/23/2012 22:08:33 E-00281  ERR_PWR_REDUCTION_DET_LI_ION_DEPLETED  INFO_ALARM  <UTC:1343081313_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=66 DetLi=35) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=V0=15338 V1=13095 V2=80 FCC0=2288 FCC1=3209 RM0=1495 RM1=1119 SN0=2C01 SN1
07/23/2012 22:08:59 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343081339_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=65 DetLi=35) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 22:10:02 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343081402_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=64 DetLi=35) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 6303
07/23/2012 22:11:24 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343081484_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=63 DetLi=35) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 22:11:44 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343081504_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=63 DetLi=35) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1969
07/23/2012 22:12:25 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343081545_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=62 DetLi=35) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 22:13:26 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343081606_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=61 DetLi=35) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 6126
07/23/2012 22:15:47 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343081747_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=59 DetLi=35) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=4
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 22:16:03 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343081763_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=58 DetLi=35) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1598
07/23/2012 22:18:25 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343081905_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=56 DetLi=35) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 22:18:27 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343081907_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=56 DetLi=35) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 210
07/23/2012 22:19:07 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343081947_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=55 DetLi=35) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 22:19:16 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343081956_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=55 DetLi=35) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 924
07/23/2012 22:20:19 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343082019_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=54 DetLi=35) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 22:20:28 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343082028_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=54 DetLi=35) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 888
07/23/2012 22:21:09 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343082069_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=53 DetLi=35) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 22:21:28 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343082088_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=53 DetLi=35) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=1
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1976
07/23/2012 22:22:28 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343082148_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=52 DetLi=35) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=6
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 22:23:03 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343082183_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=52 DetLi=35) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 3485
07/23/2012 22:23:56 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343082236_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=51 DetLi=35) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=4
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 22:23:56 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343082236_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=51 DetLi=35) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 10
07/23/2012 22:24:36 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343082276_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=50 DetLi=35) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 22:25:00 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343082300_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=50 DetLi=35) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=1
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2430
07/23/2012 22:26:30 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343082390_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=44 DetLi=35) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 22:26:44 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343082404_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=44 DetLi=35) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1411
07/23/2012 22:27:29 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343082449_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=43 DetLi=35) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 22:28:14 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343082494_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=42 DetLi=35) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 4493
07/23/2012 22:29:37 E-00281  ERR_PWR_REDUCTION_DET_LI_ION_DEPLETED  INFO_ALARM  <UTC:1343082577_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=42 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=V0=14813 V1=0 V2=80 FCC0=2169 FCC1=0 RM0=899 RM1=0 SN0=2C01 SN1=0
07/23/2012 22:32:15 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343082735_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=39 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=4
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 22:32:28 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343082748_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=39 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1346
07/23/2012 22:37:24 E-00185  ERR_LAST_BATT_INT_LI_ION_LOW  MED_ALARM  <UTC:1343083044_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=34 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=4
                         Reserved(Offset=52)=00
                         Opt.Text=NSrcs=1 V0=14686 ATR0=31 V1=0 ATR1=65535 V2=80 FCC0=2169 FCC1=0 RM0=718 RM
07/23/2012 22:37:37 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343083057_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=33 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=4
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 22:37:38 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343083058_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=33 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 105
07/23/2012 22:38:19 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343083099_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=33 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 22:38:27 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343083107_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=32 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 837
07/23/2012 22:39:36 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343083176_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=31 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 22:39:50 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343083190_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=31 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1422
07/23/2012 22:40:38 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343083238_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=30 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 22:40:56 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343083256_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=30 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1829
07/23/2012 22:43:53 E-00108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1343083433_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=27 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=5
                         Reserved(Offset=52)=00
                         Opt.Text=CP:348  
07/23/2012 22:44:29 E-00188  ERR_LAST_BATT_INT_LI_ION_NEARLY_DEPLETED  HIGH_ALARM  <UTC:1343083469_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=26 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=5
                         Reserved(Offset=52)=00
                         Opt.Text=NSrcs=1 V0=14542 ATR0=21 V1=0 ATR1=65535 V2=80 FCC0=2169 FCC1=0 RM0=553 RM
07/23/2012 22:45:56 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343083556_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=24 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 22:46:28 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343083588_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=24 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 3164
07/23/2012 22:47:43 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343083663_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=22 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=4
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 22:48:35 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343083715_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=21 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 5213
07/23/2012 22:55:17 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343084117_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=14 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=3
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 22:55:48 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343084148_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=14 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 3063
07/23/2012 22:57:09 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343084229_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=12 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=4
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 22:57:15 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343084235_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=12 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 658
07/23/2012 22:58:05 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343084285_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=11 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=4
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/23/2012 22:58:27 E-00245  ERR_SOFT_POWER_LOSS  LOG_ONLY  <UTC:1343084307_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=11 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=2
                         Reserved(Offset=52)=00
                         Opt.Text=Src=0 V0=14401 V1=0 V2=80 FCC0=2169 FCC1=0 RM0=222 RM1=0 SN0=2C01 SN1=0
07/23/2012 22:58:43 E-00108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1343084323_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2911 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=11 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=53 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=CQ:-14   MP:-44   PP:-14  
07/23/2012 23:03:28 E-00297  ERR_SLEEP_EVENT  LOG_ONLY  <UTC:1343084608_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2910 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=8 DetLi=0) MaxUsage=86 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=52 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=IntC=8 DetC=0 V0=14568 V1=0 FCC0=2169 FCC1=0 SN0=2C01 SN1=0
07/24/2012 10:52:39 E-00152  ERR_POWER_UP_SYSTEM_INITIALIZATION  LOG_ONLY  <UTC:1343127159_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm=    0 SWver=  10.2.XX HWver=    
                         ExhType=0 PwrStat=00 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=0 MinAvgLeadAcidVolt=36000 PwrSource=4(NO_SOURCE)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=0 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Flash Build
07/24/2012 10:52:39 E-00034  ERR_DSP_EXT_POWER_UP_SYSTEM_INIT  LOG_ONLY  <UTC:1343127159_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2980 SWver=  10.2.XX HWver=   0
                         ExhType=0 PwrStat=00 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=0 MinAvgLeadAcidVolt=36000 PwrSource=4(NO_SOURCE)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=0 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=
07/24/2012 10:52:39 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343127159_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2878 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=00 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=0 MinAvgLeadAcidVolt=36000 PwrSource=4(NO_SOURCE)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=0 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/24/2012 10:52:39 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343127159_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2902 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=00 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=0 MinAvgLeadAcidVolt=36000 PwrSource=4(NO_SOURCE)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=0 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1
07/24/2012 10:52:39 E-00341  ERR_FAN_CONTROL  LOG_ONLY  <UTC:1343127159_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2902 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=0 MinAvgLeadAcidVolt=80 PwrSource=4(NO_SOURCE)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=35 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Case Fan: ON 00100 IntBattT:0C DetBattT:0C Air:23.6C Mtr:21.0C
07/24/2012 10:52:40 E-00249  ERR_AC_CONNECTED  LOG_ONLY  <UTC:1343127160_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2902 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=27 MinAvgLeadAcidVolt=80 PwrSource=4(NO_SOURCE)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=37 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=
07/24/2012 10:52:40 E-00326  ERR_SOFT_POWER_LOSS_EXIT  LOG_ONLY  <UTC:1343127160_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2902 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=5 DetLi=0) MaxUsage=27 MinAvgLeadAcidVolt=80 PwrSource=4(NO_SOURCE)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=37 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Src=3 NSrcs=1 V0=14669 V1=14342 V2=80 FCC0=2088 FCC1=1805 RM0=86 RM1=0
07/24/2012 10:52:41 E-00195  ERR_BATT_LOW_STATE_OF_HEALTH_INT_LI_ION  URGENT_SERVICE  <UTC:1343127161_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2902 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=5 DetLi=0) MaxUsage=27 MinAvgLeadAcidVolt=80 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=38 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=SOH=50 FCC=2088 RemCap=86 Cycle=226 SN=2C01
07/24/2012 10:52:41 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343127161_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2902 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=5 DetLi=0) MaxUsage=27 MinAvgLeadAcidVolt=80 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=39 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
07/24/2012 10:52:41 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343127161_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2902 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=5 DetLi=0) MaxUsage=27 MinAvgLeadAcidVolt=80 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=39 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1
07/24/2012 10:52:42 E-00196  ERR_BATT_LOW_STATE_OF_HEALTH_DET_LI_ION  LOW_ALARM  <UTC:1343127162_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2902 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=5 DetLi=0) MaxUsage=27 MinAvgLeadAcidVolt=80 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=38 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=SOH=46 FCC=1805 RemCap=0 Cycle=287 SN=101397
07/24/2012 10:52:42 E-00221  ERR_TDA_RSC_LOW_DET_LI_ION  LOG_ONLY  <UTC:1343127162_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2902 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=5 DetLi=0) MaxUsage=27 MinAvgLeadAcidVolt=80 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=39 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=V0=14694 V1=14525 V2=80 FCC0=2088 FCC1=1805 SN0=2C01 SN1=101397 Cyc0=226 C
07/24/2012 10:52:44 E-00185  ERR_LAST_BATT_INT_LI_ION_LOW  MED_ALARM  <UTC:1343127164_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2902 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=5 DetLi=0) MaxUsage=27 MinAvgLeadAcidVolt=74 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=40 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Src=3 Cap0=5 V0=14706 V1=14537 V2=40 FCC0=2088 FCC1=1805 RM0=86 RM1=0
07/24/2012 10:52:50 E-00108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1343127170_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2901 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=5 DetLi=0) MaxUsage=27 MinAvgLeadAcidVolt=74 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=42 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=CP:299  
07/24/2012 10:52:52 E-00195  ERR_BATT_LOW_STATE_OF_HEALTH_INT_LI_ION  URGENT_SERVICE  <UTC:1343127172_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2901 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=5 DetLi=0) MaxUsage=27 MinAvgLeadAcidVolt=75 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=42 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=SOH=50 FCC=2088 RemCap=87 Cycle=226 SN=2C01
07/24/2012 10:53:00 E-00148  ERR_DEBUG  LOG_ONLY  <UTC:1343127180_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2902 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=80 Capacity(LA=0 IntLi=5 DetLi=0) MaxUsage=27 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=42 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=DET removed
07/24/2012 10:55:39 E-00341  ERR_FAN_CONTROL  LOG_ONLY  <UTC:1343127339_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2903 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=80 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=32 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=49 Meas.BreathRate=5
                         Reserved(Offset=52)=00
                         Opt.Text=Case Fan: OFF 00000 IntBattT:0C DetBattT:0C Air:27.4C Mtr:28.0C
07/24/2012 10:55:47 E-00057  ERR_THREAD_STACK_RESERVE  LOG_ONLY  <UTC:1343127347_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2903 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=80 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=32 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=49 Meas.BreathRate=5
                         Reserved(Offset=52)=00
                         Opt.Text=Thread: SDFileManagementThread
07/24/2012 10:55:54 E-00107  ERR_SPEAKER_2_FAILURE  URGENT_SERVICE  <UTC:1343127354_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2903 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=80 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=32 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=0  Params= d0 07 00 00 00 00 00 00 00 00 00 00 00 00 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=49 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Speaker On  Note:2638 Alarm:18 Volume: 1 VPwrFail: 4633
07/24/2012 10:55:58 E-00248  ERR_INFORMATION  LOG_ONLY  <UTC:1343127358_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2903 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=80 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=36 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=be c1 c4 
                         Rx Mode=0  Params= d0 07 00 d0 d3 d6 d9 dc df e2 e5 e8 eb ee 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=49 Meas.BreathRate=0
                         Reserved(Offset=52)=f7
                         Opt.Text=4.0  [March 30, 2009] WDOG:1 MDL:1054260 I:0 D:0
07/24/2012 10:55:58 E-00248  ERR_INFORMATION  LOG_ONLY  <UTC:1343127358_00>
                         Status=0x00  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=AutoTrak)
                         Patm= 2903 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=80 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=36 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=b0 b6 bc 
                         Rx Mode=0  Params= d0 07 00 d4 da e0 e6 ec f2 f8 fe 04 0a 10 
                            Mode=CPAP,Pr=2000,CFLex=0
                         DSPTmpr=49 Meas.BreathRate=0
                         Reserved(Offset=52)=22
                         Opt.Text=A376:11 A377:11 A378:11 A379:11 A37A:11 A37B:00 4F32:00 

COUNT  ERRCODE      Log 17 (Encrypted Significant Event Text)
    1  E-072   ERR_MMC_SD_CARD_INSERTED  BEEP_ONLY
    2  E-106   ERR_SPEAKER_1_FAILURE  URGENT_SERVICE
    3  E-107   ERR_SPEAKER_2_FAILURE  URGENT_SERVICE
   13  E-166   ERR_UI_RESET_KEY_PRESS  KEYPRESS
    1  E-174   ERR_LOSS_OF_COMM_CHARGER  URGENT_SERVICE
    4  E-179   ERR_PWR_REDUCTION_AC_DISCONNECTED  MED_ALARM
    2  E-181   ERR_PWR_REDUCTION_DET_LI_ION_DISCONNECTED  INFO_ALARM
    2  E-185   ERR_LAST_BATT_INT_LI_ION_LOW  MED_ALARM
    1  E-188   ERR_LAST_BATT_INT_LI_ION_NEARLY_DEPLETED  HIGH_ALARM
   13  E-195   ERR_BATT_LOW_STATE_OF_HEALTH_INT_LI_ION  URGENT_SERVICE
    7  E-196   ERR_BATT_LOW_STATE_OF_HEALTH_DET_LI_ION  LOW_ALARM
    2  E-197   ERR_INT_LI_ION_NOT_PRESENT  URGENT_SERVICE
    6  E-251   ERR_DET_LI_ION_CONNECTED  BEEP_ONLY
    2  E-252   ERR_INT_LI_ION_CONNECTED  BEEP_ONLY
    1  E-264   ERR_MENU_BYPASS_ACTIVATED  KEYPRESS
    7  E-281   ERR_PWR_REDUCTION_DET_LI_ION_DEPLETED  INFO_ALARM
    1  E-282   ERR_INT_LI_ION_DEPLETED  HIGH_ALARM
    3  E-284   ERR_PWR_UPGRADE_AC_IN_USE  BEEP_ONLY
    6  E-286   ERR_PWR_UPGRADE_DET_LI_ION_IN_USE  BEEP_ONLY
   11  E-290   ERR_URGENT_REMINDER  URGENT_SERVICE
    2  E-293   ERR_POWER_OFF_KEY  KEYPRESS
    2  E-294   ERR_POWER_OFF_YES_KEY  KEYPRESS
    3  E-324   ERR_POWER_ON  KEYPRESS

COUNT  ERRCODE      Log 18 (Encrypted Engineering Debug Text)
    1  E-034   ERR_DSP_EXT_POWER_UP_SYSTEM_INIT  LOG_ONLY
    1  E-057   ERR_THREAD_STACK_RESERVE  LOG_ONLY
    1  E-096   ERR_CALIBRATION_CONTROL  LOG_ONLY
    2  E-106   ERR_SPEAKER_1_FAILURE  URGENT_SERVICE
    3  E-107   ERR_SPEAKER_2_FAILURE  URGENT_SERVICE
   15  E-108   ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY
  346  E-148   ERR_DEBUG  LOG_ONLY
    1  E-152   ERR_POWER_UP_SYSTEM_INITIALIZATION  LOG_ONLY
    2  E-185   ERR_LAST_BATT_INT_LI_ION_LOW  MED_ALARM
    1  E-188   ERR_LAST_BATT_INT_LI_ION_NEARLY_DEPLETED  HIGH_ALARM
   13  E-195   ERR_BATT_LOW_STATE_OF_HEALTH_INT_LI_ION  URGENT_SERVICE
    7  E-196   ERR_BATT_LOW_STATE_OF_HEALTH_DET_LI_ION  LOW_ALARM
    5  E-211   ERR_TDA_CELL_UNDER_VOLTAGE_DET_LI_ION  LOG_ONLY
    9  E-221   ERR_TDA_RSC_LOW_DET_LI_ION  LOG_ONLY
    1  E-245   ERR_SOFT_POWER_LOSS  LOG_ONLY
    2  E-248   ERR_INFORMATION  LOG_ONLY
    4  E-249   ERR_AC_CONNECTED  LOG_ONLY
    7  E-281   ERR_PWR_REDUCTION_DET_LI_ION_DEPLETED  INFO_ALARM
    1  E-282   ERR_INT_LI_ION_DEPLETED  HIGH_ALARM
    1  E-297   ERR_SLEEP_EVENT  LOG_ONLY
    1  E-326   ERR_SOFT_POWER_LOSS_EXIT  LOG_ONLY
    1  E-334   ERR_RE_SEALED_INT_LI_ION  LOG_ONLY
    1  E-335   ERR_RE_SEALED_DET_LI_ION  LOG_ONLY
    2  E-341   ERR_FAN_CONTROL  LOG_ONLY
