[Header]
bq EVSW Version = 0.9.79	
DeviceName = bq20z80 v1.10
Time = 7/31/2012 9:33:11 AM	


[Voltage(1st Level Safety)]
COV Threshold = 4300
COV Time = 2
COV Recovery = 4100
COV Delta = 20
COV Temp. Hys = 100
POV Threshold = 16800
POV Time = 5
POV Recovery = 16000
CUV Threshold = 2500
CUV Time = 2
CUV Recovery = 3000
PUV Threshold = 10400
PUV Time = 4
PUV Recovery = 12000
[Current(1st Level Safety)]
OC (1st Tier) Chg = 4000
OC (1st Tier) Chg Time = 2
OC Chg Recovery = 200
OC (1st Tier) Dsg = 6000
OC (1st Tier) Dsg Time = 5
OC Dsg Recovery = 200
OC (2nd Tier) Chg = 8000
OC (2nd Tier) Chg Time = 1
OC (2nd Tier) Dsg = 14000
OC (2nd Tier) Dsg Time = 0
Current Recovery Time = 8
AFE OC Dsg = 1F
AFE OC Dsg Time = 0F
AFE OC Dsg Recovery = 100
AFE SC Chg Cfg = 64
AFE SC Dsg Cfg = FF
AFE SC Recovery = 100
[Temperature(1st Level Safety)]
Over Temp Chg = 500
OT Chg Time = 2
OT Chg Recovery = 400
Over Temp Dsg = 600
OT Dsg Time = 2
OT Dsg Recovery = 550
[Host Comm(1st Level Safety)]
Host Watchdog Timeout = 0

[Voltage(2nd Level Safety)]
SOV Threshold = 17500
SOV Time = 10
Cell Imbalance Current = 100
Cell Imbalance Fail Voltage = 1000
Cell Imbalance Time = 4
Battery Rest Time = 1800
PFIN Detect Time = 0
[Current(2nd Level Safety)]
SOC Chg = 10000
SOC Chg Time = 4
SOC Dsg = 20000
SOC Dsg Time = 0
[Temperature(2nd Level Safety)]
SOT Chg = 800
SOT Chg Time = 30
SOT Dsg = 800
SOT Dsg Time = 30
Open Thermistor = -450
Open Time = 30
[FET Verification(2nd Level Safety)]
FET Fail Limit = 100
FET Fail Time = 1
[AFE Verification(2nd Level Safety)]
AFE Check Time = 30
AFE Fail Limit = 10
AFE Fail Recovery Time = 20
AFE Init Retry Limit = 6
AFE Init Limit = 20
[Fuse Verification(2nd Level Safety)]
Fuse Fail Limit = 2
Fuse Fail Time = 0

[Charge Inhibit Cfg(Charge Control)]
Chg Inhibit Temp Low = 0
Chg Inhibit Temp High = 450
Temp Hys = 20
[Pre-Charge Cfg(Charge Control)]
Pre-chg Current = 250
Pre-chg Temp = 50
Pre-chg Voltage = 3000
Recovery Voltage = 3100
[Fast Charge Cfg(Charge Control)]
Fast Charge Current = 2000
Charging Voltage = 16400
Delta Temp = 50
Suspend Low Temp = -25
Suspend High Temp = 500
[Pulse Charge Cfg(Charge Control)]
Turn ON Voltage = 4150
Turn OFF Voltage = 5000
Max ON Pulse Time = 240
Min OFF Pulse Time = 0
Max OFF Voltage = 5000
[Termination Cfg.(Charge Control)]
Maintenance Current = 0
Taper Current = 100
Termination Voltage = 300
Current Taper Window = 40
TCA Set % = -1
TCA Clear % = 95
FC Set % = -1
FC Clear % = 95
[Cell Balancing Cfg(Charge Control)]
Min Cell Deviation = 1750
[Charging Faults(Charge Control)]
Over Charging Voltage = 300
Over Charging Volt Time = 2
Over Charging Current = 1000
Over Charging Curr Time = 2
Over Charging Curr Recov = 100
Depleted Voltage = 7000
Depleted Voltage Time = 2
Depleted Recovery = 8500
Over Charge Capacity = 1000
Over Charge Recovery = 2
FC-MTO = 0
PC-MTO = 3600
Charge Fault Cfg = 0E

[Data(SBS Configuration)]
Rem Cap Alarm = 400
Rem Energy Alarm = 5760
Rem Time Alarm = 10
Init Battery Mode = 0081
Design Voltage = 14400
Spec Info = 0031
Manuf Date = 24-Sep-2009
Ser. Num. = 0409
Cycle Count = 270
CC Threshold = 3760
CC % = 100
CF MaxError Limit = 5
Design Capacity = 4176
Design Energy = 6000
Manuf Name = Nexergy Inc
Device Name = LI5032
Device Chemistry = LION
[Configuration(SBS Configuration)]
TDA Set % = 0
TDA Clear % = 15
FD Set % = 0
FD Clear % = 15
TDA Set Volt Threshold = 10000
TDA Set Volt Time = 5
TDA Clear Volt = 12600
FD Set Volt Threshold = 10000
FD Volt Time = 5
FD Clear Volt = 12600

[Manufacturer Data(System Data)]
Pack Lot Code = 0000
PCB Lot Code = 0775
Firmware Version = 1220
Hardware Revision = 0000
Cell Revision = 0000
[Manufacturer Info(System Data)]
Manuf. Info = 090809
[Lifetime Data(System Data)]
Lifetime Max Temp = 452
Lifetime Min Temp = -36
Lifetime Max Cell Voltage = 4130
Lifetime Min Cell Voltage = 2431
Lifetime Max Pack Voltage = 16480
Lifetime Min Pack Voltage = 10286
Lifetime Max Chg Current = 2000
Lifetime Max Dsg Current = -4943
Lifetime Max Chg Power = 3261
Lifetime Max Dsg Power = -6924
Life Max AvgDsg Cur = -2284
Life Max AvgDsg Pow = -3441
Lifetime Avg Temp = 277
[Lifetime Temp Samples(System Data)]
LT Temp Samples = 353885

[Registers(Configuration)]
Operation Cfg A = 0F31
Operation Cfg B = 6548
Operation Cfg C = 0000
Permanent Fail Cfg = 0000
Non-Removable Cfg = 0000

[LED Cfg(LED Support)]
LED Flash Rate = 512
LED Blink Rate = 1024
LED Delay = 100
LED Hold Time = 4
CHG Flash Alarm = 10
CHG Thresh 1 = 0
CHG Thresh 2 = 20
CHG Thresh 3 = 40
CHG Thresh 4 = 60
CHG Thresh 5 = 80
DSG Flash Alarm = 10
DSG Thresh 1 = 0
DSG Thresh 2 = 20
DSG Thresh 3 = 40
DSG Thresh 4 = 60
DSG Thresh 5 = 80

[Power(Power)]
Flash Update OK Voltage = 7500
Shutdown Voltage = 10000
Shutdown Time = 4
Charger Present = 3000
Sleep Current = 20
Bus Low Time = 5
Cal Inhibit Temp Low = 50
Cal Inhibit Temp High = 450
Sleep Voltage Time = 20
Sleep Current Time = 20

[IT Cfg(Gas Gauging)]
Load Select = 3
Load Mode = 1
Term Voltage = 12000
User Rate-mA = -2100
User Rate-mW = -30000
Reserve Cap-mAh = 100
Reserve Cap-mWh = 140
[Current Thresholds(Gas Gauging)]
Dsg Current Threshold = 50
Chg Current Threshold = 50
Quit Current = 20
Dsg Relax Time = 10
Chg Relax Time = 30
[State(Gas Gauging)]
Qmax Cell 0 = 4902
Qmax Cell 1 = 4905
Qmax Cell 2 = 4911
Qmax Cell 3 = 4942
Qmax Pack = 4902
Update Status = 06
Avg I Last Run = -2171
Avg P Last Run = -3179
Delta Voltage = 432

[R_a0(Ra Table)]
Cell0 R_a flag = 0055
Cell0 R_a 0 = 97
Cell0 R_a 1 = 97
Cell0 R_a 2 = 119
Cell0 R_a 3 = 137
Cell0 R_a 4 = 137
Cell0 R_a 5 = 141
Cell0 R_a 6 = 216
Cell0 R_a 7 = 502
Cell0 R_a 8 = 639
Cell0 R_a 9 = 814
Cell0 R_a 10 = 1248
Cell0 R_a 11 = 968
Cell0 R_a 12 = 1369
Cell0 R_a 13 = 4320
Cell0 R_a 14 = 4571
[R_a1(Ra Table)]
Cell1 R_a flag = 0000
Cell1 R_a 0 = 253
Cell1 R_a 1 = 228
Cell1 R_a 2 = 253
Cell1 R_a 3 = 527
Cell1 R_a 4 = 1246
Cell1 R_a 5 = 1189
Cell1 R_a 6 = 2089
Cell1 R_a 7 = 4253
Cell1 R_a 8 = 5132
Cell1 R_a 9 = 6213
Cell1 R_a 10 = 5427
Cell1 R_a 11 = 4716
Cell1 R_a 12 = 5766
Cell1 R_a 13 = 21364
Cell1 R_a 14 = 22553
[R_a2(Ra Table)]
Cell2 R_a flag = 0000
Cell2 R_a 0 = 116
Cell2 R_a 1 = 116
Cell2 R_a 2 = 116
Cell2 R_a 3 = 237
Cell2 R_a 4 = 497
Cell2 R_a 5 = 469
Cell2 R_a 6 = 810
Cell2 R_a 7 = 1845
Cell2 R_a 8 = 2259
Cell2 R_a 9 = 2259
Cell2 R_a 10 = 1792
Cell2 R_a 11 = 1387
Cell2 R_a 12 = 1840
Cell2 R_a 13 = 6797
Cell2 R_a 14 = 7135
[R_a3(Ra Table)]
Cell3 R_a flag = 0000
Cell3 R_a 0 = 127
Cell3 R_a 1 = 113
Cell3 R_a 2 = 113
Cell3 R_a 3 = 213
Cell3 R_a 4 = 678
Cell3 R_a 5 = 641
Cell3 R_a 6 = 1024
Cell3 R_a 7 = 2319
Cell3 R_a 8 = 2931
Cell3 R_a 9 = 3410
Cell3 R_a 10 = 3148
Cell3 R_a 11 = 2440
Cell3 R_a 12 = 3468
Cell3 R_a 13 = 11878
Cell3 R_a 14 = 12819
[R_a0x(Ra Table)]
xCell0 R_a flag = 0000
xCell0 R_a 0 = 97
xCell0 R_a 1 = 97
xCell0 R_a 2 = 119
xCell0 R_a 3 = 174
xCell0 R_a 4 = 174
xCell0 R_a 5 = 179
xCell0 R_a 6 = 274
xCell0 R_a 7 = 638
xCell0 R_a 8 = 811
xCell0 R_a 9 = 1034
xCell0 R_a 10 = 1585
xCell0 R_a 11 = 1229
xCell0 R_a 12 = 1739
xCell0 R_a 13 = 5487
xCell0 R_a 14 = 5806
[R_a1x(Ra Table)]
xCell1 R_a flag = 0055
xCell1 R_a 0 = 107
xCell1 R_a 1 = 96
xCell1 R_a 2 = 107
xCell1 R_a 3 = 223
xCell1 R_a 4 = 527
xCell1 R_a 5 = 503
xCell1 R_a 6 = 883
xCell1 R_a 7 = 1799
xCell1 R_a 8 = 2170
xCell1 R_a 9 = 2628
xCell1 R_a 10 = 2295
xCell1 R_a 11 = 1995
xCell1 R_a 12 = 2439
xCell1 R_a 13 = 9035
xCell1 R_a 14 = 9538
[R_a2x(Ra Table)]
xCell2 R_a flag = 0055
xCell2 R_a 0 = 109
xCell2 R_a 1 = 109
xCell2 R_a 2 = 109
xCell2 R_a 3 = 223
xCell2 R_a 4 = 467
xCell2 R_a 5 = 441
xCell2 R_a 6 = 761
xCell2 R_a 7 = 1734
xCell2 R_a 8 = 2123
xCell2 R_a 9 = 2123
xCell2 R_a 10 = 1684
xCell2 R_a 11 = 1303
xCell2 R_a 12 = 1729
xCell2 R_a 13 = 6387
xCell2 R_a 14 = 6704
[R_a3x(Ra Table)]
xCell3 R_a flag = 0055
xCell3 R_a 0 = 125
xCell3 R_a 1 = 111
xCell3 R_a 2 = 111
xCell3 R_a 3 = 209
xCell3 R_a 4 = 666
xCell3 R_a 5 = 630
xCell3 R_a 6 = 1006
xCell3 R_a 7 = 2278
xCell3 R_a 8 = 2879
xCell3 R_a 9 = 3350
xCell3 R_a 10 = 3092
xCell3 R_a 11 = 2397
xCell3 R_a 12 = 3407
xCell3 R_a 13 = 11668
xCell3 R_a 14 = 12592

[Device Status Data(PF Status)]
PF Flags 1 = 0000
Fuse Flag = 0000
PF Voltage = 0
PF C4 Voltage = 0
PF C3 Voltage = 0
PF C2 Voltage = 0
PF C1 Voltage = 0
PF Current = 0
PF Temperature = 0
PF Batt Stat = 0000
PF RC-mAh = 0
PF RC-10mWh = 0
PF Chg Status = 0000
PF Safety Status = 0000
PF Flags 2 = 0000
[AFE Regs(PF Status)]
AFE Status = 00
AFE Output = 00
AFE State = 00
AFE Function = 00
AFE Cell Select = 00
AFE OLV = 00
AFE OLT = 00
AFE SCC = 00
AFE SCD = 00

[Data(Calibration)]
CC Gain = 0.9296
CC Delta = 277277.6875
Ref Voltage = 2451.9
AFE Corr = 1288
AFE Pack Gain = 30625
CC Offset = -12493
Board Offset = 18
Int Temp Offset = -30
Ext1 Temp Offset = -21
Ext2 Temp Offset = -14
[Config(Calibration)]
CC Current = 3000
Voltage Signal = 16800
Temp Signal = 298.0
CC Offset Time = 250
ADC Offset Time = 32
CC Gain Time = 250
Voltage Time = 1984
Temperature Time = 32
Cal Mode Timeout = 38400
[Temp Model(Calibration)]
Ext Coef 1 = -28285
Ext Coef 2 = 20848
Ext Coef 3 = -7537
Ext Coef 4 = 4012
Ext Min AD = 0
Ext Max Temp = 4012
Int Coef 1 = 0
Int Coef 2 = 0
Int Coef 3 = -11136
Int Coef 4 = 5754
Int Min AD = 0
Int Max Temp = 5754
[Current(Calibration)]
Filter = 239
Deadband = 3
CC Deadband = 34
CC Max Deadband = 5
CC Deadband Sample = 256
CC Max Offset Sample = 64
