[Header]
bq EVSW Version = 0.9.79	
DeviceName = bq20z80 v1.10
Time = 7/31/2012 9:37:52 AM	


[Voltage(1st Level Safety)]
COV Threshold = 4300
COV Time = 2
COV Recovery = 4100
COV Delta = 20
COV Temp. Hys = 100
POV Threshold = 16800
POV Time = 5
POV Recovery = 16000
CUV Threshold = 2500
CUV Time = 2
CUV Recovery = 3000
PUV Threshold = 10400
PUV Time = 4
PUV Recovery = 12000
[Current(1st Level Safety)]
OC (1st Tier) Chg = 4000
OC (1st Tier) Chg Time = 2
OC Chg Recovery = 200
OC (1st Tier) Dsg = 6000
OC (1st Tier) Dsg Time = 5
OC Dsg Recovery = 200
OC (2nd Tier) Chg = 8000
OC (2nd Tier) Chg Time = 1
OC (2nd Tier) Dsg = 14000
OC (2nd Tier) Dsg Time = 0
Current Recovery Time = 8
AFE OC Dsg = 1F
AFE OC Dsg Time = 0F
AFE OC Dsg Recovery = 100
AFE SC Chg Cfg = 64
AFE SC Dsg Cfg = FF
AFE SC Recovery = 100
[Temperature(1st Level Safety)]
Over Temp Chg = 500
OT Chg Time = 2
OT Chg Recovery = 400
Over Temp Dsg = 600
OT Dsg Time = 2
OT Dsg Recovery = 550
[Host Comm(1st Level Safety)]
Host Watchdog Timeout = 0

[Voltage(2nd Level Safety)]
SOV Threshold = 17500
SOV Time = 10
Cell Imbalance Current = 100
Cell Imbalance Fail Voltage = 1000
Cell Imbalance Time = 4
Battery Rest Time = 1800
PFIN Detect Time = 0
[Current(2nd Level Safety)]
SOC Chg = 10000
SOC Chg Time = 4
SOC Dsg = 20000
SOC Dsg Time = 0
[Temperature(2nd Level Safety)]
SOT Chg = 800
SOT Chg Time = 30
SOT Dsg = 800
SOT Dsg Time = 30
Open Thermistor = -450
Open Time = 30
[FET Verification(2nd Level Safety)]
FET Fail Limit = 100
FET Fail Time = 1
[AFE Verification(2nd Level Safety)]
AFE Check Time = 30
AFE Fail Limit = 10
AFE Fail Recovery Time = 20
AFE Init Retry Limit = 6
AFE Init Limit = 20
[Fuse Verification(2nd Level Safety)]
Fuse Fail Limit = 2
Fuse Fail Time = 0

[Charge Inhibit Cfg(Charge Control)]
Chg Inhibit Temp Low = 0
Chg Inhibit Temp High = 450
Temp Hys = 20
[Pre-Charge Cfg(Charge Control)]
Pre-chg Current = 250
Pre-chg Temp = 50
Pre-chg Voltage = 3000
Recovery Voltage = 3100
[Fast Charge Cfg(Charge Control)]
Fast Charge Current = 2000
Charging Voltage = 16400
Delta Temp = 50
Suspend Low Temp = -25
Suspend High Temp = 500
[Pulse Charge Cfg(Charge Control)]
Turn ON Voltage = 4150
Turn OFF Voltage = 5000
Max ON Pulse Time = 240
Min OFF Pulse Time = 0
Max OFF Voltage = 5000
[Termination Cfg.(Charge Control)]
Maintenance Current = 0
Taper Current = 100
Termination Voltage = 300
Current Taper Window = 40
TCA Set % = -1
TCA Clear % = 95
FC Set % = -1
FC Clear % = 95
[Cell Balancing Cfg(Charge Control)]
Min Cell Deviation = 1750
[Charging Faults(Charge Control)]
Over Charging Voltage = 300
Over Charging Volt Time = 2
Over Charging Current = 1000
Over Charging Curr Time = 2
Over Charging Curr Recov = 100
Depleted Voltage = 7000
Depleted Voltage Time = 2
Depleted Recovery = 8500
Over Charge Capacity = 1000
Over Charge Recovery = 2
FC-MTO = 0
PC-MTO = 3600
Charge Fault Cfg = 0E

[Data(SBS Configuration)]
Rem Cap Alarm = 400
Rem Energy Alarm = 5760
Rem Time Alarm = 10
Init Battery Mode = 0081
Design Voltage = 14400
Spec Info = 0031
Manuf Date = 08-Oct-2009
Ser. Num. = 0895
Cycle Count = 214
CC Threshold = 3760
CC % = 100
CF MaxError Limit = 5
Design Capacity = 4176
Design Energy = 6000
Manuf Name = Nexergy Inc
Device Name = LI5032
Device Chemistry = LION
[Configuration(SBS Configuration)]
TDA Set % = 0
TDA Clear % = 15
FD Set % = 0
FD Clear % = 15
TDA Set Volt Threshold = 10000
TDA Set Volt Time = 5
TDA Clear Volt = 12600
FD Set Volt Threshold = 10000
FD Volt Time = 5
FD Clear Volt = 12600

[Manufacturer Data(System Data)]
Pack Lot Code = 0000
PCB Lot Code = 0CA5
Firmware Version = 1220
Hardware Revision = 0000
Cell Revision = 0000
[Manufacturer Info(System Data)]
Manuf. Info = 092209
[Lifetime Data(System Data)]
Lifetime Max Temp = 460
Lifetime Min Temp = 28
Lifetime Max Cell Voltage = 4303
Lifetime Min Cell Voltage = 2200
Lifetime Max Pack Voltage = 16482
Lifetime Min Pack Voltage = 11534
Lifetime Max Chg Current = 2001
Lifetime Max Dsg Current = -4796
Lifetime Max Chg Power = 3279
Lifetime Max Dsg Power = -5978
Life Max AvgDsg Cur = -2208
Life Max AvgDsg Pow = -3056
Lifetime Avg Temp = 287
[Lifetime Temp Samples(System Data)]
LT Temp Samples = 344935

[Registers(Configuration)]
Operation Cfg A = 0F31
Operation Cfg B = 6548
Operation Cfg C = 0000
Permanent Fail Cfg = 0000
Non-Removable Cfg = 0000

[LED Cfg(LED Support)]
LED Flash Rate = 512
LED Blink Rate = 1024
LED Delay = 100
LED Hold Time = 4
CHG Flash Alarm = 10
CHG Thresh 1 = 0
CHG Thresh 2 = 20
CHG Thresh 3 = 40
CHG Thresh 4 = 60
CHG Thresh 5 = 80
DSG Flash Alarm = 10
DSG Thresh 1 = 0
DSG Thresh 2 = 20
DSG Thresh 3 = 40
DSG Thresh 4 = 60
DSG Thresh 5 = 80

[Power(Power)]
Flash Update OK Voltage = 7500
Shutdown Voltage = 10000
Shutdown Time = 4
Charger Present = 3000
Sleep Current = 20
Bus Low Time = 5
Cal Inhibit Temp Low = 50
Cal Inhibit Temp High = 450
Sleep Voltage Time = 20
Sleep Current Time = 20

[IT Cfg(Gas Gauging)]
Load Select = 3
Load Mode = 1
Term Voltage = 12000
User Rate-mA = -2100
User Rate-mW = -30000
Reserve Cap-mAh = 100
Reserve Cap-mWh = 140
[Current Thresholds(Gas Gauging)]
Dsg Current Threshold = 50
Chg Current Threshold = 50
Quit Current = 20
Dsg Relax Time = 10
Chg Relax Time = 30
[State(Gas Gauging)]
Qmax Cell 0 = 4261
Qmax Cell 1 = 4367
Qmax Cell 2 = 4351
Qmax Cell 3 = 4322
Qmax Pack = 4261
Update Status = 06
Avg I Last Run = -1192
Avg P Last Run = -1779
Delta Voltage = 1794

[R_a0(Ra Table)]
Cell0 R_a flag = 0055
Cell0 R_a 0 = 181
Cell0 R_a 1 = 181
Cell0 R_a 2 = 284
Cell0 R_a 3 = 400
Cell0 R_a 4 = 435
Cell0 R_a 5 = 567
Cell0 R_a 6 = 753
Cell0 R_a 7 = 1321
Cell0 R_a 8 = 1499
Cell0 R_a 9 = 1390
Cell0 R_a 10 = 1319
Cell0 R_a 11 = 730
Cell0 R_a 12 = 1246
Cell0 R_a 13 = 3488
Cell0 R_a 14 = 3724
[R_a1(Ra Table)]
Cell1 R_a flag = 0000
Cell1 R_a 0 = 94
Cell1 R_a 1 = 94
Cell1 R_a 2 = 102
Cell1 R_a 3 = 111
Cell1 R_a 4 = 124
Cell1 R_a 5 = 119
Cell1 R_a 6 = 175
Cell1 R_a 7 = 311
Cell1 R_a 8 = 351
Cell1 R_a 9 = 354
Cell1 R_a 10 = 298
Cell1 R_a 11 = 148
Cell1 R_a 12 = 93
Cell1 R_a 13 = 341
Cell1 R_a 14 = 351
[R_a2(Ra Table)]
Cell2 R_a flag = 0000
Cell2 R_a 0 = 94
Cell2 R_a 1 = 94
Cell2 R_a 2 = 94
Cell2 R_a 3 = 104
Cell2 R_a 4 = 115
Cell2 R_a 5 = 104
Cell2 R_a 6 = 150
Cell2 R_a 7 = 250
Cell2 R_a 8 = 270
Cell2 R_a 9 = 268
Cell2 R_a 10 = 219
Cell2 R_a 11 = 101
Cell2 R_a 12 = 29
Cell2 R_a 13 = 112
Cell2 R_a 14 = 127
[R_a3(Ra Table)]
Cell3 R_a flag = 0055
Cell3 R_a 0 = 99
Cell3 R_a 1 = 99
Cell3 R_a 2 = 103
Cell3 R_a 3 = 109
Cell3 R_a 4 = 126
Cell3 R_a 5 = 114
Cell3 R_a 6 = 163
Cell3 R_a 7 = 289
Cell3 R_a 8 = 364
Cell3 R_a 9 = 360
Cell3 R_a 10 = 310
Cell3 R_a 11 = 189
Cell3 R_a 12 = 196
Cell3 R_a 13 = 640
Cell3 R_a 14 = 681
[R_a0x(Ra Table)]
xCell0 R_a flag = 0000
xCell0 R_a 0 = 181
xCell0 R_a 1 = 181
xCell0 R_a 2 = 284
xCell0 R_a 3 = 400
xCell0 R_a 4 = 435
xCell0 R_a 5 = 1076
xCell0 R_a 6 = 1429
xCell0 R_a 7 = 2507
xCell0 R_a 8 = 2845
xCell0 R_a 9 = 2637
xCell0 R_a 10 = 2503
xCell0 R_a 11 = 1385
xCell0 R_a 12 = 2365
xCell0 R_a 13 = 6619
xCell0 R_a 14 = 7067
[R_a1x(Ra Table)]
xCell1 R_a flag = 0055
xCell1 R_a 0 = 94
xCell1 R_a 1 = 94
xCell1 R_a 2 = 102
xCell1 R_a 3 = 111
xCell1 R_a 4 = 124
xCell1 R_a 5 = 113
xCell1 R_a 6 = 166
xCell1 R_a 7 = 295
xCell1 R_a 8 = 333
xCell1 R_a 9 = 336
xCell1 R_a 10 = 283
xCell1 R_a 11 = 141
xCell1 R_a 12 = 88
xCell1 R_a 13 = 324
xCell1 R_a 14 = 333
[R_a2x(Ra Table)]
xCell2 R_a flag = 0055
xCell2 R_a 0 = 94
xCell2 R_a 1 = 94
xCell2 R_a 2 = 94
xCell2 R_a 3 = 104
xCell2 R_a 4 = 115
xCell2 R_a 5 = 105
xCell2 R_a 6 = 151
xCell2 R_a 7 = 252
xCell2 R_a 8 = 273
xCell2 R_a 9 = 271
xCell2 R_a 10 = 221
xCell2 R_a 11 = 102
xCell2 R_a 12 = 29
xCell2 R_a 13 = 113
xCell2 R_a 14 = 128
[R_a3x(Ra Table)]
xCell3 R_a flag = 0000
xCell3 R_a 0 = 99
xCell3 R_a 1 = 99
xCell3 R_a 2 = 103
xCell3 R_a 3 = 109
xCell3 R_a 4 = 126
xCell3 R_a 5 = 109
xCell3 R_a 6 = 156
xCell3 R_a 7 = 276
xCell3 R_a 8 = 348
xCell3 R_a 9 = 344
xCell3 R_a 10 = 296
xCell3 R_a 11 = 181
xCell3 R_a 12 = 187
xCell3 R_a 13 = 612
xCell3 R_a 14 = 651

[Device Status Data(PF Status)]
PF Flags 1 = 0000
Fuse Flag = 0000
PF Voltage = 0
PF C4 Voltage = 0
PF C3 Voltage = 0
PF C2 Voltage = 0
PF C1 Voltage = 0
PF Current = 0
PF Temperature = 0
PF Batt Stat = 0000
PF RC-mAh = 0
PF RC-10mWh = 0
PF Chg Status = 0000
PF Safety Status = 0000
PF Flags 2 = 0000
[AFE Regs(PF Status)]
AFE Status = 00
AFE Output = 08
AFE State = 00
AFE Function = 00
AFE Cell Select = 00
AFE OLV = 1F
AFE OLT = 0F
AFE SCC = 64
AFE SCD = FF

[Data(Calibration)]
CC Gain = 0.9318
CC Delta = 277923.9062
Ref Voltage = 2452.7
AFE Corr = 1288
AFE Pack Gain = 30625
CC Offset = -12141
Board Offset = 18
Int Temp Offset = -34
Ext1 Temp Offset = -8
Ext2 Temp Offset = -10
[Config(Calibration)]
CC Current = 3000
Voltage Signal = 16800
Temp Signal = 298.0
CC Offset Time = 250
ADC Offset Time = 32
CC Gain Time = 250
Voltage Time = 1984
Temperature Time = 32
Cal Mode Timeout = 38400
[Temp Model(Calibration)]
Ext Coef 1 = -28285
Ext Coef 2 = 20848
Ext Coef 3 = -7537
Ext Coef 4 = 4012
Ext Min AD = 0
Ext Max Temp = 4012
Int Coef 1 = 0
Int Coef 2 = 0
Int Coef 3 = -11136
Int Coef 4 = 5754
Int Min AD = 0
Int Max Temp = 5754
[Current(Calibration)]
Filter = 239
Deadband = 3
CC Deadband = 34
CC Max Deadband = 5
CC Deadband Sample = 256
CC Max Offset Sample = 64
