Product ID=2c, Serial#=TV110102228, SWVersion=10.2, HWVersion=0
---------------------------------------------------------------
LOG ID 17 (Encrypted Significant Event Text) 165316 total bytes
---------------------------------------------------------------
     UTC Time             Tril Time        Err              Descr
04/16/2012 12:10:19  04/16/2012 12:10:19   282     0 65535  ERR_INT_LI_ION_DEPLETED  HIGH_ALARM  <UTC:1334578219_17>
04/16/2012 12:10:19  04/16/2012 12:10:19   196     0 65535  ERR_BATT_LOW_STATE_OF_HEALTH_DET_LI_ION  LOW_ALARM  <UTC:1334578219_17>
04/16/2012 12:10:17  04/16/2012 12:10:17    72     0 65535  ERR_MMC_SD_CARD_INSERTED  BEEP_ONLY  <UTC:1334578217_17>
04/16/2012 12:10:17  04/16/2012 12:10:17   252     0 65535  ERR_INT_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1334578217_17>
04/16/2012 12:10:17  04/16/2012 12:10:17   251     0 65535  ERR_DET_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1334578217_17>
04/15/2012 08:15:30  04/15/2012 08:15:30   282     0 65535  ERR_INT_LI_ION_DEPLETED  HIGH_ALARM  <UTC:1334477730_17>
04/15/2012 08:15:30  04/15/2012 08:15:30   187     0 65535  ERR_LAST_BATT_DET_LI_ION_NEARLY_DEPLETED  HIGH_ALARM  <UTC:1334477730_17>
04/15/2012 08:15:30  04/15/2012 08:15:30   196     0 65535  ERR_BATT_LOW_STATE_OF_HEALTH_DET_LI_ION  LOW_ALARM  <UTC:1334477730_17>
04/15/2012 08:15:28  04/15/2012 08:15:28    72     0 65535  ERR_MMC_SD_CARD_INSERTED  BEEP_ONLY  <UTC:1334477728_17>
04/15/2012 08:15:28  04/15/2012 08:15:28   252     0 65535  ERR_INT_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1334477728_17>
04/15/2012 08:15:28  04/15/2012 08:15:28   251     0 65535  ERR_DET_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1334477728_17>
04/10/2012 03:41:10  04/10/2012 03:41:10   282     0 65535  ERR_INT_LI_ION_DEPLETED  HIGH_ALARM  <UTC:1334029270_17>
04/10/2012 03:41:10  04/10/2012 03:41:10   187     0 65535  ERR_LAST_BATT_DET_LI_ION_NEARLY_DEPLETED  HIGH_ALARM  <UTC:1334029270_17>
04/10/2012 03:41:10  04/10/2012 03:41:10   196     0 65535  ERR_BATT_LOW_STATE_OF_HEALTH_DET_LI_ION  LOW_ALARM  <UTC:1334029270_17>
04/10/2012 03:41:08  04/10/2012 03:41:08    72     0 65535  ERR_MMC_SD_CARD_INSERTED  BEEP_ONLY  <UTC:1334029268_17>
04/10/2012 03:41:08  04/10/2012 03:41:08   252     0 65535  ERR_INT_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1334029268_17>
04/10/2012 03:41:08  04/10/2012 03:41:08   251     0 65535  ERR_DET_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1334029268_17>
04/06/2012 16:54:16  04/06/2012 16:54:16   282     0 65535  ERR_INT_LI_ION_DEPLETED  HIGH_ALARM  <UTC:1333731256_17>
04/06/2012 16:54:16  04/06/2012 16:54:16   187     0 65535  ERR_LAST_BATT_DET_LI_ION_NEARLY_DEPLETED  HIGH_ALARM  <UTC:1333731256_17>
04/06/2012 16:54:16  04/06/2012 16:54:16   196     0 65535  ERR_BATT_LOW_STATE_OF_HEALTH_DET_LI_ION  LOW_ALARM  <UTC:1333731256_17>
04/06/2012 16:54:14  04/06/2012 16:54:14    72     0 65535  ERR_MMC_SD_CARD_INSERTED  BEEP_ONLY  <UTC:1333731254_17>
04/06/2012 16:54:14  04/06/2012 16:54:14   252     0 65535  ERR_INT_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1333731254_17>
04/06/2012 16:54:14  04/06/2012 16:54:14   251     0 65535  ERR_DET_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1333731254_17>
04/04/2012 11:37:30  04/04/2012 11:37:30   282     0 65535  ERR_INT_LI_ION_DEPLETED  HIGH_ALARM  <UTC:1333539450_17>
04/04/2012 11:37:30  04/04/2012 11:37:30   187     0 65535  ERR_LAST_BATT_DET_LI_ION_NEARLY_DEPLETED  HIGH_ALARM  <UTC:1333539450_17>
04/04/2012 11:37:30  04/04/2012 11:37:30   196     0 65535  ERR_BATT_LOW_STATE_OF_HEALTH_DET_LI_ION  LOW_ALARM  <UTC:1333539450_17>
04/04/2012 11:37:28  04/04/2012 11:37:28    72     0 65535  ERR_MMC_SD_CARD_INSERTED  BEEP_ONLY  <UTC:1333539448_17>
04/04/2012 11:37:28  04/04/2012 11:37:28   252     0 65535  ERR_INT_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1333539448_17>
04/04/2012 11:37:28  04/04/2012 11:37:28   251     0 65535  ERR_DET_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1333539448_17>
01/30/2012 10:08:56  01/30/2012 10:08:56   179     0 65535  ERR_PWR_REDUCTION_AC_DISCONNECTED  MED_ALARM  <UTC:1327918136_17>
01/30/2012 10:01:54  01/30/2012 10:01:54 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1327917714_17>
01/30/2012 10:01:39  01/30/2012 10:01:39 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1327917699_17>
01/30/2012 10:01:39  01/30/2012 10:01:39   324     4 65535  ERR_POWER_ON  KEYPRESS  <UTC:1327917699_17>
01/30/2012 09:57:54  01/30/2012 09:57:54 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1327917474_17>
01/30/2012 09:57:39  01/30/2012 09:57:39 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1327917459_17>
01/30/2012 09:57:39  01/30/2012 09:57:39   324     4 65535  ERR_POWER_ON  KEYPRESS  <UTC:1327917459_17>
01/30/2012 09:57:39  01/30/2012 09:57:39 16418     2     3      NV_ID= 34 (NV_RX_MODE)  P/S=P RX=0  AVAPS=0  <UTC:1327917459_17>
01/30/2012 09:56:49  01/30/2012 09:56:49    72     0 65535  ERR_MMC_SD_CARD_INSERTED  BEEP_ONLY  <UTC:1327917409_17>
01/30/2012 09:56:49  01/30/2012 09:56:49   252     0 65535  ERR_INT_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1327917409_17>
01/30/2012 09:56:49  01/30/2012 09:56:49   251     0 65535  ERR_DET_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1327917409_17>
01/19/2012 13:16:16  01/19/2012 13:16:16   179     0 65535  ERR_PWR_REDUCTION_AC_DISCONNECTED  MED_ALARM  <UTC:1326978976_17>
01/19/2012 13:16:03  01/19/2012 13:16:03   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326978963_17>
01/19/2012 13:16:00  01/19/2012 13:16:00   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326978960_17>
01/19/2012 13:15:58  01/19/2012 13:15:58   167     0 65535  ERR_UI_HIDE_KEY_PRESS  KEYPRESS  <UTC:1326978958_17>
01/19/2012 13:15:58  01/19/2012 13:15:58   110     0     5  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1326978958_17>
01/19/2012 13:15:57  01/19/2012 13:15:57   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326978957_17>
01/19/2012 13:15:57  01/19/2012 13:15:57   165  6491     6  ERR_LOW_PEP_ALARM  HIGH_ALARM  <UTC:1326978957_17>
01/19/2012 13:15:55  01/19/2012 13:15:55   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326978955_17>
01/19/2012 13:13:03  01/19/2012 13:13:03 17707   550   525      NV_ID= 43 (NV_TIDAL_VOLUME)  P/S=P RX=2  AVAPS=1  <UTC:1326978783_17>
01/19/2012 13:11:05  01/19/2012 13:11:05   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1326978665_17>
01/19/2012 13:08:56  01/19/2012 13:08:56   167     0 65535  ERR_UI_HIDE_KEY_PRESS  KEYPRESS  <UTC:1326978536_17>
01/19/2012 13:08:47  01/19/2012 13:08:47   118     0    12  ERR_LOW_CIRCUIT_LEAK_ALARM  HIGH_ALARM  <UTC:1326978527_17>
01/19/2012 13:08:30  01/19/2012 13:08:30 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326978510_17>
01/19/2012 13:08:30  01/19/2012 13:08:30   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326978510_17>
01/19/2012 13:08:29  01/19/2012 13:08:29 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326978509_17>
01/19/2012 13:08:29  01/19/2012 13:08:29   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326978509_17>
01/19/2012 13:08:27  01/19/2012 13:08:27   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326978507_17>
01/19/2012 13:08:19  01/19/2012 13:08:19   110     0     4  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1326978499_17>
01/19/2012 13:08:18  01/19/2012 13:08:18   165  6490     4  ERR_LOW_PEP_ALARM  HIGH_ALARM  <UTC:1326978498_17>
01/19/2012 13:08:13  01/19/2012 13:08:13 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326978493_17>
01/19/2012 13:08:13  01/19/2012 13:08:13   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326978493_17>
01/19/2012 13:08:05  01/19/2012 13:08:05 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326978485_17>
01/19/2012 13:08:05  01/19/2012 13:08:05   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326978485_17>
01/19/2012 13:07:58  01/19/2012 13:07:58   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326978478_17>
01/19/2012 13:07:34  01/19/2012 13:07:34   165  6490    31  ERR_LOW_PEP_ALARM  HIGH_ALARM  <UTC:1326978454_17>
01/19/2012 13:07:34  01/19/2012 13:07:34   167     0 65535  ERR_UI_HIDE_KEY_PRESS  KEYPRESS  <UTC:1326978454_17>
01/19/2012 13:07:31  01/19/2012 13:07:31   110     0    34  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1326978451_17>
01/19/2012 13:07:31  01/19/2012 13:07:31   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1326978451_17>
01/19/2012 13:07:27  01/19/2012 13:07:27   110     0     4  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1326978447_17>
01/19/2012 13:07:26  01/19/2012 13:07:26   165  6484     5  ERR_LOW_PEP_ALARM  HIGH_ALARM  <UTC:1326978446_17>
01/19/2012 13:07:21  01/19/2012 13:07:21 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326978441_17>
01/19/2012 13:07:21  01/19/2012 13:07:21   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326978441_17>
01/19/2012 13:07:16  01/19/2012 13:07:16    72     0 65535  ERR_MMC_SD_CARD_INSERTED  BEEP_ONLY  <UTC:1326978436_17>
01/19/2012 13:07:16  01/19/2012 13:07:16   252     0 65535  ERR_INT_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1326978436_17>
01/19/2012 13:07:16  01/19/2012 13:07:16   251     0 65535  ERR_DET_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1326978436_17>
01/17/2012 07:33:55  01/17/2012 07:33:55   179     0 65535  ERR_PWR_REDUCTION_AC_DISCONNECTED  MED_ALARM  <UTC:1326785635_17>
01/17/2012 07:17:02  01/17/2012 07:17:02 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326784622_17>
01/17/2012 07:17:02  01/17/2012 07:17:02   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326784622_17>
01/17/2012 07:17:02  01/17/2012 07:17:02   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326784622_17>
01/16/2012 23:27:46  01/16/2012 23:27:46 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326756466_17>
01/16/2012 23:27:46  01/16/2012 23:27:46   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326756466_17>
01/16/2012 23:27:14  01/16/2012 23:27:14 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326756434_17>
01/16/2012 23:27:14  01/16/2012 23:27:14   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326756434_17>
01/16/2012 23:27:13  01/16/2012 23:27:13   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326756433_17>
01/16/2012 23:12:01  01/16/2012 23:12:01 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326755521_17>
01/16/2012 23:12:01  01/16/2012 23:12:01   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326755521_17>
01/16/2012 23:11:53  01/16/2012 23:11:53 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326755513_17>
01/16/2012 23:11:53  01/16/2012 23:11:53   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326755513_17>
01/16/2012 23:11:51  01/16/2012 23:11:51   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326755511_17>
01/16/2012 20:55:42  01/16/2012 20:55:42 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326747342_17>
01/16/2012 20:55:42  01/16/2012 20:55:42   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326747342_17>
01/16/2012 20:52:09  01/16/2012 20:52:09 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326747129_17>
01/16/2012 20:52:09  01/16/2012 20:52:09   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326747129_17>
01/16/2012 20:52:08  01/16/2012 20:52:08   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326747128_17>
01/16/2012 20:26:37  01/16/2012 20:26:37 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326745597_17>
01/16/2012 20:26:37  01/16/2012 20:26:37   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326745597_17>
01/16/2012 20:24:49  01/16/2012 20:24:49 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326745489_17>
01/16/2012 20:24:49  01/16/2012 20:24:49   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326745489_17>
01/16/2012 20:24:48  01/16/2012 20:24:48   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326745488_17>
01/16/2012 19:34:38  01/16/2012 19:34:38 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326742478_17>
01/16/2012 19:34:38  01/16/2012 19:34:38   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326742478_17>
01/16/2012 19:23:53  01/16/2012 19:23:53 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326741833_17>
01/16/2012 19:23:52  01/16/2012 19:23:52   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326741832_17>
01/16/2012 19:23:52  01/16/2012 19:23:52   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326741832_17>
01/16/2012 18:51:58  01/16/2012 18:51:58 17702   700   800      NV_ID= 38 (NV_EPAP_PEEP_CPAP_PRESSURE)  P/S=P RX=2  AVAPS=1  <UTC:1326739918_17>
01/16/2012 18:51:14  01/16/2012 18:51:14 17702   500   700      NV_ID= 38 (NV_EPAP_PEEP_CPAP_PRESSURE)  P/S=P RX=2  AVAPS=1  <UTC:1326739874_17>
01/16/2012 18:10:00  01/16/2012 18:10:00   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326737400_17>
01/16/2012 18:08:46  01/16/2012 18:08:46   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326737326_17>
01/16/2012 18:08:46  01/16/2012 18:08:46   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326737326_17>
01/16/2012 18:07:33  01/16/2012 18:07:33   110     4     8  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1326737253_17>
01/16/2012 17:52:50  01/16/2012 17:52:50   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326736370_17>
01/16/2012 17:51:52  01/16/2012 17:51:52   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326736312_17>
01/16/2012 17:51:51  01/16/2012 17:51:51   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326736311_17>
01/16/2012 16:20:17  01/16/2012 16:20:17   110     0    39  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1326730817_17>
01/16/2012 16:20:16  01/16/2012 16:20:16   165  6500    38  ERR_LOW_PEP_ALARM  HIGH_ALARM  <UTC:1326730816_17>
01/16/2012 12:22:19  01/16/2012 12:22:19   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326716539_17>
01/16/2012 12:19:50  01/16/2012 12:19:50   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326716390_17>
01/16/2012 12:19:49  01/16/2012 12:19:49   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326716389_17>
01/16/2012 10:51:46  01/16/2012 10:51:46   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326711106_17>
01/16/2012 10:51:05  01/16/2012 10:51:05   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326711065_17>
01/16/2012 10:51:05  01/16/2012 10:51:05   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326711065_17>
01/16/2012 10:51:04  01/16/2012 10:51:04   165  6500     1  ERR_LOW_PEP_ALARM  HIGH_ALARM  <UTC:1326711064_17>
01/16/2012 10:51:03  01/16/2012 10:51:03   167     0 65535  ERR_UI_HIDE_KEY_PRESS  KEYPRESS  <UTC:1326711063_17>
01/16/2012 10:51:02  01/16/2012 10:51:02   110    43     3  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1326711062_17>
01/16/2012 10:51:02  01/16/2012 10:51:02   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326711062_17>
01/16/2012 10:10:53  01/16/2012 10:10:53 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326708653_17>
01/16/2012 10:10:53  01/16/2012 10:10:53   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326708653_17>
01/16/2012 10:10:45  01/16/2012 10:10:45 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326708645_17>
01/16/2012 10:10:45  01/16/2012 10:10:45   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326708645_17>
01/16/2012 10:10:43  01/16/2012 10:10:43   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326708643_17>
01/16/2012 09:33:27  01/16/2012 09:33:27 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326706407_17>
01/16/2012 09:33:27  01/16/2012 09:33:27   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326706407_17>
01/16/2012 09:11:25  01/16/2012 09:11:25 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326705085_17>
01/16/2012 09:11:25  01/16/2012 09:11:25   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326705085_17>
01/16/2012 09:11:25  01/16/2012 09:11:25   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326705085_17>
01/16/2012 07:47:14  01/16/2012 07:47:14 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326700034_17>
01/16/2012 07:47:14  01/16/2012 07:47:14   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326700034_17>
01/16/2012 07:44:36  01/16/2012 07:44:36 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326699876_17>
01/16/2012 07:44:35  01/16/2012 07:44:35   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326699875_17>
01/16/2012 07:44:35  01/16/2012 07:44:35   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326699875_17>
01/16/2012 07:18:56  01/16/2012 07:18:56 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326698336_17>
01/16/2012 07:18:56  01/16/2012 07:18:56   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326698336_17>
01/16/2012 07:17:09  01/16/2012 07:17:09 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326698229_17>
01/16/2012 07:17:09  01/16/2012 07:17:09   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326698229_17>
01/16/2012 07:17:08  01/16/2012 07:17:08   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326698228_17>
01/15/2012 23:55:12  01/15/2012 23:55:12 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326671712_17>
01/15/2012 23:55:11  01/15/2012 23:55:11   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326671711_17>
01/15/2012 23:44:55  01/15/2012 23:44:55 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326671095_17>
01/15/2012 23:44:55  01/15/2012 23:44:55   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326671095_17>
01/15/2012 23:44:54  01/15/2012 23:44:54   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326671094_17>
01/15/2012 23:24:36  01/15/2012 23:24:36 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326669876_17>
01/15/2012 23:24:36  01/15/2012 23:24:36   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326669876_17>
01/15/2012 23:20:18  01/15/2012 23:20:18 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326669618_17>
01/15/2012 23:20:18  01/15/2012 23:20:18   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326669618_17>
01/15/2012 23:20:17  01/15/2012 23:20:17   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326669617_17>
01/15/2012 23:19:26  01/15/2012 23:19:26 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326669566_17>
01/15/2012 23:19:26  01/15/2012 23:19:26   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326669566_17>
01/15/2012 23:16:10  01/15/2012 23:16:10 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326669370_17>
01/15/2012 23:16:10  01/15/2012 23:16:10   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326669370_17>
01/15/2012 23:16:08  01/15/2012 23:16:08   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326669368_17>
01/15/2012 21:25:17  01/15/2012 21:25:17 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326662717_17>
01/15/2012 21:25:17  01/15/2012 21:25:17   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326662717_17>
01/15/2012 21:25:07  01/15/2012 21:25:07 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326662707_17>
01/15/2012 21:25:07  01/15/2012 21:25:07   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326662707_17>
01/15/2012 21:25:06  01/15/2012 21:25:06   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326662706_17>
01/15/2012 21:25:04  01/15/2012 21:25:04   295     0 65535  ERR_POWER_OFF_NO_KEY  KEYPRESS  <UTC:1326662704_17>
01/15/2012 21:25:02  01/15/2012 21:25:02   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326662702_17>
01/15/2012 20:56:53  01/15/2012 20:56:53 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326661013_17>
01/15/2012 20:56:53  01/15/2012 20:56:53   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326661013_17>
01/15/2012 20:54:37  01/15/2012 20:54:37 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326660877_17>
01/15/2012 20:54:37  01/15/2012 20:54:37   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326660877_17>
01/15/2012 20:54:37  01/15/2012 20:54:37   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326660877_17>
01/15/2012 19:13:53  01/15/2012 19:13:53 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326654833_17>
01/15/2012 19:13:53  01/15/2012 19:13:53   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326654833_17>
01/15/2012 18:56:47  01/15/2012 18:56:47 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326653807_17>
01/15/2012 18:56:47  01/15/2012 18:56:47   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326653807_17>
01/15/2012 18:56:46  01/15/2012 18:56:46   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326653806_17>
01/15/2012 18:43:00  01/15/2012 18:43:00 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326652980_17>
01/15/2012 18:43:00  01/15/2012 18:43:00   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326652980_17>
01/15/2012 18:35:03  01/15/2012 18:35:03 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326652503_17>
01/15/2012 18:35:03  01/15/2012 18:35:03   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326652503_17>
01/15/2012 18:35:03  01/15/2012 18:35:03   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326652503_17>
01/15/2012 16:55:24  01/15/2012 16:55:24 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326646524_17>
01/15/2012 16:55:24  01/15/2012 16:55:24   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326646524_17>
01/15/2012 16:54:10  01/15/2012 16:54:10 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326646450_17>
01/15/2012 16:54:09  01/15/2012 16:54:09   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326646449_17>
01/15/2012 16:54:08  01/15/2012 16:54:08   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326646448_17>
01/15/2012 16:52:27  01/15/2012 16:52:27 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326646347_17>
01/15/2012 16:52:27  01/15/2012 16:52:27   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326646347_17>
01/15/2012 16:47:03  01/15/2012 16:47:03 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326646023_17>
01/15/2012 16:47:03  01/15/2012 16:47:03   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326646023_17>
01/15/2012 16:47:02  01/15/2012 16:47:02   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326646022_17>
01/15/2012 16:31:07  01/15/2012 16:31:07 17708    14    15      NV_ID= 44 (NV_BREATH_RATE)  P/S=P RX=2  AVAPS=1  <UTC:1326645067_17>
01/15/2012 16:31:04  01/15/2012 16:31:04 17708    15    14      NV_ID= 44 (NV_BREATH_RATE)  P/S=P RX=2  AVAPS=1  <UTC:1326645064_17>
01/15/2012 16:30:59  01/15/2012 16:30:59 17702   700   500      NV_ID= 38 (NV_EPAP_PEEP_CPAP_PRESSURE)  P/S=P RX=2  AVAPS=1  <UTC:1326645059_17>
01/15/2012 16:30:57  01/15/2012 16:30:57 17701  2000  1800      NV_ID= 37 (NV_IPAP_PRESSURE)  P/S=P RX=2  AVAPS=1  <UTC:1326645057_17>
01/15/2012 16:30:56  01/15/2012 16:30:56 17700  2600  2200      NV_ID= 36 (NV_IPAP_MAX_PRESSURE)  P/S=P RX=2  AVAPS=1  <UTC:1326645056_17>
01/15/2012 16:26:01  01/15/2012 16:26:01 17701  1800  2000      NV_ID= 37 (NV_IPAP_PRESSURE)  P/S=P RX=2  AVAPS=1  <UTC:1326644761_17>
01/15/2012 16:25:56  01/15/2012 16:25:56 17700  2400  2600      NV_ID= 36 (NV_IPAP_MAX_PRESSURE)  P/S=P RX=2  AVAPS=1  <UTC:1326644756_17>
01/15/2012 16:23:27  01/15/2012 16:23:27 17700  2200  2400      NV_ID= 36 (NV_IPAP_MAX_PRESSURE)  P/S=P RX=2  AVAPS=1  <UTC:1326644607_17>
01/15/2012 16:18:41  01/15/2012 16:18:41 17702   500   700      NV_ID= 38 (NV_EPAP_PEEP_CPAP_PRESSURE)  P/S=P RX=2  AVAPS=1  <UTC:1326644321_17>
01/15/2012 15:31:24  01/15/2012 15:31:24 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326641484_17>
01/15/2012 15:31:24  01/15/2012 15:31:24   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326641484_17>
01/15/2012 15:26:17  01/15/2012 15:26:17 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326641177_17>
01/15/2012 15:26:17  01/15/2012 15:26:17   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326641177_17>
01/15/2012 15:26:16  01/15/2012 15:26:16   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326641176_17>
01/15/2012 14:02:40  01/15/2012 14:02:40 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326636160_17>
01/15/2012 14:02:40  01/15/2012 14:02:40   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326636160_17>
01/15/2012 13:57:27  01/15/2012 13:57:27 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326635847_17>
01/15/2012 13:57:27  01/15/2012 13:57:27   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326635847_17>
01/15/2012 13:57:26  01/15/2012 13:57:26   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326635846_17>
01/15/2012 13:43:14  01/15/2012 13:43:14   284     0 65535  ERR_PWR_UPGRADE_AC_IN_USE  BEEP_ONLY  <UTC:1326634994_17>
01/15/2012 13:40:36  01/15/2012 13:40:36   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1326634836_17>
01/15/2012 13:40:02  01/15/2012 13:40:02   281     0 65535  ERR_PWR_REDUCTION_DET_LI_ION_DEPLETED  INFO_ALARM  <UTC:1326634802_17>
01/15/2012 12:09:54  01/15/2012 12:09:54   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1326629394_17>
01/15/2012 11:11:53  01/15/2012 11:11:53   173     0 65535  ERR_START_ON_BATTERY  INFO_ALARM  <UTC:1326625913_17>
01/15/2012 11:11:50  01/15/2012 11:11:50 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326625910_17>
01/15/2012 11:11:50  01/15/2012 11:11:50   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326625910_17>
01/15/2012 11:10:56  01/15/2012 11:10:56 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326625856_17>
01/15/2012 11:10:56  01/15/2012 11:10:56   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326625856_17>
01/15/2012 11:10:56  01/15/2012 11:10:56   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326625856_17>
01/15/2012 11:10:17  01/15/2012 11:10:17   173     0 65535  ERR_START_ON_BATTERY  INFO_ALARM  <UTC:1326625817_17>
01/15/2012 11:10:14  01/15/2012 11:10:14 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326625814_17>
01/15/2012 11:10:14  01/15/2012 11:10:14   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326625814_17>
01/15/2012 11:05:47  01/15/2012 11:05:47 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326625547_17>
01/15/2012 11:05:47  01/15/2012 11:05:47   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326625547_17>
01/15/2012 11:05:42  01/15/2012 11:05:42   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326625542_17>
01/15/2012 10:48:19  01/15/2012 10:48:19   110     0     4  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1326624499_17>
01/15/2012 10:48:18  01/15/2012 10:48:18   165  6500     4  ERR_LOW_PEP_ALARM  HIGH_ALARM  <UTC:1326624498_17>
01/15/2012 10:08:17  01/15/2012 10:08:17   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1326622097_17>
01/15/2012 10:05:47  01/15/2012 10:05:47   179     0 65535  ERR_PWR_REDUCTION_AC_DISCONNECTED  MED_ALARM  <UTC:1326621947_17>
01/15/2012 10:05:39  01/15/2012 10:05:39   110     0     4  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1326621939_17>
01/15/2012 10:05:38  01/15/2012 10:05:38   165  6501     4  ERR_LOW_PEP_ALARM  HIGH_ALARM  <UTC:1326621938_17>
01/15/2012 09:46:05  01/15/2012 09:46:05   110     2     4  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1326620765_17>
01/15/2012 08:09:41  01/15/2012 08:09:41 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326614981_17>
01/15/2012 08:09:41  01/15/2012 08:09:41   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326614981_17>
01/15/2012 08:07:05  01/15/2012 08:07:05 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326614825_17>
01/15/2012 08:07:05  01/15/2012 08:07:05   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326614825_17>
01/15/2012 08:07:04  01/15/2012 08:07:04   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326614824_17>
01/15/2012 07:53:45  01/15/2012 07:53:45 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326614025_17>
01/15/2012 07:53:45  01/15/2012 07:53:45   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326614025_17>
01/15/2012 07:32:44  01/15/2012 07:32:44 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326612764_17>
01/15/2012 07:32:44  01/15/2012 07:32:44   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326612764_17>
01/15/2012 07:32:43  01/15/2012 07:32:43   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326612763_17>
01/15/2012 07:03:21  01/15/2012 07:03:21 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326611001_17>
01/15/2012 07:03:21  01/15/2012 07:03:21   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326611001_17>
01/15/2012 06:55:51  01/15/2012 06:55:51 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326610551_17>
01/15/2012 06:55:51  01/15/2012 06:55:51   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326610551_17>
01/15/2012 06:55:49  01/15/2012 06:55:49   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326610549_17>
01/15/2012 06:09:02  01/15/2012 06:09:02 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326607742_17>
01/15/2012 06:09:02  01/15/2012 06:09:02   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326607742_17>
01/15/2012 06:01:39  01/15/2012 06:01:39 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326607299_17>
01/15/2012 06:01:39  01/15/2012 06:01:39   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326607299_17>
01/15/2012 06:01:38  01/15/2012 06:01:38   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326607298_17>
01/15/2012 05:07:27  01/15/2012 05:07:27 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326604047_17>
01/15/2012 05:07:27  01/15/2012 05:07:27   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326604047_17>
01/15/2012 05:04:46  01/15/2012 05:04:46 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326603886_17>
01/15/2012 05:04:46  01/15/2012 05:04:46   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326603886_17>
01/15/2012 05:04:45  01/15/2012 05:04:45   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326603885_17>
01/15/2012 04:43:16  01/15/2012 04:43:16 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326602596_17>
01/15/2012 04:43:16  01/15/2012 04:43:16   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326602596_17>
01/15/2012 04:37:16  01/15/2012 04:37:16 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326602236_17>
01/15/2012 04:37:16  01/15/2012 04:37:16   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326602236_17>
01/15/2012 04:37:14  01/15/2012 04:37:14   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326602234_17>
01/15/2012 03:48:38  01/15/2012 03:48:38 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326599318_17>
01/15/2012 03:48:38  01/15/2012 03:48:38   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326599318_17>
01/15/2012 03:32:43  01/15/2012 03:32:43 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326598363_17>
01/15/2012 03:32:43  01/15/2012 03:32:43   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326598363_17>
01/15/2012 03:32:42  01/15/2012 03:32:42   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326598362_17>
01/15/2012 00:55:04  01/15/2012 00:55:04 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326588904_17>
01/15/2012 00:55:04  01/15/2012 00:55:04   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326588904_17>
01/15/2012 00:43:46  01/15/2012 00:43:46 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326588226_17>
01/15/2012 00:43:46  01/15/2012 00:43:46   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326588226_17>
01/15/2012 00:43:45  01/15/2012 00:43:45   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326588225_17>
01/14/2012 23:10:30  01/14/2012 23:10:30 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326582630_17>
01/14/2012 23:10:30  01/14/2012 23:10:30   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326582630_17>
01/14/2012 23:10:11  01/14/2012 23:10:11 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326582611_17>
01/14/2012 23:10:11  01/14/2012 23:10:11   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326582611_17>
01/14/2012 23:10:10  01/14/2012 23:10:10   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326582610_17>
01/14/2012 23:09:34  01/14/2012 23:09:34 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326582574_17>
01/14/2012 23:09:34  01/14/2012 23:09:34   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326582574_17>
01/14/2012 23:06:10  01/14/2012 23:06:10 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326582370_17>
01/14/2012 23:06:10  01/14/2012 23:06:10   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326582370_17>
01/14/2012 23:06:09  01/14/2012 23:06:09   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326582369_17>
01/14/2012 21:21:14  01/14/2012 21:21:14 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326576074_17>
01/14/2012 21:21:13  01/14/2012 21:21:13   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326576073_17>
01/14/2012 21:12:51  01/14/2012 21:12:51 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326575571_17>
01/14/2012 21:12:51  01/14/2012 21:12:51   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326575571_17>
01/14/2012 21:12:51  01/14/2012 21:12:51   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326575571_17>
01/14/2012 21:05:41  01/14/2012 21:05:41 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326575141_17>
01/14/2012 21:05:41  01/14/2012 21:05:41   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326575141_17>
01/14/2012 20:59:13  01/14/2012 20:59:13 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326574753_17>
01/14/2012 20:59:13  01/14/2012 20:59:13   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326574753_17>
01/14/2012 20:59:11  01/14/2012 20:59:11   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326574751_17>
01/14/2012 19:37:52  01/14/2012 19:37:52 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326569872_17>
01/14/2012 19:37:51  01/14/2012 19:37:51   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326569871_17>
01/14/2012 19:37:40  01/14/2012 19:37:40 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326569860_17>
01/14/2012 19:37:40  01/14/2012 19:37:40   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326569860_17>
01/14/2012 19:37:39  01/14/2012 19:37:39   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326569859_17>
01/14/2012 19:37:23  01/14/2012 19:37:23 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326569843_17>
01/14/2012 19:37:23  01/14/2012 19:37:23   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326569843_17>
01/14/2012 19:33:42  01/14/2012 19:33:42 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326569622_17>
01/14/2012 19:33:42  01/14/2012 19:33:42   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326569622_17>
01/14/2012 19:33:41  01/14/2012 19:33:41   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326569621_17>
01/14/2012 19:14:05  01/14/2012 19:14:05 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326568445_17>
01/14/2012 19:14:05  01/14/2012 19:14:05   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326568445_17>
01/14/2012 19:12:33  01/14/2012 19:12:33 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326568353_17>
01/14/2012 19:12:33  01/14/2012 19:12:33   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326568353_17>
01/14/2012 19:12:32  01/14/2012 19:12:32   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326568352_17>
01/14/2012 19:08:18  01/14/2012 19:08:18 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326568098_17>
01/14/2012 19:08:18  01/14/2012 19:08:18   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326568098_17>
01/14/2012 19:05:06  01/14/2012 19:05:06 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326567906_17>
01/14/2012 19:05:06  01/14/2012 19:05:06   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326567906_17>
01/14/2012 19:05:05  01/14/2012 19:05:05   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326567905_17>
01/14/2012 18:14:46  01/14/2012 18:14:46 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326564886_17>
01/14/2012 18:14:46  01/14/2012 18:14:46   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326564886_17>
01/14/2012 18:05:36  01/14/2012 18:05:36 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326564336_17>
01/14/2012 18:05:36  01/14/2012 18:05:36   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326564336_17>
01/14/2012 18:05:35  01/14/2012 18:05:35   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326564335_17>
01/14/2012 17:33:21  01/14/2012 17:33:21 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326562401_17>
01/14/2012 17:33:21  01/14/2012 17:33:21   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326562401_17>
01/14/2012 17:26:53  01/14/2012 17:26:53 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326562013_17>
01/14/2012 17:26:53  01/14/2012 17:26:53   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326562013_17>
01/14/2012 17:26:50  01/14/2012 17:26:50   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326562010_17>
01/14/2012 16:42:20  01/14/2012 16:42:20   169   268 65535  ERR_HIGH_PIP_STAGE1_ALARM  BEEP_ONLY  <UTC:1326559340_17>
01/14/2012 16:42:16  01/14/2012 16:42:16   169   264 65535  ERR_HIGH_PIP_STAGE1_ALARM  BEEP_ONLY  <UTC:1326559336_17>
01/14/2012 16:42:05  01/14/2012 16:42:05   169   285 65535  ERR_HIGH_PIP_STAGE1_ALARM  BEEP_ONLY  <UTC:1326559325_17>
01/14/2012 16:41:33  01/14/2012 16:41:33   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1326559293_17>
01/14/2012 16:41:22  01/14/2012 16:41:22   118     6    10  ERR_LOW_CIRCUIT_LEAK_ALARM  HIGH_ALARM  <UTC:1326559282_17>
01/14/2012 16:26:56  01/14/2012 16:26:56   264     0 65535  ERR_MENU_BYPASS_ACTIVATED  KEYPRESS  <UTC:1326558416_17>
01/14/2012 16:18:34  01/14/2012 16:18:34 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326557914_17>
01/14/2012 16:18:34  01/14/2012 16:18:34   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326557914_17>
01/14/2012 16:02:07  01/14/2012 16:02:07 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326556927_17>
01/14/2012 16:02:07  01/14/2012 16:02:07   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326556927_17>
01/14/2012 16:02:05  01/14/2012 16:02:05   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326556925_17>
01/14/2012 15:20:39  01/14/2012 15:20:39 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326554439_17>
01/14/2012 15:20:39  01/14/2012 15:20:39   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326554439_17>
01/14/2012 15:18:10  01/14/2012 15:18:10 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326554290_17>
01/14/2012 15:18:10  01/14/2012 15:18:10   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326554290_17>
01/14/2012 15:18:09  01/14/2012 15:18:09   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326554289_17>
01/14/2012 13:49:44  01/14/2012 13:49:44 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326548984_17>
01/14/2012 13:49:44  01/14/2012 13:49:44   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326548984_17>
01/14/2012 13:46:58  01/14/2012 13:46:58 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326548818_17>
01/14/2012 13:46:58  01/14/2012 13:46:58   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326548818_17>
01/14/2012 13:46:57  01/14/2012 13:46:57   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326548817_17>
01/14/2012 13:09:32  01/14/2012 13:09:32 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326546572_17>
01/14/2012 13:09:32  01/14/2012 13:09:32   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326546572_17>
01/14/2012 13:04:43  01/14/2012 13:04:43 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326546283_17>
01/14/2012 13:04:43  01/14/2012 13:04:43   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326546283_17>
01/14/2012 13:04:42  01/14/2012 13:04:42   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326546282_17>
01/14/2012 11:36:45  01/14/2012 11:36:45   284     0 65535  ERR_PWR_UPGRADE_AC_IN_USE  BEEP_ONLY  <UTC:1326541005_17>
01/14/2012 11:24:01  01/14/2012 11:24:01 17701  2000  1800      NV_ID= 37 (NV_IPAP_PRESSURE)  P/S=P RX=2  AVAPS=1  <UTC:1326540241_17>
01/14/2012 11:23:59  01/14/2012 11:23:59 17700  2600  2200      NV_ID= 36 (NV_IPAP_MAX_PRESSURE)  P/S=P RX=2  AVAPS=1  <UTC:1326540239_17>
01/14/2012 11:23:53  01/14/2012 11:23:53 17707   600   550      NV_ID= 43 (NV_TIDAL_VOLUME)  P/S=P RX=2  AVAPS=1  <UTC:1326540233_17>
01/14/2012 11:23:06  01/14/2012 11:23:06   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1326540186_17>
01/14/2012 10:53:42  01/14/2012 10:53:42   110    32     4  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1326538422_17>
01/14/2012 10:53:41  01/14/2012 10:53:41   179     0 65535  ERR_PWR_REDUCTION_AC_DISCONNECTED  MED_ALARM  <UTC:1326538421_17>
01/14/2012 09:59:38  01/14/2012 09:59:38 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326535178_17>
01/14/2012 09:59:38  01/14/2012 09:59:38   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326535178_17>
01/14/2012 09:56:57  01/14/2012 09:56:57 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326535017_17>
01/14/2012 09:56:57  01/14/2012 09:56:57   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326535017_17>
01/14/2012 09:56:56  01/14/2012 09:56:56   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326535016_17>
01/14/2012 09:30:07  01/14/2012 09:30:07   169   292 65535  ERR_HIGH_PIP_STAGE1_ALARM  BEEP_ONLY  <UTC:1326533407_17>
01/14/2012 09:30:06  01/14/2012 09:30:06   165  6499     2  ERR_LOW_PEP_ALARM  HIGH_ALARM  <UTC:1326533406_17>
01/14/2012 09:30:04  01/14/2012 09:30:04   110    42     3  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1326533404_17>
01/14/2012 09:25:49  01/14/2012 09:25:49   284     0 65535  ERR_PWR_UPGRADE_AC_IN_USE  BEEP_ONLY  <UTC:1326533149_17>
01/14/2012 09:06:12  01/14/2012 09:06:12   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1326531972_17>
01/14/2012 09:02:54  01/14/2012 09:02:54   165  6502     3  ERR_LOW_PEP_ALARM  HIGH_ALARM  <UTC:1326531774_17>
01/14/2012 09:02:52  01/14/2012 09:02:52   110    42     3  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1326531772_17>
01/14/2012 09:02:44  01/14/2012 09:02:44   179     0 65535  ERR_PWR_REDUCTION_AC_DISCONNECTED  MED_ALARM  <UTC:1326531764_17>
01/14/2012 08:02:19  01/14/2012 08:02:19   165  6505    23  ERR_LOW_PEP_ALARM  HIGH_ALARM  <UTC:1326528139_17>
01/14/2012 08:02:17  01/14/2012 08:02:17   110    66    27  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1326528137_17>
01/14/2012 08:01:30  01/14/2012 08:01:30   110     0    16  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1326528090_17>
01/14/2012 08:01:29  01/14/2012 08:01:29   165  6507    20  ERR_LOW_PEP_ALARM  HIGH_ALARM  <UTC:1326528089_17>
01/14/2012 08:01:14  01/14/2012 08:01:14   110     0     8  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1326528074_17>
01/14/2012 08:01:13  01/14/2012 08:01:13   165  6506     8  ERR_LOW_PEP_ALARM  HIGH_ALARM  <UTC:1326528073_17>
01/14/2012 07:58:57  01/14/2012 07:58:57 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326527937_17>
01/14/2012 07:58:57  01/14/2012 07:58:57   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326527937_17>
01/14/2012 07:57:02  01/14/2012 07:57:02 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326527822_17>
01/14/2012 07:57:02  01/14/2012 07:57:02   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326527822_17>
01/14/2012 07:57:00  01/14/2012 07:57:00   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326527820_17>
01/14/2012 07:05:35  01/14/2012 07:05:35 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326524735_17>
01/14/2012 07:05:35  01/14/2012 07:05:35   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326524735_17>
01/14/2012 07:02:59  01/14/2012 07:02:59 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326524579_17>
01/14/2012 07:02:59  01/14/2012 07:02:59   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326524579_17>
01/14/2012 07:02:58  01/14/2012 07:02:58   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326524578_17>
01/14/2012 06:37:39  01/14/2012 06:37:39 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326523059_17>
01/14/2012 06:37:39  01/14/2012 06:37:39   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326523059_17>
01/14/2012 06:32:13  01/14/2012 06:32:13 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326522733_17>
01/14/2012 06:32:13  01/14/2012 06:32:13   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326522733_17>
01/14/2012 06:32:12  01/14/2012 06:32:12   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326522732_17>
01/14/2012 05:49:05  01/14/2012 05:49:05 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326520145_17>
01/14/2012 05:49:05  01/14/2012 05:49:05   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326520145_17>
01/14/2012 05:44:08  01/14/2012 05:44:08 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326519848_17>
01/14/2012 05:44:08  01/14/2012 05:44:08   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326519848_17>
01/14/2012 05:44:06  01/14/2012 05:44:06   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326519846_17>
01/14/2012 02:24:59  01/14/2012 02:24:59   165  6504     7  ERR_LOW_PEP_ALARM  HIGH_ALARM  <UTC:1326507899_17>
01/14/2012 02:24:57  01/14/2012 02:24:57   110    49    10  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1326507897_17>
01/14/2012 02:23:53  01/14/2012 02:23:53   165  6507    14  ERR_LOW_PEP_ALARM  HIGH_ALARM  <UTC:1326507833_17>
01/14/2012 02:23:51  01/14/2012 02:23:51   110    39    18  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1326507831_17>
01/14/2012 02:17:23  01/14/2012 02:17:23 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326507443_17>
01/14/2012 02:17:23  01/14/2012 02:17:23   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326507443_17>
01/14/2012 02:07:07  01/14/2012 02:07:07 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326506827_17>
01/14/2012 02:07:07  01/14/2012 02:07:07   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326506827_17>
01/14/2012 02:07:05  01/14/2012 02:07:05   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326506825_17>
01/14/2012 01:13:17  01/14/2012 01:13:17 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326503597_17>
01/14/2012 01:13:17  01/14/2012 01:13:17   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326503597_17>
01/14/2012 01:07:14  01/14/2012 01:07:14 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326503234_17>
01/14/2012 01:07:14  01/14/2012 01:07:14   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326503234_17>
01/14/2012 01:07:13  01/14/2012 01:07:13   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326503233_17>
01/13/2012 23:26:37  01/13/2012 23:26:37 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326497197_17>
01/13/2012 23:26:37  01/13/2012 23:26:37   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326497197_17>
01/13/2012 23:22:55  01/13/2012 23:22:55 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326496975_17>
01/13/2012 23:22:55  01/13/2012 23:22:55   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326496975_17>
01/13/2012 23:22:54  01/13/2012 23:22:54   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326496974_17>
01/13/2012 22:19:18  01/13/2012 22:19:18 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326493158_17>
01/13/2012 22:19:18  01/13/2012 22:19:18   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326493158_17>
01/13/2012 22:16:33  01/13/2012 22:16:33 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326492993_17>
01/13/2012 22:16:33  01/13/2012 22:16:33   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326492993_17>
01/13/2012 22:16:32  01/13/2012 22:16:32   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326492992_17>
01/13/2012 21:54:27  01/13/2012 21:54:27 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326491667_17>
01/13/2012 21:54:27  01/13/2012 21:54:27   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326491667_17>
01/13/2012 21:48:28  01/13/2012 21:48:28 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326491308_17>
01/13/2012 21:48:28  01/13/2012 21:48:28   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326491308_17>
01/13/2012 21:48:27  01/13/2012 21:48:27   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326491307_17>
01/13/2012 21:39:11  01/13/2012 21:39:11 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326490751_17>
01/13/2012 21:39:11  01/13/2012 21:39:11   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326490751_17>
01/13/2012 21:36:20  01/13/2012 21:36:20 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326490580_17>
01/13/2012 21:36:20  01/13/2012 21:36:20   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326490580_17>
01/13/2012 21:36:19  01/13/2012 21:36:19   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326490579_17>
01/13/2012 21:33:14  01/13/2012 21:33:14 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326490394_17>
01/13/2012 21:33:14  01/13/2012 21:33:14   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326490394_17>
01/13/2012 21:31:18  01/13/2012 21:31:18 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326490278_17>
01/13/2012 21:31:18  01/13/2012 21:31:18   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326490278_17>
01/13/2012 21:31:17  01/13/2012 21:31:17   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326490277_17>
01/13/2012 20:15:54  01/13/2012 20:15:54 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326485754_17>
01/13/2012 20:15:53  01/13/2012 20:15:53   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326485753_17>
01/13/2012 20:15:13  01/13/2012 20:15:13 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326485713_17>
01/13/2012 20:15:13  01/13/2012 20:15:13   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326485713_17>
01/13/2012 20:15:12  01/13/2012 20:15:12   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326485712_17>
01/13/2012 20:13:42  01/13/2012 20:13:42 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326485622_17>
01/13/2012 20:13:42  01/13/2012 20:13:42   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326485622_17>
01/13/2012 20:10:31  01/13/2012 20:10:31 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326485431_17>
01/13/2012 20:10:31  01/13/2012 20:10:31   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326485431_17>
01/13/2012 20:10:30  01/13/2012 20:10:30   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326485430_17>
01/13/2012 18:02:50  01/13/2012 18:02:50 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326477770_17>
01/13/2012 18:02:50  01/13/2012 18:02:50   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326477770_17>
01/13/2012 17:58:29  01/13/2012 17:58:29 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326477509_17>
01/13/2012 17:58:29  01/13/2012 17:58:29   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326477509_17>
01/13/2012 17:58:28  01/13/2012 17:58:28   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326477508_17>
01/13/2012 17:24:49  01/13/2012 17:24:49 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326475489_17>
01/13/2012 17:24:48  01/13/2012 17:24:48   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326475488_17>
01/13/2012 17:20:39  01/13/2012 17:20:39 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326475239_17>
01/13/2012 17:20:38  01/13/2012 17:20:38   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326475238_17>
01/13/2012 17:20:37  01/13/2012 17:20:37   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326475237_17>
01/13/2012 16:58:03  01/13/2012 16:58:03   110     0     7  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1326473883_17>
01/13/2012 16:58:02  01/13/2012 16:58:02   165  6501     7  ERR_LOW_PEP_ALARM  HIGH_ALARM  <UTC:1326473882_17>
01/13/2012 14:18:34  01/13/2012 14:18:34 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326464314_17>
01/13/2012 14:18:34  01/13/2012 14:18:34   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326464314_17>
01/13/2012 14:07:16  01/13/2012 14:07:16 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326463636_17>
01/13/2012 14:07:16  01/13/2012 14:07:16   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326463636_17>
01/13/2012 14:07:16  01/13/2012 14:07:16   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326463636_17>
01/13/2012 14:07:01  01/13/2012 14:07:01 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326463621_17>
01/13/2012 14:07:01  01/13/2012 14:07:01   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326463621_17>
01/13/2012 13:54:38  01/13/2012 13:54:38 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326462878_17>
01/13/2012 13:54:38  01/13/2012 13:54:38   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326462878_17>
01/13/2012 13:54:37  01/13/2012 13:54:37   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326462877_17>
01/13/2012 13:53:22  01/13/2012 13:53:22 17702   800   500      NV_ID= 38 (NV_EPAP_PEEP_CPAP_PRESSURE)  P/S=P RX=2  AVAPS=1  <UTC:1326462802_17>
01/13/2012 13:53:18  01/13/2012 13:53:18 17700  2800  2600      NV_ID= 36 (NV_IPAP_MAX_PRESSURE)  P/S=P RX=2  AVAPS=1  <UTC:1326462798_17>
01/13/2012 13:48:27  01/13/2012 13:48:27   284     0 65535  ERR_PWR_UPGRADE_AC_IN_USE  BEEP_ONLY  <UTC:1326462507_17>
01/13/2012 13:48:24  01/13/2012 13:48:24   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1326462504_17>
01/13/2012 13:48:21  01/13/2012 13:48:21   179     0 65535  ERR_PWR_REDUCTION_AC_DISCONNECTED  MED_ALARM  <UTC:1326462501_17>
01/13/2012 13:48:05  01/13/2012 13:48:05   284     0 65535  ERR_PWR_UPGRADE_AC_IN_USE  BEEP_ONLY  <UTC:1326462485_17>
01/13/2012 13:48:01  01/13/2012 13:48:01   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1326462481_17>
01/13/2012 13:47:58  01/13/2012 13:47:58   179     0 65535  ERR_PWR_REDUCTION_AC_DISCONNECTED  MED_ALARM  <UTC:1326462478_17>
01/13/2012 13:47:17  01/13/2012 13:47:17   284     0 65535  ERR_PWR_UPGRADE_AC_IN_USE  BEEP_ONLY  <UTC:1326462437_17>
01/13/2012 13:31:51  01/13/2012 13:31:51 17702   500   800      NV_ID= 38 (NV_EPAP_PEEP_CPAP_PRESSURE)  P/S=P RX=2  AVAPS=1  <UTC:1326461511_17>
01/13/2012 13:10:24  01/13/2012 13:10:24   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1326460224_17>
01/13/2012 13:10:21  01/13/2012 13:10:21   179     0 65535  ERR_PWR_REDUCTION_AC_DISCONNECTED  MED_ALARM  <UTC:1326460221_17>
01/13/2012 13:06:01  01/13/2012 13:06:01 17702   700   500      NV_ID= 38 (NV_EPAP_PEEP_CPAP_PRESSURE)  P/S=P RX=2  AVAPS=1  <UTC:1326459961_17>
01/13/2012 13:02:01  01/13/2012 13:02:01 17702   500   700      NV_ID= 38 (NV_EPAP_PEEP_CPAP_PRESSURE)  P/S=P RX=2  AVAPS=1  <UTC:1326459721_17>
01/13/2012 12:49:38  01/13/2012 12:49:38   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1326458978_17>
01/13/2012 12:49:37  01/13/2012 12:49:37   284     0 65535  ERR_PWR_UPGRADE_AC_IN_USE  BEEP_ONLY  <UTC:1326458977_17>
01/13/2012 12:49:35  01/13/2012 12:49:35   179     0 65535  ERR_PWR_REDUCTION_AC_DISCONNECTED  MED_ALARM  <UTC:1326458975_17>
01/13/2012 12:44:13  01/13/2012 12:44:13   284     0 65535  ERR_PWR_UPGRADE_AC_IN_USE  BEEP_ONLY  <UTC:1326458653_17>
01/13/2012 12:13:33  01/13/2012 12:13:33   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1326456813_17>
01/13/2012 11:08:47  01/13/2012 11:08:47   173     0 65535  ERR_START_ON_BATTERY  INFO_ALARM  <UTC:1326452927_17>
01/13/2012 11:08:44  01/13/2012 11:08:44 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326452924_17>
01/13/2012 11:08:44  01/13/2012 11:08:44   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326452924_17>
01/13/2012 11:06:04  01/13/2012 11:06:04 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326452764_17>
01/13/2012 11:06:04  01/13/2012 11:06:04   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326452764_17>
01/13/2012 11:06:03  01/13/2012 11:06:03   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326452763_17>
01/13/2012 11:05:43  01/13/2012 11:05:43   173     0 65535  ERR_START_ON_BATTERY  INFO_ALARM  <UTC:1326452743_17>
01/13/2012 11:05:40  01/13/2012 11:05:40 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326452740_17>
01/13/2012 11:05:40  01/13/2012 11:05:40   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326452740_17>
01/13/2012 11:02:48  01/13/2012 11:02:48 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326452568_17>
01/13/2012 11:02:48  01/13/2012 11:02:48   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326452568_17>
01/13/2012 11:02:47  01/13/2012 11:02:47   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326452567_17>
01/13/2012 10:59:17  01/13/2012 10:59:17   173     0 65535  ERR_START_ON_BATTERY  INFO_ALARM  <UTC:1326452357_17>
01/13/2012 10:59:14  01/13/2012 10:59:14 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326452354_17>
01/13/2012 10:59:14  01/13/2012 10:59:14   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326452354_17>
01/13/2012 10:58:38  01/13/2012 10:58:38 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326452318_17>
01/13/2012 10:58:38  01/13/2012 10:58:38   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326452318_17>
01/13/2012 10:58:37  01/13/2012 10:58:37   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326452317_17>
01/13/2012 10:57:41  01/13/2012 10:57:41   173     0 65535  ERR_START_ON_BATTERY  INFO_ALARM  <UTC:1326452261_17>
01/13/2012 10:57:37  01/13/2012 10:57:37 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326452257_17>
01/13/2012 10:57:37  01/13/2012 10:57:37   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326452257_17>
01/13/2012 10:56:39  01/13/2012 10:56:39 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326452199_17>
01/13/2012 10:56:39  01/13/2012 10:56:39   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326452199_17>
01/13/2012 10:56:37  01/13/2012 10:56:37   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326452197_17>
01/13/2012 10:55:40  01/13/2012 10:55:40   173     0 65535  ERR_START_ON_BATTERY  INFO_ALARM  <UTC:1326452140_17>
01/13/2012 10:55:37  01/13/2012 10:55:37 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326452137_17>
01/13/2012 10:55:37  01/13/2012 10:55:37   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326452137_17>
01/13/2012 10:53:02  01/13/2012 10:53:02 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326451982_17>
01/13/2012 10:53:02  01/13/2012 10:53:02   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326451982_17>
01/13/2012 10:53:00  01/13/2012 10:53:00   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326451980_17>
01/13/2012 09:54:04  01/13/2012 09:54:04   179     0 65535  ERR_PWR_REDUCTION_AC_DISCONNECTED  MED_ALARM  <UTC:1326448444_17>
01/13/2012 06:41:41  01/13/2012 06:41:41 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326436901_17>
01/13/2012 06:41:41  01/13/2012 06:41:41   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326436901_17>
01/13/2012 06:39:41  01/13/2012 06:39:41 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326436781_17>
01/13/2012 06:39:41  01/13/2012 06:39:41   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326436781_17>
01/13/2012 06:39:40  01/13/2012 06:39:40   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326436780_17>
01/13/2012 00:59:26  01/13/2012 00:59:26 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326416366_17>
01/13/2012 00:59:26  01/13/2012 00:59:26   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326416366_17>
01/13/2012 00:58:00  01/13/2012 00:58:00 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326416280_17>
01/13/2012 00:58:00  01/13/2012 00:58:00   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326416280_17>
01/13/2012 00:57:56  01/13/2012 00:57:56   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326416276_17>
01/13/2012 00:56:32  01/13/2012 00:56:32 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326416192_17>
01/13/2012 00:56:32  01/13/2012 00:56:32   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326416192_17>
01/13/2012 00:55:01  01/13/2012 00:55:01 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326416101_17>
01/13/2012 00:55:01  01/13/2012 00:55:01   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326416101_17>
01/13/2012 00:55:01  01/13/2012 00:55:01   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326416101_17>
01/13/2012 00:52:50  01/13/2012 00:52:50 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326415970_17>
01/13/2012 00:52:50  01/13/2012 00:52:50   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326415970_17>
01/13/2012 00:51:59  01/13/2012 00:51:59 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326415919_17>
01/13/2012 00:51:59  01/13/2012 00:51:59   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326415919_17>
01/13/2012 00:51:59  01/13/2012 00:51:59   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326415919_17>
01/13/2012 00:27:43  01/13/2012 00:27:43 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326414463_17>
01/13/2012 00:27:43  01/13/2012 00:27:43   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326414463_17>
01/13/2012 00:26:36  01/13/2012 00:26:36 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326414396_17>
01/13/2012 00:26:35  01/13/2012 00:26:35   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326414395_17>
01/13/2012 00:26:35  01/13/2012 00:26:35   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326414395_17>
01/13/2012 00:24:46  01/13/2012 00:24:46 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326414286_17>
01/13/2012 00:24:46  01/13/2012 00:24:46   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326414286_17>
01/13/2012 00:23:44  01/13/2012 00:23:44 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326414224_17>
01/13/2012 00:23:44  01/13/2012 00:23:44   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326414224_17>
01/13/2012 00:23:44  01/13/2012 00:23:44   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326414224_17>
01/13/2012 00:22:47  01/13/2012 00:22:47 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326414167_17>
01/13/2012 00:22:46  01/13/2012 00:22:46   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326414166_17>
01/13/2012 00:20:41  01/13/2012 00:20:41 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326414041_17>
01/13/2012 00:20:41  01/13/2012 00:20:41   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326414041_17>
01/13/2012 00:20:40  01/13/2012 00:20:40   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326414040_17>
01/12/2012 23:44:38  01/12/2012 23:44:38 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326411878_17>
01/12/2012 23:44:37  01/12/2012 23:44:37   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326411877_17>
01/12/2012 23:42:40  01/12/2012 23:42:40 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326411760_17>
01/12/2012 23:42:40  01/12/2012 23:42:40   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326411760_17>
01/12/2012 23:42:38  01/12/2012 23:42:38   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326411758_17>
01/12/2012 23:32:39  01/12/2012 23:32:39 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326411159_17>
01/12/2012 23:32:39  01/12/2012 23:32:39   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326411159_17>
01/12/2012 23:31:50  01/12/2012 23:31:50 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326411110_17>
01/12/2012 23:31:50  01/12/2012 23:31:50   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326411110_17>
01/12/2012 23:31:49  01/12/2012 23:31:49   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326411109_17>
01/12/2012 23:03:40  01/12/2012 23:03:40 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326409420_17>
01/12/2012 23:03:40  01/12/2012 23:03:40   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326409420_17>
01/12/2012 23:01:36  01/12/2012 23:01:36 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326409296_17>
01/12/2012 23:01:36  01/12/2012 23:01:36   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326409296_17>
01/12/2012 23:01:35  01/12/2012 23:01:35   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326409295_17>
01/12/2012 21:37:44  01/12/2012 21:37:44 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326404264_17>
01/12/2012 21:37:44  01/12/2012 21:37:44   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326404264_17>
01/12/2012 21:36:23  01/12/2012 21:36:23 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326404183_17>
01/12/2012 21:36:23  01/12/2012 21:36:23   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326404183_17>
01/12/2012 21:36:22  01/12/2012 21:36:22   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326404182_17>
01/12/2012 18:47:16  01/12/2012 18:47:16 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326394036_17>
01/12/2012 18:47:16  01/12/2012 18:47:16   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326394036_17>
01/12/2012 18:44:46  01/12/2012 18:44:46 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326393886_17>
01/12/2012 18:44:46  01/12/2012 18:44:46   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326393886_17>
01/12/2012 18:44:46  01/12/2012 18:44:46   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326393886_17>
01/12/2012 18:43:57  01/12/2012 18:43:57 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326393837_17>
01/12/2012 18:43:57  01/12/2012 18:43:57   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326393837_17>
01/12/2012 18:43:19  01/12/2012 18:43:19 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326393799_17>
01/12/2012 18:43:19  01/12/2012 18:43:19   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326393799_17>
01/12/2012 18:43:16  01/12/2012 18:43:16   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326393796_17>
01/12/2012 18:40:05  01/12/2012 18:40:05 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326393605_17>
01/12/2012 18:40:05  01/12/2012 18:40:05   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326393605_17>
01/12/2012 18:38:52  01/12/2012 18:38:52 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326393532_17>
01/12/2012 18:38:52  01/12/2012 18:38:52   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326393532_17>
01/12/2012 18:38:52  01/12/2012 18:38:52   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326393532_17>
01/12/2012 17:44:00  01/12/2012 17:44:00   284     0 65535  ERR_PWR_UPGRADE_AC_IN_USE  BEEP_ONLY  <UTC:1326390240_17>
01/12/2012 17:35:59  01/12/2012 17:35:59   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1326389759_17>
01/12/2012 17:34:21  01/12/2012 17:34:21   179     0 65535  ERR_PWR_REDUCTION_AC_DISCONNECTED  MED_ALARM  <UTC:1326389661_17>
01/12/2012 16:22:48  01/12/2012 16:22:48 17700  2600  2800      NV_ID= 36 (NV_IPAP_MAX_PRESSURE)  P/S=P RX=2  AVAPS=1  <UTC:1326385368_17>
01/12/2012 16:00:30  01/12/2012 16:00:30 17707   650   600      NV_ID= 43 (NV_TIDAL_VOLUME)  P/S=P RX=2  AVAPS=1  <UTC:1326384030_17>
01/12/2012 15:59:57  01/12/2012 15:59:57 17700  2800  2600      NV_ID= 36 (NV_IPAP_MAX_PRESSURE)  P/S=P RX=2  AVAPS=1  <UTC:1326383997_17>
01/12/2012 13:08:05  01/12/2012 13:08:05 16400     2     1      NV_ID= 16 (NV_SCREENSAVER)  P/S=P RX=0  AVAPS=0  <UTC:1326373685_17>
01/12/2012 13:07:22  01/12/2012 13:07:22 16413     0     1      NV_ID= 29 (NV_ACCESS_LEVEL)  P/S=P RX=0  AVAPS=0  <UTC:1326373642_17>
01/12/2012 13:06:58  01/12/2012 13:06:58   264     0 65535  ERR_MENU_BYPASS_ACTIVATED  KEYPRESS  <UTC:1326373618_17>
01/12/2012 13:05:27  01/12/2012 13:05:27   264     0 65535  ERR_MENU_BYPASS_ACTIVATED  KEYPRESS  <UTC:1326373527_17>
01/12/2012 13:02:54  01/12/2012 13:02:54 17700  2600  2800      NV_ID= 36 (NV_IPAP_MAX_PRESSURE)  P/S=P RX=2  AVAPS=1  <UTC:1326373374_17>
01/12/2012 13:02:49  01/12/2012 13:02:49   264     0 65535  ERR_MENU_BYPASS_ACTIVATED  KEYPRESS  <UTC:1326373369_17>
01/12/2012 12:53:54  01/12/2012 12:53:54 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326372834_17>
01/12/2012 12:53:54  01/12/2012 12:53:54   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326372834_17>
01/12/2012 12:19:51  01/12/2012 12:19:51 17702   600   500      NV_ID= 38 (NV_EPAP_PEEP_CPAP_PRESSURE)  P/S=P RX=2  AVAPS=1  <UTC:1326370791_17>
01/12/2012 12:19:35  01/12/2012 12:19:35   264     0 65535  ERR_MENU_BYPASS_ACTIVATED  KEYPRESS  <UTC:1326370775_17>
01/12/2012 12:18:23  01/12/2012 12:18:23    72     0 65535  ERR_MMC_SD_CARD_INSERTED  BEEP_ONLY  <UTC:1326370703_17>
01/12/2012 12:18:23  01/12/2012 12:18:23   252     0 65535  ERR_INT_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1326370703_17>
01/12/2012 12:18:23  01/12/2012 12:18:23   251     0 65535  ERR_DET_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1326370703_17>
01/11/2012 20:48:19  01/11/2012 20:48:19   179     0 65535  ERR_PWR_REDUCTION_AC_DISCONNECTED  MED_ALARM  <UTC:1326314899_17>
01/11/2012 13:27:53  01/11/2012 13:27:53    72     0 65535  ERR_MMC_SD_CARD_INSERTED  BEEP_ONLY  <UTC:1326288473_17>
01/11/2012 13:27:53  01/11/2012 13:27:53   252     0 65535  ERR_INT_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1326288473_17>
01/11/2012 13:27:53  01/11/2012 13:27:53   251     0 65535  ERR_DET_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1326288473_17>
01/10/2012 23:10:17  01/10/2012 23:10:17   286     0 65535  ERR_PWR_UPGRADE_DET_LI_ION_IN_USE  BEEP_ONLY  <UTC:1326237017_17>
01/10/2012 23:10:14  01/10/2012 23:10:14    72     0 65535  ERR_MMC_SD_CARD_INSERTED  BEEP_ONLY  <UTC:1326237014_17>
01/10/2012 23:10:14  01/10/2012 23:10:14   252     0 65535  ERR_INT_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1326237014_17>
01/10/2012 23:10:14  01/10/2012 23:10:14   251     0 65535  ERR_DET_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1326237014_17>
01/10/2012 23:01:28  01/10/2012 23:01:28   179     0 65535  ERR_PWR_REDUCTION_AC_DISCONNECTED  MED_ALARM  <UTC:1326236488_17>
01/10/2012 22:13:25  01/10/2012 22:13:25 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326233605_17>
01/10/2012 22:13:25  01/10/2012 22:13:25   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326233605_17>
01/10/2012 22:13:24  01/10/2012 22:13:24   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326233604_17>
01/10/2012 22:08:03  01/10/2012 22:08:03 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326233283_17>
01/10/2012 22:08:03  01/10/2012 22:08:03   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326233283_17>
01/10/2012 21:29:52  01/10/2012 21:29:52 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326230992_17>
01/10/2012 21:29:52  01/10/2012 21:29:52   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326230992_17>
01/10/2012 21:29:51  01/10/2012 21:29:51   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326230991_17>
01/10/2012 20:53:58  01/10/2012 20:53:58 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326228838_17>
01/10/2012 20:53:58  01/10/2012 20:53:58   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326228838_17>
01/10/2012 20:46:12  01/10/2012 20:46:12 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326228372_17>
01/10/2012 20:46:12  01/10/2012 20:46:12   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326228372_17>
01/10/2012 20:46:11  01/10/2012 20:46:11   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326228371_17>
01/10/2012 20:28:30  01/10/2012 20:28:30 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326227310_17>
01/10/2012 20:28:30  01/10/2012 20:28:30   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326227310_17>
01/10/2012 20:22:33  01/10/2012 20:22:33 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326226953_17>
01/10/2012 20:22:33  01/10/2012 20:22:33   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326226953_17>
01/10/2012 20:22:31  01/10/2012 20:22:31   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326226951_17>
01/10/2012 20:22:09  01/10/2012 20:22:09   110    44    24  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1326226929_17>
01/10/2012 20:21:45  01/10/2012 20:21:45   110     9     4  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1326226905_17>
01/10/2012 20:21:44  01/10/2012 20:21:44   165     9     4  ERR_LOW_PEP_ALARM  HIGH_ALARM  <UTC:1326226904_17>
01/10/2012 20:18:34  01/10/2012 20:18:34 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326226714_17>
01/10/2012 20:18:34  01/10/2012 20:18:34   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326226714_17>
01/10/2012 19:54:28  01/10/2012 19:54:28 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326225268_17>
01/10/2012 19:54:28  01/10/2012 19:54:28   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326225268_17>
01/10/2012 19:54:28  01/10/2012 19:54:28   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326225268_17>
01/10/2012 19:26:29  01/10/2012 19:26:29 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326223589_17>
01/10/2012 19:26:29  01/10/2012 19:26:29   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326223589_17>
01/10/2012 19:21:19  01/10/2012 19:21:19 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326223279_17>
01/10/2012 19:21:19  01/10/2012 19:21:19   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326223279_17>
01/10/2012 19:21:16  01/10/2012 19:21:16   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326223276_17>
01/10/2012 19:00:41  01/10/2012 19:00:41 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326222041_17>
01/10/2012 19:00:41  01/10/2012 19:00:41   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326222041_17>
01/10/2012 18:48:37  01/10/2012 18:48:37 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326221317_17>
01/10/2012 18:48:36  01/10/2012 18:48:36   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326221316_17>
01/10/2012 18:48:36  01/10/2012 18:48:36   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326221316_17>
01/10/2012 18:48:28  01/10/2012 18:48:28   110    52     8  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1326221308_17>
01/10/2012 18:06:41  01/10/2012 18:06:41   284     0 65535  ERR_PWR_UPGRADE_AC_IN_USE  BEEP_ONLY  <UTC:1326218801_17>
01/10/2012 17:56:39  01/10/2012 17:56:39   179     0 65535  ERR_PWR_REDUCTION_AC_DISCONNECTED  MED_ALARM  <UTC:1326218199_17>
01/10/2012 16:59:28  01/10/2012 16:59:28 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326214768_17>
01/10/2012 16:59:28  01/10/2012 16:59:28   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326214768_17>
01/10/2012 16:51:20  01/10/2012 16:51:20 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326214280_17>
01/10/2012 16:51:20  01/10/2012 16:51:20   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326214280_17>
01/10/2012 16:51:19  01/10/2012 16:51:19   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326214279_17>
01/10/2012 16:47:48  01/10/2012 16:47:48   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1326214068_17>
01/10/2012 16:47:43  01/10/2012 16:47:43 17707   700   650      NV_ID= 43 (NV_TIDAL_VOLUME)  P/S=P RX=2  AVAPS=1  <UTC:1326214063_17>
01/10/2012 16:47:26  01/10/2012 16:47:26   264     0 65535  ERR_MENU_BYPASS_ACTIVATED  KEYPRESS  <UTC:1326214046_17>
01/10/2012 16:44:16  01/10/2012 16:44:16   165  6500     3  ERR_LOW_PEP_ALARM  HIGH_ALARM  <UTC:1326213856_17>
01/10/2012 16:44:14  01/10/2012 16:44:14   110    38     7  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1326213854_17>
01/10/2012 16:33:14  01/10/2012 16:33:14 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326213194_17>
01/10/2012 16:33:14  01/10/2012 16:33:14   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326213194_17>
01/10/2012 16:29:01  01/10/2012 16:29:01 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326212941_17>
01/10/2012 16:29:01  01/10/2012 16:29:01   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326212941_17>
01/10/2012 16:29:01  01/10/2012 16:29:01   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326212941_17>
01/10/2012 16:25:21  01/10/2012 16:25:21 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326212721_17>
01/10/2012 16:25:20  01/10/2012 16:25:20   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326212720_17>
01/10/2012 16:15:57  01/10/2012 16:15:57 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326212157_17>
01/10/2012 16:15:57  01/10/2012 16:15:57   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326212157_17>
01/10/2012 16:15:56  01/10/2012 16:15:56   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326212156_17>
01/10/2012 16:15:55  01/10/2012 16:15:55   110    50     2  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1326212155_17>
01/10/2012 16:12:20  01/10/2012 16:12:20   110    48     4  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1326211940_17>
01/10/2012 16:12:14  01/10/2012 16:12:14 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326211934_17>
01/10/2012 16:12:14  01/10/2012 16:12:14   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326211934_17>
01/10/2012 15:57:45  01/10/2012 15:57:45 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326211065_17>
01/10/2012 15:57:44  01/10/2012 15:57:44   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326211064_17>
01/10/2012 15:57:23  01/10/2012 15:57:23   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326211043_17>
01/10/2012 15:54:55  01/10/2012 15:54:55   168     0 65535  ERR_UI_AUDIO_PAUSE_KEY_PRESS  KEYPRESS  <UTC:1326210895_17>
01/10/2012 15:54:51  01/10/2012 15:54:51   110    84   173  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1326210891_17>
01/10/2012 15:40:39  01/10/2012 15:40:39   284     0 65535  ERR_PWR_UPGRADE_AC_IN_USE  BEEP_ONLY  <UTC:1326210039_17>
01/10/2012 15:29:23  01/10/2012 15:29:23 17702   400   600      NV_ID= 38 (NV_EPAP_PEEP_CPAP_PRESSURE)  P/S=P RX=2  AVAPS=1  <UTC:1326209363_17>
01/10/2012 15:29:02  01/10/2012 15:29:02 17701  1800  2000      NV_ID= 37 (NV_IPAP_PRESSURE)  P/S=P RX=2  AVAPS=1  <UTC:1326209342_17>
01/10/2012 15:29:00  01/10/2012 15:29:00 17700  2500  2600      NV_ID= 36 (NV_IPAP_MAX_PRESSURE)  P/S=P RX=2  AVAPS=1  <UTC:1326209340_17>
01/10/2012 15:28:56  01/10/2012 15:28:56 17707   650   700      NV_ID= 43 (NV_TIDAL_VOLUME)  P/S=P RX=2  AVAPS=1  <UTC:1326209336_17>
01/10/2012 15:28:49  01/10/2012 15:28:49 17707   600   650      NV_ID= 43 (NV_TIDAL_VOLUME)  P/S=P RX=2  AVAPS=1  <UTC:1326209329_17>
01/10/2012 15:28:41  01/10/2012 15:28:41   264     0 65535  ERR_MENU_BYPASS_ACTIVATED  KEYPRESS  <UTC:1326209321_17>
01/10/2012 15:28:32  01/10/2012 15:28:32   168     0 65535  ERR_UI_AUDIO_PAUSE_KEY_PRESS  KEYPRESS  <UTC:1326209312_17>
01/10/2012 15:20:33  01/10/2012 15:20:33   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1326208833_17>
01/10/2012 15:16:48  01/10/2012 15:16:48   110    87     5  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1326208608_17>
01/10/2012 15:16:39  01/10/2012 15:16:39   168     0 65535  ERR_UI_AUDIO_PAUSE_KEY_PRESS  KEYPRESS  <UTC:1326208599_17>
01/10/2012 15:16:24  01/10/2012 15:16:24   110   142    16  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1326208584_17>
01/10/2012 15:15:55  01/10/2012 15:15:55   110    52    11  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1326208555_17>
01/10/2012 15:15:20  01/10/2012 15:15:20   168     0 65535  ERR_UI_AUDIO_PAUSE_KEY_PRESS  KEYPRESS  <UTC:1326208520_17>
01/10/2012 15:15:03  01/10/2012 15:15:03   110    69    14  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1326208503_17>
01/10/2012 15:14:43  01/10/2012 15:14:43   110    29    19  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1326208483_17>
01/10/2012 15:11:23  01/10/2012 15:11:23   264     0 65535  ERR_MENU_BYPASS_ACTIVATED  KEYPRESS  <UTC:1326208283_17>
01/10/2012 14:36:52  01/10/2012 14:36:52   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1326206212_17>
01/10/2012 14:36:37  01/10/2012 14:36:37   179     0 65535  ERR_PWR_REDUCTION_AC_DISCONNECTED  MED_ALARM  <UTC:1326206197_17>
01/10/2012 14:08:32  01/10/2012 14:08:32 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326204512_17>
01/10/2012 14:08:32  01/10/2012 14:08:32   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326204512_17>
01/10/2012 14:06:38  01/10/2012 14:06:38 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326204398_17>
01/10/2012 14:06:38  01/10/2012 14:06:38   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326204398_17>
01/10/2012 14:06:37  01/10/2012 14:06:37   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326204397_17>
01/10/2012 14:01:50  01/10/2012 14:01:50 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326204110_17>
01/10/2012 14:01:50  01/10/2012 14:01:50   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326204110_17>
01/10/2012 13:55:27  01/10/2012 13:55:27 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326203727_17>
01/10/2012 13:55:27  01/10/2012 13:55:27   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326203727_17>
01/10/2012 13:55:23  01/10/2012 13:55:23   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326203723_17>
01/10/2012 13:52:11  01/10/2012 13:52:11 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326203531_17>
01/10/2012 13:52:11  01/10/2012 13:52:11   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326203531_17>
01/10/2012 13:50:34  01/10/2012 13:50:34 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326203434_17>
01/10/2012 13:50:34  01/10/2012 13:50:34   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326203434_17>
01/10/2012 13:50:33  01/10/2012 13:50:33   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326203433_17>
01/10/2012 13:29:16  01/10/2012 13:29:16 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326202156_17>
01/10/2012 13:29:16  01/10/2012 13:29:16   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326202156_17>
01/10/2012 13:27:43  01/10/2012 13:27:43 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326202063_17>
01/10/2012 13:27:43  01/10/2012 13:27:43   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326202063_17>
01/10/2012 13:27:42  01/10/2012 13:27:42   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326202062_17>
01/10/2012 13:25:06  01/10/2012 13:25:06 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326201906_17>
01/10/2012 13:25:06  01/10/2012 13:25:06   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326201906_17>
01/10/2012 13:23:13  01/10/2012 13:23:13 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326201793_17>
01/10/2012 13:23:13  01/10/2012 13:23:13   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326201793_17>
01/10/2012 13:23:12  01/10/2012 13:23:12   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326201792_17>
01/10/2012 13:22:19  01/10/2012 13:22:19 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326201739_17>
01/10/2012 13:22:19  01/10/2012 13:22:19   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326201739_17>
01/10/2012 13:12:40  01/10/2012 13:12:40 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326201160_17>
01/10/2012 13:12:40  01/10/2012 13:12:40   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326201160_17>
01/10/2012 13:12:38  01/10/2012 13:12:38   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326201158_17>
01/10/2012 12:44:38  01/10/2012 12:44:38 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326199478_17>
01/10/2012 12:44:38  01/10/2012 12:44:38   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326199478_17>
01/10/2012 12:28:51  01/10/2012 12:28:51 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326198531_17>
01/10/2012 12:28:51  01/10/2012 12:28:51   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326198531_17>
01/10/2012 12:28:51  01/10/2012 12:28:51   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326198531_17>
01/10/2012 09:01:54  01/10/2012 09:01:54   295     0 65535  ERR_POWER_OFF_NO_KEY  KEYPRESS  <UTC:1326186114_17>
01/10/2012 09:01:43  01/10/2012 09:01:43   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326186103_17>
01/10/2012 09:01:40  01/10/2012 09:01:40 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326186100_17>
01/10/2012 09:01:40  01/10/2012 09:01:40   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326186100_17>
01/10/2012 08:32:19  01/10/2012 08:32:19 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326184339_17>
01/10/2012 08:32:19  01/10/2012 08:32:19   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326184339_17>
01/10/2012 08:32:18  01/10/2012 08:32:18   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326184338_17>
01/10/2012 07:56:16  01/10/2012 07:56:16 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326182176_17>
01/10/2012 07:56:16  01/10/2012 07:56:16   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326182176_17>
01/10/2012 07:33:49  01/10/2012 07:33:49 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326180829_17>
01/10/2012 07:33:49  01/10/2012 07:33:49   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326180829_17>
01/10/2012 07:33:48  01/10/2012 07:33:48   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326180828_17>
01/10/2012 05:11:49  01/10/2012 05:11:49 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326172309_17>
01/10/2012 05:11:49  01/10/2012 05:11:49   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326172309_17>
01/10/2012 05:03:06  01/10/2012 05:03:06 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326171786_17>
01/10/2012 05:03:06  01/10/2012 05:03:06   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326171786_17>
01/10/2012 05:03:05  01/10/2012 05:03:05   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326171785_17>
01/10/2012 04:58:45  01/10/2012 04:58:45 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326171525_17>
01/10/2012 04:58:45  01/10/2012 04:58:45   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326171525_17>
01/10/2012 04:46:26  01/10/2012 04:46:26 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326170786_17>
01/10/2012 04:46:26  01/10/2012 04:46:26   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326170786_17>
01/10/2012 04:46:25  01/10/2012 04:46:25   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326170785_17>
01/10/2012 01:27:35  01/10/2012 01:27:35 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326158855_17>
01/10/2012 01:27:35  01/10/2012 01:27:35   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326158855_17>
01/10/2012 01:12:50  01/10/2012 01:12:50 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326157970_17>
01/10/2012 01:12:50  01/10/2012 01:12:50   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326157970_17>
01/10/2012 01:12:49  01/10/2012 01:12:49   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326157969_17>
01/09/2012 23:44:28  01/09/2012 23:44:28 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326152668_17>
01/09/2012 23:44:28  01/09/2012 23:44:28   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326152668_17>
01/09/2012 23:34:08  01/09/2012 23:34:08 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326152048_17>
01/09/2012 23:34:08  01/09/2012 23:34:08   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326152048_17>
01/09/2012 23:34:07  01/09/2012 23:34:07   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326152047_17>
01/09/2012 23:16:36  01/09/2012 23:16:36 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326150996_17>
01/09/2012 23:16:36  01/09/2012 23:16:36   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326150996_17>
01/09/2012 22:40:48  01/09/2012 22:40:48 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326148848_17>
01/09/2012 22:40:48  01/09/2012 22:40:48   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326148848_17>
01/09/2012 22:40:46  01/09/2012 22:40:46   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326148846_17>
01/09/2012 21:44:02  01/09/2012 21:44:02 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326145442_17>
01/09/2012 21:44:02  01/09/2012 21:44:02   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326145442_17>
01/09/2012 21:15:53  01/09/2012 21:15:53 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326143753_17>
01/09/2012 21:15:53  01/09/2012 21:15:53   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326143753_17>
01/09/2012 21:15:52  01/09/2012 21:15:52   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326143752_17>
01/09/2012 21:05:43  01/09/2012 21:05:43 17702   600   400      NV_ID= 38 (NV_EPAP_PEEP_CPAP_PRESSURE)  P/S=P RX=2  AVAPS=1  <UTC:1326143143_17>
01/09/2012 21:04:15  01/09/2012 21:04:15 17700  2600  2500      NV_ID= 36 (NV_IPAP_MAX_PRESSURE)  P/S=P RX=2  AVAPS=1  <UTC:1326143055_17>
01/09/2012 20:59:16  01/09/2012 20:59:16 17707   645   600      NV_ID= 43 (NV_TIDAL_VOLUME)  P/S=P RX=2  AVAPS=1  <UTC:1326142756_17>
01/09/2012 20:59:09  01/09/2012 20:59:09 17707   650   645      NV_ID= 43 (NV_TIDAL_VOLUME)  P/S=P RX=2  AVAPS=1  <UTC:1326142749_17>
01/09/2012 20:58:49  01/09/2012 20:58:49 17702   400   600      NV_ID= 38 (NV_EPAP_PEEP_CPAP_PRESSURE)  P/S=P RX=2  AVAPS=1  <UTC:1326142729_17>
01/09/2012 20:58:15  01/09/2012 20:58:15 17702   600   400      NV_ID= 38 (NV_EPAP_PEEP_CPAP_PRESSURE)  P/S=P RX=2  AVAPS=1  <UTC:1326142695_17>
01/09/2012 20:58:11  01/09/2012 20:58:11 17700  2400  2600      NV_ID= 36 (NV_IPAP_MAX_PRESSURE)  P/S=P RX=2  AVAPS=1  <UTC:1326142691_17>
01/09/2012 20:58:05  01/09/2012 20:58:05   264     0 65535  ERR_MENU_BYPASS_ACTIVATED  KEYPRESS  <UTC:1326142685_17>
01/09/2012 20:50:37  01/09/2012 20:50:37 17702   400   600      NV_ID= 38 (NV_EPAP_PEEP_CPAP_PRESSURE)  P/S=P RX=2  AVAPS=1  <UTC:1326142237_17>
01/09/2012 20:50:30  01/09/2012 20:50:30   264     0 65535  ERR_MENU_BYPASS_ACTIVATED  KEYPRESS  <UTC:1326142230_17>
01/09/2012 20:50:26  01/09/2012 20:50:26   168     0 65535  ERR_UI_AUDIO_PAUSE_KEY_PRESS  KEYPRESS  <UTC:1326142226_17>
01/09/2012 20:48:42  01/09/2012 20:48:42   264     0 65535  ERR_MENU_BYPASS_ACTIVATED  KEYPRESS  <UTC:1326142122_17>
01/09/2012 20:46:41  01/09/2012 20:46:41 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326142001_17>
01/09/2012 20:46:41  01/09/2012 20:46:41   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326142001_17>
01/09/2012 20:41:53  01/09/2012 20:41:53 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326141713_17>
01/09/2012 20:41:53  01/09/2012 20:41:53   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326141713_17>
01/09/2012 20:41:53  01/09/2012 20:41:53   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326141713_17>
01/09/2012 20:38:44  01/09/2012 20:38:44 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326141524_17>
01/09/2012 20:38:44  01/09/2012 20:38:44   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326141524_17>
01/09/2012 20:06:43  01/09/2012 20:06:43 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326139603_17>
01/09/2012 20:06:43  01/09/2012 20:06:43   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326139603_17>
01/09/2012 20:06:42  01/09/2012 20:06:42   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326139602_17>
01/09/2012 20:05:59  01/09/2012 20:05:59 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326139559_17>
01/09/2012 20:05:59  01/09/2012 20:05:59   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326139559_17>
01/09/2012 19:44:20  01/09/2012 19:44:20 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326138260_17>
01/09/2012 19:44:20  01/09/2012 19:44:20   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326138260_17>
01/09/2012 19:44:19  01/09/2012 19:44:19   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326138259_17>
01/09/2012 17:22:59  01/09/2012 17:22:59 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326129779_17>
01/09/2012 17:22:59  01/09/2012 17:22:59   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326129779_17>
01/09/2012 17:03:14  01/09/2012 17:03:14 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326128594_17>
01/09/2012 17:03:14  01/09/2012 17:03:14   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326128594_17>
01/09/2012 17:03:13  01/09/2012 17:03:13   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326128593_17>
01/09/2012 16:57:07  01/09/2012 16:57:07 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326128227_17>
01/09/2012 16:57:06  01/09/2012 16:57:06   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326128226_17>
01/09/2012 16:50:08  01/09/2012 16:50:08 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326127808_17>
01/09/2012 16:50:08  01/09/2012 16:50:08   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326127808_17>
01/09/2012 16:50:06  01/09/2012 16:50:06   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326127806_17>
01/09/2012 16:43:43  01/09/2012 16:43:43 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326127423_17>
01/09/2012 16:43:43  01/09/2012 16:43:43   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326127423_17>
01/09/2012 16:29:16  01/09/2012 16:29:16 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326126556_17>
01/09/2012 16:29:15  01/09/2012 16:29:15   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326126555_17>
01/09/2012 16:29:15  01/09/2012 16:29:15   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326126555_17>
01/09/2012 14:07:06  01/09/2012 14:07:06 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326118026_17>
01/09/2012 14:07:06  01/09/2012 14:07:06   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326118026_17>
01/09/2012 13:43:18  01/09/2012 13:43:18 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326116598_17>
01/09/2012 13:43:18  01/09/2012 13:43:18   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326116598_17>
01/09/2012 13:43:17  01/09/2012 13:43:17   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326116597_17>
01/09/2012 13:18:26  01/09/2012 13:18:26 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326115106_17>
01/09/2012 13:18:26  01/09/2012 13:18:26   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326115106_17>
01/09/2012 12:15:46  01/09/2012 12:15:46 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326111346_17>
01/09/2012 12:15:46  01/09/2012 12:15:46   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326111346_17>
01/09/2012 12:15:45  01/09/2012 12:15:45   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326111345_17>
01/09/2012 11:22:41  01/09/2012 11:22:41 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326108161_17>
01/09/2012 11:22:41  01/09/2012 11:22:41   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326108161_17>
01/09/2012 10:46:23  01/09/2012 10:46:23 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326105983_17>
01/09/2012 10:46:23  01/09/2012 10:46:23   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326105983_17>
01/09/2012 10:46:22  01/09/2012 10:46:22   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326105982_17>
01/09/2012 10:10:31  01/09/2012 10:10:31 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326103831_17>
01/09/2012 10:10:31  01/09/2012 10:10:31   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326103831_17>
01/09/2012 09:58:54  01/09/2012 09:58:54 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326103134_17>
01/09/2012 09:58:54  01/09/2012 09:58:54   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326103134_17>
01/09/2012 09:58:54  01/09/2012 09:58:54   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326103134_17>
01/09/2012 09:51:14  01/09/2012 09:51:14 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326102674_17>
01/09/2012 09:51:14  01/09/2012 09:51:14   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326102674_17>
01/09/2012 09:12:13  01/09/2012 09:12:13 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326100333_17>
01/09/2012 09:12:13  01/09/2012 09:12:13   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326100333_17>
01/09/2012 09:12:11  01/09/2012 09:12:11   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326100331_17>
01/09/2012 09:03:03  01/09/2012 09:03:03 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326099783_17>
01/09/2012 09:03:03  01/09/2012 09:03:03   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326099783_17>
01/09/2012 08:20:01  01/09/2012 08:20:01 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326097201_17>
01/09/2012 08:20:01  01/09/2012 08:20:01   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326097201_17>
01/09/2012 08:20:00  01/09/2012 08:20:00   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326097200_17>
01/08/2012 22:09:28  01/08/2012 22:09:28 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326060568_17>
01/08/2012 22:09:28  01/08/2012 22:09:28   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326060568_17>
01/08/2012 22:09:27  01/08/2012 22:09:27 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326060567_17>
01/08/2012 22:09:27  01/08/2012 22:09:27   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326060567_17>
01/08/2012 22:09:26  01/08/2012 22:09:26   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326060566_17>
01/08/2012 22:09:18  01/08/2012 22:09:18   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1326060558_17>
01/08/2012 22:07:41  01/08/2012 22:07:41   284     0 65535  ERR_PWR_UPGRADE_AC_IN_USE  BEEP_ONLY  <UTC:1326060461_17>
01/08/2012 22:06:15  01/08/2012 22:06:15   173     0 65535  ERR_START_ON_BATTERY  INFO_ALARM  <UTC:1326060375_17>
01/08/2012 22:06:11  01/08/2012 22:06:11 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326060371_17>
01/08/2012 22:06:11  01/08/2012 22:06:11   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326060371_17>
01/08/2012 22:02:06  01/08/2012 22:02:06   179     0 65535  ERR_PWR_REDUCTION_AC_DISCONNECTED  MED_ALARM  <UTC:1326060126_17>
01/08/2012 20:47:39  01/08/2012 20:47:39 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326055659_17>
01/08/2012 20:47:38  01/08/2012 20:47:38   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326055658_17>
01/08/2012 20:47:38  01/08/2012 20:47:38   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326055658_17>
01/08/2012 20:43:04  01/08/2012 20:43:04 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326055384_17>
01/08/2012 20:43:04  01/08/2012 20:43:04   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326055384_17>
01/08/2012 20:41:20  01/08/2012 20:41:20 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326055280_17>
01/08/2012 20:41:19  01/08/2012 20:41:19   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326055279_17>
01/08/2012 20:41:19  01/08/2012 20:41:19   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326055279_17>
01/08/2012 20:37:48  01/08/2012 20:37:48 17701  1600  1800      NV_ID= 37 (NV_IPAP_PRESSURE)  P/S=P RX=2  AVAPS=1  <UTC:1326055068_17>
01/08/2012 20:37:42  01/08/2012 20:37:42   264     0 65535  ERR_MENU_BYPASS_ACTIVATED  KEYPRESS  <UTC:1326055062_17>
01/08/2012 20:37:13  01/08/2012 20:37:13 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326055033_17>
01/08/2012 20:37:13  01/08/2012 20:37:13   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326055033_17>
01/08/2012 20:26:33  01/08/2012 20:26:33 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326054393_17>
01/08/2012 20:26:33  01/08/2012 20:26:33   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326054393_17>
01/08/2012 20:26:32  01/08/2012 20:26:32   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326054392_17>
01/08/2012 20:22:25  01/08/2012 20:22:25 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326054145_17>
01/08/2012 20:22:25  01/08/2012 20:22:25   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326054145_17>
01/08/2012 19:59:45  01/08/2012 19:59:45 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326052785_17>
01/08/2012 19:59:45  01/08/2012 19:59:45   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326052785_17>
01/08/2012 19:59:44  01/08/2012 19:59:44   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326052784_17>
01/08/2012 19:48:30  01/08/2012 19:48:30 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326052110_17>
01/08/2012 19:48:30  01/08/2012 19:48:30   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326052110_17>
01/08/2012 18:52:11  01/08/2012 18:52:11 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326048731_17>
01/08/2012 18:52:11  01/08/2012 18:52:11   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326048731_17>
01/08/2012 18:52:10  01/08/2012 18:52:10   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326048730_17>
01/08/2012 18:33:57  01/08/2012 18:33:57 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326047637_17>
01/08/2012 18:33:57  01/08/2012 18:33:57   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326047637_17>
01/08/2012 18:21:01  01/08/2012 18:21:01 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326046861_17>
01/08/2012 18:21:01  01/08/2012 18:21:01   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326046861_17>
01/08/2012 18:21:00  01/08/2012 18:21:00   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326046860_17>
01/08/2012 17:39:46  01/08/2012 17:39:46 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326044386_17>
01/08/2012 17:39:46  01/08/2012 17:39:46   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326044386_17>
01/08/2012 16:32:06  01/08/2012 16:32:06 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326040326_17>
01/08/2012 16:32:06  01/08/2012 16:32:06   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326040326_17>
01/08/2012 16:32:05  01/08/2012 16:32:05   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326040325_17>
01/08/2012 15:40:08  01/08/2012 15:40:08 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326037208_17>
01/08/2012 15:40:08  01/08/2012 15:40:08   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326037208_17>
01/08/2012 15:19:56  01/08/2012 15:19:56 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326035996_17>
01/08/2012 15:19:56  01/08/2012 15:19:56   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326035996_17>
01/08/2012 15:19:55  01/08/2012 15:19:55   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326035995_17>
01/08/2012 14:58:44  01/08/2012 14:58:44 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326034724_17>
01/08/2012 14:58:44  01/08/2012 14:58:44   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326034724_17>
01/08/2012 14:52:16  01/08/2012 14:52:16 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326034336_17>
01/08/2012 14:52:16  01/08/2012 14:52:16   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326034336_17>
01/08/2012 14:52:07  01/08/2012 14:52:07   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326034327_17>
01/08/2012 14:25:08  01/08/2012 14:25:08 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326032708_17>
01/08/2012 14:25:08  01/08/2012 14:25:08   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326032708_17>
01/08/2012 14:20:52  01/08/2012 14:20:52   284     0 65535  ERR_PWR_UPGRADE_AC_IN_USE  BEEP_ONLY  <UTC:1326032452_17>
01/08/2012 14:19:31  01/08/2012 14:19:31   179     0 65535  ERR_PWR_REDUCTION_AC_DISCONNECTED  MED_ALARM  <UTC:1326032371_17>
01/08/2012 13:29:30  01/08/2012 13:29:30 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326029370_17>
01/08/2012 13:29:30  01/08/2012 13:29:30   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326029370_17>
01/08/2012 13:29:30  01/08/2012 13:29:30   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326029370_17>
01/08/2012 13:17:21  01/08/2012 13:17:21 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326028641_17>
01/08/2012 13:17:20  01/08/2012 13:17:20   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326028640_17>
01/08/2012 13:00:16  01/08/2012 13:00:16 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326027616_17>
01/08/2012 13:00:16  01/08/2012 13:00:16   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326027616_17>
01/08/2012 13:00:13  01/08/2012 13:00:13   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326027613_17>
01/08/2012 11:38:40  01/08/2012 11:38:40 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326022720_17>
01/08/2012 11:38:40  01/08/2012 11:38:40   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326022720_17>
01/08/2012 11:28:05  01/08/2012 11:28:05 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326022085_17>
01/08/2012 11:28:05  01/08/2012 11:28:05   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326022085_17>
01/08/2012 11:28:04  01/08/2012 11:28:04   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326022084_17>
01/08/2012 11:27:55  01/08/2012 11:27:55   169   225 65535  ERR_HIGH_PIP_STAGE1_ALARM  BEEP_ONLY  <UTC:1326022075_17>
01/08/2012 11:24:20  01/08/2012 11:24:20 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326021860_17>
01/08/2012 11:24:20  01/08/2012 11:24:20   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326021860_17>
01/08/2012 11:21:49  01/08/2012 11:21:49 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326021709_17>
01/08/2012 11:21:49  01/08/2012 11:21:49   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326021709_17>
01/08/2012 11:21:48  01/08/2012 11:21:48   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326021708_17>
01/08/2012 11:19:08  01/08/2012 11:19:08 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326021548_17>
01/08/2012 11:19:08  01/08/2012 11:19:08   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326021548_17>
01/08/2012 11:06:24  01/08/2012 11:06:24 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326020784_17>
01/08/2012 11:06:24  01/08/2012 11:06:24   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326020784_17>
01/08/2012 11:06:23  01/08/2012 11:06:23   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326020783_17>
01/08/2012 10:50:08  01/08/2012 10:50:08 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326019808_17>
01/08/2012 10:50:08  01/08/2012 10:50:08   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326019808_17>
01/08/2012 10:41:10  01/08/2012 10:41:10 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326019270_17>
01/08/2012 10:41:10  01/08/2012 10:41:10   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326019270_17>
01/08/2012 10:41:09  01/08/2012 10:41:09   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326019269_17>
01/08/2012 10:13:03  01/08/2012 10:13:03 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326017583_17>
01/08/2012 10:13:03  01/08/2012 10:13:03   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1326017583_17>
01/08/2012 09:43:53  01/08/2012 09:43:53 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1326015833_17>
01/08/2012 09:43:53  01/08/2012 09:43:53   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1326015833_17>
01/08/2012 09:43:52  01/08/2012 09:43:52   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1326015832_17>
01/08/2012 00:43:55  01/08/2012 00:43:55 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325983435_17>
01/08/2012 00:43:55  01/08/2012 00:43:55   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325983435_17>
01/08/2012 00:23:20  01/08/2012 00:23:20 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325982200_17>
01/08/2012 00:23:20  01/08/2012 00:23:20   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325982200_17>
01/08/2012 00:23:19  01/08/2012 00:23:19   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325982199_17>
01/07/2012 23:47:48  01/07/2012 23:47:48 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325980068_17>
01/07/2012 23:47:48  01/07/2012 23:47:48   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325980068_17>
01/07/2012 23:24:57  01/07/2012 23:24:57   284     0 65535  ERR_PWR_UPGRADE_AC_IN_USE  BEEP_ONLY  <UTC:1325978697_17>
01/07/2012 23:24:28  01/07/2012 23:24:28   179     0 65535  ERR_PWR_REDUCTION_AC_DISCONNECTED  MED_ALARM  <UTC:1325978668_17>
01/07/2012 23:00:14  01/07/2012 23:00:14 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325977214_17>
01/07/2012 23:00:14  01/07/2012 23:00:14   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325977214_17>
01/07/2012 23:00:13  01/07/2012 23:00:13   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325977213_17>
01/07/2012 21:59:29  01/07/2012 21:59:29   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1325973569_17>
01/07/2012 21:59:27  01/07/2012 21:59:27   284     0 65535  ERR_PWR_UPGRADE_AC_IN_USE  BEEP_ONLY  <UTC:1325973567_17>
01/07/2012 21:59:14  01/07/2012 21:59:14   173     0 65535  ERR_START_ON_BATTERY  INFO_ALARM  <UTC:1325973554_17>
01/07/2012 21:59:14  01/07/2012 21:59:14   286     0 65535  ERR_PWR_UPGRADE_DET_LI_ION_IN_USE  BEEP_ONLY  <UTC:1325973554_17>
01/07/2012 21:59:11  01/07/2012 21:59:11    72     0 65535  ERR_MMC_SD_CARD_INSERTED  BEEP_ONLY  <UTC:1325973551_17>
01/07/2012 21:59:11  01/07/2012 21:59:11   252     0 65535  ERR_INT_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1325973551_17>
01/07/2012 21:59:11  01/07/2012 21:59:11   251     0 65535  ERR_DET_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1325973551_17>
01/07/2012 21:59:11  01/07/2012 21:59:11 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325973551_17>
01/07/2012 21:59:11  01/07/2012 21:59:11   324     2 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325973551_17>
01/07/2012 19:38:25  01/07/2012 19:38:25 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325965105_17>
01/07/2012 19:38:25  01/07/2012 19:38:25   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325965105_17>
01/07/2012 19:38:24  01/07/2012 19:38:24   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325965104_17>
01/07/2012 18:39:15  01/07/2012 18:39:15   173     0 65535  ERR_START_ON_BATTERY  INFO_ALARM  <UTC:1325961555_17>
01/07/2012 18:39:12  01/07/2012 18:39:12    72     0 65535  ERR_MMC_SD_CARD_INSERTED  BEEP_ONLY  <UTC:1325961552_17>
01/07/2012 18:39:12  01/07/2012 18:39:12   252     0 65535  ERR_INT_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1325961552_17>
01/07/2012 18:39:12  01/07/2012 18:39:12   251     0 65535  ERR_DET_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1325961552_17>
01/07/2012 18:39:12  01/07/2012 18:39:12 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325961552_17>
01/07/2012 18:39:12  01/07/2012 18:39:12   324     2 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325961552_17>
01/07/2012 18:24:14  01/07/2012 18:24:14   179     0 65535  ERR_PWR_REDUCTION_AC_DISCONNECTED  MED_ALARM  <UTC:1325960654_17>
01/07/2012 18:16:05  01/07/2012 18:16:05 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325960165_17>
01/07/2012 18:16:05  01/07/2012 18:16:05   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325960165_17>
01/07/2012 18:16:04  01/07/2012 18:16:04   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325960164_17>
01/07/2012 18:10:14  01/07/2012 18:10:14 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325959814_17>
01/07/2012 18:10:13  01/07/2012 18:10:13   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325959813_17>
01/07/2012 17:59:12  01/07/2012 17:59:12 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325959152_17>
01/07/2012 17:59:12  01/07/2012 17:59:12   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325959152_17>
01/07/2012 17:59:11  01/07/2012 17:59:11   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325959151_17>
01/07/2012 16:08:54  01/07/2012 16:08:54 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325952534_17>
01/07/2012 16:08:54  01/07/2012 16:08:54   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325952534_17>
01/07/2012 15:40:45  01/07/2012 15:40:45 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325950845_17>
01/07/2012 15:40:45  01/07/2012 15:40:45   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325950845_17>
01/07/2012 15:40:44  01/07/2012 15:40:44   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325950844_17>
01/07/2012 15:03:49  01/07/2012 15:03:49 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325948629_17>
01/07/2012 15:03:49  01/07/2012 15:03:49   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325948629_17>
01/07/2012 14:59:57  01/07/2012 14:59:57 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325948397_17>
01/07/2012 14:59:57  01/07/2012 14:59:57   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325948397_17>
01/07/2012 14:59:54  01/07/2012 14:59:54   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325948394_17>
01/07/2012 14:59:07  01/07/2012 14:59:07 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325948347_17>
01/07/2012 14:59:07  01/07/2012 14:59:07   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325948347_17>
01/07/2012 14:25:01  01/07/2012 14:25:01 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325946301_17>
01/07/2012 14:25:01  01/07/2012 14:25:01   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325946301_17>
01/07/2012 14:25:01  01/07/2012 14:25:01   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325946301_17>
01/07/2012 14:00:36  01/07/2012 14:00:36 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325944836_17>
01/07/2012 14:00:36  01/07/2012 14:00:36   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325944836_17>
01/07/2012 13:48:14  01/07/2012 13:48:14   284     0 65535  ERR_PWR_UPGRADE_AC_IN_USE  BEEP_ONLY  <UTC:1325944094_17>
01/07/2012 13:47:53  01/07/2012 13:47:53   179     0 65535  ERR_PWR_REDUCTION_AC_DISCONNECTED  MED_ALARM  <UTC:1325944073_17>
01/07/2012 12:32:25  01/07/2012 12:32:25 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325939545_17>
01/07/2012 12:32:25  01/07/2012 12:32:25   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325939545_17>
01/07/2012 12:32:24  01/07/2012 12:32:24   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325939544_17>
01/07/2012 12:22:21  01/07/2012 12:22:21 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325938941_17>
01/07/2012 12:22:21  01/07/2012 12:22:21   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325938941_17>
01/07/2012 12:02:11  01/07/2012 12:02:11 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325937731_17>
01/07/2012 12:02:11  01/07/2012 12:02:11   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325937731_17>
01/07/2012 12:02:10  01/07/2012 12:02:10   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325937730_17>
01/07/2012 11:34:06  01/07/2012 11:34:06 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325936046_17>
01/07/2012 11:34:06  01/07/2012 11:34:06   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325936046_17>
01/07/2012 11:21:51  01/07/2012 11:21:51 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325935311_17>
01/07/2012 11:21:51  01/07/2012 11:21:51   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325935311_17>
01/07/2012 11:21:50  01/07/2012 11:21:50   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325935310_17>
01/07/2012 10:56:30  01/07/2012 10:56:30 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325933790_17>
01/07/2012 10:56:30  01/07/2012 10:56:30   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325933790_17>
01/07/2012 10:40:02  01/07/2012 10:40:02 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325932802_17>
01/07/2012 10:40:02  01/07/2012 10:40:02   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325932802_17>
01/07/2012 10:40:01  01/07/2012 10:40:01   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325932801_17>
01/07/2012 09:53:28  01/07/2012 09:53:28 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325930008_17>
01/07/2012 09:53:28  01/07/2012 09:53:28   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325930008_17>
01/07/2012 09:46:25  01/07/2012 09:46:25 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325929585_17>
01/07/2012 09:46:25  01/07/2012 09:46:25   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325929585_17>
01/07/2012 09:46:24  01/07/2012 09:46:24   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325929584_17>
01/07/2012 09:39:58  01/07/2012 09:39:58 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325929198_17>
01/07/2012 09:39:58  01/07/2012 09:39:58   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325929198_17>
01/07/2012 09:34:26  01/07/2012 09:34:26 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325928866_17>
01/07/2012 09:34:26  01/07/2012 09:34:26   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325928866_17>
01/07/2012 09:34:23  01/07/2012 09:34:23   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325928863_17>
01/07/2012 09:32:25  01/07/2012 09:32:25 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325928745_17>
01/07/2012 09:32:25  01/07/2012 09:32:25   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325928745_17>
01/07/2012 09:15:07  01/07/2012 09:15:07 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325927707_17>
01/07/2012 09:15:07  01/07/2012 09:15:07   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325927707_17>
01/07/2012 09:15:06  01/07/2012 09:15:06   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325927706_17>
01/06/2012 23:49:25  01/06/2012 23:49:25 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325893765_17>
01/06/2012 23:49:25  01/06/2012 23:49:25   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325893765_17>
01/06/2012 23:45:48  01/06/2012 23:45:48 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325893548_17>
01/06/2012 23:45:48  01/06/2012 23:45:48   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325893548_17>
01/06/2012 23:45:47  01/06/2012 23:45:47   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325893547_17>
01/06/2012 22:27:27  01/06/2012 22:27:27 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325888847_17>
01/06/2012 22:27:27  01/06/2012 22:27:27   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325888847_17>
01/06/2012 22:06:52  01/06/2012 22:06:52    72     0 65535  ERR_MMC_SD_CARD_INSERTED  BEEP_ONLY  <UTC:1325887612_17>
01/06/2012 22:06:52  01/06/2012 22:06:52   252     0 65535  ERR_INT_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1325887612_17>
01/06/2012 22:06:52  01/06/2012 22:06:52   251     0 65535  ERR_DET_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1325887612_17>
01/06/2012 21:09:16  01/06/2012 21:09:16   179     0 65535  ERR_PWR_REDUCTION_AC_DISCONNECTED  MED_ALARM  <UTC:1325884156_17>
01/06/2012 21:05:38  01/06/2012 21:05:38 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325883938_17>
01/06/2012 21:05:38  01/06/2012 21:05:38   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325883938_17>
01/06/2012 21:05:37  01/06/2012 21:05:37   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325883937_17>
01/06/2012 20:45:26  01/06/2012 20:45:26 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325882726_17>
01/06/2012 20:45:26  01/06/2012 20:45:26   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325882726_17>
01/06/2012 20:37:23  01/06/2012 20:37:23    72     0 65535  ERR_MMC_SD_CARD_INSERTED  BEEP_ONLY  <UTC:1325882243_17>
01/06/2012 20:37:17  01/06/2012 20:37:17    74     0 65535  ERR_MMC_SD_CARD_REMOVED  BEEP_ONLY  <UTC:1325882237_17>
01/06/2012 20:15:53  01/06/2012 20:15:53 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325880953_17>
01/06/2012 20:15:53  01/06/2012 20:15:53   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325880953_17>
01/06/2012 20:15:52  01/06/2012 20:15:52   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325880952_17>
01/06/2012 20:08:07  01/06/2012 20:08:07 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325880487_17>
01/06/2012 20:08:07  01/06/2012 20:08:07   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325880487_17>
01/06/2012 19:27:02  01/06/2012 19:27:02 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325878022_17>
01/06/2012 19:27:02  01/06/2012 19:27:02   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325878022_17>
01/06/2012 19:27:01  01/06/2012 19:27:01   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325878021_17>
01/06/2012 17:51:13  01/06/2012 17:51:13 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325872273_17>
01/06/2012 17:51:13  01/06/2012 17:51:13   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325872273_17>
01/06/2012 17:47:42  01/06/2012 17:47:42 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325872062_17>
01/06/2012 17:47:42  01/06/2012 17:47:42   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325872062_17>
01/06/2012 17:47:41  01/06/2012 17:47:41   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325872061_17>
01/06/2012 17:30:23  01/06/2012 17:30:23 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325871023_17>
01/06/2012 17:30:23  01/06/2012 17:30:23   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325871023_17>
01/06/2012 16:26:53  01/06/2012 16:26:53 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325867213_17>
01/06/2012 16:26:53  01/06/2012 16:26:53   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325867213_17>
01/06/2012 16:26:52  01/06/2012 16:26:52   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325867212_17>
01/06/2012 14:44:31  01/06/2012 14:44:31 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325861071_17>
01/06/2012 14:44:31  01/06/2012 14:44:31   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325861071_17>
01/06/2012 14:32:00  01/06/2012 14:32:00 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325860320_17>
01/06/2012 14:32:00  01/06/2012 14:32:00   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325860320_17>
01/06/2012 14:31:59  01/06/2012 14:31:59   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325860319_17>
01/06/2012 14:31:56  01/06/2012 14:31:56 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325860316_17>
01/06/2012 14:31:56  01/06/2012 14:31:56   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325860316_17>
01/06/2012 14:18:48  01/06/2012 14:18:48 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325859528_17>
01/06/2012 14:18:48  01/06/2012 14:18:48   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325859528_17>
01/06/2012 14:18:47  01/06/2012 14:18:47   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325859527_17>
01/06/2012 13:05:52  01/06/2012 13:05:52 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325855152_17>
01/06/2012 13:05:52  01/06/2012 13:05:52   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325855152_17>
01/06/2012 11:33:43  01/06/2012 11:33:43   284     0 65535  ERR_PWR_UPGRADE_AC_IN_USE  BEEP_ONLY  <UTC:1325849623_17>
01/06/2012 11:32:29  01/06/2012 11:32:29   179     0 65535  ERR_PWR_REDUCTION_AC_DISCONNECTED  MED_ALARM  <UTC:1325849549_17>
01/06/2012 11:32:17  01/06/2012 11:32:17 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325849537_17>
01/06/2012 11:32:17  01/06/2012 11:32:17   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325849537_17>
01/06/2012 11:32:16  01/06/2012 11:32:16   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325849536_17>
01/06/2012 09:57:48  01/06/2012 09:57:48 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325843868_17>
01/06/2012 09:57:48  01/06/2012 09:57:48   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325843868_17>
01/06/2012 09:48:10  01/06/2012 09:48:10 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325843290_17>
01/06/2012 09:48:10  01/06/2012 09:48:10   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325843290_17>
01/06/2012 09:48:09  01/06/2012 09:48:09   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325843289_17>
01/06/2012 09:08:20  01/06/2012 09:08:20 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325840900_17>
01/06/2012 09:08:20  01/06/2012 09:08:20   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325840900_17>
01/06/2012 09:07:50  01/06/2012 09:07:50 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325840870_17>
01/06/2012 09:07:50  01/06/2012 09:07:50   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325840870_17>
01/06/2012 09:07:48  01/06/2012 09:07:48   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325840868_17>
01/06/2012 09:06:23  01/06/2012 09:06:23 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325840783_17>
01/06/2012 09:06:23  01/06/2012 09:06:23   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325840783_17>
01/06/2012 08:26:20  01/06/2012 08:26:20 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325838380_17>
01/06/2012 08:26:20  01/06/2012 08:26:20   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325838380_17>
01/06/2012 08:26:19  01/06/2012 08:26:19   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325838379_17>
01/05/2012 21:24:55  01/05/2012 21:24:55 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325798695_17>
01/05/2012 21:24:55  01/05/2012 21:24:55   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325798695_17>
01/05/2012 21:24:54  01/05/2012 21:24:54 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325798694_17>
01/05/2012 21:24:54  01/05/2012 21:24:54   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325798694_17>
01/05/2012 21:24:52  01/05/2012 21:24:52   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325798692_17>
01/05/2012 21:22:39  01/05/2012 21:22:39 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325798559_17>
01/05/2012 21:22:39  01/05/2012 21:22:39   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325798559_17>
01/05/2012 20:58:05  01/05/2012 20:58:05   284     0 65535  ERR_PWR_UPGRADE_AC_IN_USE  BEEP_ONLY  <UTC:1325797085_17>
01/05/2012 20:57:18  01/05/2012 20:57:18   179     0 65535  ERR_PWR_REDUCTION_AC_DISCONNECTED  MED_ALARM  <UTC:1325797038_17>
01/05/2012 20:53:52  01/05/2012 20:53:52 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325796832_17>
01/05/2012 20:53:52  01/05/2012 20:53:52   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325796832_17>
01/05/2012 20:53:52  01/05/2012 20:53:52   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325796832_17>
01/05/2012 20:44:39  01/05/2012 20:44:39 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325796279_17>
01/05/2012 20:44:39  01/05/2012 20:44:39   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325796279_17>
01/05/2012 20:38:56  01/05/2012 20:38:56 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325795936_17>
01/05/2012 20:38:56  01/05/2012 20:38:56   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325795936_17>
01/05/2012 20:38:55  01/05/2012 20:38:55   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325795935_17>
01/05/2012 20:33:30  01/05/2012 20:33:30 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325795610_17>
01/05/2012 20:33:30  01/05/2012 20:33:30   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325795610_17>
01/05/2012 20:24:22  01/05/2012 20:24:22 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325795062_17>
01/05/2012 20:24:21  01/05/2012 20:24:21   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325795061_17>
01/05/2012 20:24:21  01/05/2012 20:24:21   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325795061_17>
01/05/2012 20:18:39  01/05/2012 20:18:39   169   216 65535  ERR_HIGH_PIP_STAGE1_ALARM  BEEP_ONLY  <UTC:1325794719_17>
01/05/2012 20:17:20  01/05/2012 20:17:20   264     0 65535  ERR_MENU_BYPASS_ACTIVATED  KEYPRESS  <UTC:1325794640_17>
01/05/2012 20:17:17  01/05/2012 20:17:17   168     0 65535  ERR_UI_AUDIO_PAUSE_KEY_PRESS  KEYPRESS  <UTC:1325794637_17>
01/05/2012 20:16:48  01/05/2012 20:16:48 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325794608_17>
01/05/2012 20:16:48  01/05/2012 20:16:48   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325794608_17>
01/05/2012 19:28:41  01/05/2012 19:28:41 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325791721_17>
01/05/2012 19:28:41  01/05/2012 19:28:41   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325791721_17>
01/05/2012 19:28:41  01/05/2012 19:28:41   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325791721_17>
01/05/2012 17:27:08  01/05/2012 17:27:08 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325784428_17>
01/05/2012 17:27:08  01/05/2012 17:27:08   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325784428_17>
01/05/2012 16:57:37  01/05/2012 16:57:37 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325782657_17>
01/05/2012 16:57:37  01/05/2012 16:57:37   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325782657_17>
01/05/2012 16:57:36  01/05/2012 16:57:36   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325782656_17>
01/05/2012 16:46:13  01/05/2012 16:46:13 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325781973_17>
01/05/2012 16:46:13  01/05/2012 16:46:13   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325781973_17>
01/05/2012 16:14:05  01/05/2012 16:14:05 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325780045_17>
01/05/2012 16:14:05  01/05/2012 16:14:05   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325780045_17>
01/05/2012 16:14:03  01/05/2012 16:14:03   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325780043_17>
01/05/2012 15:49:57  01/05/2012 15:49:57 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325778597_17>
01/05/2012 15:49:57  01/05/2012 15:49:57   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325778597_17>
01/05/2012 15:37:25  01/05/2012 15:37:25 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325777845_17>
01/05/2012 15:37:25  01/05/2012 15:37:25   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325777845_17>
01/05/2012 15:37:24  01/05/2012 15:37:24   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325777844_17>
01/05/2012 15:00:23  01/05/2012 15:00:23 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325775623_17>
01/05/2012 15:00:23  01/05/2012 15:00:23   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325775623_17>
01/05/2012 14:51:41  01/05/2012 14:51:41 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325775101_17>
01/05/2012 14:51:41  01/05/2012 14:51:41   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325775101_17>
01/05/2012 14:51:40  01/05/2012 14:51:40   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325775100_17>
01/05/2012 14:29:26  01/05/2012 14:29:26 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325773766_17>
01/05/2012 14:29:26  01/05/2012 14:29:26   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325773766_17>
01/05/2012 14:23:37  01/05/2012 14:23:37 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325773417_17>
01/05/2012 14:23:37  01/05/2012 14:23:37   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325773417_17>
01/05/2012 14:23:36  01/05/2012 14:23:36   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325773416_17>
01/05/2012 14:23:35  01/05/2012 14:23:35   169   285 65535  ERR_HIGH_PIP_STAGE1_ALARM  BEEP_ONLY  <UTC:1325773415_17>
01/05/2012 14:08:45  01/05/2012 14:08:45 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325772525_17>
01/05/2012 14:08:45  01/05/2012 14:08:45   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325772525_17>
01/05/2012 13:43:59  01/05/2012 13:43:59 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325771039_17>
01/05/2012 13:43:59  01/05/2012 13:43:59   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325771039_17>
01/05/2012 13:43:58  01/05/2012 13:43:58   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325771038_17>
01/05/2012 13:19:08  01/05/2012 13:19:08 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325769548_17>
01/05/2012 13:19:08  01/05/2012 13:19:08   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325769548_17>
01/05/2012 13:15:07  01/05/2012 13:15:07 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325769307_17>
01/05/2012 13:15:07  01/05/2012 13:15:07   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325769307_17>
01/05/2012 13:15:06  01/05/2012 13:15:06   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325769306_17>
01/05/2012 12:57:34  01/05/2012 12:57:34 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325768254_17>
01/05/2012 12:57:34  01/05/2012 12:57:34   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325768254_17>
01/05/2012 12:57:12  01/05/2012 12:57:12 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325768232_17>
01/05/2012 12:57:11  01/05/2012 12:57:11   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325768231_17>
01/05/2012 12:57:09  01/05/2012 12:57:09   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325768229_17>
01/05/2012 12:57:00  01/05/2012 12:57:00   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325768220_17>
01/05/2012 12:56:58  01/05/2012 12:56:58   110     0    11  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1325768218_17>
01/05/2012 12:56:57  01/05/2012 12:56:57   165  6541    10  ERR_LOW_PEP_ALARM  HIGH_ALARM  <UTC:1325768217_17>
01/05/2012 12:53:38  01/05/2012 12:53:38 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325768018_17>
01/05/2012 12:53:38  01/05/2012 12:53:38   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325768018_17>
01/05/2012 11:14:10  01/05/2012 11:14:10   284     0 65535  ERR_PWR_UPGRADE_AC_IN_USE  BEEP_ONLY  <UTC:1325762050_17>
01/05/2012 11:12:37  01/05/2012 11:12:37   179     0 65535  ERR_PWR_REDUCTION_AC_DISCONNECTED  MED_ALARM  <UTC:1325761957_17>
01/05/2012 10:58:33  01/05/2012 10:58:33 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325761113_17>
01/05/2012 10:58:33  01/05/2012 10:58:33   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325761113_17>
01/05/2012 10:58:32  01/05/2012 10:58:32   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325761112_17>
01/05/2012 09:39:01  01/05/2012 09:39:01 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325756341_17>
01/05/2012 09:39:01  01/05/2012 09:39:01   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325756341_17>
01/05/2012 09:01:45  01/05/2012 09:01:45 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325754105_17>
01/05/2012 09:01:45  01/05/2012 09:01:45   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325754105_17>
01/05/2012 09:01:44  01/05/2012 09:01:44   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325754104_17>
01/05/2012 08:39:05  01/05/2012 08:39:05 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325752745_17>
01/05/2012 08:39:05  01/05/2012 08:39:05   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325752745_17>
01/05/2012 08:22:46  01/05/2012 08:22:46 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325751766_17>
01/05/2012 08:22:46  01/05/2012 08:22:46   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325751766_17>
01/05/2012 08:22:45  01/05/2012 08:22:45   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325751765_17>
01/05/2012 06:05:54  01/05/2012 06:05:54 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325743554_17>
01/05/2012 06:05:54  01/05/2012 06:05:54   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325743554_17>
01/05/2012 06:03:18  01/05/2012 06:03:18 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325743398_17>
01/05/2012 06:03:18  01/05/2012 06:03:18   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325743398_17>
01/05/2012 06:03:16  01/05/2012 06:03:16   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325743396_17>
01/04/2012 21:57:56  01/04/2012 21:57:56 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325714276_17>
01/04/2012 21:57:56  01/04/2012 21:57:56   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325714276_17>
01/04/2012 21:57:54  01/04/2012 21:57:54 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325714274_17>
01/04/2012 21:57:54  01/04/2012 21:57:54   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325714274_17>
01/04/2012 21:57:52  01/04/2012 21:57:52   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325714272_17>
01/04/2012 21:55:53  01/04/2012 21:55:53 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325714153_17>
01/04/2012 21:55:53  01/04/2012 21:55:53   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325714153_17>
01/04/2012 21:26:56  01/04/2012 21:26:56   284     0 65535  ERR_PWR_UPGRADE_AC_IN_USE  BEEP_ONLY  <UTC:1325712416_17>
01/04/2012 21:26:25  01/04/2012 21:26:25   179     0 65535  ERR_PWR_REDUCTION_AC_DISCONNECTED  MED_ALARM  <UTC:1325712385_17>
01/04/2012 21:25:26  01/04/2012 21:25:26 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325712326_17>
01/04/2012 21:25:26  01/04/2012 21:25:26   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325712326_17>
01/04/2012 21:25:24  01/04/2012 21:25:24   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325712324_17>
01/04/2012 21:23:11  01/04/2012 21:23:11   264     0 65535  ERR_MENU_BYPASS_ACTIVATED  KEYPRESS  <UTC:1325712191_17>
01/04/2012 21:20:09  01/04/2012 21:20:09 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325712009_17>
01/04/2012 21:20:09  01/04/2012 21:20:09   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325712009_17>
01/04/2012 21:18:34  01/04/2012 21:18:34 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325711914_17>
01/04/2012 21:18:34  01/04/2012 21:18:34   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325711914_17>
01/04/2012 21:18:33  01/04/2012 21:18:33   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325711913_17>
01/04/2012 21:14:53  01/04/2012 21:14:53 17707   600   650      NV_ID= 43 (NV_TIDAL_VOLUME)  P/S=P RX=2  AVAPS=1  <UTC:1325711693_17>
01/04/2012 21:14:48  01/04/2012 21:14:48 17700  2200  2400      NV_ID= 36 (NV_IPAP_MAX_PRESSURE)  P/S=P RX=2  AVAPS=1  <UTC:1325711688_17>
01/04/2012 21:14:44  01/04/2012 21:14:44   264     0 65535  ERR_MENU_BYPASS_ACTIVATED  KEYPRESS  <UTC:1325711684_17>
01/04/2012 21:13:05  01/04/2012 21:13:05 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325711585_17>
01/04/2012 21:13:05  01/04/2012 21:13:05   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325711585_17>
01/04/2012 21:03:14  01/04/2012 21:03:14 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325710994_17>
01/04/2012 21:03:14  01/04/2012 21:03:14   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325710994_17>
01/04/2012 21:03:13  01/04/2012 21:03:13   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325710993_17>
01/04/2012 21:02:56  01/04/2012 21:02:56   110    67    18  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1325710976_17>
01/04/2012 21:00:29  01/04/2012 21:00:29 17711     5     0      NV_ID= 47 (NV_RAMP_LENGTH)  P/S=P RX=2  AVAPS=1  <UTC:1325710829_17>
01/04/2012 21:00:19  01/04/2012 21:00:19 17722    14    15      NV_ID= 58 (NV_APNEA_BREATH_RATE)  P/S=P RX=2  AVAPS=1  <UTC:1325710819_17>
01/04/2012 21:00:19  01/04/2012 21:00:19 17708    14    15      NV_ID= 44 (NV_BREATH_RATE)  P/S=P RX=2  AVAPS=1  <UTC:1325710819_17>
01/04/2012 21:00:05  01/04/2012 21:00:05   264     0 65535  ERR_MENU_BYPASS_ACTIVATED  KEYPRESS  <UTC:1325710805_17>
01/04/2012 20:58:55  01/04/2012 20:58:55 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325710735_17>
01/04/2012 20:58:55  01/04/2012 20:58:55   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325710735_17>
01/04/2012 20:58:55  01/04/2012 20:58:55 16415     1     0      NV_ID= 31 (NV_RAMP_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325710735_17>
01/04/2012 20:58:55  01/04/2012 20:58:55 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325710735_17>
01/04/2012 20:58:55  01/04/2012 20:58:55   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325710735_17>
01/04/2012 20:58:54  01/04/2012 20:58:54   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325710734_17>
01/04/2012 20:58:50  01/04/2012 20:58:50 16415     0     1      NV_ID= 31 (NV_RAMP_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325710730_17>
01/04/2012 20:58:28  01/04/2012 20:58:28 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325710708_17>
01/04/2012 20:58:28  01/04/2012 20:58:28   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325710708_17>
01/04/2012 20:57:45  01/04/2012 20:57:45 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325710665_17>
01/04/2012 20:57:45  01/04/2012 20:57:45   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325710665_17>
01/04/2012 20:57:44  01/04/2012 20:57:44   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325710664_17>
01/04/2012 20:57:43  01/04/2012 20:57:43   110    73     2  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1325710663_17>
01/04/2012 20:57:15  01/04/2012 20:57:15   169   266 65535  ERR_HIGH_PIP_STAGE1_ALARM  BEEP_ONLY  <UTC:1325710635_17>
01/04/2012 20:46:40  01/04/2012 20:46:40 17707   550   600      NV_ID= 43 (NV_TIDAL_VOLUME)  P/S=P RX=2  AVAPS=1  <UTC:1325710000_17>
01/04/2012 20:46:22  01/04/2012 20:46:22   264     0 65535  ERR_MENU_BYPASS_ACTIVATED  KEYPRESS  <UTC:1325709982_17>
01/04/2012 20:46:18  01/04/2012 20:46:18   168     0 65535  ERR_UI_AUDIO_PAUSE_KEY_PRESS  KEYPRESS  <UTC:1325709978_17>
01/04/2012 20:46:12  01/04/2012 20:46:12   168     0 65535  ERR_UI_AUDIO_PAUSE_KEY_PRESS  KEYPRESS  <UTC:1325709972_17>
01/04/2012 20:44:21  01/04/2012 20:44:21 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325709861_17>
01/04/2012 20:44:21  01/04/2012 20:44:21   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325709861_17>
01/04/2012 20:39:07  01/04/2012 20:39:07 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325709547_17>
01/04/2012 20:39:07  01/04/2012 20:39:07   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325709547_17>
01/04/2012 20:39:06  01/04/2012 20:39:06   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325709546_17>
01/04/2012 20:28:20  01/04/2012 20:28:20 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325708900_17>
01/04/2012 20:28:20  01/04/2012 20:28:20   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325708900_17>
01/04/2012 20:27:43  01/04/2012 20:27:43 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325708863_17>
01/04/2012 20:27:43  01/04/2012 20:27:43   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325708863_17>
01/04/2012 20:27:41  01/04/2012 20:27:41   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325708861_17>
01/04/2012 20:25:36  01/04/2012 20:25:36   264     0 65535  ERR_MENU_BYPASS_ACTIVATED  KEYPRESS  <UTC:1325708736_17>
01/04/2012 17:34:22  01/04/2012 17:34:22 16415     1     0      NV_ID= 31 (NV_RAMP_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325698462_17>
01/04/2012 17:29:22  01/04/2012 17:29:22 16415     0     1      NV_ID= 31 (NV_RAMP_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325698162_17>
01/04/2012 17:29:15  01/04/2012 17:29:15 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325698155_17>
01/04/2012 17:29:15  01/04/2012 17:29:15   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325698155_17>
01/04/2012 17:29:14  01/04/2012 17:29:14 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325698154_17>
01/04/2012 17:29:14  01/04/2012 17:29:14   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325698154_17>
01/04/2012 17:29:13  01/04/2012 17:29:13   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325698153_17>
01/04/2012 17:29:00  01/04/2012 17:29:00 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325698140_17>
01/04/2012 17:29:00  01/04/2012 17:29:00   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325698140_17>
01/04/2012 10:33:33  01/04/2012 10:33:33   284     0 65535  ERR_PWR_UPGRADE_AC_IN_USE  BEEP_ONLY  <UTC:1325673213_17>
01/04/2012 10:30:33  01/04/2012 10:30:33   179     0 65535  ERR_PWR_REDUCTION_AC_DISCONNECTED  MED_ALARM  <UTC:1325673033_17>
01/04/2012 08:14:18  01/04/2012 08:14:18 16415     1     0      NV_ID= 31 (NV_RAMP_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325664858_17>
01/04/2012 08:14:18  01/04/2012 08:14:18 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325664858_17>
01/04/2012 08:14:18  01/04/2012 08:14:18   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325664858_17>
01/04/2012 08:14:17  01/04/2012 08:14:17   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325664857_17>
01/04/2012 08:14:16  01/04/2012 08:14:16 16415     0     1      NV_ID= 31 (NV_RAMP_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325664856_17>
01/03/2012 20:16:54  01/03/2012 20:16:54 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325621814_17>
01/03/2012 20:16:54  01/03/2012 20:16:54   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325621814_17>
01/03/2012 08:20:17  01/03/2012 08:20:17 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325578817_17>
01/03/2012 08:20:17  01/03/2012 08:20:17   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325578817_17>
01/03/2012 08:20:16  01/03/2012 08:20:16   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325578816_17>
01/02/2012 20:17:56  01/02/2012 20:17:56 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325535476_17>
01/02/2012 20:17:56  01/02/2012 20:17:56   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325535476_17>
01/02/2012 20:17:55  01/02/2012 20:17:55 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325535475_17>
01/02/2012 20:17:55  01/02/2012 20:17:55   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325535475_17>
01/02/2012 20:17:53  01/02/2012 20:17:53   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325535473_17>
01/02/2012 20:15:40  01/02/2012 20:15:40 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325535340_17>
01/02/2012 20:15:40  01/02/2012 20:15:40   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325535340_17>
01/02/2012 19:42:48  01/02/2012 19:42:48   284     0 65535  ERR_PWR_UPGRADE_AC_IN_USE  BEEP_ONLY  <UTC:1325533368_17>
01/02/2012 19:42:01  01/02/2012 19:42:01   179     0 65535  ERR_PWR_REDUCTION_AC_DISCONNECTED  MED_ALARM  <UTC:1325533321_17>
01/02/2012 19:32:30  01/02/2012 19:32:30 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325532750_17>
01/02/2012 19:32:30  01/02/2012 19:32:30   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325532750_17>
01/02/2012 19:32:29  01/02/2012 19:32:29   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325532749_17>
01/02/2012 17:26:23  01/02/2012 17:26:23 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325525183_17>
01/02/2012 17:26:23  01/02/2012 17:26:23   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325525183_17>
01/02/2012 16:35:48  01/02/2012 16:35:48 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325522148_17>
01/02/2012 16:35:48  01/02/2012 16:35:48   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325522148_17>
01/02/2012 16:35:45  01/02/2012 16:35:45   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325522145_17>
01/02/2012 16:35:42  01/02/2012 16:35:42 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325522142_17>
01/02/2012 16:35:42  01/02/2012 16:35:42   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325522142_17>
01/02/2012 11:41:29  01/02/2012 11:41:29    72     0 65535  ERR_MMC_SD_CARD_INSERTED  BEEP_ONLY  <UTC:1325504489_17>
01/02/2012 11:41:29  01/02/2012 11:41:29   252     0 65535  ERR_INT_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1325504489_17>
01/02/2012 11:41:29  01/02/2012 11:41:29   251     0 65535  ERR_DET_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1325504489_17>
01/02/2012 11:35:32  01/02/2012 11:35:32   179     0 65535  ERR_PWR_REDUCTION_AC_DISCONNECTED  MED_ALARM  <UTC:1325504132_17>
01/02/2012 09:07:09  01/02/2012 09:07:09    72     0 65535  ERR_MMC_SD_CARD_INSERTED  BEEP_ONLY  <UTC:1325495229_17>
01/02/2012 09:07:09  01/02/2012 09:07:09   252     0 65535  ERR_INT_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1325495229_17>
01/02/2012 09:07:09  01/02/2012 09:07:09   251     0 65535  ERR_DET_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1325495229_17>
01/02/2012 08:21:20  01/02/2012 08:21:20   179     0 65535  ERR_PWR_REDUCTION_AC_DISCONNECTED  MED_ALARM  <UTC:1325492480_17>
01/02/2012 08:17:46  01/02/2012 08:17:46 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325492266_17>
01/02/2012 08:17:46  01/02/2012 08:17:46   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325492266_17>
01/02/2012 08:17:45  01/02/2012 08:17:45   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325492265_17>
01/01/2012 23:53:44  01/01/2012 23:53:44 16415     1     0      NV_ID= 31 (NV_RAMP_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325462024_17>
01/01/2012 23:48:44  01/01/2012 23:48:44 16415     0     1      NV_ID= 31 (NV_RAMP_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325461724_17>
01/01/2012 23:48:42  01/01/2012 23:48:42   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1325461722_17>
01/01/2012 23:48:35  01/01/2012 23:48:35   284     0 65535  ERR_PWR_UPGRADE_AC_IN_USE  BEEP_ONLY  <UTC:1325461715_17>
01/01/2012 23:47:44  01/01/2012 23:47:44   173     0 65535  ERR_START_ON_BATTERY  INFO_ALARM  <UTC:1325461664_17>
01/01/2012 23:47:41  01/01/2012 23:47:41    72     0 65535  ERR_MMC_SD_CARD_INSERTED  BEEP_ONLY  <UTC:1325461661_17>
01/01/2012 23:47:41  01/01/2012 23:47:41   252     0 65535  ERR_INT_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1325461661_17>
01/01/2012 23:47:41  01/01/2012 23:47:41   251     0 65535  ERR_DET_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1325461661_17>
01/01/2012 23:47:41  01/01/2012 23:47:41 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325461661_17>
01/01/2012 23:47:41  01/01/2012 23:47:41   324     2 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325461661_17>
01/01/2012 18:56:26  01/01/2012 18:56:26   179     0 65535  ERR_PWR_REDUCTION_AC_DISCONNECTED  MED_ALARM  <UTC:1325444186_17>
01/01/2012 12:31:03  01/01/2012 12:31:03 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325421063_17>
01/01/2012 12:31:03  01/01/2012 12:31:03   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325421063_17>
01/01/2012 12:31:03  01/01/2012 12:31:03   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325421063_17>
01/01/2012 12:24:24  01/01/2012 12:24:24 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325420664_17>
01/01/2012 12:24:24  01/01/2012 12:24:24   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325420664_17>
01/01/2012 12:07:55  01/01/2012 12:07:55 16415     1     0      NV_ID= 31 (NV_RAMP_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325419675_17>
01/01/2012 12:07:55  01/01/2012 12:07:55 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325419675_17>
01/01/2012 12:07:55  01/01/2012 12:07:55   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325419675_17>
01/01/2012 12:07:54  01/01/2012 12:07:54   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325419674_17>
01/01/2012 12:07:53  01/01/2012 12:07:53   295     0 65535  ERR_POWER_OFF_NO_KEY  KEYPRESS  <UTC:1325419673_17>
01/01/2012 12:07:52  01/01/2012 12:07:52   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325419672_17>
01/01/2012 12:07:52  01/01/2012 12:07:52 16415     0     1      NV_ID= 31 (NV_RAMP_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325419672_17>
01/01/2012 10:37:35  01/01/2012 10:37:35 16415     1     0      NV_ID= 31 (NV_RAMP_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325414255_17>
01/01/2012 10:32:35  01/01/2012 10:32:35 16415     0     1      NV_ID= 31 (NV_RAMP_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325413955_17>
01/01/2012 10:32:28  01/01/2012 10:32:28 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325413948_17>
01/01/2012 10:32:28  01/01/2012 10:32:28   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325413948_17>
01/01/2012 10:12:26  01/01/2012 10:12:26 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325412746_17>
01/01/2012 10:12:26  01/01/2012 10:12:26   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325412746_17>
01/01/2012 10:12:25  01/01/2012 10:12:25   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325412745_17>
01/01/2012 10:12:23  01/01/2012 10:12:23   168     0 65535  ERR_UI_AUDIO_PAUSE_KEY_PRESS  KEYPRESS  <UTC:1325412743_17>
01/01/2012 03:37:02  01/01/2012 03:37:02 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325389022_17>
01/01/2012 03:37:02  01/01/2012 03:37:02   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325389022_17>
01/01/2012 03:17:25  01/01/2012 03:17:25 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325387845_17>
01/01/2012 03:17:25  01/01/2012 03:17:25   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325387845_17>
01/01/2012 03:17:24  01/01/2012 03:17:24   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325387844_17>
01/01/2012 00:59:05  01/01/2012 00:59:05 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325379545_17>
01/01/2012 00:59:05  01/01/2012 00:59:05   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325379545_17>
01/01/2012 00:35:53  01/01/2012 00:35:53    72     0 65535  ERR_MMC_SD_CARD_INSERTED  BEEP_ONLY  <UTC:1325378153_17>
01/01/2012 00:35:53  01/01/2012 00:35:53   252     0 65535  ERR_INT_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1325378153_17>
01/01/2012 00:35:53  01/01/2012 00:35:53   251     0 65535  ERR_DET_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1325378153_17>
12/31/2011 15:31:37  12/31/2011 15:31:37 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325345497_17>
12/31/2011 15:31:37  12/31/2011 15:31:37   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325345497_17>
12/31/2011 15:31:33  12/31/2011 15:31:33   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325345493_17>
12/31/2011 15:12:40  12/31/2011 15:12:40   173     0 65535  ERR_START_ON_BATTERY  INFO_ALARM  <UTC:1325344360_17>
12/31/2011 15:12:40  12/31/2011 15:12:40   286     0 65535  ERR_PWR_UPGRADE_DET_LI_ION_IN_USE  BEEP_ONLY  <UTC:1325344360_17>
12/31/2011 15:12:37  12/31/2011 15:12:37    72     0 65535  ERR_MMC_SD_CARD_INSERTED  BEEP_ONLY  <UTC:1325344357_17>
12/31/2011 15:12:37  12/31/2011 15:12:37   252     0 65535  ERR_INT_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1325344357_17>
12/31/2011 15:12:37  12/31/2011 15:12:37   251     0 65535  ERR_DET_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1325344357_17>
12/31/2011 15:12:37  12/31/2011 15:12:37 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325344357_17>
12/31/2011 15:12:37  12/31/2011 15:12:37   324     2 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325344357_17>
12/31/2011 15:05:17  12/31/2011 15:05:17 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325343917_17>
12/31/2011 15:05:17  12/31/2011 15:05:17   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325343917_17>
12/31/2011 15:05:16  12/31/2011 15:05:16   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325343916_17>
12/31/2011 12:29:29  12/31/2011 12:29:29   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1325334569_17>
12/31/2011 12:28:19  12/31/2011 12:28:19   173     0 65535  ERR_START_ON_BATTERY  INFO_ALARM  <UTC:1325334499_17>
12/31/2011 12:28:16  12/31/2011 12:28:16    72     0 65535  ERR_MMC_SD_CARD_INSERTED  BEEP_ONLY  <UTC:1325334496_17>
12/31/2011 12:28:16  12/31/2011 12:28:16   252     0 65535  ERR_INT_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1325334496_17>
12/31/2011 12:28:16  12/31/2011 12:28:16   251     0 65535  ERR_DET_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1325334496_17>
12/31/2011 12:28:16  12/31/2011 12:28:16 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325334496_17>
12/31/2011 12:28:16  12/31/2011 12:28:16   324     2 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325334496_17>
12/31/2011 08:33:25  12/31/2011 08:33:25   179     0 65535  ERR_PWR_REDUCTION_AC_DISCONNECTED  MED_ALARM  <UTC:1325320405_17>
12/31/2011 08:31:14  12/31/2011 08:31:14 16415     1     0      NV_ID= 31 (NV_RAMP_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325320274_17>
12/31/2011 08:31:14  12/31/2011 08:31:14 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325320274_17>
12/31/2011 08:31:14  12/31/2011 08:31:14   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325320274_17>
12/31/2011 08:31:13  12/31/2011 08:31:13   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325320273_17>
12/31/2011 08:30:07  12/31/2011 08:30:07 16415     0     1      NV_ID= 31 (NV_RAMP_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325320207_17>
12/31/2011 02:42:10  12/31/2011 02:42:10 16415     1     0      NV_ID= 31 (NV_RAMP_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325299330_17>
12/31/2011 02:37:10  12/31/2011 02:37:10 16415     0     1      NV_ID= 31 (NV_RAMP_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325299030_17>
12/31/2011 02:37:07  12/31/2011 02:37:07 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325299027_17>
12/31/2011 02:37:07  12/31/2011 02:37:07   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325299027_17>
12/31/2011 01:20:16  12/31/2011 01:20:16 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325294416_17>
12/31/2011 01:20:16  12/31/2011 01:20:16   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325294416_17>
12/31/2011 01:20:15  12/31/2011 01:20:15   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325294415_17>
12/31/2011 01:20:14  12/31/2011 01:20:14   110     0     2  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1325294414_17>
12/31/2011 01:20:14  12/31/2011 01:20:14   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325294414_17>
12/31/2011 01:20:13  12/31/2011 01:20:13   165  6492     3  ERR_LOW_PEP_ALARM  HIGH_ALARM  <UTC:1325294413_17>
12/31/2011 01:20:07  12/31/2011 01:20:07 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325294407_17>
12/31/2011 01:20:07  12/31/2011 01:20:07   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325294407_17>
12/31/2011 01:20:06  12/31/2011 01:20:06    72     0 65535  ERR_MMC_SD_CARD_INSERTED  BEEP_ONLY  <UTC:1325294406_17>
12/31/2011 01:20:06  12/31/2011 01:20:06   252     0 65535  ERR_INT_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1325294406_17>
12/31/2011 01:20:06  12/31/2011 01:20:06   251     0 65535  ERR_DET_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1325294406_17>
12/30/2011 16:51:21  12/30/2011 16:51:21   179     0 65535  ERR_PWR_REDUCTION_AC_DISCONNECTED  MED_ALARM  <UTC:1325263881_17>
12/30/2011 08:37:33  12/30/2011 08:37:33   284     0 65535  ERR_PWR_UPGRADE_AC_IN_USE  BEEP_ONLY  <UTC:1325234253_17>
12/30/2011 08:35:37  12/30/2011 08:35:37   179     0 65535  ERR_PWR_REDUCTION_AC_DISCONNECTED  MED_ALARM  <UTC:1325234137_17>
12/30/2011 08:23:42  12/30/2011 08:23:42 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325233422_17>
12/30/2011 08:23:42  12/30/2011 08:23:42   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325233422_17>
12/30/2011 08:23:41  12/30/2011 08:23:41   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325233421_17>
12/29/2011 20:13:53  12/29/2011 20:13:53 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325189633_17>
12/29/2011 20:13:53  12/29/2011 20:13:53   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325189633_17>
12/29/2011 20:13:52  12/29/2011 20:13:52 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325189632_17>
12/29/2011 20:13:52  12/29/2011 20:13:52   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325189632_17>
12/29/2011 20:13:51  12/29/2011 20:13:51   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325189631_17>
12/29/2011 20:12:26  12/29/2011 20:12:26 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325189546_17>
12/29/2011 20:12:26  12/29/2011 20:12:26   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325189546_17>
12/29/2011 19:41:33  12/29/2011 19:41:33   284     0 65535  ERR_PWR_UPGRADE_AC_IN_USE  BEEP_ONLY  <UTC:1325187693_17>
12/29/2011 19:40:52  12/29/2011 19:40:52   179     0 65535  ERR_PWR_REDUCTION_AC_DISCONNECTED  MED_ALARM  <UTC:1325187652_17>
12/29/2011 08:47:53  12/29/2011 08:47:53    72     0 65535  ERR_MMC_SD_CARD_INSERTED  BEEP_ONLY  <UTC:1325148473_17>
12/29/2011 08:47:53  12/29/2011 08:47:53   252     0 65535  ERR_INT_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1325148473_17>
12/29/2011 08:47:53  12/29/2011 08:47:53   251     0 65535  ERR_DET_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1325148473_17>
12/29/2011 08:30:50  12/29/2011 08:30:50   179     0 65535  ERR_PWR_REDUCTION_AC_DISCONNECTED  MED_ALARM  <UTC:1325147450_17>
12/29/2011 08:17:38  12/29/2011 08:17:38 16415     1     0      NV_ID= 31 (NV_RAMP_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325146658_17>
12/29/2011 08:17:38  12/29/2011 08:17:38 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325146658_17>
12/29/2011 08:17:38  12/29/2011 08:17:38   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325146658_17>
12/29/2011 08:17:37  12/29/2011 08:17:37   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325146657_17>
12/29/2011 08:17:35  12/29/2011 08:17:35 16415     0     1      NV_ID= 31 (NV_RAMP_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325146655_17>
12/28/2011 23:12:22  12/28/2011 23:12:22 16415     1     0      NV_ID= 31 (NV_RAMP_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325113942_17>
12/28/2011 23:07:22  12/28/2011 23:07:22 16415     0     1      NV_ID= 31 (NV_RAMP_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325113642_17>
12/28/2011 20:11:52  12/28/2011 20:11:52 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325103112_17>
12/28/2011 20:11:52  12/28/2011 20:11:52   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325103112_17>
12/28/2011 20:11:51  12/28/2011 20:11:51 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325103111_17>
12/28/2011 20:11:51  12/28/2011 20:11:51   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325103111_17>
12/28/2011 20:11:50  12/28/2011 20:11:50   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325103110_17>
12/28/2011 20:10:50  12/28/2011 20:10:50 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325103050_17>
12/28/2011 20:10:50  12/28/2011 20:10:50   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325103050_17>
12/28/2011 19:41:47  12/28/2011 19:41:47   284     0 65535  ERR_PWR_UPGRADE_AC_IN_USE  BEEP_ONLY  <UTC:1325101307_17>
12/28/2011 19:41:10  12/28/2011 19:41:10   179     0 65535  ERR_PWR_REDUCTION_AC_DISCONNECTED  MED_ALARM  <UTC:1325101270_17>
12/28/2011 19:39:19  12/28/2011 19:39:19 16415     1     0      NV_ID= 31 (NV_RAMP_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325101159_17>
12/28/2011 19:39:19  12/28/2011 19:39:19 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325101159_17>
12/28/2011 19:39:19  12/28/2011 19:39:19   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325101159_17>
12/28/2011 19:39:18  12/28/2011 19:39:18   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325101158_17>
12/28/2011 19:39:17  12/28/2011 19:39:17 16415     0     1      NV_ID= 31 (NV_RAMP_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325101157_17>
12/28/2011 17:30:48  12/28/2011 17:30:48 16415     1     0      NV_ID= 31 (NV_RAMP_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325093448_17>
12/28/2011 17:25:48  12/28/2011 17:25:48 16415     0     1      NV_ID= 31 (NV_RAMP_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325093148_17>
12/28/2011 17:25:43  12/28/2011 17:25:43 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325093143_17>
12/28/2011 17:25:43  12/28/2011 17:25:43   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325093143_17>
12/28/2011 11:09:21  12/28/2011 11:09:21 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325070561_17>
12/28/2011 11:09:21  12/28/2011 11:09:21   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325070561_17>
12/28/2011 11:09:20  12/28/2011 11:09:20   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325070560_17>
12/28/2011 11:09:01  12/28/2011 11:09:01   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325070541_17>
12/28/2011 11:08:37  12/28/2011 11:08:37 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325070517_17>
12/28/2011 11:08:37  12/28/2011 11:08:37   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325070517_17>
12/28/2011 08:23:11  12/28/2011 08:23:11   284     0 65535  ERR_PWR_UPGRADE_AC_IN_USE  BEEP_ONLY  <UTC:1325060591_17>
12/28/2011 08:22:27  12/28/2011 08:22:27   179     0 65535  ERR_PWR_REDUCTION_AC_DISCONNECTED  MED_ALARM  <UTC:1325060547_17>
12/28/2011 08:08:58  12/28/2011 08:08:58 16415     1     0      NV_ID= 31 (NV_RAMP_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325059738_17>
12/28/2011 08:08:58  12/28/2011 08:08:58 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325059738_17>
12/28/2011 08:08:58  12/28/2011 08:08:58   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325059738_17>
12/28/2011 08:08:57  12/28/2011 08:08:57   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325059737_17>
12/28/2011 08:08:55  12/28/2011 08:08:55 16415     0     1      NV_ID= 31 (NV_RAMP_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325059735_17>
12/27/2011 20:13:13  12/27/2011 20:13:13 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325016793_17>
12/27/2011 20:13:13  12/27/2011 20:13:13   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1325016793_17>
12/27/2011 15:34:58  12/27/2011 15:34:58 16415     1     0      NV_ID= 31 (NV_RAMP_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325000098_17>
12/27/2011 15:34:58  12/27/2011 15:34:58 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1325000098_17>
12/27/2011 15:34:58  12/27/2011 15:34:58   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1325000098_17>
12/27/2011 15:34:58  12/27/2011 15:34:58   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1325000098_17>
12/27/2011 15:34:36  12/27/2011 15:34:36   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1325000076_17>
12/27/2011 15:34:31  12/27/2011 15:34:31   284     0 65535  ERR_PWR_UPGRADE_AC_IN_USE  BEEP_ONLY  <UTC:1325000071_17>
12/27/2011 15:34:22  12/27/2011 15:34:22   179     0 65535  ERR_PWR_REDUCTION_AC_DISCONNECTED  MED_ALARM  <UTC:1325000062_17>
12/27/2011 15:34:09  12/27/2011 15:34:09   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1325000049_17>
12/27/2011 15:34:00  12/27/2011 15:34:00   284     0 65535  ERR_PWR_UPGRADE_AC_IN_USE  BEEP_ONLY  <UTC:1325000040_17>
12/27/2011 15:33:44  12/27/2011 15:33:44   179     0 65535  ERR_PWR_REDUCTION_AC_DISCONNECTED  MED_ALARM  <UTC:1325000024_17>
12/27/2011 15:32:11  12/27/2011 15:32:11 16415     0     1      NV_ID= 31 (NV_RAMP_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1324999931_17>
12/27/2011 15:31:57  12/27/2011 15:31:57 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1324999917_17>
12/27/2011 15:31:57  12/27/2011 15:31:57   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1324999917_17>
12/27/2011 15:31:51  12/27/2011 15:31:51 16415     1     0      NV_ID= 31 (NV_RAMP_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1324999911_17>
12/27/2011 15:31:51  12/27/2011 15:31:51 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1324999911_17>
12/27/2011 15:31:51  12/27/2011 15:31:51   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1324999911_17>
12/27/2011 15:31:50  12/27/2011 15:31:50   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1324999910_17>
12/27/2011 15:30:35  12/27/2011 15:30:35 16415     0     1      NV_ID= 31 (NV_RAMP_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1324999835_17>
12/27/2011 15:30:25  12/27/2011 15:30:25 16415     1     0      NV_ID= 31 (NV_RAMP_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1324999825_17>
12/27/2011 15:30:06  12/27/2011 15:30:06   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1324999806_17>
12/27/2011 15:30:01  12/27/2011 15:30:01   284     0 65535  ERR_PWR_UPGRADE_AC_IN_USE  BEEP_ONLY  <UTC:1324999801_17>
12/27/2011 15:29:23  12/27/2011 15:29:23   179     0 65535  ERR_PWR_REDUCTION_AC_DISCONNECTED  MED_ALARM  <UTC:1324999763_17>
12/27/2011 15:27:20  12/27/2011 15:27:20   251     0 65535  ERR_DET_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1324999640_17>
12/27/2011 15:25:07  12/27/2011 15:25:07 16415     0     1      NV_ID= 31 (NV_RAMP_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1324999507_17>
12/27/2011 15:25:06  12/27/2011 15:25:06   251     0 65535  ERR_DET_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1324999506_17>
12/27/2011 15:24:15  12/27/2011 15:24:15   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1324999455_17>
12/27/2011 15:24:00  12/27/2011 15:24:00   282     0 65535  ERR_INT_LI_ION_DEPLETED  HIGH_ALARM  <UTC:1324999440_17>
12/27/2011 15:23:56  12/27/2011 15:23:56 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1324999436_17>
12/27/2011 15:23:56  12/27/2011 15:23:56   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1324999436_17>
12/27/2011 15:23:07  12/27/2011 15:23:07   284     0 65535  ERR_PWR_UPGRADE_AC_IN_USE  BEEP_ONLY  <UTC:1324999387_17>
12/27/2011 15:21:46  12/27/2011 15:21:46   179     0 65535  ERR_PWR_REDUCTION_AC_DISCONNECTED  MED_ALARM  <UTC:1324999306_17>
12/27/2011 15:16:54  12/27/2011 15:16:54 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1324999014_17>
12/27/2011 15:16:54  12/27/2011 15:16:54   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1324999014_17>
12/27/2011 15:16:53  12/27/2011 15:16:53   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1324999013_17>
12/27/2011 15:16:53  12/27/2011 15:16:53   110     0     1  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1324999013_17>
12/27/2011 15:16:52  12/27/2011 15:16:52   165  6495     2  ERR_LOW_PEP_ALARM  HIGH_ALARM  <UTC:1324999012_17>
12/27/2011 15:16:51  12/27/2011 15:16:51   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1324999011_17>
12/27/2011 15:16:49  12/27/2011 15:16:49   282     0 65535  ERR_INT_LI_ION_DEPLETED  HIGH_ALARM  <UTC:1324999009_17>
12/27/2011 15:16:46  12/27/2011 15:16:46 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1324999006_17>
12/27/2011 15:16:46  12/27/2011 15:16:46   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1324999006_17>
12/27/2011 15:16:01  12/27/2011 15:16:01 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1324998961_17>
12/27/2011 15:16:01  12/27/2011 15:16:01   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1324998961_17>
12/27/2011 15:16:00  12/27/2011 15:16:00   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1324998960_17>
12/27/2011 15:15:59  12/27/2011 15:15:59   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1324998959_17>
12/27/2011 15:15:58  12/27/2011 15:15:58   110     0     1  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1324998958_17>
12/27/2011 15:15:58  12/27/2011 15:15:58   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1324998958_17>
12/27/2011 15:15:54  12/27/2011 15:15:54   110     0     4  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1324998954_17>
12/27/2011 15:15:52  12/27/2011 15:15:52   165  6495     6  ERR_LOW_PEP_ALARM  HIGH_ALARM  <UTC:1324998952_17>
12/27/2011 15:15:50  12/27/2011 15:15:50   282     0 65535  ERR_INT_LI_ION_DEPLETED  HIGH_ALARM  <UTC:1324998950_17>
12/27/2011 15:15:47  12/27/2011 15:15:47 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1324998947_17>
12/27/2011 15:15:47  12/27/2011 15:15:47   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1324998947_17>
12/27/2011 15:15:44  12/27/2011 15:15:44   284     0 65535  ERR_PWR_UPGRADE_AC_IN_USE  BEEP_ONLY  <UTC:1324998944_17>
12/27/2011 15:14:49  12/27/2011 15:14:49   179     0 65535  ERR_PWR_REDUCTION_AC_DISCONNECTED  MED_ALARM  <UTC:1324998889_17>
12/27/2011 15:13:57  12/27/2011 15:13:57 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1324998837_17>
12/27/2011 15:13:57  12/27/2011 15:13:57   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1324998837_17>
12/27/2011 15:13:57  12/27/2011 15:13:57   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1324998837_17>
12/27/2011 15:13:55  12/27/2011 15:13:55   110     0     2  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1324998835_17>
12/27/2011 15:13:54  12/27/2011 15:13:54   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1324998834_17>
12/27/2011 15:13:53  12/27/2011 15:13:53   165  6495     1  ERR_LOW_PEP_ALARM  HIGH_ALARM  <UTC:1324998833_17>
12/27/2011 15:13:53  12/27/2011 15:13:53   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1324998833_17>
12/27/2011 15:13:33  12/27/2011 15:13:33   110     0    20  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1324998813_17>
12/27/2011 15:13:32  12/27/2011 15:13:32   165  6494    21  ERR_LOW_PEP_ALARM  HIGH_ALARM  <UTC:1324998812_17>
12/27/2011 15:13:30  12/27/2011 15:13:30   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1324998810_17>
12/27/2011 15:13:29  12/27/2011 15:13:29   110     0     1  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1324998809_17>
12/27/2011 15:13:28  12/27/2011 15:13:28   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1324998808_17>
12/27/2011 15:13:28  12/27/2011 15:13:28   165  6494     0  ERR_LOW_PEP_ALARM  HIGH_ALARM  <UTC:1324998808_17>
12/27/2011 15:13:25  12/27/2011 15:13:25   110     0     3  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1324998805_17>
12/27/2011 15:13:24  12/27/2011 15:13:24   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1324998804_17>
12/27/2011 15:13:12  12/27/2011 15:13:12   110     0    12  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1324998792_17>
12/27/2011 15:13:10  12/27/2011 15:13:10   165  6494    14  ERR_LOW_PEP_ALARM  HIGH_ALARM  <UTC:1324998790_17>
12/27/2011 15:13:09  12/27/2011 15:13:09   251     0 65535  ERR_DET_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1324998789_17>
12/27/2011 15:13:09  12/27/2011 15:13:09   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1324998789_17>
12/27/2011 15:12:59  12/27/2011 15:12:59   110     0    10  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1324998779_17>
12/27/2011 15:12:58  12/27/2011 15:12:58   165  6494    11  ERR_LOW_PEP_ALARM  HIGH_ALARM  <UTC:1324998778_17>
12/27/2011 15:12:55  12/27/2011 15:12:55   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1324998775_17>
12/27/2011 15:12:24  12/27/2011 15:12:24   110     0    31  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1324998744_17>
12/27/2011 15:12:23  12/27/2011 15:12:23   165  6494    32  ERR_LOW_PEP_ALARM  HIGH_ALARM  <UTC:1324998743_17>
12/27/2011 15:12:21  12/27/2011 15:12:21   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1324998741_17>
12/27/2011 15:12:20  12/27/2011 15:12:20   110     0     1  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1324998740_17>
12/27/2011 15:12:19  12/27/2011 15:12:19   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1324998739_17>
12/27/2011 15:12:19  12/27/2011 15:12:19   165  6494     2  ERR_LOW_PEP_ALARM  HIGH_ALARM  <UTC:1324998739_17>
12/27/2011 15:12:18  12/27/2011 15:12:18   251     0 65535  ERR_DET_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1324998738_17>
12/27/2011 15:12:02  12/27/2011 15:12:02   165  6494    17  ERR_LOW_PEP_ALARM  HIGH_ALARM  <UTC:1324998722_17>
12/27/2011 15:11:59  12/27/2011 15:11:59   110     0    20  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1324998719_17>
12/27/2011 15:11:58  12/27/2011 15:11:58   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1324998718_17>
12/27/2011 15:11:50  12/27/2011 15:11:50   110     0     8  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1324998710_17>
12/27/2011 15:11:49  12/27/2011 15:11:49   165  6494     9  ERR_LOW_PEP_ALARM  HIGH_ALARM  <UTC:1324998709_17>
12/27/2011 15:11:47  12/27/2011 15:11:47   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1324998707_17>
12/27/2011 15:11:46  12/27/2011 15:11:46   110     0     1  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1324998706_17>
12/27/2011 15:11:44  12/27/2011 15:11:44   165  6494     3  ERR_LOW_PEP_ALARM  HIGH_ALARM  <UTC:1324998704_17>
12/27/2011 15:11:44  12/27/2011 15:11:44   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1324998704_17>
12/27/2011 15:11:43  12/27/2011 15:11:43   251     0 65535  ERR_DET_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1324998703_17>
12/27/2011 15:11:27  12/27/2011 15:11:27   165  6494    17  ERR_LOW_PEP_ALARM  HIGH_ALARM  <UTC:1324998687_17>
12/27/2011 15:11:24  12/27/2011 15:11:24   110     0    20  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1324998684_17>
12/27/2011 15:11:24  12/27/2011 15:11:24   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1324998684_17>
12/27/2011 15:11:23  12/27/2011 15:11:23   165  6494     1  ERR_LOW_PEP_ALARM  HIGH_ALARM  <UTC:1324998683_17>
12/27/2011 15:11:23  12/27/2011 15:11:23   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1324998683_17>
12/27/2011 15:11:01  12/27/2011 15:11:01   165  6494    22  ERR_LOW_PEP_ALARM  HIGH_ALARM  <UTC:1324998661_17>
12/27/2011 15:08:56  12/27/2011 15:08:56   110    14   147  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1324998536_17>
12/27/2011 15:08:53  12/27/2011 15:08:53   282     0 65535  ERR_INT_LI_ION_DEPLETED  HIGH_ALARM  <UTC:1324998533_17>
12/27/2011 15:08:50  12/27/2011 15:08:50 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1324998530_17>
12/27/2011 15:08:50  12/27/2011 15:08:50   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1324998530_17>
12/27/2011 15:08:38  12/27/2011 15:08:38 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1324998518_17>
12/27/2011 15:08:38  12/27/2011 15:08:38   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1324998518_17>
12/27/2011 15:08:37  12/27/2011 15:08:37   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1324998517_17>
12/27/2011 15:08:22  12/27/2011 15:08:22   110    15    16  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1324998502_17>
12/27/2011 15:08:18  12/27/2011 15:08:18   282     0 65535  ERR_INT_LI_ION_DEPLETED  HIGH_ALARM  <UTC:1324998498_17>
12/27/2011 15:08:15  12/27/2011 15:08:15 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1324998495_17>
12/27/2011 15:08:15  12/27/2011 15:08:15   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1324998495_17>
12/27/2011 15:08:02  12/27/2011 15:08:02   284     0 65535  ERR_PWR_UPGRADE_AC_IN_USE  BEEP_ONLY  <UTC:1324998482_17>
12/27/2011 15:07:19  12/27/2011 15:07:19 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1324998439_17>
12/27/2011 15:07:17  12/27/2011 15:07:17   110    14     2  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1324998437_17>
12/27/2011 15:07:14  12/27/2011 15:07:14   173     0 65535  ERR_START_ON_BATTERY  INFO_ALARM  <UTC:1324998434_17>
12/27/2011 15:07:14  12/27/2011 15:07:14   282     0 65535  ERR_INT_LI_ION_DEPLETED  HIGH_ALARM  <UTC:1324998434_17>
12/27/2011 15:07:11  12/27/2011 15:07:11 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1324998431_17>
12/27/2011 15:07:11  12/27/2011 15:07:11   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1324998431_17>
12/27/2011 15:07:08  12/27/2011 15:07:08   281     0 65535  ERR_PWR_REDUCTION_DET_LI_ION_DEPLETED  INFO_ALARM  <UTC:1324998428_17>
12/27/2011 15:07:07  12/27/2011 15:07:07   179     0 65535  ERR_PWR_REDUCTION_AC_DISCONNECTED  MED_ALARM  <UTC:1324998427_17>
12/27/2011 15:06:59  12/27/2011 15:06:59 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1324998419_17>
12/27/2011 15:06:59  12/27/2011 15:06:59 16415     1     0      NV_ID= 31 (NV_RAMP_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1324998419_17>
12/27/2011 15:06:59  12/27/2011 15:06:59   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1324998419_17>
12/27/2011 15:06:59  12/27/2011 15:06:59   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1324998419_17>
12/27/2011 15:06:38  12/27/2011 15:06:38   110     5    21  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1324998398_17>
12/27/2011 15:06:11  12/27/2011 15:06:11   251     0 65535  ERR_DET_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1324998371_17>
12/27/2011 15:06:01  12/27/2011 15:06:01   169   119 65535  ERR_HIGH_PIP_STAGE1_ALARM  BEEP_ONLY  <UTC:1324998361_17>
12/27/2011 15:05:32  12/27/2011 15:05:32 16415     0     1      NV_ID= 31 (NV_RAMP_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1324998332_17>
12/27/2011 15:05:19  12/27/2011 15:05:19   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1324998319_17>
12/27/2011 15:04:13  12/27/2011 15:04:13   169   216 65535  ERR_HIGH_PIP_STAGE1_ALARM  BEEP_ONLY  <UTC:1324998253_17>
12/27/2011 15:04:10  12/27/2011 15:04:10   110    37     3  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1324998250_17>
12/27/2011 15:04:06  12/27/2011 15:04:06   168     0 65535  ERR_UI_AUDIO_PAUSE_KEY_PRESS  KEYPRESS  <UTC:1324998246_17>
12/27/2011 15:02:59  12/27/2011 15:02:59   110     0    62  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1324998179_17>
12/27/2011 15:02:57  12/27/2011 15:02:57   165  6493    63  ERR_LOW_PEP_ALARM  HIGH_ALARM  <UTC:1324998177_17>
12/27/2011 15:02:53  12/27/2011 15:02:53   264     0 65535  ERR_MENU_BYPASS_ACTIVATED  KEYPRESS  <UTC:1324998173_17>
12/27/2011 15:02:50  12/27/2011 15:02:50   169   209 65535  ERR_HIGH_PIP_STAGE1_ALARM  BEEP_ONLY  <UTC:1324998170_17>
12/27/2011 15:02:35  12/27/2011 15:02:35   168     0 65535  ERR_UI_AUDIO_PAUSE_KEY_PRESS  KEYPRESS  <UTC:1324998155_17>
12/27/2011 15:02:28  12/27/2011 15:02:28   110     0     8  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1324998148_17>
12/27/2011 15:02:26  12/27/2011 15:02:26   165  6493     9  ERR_LOW_PEP_ALARM  HIGH_ALARM  <UTC:1324998146_17>
12/27/2011 15:02:24  12/27/2011 15:02:24   282     0 65535  ERR_INT_LI_ION_DEPLETED  HIGH_ALARM  <UTC:1324998144_17>
12/27/2011 15:02:21  12/27/2011 15:02:21 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1324998141_17>
12/27/2011 15:02:21  12/27/2011 15:02:21   324     3 65535  ERR_POWER_ON  KEYPRESS  <UTC:1324998141_17>
12/27/2011 15:02:21  12/27/2011 15:02:21   284     0 65535  ERR_PWR_UPGRADE_AC_IN_USE  BEEP_ONLY  <UTC:1324998141_17>
12/27/2011 15:02:08  12/27/2011 15:02:08 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1324998128_17>
12/27/2011 15:02:07  12/27/2011 15:02:07   110     0     1  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1324998127_17>
12/27/2011 15:02:06  12/27/2011 15:02:06   165  6494     2  ERR_LOW_PEP_ALARM  HIGH_ALARM  <UTC:1324998126_17>
12/27/2011 15:02:04  12/27/2011 15:02:04   173     0 65535  ERR_START_ON_BATTERY  INFO_ALARM  <UTC:1324998124_17>
12/27/2011 15:02:04  12/27/2011 15:02:04   282     0 65535  ERR_INT_LI_ION_DEPLETED  HIGH_ALARM  <UTC:1324998124_17>
12/27/2011 15:02:00  12/27/2011 15:02:00 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1324998120_17>
12/27/2011 15:02:00  12/27/2011 15:02:00   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1324998120_17>
12/27/2011 15:01:49  12/27/2011 15:01:49   281     0 65535  ERR_PWR_REDUCTION_DET_LI_ION_DEPLETED  INFO_ALARM  <UTC:1324998109_17>
12/27/2011 15:01:48  12/27/2011 15:01:48   179     0 65535  ERR_PWR_REDUCTION_AC_DISCONNECTED  MED_ALARM  <UTC:1324998108_17>
12/27/2011 15:01:41  12/27/2011 15:01:41 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1324998101_17>
12/27/2011 15:01:41  12/27/2011 15:01:41   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1324998101_17>
12/27/2011 15:01:41  12/27/2011 15:01:41   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1324998101_17>
12/27/2011 15:01:29  12/27/2011 15:01:29   110     0    12  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1324998089_17>
12/27/2011 15:01:28  12/27/2011 15:01:28   165  6493    13  ERR_LOW_PEP_ALARM  HIGH_ALARM  <UTC:1324998088_17>
12/27/2011 15:01:26  12/27/2011 15:01:26   282     0 65535  ERR_INT_LI_ION_DEPLETED  HIGH_ALARM  <UTC:1324998086_17>
12/27/2011 15:01:22  12/27/2011 15:01:22 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1324998082_17>
12/27/2011 15:01:22  12/27/2011 15:01:22   324     3 65535  ERR_POWER_ON  KEYPRESS  <UTC:1324998082_17>
12/27/2011 15:01:22  12/27/2011 15:01:22   284     0 65535  ERR_PWR_UPGRADE_AC_IN_USE  BEEP_ONLY  <UTC:1324998082_17>
12/27/2011 15:00:59  12/27/2011 15:00:59 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1324998059_17>
12/27/2011 15:00:59  12/27/2011 15:00:59   173     0 65535  ERR_START_ON_BATTERY  INFO_ALARM  <UTC:1324998059_17>
12/27/2011 15:00:59  12/27/2011 15:00:59   282     0 65535  ERR_INT_LI_ION_DEPLETED  HIGH_ALARM  <UTC:1324998059_17>
12/27/2011 15:00:56  12/27/2011 15:00:56 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1324998056_17>
12/27/2011 15:00:56  12/27/2011 15:00:56   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1324998056_17>
12/27/2011 15:00:26  12/27/2011 15:00:26 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1324998026_17>
12/27/2011 15:00:26  12/27/2011 15:00:26   173     0 65535  ERR_START_ON_BATTERY  INFO_ALARM  <UTC:1324998026_17>
12/27/2011 15:00:26  12/27/2011 15:00:26   282     0 65535  ERR_INT_LI_ION_DEPLETED  HIGH_ALARM  <UTC:1324998026_17>
12/27/2011 15:00:23  12/27/2011 15:00:23 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1324998023_17>
12/27/2011 15:00:23  12/27/2011 15:00:23   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1324998023_17>
12/27/2011 14:59:49  12/27/2011 14:59:49 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1324997989_17>
12/27/2011 14:59:49  12/27/2011 14:59:49   173     0 65535  ERR_START_ON_BATTERY  INFO_ALARM  <UTC:1324997989_17>
12/27/2011 14:59:49  12/27/2011 14:59:49   282     0 65535  ERR_INT_LI_ION_DEPLETED  HIGH_ALARM  <UTC:1324997989_17>
12/27/2011 14:59:46  12/27/2011 14:59:46 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1324997986_17>
12/27/2011 14:59:46  12/27/2011 14:59:46   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1324997986_17>
12/27/2011 14:59:41  12/27/2011 14:59:41 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1324997981_17>
12/27/2011 14:59:40  12/27/2011 14:59:40   173     0 65535  ERR_START_ON_BATTERY  INFO_ALARM  <UTC:1324997980_17>
12/27/2011 14:59:40  12/27/2011 14:59:40   282     0 65535  ERR_INT_LI_ION_DEPLETED  HIGH_ALARM  <UTC:1324997980_17>
12/27/2011 14:59:38  12/27/2011 14:59:38   281     0 65535  ERR_PWR_REDUCTION_DET_LI_ION_DEPLETED  INFO_ALARM  <UTC:1324997978_17>
12/27/2011 14:59:37  12/27/2011 14:59:37 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1324997977_17>
12/27/2011 14:59:36  12/27/2011 14:59:36   324     3 65535  ERR_POWER_ON  KEYPRESS  <UTC:1324997976_17>
12/27/2011 14:59:36  12/27/2011 14:59:36   286     0 65535  ERR_PWR_UPGRADE_DET_LI_ION_IN_USE  BEEP_ONLY  <UTC:1324997976_17>
12/27/2011 14:59:35  12/27/2011 14:59:35   251     0 65535  ERR_DET_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1324997975_17>
12/27/2011 14:59:24  12/27/2011 14:59:24 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1324997964_17>
12/27/2011 14:59:24  12/27/2011 14:59:24   173     0 65535  ERR_START_ON_BATTERY  INFO_ALARM  <UTC:1324997964_17>
12/27/2011 14:59:24  12/27/2011 14:59:24   282     0 65535  ERR_INT_LI_ION_DEPLETED  HIGH_ALARM  <UTC:1324997964_17>
12/27/2011 14:59:20  12/27/2011 14:59:20 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1324997960_17>
12/27/2011 14:59:20  12/27/2011 14:59:20   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1324997960_17>
12/27/2011 14:58:46  12/27/2011 14:58:46 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1324997926_17>
12/27/2011 14:58:45  12/27/2011 14:58:45   110     0     1  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1324997925_17>
12/27/2011 14:58:44  12/27/2011 14:58:44   165  6494     2  ERR_LOW_PEP_ALARM  HIGH_ALARM  <UTC:1324997924_17>
12/27/2011 14:58:42  12/27/2011 14:58:42   173     0 65535  ERR_START_ON_BATTERY  INFO_ALARM  <UTC:1324997922_17>
12/27/2011 14:58:42  12/27/2011 14:58:42   282     0 65535  ERR_INT_LI_ION_DEPLETED  HIGH_ALARM  <UTC:1324997922_17>
12/27/2011 14:58:42  12/27/2011 14:58:42   188     0 65535  ERR_LAST_BATT_INT_LI_ION_NEARLY_DEPLETED  HIGH_ALARM  <UTC:1324997922_17>
12/27/2011 14:58:41  12/27/2011 14:58:41   282     0 65535  ERR_INT_LI_ION_DEPLETED  HIGH_ALARM  <UTC:1324997921_17>
12/27/2011 14:58:41  12/27/2011 14:58:41   281     0 65535  ERR_PWR_REDUCTION_DET_LI_ION_DEPLETED  INFO_ALARM  <UTC:1324997921_17>
12/27/2011 14:58:39  12/27/2011 14:58:39    72     0 65535  ERR_MMC_SD_CARD_INSERTED  BEEP_ONLY  <UTC:1324997919_17>
12/27/2011 14:58:39  12/27/2011 14:58:39   252     0 65535  ERR_INT_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1324997919_17>
12/27/2011 14:58:39  12/27/2011 14:58:39   251     0 65535  ERR_DET_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1324997919_17>
12/27/2011 14:58:39  12/27/2011 14:58:39 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1324997919_17>
12/27/2011 14:58:39  12/27/2011 14:58:39   324     2 65535  ERR_POWER_ON  KEYPRESS  <UTC:1324997919_17>
12/27/2011 09:33:09  12/27/2011 09:33:09 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1324978389_17>
12/27/2011 09:33:09  12/27/2011 09:33:09   173     0 65535  ERR_START_ON_BATTERY  INFO_ALARM  <UTC:1324978389_17>
12/27/2011 09:33:09  12/27/2011 09:33:09   282     0 65535  ERR_INT_LI_ION_DEPLETED  HIGH_ALARM  <UTC:1324978389_17>
12/27/2011 09:33:07  12/27/2011 09:33:07   281     0 65535  ERR_PWR_REDUCTION_DET_LI_ION_DEPLETED  INFO_ALARM  <UTC:1324978387_17>
12/27/2011 09:33:06  12/27/2011 09:33:06 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1324978386_17>
12/27/2011 09:33:06  12/27/2011 09:33:06   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1324978386_17>
12/27/2011 09:33:06  12/27/2011 09:33:06   286     0 65535  ERR_PWR_UPGRADE_DET_LI_ION_IN_USE  BEEP_ONLY  <UTC:1324978386_17>
12/27/2011 09:33:04  12/27/2011 09:33:04   251     0 65535  ERR_DET_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1324978384_17>
12/27/2011 09:31:51  12/27/2011 09:31:51 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1324978311_17>
12/27/2011 09:31:50  12/27/2011 09:31:50   110    15     1  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1324978310_17>
12/27/2011 09:31:47  12/27/2011 09:31:47   173     0 65535  ERR_START_ON_BATTERY  INFO_ALARM  <UTC:1324978307_17>
12/27/2011 09:31:47  12/27/2011 09:31:47   282     0 65535  ERR_INT_LI_ION_DEPLETED  HIGH_ALARM  <UTC:1324978307_17>
12/27/2011 09:31:47  12/27/2011 09:31:47   188     0 65535  ERR_LAST_BATT_INT_LI_ION_NEARLY_DEPLETED  HIGH_ALARM  <UTC:1324978307_17>
12/27/2011 09:31:46  12/27/2011 09:31:46   282     0 65535  ERR_INT_LI_ION_DEPLETED  HIGH_ALARM  <UTC:1324978306_17>
12/27/2011 09:31:46  12/27/2011 09:31:46   281     0 65535  ERR_PWR_REDUCTION_DET_LI_ION_DEPLETED  INFO_ALARM  <UTC:1324978306_17>
12/27/2011 09:31:44  12/27/2011 09:31:44    72     0 65535  ERR_MMC_SD_CARD_INSERTED  BEEP_ONLY  <UTC:1324978304_17>
12/27/2011 09:31:44  12/27/2011 09:31:44   252     0 65535  ERR_INT_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1324978304_17>
12/27/2011 09:31:44  12/27/2011 09:31:44   251     0 65535  ERR_DET_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1324978304_17>
12/27/2011 09:31:44  12/27/2011 09:31:44 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1324978304_17>
12/27/2011 09:31:44  12/27/2011 09:31:44   324     2 65535  ERR_POWER_ON  KEYPRESS  <UTC:1324978304_17>
12/27/2011 00:44:07  12/27/2011 00:44:07 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1324946647_17>
12/27/2011 00:44:03  12/27/2011 00:44:03   282     0 65535  ERR_INT_LI_ION_DEPLETED  HIGH_ALARM  <UTC:1324946643_17>
12/27/2011 00:35:23  12/27/2011 00:35:23   188     0 65535  ERR_LAST_BATT_INT_LI_ION_NEARLY_DEPLETED  HIGH_ALARM  <UTC:1324946123_17>
12/27/2011 00:35:23  12/27/2011 00:35:23   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1324946123_17>
12/27/2011 00:35:21  12/27/2011 00:35:21   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1324946121_17>
12/27/2011 00:35:21  12/27/2011 00:35:21   188     0 65535  ERR_LAST_BATT_INT_LI_ION_NEARLY_DEPLETED  HIGH_ALARM  <UTC:1324946121_17>
12/27/2011 00:35:16  12/27/2011 00:35:16   188     0 65535  ERR_LAST_BATT_INT_LI_ION_NEARLY_DEPLETED  HIGH_ALARM  <UTC:1324946116_17>
12/27/2011 00:35:12  12/27/2011 00:35:12   173     0 65535  ERR_START_ON_BATTERY  INFO_ALARM  <UTC:1324946112_17>
12/27/2011 00:35:10  12/27/2011 00:35:10   324     3 65535  ERR_POWER_ON  KEYPRESS  <UTC:1324946110_17>
12/27/2011 00:35:09  12/27/2011 00:35:09    72     0 65535  ERR_MMC_SD_CARD_INSERTED  BEEP_ONLY  <UTC:1324946109_17>
12/27/2011 00:35:09  12/27/2011 00:35:09   252     0 65535  ERR_INT_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1324946109_17>
12/27/2011 00:35:09  12/27/2011 00:35:09   251     0 65535  ERR_DET_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1324946109_17>
12/27/2011 00:35:09  12/27/2011 00:35:09 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1324946109_17>
12/27/2011 00:35:09  12/27/2011 00:35:09   324     2 65535  ERR_POWER_ON  KEYPRESS  <UTC:1324946109_17>
12/26/2011 20:59:00  12/26/2011 20:59:00 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1324933140_17>
12/26/2011 20:45:01  12/26/2011 20:45:01   188     0 65535  ERR_LAST_BATT_INT_LI_ION_NEARLY_DEPLETED  HIGH_ALARM  <UTC:1324932301_17>
12/26/2011 20:37:32  12/26/2011 20:37:32   185     0 65535  ERR_LAST_BATT_INT_LI_ION_LOW  MED_ALARM  <UTC:1324931852_17>
12/26/2011 20:27:30  12/26/2011 20:27:30   173     0 65535  ERR_START_ON_BATTERY  INFO_ALARM  <UTC:1324931250_17>
12/26/2011 20:27:27  12/26/2011 20:27:27    72     0 65535  ERR_MMC_SD_CARD_INSERTED  BEEP_ONLY  <UTC:1324931247_17>
12/26/2011 20:27:27  12/26/2011 20:27:27   252     0 65535  ERR_INT_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1324931247_17>
12/26/2011 20:27:27  12/26/2011 20:27:27   251     0 65535  ERR_DET_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1324931247_17>
12/26/2011 20:27:27  12/26/2011 20:27:27 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1324931247_17>
12/26/2011 20:27:27  12/26/2011 20:27:27   324     2 65535  ERR_POWER_ON  KEYPRESS  <UTC:1324931247_17>
12/26/2011 19:43:20  12/26/2011 19:43:20 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1324928600_17>
12/26/2011 19:43:20  12/26/2011 19:43:20   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1324928600_17>
12/26/2011 19:43:19  12/26/2011 19:43:19   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1324928599_17>
12/26/2011 18:41:23  12/26/2011 18:41:23   281     0 65535  ERR_PWR_REDUCTION_DET_LI_ION_DEPLETED  INFO_ALARM  <UTC:1324924883_17>
12/26/2011 17:35:36  12/26/2011 17:35:36   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1324920936_17>
12/26/2011 17:35:16  12/26/2011 17:35:16   173     0 65535  ERR_START_ON_BATTERY  INFO_ALARM  <UTC:1324920916_17>
12/26/2011 17:35:13  12/26/2011 17:35:13 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1324920913_17>
12/26/2011 17:35:13  12/26/2011 17:35:13   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1324920913_17>
12/26/2011 17:35:11  12/26/2011 17:35:11 16415     1     0      NV_ID= 31 (NV_RAMP_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1324920911_17>
12/26/2011 17:35:11  12/26/2011 17:35:11 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1324920911_17>
12/26/2011 17:35:11  12/26/2011 17:35:11   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1324920911_17>
12/26/2011 17:35:04  12/26/2011 17:35:04   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1324920904_17>
12/26/2011 17:34:32  12/26/2011 17:34:32   173     0 65535  ERR_START_ON_BATTERY  INFO_ALARM  <UTC:1324920872_17>
12/26/2011 17:34:31  12/26/2011 17:34:31 16415     0     1      NV_ID= 31 (NV_RAMP_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1324920871_17>
12/26/2011 17:34:29  12/26/2011 17:34:29    72     0 65535  ERR_MMC_SD_CARD_INSERTED  BEEP_ONLY  <UTC:1324920869_17>
12/26/2011 17:34:29  12/26/2011 17:34:29   252     0 65535  ERR_INT_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1324920869_17>
12/26/2011 17:34:29  12/26/2011 17:34:29   251     0 65535  ERR_DET_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1324920869_17>
12/26/2011 17:34:29  12/26/2011 17:34:29 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1324920869_17>
12/26/2011 17:34:29  12/26/2011 17:34:29   324     2 65535  ERR_POWER_ON  KEYPRESS  <UTC:1324920869_17>
12/26/2011 15:05:25  12/26/2011 15:05:25 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1324911925_17>
12/26/2011 15:05:24  12/26/2011 15:05:24   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1324911924_17>
12/26/2011 15:05:24  12/26/2011 15:05:24   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1324911924_17>
12/26/2011 15:05:20  12/26/2011 15:05:20   110    15     4  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1324911920_17>
12/26/2011 15:04:22  12/26/2011 15:04:22   110    29    15  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1324911862_17>
12/26/2011 15:04:11  12/26/2011 15:04:11   118    29     9  ERR_LOW_CIRCUIT_LEAK_ALARM  HIGH_ALARM  <UTC:1324911851_17>
12/26/2011 15:03:51  12/26/2011 15:03:51   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1324911831_17>
12/26/2011 15:03:49  12/26/2011 15:03:49   118    33     2  ERR_LOW_CIRCUIT_LEAK_ALARM  HIGH_ALARM  <UTC:1324911829_17>
12/26/2011 15:03:36  12/26/2011 15:03:36   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1324911816_17>
12/26/2011 15:03:26  12/26/2011 15:03:26   110    79     8  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1324911806_17>
12/26/2011 15:03:23  12/26/2011 15:03:23   169   169 65535  ERR_HIGH_PIP_STAGE1_ALARM  BEEP_ONLY  <UTC:1324911803_17>
12/26/2011 15:02:21  12/26/2011 15:02:21   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1324911741_17>
12/26/2011 15:01:57  12/26/2011 15:01:57   173     0 65535  ERR_START_ON_BATTERY  INFO_ALARM  <UTC:1324911717_17>
12/26/2011 15:01:53  12/26/2011 15:01:53 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1324911713_17>
12/26/2011 15:01:53  12/26/2011 15:01:53   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1324911713_17>
12/26/2011 15:01:20  12/26/2011 15:01:20   179     0 65535  ERR_PWR_REDUCTION_AC_DISCONNECTED  MED_ALARM  <UTC:1324911680_17>
12/26/2011 15:01:04  12/26/2011 15:01:04 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1324911664_17>
12/26/2011 15:01:04  12/26/2011 15:01:04   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1324911664_17>
12/26/2011 15:01:03  12/26/2011 15:01:03   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1324911663_17>
12/26/2011 15:01:03  12/26/2011 15:01:03   110     0     1  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1324911663_17>
12/26/2011 15:01:02  12/26/2011 15:01:02   165  6494     2  ERR_LOW_PEP_ALARM  HIGH_ALARM  <UTC:1324911662_17>
12/26/2011 15:00:56  12/26/2011 15:00:56 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1324911656_17>
12/26/2011 15:00:56  12/26/2011 15:00:56   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1324911656_17>
12/26/2011 15:00:42  12/26/2011 15:00:42   251     0 65535  ERR_DET_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1324911642_17>
12/26/2011 15:00:29  12/26/2011 15:00:29 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1324911629_17>
12/26/2011 15:00:29  12/26/2011 15:00:29   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1324911629_17>
12/26/2011 15:00:24  12/26/2011 15:00:24   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1324911624_17>
12/26/2011 15:00:21  12/26/2011 15:00:21   110     0     8  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1324911621_17>
12/26/2011 15:00:20  12/26/2011 15:00:20   165  6494     9  ERR_LOW_PEP_ALARM  HIGH_ALARM  <UTC:1324911620_17>
12/26/2011 15:00:19  12/26/2011 15:00:19   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1324911619_17>
12/26/2011 15:00:13  12/26/2011 15:00:13   110     0     6  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1324911613_17>
12/26/2011 15:00:12  12/26/2011 15:00:12   165  6494     4  ERR_LOW_PEP_ALARM  HIGH_ALARM  <UTC:1324911612_17>
12/26/2011 14:59:26  12/26/2011 14:59:26 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1324911566_17>
12/26/2011 14:59:26  12/26/2011 14:59:26   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1324911566_17>
12/26/2011 14:58:59  12/26/2011 14:58:59   284     0 65535  ERR_PWR_UPGRADE_AC_IN_USE  BEEP_ONLY  <UTC:1324911539_17>
12/26/2011 14:56:42  12/26/2011 14:56:42 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1324911402_17>
12/26/2011 14:56:42  12/26/2011 14:56:42   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1324911402_17>
12/26/2011 14:56:41  12/26/2011 14:56:41   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1324911401_17>
12/26/2011 14:55:41  12/26/2011 14:55:41   264     0 65535  ERR_MENU_BYPASS_ACTIVATED  KEYPRESS  <UTC:1324911341_17>
12/26/2011 14:55:32  12/26/2011 14:55:32   110     0    70  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1324911332_17>
12/26/2011 14:55:30  12/26/2011 14:55:30   165  6493    72  ERR_LOW_PEP_ALARM  HIGH_ALARM  <UTC:1324911330_17>
12/26/2011 14:55:28  12/26/2011 14:55:28   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1324911328_17>
12/26/2011 14:55:27  12/26/2011 14:55:27   110     0     1  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1324911327_17>
12/26/2011 14:55:27  12/26/2011 14:55:27   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1324911327_17>
12/26/2011 14:55:19  12/26/2011 14:55:19   110     0     8  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1324911319_17>
12/26/2011 14:55:17  12/26/2011 14:55:17   165  6494    10  ERR_LOW_PEP_ALARM  HIGH_ALARM  <UTC:1324911317_17>
12/26/2011 14:55:15  12/26/2011 14:55:15   173     0 65535  ERR_START_ON_BATTERY  INFO_ALARM  <UTC:1324911315_17>
12/26/2011 14:55:12  12/26/2011 14:55:12 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1324911312_17>
12/26/2011 14:55:12  12/26/2011 14:55:12   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1324911312_17>
12/26/2011 14:54:04  12/26/2011 14:54:04    72     0 65535  ERR_MMC_SD_CARD_INSERTED  BEEP_ONLY  <UTC:1324911244_17>
12/26/2011 14:54:02  12/26/2011 14:54:02    74     0 65535  ERR_MMC_SD_CARD_REMOVED  BEEP_ONLY  <UTC:1324911242_17>
12/26/2011 14:52:15  12/26/2011 14:52:15 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1324911135_17>
12/26/2011 14:52:15  12/26/2011 14:52:15   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1324911135_17>
12/26/2011 14:52:15  12/26/2011 14:52:15   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1324911135_17>
12/26/2011 14:49:35  12/26/2011 14:49:35 16400     1     2      NV_ID= 16 (NV_SCREENSAVER)  P/S=P RX=0  AVAPS=0  <UTC:1324910975_17>
12/26/2011 14:48:55  12/26/2011 14:48:55 16413     1     0      NV_ID= 29 (NV_ACCESS_LEVEL)  P/S=P RX=0  AVAPS=0  <UTC:1324910935_17>
12/26/2011 14:47:54  12/26/2011 14:47:54   110     0   261  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1324910874_17>
12/26/2011 14:47:53  12/26/2011 14:47:53   165  6493   262  ERR_LOW_PEP_ALARM  HIGH_ALARM  <UTC:1324910873_17>
12/26/2011 14:47:48  12/26/2011 14:47:48 16418     3     2      NV_ID= 34 (NV_RX_MODE)  P/S=P RX=0  AVAPS=0  <UTC:1324910868_17>
12/26/2011 14:47:16  12/26/2011 14:47:16 17731     1     0      NV_ID= 67 (NV_AVAPS_LOW_TIDVOL_ALARM)  P/S=P RX=2  AVAPS=1  <UTC:1324910836_17>
12/26/2011 14:47:04  12/26/2011 14:47:04 17718    10     0      NV_ID= 54 (NV_PT_DISCONNECT)  P/S=P RX=2  AVAPS=1  <UTC:1324910824_17>
12/26/2011 14:46:41  12/26/2011 14:46:41 17711     0     5      NV_ID= 47 (NV_RAMP_LENGTH)  P/S=P RX=2  AVAPS=1  <UTC:1324910801_17>
12/26/2011 14:46:23  12/26/2011 14:46:23 17722    12    14      NV_ID= 58 (NV_APNEA_BREATH_RATE)  P/S=P RX=2  AVAPS=1  <UTC:1324910783_17>
12/26/2011 14:46:23  12/26/2011 14:46:23 17708    10    14      NV_ID= 44 (NV_BREATH_RATE)  P/S=P RX=2  AVAPS=1  <UTC:1324910783_17>
12/26/2011 14:46:15  12/26/2011 14:46:15 17702   500   400      NV_ID= 38 (NV_EPAP_PEEP_CPAP_PRESSURE)  P/S=P RX=2  AVAPS=1  <UTC:1324910775_17>
12/26/2011 14:46:09  12/26/2011 14:46:09 17701  1400  1600      NV_ID= 37 (NV_IPAP_PRESSURE)  P/S=P RX=2  AVAPS=1  <UTC:1324910769_17>
12/26/2011 14:45:58  12/26/2011 14:45:58 17700  2000  2200      NV_ID= 36 (NV_IPAP_MAX_PRESSURE)  P/S=P RX=2  AVAPS=1  <UTC:1324910758_17>
12/26/2011 14:45:52  12/26/2011 14:45:52 17707   450   550      NV_ID= 43 (NV_TIDAL_VOLUME)  P/S=P RX=2  AVAPS=1  <UTC:1324910752_17>
12/26/2011 14:45:26  12/26/2011 14:45:26 16417     1     0      NV_ID= 33 (NV_DUAL_RX_ENABLED)  P/S=P RX=0  AVAPS=0  <UTC:1324910726_17>
12/26/2011 14:44:28  12/26/2011 14:44:28   264     0 65535  ERR_MENU_BYPASS_ACTIVATED  KEYPRESS  <UTC:1324910668_17>
12/26/2011 14:44:25  12/26/2011 14:44:25   110     0   203  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1324910665_17>
12/26/2011 14:44:24  12/26/2011 14:44:24   165  6492   204  ERR_LOW_PEP_ALARM  HIGH_ALARM  <UTC:1324910664_17>
12/26/2011 14:44:20  12/26/2011 14:44:20   173     0 65535  ERR_START_ON_BATTERY  INFO_ALARM  <UTC:1324910660_17>
12/26/2011 14:44:17  12/26/2011 14:44:17    72     0 65535  ERR_MMC_SD_CARD_INSERTED  BEEP_ONLY  <UTC:1324910657_17>
12/26/2011 14:44:17  12/26/2011 14:44:17   252     0 65535  ERR_INT_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1324910657_17>
12/26/2011 14:44:17  12/26/2011 14:44:17   251     0 65535  ERR_DET_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1324910657_17>
12/26/2011 14:44:17  12/26/2011 14:44:17 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1324910657_17>
12/26/2011 14:44:17  12/26/2011 14:44:17   324     2 65535  ERR_POWER_ON  KEYPRESS  <UTC:1324910657_17>
12/15/2011 14:30:18  12/15/2011 14:30:18   179     0 65535  ERR_PWR_REDUCTION_AC_DISCONNECTED  MED_ALARM  <UTC:1323959418_17>
12/15/2011 14:28:51  12/15/2011 14:28:51 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1323959331_17>
12/15/2011 14:28:51  12/15/2011 14:28:51   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1323959331_17>
12/15/2011 14:28:50  12/15/2011 14:28:50   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1323959330_17>
12/15/2011 14:28:39  12/15/2011 14:28:39 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1323959319_17>
12/15/2011 14:28:39  12/15/2011 14:28:39   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1323959319_17>
12/15/2011 14:28:36  12/15/2011 14:28:36    72     0 65535  ERR_MMC_SD_CARD_INSERTED  BEEP_ONLY  <UTC:1323959316_17>
12/15/2011 14:27:47  12/15/2011 14:27:47    74     0 65535  ERR_MMC_SD_CARD_REMOVED  BEEP_ONLY  <UTC:1323959267_17>
12/15/2011 14:27:40  12/15/2011 14:27:40 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1323959260_17>
12/15/2011 14:27:40  12/15/2011 14:27:40   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1323959260_17>
12/15/2011 14:27:39  12/15/2011 14:27:39   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1323959259_17>
12/15/2011 14:26:56  12/15/2011 14:26:56 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1323959216_17>
12/15/2011 14:26:56  12/15/2011 14:26:56   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1323959216_17>
12/15/2011 14:26:07  12/15/2011 14:26:07 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1323959167_17>
12/15/2011 14:26:04  12/15/2011 14:26:04   284     0 65535  ERR_PWR_UPGRADE_AC_IN_USE  BEEP_ONLY  <UTC:1323959164_17>
12/15/2011 14:26:01  12/15/2011 14:26:01   286     0 65535  ERR_PWR_UPGRADE_DET_LI_ION_IN_USE  BEEP_ONLY  <UTC:1323959161_17>
12/15/2011 14:26:00  12/15/2011 14:26:00   251     0 65535  ERR_DET_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1323959160_17>
12/15/2011 14:25:44  12/15/2011 14:25:44   181     0 65535  ERR_PWR_REDUCTION_DET_LI_ION_DISCONNECTED  INFO_ALARM  <UTC:1323959144_17>
12/15/2011 14:25:37  12/15/2011 14:25:37   180     0 65535  ERR_PWR_REDUCTION_LEAD_ACID_DISCONNECTED  INFO_ALARM  <UTC:1323959137_17>
12/15/2011 14:25:16  12/15/2011 14:25:16   179     0 65535  ERR_PWR_REDUCTION_AC_DISCONNECTED  MED_ALARM  <UTC:1323959116_17>
12/15/2011 14:24:45  12/15/2011 14:24:45   251     0 65535  ERR_DET_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1323959085_17>
12/15/2011 14:23:29  12/15/2011 14:23:29 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1323959009_17>
12/15/2011 14:23:29  12/15/2011 14:23:29   324     4 65535  ERR_POWER_ON  KEYPRESS  <UTC:1323959009_17>
12/15/2011 14:23:26  12/15/2011 14:23:26   250     0 65535  ERR_LEAD_ACID_BATT_CONNECTED  BEEP_ONLY  <UTC:1323959006_17>
12/15/2011 14:23:21  12/15/2011 14:23:21   251     0 65535  ERR_DET_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1323959001_17>
12/15/2011 14:23:12  12/15/2011 14:23:12 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1323958992_17>
12/15/2011 14:23:06  12/15/2011 14:23:06    72     0 65535  ERR_MMC_SD_CARD_INSERTED  BEEP_ONLY  <UTC:1323958986_17>
12/15/2011 14:23:06  12/15/2011 14:23:06   252     0 65535  ERR_INT_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1323958986_17>
12/15/2011 14:23:06  12/15/2011 14:23:06   251     0 65535  ERR_DET_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1323958986_17>
12/15/2011 14:20:25  12/15/2011 14:20:25 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1323958825_17>
12/15/2011 14:20:25  12/15/2011 14:20:25   324     4 65535  ERR_POWER_ON  KEYPRESS  <UTC:1323958825_17>
12/15/2011 14:13:10  12/15/2011 14:13:10 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1323958390_17>
12/15/2011 14:12:55  12/15/2011 14:12:55 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1323958375_17>
12/15/2011 14:12:55  12/15/2011 14:12:55   324     4 65535  ERR_POWER_ON  KEYPRESS  <UTC:1323958375_17>
12/15/2011 14:03:05  12/15/2011 15:03:05 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1323957785_17>
12/15/2011 14:02:58  12/15/2011 15:02:58   110     0     6  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1323957778_17>
12/15/2011 14:02:57  12/15/2011 15:02:57   165  6490     6  ERR_LOW_PEP_ALARM  HIGH_ALARM  <UTC:1323957777_17>
12/15/2011 14:02:50  12/15/2011 15:02:50 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1323957770_17>
12/15/2011 14:02:50  12/15/2011 15:02:50   324     4 65535  ERR_POWER_ON  KEYPRESS  <UTC:1323957770_17>
12/15/2011 14:02:50  12/15/2011 15:02:50 17966     1     3      NV_ID= 46 (NV_RISE_TIME)  P/S=P RX=3  AVAPS=0  <UTC:1323957770_17>
12/15/2011 14:02:50  12/15/2011 15:02:50 17965    20    10      NV_ID= 45 (NV_TIMED_INSP)  P/S=P RX=3  AVAPS=0  <UTC:1323957770_17>
12/15/2011 14:02:50  12/15/2011 15:02:50 17964    15    10      NV_ID= 44 (NV_BREATH_RATE)  P/S=P RX=3  AVAPS=0  <UTC:1323957770_17>
12/15/2011 14:02:50  12/15/2011 15:02:50 17957  2100  2000      NV_ID= 37 (NV_IPAP_PRESSURE)  P/S=P RX=3  AVAPS=0  <UTC:1323957770_17>
12/15/2011 14:02:50  12/15/2011 15:02:50 17956  5000  3400      NV_ID= 36 (NV_IPAP_MAX_PRESSURE)  P/S=P RX=3  AVAPS=0  <UTC:1323957770_17>
12/15/2011 14:02:50  12/15/2011 15:02:50 17958  2000   400      NV_ID= 38 (NV_EPAP_PEEP_CPAP_PRESSURE)  P/S=P RX=3  AVAPS=0  <UTC:1323957770_17>
12/15/2011 14:02:50  12/15/2011 15:02:50 17957  5000  2100      NV_ID= 37 (NV_IPAP_PRESSURE)  P/S=P RX=3  AVAPS=0  <UTC:1323957770_17>
12/15/2011 14:02:50  12/15/2011 15:02:50 16418     8     3      NV_ID= 34 (NV_RX_MODE)  P/S=P RX=0  AVAPS=0  <UTC:1323957770_17>
12/15/2011 14:02:10  12/15/2011 15:02:10    72     0 65535  ERR_MMC_SD_CARD_INSERTED  BEEP_ONLY  <UTC:1323957730_17>
12/15/2011 14:02:08  12/15/2011 15:02:08    74     0 65535  ERR_MMC_SD_CARD_REMOVED  BEEP_ONLY  <UTC:1323957728_17>
12/15/2011 14:02:00  12/15/2011 15:02:00   251     0 65535  ERR_DET_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1323957720_17>
12/15/2011 13:59:31  12/15/2011 14:59:31    72     0 65535  ERR_MMC_SD_CARD_INSERTED  BEEP_ONLY  <UTC:1323957571_17>
12/15/2011 13:59:31  12/15/2011 14:59:31   252     0 65535  ERR_INT_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1323957571_17>
12/15/2011 13:59:31  12/15/2011 14:59:31   251     0 65535  ERR_DET_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1323957571_17>
11/17/2011 21:58:50  11/17/2011 22:58:50 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1321567130_17>
11/17/2011 21:58:50  11/17/2011 22:58:50   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1321567130_17>
11/17/2011 21:58:49  11/17/2011 22:58:49   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1321567129_17>
11/17/2011 21:58:47  11/17/2011 22:58:47   168     0 65535  ERR_UI_AUDIO_PAUSE_KEY_PRESS  KEYPRESS  <UTC:1321567127_17>
11/17/2011 21:58:42  11/17/2011 22:58:42   110    48     5  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1321567122_17>
11/17/2011 21:58:39  11/17/2011 22:58:39   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1321567119_17>
11/17/2011 21:58:35  11/17/2011 22:58:35   110    76     4  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1321567115_17>
11/17/2011 21:58:33  11/17/2011 22:58:33   169   257 65535  ERR_HIGH_PIP_STAGE1_ALARM  BEEP_ONLY  <UTC:1321567113_17>
11/17/2011 21:58:31  11/17/2011 22:58:31   169   254 65535  ERR_HIGH_PIP_STAGE1_ALARM  BEEP_ONLY  <UTC:1321567111_17>
11/17/2011 21:58:25  11/17/2011 22:58:25   110    74     2  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1321567105_17>
11/17/2011 21:58:19  11/17/2011 22:58:19   110   117     1  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1321567099_17>
11/17/2011 21:58:07  11/17/2011 22:58:07   167     0 65535  ERR_UI_HIDE_KEY_PRESS  KEYPRESS  <UTC:1321567087_17>
11/17/2011 21:57:59  11/17/2011 22:57:59   110    46     1  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1321567079_17>
11/17/2011 21:57:53  11/17/2011 22:57:53   110    94     1  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1321567073_17>
11/17/2011 21:57:47  11/17/2011 22:57:47   110    58     2  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1321567067_17>
11/17/2011 21:57:39  11/17/2011 22:57:39   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1321567059_17>
11/17/2011 21:57:38  11/17/2011 22:57:38   110    72     1  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1321567058_17>
11/17/2011 21:57:27  11/17/2011 22:57:27    18     0 65535  ERR_DSP_DC_DC_CONTROL  ROUTINE_SERVICE  <UTC:1321567047_17>
11/17/2011 21:57:26  11/17/2011 22:57:26   110     0     5  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1321567046_17>
11/17/2011 21:57:25  11/17/2011 22:57:25   165  6499     5  ERR_LOW_PEP_ALARM  HIGH_ALARM  <UTC:1321567045_17>
11/17/2011 21:57:22  11/17/2011 22:57:22   173     0 65535  ERR_START_ON_BATTERY  INFO_ALARM  <UTC:1321567042_17>
11/17/2011 21:57:19  11/17/2011 22:57:19 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1321567039_17>
11/17/2011 21:57:19  11/17/2011 22:57:19   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1321567039_17>
11/17/2011 21:57:17  11/17/2011 22:57:17   179     0 65535  ERR_PWR_REDUCTION_AC_DISCONNECTED  MED_ALARM  <UTC:1321567037_17>
11/17/2011 21:57:11  11/17/2011 22:57:11 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1321567031_17>
11/17/2011 21:57:11  11/17/2011 22:57:11   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1321567031_17>
11/17/2011 21:57:09  11/17/2011 22:57:09   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1321567029_17>
11/17/2011 21:57:01  11/17/2011 22:57:01   165  6499    10  ERR_LOW_PEP_ALARM  HIGH_ALARM  <UTC:1321567021_17>
11/17/2011 21:56:59  11/17/2011 22:56:59   167     0 65535  ERR_UI_HIDE_KEY_PRESS  KEYPRESS  <UTC:1321567019_17>
11/17/2011 21:56:59  11/17/2011 22:56:59   110    54    12  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1321567019_17>
11/17/2011 21:56:56  11/17/2011 22:56:56   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1321567016_17>
11/17/2011 21:56:47  11/17/2011 22:56:47   114    29     5  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321567007_17>
11/17/2011 21:56:38  11/17/2011 22:56:38   169   670 65535  ERR_HIGH_PIP_STAGE1_ALARM  BEEP_ONLY  <UTC:1321566998_17>
11/17/2011 21:56:37  11/17/2011 22:56:37   114    28     3  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321566997_17>
11/17/2011 21:56:28  11/17/2011 22:56:28   169   670 65535  ERR_HIGH_PIP_STAGE1_ALARM  BEEP_ONLY  <UTC:1321566988_17>
11/17/2011 21:56:23  11/17/2011 22:56:23   169   671 65535  ERR_HIGH_PIP_STAGE1_ALARM  BEEP_ONLY  <UTC:1321566983_17>
11/17/2011 21:56:12  11/17/2011 22:56:12   118     3    39  ERR_LOW_CIRCUIT_LEAK_ALARM  HIGH_ALARM  <UTC:1321566972_17>
11/17/2011 21:55:52  11/17/2011 22:55:52   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1321566952_17>
11/17/2011 21:55:41  11/17/2011 22:55:41   114    19     7  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321566941_17>
11/17/2011 21:55:41  11/17/2011 22:55:41   118    19     5  ERR_LOW_CIRCUIT_LEAK_ALARM  HIGH_ALARM  <UTC:1321566941_17>
11/17/2011 21:55:36  11/17/2011 22:55:36   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1321566936_17>
11/17/2011 21:55:27  11/17/2011 22:55:27   118    25     9  ERR_LOW_CIRCUIT_LEAK_ALARM  HIGH_ALARM  <UTC:1321566927_17>
11/17/2011 21:54:55  11/17/2011 22:54:55   169   262 65535  ERR_HIGH_PIP_STAGE1_ALARM  BEEP_ONLY  <UTC:1321566895_17>
11/17/2011 21:54:50  11/17/2011 22:54:50   169   670 65535  ERR_HIGH_PIP_STAGE1_ALARM  BEEP_ONLY  <UTC:1321566890_17>
11/17/2011 21:54:42  11/17/2011 22:54:42   118    31    13  ERR_LOW_CIRCUIT_LEAK_ALARM  HIGH_ALARM  <UTC:1321566882_17>
11/17/2011 21:54:39  11/17/2011 22:54:39   169   679 65535  ERR_HIGH_PIP_STAGE1_ALARM  BEEP_ONLY  <UTC:1321566879_17>
11/17/2011 21:54:05  11/17/2011 22:54:05   118    23     4  ERR_LOW_CIRCUIT_LEAK_ALARM  HIGH_ALARM  <UTC:1321566845_17>
11/17/2011 21:52:58  11/17/2011 22:52:58   110   112     1  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1321566778_17>
11/17/2011 21:52:58  11/17/2011 22:52:58   114    16     0  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321566778_17>
11/17/2011 21:52:53  11/17/2011 22:52:53   118     0     5  ERR_LOW_CIRCUIT_LEAK_ALARM  HIGH_ALARM  <UTC:1321566773_17>
11/17/2011 21:52:26  11/17/2011 22:52:26   168     0 65535  ERR_UI_AUDIO_PAUSE_KEY_PRESS  KEYPRESS  <UTC:1321566746_17>
11/17/2011 21:52:26  11/17/2011 22:52:26   168     0 65535  ERR_UI_AUDIO_PAUSE_KEY_PRESS  KEYPRESS  <UTC:1321566746_17>
11/17/2011 21:52:25  11/17/2011 22:52:25   168     0 65535  ERR_UI_AUDIO_PAUSE_KEY_PRESS  KEYPRESS  <UTC:1321566745_17>
11/17/2011 21:52:19  11/17/2011 22:52:19   114    19    14  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321566739_17>
11/17/2011 21:52:06  11/17/2011 22:52:06   170   671    23  ERR_HIGH_PIP_STAGE2_ALARM  MED_ALARM  <UTC:1321566726_17>
11/17/2011 21:52:01  11/17/2011 22:52:01   169   670 65535  ERR_HIGH_PIP_STAGE1_ALARM  BEEP_ONLY  <UTC:1321566721_17>
11/17/2011 21:51:56  11/17/2011 22:51:56   169   670 65535  ERR_HIGH_PIP_STAGE1_ALARM  BEEP_ONLY  <UTC:1321566716_17>
11/17/2011 21:51:49  11/17/2011 22:51:49   169   672 65535  ERR_HIGH_PIP_STAGE1_ALARM  BEEP_ONLY  <UTC:1321566709_17>
11/17/2011 21:51:48  11/17/2011 22:51:48   114    30     7  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321566708_17>
11/17/2011 21:51:47  11/17/2011 22:51:47   167     0 65535  ERR_UI_HIDE_KEY_PRESS  KEYPRESS  <UTC:1321566707_17>
11/17/2011 21:51:40  11/17/2011 22:51:40   169   671 65535  ERR_HIGH_PIP_STAGE1_ALARM  BEEP_ONLY  <UTC:1321566700_17>
11/17/2011 21:51:40  11/17/2011 22:51:40   118    20    53  ERR_LOW_CIRCUIT_LEAK_ALARM  HIGH_ALARM  <UTC:1321566700_17>
11/17/2011 21:51:37  11/17/2011 22:51:37   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1321566697_17>
11/17/2011 21:51:24  11/17/2011 22:51:24   120   310    10  ERR_APNEA_ALARM  HIGH_ALARM  <UTC:1321566684_17>
11/17/2011 21:51:10  11/17/2011 22:51:10   170   670    28  ERR_HIGH_PIP_STAGE2_ALARM  MED_ALARM  <UTC:1321566670_17>
11/17/2011 21:51:05  11/17/2011 22:51:05   169   671 65535  ERR_HIGH_PIP_STAGE1_ALARM  BEEP_ONLY  <UTC:1321566665_17>
11/17/2011 21:51:00  11/17/2011 22:51:00   169   671 65535  ERR_HIGH_PIP_STAGE1_ALARM  BEEP_ONLY  <UTC:1321566660_17>
11/17/2011 21:50:53  11/17/2011 22:50:53 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1321566653_17>
11/17/2011 21:50:53  11/17/2011 22:50:53   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1321566653_17>
11/17/2011 21:50:48  11/17/2011 22:50:48 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1321566648_17>
11/17/2011 21:50:47  11/17/2011 22:50:47   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1321566647_17>
11/17/2011 21:50:44  11/17/2011 22:50:44   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1321566644_17>
11/17/2011 21:50:32  11/17/2011 22:50:32   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1321566632_17>
11/17/2011 21:50:30  11/17/2011 22:50:30   168     0 65535  ERR_UI_AUDIO_PAUSE_KEY_PRESS  KEYPRESS  <UTC:1321566630_17>
11/17/2011 21:50:29  11/17/2011 22:50:29   168     0 65535  ERR_UI_AUDIO_PAUSE_KEY_PRESS  KEYPRESS  <UTC:1321566629_17>
11/17/2011 21:50:27  11/17/2011 22:50:27   110    52     5  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1321566627_17>
11/17/2011 21:50:21  11/17/2011 22:50:21   110    40     3  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1321566621_17>
11/17/2011 21:50:21  11/17/2011 22:50:21   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1321566621_17>
11/17/2011 21:50:14  11/17/2011 22:50:14 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1321566614_17>
11/17/2011 21:50:14  11/17/2011 22:50:14   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1321566614_17>
11/17/2011 21:50:10  11/17/2011 22:50:10    72     0 65535  ERR_MMC_SD_CARD_INSERTED  BEEP_ONLY  <UTC:1321566610_17>
11/17/2011 21:49:53  11/17/2011 22:49:53    74     0 65535  ERR_MMC_SD_CARD_REMOVED  BEEP_ONLY  <UTC:1321566593_17>
11/17/2011 21:49:48  11/17/2011 22:49:48    72     0 65535  ERR_MMC_SD_CARD_INSERTED  BEEP_ONLY  <UTC:1321566588_17>
11/17/2011 21:49:48  11/17/2011 22:49:48   252     0 65535  ERR_INT_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1321566588_17>
11/17/2011 21:49:48  11/17/2011 22:49:48   251     0 65535  ERR_DET_LI_ION_CONNECTED  BEEP_ONLY  <UTC:1321566588_17>
11/15/2011 03:12:16  11/15/2011 04:12:16   179     0 65535  ERR_PWR_REDUCTION_AC_DISCONNECTED  MED_ALARM  <UTC:1321326736_17>
11/15/2011 03:04:30  11/15/2011 04:04:30 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1321326270_17>
11/15/2011 03:04:30  11/15/2011 04:04:30   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1321326270_17>
11/15/2011 03:04:28  11/15/2011 04:04:28   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1321326268_17>
11/15/2011 03:04:19  11/15/2011 04:04:19   114     0    11  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321326259_17>
11/15/2011 03:04:15  11/15/2011 04:04:15   120   310    15  ERR_APNEA_ALARM  HIGH_ALARM  <UTC:1321326255_17>
11/15/2011 03:04:07  11/15/2011 04:04:07   167     0 65535  ERR_UI_HIDE_KEY_PRESS  KEYPRESS  <UTC:1321326247_17>
11/15/2011 03:03:57  11/15/2011 04:03:57   168     0 65535  ERR_UI_AUDIO_PAUSE_KEY_PRESS  KEYPRESS  <UTC:1321326237_17>
11/15/2011 03:03:55  11/15/2011 04:03:55   110     0    35  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1321326235_17>
11/15/2011 03:03:55  11/15/2011 04:03:55   165  6501    35  ERR_LOW_PEP_ALARM  HIGH_ALARM  <UTC:1321326235_17>
11/15/2011 03:03:54  11/15/2011 04:03:54   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1321326234_17>
11/15/2011 03:03:50  11/15/2011 04:03:50   110     0     4  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1321326230_17>
11/15/2011 03:03:50  11/15/2011 04:03:50   165  6502     4  ERR_LOW_PEP_ALARM  HIGH_ALARM  <UTC:1321326230_17>
11/15/2011 03:03:49  11/15/2011 04:03:49   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1321326229_17>
11/15/2011 03:03:47  11/15/2011 04:03:47   289    18 65535  ERR_ROUTINE_REMINDER  ROUTINE_SERVICE  <UTC:1321326227_17>
11/15/2011 03:03:44  11/15/2011 04:03:44 16414     0     1      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1321326224_17>
11/15/2011 03:03:44  11/15/2011 04:03:44   324     1 65535  ERR_POWER_ON  KEYPRESS  <UTC:1321326224_17>
11/14/2011 23:38:18  11/15/2011 00:38:18 16414     1     0      NV_ID= 30 (NV_UNIT_STATE)  P/S=P RX=0  AVAPS=0  <UTC:1321313898_17>
11/14/2011 23:38:18  11/15/2011 00:38:18   294     0 65535  ERR_POWER_OFF_YES_KEY  KEYPRESS  <UTC:1321313898_17>
11/14/2011 23:38:15  11/15/2011 00:38:15   293     0 65535  ERR_POWER_OFF_KEY  KEYPRESS  <UTC:1321313895_17>
11/14/2011 23:38:09  11/15/2011 00:38:09   110    85     9  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1321313889_17>
11/14/2011 23:38:05  11/15/2011 00:38:05   110    70     1  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1321313885_17>
11/14/2011 23:37:43  11/15/2011 00:37:43   110    84     9  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1321313863_17>
11/14/2011 23:37:28  11/15/2011 00:37:28   120  2210    41  ERR_APNEA_ALARM  HIGH_ALARM  <UTC:1321313848_17>
11/14/2011 23:37:25  11/15/2011 00:37:25   114    11    53  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321313845_17>
11/14/2011 23:37:25  11/15/2011 00:37:25   291     5    21  ERR_CIRCUIT_CHECK  HIGH_ALARM  <UTC:1321313845_17>
11/14/2011 23:36:58  11/15/2011 00:36:58   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1321313818_17>
11/14/2011 23:35:44  11/15/2011 00:35:44   168     0 65535  ERR_UI_AUDIO_PAUSE_KEY_PRESS  KEYPRESS  <UTC:1321313744_17>
11/14/2011 23:35:39  11/15/2011 00:35:39   120  1120    79  ERR_APNEA_ALARM  HIGH_ALARM  <UTC:1321313739_17>
11/14/2011 23:35:37  11/15/2011 00:35:37   114    10    81  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321313737_17>
11/14/2011 23:35:37  11/15/2011 00:35:37   291     5 65535  ERR_CIRCUIT_CHECK  HIGH_ALARM  <UTC:1321313737_17>
11/14/2011 23:35:09  11/15/2011 00:35:09   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1321313709_17>
11/14/2011 23:35:02  11/15/2011 00:35:02   120   740     7  ERR_APNEA_ALARM  HIGH_ALARM  <UTC:1321313702_17>
11/14/2011 23:34:58  11/15/2011 00:34:58   114    11    11  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321313698_17>
11/14/2011 23:34:58  11/15/2011 00:34:58   291     5 65535  ERR_CIRCUIT_CHECK  HIGH_ALARM  <UTC:1321313698_17>
11/14/2011 23:34:32  11/15/2011 00:34:32   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1321313672_17>
11/14/2011 23:34:17  11/15/2011 00:34:17   120   300    15  ERR_APNEA_ALARM  HIGH_ALARM  <UTC:1321313657_17>
11/14/2011 23:33:50  11/15/2011 00:33:50   114    15    42  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321313630_17>
11/14/2011 23:33:47  11/15/2011 00:33:47   169   670 65535  ERR_HIGH_PIP_STAGE1_ALARM  BEEP_ONLY  <UTC:1321313627_17>
11/14/2011 23:33:41  11/15/2011 00:33:41   169   670 65535  ERR_HIGH_PIP_STAGE1_ALARM  BEEP_ONLY  <UTC:1321313621_17>
11/14/2011 23:33:35  11/15/2011 00:33:35 16416     1     0      NV_ID= 32 (NV_DUAL_RX_SELECTED)  P/S=P RX=0  AVAPS=0  <UTC:1321313615_17>
11/14/2011 23:33:28  11/15/2011 00:33:28   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1321313608_17>
11/14/2011 23:32:02  11/15/2011 00:32:02   110   132     8  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1321313522_17>
11/14/2011 20:29:43  11/14/2011 21:29:43   284     0 65535  ERR_PWR_UPGRADE_AC_IN_USE  BEEP_ONLY  <UTC:1321302583_17>
11/14/2011 20:22:44  11/14/2011 21:22:44   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1321302164_17>
11/14/2011 20:22:39  11/14/2011 21:22:39   179     0 65535  ERR_PWR_REDUCTION_AC_DISCONNECTED  MED_ALARM  <UTC:1321302159_17>
11/14/2011 20:09:51  11/14/2011 21:09:51   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1321301391_17>
11/14/2011 20:08:51  11/14/2011 21:08:51   110   136     6  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1321301331_17>
11/14/2011 17:58:11  11/14/2011 18:58:11 16416     0     1      NV_ID= 32 (NV_DUAL_RX_SELECTED)  P/S=P RX=0  AVAPS=0  <UTC:1321293491_17>
11/14/2011 17:57:56  11/14/2011 18:57:56 16416     1     0      NV_ID= 32 (NV_DUAL_RX_SELECTED)  P/S=P RX=0  AVAPS=0  <UTC:1321293476_17>
11/14/2011 17:54:47  11/14/2011 18:54:47 16416     0     1      NV_ID= 32 (NV_DUAL_RX_SELECTED)  P/S=P RX=0  AVAPS=0  <UTC:1321293287_17>
11/14/2011 17:33:01  11/14/2011 18:33:01    72     0 65535  ERR_MMC_SD_CARD_INSERTED  BEEP_ONLY  <UTC:1321291981_17>
11/14/2011 17:24:46  11/14/2011 18:24:46   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1321291486_17>
11/14/2011 17:24:16  11/14/2011 18:24:16   110    69     6  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1321291456_17>
11/14/2011 17:11:36  11/14/2011 18:11:36    74     0 65535  ERR_MMC_SD_CARD_REMOVED  BEEP_ONLY  <UTC:1321290696_17>
11/14/2011 16:18:58  11/14/2011 17:18:58   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1321287538_17>
11/14/2011 16:18:29  11/14/2011 17:18:29   110   117     2  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1321287509_17>
11/14/2011 15:10:40  11/14/2011 16:10:40   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1321283440_17>
11/14/2011 15:08:05  11/14/2011 16:08:05   165    15     3  ERR_LOW_PEP_ALARM  HIGH_ALARM  <UTC:1321283285_17>
11/14/2011 15:08:02  11/14/2011 16:08:02   110    69     8  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1321283282_17>
11/14/2011 15:06:52  11/14/2011 16:06:52   110   112     2  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1321283212_17>
11/14/2011 11:19:53  11/14/2011 12:19:53   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1321269593_17>
11/14/2011 11:19:34  11/14/2011 12:19:34   289    18 65534  ERR_ROUTINE_REMINDER  ROUTINE_SERVICE  <UTC:1321269574_17>
11/14/2011 10:54:25  11/14/2011 11:54:25   110    70     3  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1321268065_17>
11/14/2011 10:41:43  11/14/2011 11:41:43   284     0 65535  ERR_PWR_UPGRADE_AC_IN_USE  BEEP_ONLY  <UTC:1321267303_17>
11/14/2011 10:41:20  11/14/2011 11:41:20   110   117     2  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1321267280_17>
11/14/2011 10:33:07  11/14/2011 11:33:07   110   104     5  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1321266787_17>
11/14/2011 10:32:39  11/14/2011 11:32:39   110   105     5  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1321266759_17>
11/14/2011 10:32:29  11/14/2011 11:32:29   110   117     1  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1321266749_17>
11/14/2011 10:30:22  11/14/2011 11:30:22   110   100     4  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1321266622_17>
11/14/2011 10:30:17  11/14/2011 11:30:17   110    97     2  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1321266617_17>
11/14/2011 10:22:11  11/14/2011 11:22:11   110   118     2  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1321266131_17>
11/14/2011 10:16:27  11/14/2011 11:16:27   179     0 65535  ERR_PWR_REDUCTION_AC_DISCONNECTED  MED_ALARM  <UTC:1321265787_17>
11/14/2011 07:01:17  11/14/2011 08:01:17   110   119     3  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1321254077_17>
11/14/2011 03:05:11  11/14/2011 04:05:11   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1321239911_17>
11/14/2011 03:03:24  11/14/2011 04:03:24   110    78     7  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1321239804_17>
11/14/2011 03:03:20  11/14/2011 04:03:20   120   300    17  ERR_APNEA_ALARM  HIGH_ALARM  <UTC:1321239800_17>
11/14/2011 03:03:08  11/14/2011 04:03:08   114    21    23  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321239788_17>
11/14/2011 03:02:42  11/14/2011 04:02:42   120   300     5  ERR_APNEA_ALARM  HIGH_ALARM  <UTC:1321239762_17>
11/14/2011 03:01:10  11/14/2011 04:01:10   114     8    95  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321239670_17>
11/14/2011 03:00:50  11/14/2011 04:00:50   110    71     7  ERR_LOW_PIP_ALARM  HIGH_ALARM  <UTC:1321239650_17>
11/14/2011 03:00:29  11/14/2011 04:00:29   114    29    27  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321239629_17>
11/14/2011 03:00:18  11/14/2011 04:00:18   114    29     5  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321239618_17>
11/14/2011 03:00:07  11/14/2011 04:00:07   114    29     9  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321239607_17>
11/14/2011 03:00:00  11/14/2011 04:00:00   114    29     5  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321239600_17>
11/14/2011 02:59:56  11/14/2011 03:59:56   114    30     2  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321239596_17>
11/14/2011 02:59:52  11/14/2011 03:59:52   114    27     2  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321239592_17>
11/14/2011 02:59:40  11/14/2011 03:59:40   114    28     3  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321239580_17>
11/14/2011 02:59:37  11/14/2011 03:59:37   291     5    72  ERR_CIRCUIT_CHECK  HIGH_ALARM  <UTC:1321239577_17>
11/14/2011 02:59:28  11/14/2011 03:59:28   114    30     9  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321239568_17>
11/14/2011 02:59:22  11/14/2011 03:59:22   114    29     4  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321239562_17>
11/14/2011 02:59:18  11/14/2011 03:59:18   114    25     2  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321239558_17>
11/14/2011 02:59:16  11/14/2011 03:59:16   168     0 65535  ERR_UI_AUDIO_PAUSE_KEY_PRESS  KEYPRESS  <UTC:1321239556_17>
11/14/2011 02:59:11  11/14/2011 03:59:11   114    28     4  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321239551_17>
11/14/2011 02:59:07  11/14/2011 03:59:07   114    30     2  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321239547_17>
11/14/2011 02:59:04  11/14/2011 03:59:04   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1321239544_17>
11/14/2011 02:58:01  11/14/2011 03:58:01   114    30    63  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321239481_17>
11/14/2011 02:57:50  11/14/2011 03:57:50   114    30     4  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321239470_17>
11/14/2011 02:57:42  11/14/2011 03:57:42   168     0 65535  ERR_UI_AUDIO_PAUSE_KEY_PRESS  KEYPRESS  <UTC:1321239462_17>
11/14/2011 02:57:41  11/14/2011 03:57:41   291     5 65535  ERR_CIRCUIT_CHECK  HIGH_ALARM  <UTC:1321239461_17>
11/14/2011 02:57:39  11/14/2011 03:57:39   114    26     9  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321239459_17>
11/14/2011 02:57:33  11/14/2011 03:57:33   114    28     4  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321239453_17>
11/14/2011 02:57:18  11/14/2011 03:57:18   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1321239438_17>
11/14/2011 02:57:04  11/14/2011 03:57:04   114    27    13  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321239424_17>
11/14/2011 02:56:53  11/14/2011 03:56:53   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1321239413_17>
11/14/2011 02:56:51  11/14/2011 03:56:51   114    27     2  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321239411_17>
11/14/2011 02:56:39  11/14/2011 03:56:39   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1321239399_17>
11/14/2011 02:56:37  11/14/2011 03:56:37   114    21     2  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321239397_17>
11/14/2011 02:56:21  11/14/2011 03:56:21   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1321239381_17>
11/14/2011 02:55:10  11/14/2011 03:55:10   114    29    71  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321239310_17>
11/14/2011 02:53:31  11/14/2011 03:53:31   114    29    97  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321239211_17>
11/14/2011 02:53:24  11/14/2011 03:53:24   114    30     2  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321239204_17>
11/14/2011 02:53:08  11/14/2011 03:53:08   114    29    12  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321239188_17>
11/14/2011 02:53:01  11/14/2011 03:53:01   114    30     5  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321239181_17>
11/14/2011 02:52:42  11/14/2011 03:52:42   114    29    17  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321239162_17>
11/14/2011 02:52:27  11/14/2011 03:52:27   114    30     2  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321239147_17>
11/14/2011 02:52:20  11/14/2011 03:52:20   114    30     3  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321239140_17>
11/14/2011 02:52:01  11/14/2011 03:52:01   114    29    11  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321239121_17>
11/14/2011 02:51:57  11/14/2011 03:51:57   114    30     2  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321239117_17>
11/14/2011 02:51:46  11/14/2011 03:51:46   114    30     5  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321239106_17>
11/14/2011 02:51:39  11/14/2011 03:51:39   114    30     2  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321239099_17>
11/14/2011 02:51:17  11/14/2011 03:51:17   114    30     2  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321239077_17>
11/14/2011 02:51:10  11/14/2011 03:51:10   114    29     2  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321239070_17>
11/14/2011 02:50:32  11/14/2011 03:50:32   114    24     3  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321239032_17>
11/14/2011 02:50:06  11/14/2011 03:50:06   114    29    11  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321239006_17>
11/14/2011 02:50:02  11/14/2011 03:50:02   114    25     2  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321239002_17>
11/14/2011 02:49:35  11/14/2011 03:49:35   114    19    23  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321238975_17>
11/14/2011 02:49:26  11/14/2011 03:49:26   114    25     4  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321238966_17>
11/14/2011 02:49:21  11/14/2011 03:49:21   114    27     2  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321238961_17>
11/14/2011 02:49:14  11/14/2011 03:49:14   114    27     5  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321238954_17>
11/14/2011 02:49:09  11/14/2011 03:49:09   114    26     3  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321238949_17>
11/14/2011 02:49:02  11/14/2011 03:49:02   114    25     5  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321238942_17>
11/14/2011 02:48:33  11/14/2011 03:48:33   114    28    28  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321238913_17>
11/14/2011 02:48:02  11/14/2011 03:48:02   114    28    29  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321238882_17>
11/14/2011 02:47:56  11/14/2011 03:47:56   114    30     4  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321238876_17>
11/14/2011 02:47:32  11/14/2011 03:47:32   114    26     4  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321238852_17>
11/14/2011 02:47:26  11/14/2011 03:47:26   114    26     4  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321238846_17>
11/14/2011 02:47:13  11/14/2011 03:47:13   114    26    10  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321238833_17>
11/14/2011 02:47:07  11/14/2011 03:47:07   114    27     4  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321238827_17>
11/14/2011 02:47:00  11/14/2011 03:47:00   168     0 65535  ERR_UI_AUDIO_PAUSE_KEY_PRESS  KEYPRESS  <UTC:1321238820_17>
11/14/2011 02:46:56  11/14/2011 03:46:56   114    25     9  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321238816_17>
11/14/2011 02:46:50  11/14/2011 03:46:50   114    25     4  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321238810_17>
11/14/2011 02:46:19  11/14/2011 03:46:19   114    26    29  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321238779_17>
11/14/2011 02:46:08  11/14/2011 03:46:08   114    26     9  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321238768_17>
11/14/2011 02:46:01  11/14/2011 03:46:01   114    26     5  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321238761_17>
11/14/2011 02:45:06  11/14/2011 03:45:06   114    24    53  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321238706_17>
11/14/2011 02:45:00  11/14/2011 03:45:00   114    25     4  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321238700_17>
11/14/2011 02:44:48  11/14/2011 03:44:48   114    24     9  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321238688_17>
11/14/2011 02:44:42  11/14/2011 03:44:42   114    26     5  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321238682_17>
11/14/2011 02:44:05  11/14/2011 03:44:05   114    25    35  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321238645_17>
11/14/2011 02:43:59  11/14/2011 03:43:59   114    26     4  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321238639_17>
11/14/2011 02:25:30  11/14/2011 03:25:30   114    24  1107  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321237530_17>
11/14/2011 02:25:01  11/14/2011 03:25:01   114    26    27  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321237501_17>
11/14/2011 02:24:59  11/14/2011 03:24:59   291     5 65535  ERR_CIRCUIT_CHECK  HIGH_ALARM  <UTC:1321237499_17>
11/14/2011 02:24:56  11/14/2011 03:24:56   114    28     3  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321237496_17>
11/14/2011 02:24:50  11/14/2011 03:24:50   114    29     2  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321237490_17>
11/14/2011 02:24:36  11/14/2011 03:24:36   114    22    12  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321237476_17>
11/14/2011 02:24:26  11/14/2011 03:24:26   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1321237466_17>
11/14/2011 02:22:52  11/14/2011 03:22:52   114    20    94  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321237372_17>
11/14/2011 02:22:51  11/14/2011 03:22:51   291     5 65535  ERR_CIRCUIT_CHECK  HIGH_ALARM  <UTC:1321237371_17>
11/14/2011 02:22:48  11/14/2011 03:22:48   114    24     3  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321237368_17>
11/14/2011 02:22:26  11/14/2011 03:22:26   114    26    19  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321237346_17>
11/14/2011 02:21:22  11/14/2011 03:21:22   114    28    45  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321237282_17>
11/14/2011 02:21:20  11/14/2011 03:21:20   291     5    54  ERR_CIRCUIT_CHECK  HIGH_ALARM  <UTC:1321237280_17>
11/14/2011 02:21:02  11/14/2011 03:21:02   114    23     9  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321237262_17>
11/14/2011 02:20:50  11/14/2011 03:20:50   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1321237250_17>
11/14/2011 02:20:48  11/14/2011 03:20:48   114    30     2  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321237248_17>
11/14/2011 02:19:10  11/14/2011 03:19:10   114    30    26  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321237150_17>
11/14/2011 02:18:45  11/14/2011 03:18:45   114    28     4  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321237125_17>
11/14/2011 02:18:12  11/14/2011 03:18:12   114    27     8  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321237092_17>
11/14/2011 02:18:07  11/14/2011 03:18:07   114    27     2  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321237087_17>
11/14/2011 02:17:45  11/14/2011 03:17:45   291     5    10  ERR_CIRCUIT_CHECK  HIGH_ALARM  <UTC:1321237065_17>
11/14/2011 02:17:23  11/14/2011 03:17:23   114    27    36  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321237043_17>
11/14/2011 02:16:48  11/14/2011 03:16:48   114    29    11  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321237008_17>
11/14/2011 02:16:31  11/14/2011 03:16:31   114    29    11  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321236991_17>
11/14/2011 02:16:31  11/14/2011 03:16:31   291     5    41  ERR_CIRCUIT_CHECK  HIGH_ALARM  <UTC:1321236991_17>
11/14/2011 02:16:16  11/14/2011 03:16:16   114    28    10  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321236976_17>
11/14/2011 02:15:41  11/14/2011 03:15:41   114    26    25  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321236941_17>
11/14/2011 02:15:18  11/14/2011 03:15:18   291     5    16  ERR_CIRCUIT_CHECK  HIGH_ALARM  <UTC:1321236918_17>
11/14/2011 02:14:41  11/14/2011 03:14:41   114    28    47  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321236881_17>
11/14/2011 02:14:35  11/14/2011 03:14:35   114    30     5  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321236875_17>
11/14/2011 02:14:26  11/14/2011 03:14:26   114    29     8  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321236866_17>
11/14/2011 02:13:27  11/14/2011 03:13:27   114    27    41  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321236807_17>
11/14/2011 02:13:10  11/14/2011 03:13:10   114    30    10  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321236790_17>
11/14/2011 02:12:59  11/14/2011 03:12:59   114    29    10  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321236779_17>
11/14/2011 02:12:49  11/14/2011 03:12:49   291     5    25  ERR_CIRCUIT_CHECK  HIGH_ALARM  <UTC:1321236769_17>
11/14/2011 02:12:43  11/14/2011 03:12:43   114    30    10  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321236763_17>
11/14/2011 02:12:27  11/14/2011 03:12:27   114    29    12  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321236747_17>
11/14/2011 02:12:17  11/14/2011 03:12:17   114    30     5  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321236737_17>
11/14/2011 02:11:41  11/14/2011 03:11:41   114    29     4  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321236701_17>
11/14/2011 02:11:24  11/14/2011 03:11:24   114    27     9  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321236684_17>
11/14/2011 02:11:18  11/14/2011 03:11:18   291     5    11  ERR_CIRCUIT_CHECK  HIGH_ALARM  <UTC:1321236678_17>
11/14/2011 02:11:06  11/14/2011 03:11:06   114    30     6  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321236666_17>
11/14/2011 02:10:17  11/14/2011 03:10:17   291     5    10  ERR_CIRCUIT_CHECK  HIGH_ALARM  <UTC:1321236617_17>
11/14/2011 02:09:50  11/14/2011 03:09:50   114    24    31  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321236590_17>
11/14/2011 02:09:20  11/14/2011 03:09:20   114    30     4  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321236560_17>
11/14/2011 02:08:52  11/14/2011 03:08:52   114    30    20  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321236532_17>
11/14/2011 02:08:31  11/14/2011 03:08:31   114    28    10  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321236511_17>
11/14/2011 02:07:59  11/14/2011 03:07:59   114    28    15  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321236479_17>
11/14/2011 02:07:54  11/14/2011 03:07:54   114    30     4  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321236474_17>
11/14/2011 02:07:28  11/14/2011 03:07:28   114    27     9  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321236448_17>
11/14/2011 02:06:55  11/14/2011 03:06:55   291     5     5  ERR_CIRCUIT_CHECK  HIGH_ALARM  <UTC:1321236415_17>
11/14/2011 02:06:23  11/14/2011 03:06:23   114    27    16  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321236383_17>
11/14/2011 02:04:51  11/14/2011 03:04:51   114    30     3  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321236291_17>
11/14/2011 02:04:46  11/14/2011 03:04:46   114    30     3  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321236286_17>
11/14/2011 02:04:18  11/14/2011 03:04:18   114    29    27  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321236258_17>
11/14/2011 02:04:13  11/14/2011 03:04:13   114    29     4  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321236253_17>
11/14/2011 02:04:02  11/14/2011 03:04:02   291     5    15  ERR_CIRCUIT_CHECK  HIGH_ALARM  <UTC:1321236242_17>
11/14/2011 02:03:23  11/14/2011 03:03:23   114    29    48  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321236203_17>
11/14/2011 02:02:39  11/14/2011 03:02:39   114    26     8  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321236159_17>
11/14/2011 02:01:34  11/14/2011 03:01:34   114    28    10  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321236094_17>
11/14/2011 02:01:27  11/14/2011 03:01:27   114    30     2  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321236087_17>
11/14/2011 02:01:13  11/14/2011 03:01:13   114    26     8  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321236073_17>
11/14/2011 01:59:29  11/14/2011 02:59:29   168     0 65535  ERR_UI_AUDIO_PAUSE_KEY_PRESS  KEYPRESS  <UTC:1321235969_17>
11/14/2011 01:59:22  11/14/2011 02:59:22   114    27    10  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321235962_17>
11/14/2011 01:57:36  11/14/2011 02:57:36   114    30     4  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321235856_17>
11/14/2011 01:57:11  11/14/2011 02:57:11   114    29     4  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321235831_17>
11/14/2011 01:51:44  11/14/2011 02:51:44   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1321235504_17>
11/14/2011 01:41:03  11/14/2011 02:41:03   291     5    14  ERR_CIRCUIT_CHECK  HIGH_ALARM  <UTC:1321234863_17>
11/14/2011 01:40:36  11/14/2011 02:40:36   114    28    36  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321234836_17>
11/14/2011 01:40:32  11/14/2011 02:40:32   114    30     4  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321234832_17>
11/14/2011 01:39:52  11/14/2011 02:39:52   114    28    23  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321234792_17>
11/14/2011 01:39:37  11/14/2011 02:39:37   114    29    10  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321234777_17>
11/14/2011 01:39:05  11/14/2011 02:39:05   291     5    12  ERR_CIRCUIT_CHECK  HIGH_ALARM  <UTC:1321234745_17>
11/14/2011 01:38:37  11/14/2011 02:38:37   114    26    50  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321234717_17>
11/14/2011 01:35:30  11/14/2011 02:35:30   114    27    24  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321234530_17>
11/14/2011 01:34:36  11/14/2011 02:34:36   114    29    28  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321234476_17>
11/14/2011 01:10:22  11/14/2011 02:10:22   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1321233022_17>
11/14/2011 01:10:04  11/14/2011 02:10:04   114    25     2  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321233004_17>
11/14/2011 01:09:40  11/14/2011 02:09:40   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1321232980_17>
11/14/2011 01:09:12  11/14/2011 02:09:12   114    27     3  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321232952_17>
11/14/2011 01:07:15  11/14/2011 02:07:15   291     5    26  ERR_CIRCUIT_CHECK  HIGH_ALARM  <UTC:1321232835_17>
11/14/2011 01:07:02  11/14/2011 02:07:02   114    29     4  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321232822_17>
11/14/2011 00:57:00  11/14/2011 01:57:00   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1321232220_17>
11/14/2011 00:55:22  11/14/2011 01:55:22   114    28     4  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321232122_17>
11/14/2011 00:53:30  11/14/2011 01:53:30   114    30    51  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321232010_17>
11/14/2011 00:53:11  11/14/2011 01:53:11   114    25     3  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321231991_17>
11/14/2011 00:53:02  11/14/2011 01:53:02   114    24     4  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321231982_17>
11/14/2011 00:52:46  11/14/2011 01:52:46   114    30     8  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321231966_17>
11/14/2011 00:52:43  11/14/2011 01:52:43   114    26     2  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321231963_17>
11/14/2011 00:52:35  11/14/2011 01:52:35   114    29     4  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321231955_17>
11/14/2011 00:52:26  11/14/2011 01:52:26   114    30     2  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321231946_17>
11/14/2011 00:51:17  11/14/2011 01:51:17   114    30     2  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321231877_17>
11/14/2011 00:51:11  11/14/2011 01:51:11   114    30     3  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321231871_17>
11/14/2011 00:50:48  11/14/2011 01:50:48   114    27     5  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321231848_17>
11/14/2011 00:50:28  11/14/2011 01:50:28   114    27     6  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321231828_17>
11/14/2011 00:50:05  11/14/2011 01:50:05   114    26     3  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321231805_17>
11/14/2011 00:49:46  11/14/2011 01:49:46   114    29     5  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321231786_17>
11/14/2011 00:49:11  11/14/2011 01:49:11   114    28     3  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321231751_17>
11/14/2011 00:48:58  11/14/2011 01:48:58   291     5   159  ERR_CIRCUIT_CHECK  HIGH_ALARM  <UTC:1321231738_17>
11/14/2011 00:48:45  11/14/2011 01:48:45   114    25     8  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321231725_17>
11/14/2011 00:48:25  11/14/2011 01:48:25   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1321231705_17>
11/14/2011 00:47:26  11/14/2011 01:47:26   114    28     3  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321231646_17>
11/14/2011 00:46:26  11/14/2011 01:46:26   114    28     2  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321231586_17>
11/14/2011 00:45:02  11/14/2011 01:45:02   114    27    12  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321231502_17>
11/14/2011 00:44:25  11/14/2011 01:44:25   114    26    15  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321231465_17>
11/14/2011 00:44:21  11/14/2011 01:44:21   114    29     2  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321231461_17>
11/14/2011 00:44:14  11/14/2011 01:44:14   114    30     2  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321231454_17>
11/14/2011 00:43:13  11/14/2011 01:43:13   291     5   277  ERR_CIRCUIT_CHECK  HIGH_ALARM  <UTC:1321231393_17>
11/14/2011 00:42:00  11/14/2011 01:42:00   114    28     2  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321231320_17>
11/14/2011 00:41:54  11/14/2011 01:41:54   114    30     4  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321231314_17>
11/14/2011 00:41:49  11/14/2011 01:41:49   114    30     2  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321231309_17>
11/14/2011 00:41:42  11/14/2011 01:41:42   114    28     2  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321231302_17>
11/14/2011 00:41:31  11/14/2011 01:41:31   114    29     2  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321231291_17>
11/14/2011 00:41:13  11/14/2011 01:41:13   114    28     2  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321231273_17>
11/14/2011 00:41:09  11/14/2011 01:41:09   114    29     3  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321231269_17>
11/14/2011 00:41:03  11/14/2011 01:41:03   114    27     2  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321231263_17>
11/14/2011 00:40:47  11/14/2011 01:40:47   114    30    12  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321231247_17>
11/14/2011 00:40:37  11/14/2011 01:40:37   114    29     2  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321231237_17>
11/14/2011 00:40:31  11/14/2011 01:40:31   114    29     2  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321231231_17>
11/14/2011 00:40:12  11/14/2011 01:40:12   114    30     1  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321231212_17>
11/14/2011 00:40:03  11/14/2011 01:40:03   291     5   155  ERR_CIRCUIT_CHECK  HIGH_ALARM  <UTC:1321231203_17>
11/14/2011 00:39:45  11/14/2011 01:39:45   114    30    13  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321231185_17>
11/14/2011 00:39:35  11/14/2011 01:39:35   114    26     5  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321231175_17>
11/14/2011 00:39:31  11/14/2011 01:39:31   114    30     2  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321231171_17>
11/14/2011 00:39:17  11/14/2011 01:39:17   114    26     4  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321231157_17>
11/14/2011 00:39:10  11/14/2011 01:39:10   114    29     2  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321231150_17>
11/14/2011 00:39:03  11/14/2011 01:39:03   114    30     2  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321231143_17>
11/14/2011 00:38:49  11/14/2011 01:38:49   114    27     3  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321231129_17>
11/14/2011 00:38:35  11/14/2011 01:38:35   114    25     3  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321231115_17>
11/14/2011 00:38:29  11/14/2011 01:38:29   114    27     4  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321231109_17>
11/14/2011 00:38:24  11/14/2011 01:38:24   114    26     2  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321231104_17>
11/14/2011 00:38:12  11/14/2011 01:38:12   114    27     3  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321231092_17>
11/14/2011 00:37:51  11/14/2011 01:37:51   291     5    90  ERR_CIRCUIT_CHECK  HIGH_ALARM  <UTC:1321231071_17>
11/14/2011 00:37:24  11/14/2011 01:37:24   114    12    12  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321231044_17>
11/14/2011 00:37:02  11/14/2011 01:37:02   114    27     4  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321231022_17>
11/14/2011 00:36:42  11/14/2011 01:36:42   114    21    19  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321231002_17>
11/14/2011 00:35:57  11/14/2011 01:35:57   114    24     8  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321230957_17>
11/14/2011 00:35:52  11/14/2011 01:35:52   114    25     3  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321230952_17>
11/14/2011 00:35:48  11/14/2011 01:35:48   114    29     2  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321230948_17>
11/14/2011 00:35:48  11/14/2011 01:35:48   291     5    86  ERR_CIRCUIT_CHECK  HIGH_ALARM  <UTC:1321230948_17>
11/14/2011 00:35:42  11/14/2011 01:35:42   114    30     2  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321230942_17>
11/14/2011 00:35:37  11/14/2011 01:35:37   114    30     2  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321230937_17>
11/14/2011 00:35:31  11/14/2011 01:35:31   114    30     3  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321230931_17>
11/14/2011 00:35:24  11/14/2011 01:35:24   114    28     3  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321230924_17>
11/14/2011 00:35:09  11/14/2011 01:35:09   114    26     3  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321230909_17>
11/14/2011 00:35:01  11/14/2011 01:35:01   114    30     3  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321230901_17>
11/14/2011 00:34:50  11/14/2011 01:34:50   114    27    10  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321230890_17>
11/14/2011 00:34:39  11/14/2011 01:34:39   114    29     3  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321230879_17>
11/14/2011 00:34:28  11/14/2011 01:34:28   291     5    44  ERR_CIRCUIT_CHECK  HIGH_ALARM  <UTC:1321230868_17>
11/14/2011 00:34:07  11/14/2011 01:34:07   114    24    30  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321230847_17>
11/14/2011 00:33:30  11/14/2011 01:33:30   114    24    19  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321230810_17>
11/14/2011 00:33:12  11/14/2011 01:33:12   114    14    14  ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM  <UTC:1321230792_17>
11/14/2011 00:33:09  11/14/2011 01:33:09   166     0 65535  ERR_UI_RESET_KEY_PRESS  KEYPRESS  <UTC:1321230789_17>

---------------------------------------------------------------
LOG ID 18 (Encrypted Engineering Debug Text) 293468 total bytes
---------------------------------------------------------------
     UTC Time         Err Descr
01/15/2012 11:50:47   148  ERR_DEBUG  LOG_ONLY  <UTC:1326628247_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2957 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=52) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 11:52:19   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326628339_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2957 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=51) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=CP:128  
01/15/2012 11:52:52   148  ERR_DEBUG  LOG_ONLY  <UTC:1326628372_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2957 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=51) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 11:52:52   148  ERR_DEBUG  LOG_ONLY  <UTC:1326628372_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2957 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=51) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 11:55:57   148  ERR_DEBUG  LOG_ONLY  <UTC:1326628557_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2957 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=49) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 11:55:57   148  ERR_DEBUG  LOG_ONLY  <UTC:1326628557_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2957 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=49) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 11:56:15   148  ERR_DEBUG  LOG_ONLY  <UTC:1326628575_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=49) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 11:56:15   148  ERR_DEBUG  LOG_ONLY  <UTC:1326628575_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=49) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 11:56:40   148  ERR_DEBUG  LOG_ONLY  <UTC:1326628600_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=49) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 11:56:42   148  ERR_DEBUG  LOG_ONLY  <UTC:1326628602_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=49) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 132
01/15/2012 11:58:03   148  ERR_DEBUG  LOG_ONLY  <UTC:1326628683_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=48) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 11:58:03   148  ERR_DEBUG  LOG_ONLY  <UTC:1326628683_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=48) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 11:59:30   148  ERR_DEBUG  LOG_ONLY  <UTC:1326628770_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=48) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 11:59:30   148  ERR_DEBUG  LOG_ONLY  <UTC:1326628770_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=48) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 11:59:48   148  ERR_DEBUG  LOG_ONLY  <UTC:1326628788_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=48) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 11:59:48   148  ERR_DEBUG  LOG_ONLY  <UTC:1326628788_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=48) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=20
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 11:59:58   148  ERR_DEBUG  LOG_ONLY  <UTC:1326628798_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=48) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=20
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 11:59:58   148  ERR_DEBUG  LOG_ONLY  <UTC:1326628798_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=48) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=20
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 5
01/15/2012 12:00:51   148  ERR_DEBUG  LOG_ONLY  <UTC:1326628851_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=47) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:00:51   148  ERR_DEBUG  LOG_ONLY  <UTC:1326628851_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=47) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=20
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 12:01:22   148  ERR_DEBUG  LOG_ONLY  <UTC:1326628882_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=47) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:01:22   148  ERR_DEBUG  LOG_ONLY  <UTC:1326628882_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=47) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 7
01/15/2012 12:02:02   148  ERR_DEBUG  LOG_ONLY  <UTC:1326628922_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=47) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:02:02   148  ERR_DEBUG  LOG_ONLY  <UTC:1326628922_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=47) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 12:02:25   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326628945_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=47) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=20
                         Reserved(Offset=52)=00
                         Opt.Text=CP:128  
01/15/2012 12:03:10   148  ERR_DEBUG  LOG_ONLY  <UTC:1326628990_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=46) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:03:10   148  ERR_DEBUG  LOG_ONLY  <UTC:1326628990_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=46) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 12:04:09   148  ERR_DEBUG  LOG_ONLY  <UTC:1326629049_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=46) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:04:09   148  ERR_DEBUG  LOG_ONLY  <UTC:1326629049_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=46) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 12:04:36   148  ERR_DEBUG  LOG_ONLY  <UTC:1326629076_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=46) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:04:36   148  ERR_DEBUG  LOG_ONLY  <UTC:1326629076_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=46) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 12:05:19   148  ERR_DEBUG  LOG_ONLY  <UTC:1326629119_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=45) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:05:19   148  ERR_DEBUG  LOG_ONLY  <UTC:1326629119_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=45) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 12:05:40   148  ERR_DEBUG  LOG_ONLY  <UTC:1326629140_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=45) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:05:40   148  ERR_DEBUG  LOG_ONLY  <UTC:1326629140_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=45) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=21
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 12:06:09   148  ERR_DEBUG  LOG_ONLY  <UTC:1326629169_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=45) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:06:09   148  ERR_DEBUG  LOG_ONLY  <UTC:1326629169_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=45) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 12:06:24   148  ERR_DEBUG  LOG_ONLY  <UTC:1326629184_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=45) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=66 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:06:24   148  ERR_DEBUG  LOG_ONLY  <UTC:1326629184_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=45) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=66 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 12:07:26   148  ERR_DEBUG  LOG_ONLY  <UTC:1326629246_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=44) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:07:26   148  ERR_DEBUG  LOG_ONLY  <UTC:1326629246_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=44) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 12:08:55   148  ERR_DEBUG  LOG_ONLY  <UTC:1326629335_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=43) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:08:55   148  ERR_DEBUG  LOG_ONLY  <UTC:1326629335_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=43) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 12:09:26   148  ERR_DEBUG  LOG_ONLY  <UTC:1326629366_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=43) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:09:27   148  ERR_DEBUG  LOG_ONLY  <UTC:1326629367_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=43) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 80
01/15/2012 12:10:15   148  ERR_DEBUG  LOG_ONLY  <UTC:1326629415_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=43) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=66 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:10:15   148  ERR_DEBUG  LOG_ONLY  <UTC:1326629415_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=43) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 12:10:37   148  ERR_DEBUG  LOG_ONLY  <UTC:1326629437_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=43) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:10:37   148  ERR_DEBUG  LOG_ONLY  <UTC:1326629437_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=43) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 12:11:08   148  ERR_DEBUG  LOG_ONLY  <UTC:1326629468_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=42) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:11:08   148  ERR_DEBUG  LOG_ONLY  <UTC:1326629468_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=42) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 12:11:27   148  ERR_DEBUG  LOG_ONLY  <UTC:1326629487_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=42) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:11:27   148  ERR_DEBUG  LOG_ONLY  <UTC:1326629487_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=42) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1
01/15/2012 12:11:37   148  ERR_DEBUG  LOG_ONLY  <UTC:1326629497_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=42) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:11:37   148  ERR_DEBUG  LOG_ONLY  <UTC:1326629497_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=42) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 12:12:04   148  ERR_DEBUG  LOG_ONLY  <UTC:1326629524_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=42) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:12:04   148  ERR_DEBUG  LOG_ONLY  <UTC:1326629524_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=42) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 12:12:27   148  ERR_DEBUG  LOG_ONLY  <UTC:1326629547_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=42) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:12:28   148  ERR_DEBUG  LOG_ONLY  <UTC:1326629548_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=42) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 29
01/15/2012 12:13:10   148  ERR_DEBUG  LOG_ONLY  <UTC:1326629590_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=41) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:13:12   148  ERR_DEBUG  LOG_ONLY  <UTC:1326629592_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=41) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 143
01/15/2012 12:13:41   148  ERR_DEBUG  LOG_ONLY  <UTC:1326629621_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=41) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:13:41   148  ERR_DEBUG  LOG_ONLY  <UTC:1326629621_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=41) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 11
01/15/2012 12:14:53   148  ERR_DEBUG  LOG_ONLY  <UTC:1326629693_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=41) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:14:53   148  ERR_DEBUG  LOG_ONLY  <UTC:1326629693_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=41) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 51
01/15/2012 12:15:06   148  ERR_DEBUG  LOG_ONLY  <UTC:1326629706_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=41) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:15:06   148  ERR_DEBUG  LOG_ONLY  <UTC:1326629706_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=41) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 12:15:33   148  ERR_DEBUG  LOG_ONLY  <UTC:1326629733_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=40) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:15:33   148  ERR_DEBUG  LOG_ONLY  <UTC:1326629733_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=40) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 49
01/15/2012 12:15:55   148  ERR_DEBUG  LOG_ONLY  <UTC:1326629755_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=40) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:15:56   148  ERR_DEBUG  LOG_ONLY  <UTC:1326629756_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=40) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 88
01/15/2012 12:16:49   148  ERR_DEBUG  LOG_ONLY  <UTC:1326629809_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=40) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:16:49   148  ERR_DEBUG  LOG_ONLY  <UTC:1326629809_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=40) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 12:17:11   148  ERR_DEBUG  LOG_ONLY  <UTC:1326629831_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=40) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:17:11   148  ERR_DEBUG  LOG_ONLY  <UTC:1326629831_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=40) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 12:17:37   148  ERR_DEBUG  LOG_ONLY  <UTC:1326629857_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=39) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:17:37   148  ERR_DEBUG  LOG_ONLY  <UTC:1326629857_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=39) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 12:18:29   148  ERR_DEBUG  LOG_ONLY  <UTC:1326629909_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=39) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:18:29   148  ERR_DEBUG  LOG_ONLY  <UTC:1326629909_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=39) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 12:18:38   148  ERR_DEBUG  LOG_ONLY  <UTC:1326629918_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=39) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:18:38   148  ERR_DEBUG  LOG_ONLY  <UTC:1326629918_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=39) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 12:19:47   148  ERR_DEBUG  LOG_ONLY  <UTC:1326629987_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=38) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=27
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:19:47   148  ERR_DEBUG  LOG_ONLY  <UTC:1326629987_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=38) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=27
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 12:20:36   148  ERR_DEBUG  LOG_ONLY  <UTC:1326630036_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=38) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:20:36   148  ERR_DEBUG  LOG_ONLY  <UTC:1326630036_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=38) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=20
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 30
01/15/2012 12:20:47   148  ERR_DEBUG  LOG_ONLY  <UTC:1326630047_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=38) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:20:47   148  ERR_DEBUG  LOG_ONLY  <UTC:1326630047_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=38) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 12:21:39   148  ERR_DEBUG  LOG_ONLY  <UTC:1326630099_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=37) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:21:39   148  ERR_DEBUG  LOG_ONLY  <UTC:1326630099_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=37) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 12:22:34   148  ERR_DEBUG  LOG_ONLY  <UTC:1326630154_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=37) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:22:34   148  ERR_DEBUG  LOG_ONLY  <UTC:1326630154_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=37) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 12:23:31   148  ERR_DEBUG  LOG_ONLY  <UTC:1326630211_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=36) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:23:31   148  ERR_DEBUG  LOG_ONLY  <UTC:1326630211_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=36) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 12:24:05   148  ERR_DEBUG  LOG_ONLY  <UTC:1326630245_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=36) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:24:05   148  ERR_DEBUG  LOG_ONLY  <UTC:1326630245_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=36) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 12:24:59   148  ERR_DEBUG  LOG_ONLY  <UTC:1326630299_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=36) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:24:59   148  ERR_DEBUG  LOG_ONLY  <UTC:1326630299_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=36) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 12:25:23   148  ERR_DEBUG  LOG_ONLY  <UTC:1326630323_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=36) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:25:23   148  ERR_DEBUG  LOG_ONLY  <UTC:1326630323_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=36) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 12:25:41   148  ERR_DEBUG  LOG_ONLY  <UTC:1326630341_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=35) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:25:41   148  ERR_DEBUG  LOG_ONLY  <UTC:1326630341_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=35) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 12:26:21   148  ERR_DEBUG  LOG_ONLY  <UTC:1326630381_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=35) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:26:23   148  ERR_DEBUG  LOG_ONLY  <UTC:1326630383_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=35) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 155
01/15/2012 12:27:05   148  ERR_DEBUG  LOG_ONLY  <UTC:1326630425_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=35) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:27:05   148  ERR_DEBUG  LOG_ONLY  <UTC:1326630425_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=35) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 12:27:33   148  ERR_DEBUG  LOG_ONLY  <UTC:1326630453_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=35) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:27:33   148  ERR_DEBUG  LOG_ONLY  <UTC:1326630453_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=35) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 12:28:14   148  ERR_DEBUG  LOG_ONLY  <UTC:1326630494_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=34) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:28:15   148  ERR_DEBUG  LOG_ONLY  <UTC:1326630495_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=34) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 106
01/15/2012 12:28:49   148  ERR_DEBUG  LOG_ONLY  <UTC:1326630529_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=34) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:28:49   148  ERR_DEBUG  LOG_ONLY  <UTC:1326630529_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=34) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 12:29:05   148  ERR_DEBUG  LOG_ONLY  <UTC:1326630545_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=34) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:29:06   148  ERR_DEBUG  LOG_ONLY  <UTC:1326630546_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=34) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 98
01/15/2012 12:29:31   148  ERR_DEBUG  LOG_ONLY  <UTC:1326630571_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=34) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:29:31   148  ERR_DEBUG  LOG_ONLY  <UTC:1326630571_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=34) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 4
01/15/2012 12:29:57   148  ERR_DEBUG  LOG_ONLY  <UTC:1326630597_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=33) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:29:57   148  ERR_DEBUG  LOG_ONLY  <UTC:1326630597_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=33) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 12:30:24   148  ERR_DEBUG  LOG_ONLY  <UTC:1326630624_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=33) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:30:24   148  ERR_DEBUG  LOG_ONLY  <UTC:1326630624_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=33) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 12:30:55   148  ERR_DEBUG  LOG_ONLY  <UTC:1326630655_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=33) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:30:55   148  ERR_DEBUG  LOG_ONLY  <UTC:1326630655_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=33) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 3
01/15/2012 12:31:51   148  ERR_DEBUG  LOG_ONLY  <UTC:1326630711_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=32) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:31:51   148  ERR_DEBUG  LOG_ONLY  <UTC:1326630711_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=32) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 59
01/15/2012 12:32:18   148  ERR_DEBUG  LOG_ONLY  <UTC:1326630738_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=32) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:32:18   148  ERR_DEBUG  LOG_ONLY  <UTC:1326630738_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=32) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 12:33:52   148  ERR_DEBUG  LOG_ONLY  <UTC:1326630832_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=31) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:33:52   148  ERR_DEBUG  LOG_ONLY  <UTC:1326630832_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=31) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 12:34:05   148  ERR_DEBUG  LOG_ONLY  <UTC:1326630845_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=31) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:34:05   148  ERR_DEBUG  LOG_ONLY  <UTC:1326630845_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=31) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 12:35:41   148  ERR_DEBUG  LOG_ONLY  <UTC:1326630941_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=31) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:35:42   148  ERR_DEBUG  LOG_ONLY  <UTC:1326630942_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=31) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 77
01/15/2012 12:36:10   148  ERR_DEBUG  LOG_ONLY  <UTC:1326630970_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=30) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:36:10   148  ERR_DEBUG  LOG_ONLY  <UTC:1326630970_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=30) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 12:37:05   148  ERR_DEBUG  LOG_ONLY  <UTC:1326631025_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=30) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:37:05   148  ERR_DEBUG  LOG_ONLY  <UTC:1326631025_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=30) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 12:38:04   148  ERR_DEBUG  LOG_ONLY  <UTC:1326631084_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=29) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:38:04   148  ERR_DEBUG  LOG_ONLY  <UTC:1326631084_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=29) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 12:38:28   148  ERR_DEBUG  LOG_ONLY  <UTC:1326631108_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=29) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:38:28   148  ERR_DEBUG  LOG_ONLY  <UTC:1326631108_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=29) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 12:38:51   148  ERR_DEBUG  LOG_ONLY  <UTC:1326631131_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=29) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:38:51   148  ERR_DEBUG  LOG_ONLY  <UTC:1326631131_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=29) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 12:39:17   148  ERR_DEBUG  LOG_ONLY  <UTC:1326631157_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=29) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:39:17   148  ERR_DEBUG  LOG_ONLY  <UTC:1326631157_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=29) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 3
01/15/2012 12:40:23   148  ERR_DEBUG  LOG_ONLY  <UTC:1326631223_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=28) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:40:23   148  ERR_DEBUG  LOG_ONLY  <UTC:1326631223_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=28) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 12:40:42   148  ERR_DEBUG  LOG_ONLY  <UTC:1326631242_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=28) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:40:42   148  ERR_DEBUG  LOG_ONLY  <UTC:1326631242_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=28) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 12:41:47   148  ERR_DEBUG  LOG_ONLY  <UTC:1326631307_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=28) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=66 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:41:47   148  ERR_DEBUG  LOG_ONLY  <UTC:1326631307_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=28) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=66 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 12:44:47   148  ERR_DEBUG  LOG_ONLY  <UTC:1326631487_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=26) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:44:47   148  ERR_DEBUG  LOG_ONLY  <UTC:1326631487_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=26) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 12:45:06   148  ERR_DEBUG  LOG_ONLY  <UTC:1326631506_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=26) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:45:06   148  ERR_DEBUG  LOG_ONLY  <UTC:1326631506_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=26) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 12:45:20   148  ERR_DEBUG  LOG_ONLY  <UTC:1326631520_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=26) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:45:20   148  ERR_DEBUG  LOG_ONLY  <UTC:1326631520_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=26) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 12:45:43   148  ERR_DEBUG  LOG_ONLY  <UTC:1326631543_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=26) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:45:43   148  ERR_DEBUG  LOG_ONLY  <UTC:1326631543_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=26) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 12:46:28   148  ERR_DEBUG  LOG_ONLY  <UTC:1326631588_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=25) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:46:29   148  ERR_DEBUG  LOG_ONLY  <UTC:1326631589_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=25) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 12:47:08   148  ERR_DEBUG  LOG_ONLY  <UTC:1326631628_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=25) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:47:08   148  ERR_DEBUG  LOG_ONLY  <UTC:1326631628_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=25) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 12:47:44   148  ERR_DEBUG  LOG_ONLY  <UTC:1326631664_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=25) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:47:44   148  ERR_DEBUG  LOG_ONLY  <UTC:1326631664_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=25) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 12:48:04   148  ERR_DEBUG  LOG_ONLY  <UTC:1326631684_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=25) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:48:04   148  ERR_DEBUG  LOG_ONLY  <UTC:1326631684_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=25) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 12:48:39   148  ERR_DEBUG  LOG_ONLY  <UTC:1326631719_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=24) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:48:40   148  ERR_DEBUG  LOG_ONLY  <UTC:1326631720_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=24) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 139
01/15/2012 12:49:58   148  ERR_DEBUG  LOG_ONLY  <UTC:1326631798_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=24) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:49:58   148  ERR_DEBUG  LOG_ONLY  <UTC:1326631798_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=24) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 8
01/15/2012 12:51:03   148  ERR_DEBUG  LOG_ONLY  <UTC:1326631863_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=23) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:51:03   148  ERR_DEBUG  LOG_ONLY  <UTC:1326631863_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=23) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 12:54:05   148  ERR_DEBUG  LOG_ONLY  <UTC:1326632045_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=22) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:54:05   148  ERR_DEBUG  LOG_ONLY  <UTC:1326632045_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=22) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 12:54:30   148  ERR_DEBUG  LOG_ONLY  <UTC:1326632070_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=22) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:54:30   148  ERR_DEBUG  LOG_ONLY  <UTC:1326632070_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=22) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 10
01/15/2012 12:55:18   148  ERR_DEBUG  LOG_ONLY  <UTC:1326632118_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=21) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:55:18   148  ERR_DEBUG  LOG_ONLY  <UTC:1326632118_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=21) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 12:57:07   148  ERR_DEBUG  LOG_ONLY  <UTC:1326632227_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=20) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:57:07   148  ERR_DEBUG  LOG_ONLY  <UTC:1326632227_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=20) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 12:57:28   148  ERR_DEBUG  LOG_ONLY  <UTC:1326632248_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=20) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:57:28   148  ERR_DEBUG  LOG_ONLY  <UTC:1326632248_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=20) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 55
01/15/2012 12:59:34   148  ERR_DEBUG  LOG_ONLY  <UTC:1326632374_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=19) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 12:59:34   148  ERR_DEBUG  LOG_ONLY  <UTC:1326632374_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=19) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 13:00:22   148  ERR_DEBUG  LOG_ONLY  <UTC:1326632422_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=19) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 13:00:22   148  ERR_DEBUG  LOG_ONLY  <UTC:1326632422_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=19) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 13:00:51   148  ERR_DEBUG  LOG_ONLY  <UTC:1326632451_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=19) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 13:00:51   148  ERR_DEBUG  LOG_ONLY  <UTC:1326632451_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=19) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 13:01:21   148  ERR_DEBUG  LOG_ONLY  <UTC:1326632481_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=18) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 13:01:21   148  ERR_DEBUG  LOG_ONLY  <UTC:1326632481_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=18) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=20
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 13:02:30   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326632550_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2953 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=18) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=CP:131  
01/15/2012 13:03:14   148  ERR_DEBUG  LOG_ONLY  <UTC:1326632594_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2953 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=18) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 13:03:14   148  ERR_DEBUG  LOG_ONLY  <UTC:1326632594_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2953 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=18) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 13:04:22   148  ERR_DEBUG  LOG_ONLY  <UTC:1326632662_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2953 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=17) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 13:04:22   148  ERR_DEBUG  LOG_ONLY  <UTC:1326632662_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2953 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=17) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 13:05:54   148  ERR_DEBUG  LOG_ONLY  <UTC:1326632754_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2953 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=16) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 13:05:54   148  ERR_DEBUG  LOG_ONLY  <UTC:1326632754_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2953 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=16) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 13:06:52   148  ERR_DEBUG  LOG_ONLY  <UTC:1326632812_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2953 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=16) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 13:06:52   148  ERR_DEBUG  LOG_ONLY  <UTC:1326632812_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2953 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=16) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 13:09:47   148  ERR_DEBUG  LOG_ONLY  <UTC:1326632987_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2953 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=15) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 13:09:47   148  ERR_DEBUG  LOG_ONLY  <UTC:1326632987_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2953 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=15) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 13:11:51   148  ERR_DEBUG  LOG_ONLY  <UTC:1326633111_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2953 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=13) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 13:11:51   148  ERR_DEBUG  LOG_ONLY  <UTC:1326633111_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2953 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=13) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 14
01/15/2012 13:12:15   148  ERR_DEBUG  LOG_ONLY  <UTC:1326633135_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2953 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=13) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 13:12:15   148  ERR_DEBUG  LOG_ONLY  <UTC:1326633135_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2953 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=13) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 4
01/15/2012 13:15:58   148  ERR_DEBUG  LOG_ONLY  <UTC:1326633358_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2953 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=12) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 13:15:58   148  ERR_DEBUG  LOG_ONLY  <UTC:1326633358_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2953 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=12) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 13
01/15/2012 13:16:51   148  ERR_DEBUG  LOG_ONLY  <UTC:1326633411_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2953 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=12) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 13:16:51   148  ERR_DEBUG  LOG_ONLY  <UTC:1326633411_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2953 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=12) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 13:17:44   148  ERR_DEBUG  LOG_ONLY  <UTC:1326633464_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2953 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=12) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 13:17:44   148  ERR_DEBUG  LOG_ONLY  <UTC:1326633464_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2953 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=12) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 11
01/15/2012 13:18:33   148  ERR_DEBUG  LOG_ONLY  <UTC:1326633513_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2953 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=11) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 13:18:33   148  ERR_DEBUG  LOG_ONLY  <UTC:1326633513_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2953 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=11) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 13:19:01   148  ERR_DEBUG  LOG_ONLY  <UTC:1326633541_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2953 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=11) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 13:19:01   148  ERR_DEBUG  LOG_ONLY  <UTC:1326633541_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2953 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=11) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 13:19:32   148  ERR_DEBUG  LOG_ONLY  <UTC:1326633572_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2953 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=11) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 13:19:32   148  ERR_DEBUG  LOG_ONLY  <UTC:1326633572_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2953 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=11) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 13:20:51   148  ERR_DEBUG  LOG_ONLY  <UTC:1326633651_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2953 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=10) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 13:20:51   148  ERR_DEBUG  LOG_ONLY  <UTC:1326633651_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2953 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=10) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 13:22:08   148  ERR_DEBUG  LOG_ONLY  <UTC:1326633728_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2953 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=10) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 13:22:08   148  ERR_DEBUG  LOG_ONLY  <UTC:1326633728_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2953 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=10) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 13:22:32   148  ERR_DEBUG  LOG_ONLY  <UTC:1326633752_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=9) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 13:22:33   148  ERR_DEBUG  LOG_ONLY  <UTC:1326633753_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=9) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 102
01/15/2012 13:23:26   148  ERR_DEBUG  LOG_ONLY  <UTC:1326633806_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=9) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 13:23:26   148  ERR_DEBUG  LOG_ONLY  <UTC:1326633806_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=9) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 13:24:30   148  ERR_DEBUG  LOG_ONLY  <UTC:1326633870_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=8) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 13:24:30   148  ERR_DEBUG  LOG_ONLY  <UTC:1326633870_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=8) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 13:25:27   148  ERR_DEBUG  LOG_ONLY  <UTC:1326633927_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=8) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 13:25:27   148  ERR_DEBUG  LOG_ONLY  <UTC:1326633927_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=8) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 13:26:01   148  ERR_DEBUG  LOG_ONLY  <UTC:1326633961_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=7) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 13:26:01   148  ERR_DEBUG  LOG_ONLY  <UTC:1326633961_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=7) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 13:27:09   148  ERR_DEBUG  LOG_ONLY  <UTC:1326634029_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=7) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 13:27:09   148  ERR_DEBUG  LOG_ONLY  <UTC:1326634029_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=7) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 13:27:38   148  ERR_DEBUG  LOG_ONLY  <UTC:1326634058_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=6) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 13:27:38   148  ERR_DEBUG  LOG_ONLY  <UTC:1326634058_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=6) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 13:27:47   148  ERR_DEBUG  LOG_ONLY  <UTC:1326634067_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=6) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 13:27:49   148  ERR_DEBUG  LOG_ONLY  <UTC:1326634069_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=6) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 146
01/15/2012 13:28:03   148  ERR_DEBUG  LOG_ONLY  <UTC:1326634083_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=6) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 13:28:03   148  ERR_DEBUG  LOG_ONLY  <UTC:1326634083_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=6) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 13:28:36   148  ERR_DEBUG  LOG_ONLY  <UTC:1326634116_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=6) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 13:28:36   148  ERR_DEBUG  LOG_ONLY  <UTC:1326634116_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=6) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 13:29:15   148  ERR_DEBUG  LOG_ONLY  <UTC:1326634155_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=6) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 13:29:15   148  ERR_DEBUG  LOG_ONLY  <UTC:1326634155_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=6) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 13:29:31   148  ERR_DEBUG  LOG_ONLY  <UTC:1326634171_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=5) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 13:29:31   148  ERR_DEBUG  LOG_ONLY  <UTC:1326634171_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=5) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=20
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 10
01/15/2012 13:29:53   148  ERR_DEBUG  LOG_ONLY  <UTC:1326634193_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=5) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 13:29:53   148  ERR_DEBUG  LOG_ONLY  <UTC:1326634193_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=5) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 13:30:33   148  ERR_DEBUG  LOG_ONLY  <UTC:1326634233_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=5) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 13:30:33   148  ERR_DEBUG  LOG_ONLY  <UTC:1326634233_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=5) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 13:31:00   148  ERR_DEBUG  LOG_ONLY  <UTC:1326634260_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=5) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 13:31:00   148  ERR_DEBUG  LOG_ONLY  <UTC:1326634260_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=5) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 13:31:31   148  ERR_DEBUG  LOG_ONLY  <UTC:1326634291_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=5) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 13:31:31   148  ERR_DEBUG  LOG_ONLY  <UTC:1326634291_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=5) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 13:32:33   148  ERR_DEBUG  LOG_ONLY  <UTC:1326634353_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=4) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 13:32:33   148  ERR_DEBUG  LOG_ONLY  <UTC:1326634353_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=4) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=20
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 13:33:45   148  ERR_DEBUG  LOG_ONLY  <UTC:1326634425_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=4) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 13:33:45   148  ERR_DEBUG  LOG_ONLY  <UTC:1326634425_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=4) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 13:35:08   148  ERR_DEBUG  LOG_ONLY  <UTC:1326634508_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=3) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 13:35:08   148  ERR_DEBUG  LOG_ONLY  <UTC:1326634508_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=3) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 13:36:05   148  ERR_DEBUG  LOG_ONLY  <UTC:1326634565_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=2) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 13:36:05   148  ERR_DEBUG  LOG_ONLY  <UTC:1326634565_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=2) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 13:37:02   148  ERR_DEBUG  LOG_ONLY  <UTC:1326634622_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=2) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 13:37:02   148  ERR_DEBUG  LOG_ONLY  <UTC:1326634622_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=2) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 13:37:46   148  ERR_DEBUG  LOG_ONLY  <UTC:1326634666_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=2) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 13:37:46   148  ERR_DEBUG  LOG_ONLY  <UTC:1326634666_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=2) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 13:38:30   148  ERR_DEBUG  LOG_ONLY  <UTC:1326634710_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=1) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 13:38:30   148  ERR_DEBUG  LOG_ONLY  <UTC:1326634710_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=1) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 13
01/15/2012 13:39:14   148  ERR_DEBUG  LOG_ONLY  <UTC:1326634754_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=1) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 13:39:14   148  ERR_DEBUG  LOG_ONLY  <UTC:1326634754_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=1) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 13:39:57   148  ERR_DEBUG  LOG_ONLY  <UTC:1326634797_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=1) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 13:39:57   148  ERR_DEBUG  LOG_ONLY  <UTC:1326634797_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=1) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 10
01/15/2012 13:40:02   221  ERR_TDA_RSC_LOW_DET_LI_ION  LOG_ONLY  <UTC:1326634802_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=0) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=V0=16226 V1=13496 V2=0 FCC0=4312 FCC1=4172 SN0=27F8 SN1=103D2A Cyc0=3 Cyc1
01/15/2012 13:40:02   281  ERR_PWR_REDUCTION_DET_LI_ION_DEPLETED  INFO_ALARM  <UTC:1326634802_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=0) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=V0=16226 V1=13496 V2=0 FCC0=4312 FCC1=4172 RM0=4170 RM1=0 SN0=27F8 SN1=103
01/15/2012 13:40:30   148  ERR_DEBUG  LOG_ONLY  <UTC:1326634830_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=0) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 13:40:30   148  ERR_DEBUG  LOG_ONLY  <UTC:1326634830_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=0) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 13:41:52   148  ERR_DEBUG  LOG_ONLY  <UTC:1326634912_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=96 DetLi=0) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 13:41:52   148  ERR_DEBUG  LOG_ONLY  <UTC:1326634912_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=96 DetLi=0) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 13:42:39   148  ERR_DEBUG  LOG_ONLY  <UTC:1326634959_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=96 DetLi=0) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 13:42:40   148  ERR_DEBUG  LOG_ONLY  <UTC:1326634960_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=96 DetLi=0) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 73
01/15/2012 13:43:09   148  ERR_DEBUG  LOG_ONLY  <UTC:1326634989_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=96 DetLi=0) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 13:43:09   148  ERR_DEBUG  LOG_ONLY  <UTC:1326634989_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=96 DetLi=0) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 3
01/15/2012 13:43:14   249  ERR_AC_CONNECTED  LOG_ONLY  <UTC:1326634994_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=0) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=0(INT_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=
01/15/2012 13:43:51   148  ERR_DEBUG  LOG_ONLY  <UTC:1326635031_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=1) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 13:43:51   148  ERR_DEBUG  LOG_ONLY  <UTC:1326635031_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=1) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 13:44:16   148  ERR_DEBUG  LOG_ONLY  <UTC:1326635056_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=1) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 13:44:17   148  ERR_DEBUG  LOG_ONLY  <UTC:1326635057_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=1) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 80
01/15/2012 13:47:33   148  ERR_DEBUG  LOG_ONLY  <UTC:1326635253_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=4) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 13:47:33   148  ERR_DEBUG  LOG_ONLY  <UTC:1326635253_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=4) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 13:52:23   148  ERR_DEBUG  LOG_ONLY  <UTC:1326635543_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=8) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 13:52:23   148  ERR_DEBUG  LOG_ONLY  <UTC:1326635543_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=8) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=20
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 13:53:00   148  ERR_DEBUG  LOG_ONLY  <UTC:1326635580_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=8) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 13:53:00   148  ERR_DEBUG  LOG_ONLY  <UTC:1326635580_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=8) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 13:53:11   148  ERR_DEBUG  LOG_ONLY  <UTC:1326635591_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=8) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 13:53:11   148  ERR_DEBUG  LOG_ONLY  <UTC:1326635591_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=8) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 13:53:29   148  ERR_DEBUG  LOG_ONLY  <UTC:1326635609_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=8) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 13:53:29   148  ERR_DEBUG  LOG_ONLY  <UTC:1326635609_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=8) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 13:54:37   148  ERR_DEBUG  LOG_ONLY  <UTC:1326635677_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=9) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 13:54:37   148  ERR_DEBUG  LOG_ONLY  <UTC:1326635677_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=9) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 13:55:39   148  ERR_DEBUG  LOG_ONLY  <UTC:1326635739_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=10) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 13:55:39   148  ERR_DEBUG  LOG_ONLY  <UTC:1326635739_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=10) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 60
01/15/2012 13:55:56   148  ERR_DEBUG  LOG_ONLY  <UTC:1326635756_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=10) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 13:55:56   148  ERR_DEBUG  LOG_ONLY  <UTC:1326635756_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=10) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 13:57:30   221  ERR_TDA_RSC_LOW_DET_LI_ION  LOG_ONLY  <UTC:1326635850_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=12) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=V0=16159 V1=14421 V2=120 FCC0=4332 FCC1=4172 SN0=27F8 SN1=103D2A Cyc0=3 Cy
01/15/2012 13:57:44   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326635864_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=12) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=CQ:293   MP:361   PP:16  
01/15/2012 14:02:41   148  ERR_DEBUG  LOG_ONLY  <UTC:1326636161_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=16) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 14:02:41   148  ERR_DEBUG  LOG_ONLY  <UTC:1326636161_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=16) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1
01/15/2012 14:02:46   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326636166_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=16) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=CP:152  
01/15/2012 14:09:27   148  ERR_DEBUG  LOG_ONLY  <UTC:1326636567_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=21) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 14:09:27   148  ERR_DEBUG  LOG_ONLY  <UTC:1326636567_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=21) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 14:11:54   148  ERR_DEBUG  LOG_ONLY  <UTC:1326636714_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=23) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 14:11:54   148  ERR_DEBUG  LOG_ONLY  <UTC:1326636714_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=23) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 14:12:51   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326636771_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=24) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=CP:171  
01/15/2012 14:18:14   148  ERR_DEBUG  LOG_ONLY  <UTC:1326637094_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=28) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 14:18:14   148  ERR_DEBUG  LOG_ONLY  <UTC:1326637094_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=28) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 14:19:21   148  ERR_DEBUG  LOG_ONLY  <UTC:1326637161_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=29) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 14:19:21   148  ERR_DEBUG  LOG_ONLY  <UTC:1326637161_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=29) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 14
01/15/2012 14:19:56   148  ERR_DEBUG  LOG_ONLY  <UTC:1326637196_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=29) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 14:19:56   148  ERR_DEBUG  LOG_ONLY  <UTC:1326637196_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=29) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 14:20:08   148  ERR_DEBUG  LOG_ONLY  <UTC:1326637208_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=29) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 14:20:08   148  ERR_DEBUG  LOG_ONLY  <UTC:1326637208_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=29) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 14:20:55   148  ERR_DEBUG  LOG_ONLY  <UTC:1326637255_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=30) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 14:20:55   148  ERR_DEBUG  LOG_ONLY  <UTC:1326637255_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=30) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 14:22:56   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326637376_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=32) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=20
                         Reserved(Offset=52)=00
                         Opt.Text=CP:179  
01/15/2012 14:23:10   148  ERR_DEBUG  LOG_ONLY  <UTC:1326637390_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=32) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 14:23:10   148  ERR_DEBUG  LOG_ONLY  <UTC:1326637390_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=32) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 14:23:50   148  ERR_DEBUG  LOG_ONLY  <UTC:1326637430_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=32) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 14:23:50   148  ERR_DEBUG  LOG_ONLY  <UTC:1326637430_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=32) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 14:25:10   148  ERR_DEBUG  LOG_ONLY  <UTC:1326637510_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=33) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 14:25:10   148  ERR_DEBUG  LOG_ONLY  <UTC:1326637510_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=33) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 14:25:49   148  ERR_DEBUG  LOG_ONLY  <UTC:1326637549_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=34) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 14:25:49   148  ERR_DEBUG  LOG_ONLY  <UTC:1326637549_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=34) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 14:27:37   148  ERR_DEBUG  LOG_ONLY  <UTC:1326637657_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=35) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 14:27:37   148  ERR_DEBUG  LOG_ONLY  <UTC:1326637657_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=35) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 14:29:28   148  ERR_DEBUG  LOG_ONLY  <UTC:1326637768_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=37) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 14:29:28   148  ERR_DEBUG  LOG_ONLY  <UTC:1326637768_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=37) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 14:30:01   148  ERR_DEBUG  LOG_ONLY  <UTC:1326637801_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=37) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 14:30:01   148  ERR_DEBUG  LOG_ONLY  <UTC:1326637801_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=37) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 14:30:16   148  ERR_DEBUG  LOG_ONLY  <UTC:1326637816_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=37) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=74 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 14:30:16   148  ERR_DEBUG  LOG_ONLY  <UTC:1326637816_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=37) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=20
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 14:31:22   148  ERR_DEBUG  LOG_ONLY  <UTC:1326637882_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=38) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=74 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 14:31:22   148  ERR_DEBUG  LOG_ONLY  <UTC:1326637882_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=38) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=74 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 14:33:03   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326637983_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=39) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=CP:199  
01/15/2012 14:37:52   148  ERR_DEBUG  LOG_ONLY  <UTC:1326638272_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=43) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=74 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 14:37:52   148  ERR_DEBUG  LOG_ONLY  <UTC:1326638272_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=43) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=74 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 14:37:56   148  ERR_DEBUG  LOG_ONLY  <UTC:1326638276_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=43) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 14:37:56   148  ERR_DEBUG  LOG_ONLY  <UTC:1326638276_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=43) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=74 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 25
01/15/2012 14:41:10   148  ERR_DEBUG  LOG_ONLY  <UTC:1326638470_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=46) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=74 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 14:41:10   148  ERR_DEBUG  LOG_ONLY  <UTC:1326638470_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=46) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=75 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 4
01/15/2012 14:41:20   148  ERR_DEBUG  LOG_ONLY  <UTC:1326638480_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=46) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=74 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 14:41:20   148  ERR_DEBUG  LOG_ONLY  <UTC:1326638480_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=46) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=75 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 15
01/15/2012 14:43:11   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326638591_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=47) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=74 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=CP:200  
01/15/2012 14:44:16   341  ERR_FAN_CONTROL  LOG_ONLY  <UTC:1326638656_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=48) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=75 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Batt Fan:ON IntBattT:31C DetBattT:39C
01/15/2012 14:44:16   341  ERR_FAN_CONTROL  LOG_ONLY  <UTC:1326638656_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=48) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=75 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Case Fan: ON 10000 IntBattT:31C DetBattT:39C Air:35.0C Mtr:45.0C
01/15/2012 14:51:53   148  ERR_DEBUG  LOG_ONLY  <UTC:1326639113_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=54) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 14:51:53   148  ERR_DEBUG  LOG_ONLY  <UTC:1326639113_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=54) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 25
01/15/2012 14:51:53   148  ERR_DEBUG  LOG_ONLY  <UTC:1326639113_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=54) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 14:51:53   148  ERR_DEBUG  LOG_ONLY  <UTC:1326639113_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=54) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 7
01/15/2012 14:53:12   148  ERR_DEBUG  LOG_ONLY  <UTC:1326639192_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=55) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=74 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 14:53:12   148  ERR_DEBUG  LOG_ONLY  <UTC:1326639192_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=55) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 14:53:16   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326639196_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=55) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=CP:189  
01/15/2012 14:53:37   148  ERR_DEBUG  LOG_ONLY  <UTC:1326639217_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=55) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 14:53:37   148  ERR_DEBUG  LOG_ONLY  <UTC:1326639217_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=55) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 14:53:53   148  ERR_DEBUG  LOG_ONLY  <UTC:1326639233_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=56) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=74 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 14:53:53   148  ERR_DEBUG  LOG_ONLY  <UTC:1326639233_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=56) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=21
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 14:55:35   148  ERR_DEBUG  LOG_ONLY  <UTC:1326639335_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=57) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 14:55:35   148  ERR_DEBUG  LOG_ONLY  <UTC:1326639335_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=57) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 3
01/15/2012 14:55:51   148  ERR_DEBUG  LOG_ONLY  <UTC:1326639351_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=57) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 14:55:51   148  ERR_DEBUG  LOG_ONLY  <UTC:1326639351_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=57) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 14:57:23   148  ERR_DEBUG  LOG_ONLY  <UTC:1326639443_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=58) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 14:57:23   148  ERR_DEBUG  LOG_ONLY  <UTC:1326639443_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=58) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 14:58:14   148  ERR_DEBUG  LOG_ONLY  <UTC:1326639494_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=59) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 14:58:14   148  ERR_DEBUG  LOG_ONLY  <UTC:1326639494_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=59) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 14:58:47   148  ERR_DEBUG  LOG_ONLY  <UTC:1326639527_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=59) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 14:58:47   148  ERR_DEBUG  LOG_ONLY  <UTC:1326639527_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=59) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 14:59:39   148  ERR_DEBUG  LOG_ONLY  <UTC:1326639579_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=59) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 14:59:39   148  ERR_DEBUG  LOG_ONLY  <UTC:1326639579_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=59) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 15:00:20   148  ERR_DEBUG  LOG_ONLY  <UTC:1326639620_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=59) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=21
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 15:00:20   148  ERR_DEBUG  LOG_ONLY  <UTC:1326639620_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=59) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 15:01:03   148  ERR_DEBUG  LOG_ONLY  <UTC:1326639663_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=59) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 15:01:03   148  ERR_DEBUG  LOG_ONLY  <UTC:1326639663_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=59) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 15:01:48   148  ERR_DEBUG  LOG_ONLY  <UTC:1326639708_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=60) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 15:01:48   148  ERR_DEBUG  LOG_ONLY  <UTC:1326639708_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=60) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 4
01/15/2012 15:02:02   148  ERR_DEBUG  LOG_ONLY  <UTC:1326639722_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=60) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 15:02:02   148  ERR_DEBUG  LOG_ONLY  <UTC:1326639722_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=60) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 15:05:25   148  ERR_DEBUG  LOG_ONLY  <UTC:1326639925_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=61) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 15:05:25   148  ERR_DEBUG  LOG_ONLY  <UTC:1326639925_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=61) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 15:07:49   148  ERR_DEBUG  LOG_ONLY  <UTC:1326640069_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=62) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 15:07:49   148  ERR_DEBUG  LOG_ONLY  <UTC:1326640069_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=62) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 15:10:24   148  ERR_DEBUG  LOG_ONLY  <UTC:1326640224_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=63) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 15:10:24   148  ERR_DEBUG  LOG_ONLY  <UTC:1326640224_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=63) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 15:10:58   148  ERR_DEBUG  LOG_ONLY  <UTC:1326640258_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=63) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 15:10:58   148  ERR_DEBUG  LOG_ONLY  <UTC:1326640258_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=63) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 15:11:19   148  ERR_DEBUG  LOG_ONLY  <UTC:1326640279_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=63) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 15:11:19   148  ERR_DEBUG  LOG_ONLY  <UTC:1326640279_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=63) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 15:15:59   148  ERR_DEBUG  LOG_ONLY  <UTC:1326640559_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=65) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 15:15:59   148  ERR_DEBUG  LOG_ONLY  <UTC:1326640559_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=65) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 15:16:29   148  ERR_DEBUG  LOG_ONLY  <UTC:1326640589_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=66) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 15:16:29   148  ERR_DEBUG  LOG_ONLY  <UTC:1326640589_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=66) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 15:18:33   148  ERR_DEBUG  LOG_ONLY  <UTC:1326640713_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=67) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 15:18:33   148  ERR_DEBUG  LOG_ONLY  <UTC:1326640713_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=67) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 15:18:56   148  ERR_DEBUG  LOG_ONLY  <UTC:1326640736_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=68) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 15:18:56   148  ERR_DEBUG  LOG_ONLY  <UTC:1326640736_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=68) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 15:19:16   148  ERR_DEBUG  LOG_ONLY  <UTC:1326640756_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=68) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 15:19:16   148  ERR_DEBUG  LOG_ONLY  <UTC:1326640756_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=68) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 15:20:34   148  ERR_DEBUG  LOG_ONLY  <UTC:1326640834_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=69) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 15:20:34   148  ERR_DEBUG  LOG_ONLY  <UTC:1326640834_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=69) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 15:21:05   148  ERR_DEBUG  LOG_ONLY  <UTC:1326640865_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=69) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 15:21:05   148  ERR_DEBUG  LOG_ONLY  <UTC:1326640865_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=69) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 3
01/15/2012 15:21:18   148  ERR_DEBUG  LOG_ONLY  <UTC:1326640878_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=70) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 15:21:18   148  ERR_DEBUG  LOG_ONLY  <UTC:1326640878_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=70) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 62
01/15/2012 15:23:54   148  ERR_DEBUG  LOG_ONLY  <UTC:1326641034_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=72) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 15:23:54   148  ERR_DEBUG  LOG_ONLY  <UTC:1326641034_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=72) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 15:26:34   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326641194_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=74) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=CQ:275   MP:403   PP:42  
01/15/2012 15:31:26   148  ERR_DEBUG  LOG_ONLY  <UTC:1326641486_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=78) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 15:31:26   148  ERR_DEBUG  LOG_ONLY  <UTC:1326641486_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=78) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1
01/15/2012 15:31:30   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326641490_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=78) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=CP:167  
01/15/2012 15:31:47   148  ERR_DEBUG  LOG_ONLY  <UTC:1326641507_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=78) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=21
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 15:31:47   148  ERR_DEBUG  LOG_ONLY  <UTC:1326641507_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=78) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=21
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 15:32:03   148  ERR_DEBUG  LOG_ONLY  <UTC:1326641523_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=78) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 15:32:03   148  ERR_DEBUG  LOG_ONLY  <UTC:1326641523_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=78) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 12
01/15/2012 15:33:32   148  ERR_DEBUG  LOG_ONLY  <UTC:1326641612_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=79) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 15:33:32   148  ERR_DEBUG  LOG_ONLY  <UTC:1326641612_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=79) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 15:33:56   148  ERR_DEBUG  LOG_ONLY  <UTC:1326641636_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=79) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 15:33:57   148  ERR_DEBUG  LOG_ONLY  <UTC:1326641637_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=79) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 133
01/15/2012 15:34:29   148  ERR_DEBUG  LOG_ONLY  <UTC:1326641669_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=80) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 15:34:30   148  ERR_DEBUG  LOG_ONLY  <UTC:1326641670_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=80) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 118
01/15/2012 15:35:13   148  ERR_DEBUG  LOG_ONLY  <UTC:1326641713_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=81) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 15:35:14   148  ERR_DEBUG  LOG_ONLY  <UTC:1326641714_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=81) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 112
01/15/2012 15:36:38   148  ERR_DEBUG  LOG_ONLY  <UTC:1326641798_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=82) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 15:36:39   148  ERR_DEBUG  LOG_ONLY  <UTC:1326641799_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=82) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 92
01/15/2012 15:36:55   148  ERR_DEBUG  LOG_ONLY  <UTC:1326641815_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=82) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 15:36:55   148  ERR_DEBUG  LOG_ONLY  <UTC:1326641815_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=82) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=20
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 15:41:20   148  ERR_DEBUG  LOG_ONLY  <UTC:1326642080_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=85) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 15:41:20   148  ERR_DEBUG  LOG_ONLY  <UTC:1326642080_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=85) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 15:41:37   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326642097_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=85) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=CP:161  
01/15/2012 15:42:25   148  ERR_DEBUG  LOG_ONLY  <UTC:1326642145_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=85) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 15:42:25   148  ERR_DEBUG  LOG_ONLY  <UTC:1326642145_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=85) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 15:43:51   341  ERR_FAN_CONTROL  LOG_ONLY  <UTC:1326642231_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=86) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Batt Fan:OFF IntBattT:30C DetBattT:30C
01/15/2012 15:43:51   341  ERR_FAN_CONTROL  LOG_ONLY  <UTC:1326642231_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=86) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Case Fan: OFF 00000 IntBattT:30C DetBattT:30C Air:34.9C Mtr:45.0C
01/15/2012 15:44:45   148  ERR_DEBUG  LOG_ONLY  <UTC:1326642285_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=87) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 15:44:45   148  ERR_DEBUG  LOG_ONLY  <UTC:1326642285_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=87) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 15:49:17   148  ERR_DEBUG  LOG_ONLY  <UTC:1326642557_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=89) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 15:49:17   148  ERR_DEBUG  LOG_ONLY  <UTC:1326642557_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=89) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 15:49:52   148  ERR_DEBUG  LOG_ONLY  <UTC:1326642592_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=89) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 15:49:52   148  ERR_DEBUG  LOG_ONLY  <UTC:1326642592_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=89) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 15:51:16   148  ERR_DEBUG  LOG_ONLY  <UTC:1326642676_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=91) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 15:51:16   148  ERR_DEBUG  LOG_ONLY  <UTC:1326642676_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=91) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 15:51:42   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326642702_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=91) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=CP:152  
01/15/2012 15:51:56   148  ERR_DEBUG  LOG_ONLY  <UTC:1326642716_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=91) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 15:51:56   148  ERR_DEBUG  LOG_ONLY  <UTC:1326642716_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=91) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 15:53:47   148  ERR_DEBUG  LOG_ONLY  <UTC:1326642827_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=92) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 15:53:47   148  ERR_DEBUG  LOG_ONLY  <UTC:1326642827_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=92) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 15:56:33   148  ERR_DEBUG  LOG_ONLY  <UTC:1326642993_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=94) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 15:56:33   148  ERR_DEBUG  LOG_ONLY  <UTC:1326642993_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=94) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 15:58:08   148  ERR_DEBUG  LOG_ONLY  <UTC:1326643088_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=95) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 15:58:08   148  ERR_DEBUG  LOG_ONLY  <UTC:1326643088_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=95) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 15:58:57   148  ERR_DEBUG  LOG_ONLY  <UTC:1326643137_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=95) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 15:58:57   148  ERR_DEBUG  LOG_ONLY  <UTC:1326643137_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=95) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 16:00:06   148  ERR_DEBUG  LOG_ONLY  <UTC:1326643206_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=96) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 16:00:06   148  ERR_DEBUG  LOG_ONLY  <UTC:1326643206_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=96) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 16:00:56   148  ERR_DEBUG  LOG_ONLY  <UTC:1326643256_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=96) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 16:00:56   148  ERR_DEBUG  LOG_ONLY  <UTC:1326643256_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=96) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 16:01:48   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326643308_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=96) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=CP:190  
01/15/2012 16:02:53   148  ERR_DEBUG  LOG_ONLY  <UTC:1326643373_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=97) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 16:02:53   148  ERR_DEBUG  LOG_ONLY  <UTC:1326643373_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=97) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 16:05:37   148  ERR_DEBUG  LOG_ONLY  <UTC:1326643537_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=97) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 16:05:37   148  ERR_DEBUG  LOG_ONLY  <UTC:1326643537_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=97) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 16:07:28   148  ERR_DEBUG  LOG_ONLY  <UTC:1326643648_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 16:07:28   148  ERR_DEBUG  LOG_ONLY  <UTC:1326643648_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 16:10:22   148  ERR_DEBUG  LOG_ONLY  <UTC:1326643822_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 16:10:23   148  ERR_DEBUG  LOG_ONLY  <UTC:1326643823_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 16:11:36   148  ERR_DEBUG  LOG_ONLY  <UTC:1326643896_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 16:11:36   148  ERR_DEBUG  LOG_ONLY  <UTC:1326643896_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 16:11:52   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326643912_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=CP:185  
01/15/2012 16:16:01   148  ERR_DEBUG  LOG_ONLY  <UTC:1326644161_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 16:16:01   148  ERR_DEBUG  LOG_ONLY  <UTC:1326644161_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 16:16:38   148  ERR_DEBUG  LOG_ONLY  <UTC:1326644198_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 16:16:38   148  ERR_DEBUG  LOG_ONLY  <UTC:1326644198_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 3
01/15/2012 16:16:56   148  ERR_DEBUG  LOG_ONLY  <UTC:1326644216_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 16:16:56   148  ERR_DEBUG  LOG_ONLY  <UTC:1326644216_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 16:22:00   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326644520_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 bc 02 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=700,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=CP:192  
01/15/2012 16:29:39   148  ERR_DEBUG  LOG_ONLY  <UTC:1326644979_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= d0 07 bc 02 28 0a 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=2000,EPAP=700,IPAPMax=2600,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 16:29:39   148  ERR_DEBUG  LOG_ONLY  <UTC:1326644979_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= d0 07 bc 02 28 0a 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=2000,EPAP=700,IPAPMax=2600,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=21
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 16:29:58   148  ERR_DEBUG  LOG_ONLY  <UTC:1326644998_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= d0 07 bc 02 28 0a 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=2000,EPAP=700,IPAPMax=2600,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 16:29:58   148  ERR_DEBUG  LOG_ONLY  <UTC:1326644998_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= d0 07 bc 02 28 0a 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=2000,EPAP=700,IPAPMax=2600,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 16:30:53   148  ERR_DEBUG  LOG_ONLY  <UTC:1326645053_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= d0 07 bc 02 28 0a 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=2000,EPAP=700,IPAPMax=2600,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 16:30:53   148  ERR_DEBUG  LOG_ONLY  <UTC:1326645053_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= d0 07 bc 02 28 0a 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=2000,EPAP=700,IPAPMax=2600,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 16:34:45   148  ERR_DEBUG  LOG_ONLY  <UTC:1326645285_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=74 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 16:34:45   148  ERR_DEBUG  LOG_ONLY  <UTC:1326645285_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=74 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 16:35:05   148  ERR_DEBUG  LOG_ONLY  <UTC:1326645305_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=74 Meas.BreathRate=20
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 16:35:05   148  ERR_DEBUG  LOG_ONLY  <UTC:1326645305_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=23
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 16:38:49   148  ERR_DEBUG  LOG_ONLY  <UTC:1326645529_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=74 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 16:38:49   148  ERR_DEBUG  LOG_ONLY  <UTC:1326645529_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 16:40:02   148  ERR_DEBUG  LOG_ONLY  <UTC:1326645602_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 16:40:02   148  ERR_DEBUG  LOG_ONLY  <UTC:1326645602_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 16:40:51   148  ERR_DEBUG  LOG_ONLY  <UTC:1326645651_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 16:40:51   148  ERR_DEBUG  LOG_ONLY  <UTC:1326645651_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 16:41:16   148  ERR_DEBUG  LOG_ONLY  <UTC:1326645676_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 16:41:16   148  ERR_DEBUG  LOG_ONLY  <UTC:1326645676_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 7
01/15/2012 16:41:40   148  ERR_DEBUG  LOG_ONLY  <UTC:1326645700_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=21
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 16:41:40   148  ERR_DEBUG  LOG_ONLY  <UTC:1326645700_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=20
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 16:42:26   148  ERR_DEBUG  LOG_ONLY  <UTC:1326645746_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 16:42:26   148  ERR_DEBUG  LOG_ONLY  <UTC:1326645746_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 13
01/15/2012 16:43:03   148  ERR_DEBUG  LOG_ONLY  <UTC:1326645783_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 16:43:04   148  ERR_DEBUG  LOG_ONLY  <UTC:1326645784_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 76
01/15/2012 16:43:41   148  ERR_DEBUG  LOG_ONLY  <UTC:1326645821_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 16:43:41   148  ERR_DEBUG  LOG_ONLY  <UTC:1326645821_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 8
01/15/2012 16:43:58   148  ERR_DEBUG  LOG_ONLY  <UTC:1326645838_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 16:43:59   148  ERR_DEBUG  LOG_ONLY  <UTC:1326645839_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 114
01/15/2012 16:44:46   148  ERR_DEBUG  LOG_ONLY  <UTC:1326645886_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 16:44:46   148  ERR_DEBUG  LOG_ONLY  <UTC:1326645886_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 27
01/15/2012 16:45:11   148  ERR_DEBUG  LOG_ONLY  <UTC:1326645911_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 16:45:11   148  ERR_DEBUG  LOG_ONLY  <UTC:1326645911_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 7
01/15/2012 16:45:34   148  ERR_DEBUG  LOG_ONLY  <UTC:1326645934_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 16:45:35   148  ERR_DEBUG  LOG_ONLY  <UTC:1326645935_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 76
01/15/2012 16:46:01   148  ERR_DEBUG  LOG_ONLY  <UTC:1326645961_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 16:46:01   148  ERR_DEBUG  LOG_ONLY  <UTC:1326645961_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 16:47:19   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326646039_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=CQ:275   MP:446   PP:74  
01/15/2012 16:51:50   341  ERR_FAN_CONTROL  LOG_ONLY  <UTC:1326646310_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Case Fan: ON 00010 IntBattT:31C DetBattT:35C Air:43.0C Mtr:42.0C
01/15/2012 16:52:28   148  ERR_DEBUG  LOG_ONLY  <UTC:1326646348_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 16:52:28   148  ERR_DEBUG  LOG_ONLY  <UTC:1326646348_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1
01/15/2012 16:52:32   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326646352_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=CP:186  
01/15/2012 16:52:44   148  ERR_DEBUG  LOG_ONLY  <UTC:1326646364_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 16:52:44   148  ERR_DEBUG  LOG_ONLY  <UTC:1326646364_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 16:53:28   148  ERR_DEBUG  LOG_ONLY  <UTC:1326646408_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 16:53:28   148  ERR_DEBUG  LOG_ONLY  <UTC:1326646408_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 16:54:26   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326646466_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=CQ:288   MP:451   PP:84  
01/15/2012 16:55:25   148  ERR_DEBUG  LOG_ONLY  <UTC:1326646525_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 16:55:25   148  ERR_DEBUG  LOG_ONLY  <UTC:1326646525_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1
01/15/2012 16:55:30   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326646530_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=CP:198  
01/15/2012 16:56:16   341  ERR_FAN_CONTROL  LOG_ONLY  <UTC:1326646576_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Case Fan: OFF 00000 IntBattT:31C DetBattT:35C Air:34.9C Mtr:42.0C
01/15/2012 17:01:58   148  ERR_DEBUG  LOG_ONLY  <UTC:1326646918_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 17:01:59   148  ERR_DEBUG  LOG_ONLY  <UTC:1326646919_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 17:05:35   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326647135_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=CP:181  
01/15/2012 17:14:14   148  ERR_DEBUG  LOG_ONLY  <UTC:1326647654_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 17:14:14   148  ERR_DEBUG  LOG_ONLY  <UTC:1326647654_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 17:15:38   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326647738_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=CP:174  
01/15/2012 17:18:43   148  ERR_DEBUG  LOG_ONLY  <UTC:1326647923_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 17:18:43   148  ERR_DEBUG  LOG_ONLY  <UTC:1326647923_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 17:18:53   148  ERR_DEBUG  LOG_ONLY  <UTC:1326647933_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 17:18:54   148  ERR_DEBUG  LOG_ONLY  <UTC:1326647934_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 82
01/15/2012 17:20:24   148  ERR_DEBUG  LOG_ONLY  <UTC:1326648024_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 17:20:24   148  ERR_DEBUG  LOG_ONLY  <UTC:1326648024_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 17:21:57   148  ERR_DEBUG  LOG_ONLY  <UTC:1326648117_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 17:21:57   148  ERR_DEBUG  LOG_ONLY  <UTC:1326648117_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 17:22:46   148  ERR_DEBUG  LOG_ONLY  <UTC:1326648166_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 17:22:46   148  ERR_DEBUG  LOG_ONLY  <UTC:1326648166_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 17:22:59   148  ERR_DEBUG  LOG_ONLY  <UTC:1326648179_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 17:22:59   148  ERR_DEBUG  LOG_ONLY  <UTC:1326648179_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 17:23:11   148  ERR_DEBUG  LOG_ONLY  <UTC:1326648191_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 17:23:11   148  ERR_DEBUG  LOG_ONLY  <UTC:1326648191_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 17:24:15   148  ERR_DEBUG  LOG_ONLY  <UTC:1326648255_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 17:24:16   148  ERR_DEBUG  LOG_ONLY  <UTC:1326648256_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 18
01/15/2012 17:24:44   148  ERR_DEBUG  LOG_ONLY  <UTC:1326648284_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 17:24:45   148  ERR_DEBUG  LOG_ONLY  <UTC:1326648285_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 69
01/15/2012 17:24:58   148  ERR_DEBUG  LOG_ONLY  <UTC:1326648298_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 17:24:58   148  ERR_DEBUG  LOG_ONLY  <UTC:1326648298_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 17:25:12   148  ERR_DEBUG  LOG_ONLY  <UTC:1326648312_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 17:25:12   148  ERR_DEBUG  LOG_ONLY  <UTC:1326648312_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 17:25:30   148  ERR_DEBUG  LOG_ONLY  <UTC:1326648330_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 17:25:31   148  ERR_DEBUG  LOG_ONLY  <UTC:1326648331_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 86
01/15/2012 17:25:43   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326648343_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=CP:172  
01/15/2012 17:25:58   148  ERR_DEBUG  LOG_ONLY  <UTC:1326648358_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 17:25:59   148  ERR_DEBUG  LOG_ONLY  <UTC:1326648359_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 95
01/15/2012 17:26:26   148  ERR_DEBUG  LOG_ONLY  <UTC:1326648386_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 17:26:27   148  ERR_DEBUG  LOG_ONLY  <UTC:1326648387_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 87
01/15/2012 17:27:12   148  ERR_DEBUG  LOG_ONLY  <UTC:1326648432_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 17:27:12   148  ERR_DEBUG  LOG_ONLY  <UTC:1326648432_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 17:27:27   148  ERR_DEBUG  LOG_ONLY  <UTC:1326648447_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 17:27:27   148  ERR_DEBUG  LOG_ONLY  <UTC:1326648447_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 12
01/15/2012 17:27:45   148  ERR_DEBUG  LOG_ONLY  <UTC:1326648465_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 17:27:45   148  ERR_DEBUG  LOG_ONLY  <UTC:1326648465_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 3
01/15/2012 17:28:05   148  ERR_DEBUG  LOG_ONLY  <UTC:1326648485_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 17:28:06   148  ERR_DEBUG  LOG_ONLY  <UTC:1326648486_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 77
01/15/2012 17:28:58   148  ERR_DEBUG  LOG_ONLY  <UTC:1326648538_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 17:28:58   148  ERR_DEBUG  LOG_ONLY  <UTC:1326648538_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 17:29:29   148  ERR_DEBUG  LOG_ONLY  <UTC:1326648569_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 17:29:29   148  ERR_DEBUG  LOG_ONLY  <UTC:1326648569_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 59
01/15/2012 17:29:39   148  ERR_DEBUG  LOG_ONLY  <UTC:1326648579_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 17:29:39   148  ERR_DEBUG  LOG_ONLY  <UTC:1326648579_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 15
01/15/2012 17:30:54   148  ERR_DEBUG  LOG_ONLY  <UTC:1326648654_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 17:30:54   148  ERR_DEBUG  LOG_ONLY  <UTC:1326648654_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 12
01/15/2012 17:31:15   148  ERR_DEBUG  LOG_ONLY  <UTC:1326648675_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 17:31:16   148  ERR_DEBUG  LOG_ONLY  <UTC:1326648676_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 135
01/15/2012 17:31:59   148  ERR_DEBUG  LOG_ONLY  <UTC:1326648719_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 17:32:00   148  ERR_DEBUG  LOG_ONLY  <UTC:1326648720_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 94
01/15/2012 17:33:37   148  ERR_DEBUG  LOG_ONLY  <UTC:1326648817_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 17:33:38   148  ERR_DEBUG  LOG_ONLY  <UTC:1326648818_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 148
01/15/2012 17:35:44   148  ERR_DEBUG  LOG_ONLY  <UTC:1326648944_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 17:35:44   148  ERR_DEBUG  LOG_ONLY  <UTC:1326648944_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 17:35:48   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326648948_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=CP:172  
01/15/2012 17:36:10   148  ERR_DEBUG  LOG_ONLY  <UTC:1326648970_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 17:36:10   148  ERR_DEBUG  LOG_ONLY  <UTC:1326648970_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 17:36:19   148  ERR_DEBUG  LOG_ONLY  <UTC:1326648979_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 17:36:19   148  ERR_DEBUG  LOG_ONLY  <UTC:1326648979_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 17:36:57   148  ERR_DEBUG  LOG_ONLY  <UTC:1326649017_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 17:36:58   148  ERR_DEBUG  LOG_ONLY  <UTC:1326649018_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 98
01/15/2012 17:37:23   148  ERR_DEBUG  LOG_ONLY  <UTC:1326649043_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 17:37:24   148  ERR_DEBUG  LOG_ONLY  <UTC:1326649044_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 99
01/15/2012 17:37:48   148  ERR_DEBUG  LOG_ONLY  <UTC:1326649068_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 17:37:48   148  ERR_DEBUG  LOG_ONLY  <UTC:1326649068_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 17:38:45   148  ERR_DEBUG  LOG_ONLY  <UTC:1326649125_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 17:38:45   148  ERR_DEBUG  LOG_ONLY  <UTC:1326649125_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 17:39:00   148  ERR_DEBUG  LOG_ONLY  <UTC:1326649140_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 17:39:00   148  ERR_DEBUG  LOG_ONLY  <UTC:1326649140_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 17:42:00   148  ERR_DEBUG  LOG_ONLY  <UTC:1326649320_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 17:42:00   148  ERR_DEBUG  LOG_ONLY  <UTC:1326649320_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 17:42:29   148  ERR_DEBUG  LOG_ONLY  <UTC:1326649349_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 17:42:29   148  ERR_DEBUG  LOG_ONLY  <UTC:1326649349_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 17:42:48   148  ERR_DEBUG  LOG_ONLY  <UTC:1326649368_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 17:42:48   148  ERR_DEBUG  LOG_ONLY  <UTC:1326649368_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 17:43:11   148  ERR_DEBUG  LOG_ONLY  <UTC:1326649391_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 17:43:11   148  ERR_DEBUG  LOG_ONLY  <UTC:1326649391_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 17:43:47   148  ERR_DEBUG  LOG_ONLY  <UTC:1326649427_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 17:43:47   148  ERR_DEBUG  LOG_ONLY  <UTC:1326649427_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 17:44:20   148  ERR_DEBUG  LOG_ONLY  <UTC:1326649460_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 17:44:21   148  ERR_DEBUG  LOG_ONLY  <UTC:1326649461_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 82
01/15/2012 17:45:05   148  ERR_DEBUG  LOG_ONLY  <UTC:1326649505_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 17:45:05   148  ERR_DEBUG  LOG_ONLY  <UTC:1326649505_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 8
01/15/2012 17:45:23   148  ERR_DEBUG  LOG_ONLY  <UTC:1326649523_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 17:45:23   148  ERR_DEBUG  LOG_ONLY  <UTC:1326649523_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 17:45:54   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326649554_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=CP:171  
01/15/2012 17:46:24   148  ERR_DEBUG  LOG_ONLY  <UTC:1326649584_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 17:46:24   148  ERR_DEBUG  LOG_ONLY  <UTC:1326649584_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 17:46:53   148  ERR_DEBUG  LOG_ONLY  <UTC:1326649613_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 17:46:54   148  ERR_DEBUG  LOG_ONLY  <UTC:1326649614_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 14
01/15/2012 17:47:27   148  ERR_DEBUG  LOG_ONLY  <UTC:1326649647_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 17:47:27   148  ERR_DEBUG  LOG_ONLY  <UTC:1326649647_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 8
01/15/2012 17:47:58   148  ERR_DEBUG  LOG_ONLY  <UTC:1326649678_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 17:47:59   148  ERR_DEBUG  LOG_ONLY  <UTC:1326649679_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 42
01/15/2012 17:48:16   148  ERR_DEBUG  LOG_ONLY  <UTC:1326649696_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 17:48:16   148  ERR_DEBUG  LOG_ONLY  <UTC:1326649696_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 8
01/15/2012 17:48:45   148  ERR_DEBUG  LOG_ONLY  <UTC:1326649725_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 17:48:45   148  ERR_DEBUG  LOG_ONLY  <UTC:1326649725_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 17:49:18   148  ERR_DEBUG  LOG_ONLY  <UTC:1326649758_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 17:49:18   148  ERR_DEBUG  LOG_ONLY  <UTC:1326649758_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 17:50:29   148  ERR_DEBUG  LOG_ONLY  <UTC:1326649829_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2949 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 17:50:29   148  ERR_DEBUG  LOG_ONLY  <UTC:1326649829_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2949 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 59
01/15/2012 17:50:39   148  ERR_DEBUG  LOG_ONLY  <UTC:1326649839_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 17:50:40   148  ERR_DEBUG  LOG_ONLY  <UTC:1326649840_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2949 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 54
01/15/2012 17:51:03   148  ERR_DEBUG  LOG_ONLY  <UTC:1326649863_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2949 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 17:51:03   148  ERR_DEBUG  LOG_ONLY  <UTC:1326649863_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 17:51:18   148  ERR_DEBUG  LOG_ONLY  <UTC:1326649878_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 17:51:18   148  ERR_DEBUG  LOG_ONLY  <UTC:1326649878_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2949 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 17:52:06   148  ERR_DEBUG  LOG_ONLY  <UTC:1326649926_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2949 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 17:52:06   148  ERR_DEBUG  LOG_ONLY  <UTC:1326649926_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2949 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 4
01/15/2012 17:52:19   148  ERR_DEBUG  LOG_ONLY  <UTC:1326649939_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2949 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 17:52:19   148  ERR_DEBUG  LOG_ONLY  <UTC:1326649939_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2949 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 72
01/15/2012 17:53:06   148  ERR_DEBUG  LOG_ONLY  <UTC:1326649986_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 17:53:06   148  ERR_DEBUG  LOG_ONLY  <UTC:1326649986_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 10
01/15/2012 17:55:38   148  ERR_DEBUG  LOG_ONLY  <UTC:1326650138_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 17:55:38   148  ERR_DEBUG  LOG_ONLY  <UTC:1326650138_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2949 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 17:55:47   148  ERR_DEBUG  LOG_ONLY  <UTC:1326650147_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 17:55:47   148  ERR_DEBUG  LOG_ONLY  <UTC:1326650147_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 17:56:48   148  ERR_DEBUG  LOG_ONLY  <UTC:1326650208_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 17:56:48   148  ERR_DEBUG  LOG_ONLY  <UTC:1326650208_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 17:57:36   148  ERR_DEBUG  LOG_ONLY  <UTC:1326650256_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 17:57:37   148  ERR_DEBUG  LOG_ONLY  <UTC:1326650257_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 31
01/15/2012 17:58:19   148  ERR_DEBUG  LOG_ONLY  <UTC:1326650299_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 17:58:20   148  ERR_DEBUG  LOG_ONLY  <UTC:1326650300_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 17:58:32   148  ERR_DEBUG  LOG_ONLY  <UTC:1326650312_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 17:58:32   148  ERR_DEBUG  LOG_ONLY  <UTC:1326650312_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 15
01/15/2012 17:58:49   148  ERR_DEBUG  LOG_ONLY  <UTC:1326650329_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 17:58:49   148  ERR_DEBUG  LOG_ONLY  <UTC:1326650329_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 17:59:08   148  ERR_DEBUG  LOG_ONLY  <UTC:1326650348_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 17:59:08   148  ERR_DEBUG  LOG_ONLY  <UTC:1326650348_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 17:59:53   148  ERR_DEBUG  LOG_ONLY  <UTC:1326650393_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2949 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 17:59:54   148  ERR_DEBUG  LOG_ONLY  <UTC:1326650394_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2949 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 11
01/15/2012 18:00:22   148  ERR_DEBUG  LOG_ONLY  <UTC:1326650422_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 18:00:23   148  ERR_DEBUG  LOG_ONLY  <UTC:1326650423_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 18:01:34   148  ERR_DEBUG  LOG_ONLY  <UTC:1326650494_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2949 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 18:01:34   148  ERR_DEBUG  LOG_ONLY  <UTC:1326650494_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2949 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 18:07:26   148  ERR_DEBUG  LOG_ONLY  <UTC:1326650846_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 18:07:26   148  ERR_DEBUG  LOG_ONLY  <UTC:1326650846_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 18:08:33   148  ERR_DEBUG  LOG_ONLY  <UTC:1326650913_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 18:08:33   148  ERR_DEBUG  LOG_ONLY  <UTC:1326650913_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 18:09:07   148  ERR_DEBUG  LOG_ONLY  <UTC:1326650947_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 18:09:07   148  ERR_DEBUG  LOG_ONLY  <UTC:1326650947_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 48
01/15/2012 18:12:13   148  ERR_DEBUG  LOG_ONLY  <UTC:1326651133_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 18:12:13   148  ERR_DEBUG  LOG_ONLY  <UTC:1326651133_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=21
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 18:12:26   148  ERR_DEBUG  LOG_ONLY  <UTC:1326651146_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 18:12:26   148  ERR_DEBUG  LOG_ONLY  <UTC:1326651146_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 18:14:05   148  ERR_DEBUG  LOG_ONLY  <UTC:1326651245_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 18:14:05   148  ERR_DEBUG  LOG_ONLY  <UTC:1326651245_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 18:16:14   148  ERR_DEBUG  LOG_ONLY  <UTC:1326651374_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 18:16:14   148  ERR_DEBUG  LOG_ONLY  <UTC:1326651374_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 18:16:25   148  ERR_DEBUG  LOG_ONLY  <UTC:1326651385_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 18:16:25   148  ERR_DEBUG  LOG_ONLY  <UTC:1326651385_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 18:17:30   148  ERR_DEBUG  LOG_ONLY  <UTC:1326651450_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 18:17:30   148  ERR_DEBUG  LOG_ONLY  <UTC:1326651450_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 18:17:44   148  ERR_DEBUG  LOG_ONLY  <UTC:1326651464_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 18:17:44   148  ERR_DEBUG  LOG_ONLY  <UTC:1326651464_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 34
01/15/2012 18:18:50   148  ERR_DEBUG  LOG_ONLY  <UTC:1326651530_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 18:18:51   148  ERR_DEBUG  LOG_ONLY  <UTC:1326651531_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 94
01/15/2012 18:22:01   148  ERR_DEBUG  LOG_ONLY  <UTC:1326651721_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 18:22:01   148  ERR_DEBUG  LOG_ONLY  <UTC:1326651721_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 18:23:35   148  ERR_DEBUG  LOG_ONLY  <UTC:1326651815_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 18:23:35   148  ERR_DEBUG  LOG_ONLY  <UTC:1326651815_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 18:23:44   148  ERR_DEBUG  LOG_ONLY  <UTC:1326651824_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 18:23:44   148  ERR_DEBUG  LOG_ONLY  <UTC:1326651824_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 18:24:43   148  ERR_DEBUG  LOG_ONLY  <UTC:1326651883_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 18:24:43   148  ERR_DEBUG  LOG_ONLY  <UTC:1326651883_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 3
01/15/2012 18:25:04   148  ERR_DEBUG  LOG_ONLY  <UTC:1326651904_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 18:25:04   148  ERR_DEBUG  LOG_ONLY  <UTC:1326651904_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 18:25:58   148  ERR_DEBUG  LOG_ONLY  <UTC:1326651958_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 18:25:58   148  ERR_DEBUG  LOG_ONLY  <UTC:1326651958_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 18:26:20   148  ERR_DEBUG  LOG_ONLY  <UTC:1326651980_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 18:26:20   148  ERR_DEBUG  LOG_ONLY  <UTC:1326651980_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 18:26:44   148  ERR_DEBUG  LOG_ONLY  <UTC:1326652004_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 18:26:44   148  ERR_DEBUG  LOG_ONLY  <UTC:1326652004_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 18:26:54   148  ERR_DEBUG  LOG_ONLY  <UTC:1326652014_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 18:26:54   148  ERR_DEBUG  LOG_ONLY  <UTC:1326652014_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 18:27:08   148  ERR_DEBUG  LOG_ONLY  <UTC:1326652028_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 18:27:08   148  ERR_DEBUG  LOG_ONLY  <UTC:1326652028_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 18:29:13   148  ERR_DEBUG  LOG_ONLY  <UTC:1326652153_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 18:29:13   148  ERR_DEBUG  LOG_ONLY  <UTC:1326652153_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 18:31:03   148  ERR_DEBUG  LOG_ONLY  <UTC:1326652263_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 18:31:03   148  ERR_DEBUG  LOG_ONLY  <UTC:1326652263_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 18:32:44   148  ERR_DEBUG  LOG_ONLY  <UTC:1326652364_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 18:32:45   148  ERR_DEBUG  LOG_ONLY  <UTC:1326652365_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 113
01/15/2012 18:35:02   148  ERR_DEBUG  LOG_ONLY  <UTC:1326652502_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 18:35:02   148  ERR_DEBUG  LOG_ONLY  <UTC:1326652502_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 18:35:20   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326652520_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=CQ:284   MP:396   PP:42  
01/15/2012 18:43:01   148  ERR_DEBUG  LOG_ONLY  <UTC:1326652981_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 18:43:01   148  ERR_DEBUG  LOG_ONLY  <UTC:1326652981_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1
01/15/2012 18:43:05   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326652985_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=CP:159  
01/15/2012 18:53:12   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326653592_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=CP:155  
01/15/2012 18:56:37   148  ERR_DEBUG  LOG_ONLY  <UTC:1326653797_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 18:56:37   148  ERR_DEBUG  LOG_ONLY  <UTC:1326653797_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 18:57:03   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326653823_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=CQ:282   MP:384   PP:28  
01/15/2012 19:13:54   148  ERR_DEBUG  LOG_ONLY  <UTC:1326654834_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 19:13:54   148  ERR_DEBUG  LOG_ONLY  <UTC:1326654834_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1
01/15/2012 19:13:59   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326654839_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=CP:111  
01/15/2012 19:15:25   148  ERR_DEBUG  LOG_ONLY  <UTC:1326654925_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 19:15:25   148  ERR_DEBUG  LOG_ONLY  <UTC:1326654925_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 19:16:06   148  ERR_DEBUG  LOG_ONLY  <UTC:1326654966_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 19:16:06   148  ERR_DEBUG  LOG_ONLY  <UTC:1326654966_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 19:23:02   148  ERR_DEBUG  LOG_ONLY  <UTC:1326655382_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 19:23:02   148  ERR_DEBUG  LOG_ONLY  <UTC:1326655382_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 19:24:04   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326655444_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=CP:105  
01/15/2012 19:25:04   148  ERR_DEBUG  LOG_ONLY  <UTC:1326655504_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 19:25:04   148  ERR_DEBUG  LOG_ONLY  <UTC:1326655504_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 19:29:41   148  ERR_DEBUG  LOG_ONLY  <UTC:1326655781_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 19:29:41   148  ERR_DEBUG  LOG_ONLY  <UTC:1326655781_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 19:32:57   148  ERR_DEBUG  LOG_ONLY  <UTC:1326655977_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 19:32:57   148  ERR_DEBUG  LOG_ONLY  <UTC:1326655977_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 19:34:08   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326656048_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=CP:98  
01/15/2012 19:35:21   148  ERR_DEBUG  LOG_ONLY  <UTC:1326656121_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 19:35:21   148  ERR_DEBUG  LOG_ONLY  <UTC:1326656121_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 9
01/15/2012 19:37:04   148  ERR_DEBUG  LOG_ONLY  <UTC:1326656224_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 19:37:04   148  ERR_DEBUG  LOG_ONLY  <UTC:1326656224_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 19:37:21   148  ERR_DEBUG  LOG_ONLY  <UTC:1326656241_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 19:37:21   148  ERR_DEBUG  LOG_ONLY  <UTC:1326656241_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 19:39:36   148  ERR_DEBUG  LOG_ONLY  <UTC:1326656376_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 19:39:36   148  ERR_DEBUG  LOG_ONLY  <UTC:1326656376_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 19:40:57   148  ERR_DEBUG  LOG_ONLY  <UTC:1326656457_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 19:40:57   148  ERR_DEBUG  LOG_ONLY  <UTC:1326656457_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 19:43:24   148  ERR_DEBUG  LOG_ONLY  <UTC:1326656604_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 19:43:24   148  ERR_DEBUG  LOG_ONLY  <UTC:1326656604_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 19:43:45   148  ERR_DEBUG  LOG_ONLY  <UTC:1326656625_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2949 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 19:43:45   148  ERR_DEBUG  LOG_ONLY  <UTC:1326656625_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2949 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 19:44:13   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326656653_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=CP:95  
01/15/2012 19:44:47   148  ERR_DEBUG  LOG_ONLY  <UTC:1326656687_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 19:44:47   148  ERR_DEBUG  LOG_ONLY  <UTC:1326656687_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 19:49:45   148  ERR_DEBUG  LOG_ONLY  <UTC:1326656985_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 19:49:45   148  ERR_DEBUG  LOG_ONLY  <UTC:1326656985_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 7
01/15/2012 19:51:23   148  ERR_DEBUG  LOG_ONLY  <UTC:1326657083_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 19:51:23   148  ERR_DEBUG  LOG_ONLY  <UTC:1326657083_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 19:52:29   148  ERR_DEBUG  LOG_ONLY  <UTC:1326657149_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 19:52:29   148  ERR_DEBUG  LOG_ONLY  <UTC:1326657149_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 19:53:07   148  ERR_DEBUG  LOG_ONLY  <UTC:1326657187_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 19:53:07   148  ERR_DEBUG  LOG_ONLY  <UTC:1326657187_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 19:53:40   148  ERR_DEBUG  LOG_ONLY  <UTC:1326657220_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 19:53:40   148  ERR_DEBUG  LOG_ONLY  <UTC:1326657220_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 19:54:16   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326657256_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=74 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=CP:96  
01/15/2012 19:57:12   148  ERR_DEBUG  LOG_ONLY  <UTC:1326657432_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 19:57:12   148  ERR_DEBUG  LOG_ONLY  <UTC:1326657432_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 20:03:56   148  ERR_DEBUG  LOG_ONLY  <UTC:1326657836_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 20:03:56   148  ERR_DEBUG  LOG_ONLY  <UTC:1326657836_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 20:04:16   148  ERR_DEBUG  LOG_ONLY  <UTC:1326657856_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 20:04:16   148  ERR_DEBUG  LOG_ONLY  <UTC:1326657856_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 20:04:20   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326657860_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=74 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=CP:97  
01/15/2012 20:05:17   148  ERR_DEBUG  LOG_ONLY  <UTC:1326657917_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=74 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 20:05:17   148  ERR_DEBUG  LOG_ONLY  <UTC:1326657917_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=74 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 20:06:07   148  ERR_DEBUG  LOG_ONLY  <UTC:1326657967_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 20:06:07   148  ERR_DEBUG  LOG_ONLY  <UTC:1326657967_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1
01/15/2012 20:08:36   148  ERR_DEBUG  LOG_ONLY  <UTC:1326658116_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=74 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 20:08:36   148  ERR_DEBUG  LOG_ONLY  <UTC:1326658116_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 8
01/15/2012 20:10:48   148  ERR_DEBUG  LOG_ONLY  <UTC:1326658248_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 20:10:48   148  ERR_DEBUG  LOG_ONLY  <UTC:1326658248_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=74 Meas.BreathRate=22
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 14
01/15/2012 20:15:11   148  ERR_DEBUG  LOG_ONLY  <UTC:1326658511_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 20:15:11   148  ERR_DEBUG  LOG_ONLY  <UTC:1326658511_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=73 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 20:16:27   148  ERR_DEBUG  LOG_ONLY  <UTC:1326658587_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 20:16:28   148  ERR_DEBUG  LOG_ONLY  <UTC:1326658588_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 3
01/15/2012 20:16:38   148  ERR_DEBUG  LOG_ONLY  <UTC:1326658598_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 20:16:38   148  ERR_DEBUG  LOG_ONLY  <UTC:1326658598_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 4
01/15/2012 20:18:48   148  ERR_DEBUG  LOG_ONLY  <UTC:1326658728_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 20:18:48   148  ERR_DEBUG  LOG_ONLY  <UTC:1326658728_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=72 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 20:27:07   148  ERR_DEBUG  LOG_ONLY  <UTC:1326659227_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 20:27:07   148  ERR_DEBUG  LOG_ONLY  <UTC:1326659227_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 20:34:50   148  ERR_DEBUG  LOG_ONLY  <UTC:1326659690_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 20:34:50   148  ERR_DEBUG  LOG_ONLY  <UTC:1326659690_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 8
01/15/2012 20:35:06   148  ERR_DEBUG  LOG_ONLY  <UTC:1326659706_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 20:35:06   148  ERR_DEBUG  LOG_ONLY  <UTC:1326659706_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 20:36:39   148  ERR_DEBUG  LOG_ONLY  <UTC:1326659799_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 20:36:39   148  ERR_DEBUG  LOG_ONLY  <UTC:1326659799_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 20:38:24   148  ERR_DEBUG  LOG_ONLY  <UTC:1326659904_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 20:38:24   148  ERR_DEBUG  LOG_ONLY  <UTC:1326659904_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=20
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 12
01/15/2012 20:38:33   148  ERR_DEBUG  LOG_ONLY  <UTC:1326659913_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 20:38:34   148  ERR_DEBUG  LOG_ONLY  <UTC:1326659914_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 20:38:51   148  ERR_DEBUG  LOG_ONLY  <UTC:1326659931_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 20:38:51   148  ERR_DEBUG  LOG_ONLY  <UTC:1326659931_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 13
01/15/2012 20:39:15   148  ERR_DEBUG  LOG_ONLY  <UTC:1326659955_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 20:39:15   148  ERR_DEBUG  LOG_ONLY  <UTC:1326659955_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 20:40:25   148  ERR_DEBUG  LOG_ONLY  <UTC:1326660025_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 20:40:25   148  ERR_DEBUG  LOG_ONLY  <UTC:1326660025_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=20
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 17
01/15/2012 20:41:00   148  ERR_DEBUG  LOG_ONLY  <UTC:1326660060_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 20:41:00   148  ERR_DEBUG  LOG_ONLY  <UTC:1326660060_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 20:43:31   148  ERR_DEBUG  LOG_ONLY  <UTC:1326660211_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 20:43:31   148  ERR_DEBUG  LOG_ONLY  <UTC:1326660211_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 20:44:01   148  ERR_DEBUG  LOG_ONLY  <UTC:1326660241_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 20:44:01   148  ERR_DEBUG  LOG_ONLY  <UTC:1326660241_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 61
01/15/2012 20:46:30   148  ERR_DEBUG  LOG_ONLY  <UTC:1326660390_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 20:46:30   148  ERR_DEBUG  LOG_ONLY  <UTC:1326660390_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 20:51:39   148  ERR_DEBUG  LOG_ONLY  <UTC:1326660699_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 20:51:39   148  ERR_DEBUG  LOG_ONLY  <UTC:1326660699_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 20:51:57   148  ERR_DEBUG  LOG_ONLY  <UTC:1326660717_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 20:51:57   148  ERR_DEBUG  LOG_ONLY  <UTC:1326660717_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 20:52:56   148  ERR_DEBUG  LOG_ONLY  <UTC:1326660776_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=71 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 20:52:56   148  ERR_DEBUG  LOG_ONLY  <UTC:1326660776_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 3
01/15/2012 20:54:54   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326660894_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=CQ:347 N MP:385   PP:32  
01/15/2012 20:56:54   148  ERR_DEBUG  LOG_ONLY  <UTC:1326661014_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 20:56:54   148  ERR_DEBUG  LOG_ONLY  <UTC:1326661014_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1
01/15/2012 20:56:59   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326661019_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=CP:157  
01/15/2012 20:59:24   148  ERR_DEBUG  LOG_ONLY  <UTC:1326661164_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=20
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 20:59:24   148  ERR_DEBUG  LOG_ONLY  <UTC:1326661164_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=20
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 3
01/15/2012 20:59:38   148  ERR_DEBUG  LOG_ONLY  <UTC:1326661178_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=20
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 20:59:38   148  ERR_DEBUG  LOG_ONLY  <UTC:1326661178_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=22
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 21:00:54   148  ERR_DEBUG  LOG_ONLY  <UTC:1326661254_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 21:00:55   148  ERR_DEBUG  LOG_ONLY  <UTC:1326661255_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 74
01/15/2012 21:01:50   148  ERR_DEBUG  LOG_ONLY  <UTC:1326661310_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 21:01:50   148  ERR_DEBUG  LOG_ONLY  <UTC:1326661310_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 21:04:08   148  ERR_DEBUG  LOG_ONLY  <UTC:1326661448_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 21:04:08   148  ERR_DEBUG  LOG_ONLY  <UTC:1326661448_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 21:05:07   148  ERR_DEBUG  LOG_ONLY  <UTC:1326661507_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 21:05:07   148  ERR_DEBUG  LOG_ONLY  <UTC:1326661507_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 21:07:03   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326661623_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=CP:158  
01/15/2012 21:11:03   148  ERR_DEBUG  LOG_ONLY  <UTC:1326661863_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 21:11:04   148  ERR_DEBUG  LOG_ONLY  <UTC:1326661864_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 48
01/15/2012 21:14:37   148  ERR_DEBUG  LOG_ONLY  <UTC:1326662077_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 21:14:37   148  ERR_DEBUG  LOG_ONLY  <UTC:1326662077_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 5
01/15/2012 21:15:09   148  ERR_DEBUG  LOG_ONLY  <UTC:1326662109_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 21:15:09   148  ERR_DEBUG  LOG_ONLY  <UTC:1326662109_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 21:17:07   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326662227_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=27
                         Reserved(Offset=52)=00
                         Opt.Text=CP:156  
01/15/2012 21:25:18   148  ERR_DEBUG  LOG_ONLY  <UTC:1326662718_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 21:25:18   148  ERR_DEBUG  LOG_ONLY  <UTC:1326662718_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1
01/15/2012 21:25:23   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326662723_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=CP:157  
01/15/2012 21:25:33   148  ERR_DEBUG  LOG_ONLY  <UTC:1326662733_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 21:25:33   148  ERR_DEBUG  LOG_ONLY  <UTC:1326662733_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 21:27:42   148  ERR_DEBUG  LOG_ONLY  <UTC:1326662862_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 21:27:42   148  ERR_DEBUG  LOG_ONLY  <UTC:1326662862_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 21:28:29   148  ERR_DEBUG  LOG_ONLY  <UTC:1326662909_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 21:28:29   148  ERR_DEBUG  LOG_ONLY  <UTC:1326662909_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 21:28:54   148  ERR_DEBUG  LOG_ONLY  <UTC:1326662934_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 21:28:54   148  ERR_DEBUG  LOG_ONLY  <UTC:1326662934_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 21:32:27   148  ERR_DEBUG  LOG_ONLY  <UTC:1326663147_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 21:32:27   148  ERR_DEBUG  LOG_ONLY  <UTC:1326663147_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 21:35:30   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326663330_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=CP:155  
01/15/2012 21:36:21   148  ERR_DEBUG  LOG_ONLY  <UTC:1326663381_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 21:36:22   148  ERR_DEBUG  LOG_ONLY  <UTC:1326663382_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 101
01/15/2012 21:36:47   148  ERR_DEBUG  LOG_ONLY  <UTC:1326663407_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 21:36:47   148  ERR_DEBUG  LOG_ONLY  <UTC:1326663407_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 21:38:16   148  ERR_DEBUG  LOG_ONLY  <UTC:1326663496_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 21:38:16   148  ERR_DEBUG  LOG_ONLY  <UTC:1326663496_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 20
01/15/2012 21:42:01   148  ERR_DEBUG  LOG_ONLY  <UTC:1326663721_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 21:42:01   148  ERR_DEBUG  LOG_ONLY  <UTC:1326663721_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 21:45:36   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326663936_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=CP:165  
01/15/2012 21:55:41   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326664541_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=24
                         Reserved(Offset=52)=00
                         Opt.Text=CP:165  
01/15/2012 22:05:47   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326665147_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=CP:163  
01/15/2012 22:15:53   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326665753_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=25
                         Reserved(Offset=52)=00
                         Opt.Text=CP:160  
01/15/2012 22:25:11   148  ERR_DEBUG  LOG_ONLY  <UTC:1326666311_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 22:25:11   148  ERR_DEBUG  LOG_ONLY  <UTC:1326666311_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 22:25:52   148  ERR_DEBUG  LOG_ONLY  <UTC:1326666352_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=21
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 22:25:52   148  ERR_DEBUG  LOG_ONLY  <UTC:1326666352_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=22
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 22:27:00   148  ERR_DEBUG  LOG_ONLY  <UTC:1326666420_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 22:27:01   148  ERR_DEBUG  LOG_ONLY  <UTC:1326666421_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 94
01/15/2012 22:27:33   148  ERR_DEBUG  LOG_ONLY  <UTC:1326666453_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=20
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 22:27:33   148  ERR_DEBUG  LOG_ONLY  <UTC:1326666453_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=20
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 22:27:58   148  ERR_DEBUG  LOG_ONLY  <UTC:1326666478_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=22
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 22:27:58   148  ERR_DEBUG  LOG_ONLY  <UTC:1326666478_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=22
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 3
01/15/2012 22:28:38   148  ERR_DEBUG  LOG_ONLY  <UTC:1326666518_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 22:28:38   148  ERR_DEBUG  LOG_ONLY  <UTC:1326666518_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 22:29:32   148  ERR_DEBUG  LOG_ONLY  <UTC:1326666572_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 22:29:33   148  ERR_DEBUG  LOG_ONLY  <UTC:1326666573_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 136
01/15/2012 22:30:57   148  ERR_DEBUG  LOG_ONLY  <UTC:1326666657_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 22:30:58   148  ERR_DEBUG  LOG_ONLY  <UTC:1326666658_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 4
01/15/2012 22:33:32   148  ERR_DEBUG  LOG_ONLY  <UTC:1326666812_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 22:33:32   148  ERR_DEBUG  LOG_ONLY  <UTC:1326666812_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=20
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 22:35:16   148  ERR_DEBUG  LOG_ONLY  <UTC:1326666916_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 22:35:16   148  ERR_DEBUG  LOG_ONLY  <UTC:1326666916_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 22:35:51   148  ERR_DEBUG  LOG_ONLY  <UTC:1326666951_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 22:35:51   148  ERR_DEBUG  LOG_ONLY  <UTC:1326666951_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 22:36:48   148  ERR_DEBUG  LOG_ONLY  <UTC:1326667008_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=66 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 22:36:49   148  ERR_DEBUG  LOG_ONLY  <UTC:1326667009_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=66 Meas.BreathRate=20
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 4
01/15/2012 22:37:45   148  ERR_DEBUG  LOG_ONLY  <UTC:1326667065_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 22:37:45   148  ERR_DEBUG  LOG_ONLY  <UTC:1326667065_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 22:39:42   148  ERR_DEBUG  LOG_ONLY  <UTC:1326667182_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 22:39:42   148  ERR_DEBUG  LOG_ONLY  <UTC:1326667182_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 8
01/15/2012 22:41:10   148  ERR_DEBUG  LOG_ONLY  <UTC:1326667270_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 22:41:10   148  ERR_DEBUG  LOG_ONLY  <UTC:1326667270_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 22:43:16   148  ERR_DEBUG  LOG_ONLY  <UTC:1326667396_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 22:43:16   148  ERR_DEBUG  LOG_ONLY  <UTC:1326667396_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 22:46:41   148  ERR_DEBUG  LOG_ONLY  <UTC:1326667601_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 22:46:41   148  ERR_DEBUG  LOG_ONLY  <UTC:1326667601_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 22:47:08   148  ERR_DEBUG  LOG_ONLY  <UTC:1326667628_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 22:47:08   148  ERR_DEBUG  LOG_ONLY  <UTC:1326667628_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 22:47:45   148  ERR_DEBUG  LOG_ONLY  <UTC:1326667665_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 22:47:45   148  ERR_DEBUG  LOG_ONLY  <UTC:1326667665_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 22:48:15   148  ERR_DEBUG  LOG_ONLY  <UTC:1326667695_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 22:48:15   148  ERR_DEBUG  LOG_ONLY  <UTC:1326667695_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 22:51:19   148  ERR_DEBUG  LOG_ONLY  <UTC:1326667879_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 22:51:19   148  ERR_DEBUG  LOG_ONLY  <UTC:1326667879_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 22:52:16   148  ERR_DEBUG  LOG_ONLY  <UTC:1326667936_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=66 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 22:52:16   148  ERR_DEBUG  LOG_ONLY  <UTC:1326667936_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=66 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 22:52:42   148  ERR_DEBUG  LOG_ONLY  <UTC:1326667962_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 22:52:42   148  ERR_DEBUG  LOG_ONLY  <UTC:1326667962_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 22:53:11   148  ERR_DEBUG  LOG_ONLY  <UTC:1326667991_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 22:53:11   148  ERR_DEBUG  LOG_ONLY  <UTC:1326667991_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 22:54:15   148  ERR_DEBUG  LOG_ONLY  <UTC:1326668055_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 22:54:15   148  ERR_DEBUG  LOG_ONLY  <UTC:1326668055_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 22:54:42   148  ERR_DEBUG  LOG_ONLY  <UTC:1326668082_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 22:54:42   148  ERR_DEBUG  LOG_ONLY  <UTC:1326668082_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 22:55:40   148  ERR_DEBUG  LOG_ONLY  <UTC:1326668140_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 22:55:40   148  ERR_DEBUG  LOG_ONLY  <UTC:1326668140_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 22:56:19   148  ERR_DEBUG  LOG_ONLY  <UTC:1326668179_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 22:56:19   148  ERR_DEBUG  LOG_ONLY  <UTC:1326668179_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 22:57:20   148  ERR_DEBUG  LOG_ONLY  <UTC:1326668240_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 22:57:20   148  ERR_DEBUG  LOG_ONLY  <UTC:1326668240_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 22:58:03   148  ERR_DEBUG  LOG_ONLY  <UTC:1326668283_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 22:58:03   148  ERR_DEBUG  LOG_ONLY  <UTC:1326668283_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 22:59:33   148  ERR_DEBUG  LOG_ONLY  <UTC:1326668373_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 22:59:33   148  ERR_DEBUG  LOG_ONLY  <UTC:1326668373_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 23:00:09   148  ERR_DEBUG  LOG_ONLY  <UTC:1326668409_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 23:00:09   148  ERR_DEBUG  LOG_ONLY  <UTC:1326668409_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 23:01:30   148  ERR_DEBUG  LOG_ONLY  <UTC:1326668490_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 23:01:30   148  ERR_DEBUG  LOG_ONLY  <UTC:1326668490_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 28
01/15/2012 23:04:23   148  ERR_DEBUG  LOG_ONLY  <UTC:1326668663_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 23:04:24   148  ERR_DEBUG  LOG_ONLY  <UTC:1326668664_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 103
01/15/2012 23:06:22   148  ERR_DEBUG  LOG_ONLY  <UTC:1326668782_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=20
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 23:06:22   148  ERR_DEBUG  LOG_ONLY  <UTC:1326668782_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=20
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 23:07:58   148  ERR_DEBUG  LOG_ONLY  <UTC:1326668878_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 23:07:58   148  ERR_DEBUG  LOG_ONLY  <UTC:1326668878_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 23:09:09   148  ERR_DEBUG  LOG_ONLY  <UTC:1326668949_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 23:09:09   148  ERR_DEBUG  LOG_ONLY  <UTC:1326668949_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 23:12:03   148  ERR_DEBUG  LOG_ONLY  <UTC:1326669123_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 23:12:03   148  ERR_DEBUG  LOG_ONLY  <UTC:1326669123_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 3
01/15/2012 23:15:58   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326669358_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=CP:151  
01/15/2012 23:16:26   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326669386_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=CQ:279   MP:358   PP:22  
01/15/2012 23:19:27   148  ERR_DEBUG  LOG_ONLY  <UTC:1326669567_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 23:19:27   148  ERR_DEBUG  LOG_ONLY  <UTC:1326669567_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1
01/15/2012 23:19:32   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326669572_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=CP:150  
01/15/2012 23:20:35   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326669635_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=CQ:284   MP:362   PP:21  
01/15/2012 23:24:37   148  ERR_DEBUG  LOG_ONLY  <UTC:1326669877_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=97 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 23:24:37   148  ERR_DEBUG  LOG_ONLY  <UTC:1326669877_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=97 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1
01/15/2012 23:24:41   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326669881_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=97 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=65 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=CP:150  
01/15/2012 23:29:53   148  ERR_DEBUG  LOG_ONLY  <UTC:1326670193_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=98 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=66 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 23:29:53   148  ERR_DEBUG  LOG_ONLY  <UTC:1326670193_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=98 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=66 Meas.BreathRate=21
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 23:31:20   148  ERR_DEBUG  LOG_ONLY  <UTC:1326670280_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=98 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 23:31:20   148  ERR_DEBUG  LOG_ONLY  <UTC:1326670280_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=98 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 23:34:46   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326670486_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=99 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=CP:158  
01/15/2012 23:43:44   148  ERR_DEBUG  LOG_ONLY  <UTC:1326671024_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 23:43:44   148  ERR_DEBUG  LOG_ONLY  <UTC:1326671024_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/15/2012 23:44:53   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326671093_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=CP:153  
01/15/2012 23:45:11   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326671111_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=CQ:277   MP:377   PP:23  
01/15/2012 23:55:13   148  ERR_DEBUG  LOG_ONLY  <UTC:1326671713_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/15/2012 23:55:13   148  ERR_DEBUG  LOG_ONLY  <UTC:1326671713_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1
01/15/2012 23:55:17   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326671717_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=66 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=CP:154  
01/16/2012 00:05:22   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326672322_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=23
                         Reserved(Offset=52)=00
                         Opt.Text=CP:165  
01/16/2012 00:15:25   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326672925_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2949 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=100) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=CP:160  
01/16/2012 00:25:33   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326673533_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2949 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=CP:155  
01/16/2012 00:35:38   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326674138_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2949 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=CP:155  
01/16/2012 00:45:46   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326674746_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2948 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=66 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=CP:154  
01/16/2012 01:45:52   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326678352_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2947 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=CP:142  
01/16/2012 01:56:30   148  ERR_DEBUG  LOG_ONLY  <UTC:1326678990_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2947 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 01:56:31   148  ERR_DEBUG  LOG_ONLY  <UTC:1326678991_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2947 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 62
01/16/2012 02:35:24   148  ERR_DEBUG  LOG_ONLY  <UTC:1326681324_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2947 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 02:35:24   148  ERR_DEBUG  LOG_ONLY  <UTC:1326681324_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2947 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 9
01/16/2012 02:36:27   148  ERR_DEBUG  LOG_ONLY  <UTC:1326681387_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2947 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 02:36:27   148  ERR_DEBUG  LOG_ONLY  <UTC:1326681387_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2947 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/16/2012 02:40:46   148  ERR_DEBUG  LOG_ONLY  <UTC:1326681646_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2947 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 02:40:46   148  ERR_DEBUG  LOG_ONLY  <UTC:1326681646_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2947 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 4
01/16/2012 02:41:21   148  ERR_DEBUG  LOG_ONLY  <UTC:1326681681_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2947 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 02:41:21   148  ERR_DEBUG  LOG_ONLY  <UTC:1326681681_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2947 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 11
01/16/2012 02:45:57   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326681957_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2947 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=CP:142  
01/16/2012 03:07:25   148  ERR_DEBUG  LOG_ONLY  <UTC:1326683245_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2947 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 03:07:26   148  ERR_DEBUG  LOG_ONLY  <UTC:1326683246_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2947 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 33
01/16/2012 03:46:04   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326685564_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2946 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=CP:143  
01/16/2012 03:57:20   148  ERR_DEBUG  LOG_ONLY  <UTC:1326686240_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2946 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 03:57:20   148  ERR_DEBUG  LOG_ONLY  <UTC:1326686240_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2946 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/16/2012 04:04:59   148  ERR_DEBUG  LOG_ONLY  <UTC:1326686699_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2946 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 04:04:59   148  ERR_DEBUG  LOG_ONLY  <UTC:1326686699_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2946 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/16/2012 04:14:35   148  ERR_DEBUG  LOG_ONLY  <UTC:1326687275_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2946 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 04:14:35   148  ERR_DEBUG  LOG_ONLY  <UTC:1326687275_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2946 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/16/2012 04:18:01   148  ERR_DEBUG  LOG_ONLY  <UTC:1326687481_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2946 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=65 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 04:18:01   148  ERR_DEBUG  LOG_ONLY  <UTC:1326687481_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2946 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=65 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/16/2012 04:19:48   148  ERR_DEBUG  LOG_ONLY  <UTC:1326687588_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2946 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 04:19:48   148  ERR_DEBUG  LOG_ONLY  <UTC:1326687588_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2946 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/16/2012 04:22:09   148  ERR_DEBUG  LOG_ONLY  <UTC:1326687729_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2946 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 04:22:09   148  ERR_DEBUG  LOG_ONLY  <UTC:1326687729_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2946 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/16/2012 04:23:49   148  ERR_DEBUG  LOG_ONLY  <UTC:1326687829_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2946 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 04:23:49   148  ERR_DEBUG  LOG_ONLY  <UTC:1326687829_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2946 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/16/2012 04:35:25   148  ERR_DEBUG  LOG_ONLY  <UTC:1326688525_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2946 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 04:35:26   148  ERR_DEBUG  LOG_ONLY  <UTC:1326688526_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2946 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 17
01/16/2012 04:35:47   148  ERR_DEBUG  LOG_ONLY  <UTC:1326688547_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2946 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 04:35:47   148  ERR_DEBUG  LOG_ONLY  <UTC:1326688547_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2946 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/16/2012 04:46:11   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326689171_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2947 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=CP:140  
01/16/2012 05:01:22   148  ERR_DEBUG  LOG_ONLY  <UTC:1326690082_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2947 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 05:01:22   148  ERR_DEBUG  LOG_ONLY  <UTC:1326690082_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2947 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/16/2012 05:46:18   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326692778_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2947 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=CP:133  
01/16/2012 06:46:24   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326696384_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2948 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=CP:131  
01/16/2012 07:17:25   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326698245_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2949 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=CQ:284   MP:343   PP:14  
01/16/2012 07:18:58   148  ERR_DEBUG  LOG_ONLY  <UTC:1326698338_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2949 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 07:18:58   148  ERR_DEBUG  LOG_ONLY  <UTC:1326698338_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2949 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1
01/16/2012 07:19:02   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326698342_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2949 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=66 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=CP:128  
01/16/2012 07:29:07   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326698947_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2949 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=29
                         Reserved(Offset=52)=00
                         Opt.Text=CP:136  
01/16/2012 07:39:14   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326699554_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=66 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=CP:127  
01/16/2012 07:44:52   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326699892_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=CQ:285   MP:341   PP:14  
01/16/2012 07:47:15   148  ERR_DEBUG  LOG_ONLY  <UTC:1326700035_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=66 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 07:47:15   148  ERR_DEBUG  LOG_ONLY  <UTC:1326700035_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=65 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1
01/16/2012 07:47:20   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326700040_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=66 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=CP:126  
01/16/2012 07:51:56   148  ERR_DEBUG  LOG_ONLY  <UTC:1326700316_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=65 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 07:51:56   148  ERR_DEBUG  LOG_ONLY  <UTC:1326700316_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2950 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=66 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 4
01/16/2012 07:56:23   148  ERR_DEBUG  LOG_ONLY  <UTC:1326700583_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=66 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 07:56:23   148  ERR_DEBUG  LOG_ONLY  <UTC:1326700583_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 4
01/16/2012 07:57:23   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326700643_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=66 Meas.BreathRate=20
                         Reserved(Offset=52)=00
                         Opt.Text=CP:128  
01/16/2012 07:57:24   148  ERR_DEBUG  LOG_ONLY  <UTC:1326700644_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=20
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 07:57:24   148  ERR_DEBUG  LOG_ONLY  <UTC:1326700644_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=66 Meas.BreathRate=20
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 8
01/16/2012 08:07:29   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326701249_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=CP:143  
01/16/2012 08:17:37   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326701857_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=66 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=CP:126  
01/16/2012 08:27:44   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326702464_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2951 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=CP:127  
01/16/2012 08:34:57   148  ERR_DEBUG  LOG_ONLY  <UTC:1326702897_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 08:34:57   148  ERR_DEBUG  LOG_ONLY  <UTC:1326702897_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=20
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 12
01/16/2012 08:37:48   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326703068_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=25
                         Reserved(Offset=52)=00
                         Opt.Text=CP:129  
01/16/2012 08:48:08   148  ERR_DEBUG  LOG_ONLY  <UTC:1326703688_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 08:48:08   148  ERR_DEBUG  LOG_ONLY  <UTC:1326703688_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 5
01/16/2012 09:11:42   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326705102_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2952 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=CQ:283   MP:345   PP:11  
01/16/2012 09:33:28   148  ERR_DEBUG  LOG_ONLY  <UTC:1326706408_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2953 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=64 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 09:33:28   148  ERR_DEBUG  LOG_ONLY  <UTC:1326706408_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2953 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=64 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1
01/16/2012 09:33:32   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326706412_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2953 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=63 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=CP:127  
01/16/2012 09:35:12   148  ERR_DEBUG  LOG_ONLY  <UTC:1326706512_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2953 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=63 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 09:35:12   148  ERR_DEBUG  LOG_ONLY  <UTC:1326706512_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2953 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=63 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/16/2012 09:36:51   148  ERR_DEBUG  LOG_ONLY  <UTC:1326706611_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2953 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=63 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 09:36:51   148  ERR_DEBUG  LOG_ONLY  <UTC:1326706611_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2953 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=63 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 5
01/16/2012 09:39:56   148  ERR_DEBUG  LOG_ONLY  <UTC:1326706796_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=64 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 09:39:56   148  ERR_DEBUG  LOG_ONLY  <UTC:1326706796_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=64 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/16/2012 09:40:07   148  ERR_DEBUG  LOG_ONLY  <UTC:1326706807_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=64 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 09:40:07   148  ERR_DEBUG  LOG_ONLY  <UTC:1326706807_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=63 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/16/2012 09:43:35   148  ERR_DEBUG  LOG_ONLY  <UTC:1326707015_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=64 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 09:43:35   148  ERR_DEBUG  LOG_ONLY  <UTC:1326707015_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=63 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 20
01/16/2012 09:43:40   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326707020_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=65 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=CP:141  
01/16/2012 09:49:11   148  ERR_DEBUG  LOG_ONLY  <UTC:1326707351_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=65 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 09:49:11   148  ERR_DEBUG  LOG_ONLY  <UTC:1326707351_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=99) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=65 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/16/2012 09:53:44   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326707624_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=66 Meas.BreathRate=25
                         Reserved(Offset=52)=00
                         Opt.Text=CP:126  
01/16/2012 10:03:48   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326708228_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=66 Meas.BreathRate=20
                         Reserved(Offset=52)=00
                         Opt.Text=CP:128  
01/16/2012 10:05:17   148  ERR_DEBUG  LOG_ONLY  <UTC:1326708317_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 10:05:18   148  ERR_DEBUG  LOG_ONLY  <UTC:1326708318_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 36
01/16/2012 10:06:31   148  ERR_DEBUG  LOG_ONLY  <UTC:1326708391_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 10:06:31   148  ERR_DEBUG  LOG_ONLY  <UTC:1326708391_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/16/2012 10:10:54   148  ERR_DEBUG  LOG_ONLY  <UTC:1326708654_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 10:10:54   148  ERR_DEBUG  LOG_ONLY  <UTC:1326708654_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1
01/16/2012 10:10:59   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326708659_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=65 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=CP:130  
01/16/2012 10:14:04   148  ERR_DEBUG  LOG_ONLY  <UTC:1326708844_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 10:14:04   148  ERR_DEBUG  LOG_ONLY  <UTC:1326708844_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=66 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 13
01/16/2012 10:21:06   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326709266_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=66 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=CP:133  
01/16/2012 10:31:11   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326709871_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=CP:137  
01/16/2012 10:33:49   148  ERR_DEBUG  LOG_ONLY  <UTC:1326710029_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 10:33:50   148  ERR_DEBUG  LOG_ONLY  <UTC:1326710030_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/16/2012 10:34:03   148  ERR_DEBUG  LOG_ONLY  <UTC:1326710043_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 10:34:03   148  ERR_DEBUG  LOG_ONLY  <UTC:1326710043_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/16/2012 10:41:17   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326710477_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2957 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=CP:138  
01/16/2012 10:51:01   148  ERR_DEBUG  LOG_ONLY  <UTC:1326711061_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2957 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 10:51:04   148  ERR_DEBUG  LOG_ONLY  <UTC:1326711064_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2957 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 306
01/16/2012 10:51:05   148  ERR_DEBUG  LOG_ONLY  <UTC:1326711065_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2957 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 10:51:05   148  ERR_DEBUG  LOG_ONLY  <UTC:1326711065_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2957 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 15
01/16/2012 10:51:22   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326711082_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2957 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=CQ:280   MP:361   PP:14  
01/16/2012 10:51:47   148  ERR_DEBUG  LOG_ONLY  <UTC:1326711107_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2957 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 10:51:47   148  ERR_DEBUG  LOG_ONLY  <UTC:1326711107_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2957 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1
01/16/2012 10:51:52   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326711112_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2957 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=CP:140  
01/16/2012 10:53:56   148  ERR_DEBUG  LOG_ONLY  <UTC:1326711236_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2957 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 10:53:56   148  ERR_DEBUG  LOG_ONLY  <UTC:1326711236_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2957 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/16/2012 10:54:21   148  ERR_DEBUG  LOG_ONLY  <UTC:1326711261_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2957 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 10:54:21   148  ERR_DEBUG  LOG_ONLY  <UTC:1326711261_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2957 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 7
01/16/2012 11:01:58   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326711718_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2957 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=CP:144  
01/16/2012 11:12:02   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326712322_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2957 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=CP:149  
01/16/2012 11:22:09   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326712929_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2957 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=CP:152  
01/16/2012 11:32:16   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326713536_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2957 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=CP:153  
01/16/2012 11:42:22   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326714142_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=CP:154  
01/16/2012 12:20:06   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326716406_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=CQ:275   MP:374   PP:16  
01/16/2012 12:22:20   148  ERR_DEBUG  LOG_ONLY  <UTC:1326716540_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 12:22:20   148  ERR_DEBUG  LOG_ONLY  <UTC:1326716540_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1
01/16/2012 12:22:24   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326716544_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=CP:160  
01/16/2012 12:22:29   148  ERR_DEBUG  LOG_ONLY  <UTC:1326716549_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 12:22:29   148  ERR_DEBUG  LOG_ONLY  <UTC:1326716549_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 5
01/16/2012 12:23:38   148  ERR_DEBUG  LOG_ONLY  <UTC:1326716618_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=24
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 12:23:38   148  ERR_DEBUG  LOG_ONLY  <UTC:1326716618_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=22
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 8
01/16/2012 12:24:42   148  ERR_DEBUG  LOG_ONLY  <UTC:1326716682_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=22
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 12:24:43   148  ERR_DEBUG  LOG_ONLY  <UTC:1326716683_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=23
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 74
01/16/2012 12:32:30   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326717150_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=CP:159  
01/16/2012 12:42:34   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326717754_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=CP:160  
01/16/2012 12:52:39   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326718359_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=CP:160  
01/16/2012 13:02:43   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326718963_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=20
                         Reserved(Offset=52)=00
                         Opt.Text=CP:161  
01/16/2012 13:12:49   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326719569_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=22
                         Reserved(Offset=52)=00
                         Opt.Text=CP:161  
01/16/2012 14:12:53   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326723173_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2954 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=23
                         Reserved(Offset=52)=00
                         Opt.Text=CP:152  
01/16/2012 15:13:00   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326726780_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2955 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=CP:153  
01/16/2012 16:13:04   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326730384_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=25
                         Reserved(Offset=52)=00
                         Opt.Text=CP:155  
01/16/2012 16:20:13   148  ERR_DEBUG  LOG_ONLY  <UTC:1326730813_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=21
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 16:20:16   148  ERR_DEBUG  LOG_ONLY  <UTC:1326730816_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 249
01/16/2012 16:20:17   148  ERR_DEBUG  LOG_ONLY  <UTC:1326730817_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 16:20:20   148  ERR_DEBUG  LOG_ONLY  <UTC:1326730820_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 317
01/16/2012 16:20:21   148  ERR_DEBUG  LOG_ONLY  <UTC:1326730821_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 16:20:24   148  ERR_DEBUG  LOG_ONLY  <UTC:1326730824_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 318
01/16/2012 16:20:25   148  ERR_DEBUG  LOG_ONLY  <UTC:1326730825_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 16:20:28   148  ERR_DEBUG  LOG_ONLY  <UTC:1326730828_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 318
01/16/2012 16:20:29   148  ERR_DEBUG  LOG_ONLY  <UTC:1326730829_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 16:20:32   148  ERR_DEBUG  LOG_ONLY  <UTC:1326730832_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 318
01/16/2012 16:20:33   148  ERR_DEBUG  LOG_ONLY  <UTC:1326730833_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 16:20:36   148  ERR_DEBUG  LOG_ONLY  <UTC:1326730836_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 318
01/16/2012 16:20:37   148  ERR_DEBUG  LOG_ONLY  <UTC:1326730837_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 16:20:40   148  ERR_DEBUG  LOG_ONLY  <UTC:1326730840_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 318
01/16/2012 16:20:41   148  ERR_DEBUG  LOG_ONLY  <UTC:1326730841_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 16:20:44   148  ERR_DEBUG  LOG_ONLY  <UTC:1326730844_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 318
01/16/2012 16:20:45   148  ERR_DEBUG  LOG_ONLY  <UTC:1326730845_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 16:20:48   148  ERR_DEBUG  LOG_ONLY  <UTC:1326730848_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 318
01/16/2012 16:20:49   148  ERR_DEBUG  LOG_ONLY  <UTC:1326730849_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 16:20:52   148  ERR_DEBUG  LOG_ONLY  <UTC:1326730852_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 318
01/16/2012 16:20:53   148  ERR_DEBUG  LOG_ONLY  <UTC:1326730853_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 16:20:54   148  ERR_DEBUG  LOG_ONLY  <UTC:1326730854_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 93
01/16/2012 16:20:54   148  ERR_DEBUG  LOG_ONLY  <UTC:1326730854_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 16:20:54   148  ERR_DEBUG  LOG_ONLY  <UTC:1326730854_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2956 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 10
01/16/2012 17:13:08   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326733988_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2959 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=CP:156  
01/16/2012 17:52:08   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326736328_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2960 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=CQ:272   MP:379   PP:29  
01/16/2012 17:52:51   148  ERR_DEBUG  LOG_ONLY  <UTC:1326736371_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2960 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 17:52:51   148  ERR_DEBUG  LOG_ONLY  <UTC:1326736371_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2960 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1
01/16/2012 17:52:56   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326736376_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2960 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=CP:152  
01/16/2012 18:03:03   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326736983_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2961 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=21
                         Reserved(Offset=52)=00
                         Opt.Text=CP:151  
01/16/2012 18:07:31   148  ERR_DEBUG  LOG_ONLY  <UTC:1326737251_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2961 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 18:07:32   148  ERR_DEBUG  LOG_ONLY  <UTC:1326737252_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2961 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 150
01/16/2012 18:07:33   148  ERR_DEBUG  LOG_ONLY  <UTC:1326737253_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2961 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 18:07:36   148  ERR_DEBUG  LOG_ONLY  <UTC:1326737256_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2961 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 309
01/16/2012 18:07:37   148  ERR_DEBUG  LOG_ONLY  <UTC:1326737257_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2961 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 18:07:38   148  ERR_DEBUG  LOG_ONLY  <UTC:1326737258_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2961 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 83
01/16/2012 18:07:39   148  ERR_DEBUG  LOG_ONLY  <UTC:1326737259_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2961 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 18:07:39   148  ERR_DEBUG  LOG_ONLY  <UTC:1326737259_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2961 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 8
01/16/2012 18:08:34   148  ERR_DEBUG  LOG_ONLY  <UTC:1326737314_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2962 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 18:08:34   148  ERR_DEBUG  LOG_ONLY  <UTC:1326737314_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2962 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/16/2012 18:08:36   148  ERR_DEBUG  LOG_ONLY  <UTC:1326737316_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2962 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 18:08:38   148  ERR_DEBUG  LOG_ONLY  <UTC:1326737318_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2962 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 217
01/16/2012 18:09:03   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326737343_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2961 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=CQ:272   MP:377   PP:26  
01/16/2012 18:10:01   148  ERR_DEBUG  LOG_ONLY  <UTC:1326737401_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2961 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 18:10:01   148  ERR_DEBUG  LOG_ONLY  <UTC:1326737401_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2961 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1
01/16/2012 18:10:06   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326737406_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2962 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=CP:160  
01/16/2012 18:10:17   148  ERR_DEBUG  LOG_ONLY  <UTC:1326737417_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2961 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 18:10:17   148  ERR_DEBUG  LOG_ONLY  <UTC:1326737417_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2961 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/16/2012 18:12:52   148  ERR_DEBUG  LOG_ONLY  <UTC:1326737572_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2961 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 18:12:53   148  ERR_DEBUG  LOG_ONLY  <UTC:1326737573_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2961 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 5
01/16/2012 18:20:10   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326738010_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2962 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=CP:152  
01/16/2012 18:30:18   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326738618_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2962 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=CP:152  
01/16/2012 18:40:22   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326739222_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2962 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=CP:152  
01/16/2012 18:50:26   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326739826_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2963 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 f4 01 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=500,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=CP:150  
01/16/2012 18:58:41   148  ERR_DEBUG  LOG_ONLY  <UTC:1326740321_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2963 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 18:58:41   148  ERR_DEBUG  LOG_ONLY  <UTC:1326740321_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2963 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/16/2012 19:00:32   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326740432_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2963 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=20
                         Reserved(Offset=52)=00
                         Opt.Text=CP:155  
01/16/2012 19:12:33   148  ERR_DEBUG  LOG_ONLY  <UTC:1326741153_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2964 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 19:12:33   148  ERR_DEBUG  LOG_ONLY  <UTC:1326741153_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2964 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/16/2012 19:13:03   148  ERR_DEBUG  LOG_ONLY  <UTC:1326741183_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2964 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=20
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 19:13:03   148  ERR_DEBUG  LOG_ONLY  <UTC:1326741183_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2964 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=20
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/16/2012 19:13:41   148  ERR_DEBUG  LOG_ONLY  <UTC:1326741221_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2964 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 19:13:41   148  ERR_DEBUG  LOG_ONLY  <UTC:1326741221_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2964 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 12
01/16/2012 19:19:56   148  ERR_DEBUG  LOG_ONLY  <UTC:1326741596_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2964 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 19:19:56   148  ERR_DEBUG  LOG_ONLY  <UTC:1326741596_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2964 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/16/2012 19:20:17   148  ERR_DEBUG  LOG_ONLY  <UTC:1326741617_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2964 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 19:20:17   148  ERR_DEBUG  LOG_ONLY  <UTC:1326741617_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2964 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 13
01/16/2012 19:24:09   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326741849_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2964 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=CQ:270   MP:377   PP:30  
01/16/2012 19:34:39   148  ERR_DEBUG  LOG_ONLY  <UTC:1326742479_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2965 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 19:34:39   148  ERR_DEBUG  LOG_ONLY  <UTC:1326742479_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2965 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1
01/16/2012 19:34:43   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326742483_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2965 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=65 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=CP:150  
01/16/2012 19:44:51   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326743091_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2965 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=66 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=CP:164  
01/16/2012 19:54:57   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326743697_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2965 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=26
                         Reserved(Offset=52)=00
                         Opt.Text=CP:162  
01/16/2012 19:56:43   148  ERR_DEBUG  LOG_ONLY  <UTC:1326743803_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2965 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=66 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 19:56:43   148  ERR_DEBUG  LOG_ONLY  <UTC:1326743803_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2965 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/16/2012 19:56:57   148  ERR_DEBUG  LOG_ONLY  <UTC:1326743817_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2965 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 19:56:57   148  ERR_DEBUG  LOG_ONLY  <UTC:1326743817_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2965 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/16/2012 19:59:49   148  ERR_DEBUG  LOG_ONLY  <UTC:1326743989_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2965 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 19:59:50   148  ERR_DEBUG  LOG_ONLY  <UTC:1326743990_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2965 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=66 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 98
01/16/2012 20:05:02   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326744302_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2966 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=CP:163  
01/16/2012 20:05:36   148  ERR_DEBUG  LOG_ONLY  <UTC:1326744336_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2966 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 20:05:36   148  ERR_DEBUG  LOG_ONLY  <UTC:1326744336_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2966 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/16/2012 20:15:08   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326744908_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2966 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=CP:162  
01/16/2012 20:20:08   148  ERR_DEBUG  LOG_ONLY  <UTC:1326745208_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2966 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 20:20:08   148  ERR_DEBUG  LOG_ONLY  <UTC:1326745208_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2966 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/16/2012 20:20:24   148  ERR_DEBUG  LOG_ONLY  <UTC:1326745224_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2966 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 20:20:24   148  ERR_DEBUG  LOG_ONLY  <UTC:1326745224_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2966 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 4
01/16/2012 20:22:18   148  ERR_DEBUG  LOG_ONLY  <UTC:1326745338_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2966 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 20:22:18   148  ERR_DEBUG  LOG_ONLY  <UTC:1326745338_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2966 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 8
01/16/2012 20:25:05   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326745505_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2966 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=CQ:270   MP:377   PP:24  
01/16/2012 20:26:38   148  ERR_DEBUG  LOG_ONLY  <UTC:1326745598_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2966 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 20:26:38   148  ERR_DEBUG  LOG_ONLY  <UTC:1326745598_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2966 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1
01/16/2012 20:26:43   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326745603_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2966 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=CP:150  
01/16/2012 20:36:50   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326746210_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2967 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=CP:163  
01/16/2012 20:40:43   148  ERR_DEBUG  LOG_ONLY  <UTC:1326746443_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2967 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 20:40:44   148  ERR_DEBUG  LOG_ONLY  <UTC:1326746444_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2967 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/16/2012 20:44:15   148  ERR_DEBUG  LOG_ONLY  <UTC:1326746655_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2967 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 20:44:15   148  ERR_DEBUG  LOG_ONLY  <UTC:1326746655_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2967 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/16/2012 20:46:57   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326746817_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2968 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=CP:162  
01/16/2012 20:52:25   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326747145_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2968 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=CQ:272   MP:372   PP:23  
01/16/2012 20:55:43   148  ERR_DEBUG  LOG_ONLY  <UTC:1326747343_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2968 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=66 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 20:55:43   148  ERR_DEBUG  LOG_ONLY  <UTC:1326747343_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2968 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=66 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1
01/16/2012 20:55:48   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326747348_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2968 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=66 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=CP:163  
01/16/2012 20:56:48   148  ERR_DEBUG  LOG_ONLY  <UTC:1326747408_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2968 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 20:56:48   148  ERR_DEBUG  LOG_ONLY  <UTC:1326747408_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2968 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 3
01/16/2012 20:56:54   148  ERR_DEBUG  LOG_ONLY  <UTC:1326747414_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2968 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=66 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 20:56:55   148  ERR_DEBUG  LOG_ONLY  <UTC:1326747415_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2968 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 95
01/16/2012 20:57:03   148  ERR_DEBUG  LOG_ONLY  <UTC:1326747423_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2968 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=66 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 20:57:03   148  ERR_DEBUG  LOG_ONLY  <UTC:1326747423_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2968 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=66 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/16/2012 20:57:06   148  ERR_DEBUG  LOG_ONLY  <UTC:1326747426_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2968 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 20:57:07   148  ERR_DEBUG  LOG_ONLY  <UTC:1326747427_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2968 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=66 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 61
01/16/2012 20:57:10   148  ERR_DEBUG  LOG_ONLY  <UTC:1326747430_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2968 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 20:57:11   148  ERR_DEBUG  LOG_ONLY  <UTC:1326747431_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2968 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 54
01/16/2012 20:57:22   148  ERR_DEBUG  LOG_ONLY  <UTC:1326747442_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2968 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 20:57:22   148  ERR_DEBUG  LOG_ONLY  <UTC:1326747442_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2968 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/16/2012 20:57:24   148  ERR_DEBUG  LOG_ONLY  <UTC:1326747444_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2968 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 20:57:25   148  ERR_DEBUG  LOG_ONLY  <UTC:1326747445_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2968 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 80
01/16/2012 20:57:25   148  ERR_DEBUG  LOG_ONLY  <UTC:1326747445_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2968 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=66 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 20:57:25   148  ERR_DEBUG  LOG_ONLY  <UTC:1326747445_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2968 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 26
01/16/2012 21:05:55   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326747955_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2969 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=CP:161  
01/16/2012 21:11:15   148  ERR_DEBUG  LOG_ONLY  <UTC:1326748275_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2969 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 21:11:15   148  ERR_DEBUG  LOG_ONLY  <UTC:1326748275_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2969 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=18
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/16/2012 21:16:00   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326748560_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2969 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=CP:161  
01/16/2012 21:16:15   148  ERR_DEBUG  LOG_ONLY  <UTC:1326748575_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2969 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 21:16:15   148  ERR_DEBUG  LOG_ONLY  <UTC:1326748575_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2969 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/16/2012 21:17:03   148  ERR_DEBUG  LOG_ONLY  <UTC:1326748623_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2969 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 21:17:03   148  ERR_DEBUG  LOG_ONLY  <UTC:1326748623_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2969 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/16/2012 21:26:06   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326749166_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2969 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=38
                         Reserved(Offset=52)=00
                         Opt.Text=CP:160  
01/16/2012 21:36:11   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326749771_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2969 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=35
                         Reserved(Offset=52)=00
                         Opt.Text=CP:164  
01/16/2012 21:37:40   148  ERR_DEBUG  LOG_ONLY  <UTC:1326749860_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2969 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=19
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 21:37:40   148  ERR_DEBUG  LOG_ONLY  <UTC:1326749860_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2969 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/16/2012 21:46:15   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326750375_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2969 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=98) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=32
                         Reserved(Offset=52)=00
                         Opt.Text=CP:150  
01/16/2012 22:46:19   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326753979_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2972 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=97) MaxUsage=90 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=CP:152  
01/16/2012 23:12:02   148  ERR_DEBUG  LOG_ONLY  <UTC:1326755522_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2972 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=97) MaxUsage=96 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=70 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 23:12:02   148  ERR_DEBUG  LOG_ONLY  <UTC:1326755522_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2972 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=97) MaxUsage=96 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1
01/16/2012 23:12:07   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326755527_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2972 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=97) MaxUsage=96 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=CP:151  
01/16/2012 23:14:17   148  ERR_DEBUG  LOG_ONLY  <UTC:1326755657_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2972 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=97) MaxUsage=96 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 23:14:17   148  ERR_DEBUG  LOG_ONLY  <UTC:1326755657_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2972 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=97) MaxUsage=96 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/16/2012 23:22:14   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326756134_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2972 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=97) MaxUsage=96 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=CP:150  
01/16/2012 23:26:16   148  ERR_DEBUG  LOG_ONLY  <UTC:1326756376_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2972 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=97) MaxUsage=96 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 23:26:16   148  ERR_DEBUG  LOG_ONLY  <UTC:1326756376_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2972 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=97) MaxUsage=96 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 2
01/16/2012 23:26:20   148  ERR_DEBUG  LOG_ONLY  <UTC:1326756380_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2972 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=97) MaxUsage=96 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 23:26:20   148  ERR_DEBUG  LOG_ONLY  <UTC:1326756380_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2972 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=97) MaxUsage=96 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 44
01/16/2012 23:27:31   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326756451_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2972 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=97) MaxUsage=96 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=CQ:278   MP:378   PP:33  
01/16/2012 23:27:47   148  ERR_DEBUG  LOG_ONLY  <UTC:1326756467_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2972 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=97) MaxUsage=96 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 23:27:47   148  ERR_DEBUG  LOG_ONLY  <UTC:1326756467_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2972 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=97) MaxUsage=96 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1
01/16/2012 23:27:52   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326756472_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2972 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=97) MaxUsage=96 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=CP:150  
01/16/2012 23:27:56   148  ERR_DEBUG  LOG_ONLY  <UTC:1326756476_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2972 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=97) MaxUsage=96 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/16/2012 23:27:56   148  ERR_DEBUG  LOG_ONLY  <UTC:1326756476_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2972 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=97) MaxUsage=96 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 3
01/16/2012 23:37:57   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326757077_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2972 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=97) MaxUsage=96 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=33
                         Reserved(Offset=52)=00
                         Opt.Text=CP:151  
01/16/2012 23:48:01   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326757681_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2973 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=97) MaxUsage=96 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=28
                         Reserved(Offset=52)=00
                         Opt.Text=CP:153  
01/16/2012 23:58:03   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326758283_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2974 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=97) MaxUsage=96 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=36
                         Reserved(Offset=52)=00
                         Opt.Text=CP:152  
01/17/2012 00:08:05   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326758885_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2974 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=97) MaxUsage=96 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=37
                         Reserved(Offset=52)=00
                         Opt.Text=CP:163  
01/17/2012 00:18:08   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326759488_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2973 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=97) MaxUsage=96 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=69 Meas.BreathRate=33
                         Reserved(Offset=52)=00
                         Opt.Text=CP:163  
01/17/2012 01:18:12   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326763092_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2974 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=97) MaxUsage=96 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=29
                         Reserved(Offset=52)=00
                         Opt.Text=CP:164  
01/17/2012 02:18:15   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326766695_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2975 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=97) MaxUsage=96 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=33
                         Reserved(Offset=52)=00
                         Opt.Text=CP:154  
01/17/2012 03:18:20   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326770300_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2976 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=97) MaxUsage=96 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=37
                         Reserved(Offset=52)=00
                         Opt.Text=CP:158  
01/17/2012 04:18:22   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326773902_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2977 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=97) MaxUsage=96 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=17
                         Reserved(Offset=52)=00
                         Opt.Text=CP:163  
01/17/2012 05:18:26   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326777506_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2979 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=97) MaxUsage=96 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=CP:157  
01/17/2012 06:18:34   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326781114_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2980 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=97) MaxUsage=96 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=68 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=CP:161  
01/17/2012 07:17:19   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326784639_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2981 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=100 DetLi=97) MaxUsage=96 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=67 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=CQ:282   MP:368   PP:14  
01/17/2012 07:38:55   297  ERR_SLEEP_EVENT  LOG_ONLY  <UTC:1326785935_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2982 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=100 DetLi=95) MaxUsage=96 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=63 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=IntC=100 DetC=95 V0=16339 V1=16109 FCC0=4332 FCC1=4168 SN0=27F8 SN1=103D2A
01/19/2012 13:07:16   152  ERR_POWER_UP_SYSTEM_INITIALIZATION  LOG_ONLY  <UTC:1326978436_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm=    0 SWver=  10.2.XX HWver=    
                         ExhType=0 PwrStat=00 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=0 MinAvgLeadAcidVolt=36000 PwrSource=4(NO_SOURCE)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=0 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Flash Build
01/19/2012 13:07:16    34  ERR_DSP_EXT_POWER_UP_SYSTEM_INIT  LOG_ONLY  <UTC:1326978436_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2881 SWver=  10.2.XX HWver=   0
                         ExhType=0 PwrStat=00 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=0 MinAvgLeadAcidVolt=36000 PwrSource=4(NO_SOURCE)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=0 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=
01/19/2012 13:07:16   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978436_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2853 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=00 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=0 MinAvgLeadAcidVolt=36000 PwrSource=4(NO_SOURCE)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=0 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:07:16   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978436_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3047 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=00 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=0 MinAvgLeadAcidVolt=36000 PwrSource=4(NO_SOURCE)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=0 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1
01/19/2012 13:07:16   341  ERR_FAN_CONTROL  LOG_ONLY  <UTC:1326978436_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3047 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=0 MinAvgLeadAcidVolt=0 PwrSource=4(NO_SOURCE)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=21 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Case Fan: ON 00100 IntBattT:0C DetBattT:0C Air:12.7C Mtr:11.0C
01/19/2012 13:07:17   249  ERR_AC_CONNECTED  LOG_ONLY  <UTC:1326978437_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3047 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=27 MinAvgLeadAcidVolt=0 PwrSource=4(NO_SOURCE)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=23 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=
01/19/2012 13:07:22   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978442_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3047 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=95 DetLi=91) MaxUsage=27 MinAvgLeadAcidVolt=0 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=26 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:07:22   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978442_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3047 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=95 DetLi=91) MaxUsage=27 MinAvgLeadAcidVolt=0 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=26 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1
01/19/2012 13:07:27   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326978447_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=95 DetLi=91) MaxUsage=27 MinAvgLeadAcidVolt=0 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=26 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=CP:-185  
01/19/2012 13:07:27   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978447_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=95 DetLi=91) MaxUsage=27 MinAvgLeadAcidVolt=0 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=27 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:07:29    57  ERR_THREAD_STACK_RESERVE  LOG_ONLY  <UTC:1326978449_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=95 DetLi=91) MaxUsage=27 MinAvgLeadAcidVolt=0 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=27 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Thread: SDFileManagementThread
01/19/2012 13:07:30   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978450_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=95 DetLi=91) MaxUsage=27 MinAvgLeadAcidVolt=0 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=27 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 322
01/19/2012 13:07:31   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978451_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=95 DetLi=91) MaxUsage=27 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=27 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:07:34   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978454_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=95 DetLi=91) MaxUsage=27 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=27 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 321
01/19/2012 13:07:35   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978455_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=95 DetLi=91) MaxUsage=27 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=28 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:07:38   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978458_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=95 DetLi=91) MaxUsage=27 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=28 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 321
01/19/2012 13:07:39   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978459_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=95 DetLi=91) MaxUsage=27 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=28 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:07:42   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978462_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=95 DetLi=91) MaxUsage=40 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=28 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 321
01/19/2012 13:07:43   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978463_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=95 DetLi=91) MaxUsage=40 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=28 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:07:46   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978466_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=95 DetLi=91) MaxUsage=40 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=29 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 321
01/19/2012 13:07:47   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978467_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=95 DetLi=91) MaxUsage=40 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=29 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:07:50   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978470_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=95 DetLi=91) MaxUsage=40 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=29 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 321
01/19/2012 13:07:51   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978471_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=95 DetLi=91) MaxUsage=40 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=29 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:07:54   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978474_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=95 DetLi=91) MaxUsage=40 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=29 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 321
01/19/2012 13:07:55   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978475_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=95 DetLi=91) MaxUsage=40 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=29 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:07:58   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978478_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=95 DetLi=91) MaxUsage=40 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=29 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 321
01/19/2012 13:07:59   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978479_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=95 DetLi=91) MaxUsage=40 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=29 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:08:02   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978482_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=95 DetLi=91) MaxUsage=40 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=30 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 321
01/19/2012 13:08:03   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978483_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=95 DetLi=91) MaxUsage=40 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=29 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:08:05   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978485_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=95 DetLi=91) MaxUsage=40 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=30 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 190
01/19/2012 13:08:14   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978494_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=95 DetLi=91) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=31 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:08:14   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978494_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=95 DetLi=91) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=31 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1
01/19/2012 13:08:18   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326978498_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=95 DetLi=91) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=31 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=CP:-180  
01/19/2012 13:08:19   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978499_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=95 DetLi=91) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=31 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:08:21   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978501_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=95 DetLi=91) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=31 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 217
01/19/2012 13:08:22   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978502_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=95 DetLi=91) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=31 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:08:22   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978502_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=95 DetLi=91) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=31 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 37
01/19/2012 13:08:24   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978504_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=95 DetLi=92) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=31 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:08:26   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978506_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=95 DetLi=92) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=31 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 200
01/19/2012 13:08:31   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978511_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=95 DetLi=92) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=31 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:08:31   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978511_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=95 DetLi=92) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=31 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1
01/19/2012 13:08:35   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326978515_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=95 DetLi=92) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=31 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=CP:-178  
01/19/2012 13:08:54   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978534_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=95 DetLi=92) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=32 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:08:55   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978535_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=95 DetLi=92) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=32 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 58
01/19/2012 13:08:57   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978537_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=95 DetLi=92) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=32 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:08:59   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978539_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=95 DetLi=92) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=32 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 220
01/19/2012 13:09:02   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978542_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=95 DetLi=92) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=33 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:09:03   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978543_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=95 DetLi=92) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=33 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 111
01/19/2012 13:09:05   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978545_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=95 DetLi=92) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=33 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:09:07   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978547_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=95 DetLi=92) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=33 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 197
01/19/2012 13:09:10   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978550_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=95 DetLi=92) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=33 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:09:11   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978551_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=95 DetLi=92) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=33 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 133
01/19/2012 13:09:13   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978553_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=95 DetLi=92) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=33 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:09:15   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978555_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=95 DetLi=92) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=33 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 184
01/19/2012 13:09:17   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978557_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=95 DetLi=92) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=33 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:09:19   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978559_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=95 DetLi=92) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=33 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 146
01/19/2012 13:09:21   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978561_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=95 DetLi=92) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=33 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:09:23   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978563_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=95 DetLi=92) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=33 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 175
01/19/2012 13:09:25   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978565_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=95 DetLi=92) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=33 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:09:27   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978567_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=95 DetLi=92) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=34 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 153
01/19/2012 13:09:29   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978569_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=95 DetLi=92) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=34 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:09:31   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978571_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=95 DetLi=92) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=34 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 170
01/19/2012 13:09:33   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978573_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=92) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=34 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:09:35   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978575_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=92) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=33 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 158
01/19/2012 13:09:37   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978577_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=92) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=34 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:09:39   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978579_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=92) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=33 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 166
01/19/2012 13:09:41   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978581_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=92) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=34 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:09:43   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978583_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=92) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=34 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 160
01/19/2012 13:09:45   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978585_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=92) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=34 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:09:47   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978587_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=92) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=33 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 165
01/19/2012 13:09:49   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978589_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=92) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=34 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:09:51   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978591_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=92) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=34 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 161
01/19/2012 13:09:53   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978593_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=92) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=34 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:09:55   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978595_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=92) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=35 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 164
01/19/2012 13:09:57   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978597_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=92) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=34 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:09:59   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978599_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=92) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=35 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 162
01/19/2012 13:10:01   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978601_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=92) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=34 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:10:03   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978603_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=92) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=35 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 163
01/19/2012 13:10:05   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978605_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=92) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=35 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:10:07   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978607_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=92) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=34 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 162
01/19/2012 13:10:09   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978609_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=92) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=35 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:10:11   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978611_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=92) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=35 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 163
01/19/2012 13:10:13   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978613_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=92) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=35 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:10:15   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978615_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=92) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=35 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 162
01/19/2012 13:10:17   341  ERR_FAN_CONTROL  LOG_ONLY  <UTC:1326978617_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=92) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=35 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Case Fan: OFF 00000 IntBattT:11C DetBattT:12C Air:15.3C Mtr:18.0C
01/19/2012 13:10:17   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978617_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=92) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=35 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:10:19   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978619_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=92) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=35 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 163
01/19/2012 13:10:21   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978621_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=92) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=35 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:10:23   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978623_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=92) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=35 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 163
01/19/2012 13:10:25   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978625_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=92) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=35 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:10:27   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978627_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=35 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 163
01/19/2012 13:10:29   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978629_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=35 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:10:31   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978631_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=35 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 163
01/19/2012 13:10:33   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978633_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=36 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:10:35   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978635_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=36 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 162
01/19/2012 13:10:37   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978637_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=36 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:10:39   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978639_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=36 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 163
01/19/2012 13:10:41   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978641_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=36 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:10:43   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978643_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=36 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 162
01/19/2012 13:10:45   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978645_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=36 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:10:47   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978647_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=36 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 164
01/19/2012 13:10:49   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978649_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=36 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:10:51   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978651_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=36 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 162
01/19/2012 13:10:53   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978653_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=36 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:10:55   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978655_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=36 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 164
01/19/2012 13:10:57   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978657_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=36 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:10:59   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978659_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=36 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 162
01/19/2012 13:11:01   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978661_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=36 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:11:03   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978663_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=36 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 164
01/19/2012 13:11:05   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978665_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=36 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:11:07   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978667_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=36 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 162
01/19/2012 13:11:09   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978669_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=37 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:11:11   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978671_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=36 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 164
01/19/2012 13:11:13   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978673_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=37 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:11:15   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978675_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=36 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 162
01/19/2012 13:11:17   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978677_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=36 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:11:19   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978679_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=37 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 163
01/19/2012 13:11:21   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978681_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=37 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:11:23   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978683_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=37 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 158
01/19/2012 13:11:25   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978685_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=37 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:11:27   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978687_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=37 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 166
01/19/2012 13:11:29   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978689_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=37 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:11:31   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978691_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=37 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 160
01/19/2012 13:11:33   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978693_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3045 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=37 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:11:35   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978695_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=37 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 165
01/19/2012 13:11:37   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978697_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=37 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:11:39   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978699_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3045 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=37 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 161
01/19/2012 13:11:41   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978701_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=37 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:11:43   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978703_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=37 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 164
01/19/2012 13:11:45   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978705_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=37 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:11:47   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978707_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=37 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 162
01/19/2012 13:11:49   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978709_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=38 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:11:51   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978711_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3045 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=37 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 163
01/19/2012 13:11:53   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978713_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=37 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:11:55   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978715_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=37 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 163
01/19/2012 13:11:57   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978717_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3045 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=37 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:11:59   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978719_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3045 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=37 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 163
01/19/2012 13:12:01   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978721_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3045 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=37 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:12:03   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978723_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=38 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 162
01/19/2012 13:12:05   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978725_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3045 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=38 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:12:07   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978727_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3045 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=37 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 163
01/19/2012 13:12:09   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978729_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3045 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=38 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:12:11   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978731_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3045 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=38 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 163
01/19/2012 13:12:13   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978733_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3046 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=37 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:12:15   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978735_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3045 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=38 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 163
01/19/2012 13:12:17   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978737_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3045 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=38 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:12:19   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978739_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3045 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=38 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 163
01/19/2012 13:12:21   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978741_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3045 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=38 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:12:23   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978743_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3045 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=38 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 163
01/19/2012 13:12:25   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978745_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3045 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=38 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:12:27   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978747_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3045 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=38 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 162
01/19/2012 13:12:29   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978749_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3045 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=38 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:12:31   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978751_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3045 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=43 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=38 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 154
01/19/2012 13:12:33   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978753_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3045 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=49 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=38 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:12:35   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978755_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3045 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=49 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=38 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 144
01/19/2012 13:12:37   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978757_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3045 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=49 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=38 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:12:39   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978759_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3045 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=49 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=38 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 165
01/19/2012 13:12:41   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978761_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3045 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=49 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=38 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:12:43   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978763_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3045 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=49 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=38 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 136
01/19/2012 13:12:45   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978765_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3045 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=49 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=38 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:12:47   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978767_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3045 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=49 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=38 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 150
01/19/2012 13:12:50   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978770_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3045 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=49 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 12 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=530,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=39 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:12:51   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978771_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3045 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=49 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 12 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=530,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=38 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 128
01/19/2012 13:12:54   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978774_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3045 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=49 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=38 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:12:55   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978775_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3045 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=49 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=39 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 99
01/19/2012 13:12:57   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978777_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3045 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=49 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 26 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=550,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=38 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:12:59   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978779_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3045 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=49 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 21 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=545,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=39 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 143
01/19/2012 13:13:02   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978782_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3045 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=53 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 0d 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=525,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=39 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:13:03   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978783_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3045 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=93) MaxUsage=53 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 0d 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=525,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=39 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 48
01/19/2012 13:13:06   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978786_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3045 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=94) MaxUsage=53 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 0d 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=525,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=38 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:13:07   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978787_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3045 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=94) MaxUsage=53 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 0d 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=525,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=39 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 124
01/19/2012 13:13:09   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978789_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3045 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=94) MaxUsage=53 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 0d 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=525,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=39 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:13:11   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978791_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3045 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=94) MaxUsage=53 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 0d 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=525,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=39 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 179
01/19/2012 13:13:14   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978794_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3045 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=94) MaxUsage=53 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 0d 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=525,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=39 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:13:15   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978795_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3045 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=94) MaxUsage=53 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 0d 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=525,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=39 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 86
01/19/2012 13:13:17   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978797_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3045 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=94) MaxUsage=53 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 0d 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=525,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=39 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:13:19   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978799_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3045 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=94) MaxUsage=53 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 0d 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=525,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=39 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 166
01/19/2012 13:13:22   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978802_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3045 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=94) MaxUsage=53 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 0d 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=525,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=39 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:13:23   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978803_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3045 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=94) MaxUsage=53 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 0d 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=525,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=39 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 115
01/19/2012 13:13:25   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978805_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3045 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=96 DetLi=94) MaxUsage=53 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 0d 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=525,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=39 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:13:27   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978807_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3045 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=97 DetLi=94) MaxUsage=53 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 0d 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=525,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=39 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 139
01/19/2012 13:13:30   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978810_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3045 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=97 DetLi=94) MaxUsage=53 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 0d 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=525,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=39 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:13:31   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978811_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3045 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=97 DetLi=94) MaxUsage=53 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 0d 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=525,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=39 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 125
01/19/2012 13:13:34   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978814_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3045 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=97 DetLi=94) MaxUsage=53 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 0d 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=525,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=39 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:13:35   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978815_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3045 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=97 DetLi=94) MaxUsage=53 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 0d 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=525,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=39 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 78
01/19/2012 13:15:54   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978954_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3045 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=97 DetLi=94) MaxUsage=60 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 0d 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=525,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=41 Meas.BreathRate=16
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:15:57   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978957_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3045 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=97 DetLi=94) MaxUsage=60 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 0d 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=525,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=41 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 279
01/19/2012 13:15:58   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978958_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3045 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=97 DetLi=94) MaxUsage=60 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 0d 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=525,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=41 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:16:01   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978961_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3045 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=97 DetLi=94) MaxUsage=60 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 0d 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=525,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=41 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 320
01/19/2012 13:16:02   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978962_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3045 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=97 DetLi=94) MaxUsage=60 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 0d 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=525,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=41 Meas.BreathRate=15
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/19/2012 13:16:03   148  ERR_DEBUG  LOG_ONLY  <UTC:1326978963_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3045 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=97 DetLi=94) MaxUsage=60 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 0d 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=525,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=42 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 163
01/19/2012 13:16:20   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1326978980_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3045 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=94) MaxUsage=60 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 0d 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=525,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=41 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=CQ:332   MP:32   PP:-229  
01/19/2012 13:21:16   297  ERR_SLEEP_EVENT  LOG_ONLY  <UTC:1326979276_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 3045 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=97 DetLi=94) MaxUsage=60 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 0d 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=525,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=43 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=IntC=97 DetC=94 V0=16274 V1=16071 FCC0=4299 FCC1=4104 SN0=27F8 SN1=103D2A
01/30/2012 09:56:49   152  ERR_POWER_UP_SYSTEM_INITIALIZATION  LOG_ONLY  <UTC:1327917409_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm=    0 SWver=  10.2.XX HWver=    
                         ExhType=0 PwrStat=00 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=0 MinAvgLeadAcidVolt=36000 PwrSource=4(NO_SOURCE)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 0d 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=525,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=0 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Flash Build
01/30/2012 09:56:49    34  ERR_DSP_EXT_POWER_UP_SYSTEM_INIT  LOG_ONLY  <UTC:1327917409_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2881 SWver=  10.2.XX HWver=   0
                         ExhType=0 PwrStat=00 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=0 MinAvgLeadAcidVolt=36000 PwrSource=4(NO_SOURCE)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 0d 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=525,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=0 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=
01/30/2012 09:56:49   148  ERR_DEBUG  LOG_ONLY  <UTC:1327917409_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2853 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=00 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=0 MinAvgLeadAcidVolt=36000 PwrSource=4(NO_SOURCE)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 0d 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=525,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=0 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/30/2012 09:56:49   148  ERR_DEBUG  LOG_ONLY  <UTC:1327917409_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2995 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=00 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=0 MinAvgLeadAcidVolt=36000 PwrSource=4(NO_SOURCE)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 0d 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=525,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=0 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1
01/30/2012 09:56:49   341  ERR_FAN_CONTROL  LOG_ONLY  <UTC:1327917409_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2995 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=0 MinAvgLeadAcidVolt=0 PwrSource=4(NO_SOURCE)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 0d 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=525,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=17 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Case Fan: ON 00100 IntBattT:0C DetBattT:0C Air:8.5C Mtr:7.0C
01/30/2012 09:56:50   249  ERR_AC_CONNECTED  LOG_ONLY  <UTC:1327917410_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2995 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=27 MinAvgLeadAcidVolt=0 PwrSource=4(NO_SOURCE)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 0d 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=525,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=18 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=
01/30/2012 09:57:29   148  ERR_DEBUG  LOG_ONLY  <UTC:1327917449_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2994 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=78 DetLi=81) MaxUsage=40 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=2  Params= 08 07 20 03 98 08 0d 02 01 03 0f 0c 00 00 
                            Mode=S/T,IPAP=1800,EPAP=800,IPAPMax=2200,TidVol=525,VolCtrl=1,Rise=3,BR=15,InspTime=12,flex=0
                         DSPTmpr=25 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/30/2012 09:57:40   148  ERR_DEBUG  LOG_ONLY  <UTC:1327917460_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2994 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=78 DetLi=81) MaxUsage=40 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=25 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1143
01/30/2012 09:57:43    57  ERR_THREAD_STACK_RESERVE  LOG_ONLY  <UTC:1327917463_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2994 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=78 DetLi=81) MaxUsage=40 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=25 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Thread: SDFileManagementThread
01/30/2012 09:57:47   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1327917467_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2994 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=78 DetLi=82) MaxUsage=40 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=25 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=CP:-200  
01/30/2012 09:57:58    96  ERR_CALIBRATION_CONTROL  LOG_ONLY  <UTC:1327917478_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2994 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=78 DetLi=82) MaxUsage=40 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=26 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=ENTER
01/30/2012 09:59:39    96  ERR_CALIBRATION_CONTROL  LOG_ONLY  <UTC:1327917579_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2994 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=79 DetLi=82) MaxUsage=40 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=29 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=EXIT
01/30/2012 09:59:39   341  ERR_FAN_CONTROL  LOG_ONLY  <UTC:1327917579_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2994 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=79 DetLi=82) MaxUsage=40 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=29 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Case Fan: OFF 00000 IntBattT:7C DetBattT:7C Air:9.1C Mtr:9.0C
01/30/2012 09:59:44   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1327917584_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2994 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=79 DetLi=82) MaxUsage=40 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=29 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=CQ:345   MP:-45   PP:-369  
01/30/2012 09:59:44    96  ERR_CALIBRATION_CONTROL  LOG_ONLY  <UTC:1327917584_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2994 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=79 DetLi=82) MaxUsage=40 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=29 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=ENTER
01/30/2012 10:00:20   148  ERR_DEBUG  LOG_ONLY  <UTC:1327917620_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2994 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=79 DetLi=82) MaxUsage=40 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=31 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/30/2012 10:00:26    96  ERR_CALIBRATION_CONTROL  LOG_ONLY  <UTC:1327917626_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2993 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=79 DetLi=82) MaxUsage=40 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=31 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=EXIT
01/30/2012 10:00:26   148  ERR_DEBUG  LOG_ONLY  <UTC:1327917626_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2993 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=79 DetLi=82) MaxUsage=40 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=31 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 633
01/30/2012 10:01:40   148  ERR_DEBUG  LOG_ONLY  <UTC:1327917700_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2993 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=80 DetLi=83) MaxUsage=40 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=33 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/30/2012 10:01:40   148  ERR_DEBUG  LOG_ONLY  <UTC:1327917700_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2993 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=80 DetLi=83) MaxUsage=40 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=33 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1
01/30/2012 10:01:46   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1327917706_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2993 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=80 DetLi=83) MaxUsage=40 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=33 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=CP:-161  
01/30/2012 10:02:00    96  ERR_CALIBRATION_CONTROL  LOG_ONLY  <UTC:1327917720_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2993 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=80 DetLi=83) MaxUsage=40 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=32 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=ENTER
01/30/2012 10:02:33   148  ERR_DEBUG  LOG_ONLY  <UTC:1327917753_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2993 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=80 DetLi=83) MaxUsage=40 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=33 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/30/2012 10:03:27    96  ERR_CALIBRATION_CONTROL  LOG_ONLY  <UTC:1327917807_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2993 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=81 DetLi=83) MaxUsage=40 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=34 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=EXIT
01/30/2012 10:03:27   148  ERR_DEBUG  LOG_ONLY  <UTC:1327917807_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2993 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=81 DetLi=83) MaxUsage=40 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=34 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 5517
01/30/2012 10:03:31    96  ERR_CALIBRATION_CONTROL  LOG_ONLY  <UTC:1327917811_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2993 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=81 DetLi=83) MaxUsage=40 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=34 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=ENTER
01/30/2012 10:04:08   148  ERR_DEBUG  LOG_ONLY  <UTC:1327917848_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2993 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=81 DetLi=84) MaxUsage=40 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=35 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/30/2012 10:05:18    96  ERR_CALIBRATION_CONTROL  LOG_ONLY  <UTC:1327917918_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2993 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=82 DetLi=84) MaxUsage=40 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=36 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=EXIT
01/30/2012 10:05:18   148  ERR_DEBUG  LOG_ONLY  <UTC:1327917918_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2993 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=82 DetLi=84) MaxUsage=40 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=36 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 6964
01/30/2012 10:05:21   108  ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY  <UTC:1327917921_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2993 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=82 DetLi=84) MaxUsage=40 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=36 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=CQ:354   MP:-8   PP:-249  
01/30/2012 10:07:10    96  ERR_CALIBRATION_CONTROL  LOG_ONLY  <UTC:1327918030_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2993 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=82 DetLi=85) MaxUsage=40 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=37 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=ENTER
01/30/2012 10:07:48   148  ERR_DEBUG  LOG_ONLY  <UTC:1327918068_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2993 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=83 DetLi=85) MaxUsage=40 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=38 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
01/30/2012 10:08:31    96  ERR_CALIBRATION_CONTROL  LOG_ONLY  <UTC:1327918111_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2993 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=83 DetLi=85) MaxUsage=40 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=39 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=EXIT
01/30/2012 10:08:31   148  ERR_DEBUG  LOG_ONLY  <UTC:1327918111_18>
                         Status=0x0c  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=Yes  FlowTrig=Yes)
                         Patm= 2993 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=83 DetLi=85) MaxUsage=40 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=38 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 4321
01/30/2012 10:13:56   297  ERR_SLEEP_EVENT  LOG_ONLY  <UTC:1327918436_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2992 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=83 DetLi=84) MaxUsage=40 MinAvgLeadAcidVolt=36000 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=40 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=IntC=83 DetC=84 V0=15782 V1=15730 FCC0=4300 FCC1=4091 SN0=27F8 SN1=103D2A
04/04/2012 11:37:28   152  ERR_POWER_UP_SYSTEM_INITIALIZATION  LOG_ONLY  <UTC:1333539448_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm=    0 SWver=  10.2.XX HWver=    
                         ExhType=0 PwrStat=00 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=0 MinAvgLeadAcidVolt=36000 PwrSource=4(NO_SOURCE)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=0 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Flash Build
04/04/2012 11:37:28    34  ERR_DSP_EXT_POWER_UP_SYSTEM_INIT  LOG_ONLY  <UTC:1333539448_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2881 SWver=  10.2.XX HWver=   0
                         ExhType=0 PwrStat=00 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=0 MinAvgLeadAcidVolt=36000 PwrSource=4(NO_SOURCE)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=0 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=
04/04/2012 11:37:28   148  ERR_DEBUG  LOG_ONLY  <UTC:1333539448_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2853 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=00 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=0 MinAvgLeadAcidVolt=36000 PwrSource=4(NO_SOURCE)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=0 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
04/04/2012 11:37:28   148  ERR_DEBUG  LOG_ONLY  <UTC:1333539448_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2790 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=00 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=0 MinAvgLeadAcidVolt=36000 PwrSource=4(NO_SOURCE)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=0 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1
04/04/2012 11:37:28   341  ERR_FAN_CONTROL  LOG_ONLY  <UTC:1333539448_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2790 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=0 MinAvgLeadAcidVolt=0 PwrSource=4(NO_SOURCE)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=30 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Case Fan: ON 00100 IntBattT:0C DetBattT:0C Air:21.4C Mtr:19.0C
04/04/2012 11:37:30   196  ERR_BATT_LOW_STATE_OF_HEALTH_DET_LI_ION  LOW_ALARM  <UTC:1333539450_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2790 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=27 MinAvgLeadAcidVolt=0 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=32 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=SOH=28 FCC=1141 RemCap=0 Cycle=269 SN=409
04/04/2012 11:37:30   221  ERR_TDA_RSC_LOW_DET_LI_ION  LOG_ONLY  <UTC:1333539450_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2790 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=27 MinAvgLeadAcidVolt=0 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=32 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=V0=11819 V1=11751 V2=0 FCC0=4300 FCC1=1141 SN0=27F8 SN1=409 Cyc0=5 Cyc1=26
04/04/2012 11:37:30   220  ERR_TDA_RSC_LOW_INT_LI_ION  LOG_ONLY  <UTC:1333539450_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2790 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=27 MinAvgLeadAcidVolt=0 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=32 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=V0=11819 V1=11751 V2=0 FCC0=4300 FCC1=1141 SN0=27F8 SN1=409 Cyc0=5 Cyc1=26
04/04/2012 11:37:30   210  ERR_TDA_CELL_UNDER_VOLTAGE_INT_LI_ION  LOG_ONLY  <UTC:1333539450_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2790 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=27 MinAvgLeadAcidVolt=0 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=32 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=V=11819 C1=2957 C2=2996 C3=2934 C4=2932 C=0 FCC=4300 SN=27F8 Cyc=5
04/04/2012 11:37:30   187  ERR_LAST_BATT_DET_LI_ION_NEARLY_DEPLETED  HIGH_ALARM  <UTC:1333539450_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2790 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=27 MinAvgLeadAcidVolt=0 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=32 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=NSrcs=0 V0=11819 ATR0=0 V1=11751 ATR1=0 V2=0 FCC0=4300 FCC1=1141 RM0=0 RM1
04/04/2012 11:37:30   282  ERR_INT_LI_ION_DEPLETED  HIGH_ALARM  <UTC:1333539450_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2790 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=27 MinAvgLeadAcidVolt=0 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=32 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Src=1 V0=11819 V1=11751 V2=0 FCC0=4300 FCC1=1141 RM0=0 RM1=0 SN0=27F8 SN1=
04/06/2012 16:54:14   152  ERR_POWER_UP_SYSTEM_INITIALIZATION  LOG_ONLY  <UTC:1333731254_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm=    0 SWver=  10.2.XX HWver=    
                         ExhType=0 PwrStat=00 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=0 MinAvgLeadAcidVolt=36000 PwrSource=4(NO_SOURCE)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=0 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Flash Build
04/06/2012 16:54:14    34  ERR_DSP_EXT_POWER_UP_SYSTEM_INIT  LOG_ONLY  <UTC:1333731254_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2881 SWver=  10.2.XX HWver=   0
                         ExhType=0 PwrStat=00 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=0 MinAvgLeadAcidVolt=36000 PwrSource=4(NO_SOURCE)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=0 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=
04/06/2012 16:54:14   148  ERR_DEBUG  LOG_ONLY  <UTC:1333731254_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2853 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=00 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=0 MinAvgLeadAcidVolt=36000 PwrSource=4(NO_SOURCE)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=0 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
04/06/2012 16:54:14   148  ERR_DEBUG  LOG_ONLY  <UTC:1333731254_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2792 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=00 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=0 MinAvgLeadAcidVolt=36000 PwrSource=4(NO_SOURCE)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=0 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1
04/06/2012 16:54:14   341  ERR_FAN_CONTROL  LOG_ONLY  <UTC:1333731254_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2792 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=0 MinAvgLeadAcidVolt=0 PwrSource=4(NO_SOURCE)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=30 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Case Fan: ON 00100 IntBattT:0C DetBattT:0C Air:20.5C Mtr:19.0C
04/06/2012 16:54:16   196  ERR_BATT_LOW_STATE_OF_HEALTH_DET_LI_ION  LOW_ALARM  <UTC:1333731256_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2792 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=27 MinAvgLeadAcidVolt=0 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=32 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=SOH=28 FCC=1141 RemCap=0 Cycle=269 SN=409
04/06/2012 16:54:16   221  ERR_TDA_RSC_LOW_DET_LI_ION  LOG_ONLY  <UTC:1333731256_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2792 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=27 MinAvgLeadAcidVolt=0 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=32 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=V0=11980 V1=11741 V2=0 FCC0=4300 FCC1=1141 SN0=27F8 SN1=409 Cyc0=5 Cyc1=26
04/06/2012 16:54:16   220  ERR_TDA_RSC_LOW_INT_LI_ION  LOG_ONLY  <UTC:1333731256_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2792 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=27 MinAvgLeadAcidVolt=0 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=32 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=V0=11979 V1=11741 V2=0 FCC0=4300 FCC1=1141 SN0=27F8 SN1=409 Cyc0=5 Cyc1=26
04/06/2012 16:54:16   210  ERR_TDA_CELL_UNDER_VOLTAGE_INT_LI_ION  LOG_ONLY  <UTC:1333731256_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2792 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=27 MinAvgLeadAcidVolt=0 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=32 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=V=11979 C1=2996 C2=3029 C3=2979 C4=2976 C=0 FCC=4300 SN=27F8 Cyc=5
04/06/2012 16:54:16   187  ERR_LAST_BATT_DET_LI_ION_NEARLY_DEPLETED  HIGH_ALARM  <UTC:1333731256_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2792 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=27 MinAvgLeadAcidVolt=0 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=32 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=NSrcs=0 V0=11979 ATR0=0 V1=11741 ATR1=0 V2=0 FCC0=4300 FCC1=1141 RM0=0 RM1
04/06/2012 16:54:16   282  ERR_INT_LI_ION_DEPLETED  HIGH_ALARM  <UTC:1333731256_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2792 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=27 MinAvgLeadAcidVolt=0 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=32 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Src=1 V0=11979 V1=11741 V2=0 FCC0=4300 FCC1=1141 RM0=0 RM1=0 SN0=27F8 SN1=
04/10/2012 03:41:08   152  ERR_POWER_UP_SYSTEM_INITIALIZATION  LOG_ONLY  <UTC:1334029268_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm=    0 SWver=  10.2.XX HWver=    
                         ExhType=0 PwrStat=00 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=0 MinAvgLeadAcidVolt=36000 PwrSource=4(NO_SOURCE)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=0 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Flash Build
04/10/2012 03:41:08    34  ERR_DSP_EXT_POWER_UP_SYSTEM_INIT  LOG_ONLY  <UTC:1334029268_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2881 SWver=  10.2.XX HWver=   0
                         ExhType=0 PwrStat=00 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=0 MinAvgLeadAcidVolt=36000 PwrSource=4(NO_SOURCE)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=0 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=
04/10/2012 03:41:08   148  ERR_DEBUG  LOG_ONLY  <UTC:1334029268_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2853 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=00 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=0 MinAvgLeadAcidVolt=36000 PwrSource=4(NO_SOURCE)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=0 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
04/10/2012 03:41:08   148  ERR_DEBUG  LOG_ONLY  <UTC:1334029268_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2782 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=00 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=0 MinAvgLeadAcidVolt=36000 PwrSource=4(NO_SOURCE)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=0 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1
04/10/2012 03:41:08   341  ERR_FAN_CONTROL  LOG_ONLY  <UTC:1334029268_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2782 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=0 MinAvgLeadAcidVolt=0 PwrSource=4(NO_SOURCE)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=27 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Case Fan: ON 00100 IntBattT:0C DetBattT:0C Air:18.6C Mtr:17.0C
04/10/2012 03:41:10   196  ERR_BATT_LOW_STATE_OF_HEALTH_DET_LI_ION  LOW_ALARM  <UTC:1334029270_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2782 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=27 MinAvgLeadAcidVolt=0 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=29 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=SOH=28 FCC=1141 RemCap=0 Cycle=269 SN=409
04/10/2012 03:41:10   221  ERR_TDA_RSC_LOW_DET_LI_ION  LOG_ONLY  <UTC:1334029270_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2782 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=27 MinAvgLeadAcidVolt=0 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=29 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=V0=12070 V1=11704 V2=0 FCC0=4300 FCC1=1141 SN0=27F8 SN1=409 Cyc0=5 Cyc1=26
04/10/2012 03:41:10   220  ERR_TDA_RSC_LOW_INT_LI_ION  LOG_ONLY  <UTC:1334029270_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2782 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=27 MinAvgLeadAcidVolt=0 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=30 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=V0=12071 V1=11704 V2=0 FCC0=4300 FCC1=1141 SN0=27F8 SN1=409 Cyc0=5 Cyc1=26
04/10/2012 03:41:10   210  ERR_TDA_CELL_UNDER_VOLTAGE_INT_LI_ION  LOG_ONLY  <UTC:1334029270_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2782 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=27 MinAvgLeadAcidVolt=0 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=30 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=V=12071 C1=3019 C2=3049 C3=3004 C4=2998 C=0 FCC=4300 SN=27F8 Cyc=5
04/10/2012 03:41:10   187  ERR_LAST_BATT_DET_LI_ION_NEARLY_DEPLETED  HIGH_ALARM  <UTC:1334029270_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2782 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=27 MinAvgLeadAcidVolt=0 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=30 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=NSrcs=0 V0=12071 ATR0=0 V1=11704 ATR1=0 V2=0 FCC0=4300 FCC1=1141 RM0=0 RM1
04/10/2012 03:41:10   282  ERR_INT_LI_ION_DEPLETED  HIGH_ALARM  <UTC:1334029270_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2782 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=27 MinAvgLeadAcidVolt=0 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=30 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Src=1 V0=12071 V1=11704 V2=0 FCC0=4300 FCC1=1141 RM0=0 RM1=0 SN0=27F8 SN1=
04/15/2012 08:15:28   152  ERR_POWER_UP_SYSTEM_INITIALIZATION  LOG_ONLY  <UTC:1334477728_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm=    0 SWver=  10.2.XX HWver=    
                         ExhType=0 PwrStat=00 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=0 MinAvgLeadAcidVolt=36000 PwrSource=4(NO_SOURCE)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=0 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Flash Build
04/15/2012 08:15:28    34  ERR_DSP_EXT_POWER_UP_SYSTEM_INIT  LOG_ONLY  <UTC:1334477728_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2881 SWver=  10.2.XX HWver=   0
                         ExhType=0 PwrStat=00 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=0 MinAvgLeadAcidVolt=36000 PwrSource=4(NO_SOURCE)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=0 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=
04/15/2012 08:15:28   148  ERR_DEBUG  LOG_ONLY  <UTC:1334477728_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2853 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=00 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=0 MinAvgLeadAcidVolt=36000 PwrSource=4(NO_SOURCE)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=0 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
04/15/2012 08:15:28   148  ERR_DEBUG  LOG_ONLY  <UTC:1334477728_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2771 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=00 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=0 MinAvgLeadAcidVolt=36000 PwrSource=4(NO_SOURCE)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=0 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1
04/15/2012 08:15:28   341  ERR_FAN_CONTROL  LOG_ONLY  <UTC:1334477728_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2771 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=0 MinAvgLeadAcidVolt=0 PwrSource=4(NO_SOURCE)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=29 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Case Fan: ON 00100 IntBattT:0C DetBattT:0C Air:20.1C Mtr:18.0C
04/15/2012 08:15:30   196  ERR_BATT_LOW_STATE_OF_HEALTH_DET_LI_ION  LOW_ALARM  <UTC:1334477730_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2771 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=27 MinAvgLeadAcidVolt=0 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=31 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=SOH=28 FCC=1141 RemCap=0 Cycle=269 SN=409
04/15/2012 08:15:30   221  ERR_TDA_RSC_LOW_DET_LI_ION  LOG_ONLY  <UTC:1334477730_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2771 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=27 MinAvgLeadAcidVolt=0 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=31 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=V0=12056 V1=11728 V2=0 FCC0=4300 FCC1=1141 SN0=27F8 SN1=409 Cyc0=5 Cyc1=26
04/15/2012 08:15:30   220  ERR_TDA_RSC_LOW_INT_LI_ION  LOG_ONLY  <UTC:1334477730_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2771 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=27 MinAvgLeadAcidVolt=0 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=31 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=V0=12057 V1=11728 V2=0 FCC0=4300 FCC1=1141 SN0=27F8 SN1=409 Cyc0=5 Cyc1=26
04/15/2012 08:15:30   210  ERR_TDA_CELL_UNDER_VOLTAGE_INT_LI_ION  LOG_ONLY  <UTC:1334477730_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2771 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=27 MinAvgLeadAcidVolt=0 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=31 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=V=12057 C1=3019 C2=3050 C3=2999 C4=2988 C=0 FCC=4300 SN=27F8 Cyc=5
04/15/2012 08:15:30   187  ERR_LAST_BATT_DET_LI_ION_NEARLY_DEPLETED  HIGH_ALARM  <UTC:1334477730_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2771 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=27 MinAvgLeadAcidVolt=0 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=31 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=NSrcs=0 V0=12057 ATR0=0 V1=11728 ATR1=0 V2=0 FCC0=4300 FCC1=1141 RM0=0 RM1
04/15/2012 08:15:30   282  ERR_INT_LI_ION_DEPLETED  HIGH_ALARM  <UTC:1334477730_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2771 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=27 MinAvgLeadAcidVolt=0 PwrSource=1(DET_LI_ION)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=31 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Src=1 V0=12057 V1=11728 V2=0 FCC0=4300 FCC1=1141 RM0=0 RM1=0 SN0=27F8 SN1=
04/16/2012 12:10:17   152  ERR_POWER_UP_SYSTEM_INITIALIZATION  LOG_ONLY  <UTC:1334578217_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm=    0 SWver=  10.2.XX HWver=    
                         ExhType=0 PwrStat=00 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=0 MinAvgLeadAcidVolt=36000 PwrSource=4(NO_SOURCE)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=0 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Flash Build
04/16/2012 12:10:17    34  ERR_DSP_EXT_POWER_UP_SYSTEM_INIT  LOG_ONLY  <UTC:1334578217_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2881 SWver=  10.2.XX HWver=   0
                         ExhType=0 PwrStat=00 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=0 MinAvgLeadAcidVolt=36000 PwrSource=4(NO_SOURCE)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=0 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=
04/16/2012 12:10:17   148  ERR_DEBUG  LOG_ONLY  <UTC:1334578217_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2853 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=00 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=0 MinAvgLeadAcidVolt=36000 PwrSource=4(NO_SOURCE)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=0 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start
04/16/2012 12:10:17   148  ERR_DEBUG  LOG_ONLY  <UTC:1334578217_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2810 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=00 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=0 MinAvgLeadAcidVolt=36000 PwrSource=4(NO_SOURCE)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=0 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error End, Duration (0.01 sec): 1
04/16/2012 12:10:17   341  ERR_FAN_CONTROL  LOG_ONLY  <UTC:1334578217_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2809 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=20 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=0 MinAvgLeadAcidVolt=0 PwrSource=4(NO_SOURCE)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=29 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Case Fan: ON 00100 IntBattT:0C DetBattT:0C Air:20.5C Mtr:19.0C
04/16/2012 12:10:18   249  ERR_AC_CONNECTED  LOG_ONLY  <UTC:1334578218_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2809 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=27 MinAvgLeadAcidVolt=0 PwrSource=4(NO_SOURCE)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=31 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=
04/16/2012 12:10:19   196  ERR_BATT_LOW_STATE_OF_HEALTH_DET_LI_ION  LOW_ALARM  <UTC:1334578219_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2809 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=27 MinAvgLeadAcidVolt=0 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=32 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=SOH=28 FCC=1141 RemCap=0 Cycle=269 SN=409
04/16/2012 12:10:19   221  ERR_TDA_RSC_LOW_DET_LI_ION  LOG_ONLY  <UTC:1334578219_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2809 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=27 MinAvgLeadAcidVolt=0 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=32 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=V0=12040 V1=11852 V2=0 FCC0=4300 FCC1=1141 SN0=27F8 SN1=409 Cyc0=5 Cyc1=26
04/16/2012 12:10:19   211  ERR_TDA_CELL_UNDER_VOLTAGE_DET_LI_ION  LOG_ONLY  <UTC:1334578219_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2809 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=27 MinAvgLeadAcidVolt=0 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=32 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=V=11852 C1=2940 C2=2932 C3=2926 C4=3054 C=0 FCC=1141 SN=409 Cyc=269
04/16/2012 12:10:19   220  ERR_TDA_RSC_LOW_INT_LI_ION  LOG_ONLY  <UTC:1334578219_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2809 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=27 MinAvgLeadAcidVolt=0 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=32 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=V0=12040 V1=11852 V2=0 FCC0=4300 FCC1=1141 SN0=27F8 SN1=409 Cyc0=5 Cyc1=26
04/16/2012 12:10:19   210  ERR_TDA_CELL_UNDER_VOLTAGE_INT_LI_ION  LOG_ONLY  <UTC:1334578219_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2809 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=27 MinAvgLeadAcidVolt=0 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=32 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=V=12040 C1=3015 C2=3048 C3=2994 C4=2983 C=0 FCC=4300 SN=27F8 Cyc=5
04/16/2012 12:10:19   282  ERR_INT_LI_ION_DEPLETED  HIGH_ALARM  <UTC:1334578219_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2809 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=27 MinAvgLeadAcidVolt=0 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=32 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Src=3 V0=12040 V1=11852 V2=0 FCC0=4300 FCC1=1141 RM0=0 RM1=0 SN0=27F8 SN1=
04/16/2012 12:10:57   148  ERR_DEBUG  LOG_ONLY  <UTC:1334578257_18>
                         Status=0x04  (Humidif=OFF/NotPresent  O2=NotPresent  Accesory=NotPresent  ExcessFlow=No  FlowTrig=Yes)
                         Patm= 2809 SWver=  10.2.03 HWver=   0
                         ExhType=0 PwrStat=a0 Capacity(LA=0 IntLi=0 DetLi=0) MaxUsage=40 MinAvgLeadAcidVolt=36000 PwrSource=3(AC_POWER)
                         Reserved(Offset=33) (Little-endian!)=00 00 00 
                         Rx Mode=3  Params= d0 07 90 01 48 0d f4 01 00 03 0a 0a 00 00 
                            Mode=T,IPAP=2000,EPAP=400,IPAPMax=3400,TidVol=500,VolCtrl=0,Rise=3,BR=10,InspTime=10,flex=0
                         DSPTmpr=37 Meas.BreathRate=0
                         Reserved(Offset=52)=00
                         Opt.Text=Leak Error Start

COUNT  ERRCODE      Log 17 (Encrypted Significant Event Text)
    1  E-018   ERR_DSP_DC_DC_CONTROL  ROUTINE_SERVICE
   36  E-072   ERR_MMC_SD_CARD_INSERTED  BEEP_ONLY
    6  E-074   ERR_MMC_SD_CARD_REMOVED  BEEP_ONLY
  108  E-110   ERR_LOW_PIP_ALARM  HIGH_ALARM
  197  E-114   ERR_LOW_MIN_VENT_ALARM  HIGH_ALARM
   11  E-118   ERR_LOW_CIRCUIT_LEAK_ALARM  HIGH_ALARM
    8  E-120   ERR_APNEA_ALARM  HIGH_ALARM
   53  E-165   ERR_LOW_PEP_ALARM  HIGH_ALARM
   80  E-166   ERR_UI_RESET_KEY_PRESS  KEYPRESS
    8  E-167   ERR_UI_HIDE_KEY_PRESS  KEYPRESS
   23  E-168   ERR_UI_AUDIO_PAUSE_KEY_PRESS  KEYPRESS
   28  E-169   ERR_HIGH_PIP_STAGE1_ALARM  BEEP_ONLY
    2  E-170   ERR_HIGH_PIP_STAGE2_ALARM  MED_ALARM
   31  E-173   ERR_START_ON_BATTERY  INFO_ALARM
   52  E-179   ERR_PWR_REDUCTION_AC_DISCONNECTED  MED_ALARM
    1  E-180   ERR_PWR_REDUCTION_LEAD_ACID_DISCONNECTED  INFO_ALARM
    1  E-181   ERR_PWR_REDUCTION_DET_LI_ION_DISCONNECTED  INFO_ALARM
    1  E-185   ERR_LAST_BATT_INT_LI_ION_LOW  MED_ALARM
    4  E-187   ERR_LAST_BATT_DET_LI_ION_NEARLY_DEPLETED  HIGH_ALARM
    6  E-188   ERR_LAST_BATT_INT_LI_ION_NEARLY_DEPLETED  HIGH_ALARM
    5  E-196   ERR_BATT_LOW_STATE_OF_HEALTH_DET_LI_ION  LOW_ALARM
    1  E-250   ERR_LEAD_ACID_BATT_CONNECTED  BEEP_ONLY
   43  E-251   ERR_DET_LI_ION_CONNECTED  BEEP_ONLY
   30  E-252   ERR_INT_LI_ION_CONNECTED  BEEP_ONLY
   21  E-264   ERR_MENU_BYPASS_ACTIVATED  KEYPRESS
    8  E-281   ERR_PWR_REDUCTION_DET_LI_ION_DEPLETED  INFO_ALARM
   25  E-282   ERR_INT_LI_ION_DEPLETED  HIGH_ALARM
   39  E-284   ERR_PWR_UPGRADE_AC_IN_USE  BEEP_ONLY
    6  E-286   ERR_PWR_UPGRADE_DET_LI_ION_IN_USE  BEEP_ONLY
    2  E-289   ERR_ROUTINE_REMINDER  ROUTINE_SERVICE
   25  E-291   ERR_CIRCUIT_CHECK  HIGH_ALARM
  255  E-293   ERR_POWER_OFF_KEY  KEYPRESS
  240  E-294   ERR_POWER_OFF_YES_KEY  KEYPRESS
    3  E-295   ERR_POWER_OFF_NO_KEY  KEYPRESS
  258  E-324   ERR_POWER_ON  KEYPRESS

COUNT  ERRCODE      Log 18 (Encrypted Engineering Debug Text)
    7  E-034   ERR_DSP_EXT_POWER_UP_SYSTEM_INIT  LOG_ONLY
    2  E-057   ERR_THREAD_STACK_RESERVE  LOG_ONLY
   10  E-096   ERR_CALIBRATION_CONTROL  LOG_ONLY
  156  E-108   ERR_DRIFT_MEASURED_DEBUG  LOG_ONLY
 1324  E-148   ERR_DEBUG  LOG_ONLY
    7  E-152   ERR_POWER_UP_SYSTEM_INITIALIZATION  LOG_ONLY
    4  E-187   ERR_LAST_BATT_DET_LI_ION_NEARLY_DEPLETED  HIGH_ALARM
    5  E-196   ERR_BATT_LOW_STATE_OF_HEALTH_DET_LI_ION  LOW_ALARM
    5  E-210   ERR_TDA_CELL_UNDER_VOLTAGE_INT_LI_ION  LOG_ONLY
    1  E-211   ERR_TDA_CELL_UNDER_VOLTAGE_DET_LI_ION  LOG_ONLY
    5  E-220   ERR_TDA_RSC_LOW_INT_LI_ION  LOG_ONLY
    7  E-221   ERR_TDA_RSC_LOW_DET_LI_ION  LOG_ONLY
    4  E-249   ERR_AC_CONNECTED  LOG_ONLY
    1  E-281   ERR_PWR_REDUCTION_DET_LI_ION_DEPLETED  INFO_ALARM
    5  E-282   ERR_INT_LI_ION_DEPLETED  HIGH_ALARM
    3  E-297   ERR_SLEEP_EVENT  LOG_ONLY
   15  E-341   ERR_FAN_CONTROL  LOG_ONLY
