[Header]
bq EVSW Version = 0.9.79	
DeviceName = bq20z95 v1.50
Time = 7/26/2012 6:59:08 AM	


[Voltage(1st Level Safety)]
COV Threshold = 4300
COV Time = 2
COV Recovery = 3900
COV Delta = 20
COV Temp. Hys = 10.0
POV Threshold = 16900
POV Time = 2
POV Recovery = 16000
CUV Threshold = 2300
CUV Time = 2
CUV Recovery = 3000
PUV Threshold = 10400
PUV Time = 2
PUV Recovery = 12000
[Current(1st Level Safety)]
OC (1st Tier) Chg = 3200
OC (1st Tier) Chg Time = 5
OC Chg Recovery = 200
OC (1st Tier) Dsg = 6000
OC (1st Tier) Dsg Time = 5
OC Dsg Recovery = 200
OC (2nd Tier) Chg = 8000
OC (2nd Tier) Chg Time = 2
OC (2nd Tier) Dsg = 8000
OC (2nd Tier) Dsg Time = 2
Current Recovery Time = 8
AFE OC Dsg = 16
AFE OC Dsg Time = 06
AFE OC Dsg Recovery = 5
AFE SC Chg Cfg = 64
AFE SC Dsg Cfg = FB
AFE SC Recovery = 5
[Temperature(1st Level Safety)]
Over Temp Chg = 50.0
OT Chg Time = 2
OT Chg Recovery = 40.0
Over Temp Dsg = 60.0
OT Dsg Time = 2
OT Dsg Recovery = 55.0
[Host Comm(1st Level Safety)]
Host Watchdog Timeout = 0

[Voltage(2nd Level Safety)]
SOV Threshold = 18000
SOV Time = 0
Cell Imbalance Current = 100
Cell Imbalance Fail Voltage = 1000
Cell Imbalance Time = 4
Battery Rest Time = 1800
Min CIM-check voltage = 3000
PFIN Detect Time = 2
[Current(2nd Level Safety)]
SOC Chg = 8000
SOC Chg Time = 4
SOC Dsg = 8000
SOC Dsg Time = 4
[Temperature(2nd Level Safety)]
SOT Chg = 65.0
SOT Chg Time = 4
SOT Dsg = 80.0
SOT Dsg Time = 0
Open Thermistor = -33.3
Open Time = 4
[FET Verification(2nd Level Safety)]
FET Fail Limit = 20
FET Fail Time = 4
[AFE Verification(2nd Level Safety)]
AFE Check Time = 30
AFE Fail Limit = 10
AFE Fail Recovery Time = 20
AFE Init Retry Limit = 6
AFE Init Limit = 20
[Fuse Verification(2nd Level Safety)]
Fuse Fail Limit = 2
Fuse Fail Time = 0

[Charge Inhibit Cfg(Charge Control)]
Chg Inhibit Temp Low = 0.0
Chg Inhibit Temp High = 45.0
Temp Hys = 2.0
[Pre-Charge Cfg(Charge Control)]
Pre-chg Current = 250
Pre-chg Temp = 5.0
Pre-chg Voltage = 3000
Recovery Voltage = 3100
[Fast Charge Cfg(Charge Control)]
Fast Charge Current = 2000
Charging Voltage = 16400
Delta Temp = 5.0
Suspend Low Temp = -5.0
Suspend High Temp = 50.0
[Pulse Charge Cfg(Charge Control)]
Turn ON Voltage = 4150
Turn OFF Voltage = 5000
Max ON Pulse Time = 60.00
Min OFF Pulse Time = 0.00
Max OFF Voltage = 5000
[Termination Cfg.(Charge Control)]
Maintenance Current = 0
Taper Current = 100
Taper Voltage = 300
Current Taper Window = 40
TCA Set % = -1
TCA Clear % = 95
FC Set % = -1
FC Clear % = 95
[Cell Balancing Cfg(Charge Control)]
Min Cell Deviation = 1750
[Charging Faults(Charge Control)]
Over Charging Voltage = 500
Over Charging Volt Time = 2
Over Charging Current = 500
Over Charging Curr Time = 2
Over Charging Curr Recov = 100
Depleted Voltage = 7000
Depleted Voltage Time = 2
Depleted Recovery = 8500
Over Charge Capacity = 300
Over Charge Recovery = 2
FC-MTO = 0
PC-MTO = 3600
Charge Fault Cfg = 2E

[Data(SBS Configuration)]
Rem Cap Alarm = 400
Rem Energy Alarm = 5760
Rem Time Alarm = 10
Init Battery Mode = 0081
Design Voltage = 14400
Spec Info = 0031
Manuf Date = 12-Jun-2010
Ser. Num. = 1397
Cycle Count = 288
CC Threshold = 2100
CC % = 100
CF MaxError Limit = 5
Design Capacity = 4000
Design Energy = 57600
Manuf Name = Micro_Power
Device Name = LI0444
Device Chemistry = LION
[Configuration(SBS Configuration)]
TDA Set % = 0
TDA Clear % = 15
FD Set % = 0
FD Clear % = 15
TDA Set Volt Threshold = 10000
TDA Set Volt Time = 5
TDA Clear Volt = 12600
FD Set Volt Threshold = 10000
FD Volt Time = 5
FD Clear Volt = 12600

[Manufacturer Data(System Data)]
Pack Lot Code = 1000
PCB Lot Code = 0001
Firmware Version = A003
Hardware Revision = 0001
Cell Revision = B001
[Manufacturer Info(System Data)]
Manuf. Info = 0123456789ABCDEF0123456789ABCDE
[Lifetime Data(System Data)]
Lifetime Max Temp = 43.9
Lifetime Min Temp = 1.8
Lifetime Max Cell Voltage = 4305
Lifetime Min Cell Voltage = 1663
Lifetime Max Pack Voltage = 16901
Lifetime Min Pack Voltage = 9241
Lifetime Max Chg Current = 2390
Lifetime Max Dsg Current = -4119
Lifetime Max Chg Power = 39260
Lifetime Max Dsg Power = -63900
Life Max AvgDsg Cur = -3999
Life Max AvgDsg Pow = -5728
Lifetime Avg Temp = 26.8
[Lifetime Temp Samples(System Data)]
LT Temp Samples = 305594

[Registers(Configuration)]
Operation Cfg A = 0F29
Operation Cfg B = 25D8
Operation Cfg C = 0005
Permanent Fail Cfg = 1CE4
Non-Removable Cfg = 0000
[AFE(Configuration)]
AFE.State_CTL = 00

[LED Cfg(LED Support)]
LED Flash Rate = 2.000
LED Blink Rate = 1.000
LED Delay = 48.8
LED Hold Time = 4
CHG Flash Alarm = 10
CHG Thresh 1 = 0
CHG Thresh 2 = 20
CHG Thresh 3 = 40
CHG Thresh 4 = 60
CHG Thresh 5 = 80
DSG Flash Alarm = 10
DSG Thresh 1 = 0
DSG Thresh 2 = 20
DSG Thresh 3 = 40
DSG Thresh 4 = 60
DSG Thresh 5 = 80
Sink Current = 3

[Power(Power)]
Flash Update OK Voltage = 7500
Shutdown Voltage = 7000
Shutdown Time = 0
Cell Shutdown Voltage = 2200
Cell Shutdown Time = 4
Charger Present = 3000
Sleep Current = 10
Bus Low Time = 5
Cal Inhibit Temp Low = 5.0
Cal Inhibit Temp High = 45.0
Sleep Voltage Time = 20
Sleep Current Time = 20
Wake Current Reg = 00

[IT Cfg(Gas Gauging)]
Load Select = 3
Load Mode = 1
Term Voltage = 12000
User Rate-mA = -2100
User Rate-mW = -30000
Reserve Cap-mAh = 250
Reserve Cap-mWh = 3600
[Current Thresholds(Gas Gauging)]
Dsg Current Threshold = 50
Chg Current Threshold = 50
Quit Current = 20
Dsg Relax Time = 10
Chg Relax Time = 30
[State(Gas Gauging)]
Qmax Cell 0 = 4581
Qmax Cell 1 = 4543
Qmax Cell 2 = 4555
Qmax Cell 3 = 4552
Qmax Pack = 4543
Update Status = 06
Avg I Last Run = -3957
Avg P Last Run = -5728
Delta Voltage = 55

[R_a0(Ra Table)]
Cell0 R_a flag = 0000
Cell0 R_a 0 = 132
Cell0 R_a 1 = 170
Cell0 R_a 2 = 250
Cell0 R_a 3 = 267
Cell0 R_a 4 = 310
Cell0 R_a 5 = 945
Cell0 R_a 6 = 1437
Cell0 R_a 7 = 2842
Cell0 R_a 8 = 2907
Cell0 R_a 9 = 5869
Cell0 R_a 10 = 7193
Cell0 R_a 11 = 1476
Cell0 R_a 12 = 4057
Cell0 R_a 13 = 4606
Cell0 R_a 14 = 4606
[R_a1(Ra Table)]
Cell1 R_a flag = 0055
Cell1 R_a 0 = 64
Cell1 R_a 1 = 78
Cell1 R_a 2 = 93
Cell1 R_a 3 = 97
Cell1 R_a 4 = 112
Cell1 R_a 5 = 123
Cell1 R_a 6 = 205
Cell1 R_a 7 = 446
Cell1 R_a 8 = 529
Cell1 R_a 9 = 585
Cell1 R_a 10 = 837
Cell1 R_a 11 = 652
Cell1 R_a 12 = 1761
Cell1 R_a 13 = 1845
Cell1 R_a 14 = 1992
[R_a2(Ra Table)]
Cell2 R_a flag = 0000
Cell2 R_a 0 = 83
Cell2 R_a 1 = 88
Cell2 R_a 2 = 93
Cell2 R_a 3 = 95
Cell2 R_a 4 = 107
Cell2 R_a 5 = 97
Cell2 R_a 6 = 132
Cell2 R_a 7 = 255
Cell2 R_a 8 = 294
Cell2 R_a 9 = 387
Cell2 R_a 10 = 436
Cell2 R_a 11 = 358
Cell2 R_a 12 = 759
Cell2 R_a 13 = 821
Cell2 R_a 14 = 870
[R_a3(Ra Table)]
Cell3 R_a flag = 0055
Cell3 R_a 0 = 63
Cell3 R_a 1 = 83
Cell3 R_a 2 = 83
Cell3 R_a 3 = 85
Cell3 R_a 4 = 98
Cell3 R_a 5 = 108
Cell3 R_a 6 = 157
Cell3 R_a 7 = 323
Cell3 R_a 8 = 467
Cell3 R_a 9 = 449
Cell3 R_a 10 = 323
Cell3 R_a 11 = 275
Cell3 R_a 12 = 698
Cell3 R_a 13 = 698
Cell3 R_a 14 = 761
[R_a0x(Ra Table)]
xCell0 R_a flag = 0055
xCell0 R_a 0 = 132
xCell0 R_a 1 = 170
xCell0 R_a 2 = 250
xCell0 R_a 3 = 267
xCell0 R_a 4 = 310
xCell0 R_a 5 = 1006
xCell0 R_a 6 = 1530
xCell0 R_a 7 = 3025
xCell0 R_a 8 = 3095
xCell0 R_a 9 = 6248
xCell0 R_a 10 = 7657
xCell0 R_a 11 = 1571
xCell0 R_a 12 = 4319
xCell0 R_a 13 = 4903
xCell0 R_a 14 = 4903
[R_a1x(Ra Table)]
xCell1 R_a flag = 0000
xCell1 R_a 0 = 64
xCell1 R_a 1 = 78
xCell1 R_a 2 = 93
xCell1 R_a 3 = 97
xCell1 R_a 4 = 112
xCell1 R_a 5 = 104
xCell1 R_a 6 = 173
xCell1 R_a 7 = 377
xCell1 R_a 8 = 447
xCell1 R_a 9 = 495
xCell1 R_a 10 = 708
xCell1 R_a 11 = 551
xCell1 R_a 12 = 1489
xCell1 R_a 13 = 1560
xCell1 R_a 14 = 1684
[R_a2x(Ra Table)]
xCell2 R_a flag = 0055
xCell2 R_a 0 = 83
xCell2 R_a 1 = 88
xCell2 R_a 2 = 93
xCell2 R_a 3 = 95
xCell2 R_a 4 = 107
xCell2 R_a 5 = 123
xCell2 R_a 6 = 167
xCell2 R_a 7 = 323
xCell2 R_a 8 = 373
xCell2 R_a 9 = 491
xCell2 R_a 10 = 553
xCell2 R_a 11 = 454
xCell2 R_a 12 = 962
xCell2 R_a 13 = 1041
xCell2 R_a 14 = 1103
[R_a3x(Ra Table)]
xCell3 R_a flag = 0000
xCell3 R_a 0 = 63
xCell3 R_a 1 = 83
xCell3 R_a 2 = 83
xCell3 R_a 3 = 85
xCell3 R_a 4 = 98
xCell3 R_a 5 = 89
xCell3 R_a 6 = 129
xCell3 R_a 7 = 266
xCell3 R_a 8 = 385
xCell3 R_a 9 = 370
xCell3 R_a 10 = 266
xCell3 R_a 11 = 227
xCell3 R_a 12 = 575
xCell3 R_a 13 = 575
xCell3 R_a 14 = 627

[Device Status Data(PF Status)]
PF Flags 1 = 0000
Fuse Flag = 00
PF Voltage = 0
PF C4 Voltage = 0
PF C3 Voltage = 0
PF C2 Voltage = 0
PF C1 Voltage = 0
PF Current = 0
PF Temperature = 0.0
PF Batt Stat = 00
PF RC-mAh = 0
PF RC-10mWh = 0
PF Chg Status = 0000
PF Safety Status = 0000
PF Flags 2 = 0000
[AFE Regs(PF Status)]
AFE Status = 00
AFE Output = 00
AFE State = 00
AFE Function = 00
AFE Cell Select = 00
AFE OLV = 00
AFE OLT = 00
AFE SCC = 00
AFE SCD = 00

[Data(Calibration)]
CC Gain = 10.115
CC Delta = 10.115
Ref Voltage = 1224.85
AFE Pack Gain = 672.91
CC Offset = -0.29
Board Offset = -34
Int Temp Offset = 0.0
Ext1 Temp Offset = -1.2
Ext2 Temp Offset = 0.0
[Config(Calibration)]
CC Current = 2000
Voltage Signal = 16000
Temp Signal = 298.0
CC Offset Time = 250
ADC Offset Time = 32
CC Gain Time = 250
Voltage Time = 1984
Temperature Time = 32
Cal Mode Timeout = 300
[Temp Model(Calibration)]
Ext Coef 1 = -28285
Ext Coef 2 = 20848
Ext Coef 3 = -7537
Ext Coef 4 = 401.2
Ext Min AD = 0
Ext Max Temp = 401.2
Int Coef 1 = 0
Int Coef 2 = 0
Int Coef 3 = -11136
Int Coef 4 = 575.4
Int Min AD = 0
Int Max Temp = 575.4
[Current(Calibration)]
Filter = 239
Deadband = 3
CC Deadband = 10.0
