My Computer
Intel(R) 6 Series/C200 Series Chipset Family USB Enhanced Host Controller - 1C26


DriverKey: {36fc9e60-c465-11cf-8056-444553540000}\0001
VendorID: 8086
DeviceID: 1C26
SubSysID: 76801462
Revision: 05

Debug Port Number:  2
Bus.Device.Function (in decimal): 0.29.0

Host Controller Power State Mappings
System State		Host Controller		Root Hub	USB wakeup	Powered
S0 (working)    	D0              	D0              		
S1 (sleep)      	D3              	D2              Yes		Yes
S2 (sleep)      	D? (unspecified)	D3              		
S3 (sleep)      	D3              	D2              Yes		Yes
S4 (Hibernate)  	D3              	D2              Yes		Yes
Last Sleep State	S? (unmapped)   
RootHub


Root Hub: USB#ROOT_HUB20#4&2f2a6bf6&0#{f18a0e88-c30c-11d0-8815-00a0c906bed8}
Hub Power:                    Self Power
Number of Ports:              2
Power switching:              Ganged
Compound device:              No
Over-current Protection:      Global
High speed capable:           Yes
High speed:                   Yes
Multiple transaction translations capable:                 No
Performs multiple transaction translations simultaneously: No
Hub wakes when device is connected:                        No
Hub is bus powered:           No
Hub is root:                  Yes
[Port1]  :  Generic USB Hub


External Hub: USB#VID_8087&PID_0024#5&33774b32&0&1#{f18a0e88-c30c-11d0-8815-00a0c906bed8}
Hub Power:                    Self Power
Number of Ports:              6
Power switching:              Individual
Compound device:              No
Over-current Protection:      Individual
High speed capable:           Yes
High speed:                   Yes
Multiple transaction translations capable:                 No
Performs multiple transaction translations simultaneously: No
Hub wakes when device is connected:                        No
Hub is bus powered:           No
Hub is root:                  No
       ---===>Device Information<===---

ConnectionStatus:                  
Current Config Value:              0x01  -> Device Bus Speed: High
Device Address:                    0x01
Open Pipes:                           1

          ===>Device Descriptor<===
bLength:                           0x12
bDescriptorType:                   0x01
bcdUSB:                          0x0200
bDeviceClass:                      0x09  -> This is a HUB Device
bDeviceSubClass:                   0x00
bDeviceProtocol:                   0x01
bMaxPacketSize0:                   0x40 = (64) Bytes
idVendor:                        0x8087 = Intel 
idProduct:                       0x0024
bcdDevice:                       0x0000
iManufacturer:                     0x00
iProduct:                          0x00
iSerialNumber:                     0x00
bNumConfigurations:                0x01

          ---===>Open Pipes<===---

          ===>Endpoint Descriptor<===
bLength:                           0x07
bDescriptorType:                   0x05
bEndpointAddress:                  0x81  -> Direction: IN - EndpointID: 1
bmAttributes:                      0x03  -> Interrupt Transfer Type
wMaxPacketSize:                  0x0001 = 1 transactions per microframe, 0x01 max bytes
bInterval:                         0x0C

       ---===>Full Configuration Descriptor<===---

          ===>Configuration Descriptor<===
bLength:                           0x09
bDescriptorType:                   0x02
wTotalLength:                    0x0019  -> Validated
bNumInterfaces:                    0x01
bConfigurationValue:               0x01
iConfiguration:                    0x00
bmAttributes:                      0xE0  -> Self Powered
  -> Remote Wakeup
MaxPower:                          0x00 =   0 mA

          ===>Interface Descriptor<===
bLength:                           0x09
bDescriptorType:                   0x04
bInterfaceNumber:                  0x00
bAlternateSetting:                 0x00
bNumEndpoints:                     0x01
bInterfaceClass:                   0x09  -> HUB Interface Class
bInterfaceSubClass:                0x00
bInterfaceProtocol:                0x00
iInterface:                        0x00

          ===>Endpoint Descriptor<===
bLength:                           0x07
bDescriptorType:                   0x05
bEndpointAddress:                  0x81  -> Direction: IN - EndpointID: 1
bmAttributes:                      0x03  -> Interrupt Transfer Type
wMaxPacketSize:                  0x0001 = 1 transactions per microframe, 0x01 max bytes
bInterval:                         0x0C
[Port1] 


ConnectionStatus:      NoDeviceConnected
[Port2]  :  USB Serial Converter


Device Power State:               PowerDeviceD0

       ---===>Device Information<===---
English product name: "TTL232R-3V3"

ConnectionStatus:                  
Current Config Value:              0x01  -> Device Bus Speed: Full
Device Address:                    0x02
Open Pipes:                           2

          ===>Device Descriptor<===
bLength:                           0x12
bDescriptorType:                   0x01
bcdUSB:                          0x0200
bDeviceClass:                      0x00  -> This is an Interface Class Defined Device
bDeviceSubClass:                   0x00
bDeviceProtocol:                   0x00
bMaxPacketSize0:                   0x08 = (8) Bytes
idVendor:                        0x0403 = Future Technology Devices International Limited
idProduct:                       0x6001
bcdDevice:                       0x0600
iManufacturer:                     0x01
     English (United States)  "FTDI"
iProduct:                          0x02
     English (United States)  "TTL232R-3V3"
iSerialNumber:                     0x03
     English (United States)  "FTAK06WP"
bNumConfigurations:                0x01

          ---===>Open Pipes<===---

          ===>Endpoint Descriptor<===
bLength:                           0x07
bDescriptorType:                   0x05
bEndpointAddress:                  0x81  -> Direction: IN - EndpointID: 1
bmAttributes:                      0x02  -> Bulk Transfer Type
wMaxPacketSize:                  0x0040 = 0x40 bytes
bInterval:                         0x00

          ===>Endpoint Descriptor<===
bLength:                           0x07
bDescriptorType:                   0x05
bEndpointAddress:                  0x02  -> Direction: OUT - EndpointID: 2
bmAttributes:                      0x02  -> Bulk Transfer Type
wMaxPacketSize:                  0x0040 = 0x40 bytes
bInterval:                         0x00

       ---===>Full Configuration Descriptor<===---

          ===>Configuration Descriptor<===
bLength:                           0x09
bDescriptorType:                   0x02
wTotalLength:                    0x0020  -> Validated
bNumInterfaces:                    0x01
bConfigurationValue:               0x01
iConfiguration:                    0x00
bmAttributes:                      0x80  -> Bus Powered
MaxPower:                          0x2D =  90 mA

          ===>Interface Descriptor<===
bLength:                           0x09
bDescriptorType:                   0x04
bInterfaceNumber:                  0x00
bAlternateSetting:                 0x00
bNumEndpoints:                     0x02
bInterfaceClass:                   0xFF  -> Interface Class Unknown to USBView
bInterfaceSubClass:                0xFF
bInterfaceProtocol:                0xFF
iInterface:                        0x02
     English (United States)  "TTL232R-3V3"

          ===>Endpoint Descriptor<===
bLength:                           0x07
bDescriptorType:                   0x05
bEndpointAddress:                  0x81  -> Direction: IN - EndpointID: 1
bmAttributes:                      0x02  -> Bulk Transfer Type
wMaxPacketSize:                  0x0040 = 0x40 bytes
bInterval:                         0x00

          ===>Endpoint Descriptor<===
bLength:                           0x07
bDescriptorType:                   0x05
bEndpointAddress:                  0x02  -> Direction: OUT - EndpointID: 2
bmAttributes:                      0x02  -> Bulk Transfer Type
wMaxPacketSize:                  0x0040 = 0x40 bytes
bInterval:                         0x00
[Port3] 


ConnectionStatus:      NoDeviceConnected
[Port4]  :  Generic USB Hub


External Hub: USB#VID_058F&PID_9254#6&13b4887a&0&4#{f18a0e88-c30c-11d0-8815-00a0c906bed8}
Hub Power:                    Self Power
Number of Ports:              4
Power switching:              Individual
Compound device:              No
Over-current Protection:      Individual
High speed capable:           No
High speed:                   No
Multiple transaction translations capable:                 No
Performs multiple transaction translations simultaneously: No
Hub wakes when device is connected:                        No
Hub is bus powered:           No
Hub is root:                  No
       ---===>Device Information<===---
English product name: "Generic USB Hub"

ConnectionStatus:                  
Current Config Value:              0x01  -> Device Bus Speed: Full
Device Address:                    0x03
Open Pipes:                           1

          ===>Device Descriptor<===
bLength:                           0x12
bDescriptorType:                   0x01
bcdUSB:                          0x0110
bDeviceClass:                      0x09  -> This is a HUB Device
bDeviceSubClass:                   0x00
bDeviceProtocol:                   0x00
bMaxPacketSize0:                   0x08 = (8) Bytes
idVendor:                        0x058F = Alcor Micro, Corp.
idProduct:                       0x9254
bcdDevice:                       0x0312
iManufacturer:                     0x01
     English (United States)  "ALCOR"
iProduct:                          0x02
     English (United States)  "Generic USB Hub"
iSerialNumber:                     0x00
bNumConfigurations:                0x01

          ---===>Open Pipes<===---

          ===>Endpoint Descriptor<===
bLength:                           0x07
bDescriptorType:                   0x05
bEndpointAddress:                  0x81  -> Direction: IN - EndpointID: 1
bmAttributes:                      0x03  -> Interrupt Transfer Type
wMaxPacketSize:                  0x0001 = 0x01 bytes
bInterval:                         0xFF

       ---===>Full Configuration Descriptor<===---

          ===>Configuration Descriptor<===
bLength:                           0x09
bDescriptorType:                   0x02
wTotalLength:                    0x0019  -> Validated
bNumInterfaces:                    0x01
bConfigurationValue:               0x01
iConfiguration:                    0x00
bmAttributes:                      0xE0  -> Self Powered
  -> Remote Wakeup
MaxPower:                          0x32 = 100 mA

          ===>Interface Descriptor<===
bLength:                           0x09
bDescriptorType:                   0x04
bInterfaceNumber:                  0x00
bAlternateSetting:                 0x00
bNumEndpoints:                     0x01
bInterfaceClass:                   0x09  -> HUB Interface Class
bInterfaceSubClass:                0x00
bInterfaceProtocol:                0x00
iInterface:                        0x00

          ===>Endpoint Descriptor<===
bLength:                           0x07
bDescriptorType:                   0x05
bEndpointAddress:                  0x81  -> Direction: IN - EndpointID: 1
bmAttributes:                      0x03  -> Interrupt Transfer Type
wMaxPacketSize:                  0x0001 = 0x01 bytes
bInterval:                         0xFF
[Port1] 


ConnectionStatus:      NoDeviceConnected
[Port2]  :  Prolific USB-to-Serial Comm Port


Device Power State:               PowerDeviceD0

       ---===>Device Information<===---
English product name: "USB-Serial Controller"

ConnectionStatus:                  
Current Config Value:              0x01  -> Device Bus Speed: Full
Device Address:                    0x04
Open Pipes:                           3

          ===>Device Descriptor<===
bLength:                           0x12
bDescriptorType:                   0x01
bcdUSB:                          0x0110
bDeviceClass:                      0x00  -> This is an Interface Class Defined Device
bDeviceSubClass:                   0x00
bDeviceProtocol:                   0x00
bMaxPacketSize0:                   0x40 = (64) Bytes
idVendor:                        0x067B = Prolific Technology, Inc.
idProduct:                       0x2303
bcdDevice:                       0x0300
iManufacturer:                     0x01
     English (United States)  "Prolific Technology Inc."
iProduct:                          0x02
     English (United States)  "USB-Serial Controller"
iSerialNumber:                     0x00
bNumConfigurations:                0x01

          ---===>Open Pipes<===---

          ===>Endpoint Descriptor<===
bLength:                           0x07
bDescriptorType:                   0x05
bEndpointAddress:                  0x81  -> Direction: IN - EndpointID: 1
bmAttributes:                      0x03  -> Interrupt Transfer Type
wMaxPacketSize:                  0x000A = 0x0A bytes
bInterval:                         0x01

          ===>Endpoint Descriptor<===
bLength:                           0x07
bDescriptorType:                   0x05
bEndpointAddress:                  0x02  -> Direction: OUT - EndpointID: 2
bmAttributes:                      0x02  -> Bulk Transfer Type
wMaxPacketSize:                  0x0040 = 0x40 bytes
bInterval:                         0x00

          ===>Endpoint Descriptor<===
bLength:                           0x07
bDescriptorType:                   0x05
bEndpointAddress:                  0x83  -> Direction: IN - EndpointID: 3
bmAttributes:                      0x02  -> Bulk Transfer Type
wMaxPacketSize:                  0x0040 = 0x40 bytes
bInterval:                         0x00

       ---===>Full Configuration Descriptor<===---

          ===>Configuration Descriptor<===
bLength:                           0x09
bDescriptorType:                   0x02
wTotalLength:                    0x0027  -> Validated
bNumInterfaces:                    0x01
bConfigurationValue:               0x01
iConfiguration:                    0x00
bmAttributes:                      0xA0  -> Bus Powered
  -> Remote Wakeup
MaxPower:                          0x32 = 100 mA

          ===>Interface Descriptor<===
bLength:                           0x09
bDescriptorType:                   0x04
bInterfaceNumber:                  0x00
bAlternateSetting:                 0x00
bNumEndpoints:                     0x03
bInterfaceClass:                   0xFF  -> Interface Class Unknown to USBView
bInterfaceSubClass:                0x00
bInterfaceProtocol:                0x00
iInterface:                        0x00

          ===>Endpoint Descriptor<===
bLength:                           0x07
bDescriptorType:                   0x05
bEndpointAddress:                  0x81  -> Direction: IN - EndpointID: 1
bmAttributes:                      0x03  -> Interrupt Transfer Type
wMaxPacketSize:                  0x000A = 0x0A bytes
bInterval:                         0x01

          ===>Endpoint Descriptor<===
bLength:                           0x07
bDescriptorType:                   0x05
bEndpointAddress:                  0x02  -> Direction: OUT - EndpointID: 2
bmAttributes:                      0x02  -> Bulk Transfer Type
wMaxPacketSize:                  0x0040 = 0x40 bytes
bInterval:                         0x00

          ===>Endpoint Descriptor<===
bLength:                           0x07
bDescriptorType:                   0x05
bEndpointAddress:                  0x83  -> Direction: IN - EndpointID: 3
bmAttributes:                      0x02  -> Bulk Transfer Type
wMaxPacketSize:                  0x0040 = 0x40 bytes
bInterval:                         0x00
[Port3]  :  Prolific USB-to-Serial Comm Port


Device Power State:               PowerDeviceD0

       ---===>Device Information<===---
English product name: "USB-Serial Controller"

ConnectionStatus:                  
Current Config Value:              0x01  -> Device Bus Speed: Full
Device Address:                    0x05
Open Pipes:                           3

          ===>Device Descriptor<===
bLength:                           0x12
bDescriptorType:                   0x01
bcdUSB:                          0x0110
bDeviceClass:                      0x00  -> This is an Interface Class Defined Device
bDeviceSubClass:                   0x00
bDeviceProtocol:                   0x00
bMaxPacketSize0:                   0x40 = (64) Bytes
idVendor:                        0x067B = Prolific Technology, Inc.
idProduct:                       0x2303
bcdDevice:                       0x0300
iManufacturer:                     0x01
     English (United States)  "Prolific Technology Inc."
iProduct:                          0x02
     English (United States)  "USB-Serial Controller"
iSerialNumber:                     0x00
bNumConfigurations:                0x01

          ---===>Open Pipes<===---

          ===>Endpoint Descriptor<===
bLength:                           0x07
bDescriptorType:                   0x05
bEndpointAddress:                  0x81  -> Direction: IN - EndpointID: 1
bmAttributes:                      0x03  -> Interrupt Transfer Type
wMaxPacketSize:                  0x000A = 0x0A bytes
bInterval:                         0x01

          ===>Endpoint Descriptor<===
bLength:                           0x07
bDescriptorType:                   0x05
bEndpointAddress:                  0x02  -> Direction: OUT - EndpointID: 2
bmAttributes:                      0x02  -> Bulk Transfer Type
wMaxPacketSize:                  0x0040 = 0x40 bytes
bInterval:                         0x00

          ===>Endpoint Descriptor<===
bLength:                           0x07
bDescriptorType:                   0x05
bEndpointAddress:                  0x83  -> Direction: IN - EndpointID: 3
bmAttributes:                      0x02  -> Bulk Transfer Type
wMaxPacketSize:                  0x0040 = 0x40 bytes
bInterval:                         0x00

       ---===>Full Configuration Descriptor<===---

          ===>Configuration Descriptor<===
bLength:                           0x09
bDescriptorType:                   0x02
wTotalLength:                    0x0027  -> Validated
bNumInterfaces:                    0x01
bConfigurationValue:               0x01
iConfiguration:                    0x00
bmAttributes:                      0xA0  -> Bus Powered
  -> Remote Wakeup
MaxPower:                          0x32 = 100 mA

          ===>Interface Descriptor<===
bLength:                           0x09
bDescriptorType:                   0x04
bInterfaceNumber:                  0x00
bAlternateSetting:                 0x00
bNumEndpoints:                     0x03
bInterfaceClass:                   0xFF  -> Interface Class Unknown to USBView
bInterfaceSubClass:                0x00
bInterfaceProtocol:                0x00
iInterface:                        0x00

          ===>Endpoint Descriptor<===
bLength:                           0x07
bDescriptorType:                   0x05
bEndpointAddress:                  0x81  -> Direction: IN - EndpointID: 1
bmAttributes:                      0x03  -> Interrupt Transfer Type
wMaxPacketSize:                  0x000A = 0x0A bytes
bInterval:                         0x01

          ===>Endpoint Descriptor<===
bLength:                           0x07
bDescriptorType:                   0x05
bEndpointAddress:                  0x02  -> Direction: OUT - EndpointID: 2
bmAttributes:                      0x02  -> Bulk Transfer Type
wMaxPacketSize:                  0x0040 = 0x40 bytes
bInterval:                         0x00

          ===>Endpoint Descriptor<===
bLength:                           0x07
bDescriptorType:                   0x05
bEndpointAddress:                  0x83  -> Direction: IN - EndpointID: 3
bmAttributes:                      0x02  -> Bulk Transfer Type
wMaxPacketSize:                  0x0040 = 0x40 bytes
bInterval:                         0x00
[Port4] 


ConnectionStatus:      NoDeviceConnected
[Port5]  :  CC2531 USB dongle


Device Power State:               PowerDeviceD0

       ---===>Device Information<===---
English product name: "CC2531 USB Dongle"

ConnectionStatus:                  
Current Config Value:              0x00  -> Device Bus Speed: Full
Device Address:                    0x06
Open Pipes:                           0
*!*ERROR:  No open pipes!

          ===>Device Descriptor<===
bLength:                           0x12
bDescriptorType:                   0x01
bcdUSB:                          0x0200
bDeviceClass:                      0x00  -> This is an Interface Class Defined Device
bDeviceSubClass:                   0x00
bDeviceProtocol:                   0x00
bMaxPacketSize0:                   0x20 = (32) Bytes
idVendor:                        0x0451 = Texas Instruments
idProduct:                       0x16AE
bcdDevice:                       0x6296
iManufacturer:                     0x01
     English (United States)  "Texas Instruments"
iProduct:                          0x02
     English (United States)  "CC2531 USB Dongle"
iSerialNumber:                     0x00
bNumConfigurations:                0x01

       ---===>Full Configuration Descriptor<===---

          ===>Configuration Descriptor<===
bLength:                           0x09
bDescriptorType:                   0x02
wTotalLength:                    0x0019  -> Validated
bNumInterfaces:                    0x01
bConfigurationValue:               0x01
iConfiguration:                    0x00
bmAttributes:                      0x80  -> Bus Powered
MaxPower:                          0x32 = 100 mA

          ===>Interface Descriptor<===
bLength:                           0x09
bDescriptorType:                   0x04
bInterfaceNumber:                  0x00
bAlternateSetting:                 0x00
bNumEndpoints:                     0x01
bInterfaceClass:                   0xFF  -> Interface Class Unknown to USBView
bInterfaceSubClass:                0xFF
bInterfaceProtocol:                0xFF
iInterface:                        0x00

          ===>Endpoint Descriptor<===
bLength:                           0x07
bDescriptorType:                   0x05
bEndpointAddress:                  0x83  -> Direction: IN - EndpointID: 3
bmAttributes:                      0x02  -> Bulk Transfer Type
wMaxPacketSize:                  0x0040 = 0x40 bytes
bInterval:                         0x05
[Port6] 


       ---===>Device Information<===---
English product name: "Texas Instruments XDS100v3"

ConnectionStatus:                  
Current Config Value:              0x00  -> Device Bus Speed: High
Device Address:                    0x07
Open Pipes:                           0
*!*ERROR:  No open pipes!

          ===>Device Descriptor<===
bLength:                           0x12
bDescriptorType:                   0x01
bcdUSB:                          0x0200
bDeviceClass:                      0x00  -> This is an Interface Class Defined Device
bDeviceSubClass:                   0x00
bDeviceProtocol:                   0x00
bMaxPacketSize0:                   0x40 = (64) Bytes
idVendor:                        0x0403 = Future Technology Devices International Limited
idProduct:                       0xA6D1
bcdDevice:                       0x0700
iManufacturer:                     0x01
     English (United States)  "TI"
iProduct:                          0x02
     English (United States)  "Texas Instruments XDS100v3"
iSerialNumber:                     0x03
     English (United States)  "06EB12100425"
bNumConfigurations:                0x01

       ---===>Full Configuration Descriptor<===---

          ===>Configuration Descriptor<===
bLength:                           0x09
bDescriptorType:                   0x02
wTotalLength:                    0x0037  -> Validated
bNumInterfaces:                    0x02
bConfigurationValue:               0x01
iConfiguration:                    0x00
bmAttributes:                      0x80  -> Bus Powered
MaxPower:                          0x32 = 100 mA

          ===>Interface Descriptor<===
bLength:                           0x09
bDescriptorType:                   0x04
bInterfaceNumber:                  0x00
bAlternateSetting:                 0x00
bNumEndpoints:                     0x02
bInterfaceClass:                   0xFF  -> Interface Class Unknown to USBView
bInterfaceSubClass:                0xFF
bInterfaceProtocol:                0xFF
iInterface:                        0x02
     English (United States)  "Texas Instruments XDS100v3"

          ===>Endpoint Descriptor<===
bLength:                           0x07
bDescriptorType:                   0x05
bEndpointAddress:                  0x81  -> Direction: IN - EndpointID: 1
bmAttributes:                      0x02  -> Bulk Transfer Type
wMaxPacketSize:                  0x0200 = 0x200 max bytes
bInterval:                         0x00

          ===>Endpoint Descriptor<===
bLength:                           0x07
bDescriptorType:                   0x05
bEndpointAddress:                  0x02  -> Direction: OUT - EndpointID: 2
bmAttributes:                      0x02  -> Bulk Transfer Type
wMaxPacketSize:                  0x0200 = 0x200 max bytes
bInterval:                         0x00

          ===>Interface Descriptor<===
bLength:                           0x09
bDescriptorType:                   0x04
bInterfaceNumber:                  0x01
bAlternateSetting:                 0x00
bNumEndpoints:                     0x02
bInterfaceClass:                   0xFF  -> Interface Class Unknown to USBView
bInterfaceSubClass:                0xFF
bInterfaceProtocol:                0xFF
iInterface:                        0x02
     English (United States)  "Texas Instruments XDS100v3"

          ===>Endpoint Descriptor<===
bLength:                           0x07
bDescriptorType:                   0x05
bEndpointAddress:                  0x83  -> Direction: IN - EndpointID: 3
bmAttributes:                      0x02  -> Bulk Transfer Type
wMaxPacketSize:                  0x0200 = 0x200 max bytes
bInterval:                         0x00

          ===>Endpoint Descriptor<===
bLength:                           0x07
bDescriptorType:                   0x05
bEndpointAddress:                  0x04  -> Direction: OUT - EndpointID: 4
bmAttributes:                      0x02  -> Bulk Transfer Type
wMaxPacketSize:                  0x0200 = 0x200 max bytes
bInterval:                         0x00
[Port2] 


ConnectionStatus:      NoDeviceConnected
Intel(R) 6 Series/C200 Series Chipset Family USB Enhanced Host Controller - 1C2D


DriverKey: {36fc9e60-c465-11cf-8056-444553540000}\0002
VendorID: 8086
DeviceID: 1C2D
SubSysID: 76801462
Revision: 05

Debug Port Number:  2
Bus.Device.Function (in decimal): 0.26.0

Host Controller Power State Mappings
System State		Host Controller		Root Hub	USB wakeup	Powered
S0 (working)    	D0              	D0              		
S1 (sleep)      	D3              	D2              Yes		Yes
S2 (sleep)      	D? (unspecified)	D3              		
S3 (sleep)      	D3              	D2              Yes		Yes
S4 (Hibernate)  	D3              	D2              Yes		Yes
Last Sleep State	S? (unmapped)   
RootHub


Root Hub: USB#ROOT_HUB20#4&18f8b8af&0#{f18a0e88-c30c-11d0-8815-00a0c906bed8}
Hub Power:                    Self Power
Number of Ports:              2
Power switching:              Ganged
Compound device:              No
Over-current Protection:      Global
High speed capable:           Yes
High speed:                   Yes
Multiple transaction translations capable:                 No
Performs multiple transaction translations simultaneously: No
Hub wakes when device is connected:                        No
Hub is bus powered:           No
Hub is root:                  Yes
[Port1]  :  Generic USB Hub


External Hub: USB#VID_8087&PID_0024#5&95ebd87&0&1#{f18a0e88-c30c-11d0-8815-00a0c906bed8}
Hub Power:                    Self Power
Number of Ports:              4
Power switching:              Individual
Compound device:              No
Over-current Protection:      Individual
High speed capable:           Yes
High speed:                   Yes
Multiple transaction translations capable:                 No
Performs multiple transaction translations simultaneously: No
Hub wakes when device is connected:                        No
Hub is bus powered:           No
Hub is root:                  No
       ---===>Device Information<===---

ConnectionStatus:                  
Current Config Value:              0x01  -> Device Bus Speed: High
Device Address:                    0x01
Open Pipes:                           1

          ===>Device Descriptor<===
bLength:                           0x12
bDescriptorType:                   0x01
bcdUSB:                          0x0200
bDeviceClass:                      0x09  -> This is a HUB Device
bDeviceSubClass:                   0x00
bDeviceProtocol:                   0x01
bMaxPacketSize0:                   0x40 = (64) Bytes
idVendor:                        0x8087 = Intel 
idProduct:                       0x0024
bcdDevice:                       0x0000
iManufacturer:                     0x00
iProduct:                          0x00
iSerialNumber:                     0x00
bNumConfigurations:                0x01

          ---===>Open Pipes<===---

          ===>Endpoint Descriptor<===
bLength:                           0x07
bDescriptorType:                   0x05
bEndpointAddress:                  0x81  -> Direction: IN - EndpointID: 1
bmAttributes:                      0x03  -> Interrupt Transfer Type
wMaxPacketSize:                  0x0001 = 1 transactions per microframe, 0x01 max bytes
bInterval:                         0x0C

       ---===>Full Configuration Descriptor<===---

          ===>Configuration Descriptor<===
bLength:                           0x09
bDescriptorType:                   0x02
wTotalLength:                    0x0019  -> Validated
bNumInterfaces:                    0x01
bConfigurationValue:               0x01
iConfiguration:                    0x00
bmAttributes:                      0xE0  -> Self Powered
  -> Remote Wakeup
MaxPower:                          0x00 =   0 mA

          ===>Interface Descriptor<===
bLength:                           0x09
bDescriptorType:                   0x04
bInterfaceNumber:                  0x00
bAlternateSetting:                 0x00
bNumEndpoints:                     0x01
bInterfaceClass:                   0x09  -> HUB Interface Class
bInterfaceSubClass:                0x00
bInterfaceProtocol:                0x00
iInterface:                        0x00

          ===>Endpoint Descriptor<===
bLength:                           0x07
bDescriptorType:                   0x05
bEndpointAddress:                  0x81  -> Direction: IN - EndpointID: 1
bmAttributes:                      0x03  -> Interrupt Transfer Type
wMaxPacketSize:                  0x0001 = 1 transactions per microframe, 0x01 max bytes
bInterval:                         0x0C
[Port1]  :  Périphérique USB composite


Device Power State:               PowerDeviceD0

       ---===>Device Information<===---
English product name: "G500"

ConnectionStatus:                  
Current Config Value:              0x01  -> Device Bus Speed: Full
Device Address:                    0x02
Open Pipes:                           2

          ===>Device Descriptor<===
bLength:                           0x12
bDescriptorType:                   0x01
bcdUSB:                          0x0200
bDeviceClass:                      0x00  -> This is an Interface Class Defined Device
bDeviceSubClass:                   0x00
bDeviceProtocol:                   0x00
bMaxPacketSize0:                   0x08 = (8) Bytes
idVendor:                        0x046D = Logitech Inc.
idProduct:                       0xC068
bcdDevice:                       0x5801
iManufacturer:                     0x01
     English (United States)  "Logitech"
iProduct:                          0x02
     English (United States)  "G500"
iSerialNumber:                     0x03
     English (United States)  "0E298DEA250016"
bNumConfigurations:                0x01

          ---===>Open Pipes<===---

          ===>Endpoint Descriptor<===
bLength:                           0x07
bDescriptorType:                   0x05
bEndpointAddress:                  0x81  -> Direction: IN - EndpointID: 1
bmAttributes:                      0x03  -> Interrupt Transfer Type
wMaxPacketSize:                  0x0008 = 0x08 bytes
bInterval:                         0x01

          ===>Endpoint Descriptor<===
bLength:                           0x07
bDescriptorType:                   0x05
bEndpointAddress:                  0x82  -> Direction: IN - EndpointID: 2
bmAttributes:                      0x03  -> Interrupt Transfer Type
wMaxPacketSize:                  0x0014 = 0x14 bytes
bInterval:                         0x01

       ---===>Full Configuration Descriptor<===---

          ===>Configuration Descriptor<===
bLength:                           0x09
bDescriptorType:                   0x02
wTotalLength:                    0x003B  -> Validated
bNumInterfaces:                    0x02
bConfigurationValue:               0x01
iConfiguration:                    0x04
     English (United States)  "U58.01_B0016"
bmAttributes:                      0xA0  -> Bus Powered
  -> Remote Wakeup
MaxPower:                          0x31 =  98 mA

          ===>Interface Descriptor<===
bLength:                           0x09
bDescriptorType:                   0x04
bInterfaceNumber:                  0x00
bAlternateSetting:                 0x00
bNumEndpoints:                     0x01
bInterfaceClass:                   0x03  -> HID Interface Class
bInterfaceSubClass:                0x01
bInterfaceProtocol:                0x02
iInterface:                        0x00

          ===>HID Descriptor<===
bLength:                           0x09
bDescriptorType:                   0x21
bcdHID:                          0x0111
bCountryCode:                      0x00
bNumDescriptors:                   0x01
bDescriptorType:                   0x22 (Report Descriptor)
wDescriptorLength:               0x0043

          ===>Endpoint Descriptor<===
bLength:                           0x07
bDescriptorType:                   0x05
bEndpointAddress:                  0x81  -> Direction: IN - EndpointID: 1
bmAttributes:                      0x03  -> Interrupt Transfer Type
wMaxPacketSize:                  0x0008 = 0x08 bytes
bInterval:                         0x01

          ===>Interface Descriptor<===
bLength:                           0x09
bDescriptorType:                   0x04
bInterfaceNumber:                  0x01
bAlternateSetting:                 0x00
bNumEndpoints:                     0x01
bInterfaceClass:                   0x03  -> HID Interface Class
bInterfaceSubClass:                0x00
bInterfaceProtocol:                0x00
iInterface:                        0x00

          ===>HID Descriptor<===
bLength:                           0x09
bDescriptorType:                   0x21
bcdHID:                          0x0111
bCountryCode:                      0x00
bNumDescriptors:                   0x01
bDescriptorType:                   0x22 (Report Descriptor)
wDescriptorLength:               0x007A

          ===>Endpoint Descriptor<===
bLength:                           0x07
bDescriptorType:                   0x05
bEndpointAddress:                  0x82  -> Direction: IN - EndpointID: 2
bmAttributes:                      0x03  -> Interrupt Transfer Type
wMaxPacketSize:                  0x0014 = 0x14 bytes
bInterval:                         0x01
[Port2]  :  Périphérique USB composite


Device Power State:               PowerDeviceD0

       ---===>Device Information<===---
English product name: "USB Multimedia Keyboard"

ConnectionStatus:                  
Current Config Value:              0x01  -> Device Bus Speed: Low
Device Address:                    0x03
Open Pipes:                           2

          ===>Device Descriptor<===
bLength:                           0x12
bDescriptorType:                   0x01
bcdUSB:                          0x0110
bDeviceClass:                      0x00  -> This is an Interface Class Defined Device
bDeviceSubClass:                   0x00
bDeviceProtocol:                   0x00
bMaxPacketSize0:                   0x08 = (8) Bytes
idVendor:                        0x046D = Logitech Inc.
idProduct:                       0xC313
bcdDevice:                       0x0100
iManufacturer:                     0x01
     English (United States)  "BTC"
iProduct:                          0x02
     English (United States)  "USB Multimedia Keyboard"
iSerialNumber:                     0x00
bNumConfigurations:                0x01

          ---===>Open Pipes<===---

          ===>Endpoint Descriptor<===
bLength:                           0x07
bDescriptorType:                   0x05
bEndpointAddress:                  0x81  -> Direction: IN - EndpointID: 1
bmAttributes:                      0x03  -> Interrupt Transfer Type
wMaxPacketSize:                  0x0008
bInterval:                         0x0A

          ===>Endpoint Descriptor<===
bLength:                           0x07
bDescriptorType:                   0x05
bEndpointAddress:                  0x82  -> Direction: IN - EndpointID: 2
bmAttributes:                      0x03  -> Interrupt Transfer Type
wMaxPacketSize:                  0x0008
bInterval:                         0x0A

       ---===>Full Configuration Descriptor<===---

          ===>Configuration Descriptor<===
bLength:                           0x09
bDescriptorType:                   0x02
wTotalLength:                    0x003B  -> Validated
bNumInterfaces:                    0x02
bConfigurationValue:               0x01
iConfiguration:                    0x00
bmAttributes:                      0xA0  -> Bus Powered
  -> Remote Wakeup
MaxPower:                          0x32 = 100 mA

          ===>Interface Descriptor<===
bLength:                           0x09
bDescriptorType:                   0x04
bInterfaceNumber:                  0x00
bAlternateSetting:                 0x00
bNumEndpoints:                     0x01
bInterfaceClass:                   0x03  -> HID Interface Class
bInterfaceSubClass:                0x01
bInterfaceProtocol:                0x01
iInterface:                        0x00

          ===>HID Descriptor<===
bLength:                           0x09
bDescriptorType:                   0x21
bcdHID:                          0x0110
bCountryCode:                      0x00
bNumDescriptors:                   0x01
bDescriptorType:                   0x22 (Report Descriptor)
wDescriptorLength:               0x0041

          ===>Endpoint Descriptor<===
bLength:                           0x07
bDescriptorType:                   0x05
bEndpointAddress:                  0x81  -> Direction: IN - EndpointID: 1
bmAttributes:                      0x03  -> Interrupt Transfer Type
wMaxPacketSize:                  0x0008
bInterval:                         0x0A

          ===>Interface Descriptor<===
bLength:                           0x09
bDescriptorType:                   0x04
bInterfaceNumber:                  0x01
bAlternateSetting:                 0x00
bNumEndpoints:                     0x01
bInterfaceClass:                   0x03  -> HID Interface Class
bInterfaceSubClass:                0x00
bInterfaceProtocol:                0x00
iInterface:                        0x00

          ===>HID Descriptor<===
bLength:                           0x09
bDescriptorType:                   0x21
bcdHID:                          0x0110
bCountryCode:                      0x00
bNumDescriptors:                   0x01
bDescriptorType:                   0x22 (Report Descriptor)
wDescriptorLength:               0x00A0

          ===>Endpoint Descriptor<===
bLength:                           0x07
bDescriptorType:                   0x05
bEndpointAddress:                  0x82  -> Direction: IN - EndpointID: 2
bmAttributes:                      0x03  -> Interrupt Transfer Type
wMaxPacketSize:                  0x0008
bInterval:                         0x0A
[Port3] 


ConnectionStatus:      NoDeviceConnected
[Port4] 


ConnectionStatus:      NoDeviceConnected
[Port2] 


ConnectionStatus:      NoDeviceConnected
