Starting kernel ...

Uncompressing Linux... done, booting the kernel.
[    0.000000] Booting Linux on physical CPU 0
[    0.000000] Initializing cgroup subsys cpu
[    0.000000] Linux version 3.4.61-00018-g77987d5 (root@pcz-pcz-2tlab-1.sasken.com) (gcc version 4.6.x-google 20120106 (prerelease)4
[    0.000000] CPU: ARMv7 Processor [411fc092] revision 2 (ARMv7), cr=10c5387d
[    0.000000] CPU: PIPT / VIPT nonaliasing data cache, VIPT aliasing instruction cache
[    0.000000] Machine: OMAP4 Blaze board
[    0.000000] Initialized persistent memory from a0000000-a01fffff
[    0.000000] android_display: setting lcd resolution to 1920*1080, bpp=4
[    0.000000] android_display: tiler1d 66355200
[    0.000000] android_display: setting fb0.vram to 8294400
[    0.000000] android_display: setting hdmi resolution to 1920*1080, bpp=4
[    0.000000] android_display: tiler1d 66355200
[    0.000000] android_display: setting fb1.vram to 16588800
[    0.000000] android_display: setting vram to 24883200
[    0.000000] Cannot detect omap type!
[    0.000000] Reserving 25165824 bytes SDRAM for VRAM
[    0.000000] cma: CMA: reserved 16 MiB at 96000000
[    0.000000] Memory policy: ECC disabled, Data cache writealloc
[    0.000000] OMAP4: Map 0x97600000 to 0xfe600000 for dram barrier
[    0.000000] OMAP4430 ES2.1
[    0.000000] PERCPU: Embedded 9 pages/cpu @c1857000 s12736 r8192 d15936 u36864
[    0.000000] Built 1 zonelists in Zone order, mobility grouping on.  Total pages: 168192
[    0.000000] Kernel command line: console=ttyO2,115200n8 androidboot.console=ttyO2 omap_wdt.timer_margin=30 vmalloc=496M omapfb.fb0
[    0.000000] PID hash table entries: 2048 (order: 1, 8192 bytes)
[    0.000000] Dentry cache hash table entries: 65536 (order: 6, 262144 bytes)
[    0.000000] Inode-cache hash table entries: 32768 (order: 5, 131072 bytes)
[    0.000000] Memory: 374MB 2MB 289MB = 665MB total
[    0.000000] Memory: 642164k/642164k available, 406412k reserved, 295936K highmem
[    0.000000] Virtual kernel memory layout:
[    0.000000]     vector  : 0xffff0000 - 0xffff1000   (   4 kB)
[    0.000000]     fixmap  : 0xfff00000 - 0xfffe0000   ( 896 kB)
[    0.000000]     vmalloc : 0xe0800000 - 0xff000000   ( 488 MB)
[    0.000000]     lowmem  : 0xc0000000 - 0xe0000000   ( 512 MB)
[    0.000000]     pkmap   : 0xbfe00000 - 0xc0000000   (   2 MB)
[    0.000000]     modules : 0xbf000000 - 0xbfe00000   (  14 MB)
[    0.000000]       .text : 0xc0008000 - 0xc08bb000   (8908 kB)
[    0.000000]       .init : 0xc08bb000 - 0xc09091c0   ( 313 kB)
[    0.000000]       .data : 0xc090a000 - 0xc0994470   ( 554 kB)
[    0.000000]        .bss : 0xc0994494 - 0xc0b0c768   (1505 kB)
[    0.000000] Preemptible hierarchical RCU implementation.
[    0.000000] NR_IRQS:602
[    0.000000] OMAP clockevent source: GPTIMER1 at 32768 Hz
[    0.000000] sched_clock: 32 bits at 32kHz, resolution 30517ns, wraps every 131071999ms
[    0.000274] Calibrating delay loop... 1194.24 BogoMIPS (lpj=4665344)
[    0.070312] pid_max: default: 32768 minimum: 301
[    0.070556] Security Framework initialized
[    0.070678] Mount-cache hash table entries: 512
[    0.072235] Initializing cgroup subsys debug
[    0.072265] Initializing cgroup subsys cpuacct
[    0.072296] Initializing cgroup subsys freezer
[    0.072296] Initializing cgroup subsys net_cls
[    0.072357] CPU: Testing write buffer coherency: ok
[    0.072662] CPU0: thread -1, cpu 0, socket 0, mpidr 80000000
[    0.072967] hw perfevents: enabled with ARMv7 Cortex-A9 PMU driver, 7 counters available
[    0.073120] Setting up static identity map for 0x8066a930 - 0x8066a988
[    0.073150] L310 cache controller enabled
[    0.073181] l2x0: 16 ways, CACHE_ID 0x410000c4, AUX_CTRL 0x7e470000, Cache size: 1048576 B
[    0.073699] generating sar_ram layout...
[    0.073974] sar ram layout created
[    0.151611] CPU1: Booted secondary processor
[    0.182312] CPU1: thread -1, cpu 1, socket 0, mpidr 80000001
[    0.182373] CPU1: Unknown IPI message 0x1
[    0.182403] Brought up 2 CPUs
[    0.182403] SMP: Total of 2 processors activated (2388.48 BogoMIPS).
[    0.192535] omap_hwmod: aess: _wait_target_disable failed
[    0.195312] omap_hwmod: dss_dispc: cannot be enabled (3)
[    0.198028] omap_hwmod: dss_dsi1: cannot be enabled (3)
[    0.200744] omap_hwmod: dss_dsi2: cannot be enabled (3)
[    0.203460] omap_hwmod: dss_hdmi: cannot be enabled (3)
[    0.206176] omap_hwmod: dss_rfbi: cannot be enabled (3)
[    0.208892] omap_hwmod: dss_venc: cannot be enabled (3)
[    0.212768] omap_hwmod: mcpdm: cannot be enabled (3)
[    0.214691] omap_device: cannot add global notifier for dev PM QoS
[    0.215362] dummy: 
[    0.216888] NET: Registered protocol family 16
[    0.232513] DMA: preallocated 256 KiB pool for atomic coherent allocations
[    0.233032] GPMC revision 6.0
[    0.235107] gpiochip_add: registered GPIOs 0 to 31 on device: gpio
[    0.235168] OMAP GPIO hardware version 0.1
[    0.235351] gpiochip_add: registered GPIOs 32 to 63 on device: gpio
[    0.235626] gpiochip_add: registered GPIOs 64 to 95 on device: gpio
[    0.235870] gpiochip_add: registered GPIOs 96 to 127 on device: gpio
[    0.236114] gpiochip_add: registered GPIOs 128 to 159 on device: gpio
[    0.236358] gpiochip_add: registered GPIOs 160 to 191 on device: gpio
[    0.237823] omap_mux_init: Add partition: #1: core, flags: 2
[    0.238983] omap_mux_init: Add partition: #2: wkup, flags: 2
[    0.247894] dmm dmm: initialized all PAT entries
[    0.249969] hw-breakpoint: found 5 (+1 reserved) breakpoint and 1 watchpoint registers.
[    0.249999] hw-breakpoint: maximum watchpoint size is 4 bytes.
[    0.254547]  omap-mcbsp.1: alias pad_fck already exists
[    0.254730]  omap-mcbsp.2: alias pad_fck already exists
[    0.254913]  omap-mcbsp.3: alias pad_fck already exists
[    0.255096]  omap-mcbsp.4: alias pad_fck already exists
[    0.255676] gcxxx_int failed. gcx hardware is not present
[    0.255859] OMAP DMA hardware revision 0.0
[    0.256622] emif emif.1: emif_probe: device configured with addr = e0984000 and IRQ142
[    0.256958] emif emif.2: emif_probe: device configured with addr = e0986000 and IRQ143
[    0.258819] SmartReflex Recalibration delay = 86400000ms
[    0.258819] SmartReflex Class 1.5 initialized
[    0.259277] Reprogramming LPDDR2 timings to 800000000 Hz
[    0.269073] bio: create slab <bio-0> at 0
[    0.269958] VBAT: 3750 mV 
[    0.271301] SCSI subsystem initialized
[    0.271667] usbcore: registered new interface driver usbfs
[    0.271789] usbcore: registered new interface driver hub
[    0.271942] usbcore: registered new device driver usb
[    0.273284] omap_i2c omap_i2c.1: bus 1 rev2.4.0 at 400 kHz
[    0.274475] twl_core: detected twl6030 rev.1 eepromrev.123
[    0.278015] twl 1-0048: PIH (irq 39) chaining IRQs 416..436
[    0.279327] VUSB: 3300 mV normal standby
[    0.994842] PC detected
[    0.994934] musb-omap2430 musb-omap2430: musb core is not yet ready
[    0.995269] twl6030_usb twl6030_usb: Initialized TWL6030 USB module
[    0.996612] V1V8: 1800 mV normal standby
[    0.997894] V2V1: 2100 mV normal standby
[    0.998748] VMMC: 1200 <--> 3000 mV at 1800 mV normal standby
[    0.999816] VPP: 1800 <--> 2500 mV at 1900 mV normal standby
[    1.000854] VUSIM: 1200 <--> 2900 mV at 1800 mV normal standby
[    1.002319] VCXIO: 1800 mV normal standby
[    1.002380] VCXIO: supplied by V2V1
[    1.004394] VDAC: 1800 mV normal standby
[    1.004455] VDAC: supplied by V2V1
[    1.005706] VAUX1_6030: 1000 <--> 3000 mV at 2800 mV normal standby
[    1.006774] VAUX2_6030: 1200 <--> 2800 mV at 1800 mV normal standby
[    1.007843] VAUX3_6030: 1000 <--> 3000 mV at 1200 mV normal standby
[    1.009033] VANA: 2100 mV normal standby
[    1.010040] CLK32KAUDIO: 
[    1.011260] SYSEN: 
[    1.012512] REGEN1: 
[    1.013488] CLK32KG: 
[    1.013702] twl6030: set (mod=0x0D reg=0x53 val=0x01): VCORE1 OFF=OFF SLEEP=OFF ACT=AUTO
[    1.013854] twl6030: set (mod=0x0D reg=0x59 val=0x01): VCORE2 OFF=OFF SLEEP=OFF ACT=AUTO
[    1.013977] twl6030: set (mod=0x0D reg=0x5f val=0x01): VCORE3 OFF=OFF SLEEP=OFF ACT=AUTO
[    1.014770] omap_i2c omap_i2c.2: bus 2 rev2.4.0 at 400 kHz
[    1.015289] omap_i2c omap_i2c.3: bus 3 rev2.4.0 at 400 kHz
[    1.016052] omap_i2c omap_i2c.4: bus 4 rev2.4.0 at 400 kHz
[    1.016876] Linux video capture interface: v2.00
[    1.016967] sr_init: No PMIC hook to init smartreflex
[    1.017761] omap-iommu omap-iommu.0: dsp registered
[    1.017852] omap-iommu omap-iommu.1: ipu registered
[    1.018218] Advanced Linux Sound Architecture Driver Version 1.0.25.
[    1.019104] Bluetooth: Core ver 2.16
[    1.019195] NET: Registered protocol family 31
[    1.019195] Bluetooth: HCI device and connection manager initialized
[    1.019226] Bluetooth: HCI socket layer initialized
[    1.019226] Bluetooth: L2CAP socket layer initialized
[    1.019287] Bluetooth: SCO socket layer initialized
[    1.021301] smartreflex smartreflex.0: omap_sr_probe: SmartReflex driver initialized
[    1.021881] smartreflex smartreflex.1: omap_sr_probe: SmartReflex driver initialized
[    1.022521] smartreflex smartreflex.2: omap_sr_probe: SmartReflex driver initialized
[    1.022552] Power Management for TI OMAP4XX/OMAP5XXX devices.
[    1.023071] omap4_pm_init: ############Added by siva################
[    1.023162] omap_opp_set_min_rate: Missing opp info for hwmod dsp_c0
[    1.023193] Forcing clock virt_dpll_dsp_ck to minimum rate 232750000
[    1.023223] omap_opp_set_min_rate: Missing opp info for hwmod hsi
[    1.023223] Forcing clock hsi_fck to minimum rate 96000000
[    1.023956] Switching to clocksource 32k_counter
[    1.046997] NET: Registered protocol family 2
[    1.047363] IP route cache hash table entries: 16384 (order: 4, 65536 bytes)
[    1.048187] TCP established hash table entries: 65536 (order: 7, 524288 bytes)
[    1.049530] TCP bind hash table entries: 65536 (order: 7, 786432 bytes)
[    1.050964] TCP: Hash tables configured (established 65536 bind 65536)
[    1.050994] TCP: reno registered
[    1.051025] UDP hash table entries: 256 (order: 1, 8192 bytes)
[    1.051055] UDP-Lite hash table entries: 256 (order: 1, 8192 bytes)
[    1.051452] NET: Registered protocol family 1
[    1.051971] RPC: Registered named UNIX socket transport module.
[    1.051971] RPC: Registered udp transport module.
[    1.052001] RPC: Registered tcp transport module.
[    1.052001] RPC: Registered tcp NFSv4.1 backchannel transport module.
[    1.052215] usbhs_omap usbhs_omap: ehci_logic_fck failed:-2
[    1.053436] Trying to unpack rootfs image as initramfs...
[    1.071044] sr_classp5_calib_work: smartreflex_core: Calibration complete: Voltage Nominal=1127000 Calib=987520 Dyn=1037520 OPP_m0
[    1.071105] sr_classp5_calib_work: smartreflex_mpu: Calibration complete: Voltage Nominal=1200000 Calib=1025500 Dyn=1075500 OPP_m0
[    1.071197] sr_classp5_calib_work: smartreflex_iva: Calibration complete: Voltage Nominal=950000 Calib=835600 Dyn=885600 OPP_marg0
[    1.084045] Freeing initrd memory: 316K
[    1.084381] NetWinder Floating Point Emulator V0.97 (double precision)
[    1.085479]  omap-rproc.1: alias fck already exists
[    1.086303] persistent_ram: uncorrectable error in header
[    1.086334] persistent_ram: no valid data in buffer (sig = 0x80c29400)
[    1.115722] console [ram-1] enabled
[    1.292907] highmem bounce pool size: 64 pages
[    1.294586] fuse init (API version 7.18)
[    1.294952] msgmni has been set to 708
[    1.297576] io scheduler noop registered
[    1.297729] io scheduler deadline registered
[    1.298034] io scheduler cfq registered (default)
[    1.299835] OMAP DSS rev 4.0
[    1.323577] Keyboard driver not present
[    1.324157] omapdss DSI error: can't get regulator for panel
[    1.336730] omapdss DSI error: can't get regulator for panel
[    1.353240] dsscomp: initializing.
[    1.353485] misc dsscomp: found 4 displays and 4 overlays, WB overlay 1
[    1.354858] omap_uart.1: ttyO1 at MMIO 0x4806c000 (irq = 105) is a OMAP UART1
[    1.355682] omap_uart.2: ttyO2 at MMIO 0x48020000 (irq = 106) is a OMAP UART2
[    2.517333] console [ttyO2] enabled
[    2.521728] omap_uart.3: ttyO3 at MMIO 0x4806e000 (irq = 102) is a OMAP UART3
[    2.530242] [drm] Initialized drm 1.1.0 20060810
[    2.535583] omap_ion_probe: adding heap secure_input of type 2 with ba300000@5a00000
[    2.544128] omap_ion_probe: adding heap tiler of type 4 with b4300000@6000000
[    2.551910] omap_ion_probe: adding heap nonsecure_tiler of type 4 with a0200000@2000000
[    2.560729] omap_ion_probe: adding heap system of type 0 with 0@0
[    2.567504] omap_ion_probe: adding heap tiler_reservation of type 5 with 0@0
[    2.584350] brd: module loaded
[    2.592468] loop: module loaded
[    2.596343] AK8975 compass driver: init
[    2.611755] tps6130x 1-0033: tps6130x_probe: Revision 5
[    2.618164] VOUT: 4075 <--> 4950 mV at 4950 mV normal standby
[    2.627960] mtdoops: mtd device (mtddev=name/number) must be supplied
[    2.636077] omap2_mcspi omap2_mcspi.1: master is unqueued, this is deprecated
[    2.644287] omap2_mcspi omap2_mcspi.2: master is unqueued, this is deprecated
[    2.652557] omap2_mcspi omap2_mcspi.3: master is unqueued, this is deprecated
[    2.660827] omap2_mcspi omap2_mcspi.4: master is unqueued, this is deprecated
[    2.668975] tun: Universal TUN/TAP device driver, 1.6
[    2.674621] tun: (C) 1999-2004 Max Krasnyansky <maxk@qualcomm.com>
[    2.682067] usbcore: registered new interface driver asix
[    2.688201] usbcore: registered new interface driver cdc_ether
[    2.694641] usbcore: registered new interface driver smsc95xx
[    2.701080] usbcore: registered new interface driver net1080
[    2.707336] usbcore: registered new interface driver cdc_subset
[    2.713989] usbcore: registered new interface driver zaurus
[    2.720184] usbcore: registered new interface driver cdc_ncm
[    2.726898] ehci_hcd: USB 2.0 'Enhanced' Host Controller (EHCI) Driver
[    3.740356] ehci: omap_ehci_ulpi_write: Error
[    3.745483] ehci-omap ehci-omap.0: OMAP-EHCI Host Controller
[    3.752044] ehci-omap ehci-omap.0: new USB bus registered, assigned bus number 1
[    3.763305] ehci-omap ehci-omap.0: irq 109, io mem 0x4a064c00
[    3.781890] ehci-omap ehci-omap.0: USB 2.0 started, EHCI 1.00
[    3.788513] usb usb1: New USB device found, idVendor=1d6b, idProduct=0002
[    3.795928] usb usb1: New USB device strings: Mfr=3, Product=2, SerialNumber=1
[    3.803863] usb usb1: Product: OMAP-EHCI Host Controller
[    3.809692] usb usb1: Manufacturer: Linux 3.4.61-00018-g77987d5 ehci_hcd
[    3.817077] usb usb1: SerialNumber: ehci-omap.0
[    3.822692] hub 1-0:1.0: USB hub found
[    3.826965] hub 1-0:1.0: 3 ports detected
[    3.860198] usbcore: registered new interface driver cdc_wdm
[    3.866485] Initializing USB Mass Storage driver...
[    3.872039] usbcore: registered new interface driver usb-storage
[    3.878692] USB Mass Storage support registered.
[    3.883880] usbcore: registered new interface driver libusual
[    3.890319] usbcore: registered new interface driver usbtest
[    3.896514] musb-hdrc: version 6.0, ?dma?, otg (peripheral+host)
[    4.103637] musb-hdrc musb-hdrc: USB OTG mode controller at e0b16000 using DMA, IRQ 124
[    4.112884] file system registered
[    4.118347]  gadget: Mass Storage Function, version: 2009/09/11
[    4.124786]  gadget: Number of LUNs=1
[    4.128845]  lun0: LUN: removable file: (no medium)
[    4.134613]  gadget: android_usb ready
[    4.338287] musb-hdrc musb-hdrc: MUSB HDRC host driver
[    4.344238] musb-hdrc musb-hdrc: new USB bus registered, assigned bus number 2
[    4.352264] usb usb2: New USB device found, idVendor=1d6b, idProduct=0002
[    4.359741] usb usb2: New USB device strings: Mfr=3, Product=2, SerialNumber=1
[    4.367706] usb usb2: Product: MUSB HDRC host driver
[    4.373138] usb usb2: Manufacturer: Linux 3.4.61-00018-g77987d5 musb-hcd
[    4.380523] usb usb2: SerialNumber: musb-hdrc
[    4.385894] hub 2-0:1.0: USB hub found
[    4.390045] hub 2-0:1.0: 1 port detected
[    4.430572] mousedev: PS/2 mouse device common for all mice
[    4.437469] input: omap4-keypad as /devices/platform/omap4-keypad/input/input0
[    4.452789] tm12xx_ts: Synaptic TM12xx Touchscreen Driver found man id 1 (1)
[    4.466064] tm12xx_ts 2-004b: resetting device (reg 0x62)
[    4.609374] tm12xx_ts 2-004b: no button capabilities found
[    4.615753] tm12xx_ts: Synaptic TM12xx Touchscreen Driver found man id 1 (1)
[    4.624176] tm12xx_ts: product ID: TM1217 family:1 fw:9
[    4.630218] input: syn_tm12xx_ts_1 as /devices/platform/omap_i2c.2/i2c-2/2-004b/input/input1
[    4.641021] tm12xx_ts 2-004b: device status: 0x0, no error
[    4.650726] tm12xx_ts 3-004b: resetting device (reg 0x62)
[    4.805358] tm12xx_ts 3-004b: no button capabilities found
[    4.817993] CMA3000 Acclerometer : Revision 10
[    4.823516] tm12xx_ts: product ID: TM1217 family:1 fw:9
[    4.829559] input: syn_tm12xx_ts_2 as /devices/platform/omap_i2c.3/i2c-3/3-004b/input/input2
[    4.840087] tm12xx_ts 3-004b: device status: 0x0, no error
[    4.875885] input: cma3000-acclerometer as /devices/virtual/input/input3
[    4.923065] twl6030_pwrbutton_probe: Enter
[    4.928039] input: twl6030_pwrbutton as /devices/platform/omap_i2c.1/i2c-1/1-0049/twl6030_pwrbutton/input/input4
[    4.940643] bh1780 3-0029: Ambient Light Sensor, Rev : 1
[    4.946685] input: bh1780gli as /devices/virtual/input/input5
[    4.954284] bmp085 4-0077: BMP085 ver. 1.0 found.
[    4.959655] input: bmp085 as /devices/virtual/input/input6
[    4.965820] bmp085 4-0077: Succesfully initialized bmp085!
[    4.972595] input: hmc5843 as /devices/virtual/input/input7
[    4.979034] sfh7741_probe: Proximity sensor
[    4.983978] input: sfh7741 as /devices/platform/sfh7741.1/input/input8
[    4.992736] twl_rtc twl_rtc: Enabling TWL-RTC
[    5.000885] twl_rtc twl_rtc: rtc core: registered twl_rtc as rtc0
[    5.039764] i2c /dev entries driver
[    5.044403] usbcore: registered new interface driver uvcvideo
[    5.050689] USB Video Class driver (1.1.1)
[    5.055389] Driver for 1-wire Dallas network protocol.
[    5.173187] twl6030_bci twl6030_bci: Battery Voltage at Bootup is 3681 mV
[    5.213439] omap-bandgap omap-bandgap: failed to request fclock reference
[    5.221405] omap-bandgap: probe of omap-bandgap failed with error 1
[    5.230133] omap_wdt: OMAP Watchdog Timer Rev 0x00: initial timeout 30 sec
[    5.238189] device-mapper: ioctl: 4.22.0-ioctl (2011-10-19) initialised: dm-devel@redhat.com
[    5.249633] cpuidle: using governor ladder
[    5.254516] cpuidle: using governor menu
[    5.271881] omap4430_sdp_display_probe:Enter
[    5.277160] omap4430_sdp_display_probe:Exit
[    5.282104] omap4430_keypad_led_probe:Enter
[    5.287322] omap4430_keypad_led_probe:Exit
[    5.292205] usbcore: registered new interface driver usbhid
[    5.298309] usbhid: USB HID core driver
[    5.302886] ashmem: initialized
[    5.306457] logger: created 256K log 'log_main'
[    5.311584] logger: created 256K log 'log_events'
[    5.317840] logger: created 256K log 'log_radio'
[    5.324951] logger: created 256K log 'log_system'
[    5.330413] thermal_get_slope:Getting slope is not supported for domain cpu
[    5.338104] thermal_get_offset:Getting offset is not supported for domain cpu
[    5.345886] omap_governor_init: domain cpu slope -22 const -22
[    5.352386] thermal_get_slope:Getting slope is not supported for domain gpu
[    5.359985] thermal_get_offset:Getting offset is not supported for domain gpu
[    5.367828] omap_governor_init: domain gpu slope -22 const -22
[    5.374786] duty_cycle_apply_cooling: not throttling
[    5.380340] duty_cycle_apply_cooling: not throttling
[    5.389190] rproc remoteproc0: ipu_c0 is available
[    5.394500] rproc remoteproc0: Note: remoteproc is still under development and considered experimental.
[    5.404724] rproc remoteproc0: THE BINARY FORMAT IS NOT YET FINALIZED, and backward compatibility isn't yet guaranteed.
[    5.416809] OMAP HSI: HSI driver version 0.4.4
[    5.422149] usbcore: registered new interface driver snd-usb-audio
[    5.432281] aess aess: ABE Firmware version 9560
[    5.478454] mmc0: new high speed MMC card at address 0001
[    5.485137] mmcblk0: mmc0:0001 SEM08G 7.39 GiB 
[    5.491638] asoc: snd-soc-dummy-dai <-> MultiMedia1 mapping ok
[    5.498016] mmcblk0boot0: mmc0:0001 SEM08G partition 1 1.00 MiB
[    5.506042] asoc: snd-soc-dummy-dai <-> MultiMedia2 mapping ok
[    5.512603] mmcblk0boot1: mmc0:0001 SEM08G partition 2 1.00 MiB
[    5.522155] asoc: snd-soc-dummy-dai <-> Voice mapping ok
[    5.529632] asoc: snd-soc-dummy-dai <-> Tones mapping ok
[    5.537048] asoc: snd-soc-dummy-dai <-> Vibra mapping ok
[    5.543365] asoc: snd-soc-dummy-dai <-> MODEM mapping ok
[    5.549255] Alternate GPT is invalid, using primary GPT.
[    5.555114]  mmcblk0: p1 p2 p3 p4 p5 p6 p7 p8 p9 p10
[    5.560821] asoc: snd-soc-dummy-dai <-> MultiMedia1 LP mapping ok
[    5.569396] asoc: snd-soc-dummy-dai <-> omap-mcbsp.2 mapping ok
[    5.577545]  mmcblk0boot1: unknown partition table
[    5.584320]  mmcblk0boot0: unknown partition table
[    5.584686] asoc: twl6040-legacy <-> mcpdm-legacy mapping ok
[    5.597656] asoc: dit-hifi <-> mcasp-legacy mapping ok
[    5.604827] asoc: dmic-hifi <-> omap-dmic mapping ok
[    5.610839] ##################Added by siva###############sound/soc/omap/omap-abe-twl6040.c:597
[    5.620452] asoc: twl6040-dl1 <-> mcpdm-dl1 mapping ok
[    5.626617] asoc: twl6040-ul <-> mcpdm-ul1 mapping ok
[    5.632415] asoc: twl6040-dl2 <-> mcpdm-dl2 mapping ok
[    5.638275] asoc: twl6040-vib <-> mcpdm-vib mapping ok
[    5.641296] sr_classp5_calib_work: smartreflex_mpu: Calibration complete: Voltage Nominal=1388000 Calib=1190080 Dyn=1240080 OPP_m0
[    5.658813] asoc: snd-soc-dummy-dai <-> omap-mcbsp.1 mapping ok
[    5.665557] asoc: snd-soc-dummy-dai <-> omap-mcbsp.1 mapping ok
[    5.672332] asoc: snd-soc-dummy-dai <-> omap-mcbsp.2 mapping ok
[    5.679016] asoc: snd-soc-dummy-dai <-> omap-mcbsp.2 mapping ok
[    5.685791] asoc: snd-soc-dummy-dai <-> omap-mcbsp.2 mapping ok
[    5.692474] asoc: dmic-hifi <-> omap-dmic-abe-dai-0 mapping ok
[    5.699218] asoc: dmic-hifi <-> omap-dmic-abe-dai-1 mapping ok
[    5.705841] asoc: dmic-hifi <-> omap-dmic-abe-dai-2 mapping ok
[    5.712524] asoc: snd-soc-dummy-dai <-> omap-abe-vxrec-dai mapping ok
[    5.719787] asoc: snd-soc-dummy-dai <-> omap-abe-echo-dai mapping ok
[    5.727691] input: SDP4430 Headset Jack as /devices/platform/omap-abe-twl6040/sound/card0/input9
[    5.741027] asoc: omap-hdmi-hifi <-> omap-hdmi-audio-dai mapping ok
[    5.748779] oprofile: using arm/armv7-ca9
[    5.753417] GACT probability NOT on
[    5.757232] Mirror/redirect action on
[    5.761230] u32 classifier
[    5.764282]     Actions configured
[    5.768005] Netfilter messages via NETLINK v0.30.
[    5.773193] nf_conntrack version 0.5.0 (10294 buckets, 41176 max)
[    5.780242] ctnetlink v0.93: registering with nfnetlink.
[    5.786163] NF_TPROXY: Transparent proxy support initialized, version 4.1.0
[    5.793823] NF_TPROXY: Copyright (c) 2006-2007 BalaBit IT Ltd.
[    5.800231] xt_time: kernel timezone is -0000
[    5.805511] ip_tables: (C) 2000-2006 Netfilter Core Team
[    5.811523] arp_tables: (C) 2002 David S. Miller
[    5.816741] TCP: cubic registered
[    5.820404] Initializing XFRM netlink socket
[    5.825256] NET: Registered protocol family 10
[    5.831115] Mobile IPv6
[    5.833923] ip6_tables: (C) 2000-2006 Netfilter Core Team
[    5.840057] IPv6 over IPv4 tunneling driver
[    5.845825] NET: Registered protocol family 17
[    5.850708] NET: Registered protocol family 15
[    5.855743] Bridge firewalling registered
[    5.860260] Bluetooth: RFCOMM TTY layer initialized
[    5.865570] Bluetooth: RFCOMM socket layer initialized
[    5.871246] Bluetooth: RFCOMM ver 1.11
[    5.875335] Bluetooth: BNEP (Ethernet Emulation) ver 1.3
[    5.881164] Bluetooth: BNEP filters: protocol multicast
[    5.886840] Bluetooth: HIDP (Human Interface Emulation) ver 1.2
[    5.893493] NET: Registered protocol family 35
[    5.898498] NET: Registered protocol family 37
[    5.903503] safe_suspend_freq_set: suspend will take place at frequency 600000000
[    5.911804] VFP support v0.3: implementor 41 architecture 3 part 30 variant 9 rev 1
[    5.920379] ThumbEE CPU extension supported.
[    5.925140] Registering SWP/SWPB emulation handler
[    5.939422] clock: disabling unused clocks to save power
[    6.630218] cannot apply mgr(lcd) on inactive device
[    6.636047] cannot apply mgr(lcd) on inactive device
[    6.641937] omapfb omapfb: failed to apply dispc config
[    6.647888] cannot apply mgr(tv) on inactive device
[    6.653686] omapfb omapfb: failed to apply dispc config
[    6.659423] cannot apply mgr(lcd2) on inactive device
[    6.664978] omapfb omapfb: failed to apply dispc config
[    6.813232] taal display0: taal panel revision e3.84.7d
[    6.927551] gpio-keys gpio-keys: Failed to request GPIO 184, error -16
[    6.935028] gpio-keys: probe of gpio-keys failed with error -16
[    6.943695] twl_rtc twl_rtc: setting system clock to 2000-01-01 02:33:34 UTC (946694014)
[    6.952972] ALSA device list:
[    6.956420]   #0: SDP4430
[    6.959350]   #1: OMAPHDMI
[    6.962982] Freeing init memory: 312K
[    7.814331] init: could not import file 'init.modem.rc' from '/init.omap4blazeboard.rc'
[    7.823333] init (1): /proc/1/oom_adj is deprecated, please use /proc/1/oom_score_adj instead.
[    7.835784] init: invalid uid 'fmradio'
[    7.976531] init: /dev/hw_random not found
[    7.981689] init: could not open /dev/keychord
[    8.000793] sr_classp5_calib_work: smartreflex_core: Calibration complete: Voltage Nominal=962000 Calib=822940 Dyn=872940 OPP_mar0
[    8.015991] sr_classp5_calib_work: smartreflex_mpu: Calibration complete: Voltage Nominal=1025000 Calib=898900 Dyn=948900 OPP_mar0
[    8.088134] EXT4-fs (mmcblk0p8): mounted filesystem with ordered data mode. Opts: (null)
[    8.107391] EXT4-fs (mmcblk0p4): mounted filesystem with ordered data mode. Opts: (null)
[    8.117401] EXT4-fs (mmcblk0p9): VFS: Can't find ext4 filesystem
[    8.157257] fs_mgr: Running /system/bin/e2fsck on /dev/block/platform/omap/omap_hsmmc.1/by-name/cache
[    8.463012] e2fsck: e2fsck 1.41.14 (22-Dec-2010)
[    8.468139] e2fsck: /system/bin/e2fsck: Superblock invalid, trying backup blocks...
[    8.480621] e2fsck: /system/bin/e2fsck: Bad magic number in super-block while trying to open /dev/block/platform/omap/omap_hsmmc.e
[    8.498809] e2fsck: 
[    8.501342] e2fsck: The superblock could not be read or does not describe a correct ext2
[    8.514129] e2fsck: filesystem.  If the device is valid and it really contains an ext2
[    8.522766] e2fsck: filesystem (and not swap or ufs or something else), then the superblock
[    8.535949] e2fsck: is corrupt, and you might try running e2fsck with an alternate superblock:
[    8.549499] e2fsck:     e2fsck -b 8193 <device>
[    8.554443] e2fsck: 
[    8.556884] e2fsck: e2fsck terminated by exit(8)
[    8.606262] EXT4-fs (mmcblk0p9): VFS: Can't find ext4 filesystem
[    8.606353] rproc remoteproc0: skipping power up until last virtio device ipu_c0
[    8.606933] virtio_rpmsg_bus virtio0: rpmsg host is online
[    8.606964] rproc remoteproc0: registered virtio0 (type 7)
[    8.607208] rproc remoteproc0: powering up ipu_c0
[    8.655059] rproc remoteproc0: Booting fw image ducati-m3-core0.xem3, size 6684059
[    8.680541] fs_mgr: Cannot mount filesystem on /dev/block/platform/omap/omap_hsmmc.1/by-name/cache at /cache
[    8.691375] init: fs_mgr_mount_all returned an error
[    8.813293] EXT4-fs (mmcblk0p10): recovery complete
[    8.820190] EXT4-fs (mmcblk0p10): mounted filesystem with ordered data mode. Opts: nomblk_io_submit
[    8.831115] EXT4-fs (mmcblk0p9): VFS: Can't find ext4 filesystem
[    8.898864] init: /dev/hw_random not found
[    8.916290] init: cannot find '/system/bin/setup_fs', disabling 'setup_fs'
[    8.925384] init: cannot find '/system/bin/uim-sysfs', disabling 'uim'
[    8.927124] healthd: wakealarm_init: timerfd_create failed
[    8.928436] healthd: BatteryPresentPath not found
[    8.928436] healthd: BatteryTechnologyPath not found
[    8.928466] binder: 90:90 transaction failed 29189, size 0-0
[    8.962677] init: cannot find '/system/bin/shm_service', disabling 'shm_service'
[    9.026702] init: cannot find '/system/etc/install-recovery.sh', disabling 'flash_recovery'
[    9.039703] init: cannot find '/system/bin/arxd', disabling 'arxd'
[    9.158966] omap-iommu omap-iommu.1: ipu: version 2.1
[    9.170227] rproc remoteproc0: remote processor ipu_c0 is now up
[    9.178253] virtio_rpmsg_bus virtio1: rpmsg host is online
[    9.184265] rproc remoteproc0: registered virtio1 (type 7)
[    9.193389] omap-rproc omap-rproc.1: received echo reply from ipu_c0
[    9.204742] virtio_rpmsg_bus virtio0: creating channel rpmsg-client-sample addr 0x32
[    9.216247] virtio_rpmsg_bus virtio0: creating channel rpmsg-client-sample addr 0x33
[    9.219573] init: property 'sys.powerctl' doesn't exist while expanding '${sys.powerctl}'
[    9.219573] init: powerctl: cannot expand '${sys.powerctl}'
[    9.219604] init: property 'sys.sysctl.extra_free_kbytes' doesn't exist while expanding '${sys.sysctl.extra_free_kbytes}'
[    9.219604] init: cannot expand '${sys.sysctl.extra_free_kbytes}' while writing to '/proc/sys/vm/extra_free_kbytes'
[    9.220703] android_usb: already disabled
[    9.233337] adb_open
[    9.233337] mtp_bind_config
[    9.233398] adb_bind_config
[    9.267517] virtio_rpmsg_bus virtio1: creating channel rpmsg-omx1 addr 0x3c
[    9.268157] rpmsg_omx rpmsg-omx1: new OMX connection srv channel: 1024 -> 60!
[    9.268280] virtio_rpmsg_bus virtio1: creating channel omaprpc addr 0x3b
[    9.300323] virtio_rpmsg_bus virtio0: creating channel rpmsg-omx0 addr 0x3c
[    9.308441] rpmsg_omx rpmsg-omx0: new OMX connection srv channel: 1024 -> 60!
[    9.390930] PVR: PVRCore_Init
[    9.394775] PVR: LinuxMMInit: Maximum page pool size: 10800
[    9.401092] PVR: PVRSRVDriverProbe(pDevice=d70e7600)
[    9.406524] PVR: SGX register base: 0x56000000
[    9.411499] PVR: SGX register size: 65535
[    9.415893] PVR: SGX IRQ: 53
[    9.419464] PVR: EnableSystemClocks: Enabling System Clocks
[    9.426116] PVR: PVRCore_Init: major device 247
shell@blaze:/ $ [    9.523803] android_work: sent uevent USB_STATE=CONNECTED
[    9.524536] fs_mgr: Cannot open file /fstab.omap4blazeboard
[    9.538787] android_work: sent uevent USB_STATE=DISCONNECTED
[    9.641754] PVR: Installing MISR with cookie bf0437a4
[    9.648834] PVR: Installing device LISR SGX ISR on IRQ 53 with cookie d5a8c9c0
[    9.656951] android_work: sent uevent USB_STATE=CONNECTED
[    9.663299] PVR: SysFinalise: Version string: SGX revision = 1.2.0
[    9.670288] omaplfbOMAPLFBInit: Blitsville gc2d not present, blits disabled
[    9.677978]  gadget: high-speed config #1: android
[    9.683502] omaplfb: OMAPLFBInitFBDev: Device 2: invalid framebuffer size
[    9.691070] android_work: sent uevent USB_STATE=CONFIGURED
[    9.708862] EXT4-fs (mmcblk0p8): re-mounted. Opts: (null)
[    9.766174] EXT4-fs (mmcblk0p8): re-mounted. Opts: (null)
[   10.396148] request_suspend_state: wakeup (3->0) at 10387725954 (2000-01-01 02:33:37.947479312 UTC)
[   10.409759] init: untracked pid 194 exited
[   19.096374] request_suspend_state: wakeup (0->0) at 19087921266 (2000-01-01 02:33:46.647674624 UTC)

