Capture from COM4:

========================================

/etc/init.d/matrix-gui-e stop
Stopping Matrix GUI application.
root@dm814x-evm:~# /etc/init.d/pvr-init stop
Stopping PVR
root@dm814x-evm:~# lsmod
Module                  Size  Used by
tlc59108                1545  0 
ti81xxhdmi             17685  0 
ti81xxfb               21979  0 
vpss                   74936  2 ti81xxhdmi,ti81xxfb
syslink              1133911  0 
ipv6                  214095  14 
root@dm814x-evm:~# insmod tvp7002.ko
insmod: can't read 'tvp7002.ko': No such file or directory
root@dm814x-evm:~# find . -iname tvp7002.ko
root@dm814x-evm:~# find / -iname tvp7002.ko
/lib/modules/2.6.37/kernel/drivers/media/video/tvp7002.ko
/media/mmcblk0p2/lib/modules/2.6.37/kernel/drivers/media/video/tvp7002.ko
root@dm814x-evm:~# insmod /lib/modules/2.6.37/kernel/drivers/media/video/tvp7002
.ko
root@dm814x-evm:~# find / -iname ti81xxvin.ko
/lib/modules/2.6.37/kernel/drivers/media/video/ti81xx/ti81xxvin.ko
/media/mmcblk0p2/lib/modules/2.6.37/kernel/drivers/media/video/ti81xx/ti81xxvin.ko

root@dm814x-evm:~# insmod /lib/modules/2.6.37/kernel/drivers/media/video/ti81xx/
ti81xxvin.ko
tvp7002 3-005d: tvp7002 found @ 0x5d (OMAP I2C adapter)
omap_i2c omap_i2c.3: controller timed out
omap_i2c omap_i2c.3: controller timed out
omap_i2c omap_i2c.3: controller timed out
omap_i2c omap_i2c.3: controller timed out
omap_i2c omap_i2c.3: controller timed out
tvp7002 3-005d: TVP7002 read error -110
tvp7002: probe of 3-005d failed with error -110
ti81xxvin ti81xxvin: Error registering v4l2 subdevice
root@dm814x-evm:~# lsmod
Module                  Size  Used by
ti81xxvin              20591  0 
tvp7002                 6429  0 
tlc59108                1545  0 
ti81xxhdmi             17685  0 
ti81xxfb               21979  0 
vpss                   74936  3 ti81xxvin,ti81xxhdmi,ti81xxfb
syslink              1133911  0 
ipv6                  214095  14 
root@dm814x-evm:~# find / -ina, me load-hd-v4l2-firmware.sh
/media/mmcblk0p2/usr/share/ti/ti-media-controller-utils/load-hd-v4l2-firmware.sh
/usr/share/ti/ti-media-controller-utils/load-hd-v4l2-firmware.sh
root@dm814x-evm:~# cd /usr/share/ti/ti-media-controller-utils
root@dm814x-evm:/usr/share/ti/ti-media-controller-utils# ./load-hd-v4l2-firmware
.sh
Usage: /etc/init.d/load-hd-v4l2-firmware.sh {start|stop}
root@dm814x-evm:/usr/share/ti/ti-media-controller-utils# load-hd-v4l2-firmware.s
h start
-sh: load-hd-v4l2-firmware.sh: not found
root@dm814x-evm:/usr/share/ti/ti-media-controller-utils# ./load-hd-v4l2-firmware
.sh start
Loading HDVICP2 Firmware
DM814X prcm_config_app version: 2.0.0.1
Doing PRCM settings...
	PRCM for IVHD0 is in Progress, Please wait.....  
			BW Phy Addr : 0x48180600 Data : 0x00000102
			AW Phy Addr : 0x48180600 Data : 0x00000102
			Phy Addr : 0x48180c04 Data : 0x00000037
			BW Phy Addr : 0x48180620 Data : 0x00000002
			AW Phy Addr : 0x48180620 Data : 0x00000002
			BW Phy Addr : 0x48180624 Data : 0x00000002
			AW Phy Addr : 0x48180624 Data : 0x00000002
			Phy Addr : 0x48180600 Data : 0x00000102
			BW Phy Addr : 0x48180c10 Data : 0x00000000
			AW Phy Addr : 0x48180c10 Data : 0x00000003
			Phy Addr : 0x48180c14 Data : 0x00000007
			BW Phy Addr : 0x58088000 Data : 0xeafffffe
			AW Phy Addr : 0x58088000 Data : 0xeafffffe
			BW Phy Addr : 0x58098000 Data : 0xeafffffe
			AW Phy Addr : 0x58098000 Data : 0xeafffffe
			BW Phy Addr : 0x48180c10 Data : 0x00000003
			AW Phy Addr : 0x48180c10 Data : 0x00000000
			Phy Addr : 0x48180c14 Data : 0x00000007
	PRCM for IVHD0 is Done Successfully  
PRCM Initialization completed 
FIRMWARE: I2cInit will be done by M3
FIRMWARE: Memory map bin file not passed
Usage : firmware_loader <Processor Id> <Location of Firmware> <start|stop> [-mmap <memory_map_file>] [-i2c <0|1>]
===Mandatory arguments=== 
<Processor Id>         0: DSP, 1: Video-M3, 2: Vpss-M3 
<Location of Firmware> firmware binary file 
<start|stop>           to start/stop the firmware 
===Optional arguments=== 
-mmap                  input memory map bin file name 
-i2c                   0: i2c init not done by M3, 1(default): i2c init done by M3 
FIRMWARE: isI2cInitRequiredOnM3: 1
FIRMWARE: Default memory configuration is used
Firmware Loader debugging not configured
Default FL_DEBUG: warning
Allowed FL_DEBUG levels: error, warning, info, debug, log
MemCfg: DCMM (Dynamically Configurable Memory Map) Version :  2.1.2.1
FIRMWARE: 1 start Successful
Loading HDVPSS (V4L2) Firmware 
FIRMWARE: Memory map bin file not passed
Usage : firmware_loader <Processor Id> <Location of Firmware> <start|stop> [-mmap <memory_map_file>] [-i2c <0|1>]
===Mandatory arguments=== 
<Processor Id>         0: DSP, 1: Video-M3, 2: Vpss-M3 
<Location of Firmware> firmware binary file 
<start|stop>           to start/stop the firmware 
===Optional arguments=== 
-mmap                  input memory map bin file name 
-i2c                   0: i2c init not done by M3, 1(default): i2c init done by M3 
FIRMWARE: isI2cInitRequiredOnM3: 0
FIRMWARE: Default memory configuration is used
Firmware Loader debugging not configured
Default FL_DEBUG: warning
Allowed FL_DEBUG levels: error, warning, info, debug, log
MemCfg: DCMM (Dynamically Configurable Memory Map) Version :  2.1.2.1
FIRMWARE: 2 start Successful
Configuring fb0 to LCD
VPSS_FVID2: contrl event 0x1004001a timeout
VPSS_DCTRL: failed to get venc info.

>>SyStem Hanged. Hence did a Restart <<
U-Boot 2010.06 (Dec 09 2011 - 17:20:03)

TI8148-GP rev 2.1

ARM clk: 600MHz
DDR clk: 400MHz

I2C:   ready
DRAM:  2 GiB
NAND:  HW ECC Hamming Code selected
256 MiB
                          .:;rrr;;.                   
                    ,5#@@@@#####@@@@@@#2,             
                 ,A@@@hi;;;r5;;;;r;rrSG@@@A,          
               r@@#i;:;s222hG;rrsrrrrrr;ri#@@r        
             :@@hr:r;SG3ssrr2r;rrsrsrsrsrr;rh@@:      
            B@H;;rr;3Hs;rrr;sr;;rrsrsrsrsrsr;;H@B     
           @@s:rrs;5#;;rrrr;r#@H:;;rrsrsrsrsrr:s@@    
          @@;;srs&X#9;r;r;;,2@@@rrr:;;rrsrsrsrr;;@@   
         @@;;rrsrrs@MB#@@@@@###@@@@@@#rsrsrsrsrr;;@@  
        G@r;rrsrsr;#X;SX25Ss#@@#M@#9H9rrsrsrsrsrs;r@G 
        @9:srsrsrs;2@;:;;:.X@@@@@H::;rrsrsrsrsrsrr:3@ 
       X@;rrsrsrsrr;XAi;;:&@@#@Bs:rrsrsrsrsrsrsrsrr;@X
       @#;rsrsrsrsrr;r2ir@@@###::rrsrsrsrsrsrsrsrsr:@@
       @A:rrsrsrsrr;:2@29@@M@@@;:;rrrrsrsrsrsrsrsrs;H@
       @&;rsrsrsrr;A@@@@@@###@@@s::;:;;rrsrsrsrsrsr;G@
       @#:rrsrsrsr;G@5Hr25@@@#@@@#9XG9s:rrrrsrsrsrs:#@
       M@;rsrsrsrs;r@&#;::S@@@@@@@M@@@@Grr:;rsrsrsr;@#
       :@s;rsrsrsrr:M#Msrr;;&#@@@@@@@@@@H@@5;rsrsr;s@,
        @@:rrsrsrsr;S@rrrsr;:;r3MH@@#@M5,S@@irrsrr:@@ 
         @A:rrsrsrsrrrrrsrsrrr;::;@##@r:;rH@h;srr:H@  
         ;@9:rrsrsrsrrrsrsrsrsr;,S@Hi@i:;s;MX;rr:h@;  
          r@B:rrrrsrsrsrsrsrr;;sA@#i,i@h;r;S5;r:H@r   
           ,@@r;rrrsrsrsrsrr;2BM3r:;r:G@:rrr;;r@@,    
             B@Mr;rrrrsrsrsr@@S;;;rrr:5M;rr;rM@H      
              .@@@i;;rrrrsrs2i;rrrrr;r@M:;i@@@.       
                .A@@#5r;;;r;;;rrr;r:r#AsM@@H.         
                   ;&@@@@MhXS5i5SX9B@@@@G;            
                       :ihM#@@@@@##hs,                

MMC:   OMAP SD/MMC: 0
Net:   Detected MACID:40:5f:c2:6d:f:29
cpsw
Hit any key to stop autoboot:  4  3  2  1  0 
link up on port 0, speed 1000, full duplex
BOOTP broadcast 1
BOOTP broadcast 2
DHCP client bound to address 10.143.25.248
link up on port 0, speed 1000, full duplex
Using cpsw device
TFTP from server 10.143.25.77; our IP address is 10.143.25.248
Filename 'uImage-dm814x-evm.bin'.
Load address: 0x81000000
Loading: *T #################################################################
	 #################################################################
	 #################################################################
	 #################################################################
	 #################################################################
	 #################################################################
	 #################################################################
	 #################################################################
	 ###########################
done
Bytes transferred = 2796444 (2aab9c hex)
## Booting kernel from Legacy Image at 81000000 ...
   Image Name:   Arago/2.6.37-psp04.04.00.01/dm81
   Image Type:   ARM Linux Kernel Image (uncompressed)
   Data Size:    2796380 Bytes = 2.7 MiB
   Load Address: 80008000
   Entry Point:  80008000
   Verifying Checksum ... OK
   Loading Kernel Image ... OK
OK

Starting kernel ...

Uncompressing Linux... done, booting the kernel.
Linux version 2.6.37 (x0029463@swubn01) (gcc version 4.3.3 (Sourcery G++ Lite 2009q1-203) ) #1 Wed Dec 26 18:11:35 IST 2012
CPU: ARMv7 Processor [413fc082] revision 2 (ARMv7), cr=10c53c7f
CPU: VIPT nonaliasing data cache, VIPT aliasing instruction cache
Machine: ti8148evm
reserved size = 52428800 at 0x0
FB: Reserving 52428800 bytes SDRAM for VRAM
Memory policy: ECC disabled, Data cache writeback
OMAP chip is TI8148 2.1
SRAM: Mapped pa 0x402f1000 to va 0xfe400000 size: 0xf000
Built 1 zonelists in Zone order, mobility grouping on.  Total pages: 160648
Kernel command line: setenv bootargs console=ttyO0,115200n8 rootwait rw mem=364M@0x80000000 mem=320M@0x9FC00000 vmalloc=500M notifyk.vpssm3_sva=0xBF900000 root=/dev/nfs nfsroot=10.143.25.77:/home/subhvisw/targetfs ip=dhcp
PID hash table entries: 2048 (order: 1, 8192 bytes)
Dentry cache hash table entries: 65536 (order: 6, 262144 bytes)
Inode-cache hash table entries: 32768 (order: 5, 131072 bytes)
Memory: 364MB 270MB = 634MB total
Memory: 637324k/637324k available, 63092k reserved, 276480K highmem
Virtual kernel memory layout:
    vector  : 0xffff0000 - 0xffff1000   (   4 kB)
    fixmap  : 0xfff00000 - 0xfffe0000   ( 896 kB)
    DMA     : 0xffc00000 - 0xffe00000   (   2 MB)
    vmalloc : 0xd7000000 - 0xf8000000   ( 528 MB)
    lowmem  : 0xc0000000 - 0xd6c00000   ( 364 MB)
    pkmap   : 0xbfe00000 - 0xc0000000   (   2 MB)
    modules : 0xbf000000 - 0xbfe00000   (  14 MB)
      .init : 0xc0008000 - 0xc003d000   ( 212 kB)
      .text : 0xc003d000 - 0xc0549000   (5168 kB)
      .data : 0xc054a000 - 0xc05970c0   ( 309 kB)
SLUB: Genslabs=11, HWalign=64, Order=0-3, MinObjects=0, CPUs=1, Nodes=1
NR_IRQS:407
IRQ: Found an INTC at 0xfa200000 (revision 5.0) with 128 interrupts
Total of 128 interrupts on 1 active controller
GPMC revision 6.0
Trying to install interrupt handler for IRQ400
Trying to install interrupt handler for IRQ401
Trying to install interrupt handler for IRQ402
Trying to install interrupt handler for IRQ403
Trying to install interrupt handler for IRQ404
Trying to install interrupt handler for IRQ405
Trying to install interrupt handler for IRQ406
Trying to install type control for IRQ407
Trying to set irq flags for IRQ407
OMAP clockevent source: GPTIMER1 at 20000000 Hz
Console: colour dummy device 80x30
Calibrating delay loop... 599.65 BogoMIPS (lpj=2998272)
pid_max: default: 32768 minimum: 301
Security Framework initialized
Mount-cache hash table entries: 512
CPU: Testing write buffer coherency: ok
devtmpfs: initialized
omap_voltage_early_init: voltage driver support not added
regulator: core version 0.5
regulator: dummy: 
NET: Registered protocol family 16
omap_voltage_domain_lookup: Voltage driver init not yet happened.Faulting!
omap_voltage_add_dev: VDD specified does not exist!
OMAP GPIO hardware version 0.1
OMAP GPIO hardware version 0.1
OMAP GPIO hardware version 0.1
OMAP GPIO hardware version 0.1
omap_mux_init: Add partition: #1: core, flags: 4
NOR: Can't request GPMC CS
Debugfs: Only enabling/disabling deep sleep and wakeup timer is supported now
registered ti81xx_vpss device
registered ti81xx_vidout device
registered ti81xx on-chip HDMI device
registered ti81xx_fb device
registered ti81xx_vin device
ti81xx_pcie: Invoking PCI BIOS...
ti81xx_pcie: Setting up Host Controller...
ti81xx_pcie: Register base mapped @0xd7020000
ti81xx_pcie: Starting PCI scan...
PCI: bus0: Fast back to back transfers enabled
bio: create slab <bio-0> at 0
vgaarb: loaded
SCSI subsystem initialized
usbcore: registered new interface driver usbfs
usbcore: registered new interface driver hub
usbcore: registered new device driver usb
USBSS revision 4ea2080b
registerd cppi-dma Intr @ IRQ 17
Cppi41 Init Done
omap_i2c omap_i2c.1: bus 1 rev4.0 at 100 kHz
pcf857x 1-0021: gpios 128..143 on a pcf8575
regulator: VRTC: 1800 mV 
regulator: VIO: 1500 mV 
regulator: VDD1: 600 <--> 1500 mV at 1200 mV 
regulator: VDD2: 600 <--> 1500 mV at 1200 mV 
regulator: VDDCTRL: 600 <--> 1400 mV at 1200 mV 
regulator: LDO1: 1100 <--> 3300 mV at 1800 mV 
regulator: LDO2: 1100 <--> 3300 mV at 1800 mV 
regulator: LDO3: 1100 <--> 3300 mV at 3300 mV 
regulator: LDO4: 1100 <--> 3300 mV at 1800 mV 
regulator: LDO5: 1100 <--> 3300 mV at 3300 mV 
regulator: LDO6: 1100 <--> 3300 mV at 3300 mV 
regulator: LDO7: 1100 <--> 3300 mV at 3300 mV 
regulator: LDO8: 1100 <--> 3300 mV at 1800 mV 
tps65910 1-002d: No interrupt support, no core IRQ
omap_i2c omap_i2c.3: bus 3 rev4.0 at 100 kHz
Advanced Linux Sound Architecture Driver Version 1.0.23.
Switching to clocksource gp timer
musb-hdrc: version 6.0, host, debug=0
musb-hdrc musb-hdrc.0: dma type: dma-cppi41
MUSB controller-0 revision 4ea20800
musb-hdrc musb-hdrc.0: MUSB HDRC host driver
musb-hdrc musb-hdrc.0: new USB bus registered, assigned bus number 1
usb usb1: New USB device found, idVendor=1d6b, idProduct=0002
usb usb1: New USB device strings: Mfr=3, Product=2, SerialNumber=1
usb usb1: Product: MUSB HDRC host driver
usb usb1: Manufacturer: Linux 2.6.37 musb-hcd
usb usb1: SerialNumber: musb-hdrc.0
hub 1-0:1.0: USB hub found
hub 1-0:1.0: 1 port detected
musb-hdrc musb-hdrc.0: USB Host mode controller at d701e000 using DMA, IRQ 18
musb-hdrc musb-hdrc.1: dma type: dma-cppi41
MUSB controller-1 revision 4ea20800
musb-hdrc musb-hdrc.1: MUSB HDRC host driver
musb-hdrc musb-hdrc.1: new USB bus registered, assigned bus number 2
usb usb2: New USB device found, idVendor=1d6b, idProduct=0002
usb usb2: New USB device strings: Mfr=3, Product=2, SerialNumber=1
usb usb2: Product: MUSB HDRC host driver
usb usb2: Manufacturer: Linux 2.6.37 musb-hcd
usb usb2: SerialNumber: musb-hdrc.1
hub 2-0:1.0: USB hub found
hub 2-0:1.0: 1 port detected
musb-hdrc musb-hdrc.1: USB Host mode controller at d7026800 using DMA, IRQ 19
NET: Registered protocol family 2
IP route cache hash table entries: 16384 (order: 4, 65536 bytes)
TCP established hash table entries: 65536 (order: 7, 524288 bytes)
TCP bind hash table entries: 65536 (order: 6, 262144 bytes)
TCP: Hash tables configured (established 65536 bind 65536)
TCP reno registered
UDP hash table entries: 256 (order: 0, 4096 bytes)
UDP-Lite hash table entries: 256 (order: 0, 4096 bytes)
NET: Registered protocol family 1
RPC: Registered udp transport module.
RPC: Registered tcp transport module.
RPC: Registered tcp NFSv4.1 backchannel transport module.
NetWinder Floating Point Emulator V0.97 (double precision)
PMU: registered new PMU device of type 0
omap-iommu omap-iommu.0: ducati registered
omap-iommu omap-iommu.1: sys registered
highmem bounce pool size: 64 pages
JFFS2 version 2.2. (NAND) Â© 2001-2006 Red Hat, Inc.
msgmni has been set to 704
io scheduler noop registered
io scheduler deadline registered
io scheduler cfq registered (default)
Serial: 8250/16550 driver, 4 ports, IRQ sharing enabled
omap_uart.0: ttyO0 at MMIO 0x48020000 (irq = 72) is a OMAP UART0
console [ttyO0] enabled
omap_uart.1: ttyO1 at MMIO 0x48022000 (irq = 73) is a OMAP UART1
omap_uart.2: ttyO2 at MMIO 0x48024000 (irq = 74) is a OMAP UART2
omap_uart.3: ttyO3 at MMIO 0x481a6000 (irq = 44) is a OMAP UART3
omap_uart.4: ttyO4 at MMIO 0x481a8000 (irq = 45) is a OMAP UART4
omap_uart.5: ttyO5 at MMIO 0x481aa000 (irq = 46) is a OMAP UART5
brd: module loaded
loop: module loaded
ahci ahci.0: forcing PORTS_IMPL to 0x1
ahci ahci.0: AHCI 0001.0300 32 slots 1 ports 3 Gbps 0x1 impl platform mode
ahci ahci.0: flags: ncq sntf pm led clo only pmp pio slum part ccc apst 
scsi0 : ahci_platform
ata1: SATA max UDMA/133 mmio [mem 0x4a140000-0x4a150fff] port 0x100 irq 16
m25p80 spi1.0: w25x32 (4096 Kbytes)
Creating 5 MTD partitions on "spi_flash":
0x000000000000-0x000000020000 : "U-Boot-min"
0x000000020000-0x000000060000 : "U-Boot"
0x000000060000-0x000000062000 : "U-Boot Env"
0x000000062000-0x0000002e2000 : "Kernel"
0x0000002e2000-0x000000400000 : "File System"
omap2-nand driver initializing
ONFI flash detected
NAND device: Manufacturer ID: 0x2c, Chip ID: 0xca (Micron )
Creating 6 MTD partitions on "omap2-nand.0":
0x000000000000-0x000000020000 : "U-Boot-min"
0x000000020000-0x000000260000 : "U-Boot"
0x000000260000-0x000000280000 : "U-Boot Env"
0x000000280000-0x0000006c0000 : "Kernel"
0x0000006c0000-0x00000cee0000 : "File System"
0x00000cee0000-0x000010000000 : "Reserved"
davinci_mdio davinci_mdio.0: davinci mdio revision 1.6
davinci_mdio davinci_mdio.0: detected phy mask fffffffc
davinci_mdio.0: probed
davinci_mdio davinci_mdio.0: phy[0]: device 0:00, driver unknown
davinci_mdio davinci_mdio.0: phy[1]: device 0:01, driver unknown
CAN device driver interface
CAN bus driver for Bosch D_CAN controller 1.0
d_can d_can: d_can device registered (irq=52, irq_obj=53)
usbcore: registered new interface driver cdc_ether
usbcore: registered new interface driver dm9601
usbcore: registered new interface driver cdc_acm
cdc_acm: v0.26:USB Abstract Control Model driver for USB modems and ISDN adapters
Initializing USB Mass Storage driver...
usbcore: registered new interface driver usb-storage
USB Mass Storage support registered.
mice: PS/2 mouse device common for all mice
ata1: SATA link down (SStatus 0 SControl 300)
qt602240_ts 1-004a: Family ID: 128 Variant ID: 1 Version: 22 Build: 171
qt602240_ts 1-004a: Matrix X Size: 18 Matrix Y Size: 12 Object Num: 17
input: AT42QT602240/ATMXT224 Touchscreen as /devices/platform/omap/omap_i2c.1/i2c-1/1-004a/input/input0
omap_rtc omap_rtc: rtc core: registered omap_rtc as rtc0
i2c /dev entries driver
Linux video capture interface: v2.00
usbcore: registered new interface driver uvcvideo
USB Video Class driver (v1.0.0)
OMAP Watchdog Timer Rev 0x00: initial timeout 60 sec
usbcore: registered new interface driver usbhid
usbhid: USB HID core driver
notify_init : notify drivercreated  for  remote proc id 2 at physical Address 0xbf900000
usbcore: registered new interface driver snd-usb-audio
asoc: tlv320aic3x-hifi <-> davinci-mcasp.2 mapping ok
ALSA device list:
  #0: TI81XX EVM
nf_conntrack version 0.5.0 (9958 buckets, 39832 max)
ip_tables: (C) 2000-2006 Netfilter Core Team
TCP cubic registered
NET: Registered protocol family 17
can: controller area network core (rev 20090105 abi 8)
NET: Registered protocol family 29
can: raw protocol (rev 20090105)
can: broadcast manager protocol (rev 20090105 t)
Registering the dns_resolver key type
VFP support v0.3: implementor 41 architecture 3 part 30 variant c rev 3
omap_voltage_late_init: Voltage driver support not added
Power Management for TI81XX.
Detected MACID=40:5f:c2:6d:f:29
omap_rtc omap_rtc: setting system clock to 2000-01-01 00:00:00 UTC (946684800)
mmc0: new high speed SD card at address 0002
mmcblk0: mmc0:0002 00000 1.86 GiB 
 mmcblk0: p1 p2

CPSW phy found : id is : 0x4dd074

CPSW phy found : id is : 0x4dd074
Sending DHCP requests .
PHY: 0:01 - Link is Up - 0/Half
PHY: 0:01 - Link is Down
.
PHY: 0:00 - Link is Up - 1000/Full
., OK
IP-Config: Got DHCP answer from 171.70.177.12, my address is 10.143.25.248
IP-Config: Complete:
     device=eth0, addr=10.143.25.248, mask=255.255.252.0, gw=10.143.24.1,
     host=10.143.25.248, domain=cisco.com, nis-domain=(none),
     bootserver=171.70.177.12, rootserver=10.143.25.77, rootpath=, mtu=576
VFS: Mounted root (nfs filesystem) on device 0:15.
devtmpfs: mounted
Freeing init memory: 212K
INIT: version 2.86 booting
Please wait: booting...
Starting udev
udevd (79): /proc/79/oom_adj is deprecated, please use /proc/79/oom_score_adj instead.
FAT: bogus number of reserved sectors
VFS: Can't find a valid FAT filesystem on dev mmcblk0.
EXT3-fs: barriers not enabled
kjournald starting.  Commit interval 5 seconds
EXT3-fs (mmcblk0p2): warning: maximal mount count reached, running e2fsck is recommended
EXT3-fs (mmcblk0p2): using internal journal
EXT3-fs (mmcblk0p2): recovery complete
EXT3-fs (mmcblk0p2): mounted filesystem with writeback data mode
Root filesystem already rw, not remounting
Caching udev devnodes
NET: Registered protocol family 10
ALSA: Restoring mixer settings...
No state is present for card EVM
Found hardware: "" "" "" "" ""
Hardware is initialized using a generic method
No state is present for card EVM
NOT configuring network interfaces: / is an NFS mount
Mon Dec 31 10:37:00 UTC 2012
INIT: Entering runlevel: 5
Loading HDVICP2 Firmware
DM814X prcm_config_app version: 2.0.0.1
Doing PRCM settings...
	PRCM for IVHD0 is in Progress, Please wait.....  
			BW Phy Addr : 0x48180600 Data : 0x00000001
			AW Phy Addr : 0x48180600 Data : 0x00000002
			Phy Addr : 0x48180c04 Data : 0x00000037
			BW Phy Addr : 0x48180620 Data : 0x00070000
			AW Phy Addr : 0x48180620 Data : 0x00070002
			BW Phy Addr : 0x48180624 Data : 0x00030000
			AW Phy Addr : 0x48180624 Data : 0x00010002
			Phy Addr : 0x48180600 Data : 0x00000102
			BW Phy Addr : 0x48180c10 Data : 0x00000007
			AW Phy Addr : 0x48180c10 Data : 0x00000003
			Phy Addr : 0x48180c14 Data : 0x00000004
			BW Phy Addr : 0x58088000 Data : 0x9f6bad71
			AW Phy Addr : 0x58088000 Data : 0xeafffffe
			BW Phy Addr : 0x58098000 Data : 0xa2c6cc2e
			AW Phy Addr : 0x58098000 Data : 0xeafffffe
			BW Phy Addr : 0x48180c10 Data : 0x00000003
			AW Phy Addr : 0x48180c10 Data : 0x00000000
			Phy Addr : 0x48180c14 Data : 0x00000007
	PRCM for IVHD0 is Done Successfully  
PRCM Initialization completed 
SysLink version : 2.20.02.20
SysLink module created on Date:Dec 26 2012 Time:18:39:49
FIRMWARE: I2cInit will be done by M3
FIRMWARE: Memory map bin file not passed
Usage : firmware_loader <Processor Id> <Location of Firmware> <start|stop> [-mmap <memory_map_file>] [-i2c <0|1>]
===Mandatory arguments=== 
<Processor Id>         0: DSP, 1: Video-M3, 2: Vpss-M3 
<Location of Firmware> firmware binary file 
<start|stop>           to start/stop the firmware 
===Optional arguments=== 
-mmap                  input memory map bin file name 
-i2c                   0: i2c init not done by M3, 1(default): i2c init done by M3 
FIRMWARE: isI2cInitRequiredOnM3: 1
FIRMWARE: Default memory configuration is used
Firmware Loader debugging not configured
Default FL_DEBUG: warning
Allowed FL_DEBUG levels: error, warning, info, debug, log
MemCfg: DCMM (Dynamically Configurable Memory Map) Version :  2.1.2.1
FIRMWARE: 1 start Successful
Loading HDVPSS Firmware
FIRMWARE: I2cInit will be done by M3
FIRMWARE: Memory map bin file not passed
Usage : firmware_loader <Processor Id> <Location of Firmware> <start|stop> [-mmap <memory_map_file>] [-i2c <0|1>]
===Mandatory arguments=== 
<Processor Id>         0: DSP, 1: Video-M3, 2: Vpss-M3 
<Location of Firmware> firmware binary file 
<start|stop>           to start/stop the firmware 
===Optional arguments=== 
-mmap                  input memory map bin file name 
-i2c                   0: i2c init not done by M3, 1(default): i2c init done by M3 
FIRMWARE: isI2cInitRequiredOnM3: 1
FIRMWARE: Default memory configuration is used
Firmware Loader debugging not configured
Default FL_DEBUG: warning
Allowed FL_DEBUG levels: error, warning, info, debug, log
MemCfg: DCMM (Dynamically Configurable Memory Map) Version :  2.1.2.1
FIRMWARE: 2 start Successful
VPSS_FVID2: M3 firmware version 0x1000145 is newer,driver may not work properly.
Configuring fb0 to LCD
HDMI W1 rev 4.0
HDMI CEC Spec version 1.2
Starting system message bus: dbus.
Starting Dropbear SSH server: dropbear.
Starting telnet daemon.
Starting network benchmark server: netserver.
Starting syslogd/klogd: done
Starting thttpd.
Starting PVR
/dev/mem opened.
Memory mapped at address 0x4021d000.
Read at address  0x48180F04 (0x4021df04): 0x00000001
Write at address 0x48180F04 (0x4021df04): 0x00000000, readback 0x00000000
/dev/mem opened.
Memory mapped at address 0x40344000.
Read at address  0x48180900 (0x40344900): 0x00000102
Write at address 0x48180900 (0x40344900): 0x00000002, readback 0x00000002
/dev/mem opened.
Memory mapped at address 0x4029a000.
Read at address  0x48180920 (0x4029a920): 0x00040002
Write at address 0x48180920 (0x4029a920): 0x00000002, readback 0x00000002
Starting Matrix GUI application.

 _____                    _____           _         _   
|  _  |___ ___ ___ ___   |  _  |___ ___  |_|___ ___| |_ 
|     |  _| .'| . | . |  |   __|  _| . | | | -_|  _|  _|
|__|__|_| |__,|_  |___|  |__|  |_| |___|_| |___|___|_|  
              |___|                    |___|            

Arago Project http://arago-project.org dm814x-evm ttyO0

Arago 2011.09 dm814x-evm ttyO0

dm814x-evm login: root