/*
 * Do not modify this file; it is automatically generated from the template
 * linkcmd.xdt in the ti.targets package and will be overwritten.
 */

/*
 * put '"'s around paths because, without this, the linker
 * considers '-' as minus operator, not a file name character.
 */



-l"C:\CCStudio_v5.1\ccsv5\bios_6_31_04_27\packages\ti\sysbios\heaps\lib\whole_program_debug\ti.sysbios.heaps.a674"
-l"C:\CCStudio_v5.1\ccsv5\bios_6_31_04_27\packages\ti\sysbios\gates\lib\whole_program_debug\ti.sysbios.gates.a674"
-l"C:\CCStudio_v5.1\ccsv5\bios_6_31_04_27\packages\ti\sysbios\knl\lib\whole_program_debug\ti.sysbios.knl.a674"
-l"C:\CCStudio_v5.1\ccsv5\bios_6_31_04_27\packages\ti\sysbios\timers\dmtimer\lib\whole_program_debug\ti.sysbios.timers.dmtimer.a674"
-l"C:\CCStudio_v5.1\ccsv5\bios_6_31_04_27\packages\ti\sysbios\hal\lib\whole_program_debug\ti.sysbios.hal.a674"
-l"C:\CCStudio_v5.1\ccsv5\bios_6_31_04_27\packages\ti\sysbios\family\c64p\lib\whole_program_debug\ti.sysbios.family.c64p.a674"
-l"C:\CCStudio_v5.1\ccsv5\bios_6_31_04_27\packages\ti\sysbios\xdcruntime\lib\whole_program_debug\ti.sysbios.xdcruntime.a674"
-l"C:\CCStudio_v5.1\ccsv5\bios_6_31_04_27\packages\ti\sysbios\lib\whole_program_debug\ti.sysbios.a674"
-l"C:\CCStudio_v5.1\ccsv5\bios_6_31_04_27\packages\ti\sysbios\family\c64p\ti81xx\lib\whole_program_debug\ti.sysbios.family.c64p.ti81xx.a674"
-l"C:\CCStudio_v5.1\ccsv5\bios_6_31_04_27\packages\ti\sysbios\family\c62\lib\whole_program_debug\ti.sysbios.family.c62.a674"
-l"C:\CCStudio_v5.1\ccsv5\xdctools_3_20_08_88\packages\ti\targets\rts6000\lib\ti.targets.rts6000.a674"
-l"C:\CCStudio_v5.1\ccsv5\xdctools_3_20_08_88\packages\ti\targets\rts6000\lib\boot.a674"



/* Elf symbols */
--symbol_map ___TI_STACK_BASE=__stack
--symbol_map ___TI_STACK_SIZE=__STACK_SIZE
--symbol_map ___TI_STATIC_BASE=___bss__
--symbol_map __c_int00=_c_int00





--args 0x8
-heap  0x1000
-stack 0x1000

MEMORY
{
    IRAM (RWX) : org = 0x10800000, len = 0x40000
    OCMC_0 (RWX) : org = 0x40300000, len = 0x20000
    OCMC_1 (RWX) : org = 0x40400000, len = 0x20000
    DDR3_RAM : org = 0x80000000, len = 0x10000000
}

/*
 * Linker command file contributions from all loaded packages:
 */

/* Content from xdc.services.global (null): */

/* Content from xdc (null): */

/* Content from xdc.corevers (null): */

/* Content from xdc.shelf (null): */

/* Content from xdc.services.spec (null): */

/* Content from xdc.services.intern.xsr (null): */

/* Content from xdc.services.intern.gen (null): */

/* Content from xdc.services.intern.cmd (null): */

/* Content from xdc.rov (null): */

/* Content from ti.catalog.c6000 (null): */

/* Content from ti.catalog (null): */

/* Content from ti.catalog.peripherals.hdvicp2 (null): */

/* Content from xdc.platform (null): */

/* Content from xdc.cfg (null): */

/* Content from ti.catalog.arm.peripherals.timers (null): */

/* Content from ti.catalog.arm.cortexm3 (null): */

/* Content from ti.catalog.arm.cortexa8 (null): */

/* Content from ti.platforms.evmC6A8168 (null): */

/* Content from ti.targets.rts6000 (null): */

/* Content from xdc.runtime (null): */

/* Content from ti.sysbios.interfaces (null): */

/* Content from xdc.runtime.knl (null): */

/* Content from ti.sysbios.family.c62 (null): */

/* Content from ti.sysbios.family.c64p.ti81xx (null): */

/* Content from ti.sysbios (null): */

/* Content from ti.sysbios.xdcruntime (null): */

/* Content from ti.sysbios.family.c64p (null): */

/* Content from ti.sysbios.hal (null): */

/* Content from ti.sysbios.timers.dmtimer (null): */

/* Content from ti.sysbios.knl (null): */

/* Content from ti.sysbios.gates (null): */

/* Content from ti.sysbios.family (null): */

/* Content from ti.sysbios.heaps (null): */

/* Content from configPkg (null): */


/*
 * symbolic aliases for numeric constants or static instance objects
 */
_xdc_runtime_Startup__EXECFXN__C = 1;
_xdc_runtime_Startup__RESETFXN__C = 1;
_TSK_idle = _ti_sysbios_knl_Task_Object__table__V + 136;

SECTIONS
{


    .text: load >> DDR3_RAM
    .switch: load >> DDR3_RAM
    .stack: load > DDR3_RAM
    .vecs: load >> DDR3_RAM
    .taskStackSection: load >> DDR3_RAM
    .args: load > DDR3_RAM align = 0x4, fill = 0 {_argsize = 0x8; }
    .sysmem: load > DDR3_RAM
    .far: load >> DDR3_RAM
    .data: load >> DDR3_RAM
    .cinit: load > DDR3_RAM
    .bss: load > DDR3_RAM
    .const: load > DDR3_RAM START(const_start) SIZE(const_size)
    .pinit: load > DDR3_RAM
    .cio: load >> DDR3_RAM
    xdc.meta: load >> DDR3_RAM, type = COPY

}



