- Main Page
- Related Pages
- Data Structures
- Files

- File List
- Globals

# af_zdo.h

Go to the documentation of this file.

    00001
    00010 #ifndef AF_ZDO_H
    00011 #define AF_ZDO_H
    00012
    00013 #include "application_configuration.h"
    00014
    00015 void afRegisterApplication(struct applicationConfiguration ac);
    00016 void afRegisterGenericApplication();
    00017 void zdoStartApplication();
    00018 //signed int setJoiningPermissions(unsigned int destination, unsigned char timeout);
    00019 void afSendData(unsigned char destinationEndpoint, unsigned char sourceEndpoint,
    00020                       unsigned int destinationShortAddress, unsigned int clusterId,
    00021                       unsigned char* data, unsigned char dataLength);
    00022 void zdoRequestIeeeAddress(unsigned int shortAddress, unsigned char requestType, unsigned char startIndex);
    00023 unsigned char* zdoNetworkAddressRequest(unsigned char* ieeeAddress, unsigned char requestType, unsigned char startIndex);
    00024 void printZdoNetworkAddressResponse(unsigned char* rsp);
    00025
    00026 #define SINGLE_DEVICE_RESPONSE          0
    00027 #define INCLUDE_ASSOCIATED_DEVICES      1
    00028
    00029 #define AF_DATA_REQUEST_HEADER_SIZE     10
    00030
    00031 #define AF_DATA_CONFIRM_TIMEOUT_MS    2000   //timeout to wait for AF_DATA_CONFIRM. Adjust for network size.
    00032 #define AF_DATA_CONFIRM_INTERVAL_MS   2    //how often to poll for AF_DATA_CONFIRM. Must be less than AF_DATA_CONFIRM_TIMEOUT_MS. Minimum is ~2mSec.
    00033
    00034 #define ZDO_IEEE_ADDR_RSP_TIMEOUT_MS    2000   //timeout to wait for ZDO_IEEE_ADDR_RSP. Adjust for network size.
    00035 #define ZDO_IEEE_ADDR_RSP_INTERVAL_MS   20    //how often to poll for ZDO_IEEE_ADDR_RSP. Must be less than ZDO_IEEE_ADDR_RSP_MS. Typ is ~20mSec.
    00036
    00037 #define ZDO_NWK_ADDR_RSP_TIMEOUT_MS    2000   //timeout to wait for ZDO_NWK_ADDR_RSP. Adjust for network size.
    00038 #define ZDO_NWK_ADDR_RSP_INTERVAL_MS   50    //how often to poll for ZDO_NWK_ADDR_RSP. Must be less than ZDO_NWK_ADDR_RSP_TIMEOUT_MS. Minimum is ~2mSec.
    00039
    00040
    00041
    00042
    00043 #endif

All Data Structures Files Functions Variables Defines