- Main Page
- Related Pages
- Modules
- Files

- File List
- Globals

# hal_cc2530znp_target_board.h

Go to the documentation of this file.

    00001
    00010 #ifndef hal_cc2530znp_target_board_H
    00011 #define hal_cc2530znp_target_board_H
    00012
    00013 #define HAL_SLEEP()     ( __bis_SR_register(LPM3_bits + GIE))
    00014 #define HAL_WAKEUP()    ( __bic_SR_register_on_exit(LPM3_bits))
    00015
    00016 //
    00017 //  Common Includes (will be included in all projects)
    00018 //
    00019 #include "msp430x22x4.h"
    00020 #include "../Common/printf.h"
    00021 #include "../Common/utilities.h"
    00022
    00023 //
    00024 //  METHODS REQUIRED FOR ZNP
    00025 //
    00026 void halInit();
    00027 void halEnableInterrupts();
    00028 void delayMs(unsigned int ms);
    00029 void delayUs(unsigned int us);
    00030 signed int toggleLed(unsigned char led);
    00031 signed int setLed(unsigned char led);
    00032 void clearLeds();
    00033 void halSpiInitZnp();
    00034 void spiWrite(unsigned char *bytes, unsigned char numBytes);
    00035 unsigned int calibrateVlo();
    00036 signed int initTimer(unsigned char seconds, unsigned char wakeOnTimer);
    00037
    00038 //
    00039 //  METHODS NOT REQUIRED FOR ZNP
    00040 //
    00041 unsigned int getVcc3();
    00042 unsigned int getLightSensor();
    00043
    00044 void setZnpInterfaceToInputs(void);
    00045
    00046 void halSpiInitAccelerometer();
    00047 signed int halEnableAccelerometerInterrupt(unsigned char wakeOnAccelerometer);
    00048 unsigned char spiWriteAccelerometer(unsigned char b);
    00049
    00050 //
    00051 //  MACROS REQUIRED FOR ZNP
    00052 //
    00053 #define RADIO_ON()                  (P3OUT |= BIT7)  //ZNP Reset Line
    00054 #define RADIO_OFF()                 (P3OUT &= ~BIT7)
    00055 //  ZNP SPI
    00056 #define SPI_SS_SET()                (P3OUT &= ~(BIT0 | BIT6))  //active low, control SS and MRDY
    00057 #define SPI_SS_CLEAR()              (P3OUT |= (BIT0 | BIT6))
    00058 #define SRDY_IS_HIGH()              (P2IN & BIT6)
    00059 #define SRDY_IS_LOW()               ((~P2IN) & BIT6)
    00060
    00061 #define DEBUG_ON()                  (P4OUT |= BIT4)
    00062 #define DEBUG_OFF()                 (P4OUT &= BIT4)
    00063
    00064 #define NO_WAKEUP 0
    00065 #define WAKEUP_AFTER_TIMER 1
    00066 #define WAKEUP_AFTER_ACCELEROMETER 2
    00067
    00068 //
    00069 //  MISC OTHER DEFINES
    00070 //
    00071 #define XTAL 8000000L
    00072 #define TICKS_PER_MS (XTAL / 1000 / 5 - 1)
    00073 #define TICKS_PER_US (TICKS_PER_MS / 1000)
    00074
    00075 //Required for Light Sensor - NOT REQUIRED FOR ZNP
    00076 #define LIGHT_SENSOR_ON()                  (P2OUT |= BIT1)  //ZNP Reset Line
    00077 #define LIGHT_SENSOR_OFF()                 (P2OUT &= ~BIT1)
    00078
    00079 //Required for Accelerometer - NOT REQUIRED FOR ZNP
    00080 #define ACCELEROMETER_SS_SET()                (P2OUT &= ~(BIT2|BIT7))  //active low
    00081 #define ACCELEROMETER_SS_CLEAR()              (P2OUT |= (BIT2|BIT7))
    00082 #define ACCELEROMETER_RX_BUF    UCB0RXBUF
    00083
    00084
    00085
    00086
    00087 #endif

All Files Functions Variables Defines