# example_get_znp_version.c File Reference

Resets Radio, gets ZNP version information using SYS_VERSION command and displays it. More...

`#include "../HAL/hal.h"`
`#include "../ZNP/znp_interface.h"`

signed int | znpResult
int | main (void)

## Detailed Description

Resets Radio, gets ZNP version information using SYS_VERSION command and displays it.

Configures the MSP430 to communicate with the radio, resets the radio, and sends the SYS_VERSION command and parses the received response and displays it to the console. Demonstrates basic request-response functionality of the ZNP.

Note:
  these fields should not be all zeroes. If you're only seeing zeroes then you may have a bug. Typical values seen are Version: TransportRev=2, ProductId=0, FW Rev=2.3, HW Rev=1

See also:
  http://processors.wiki.ti.com/index.php/Tutorial_on_the_Examples and http://e2e.ti.com/support/low_power_rf/default.aspx

Rev
  718

Author
  dsmith

Date
  2010-08-19 10:51:40 -0700 (Thu, 19 Aug 2010)

YOU ACKNOWLEDGE AND AGREE THAT THE SOFTWARE AND DOCUMENTATION ARE PROVIDED “AS IS” WITHOUT WARRANTY OF ANY KIND, EITHER EXPRESS OR IMPLIED, INCLUDING WITHOUT LIMITATION, ANY WARRANTY OF MERCHANTABILITY, TITLE, NON-INFRINGEMENT AND FITNESS FOR A PARTICULAR PURPOSE. IN NO EVENT SHALL TEXAS INSTRUMENTS OR ITS LICENSORS BE LIABLE OR OBLIGATED UNDER CONTRACT, NEGLIGENCE, STRICT LIABILITY, CONTRIBUTION, BREACH OF WARRANTY, OR OTHER LEGAL EQUITABLE THEORY ANY DIRECT OR INDIRECT DAMAGES OR EXPENSES INCLUDING BUT NOT LIMITED TO ANY INCIDENTAL, SPECIAL, INDIRECT, PUNITIVE OR CONSEQUENTIAL DAMAGES, LOST PROFITS OR LOST DATA, COST OF PROCUREMENT OF SUBSTITUTE GOODS, TECHNOLOGY, SERVICES, OR ANY CLAIMS BY THIRD PARTIES (INCLUDING BUT NOT LIMITED TO ANY DEFENSE THEREOF), OR OTHER SIMILAR COSTS.

All Data Structures Files Functions Variables Defines