# example_read_nv_items.c File Reference

Resets Radio, reads out the contents of all non-volatile (NV) items and displays to console. More...

`#include "../HAL/hal.h"`
`#include "../ZNP/znp_interface.h"`

signed int | znpResult
int | main (void)

## Detailed Description

Resets Radio, reads out the contents of all non-volatile (NV) items and displays to console.

The ZNP supports six NV storage buffers (named "NV Items"). 1 through 4 are 2 bytes each; 5 & 6 are 16 bytes each. These NV items are stored in the ZNP's flash memory and can be used for non-volatile storage. To verify, run the Write NV Items example, power cycle the CC2530, and then run this example. You should see that the values are retained through loss of power.

See also:
  http://processors.wiki.ti.com/index.php/Tutorial_on_the_Examples and http://e2e.ti.com/support/low_power_rf/default.aspx

Rev
  718

Author
  dsmith

Date
  2010-08-19 10:51:40 -0700 (Thu, 19 Aug 2010)

YOU ACKNOWLEDGE AND AGREE THAT THE SOFTWARE AND DOCUMENTATION ARE PROVIDED “AS IS” WITHOUT WARRANTY OF ANY KIND, EITHER EXPRESS OR IMPLIED, INCLUDING WITHOUT LIMITATION, ANY WARRANTY OF MERCHANTABILITY, TITLE, NON-INFRINGEMENT AND FITNESS FOR A PARTICULAR PURPOSE. IN NO EVENT SHALL TEXAS INSTRUMENTS OR ITS LICENSORS BE LIABLE OR OBLIGATED UNDER CONTRACT, NEGLIGENCE, STRICT LIABILITY, CONTRIBUTION, BREACH OF WARRANTY, OR OTHER LEGAL EQUITABLE THEORY ANY DIRECT OR INDIRECT DAMAGES OR EXPENSES INCLUDING BUT NOT LIMITED TO ANY INCIDENTAL, SPECIAL, INDIRECT, PUNITIVE OR CONSEQUENTIAL DAMAGES, LOST PROFITS OR LOST DATA, COST OF PROCUREMENT OF SUBSTITUTE GOODS, TECHNOLOGY, SERVICES, OR ANY CLAIMS BY THIRD PARTIES (INCLUDING BUT NOT LIMITED TO ANY DEFENSE THEREOF), OR OTHER SIMILAR COSTS.

All Data Structures Files Functions Variables Defines