--------------------------------------------------------
It is recommended that for final product release the image build using the ProdHex project be used. 
Refer to Z-Stack User Guide – CC2530ZNP document included with ZAP-MSP430-2.5.0 release for more details. 
The following images included in this folder are built using the ProdHex project with compile options as described below.

Images – 
Image #1:
CC2530ZNP-MK-Pro.Hex

CC2530_MK
POWER_SAVING
ASSERT_RESET
FAKE_CRC_SHDW
ZDNWKMGR_MIN_TRANSMISSIONS=0 
SECURE=0

-------------------------------------------------------
Image #2:
CC2530-MK-Pro-Secure_Standard.hex

CC2530_MK
POWER_SAVING
ASSERT_RESET
FAKE_CRC_SHDW
ZDNWKMGR_MIN_TRANSMISSIONS=0 
SECURE=1

-----------------------------------------------------------
Image #3:
CC2530-MK-Pro-Secure_LinkKeyJoin.hex

CC2530_MK
POWER_SAVING
ASSERT_RESET
FAKE_CRC_SHDW
ZDNWKMGR_MIN_TRANSMISSIONS=0 
SECURE=1
TC_LINKKEY_JOIN
ZDSECMGR_TC_DEVICE_MAX=16

----------------------------------------------------------------
Image #4:
CC2530-MK-Pro-Secure_LinkKeyJoin_ECC.hex
(Using live ECC libraries)

CC2530_MK
POWER_SAVING
ASSERT_RESET
FAKE_CRC_SHDW
ZDNWKMGR_MIN_TRANSMISSIONS=0 
SECURE=1
TC_LINKKEY_JOIN
ZDSECMGR_TC_DEVICE_MAX=16

----------------------------------------------------------------
Image #5:
CC2530-MK-Pro-Secure_LinkKeyJoin_ECC_KeyAccess.hex
(Using live ECC libraries)

CC2530_MK
POWER_SAVING
ASSERT_RESET
FAKE_CRC_SHDW
ZDNWKMGR_MIN_TRANSMISSIONS=0 
SECURE=1
TC_LINKKEY_JOIN
ZDSECMGR_TC_DEVICE_MAX=16
MT_SYS_OSAL_NV_READ_CERTIFICATE_DATA=1
MT_SYS_KEY_MANAGEMENT
