# PCIE LLD Port Logic Register Definitions
[PCIE LLD Configuration Register Definitions]

## Data Structures

struct | pciePlAckTimerReg_s
| Specification of the Ack Latency Time and Replay Timer register. More...
struct | pciePlOMsgReg_s
| Specification of the Other Message register. More...
struct | pciePlForceLinkReg_s
| Specification of the Port Force Link register. More...
struct | pcieAckFreqReg_s
| Specification of the Ack Frequency register. More...
struct | pcieLnkCtrlReg_s
| Specification of the Port Link Control Register. More...
struct | pcieLaneSkewReg_s
| Specification of the Lane Skew register. More...
struct | pcieSymNumReg_s
| Specification of the Symbol Number register. More...
struct | pcieSymTimerFltMaskReg_s
| Specification of the Symbol Timer and Filter Mask register. More...
struct | pcieFltMask2Reg_s
| Specification of the Filter Mask 2 register. More...
struct | pcieDebug0Reg_s
| Specification of the Debug0 Register. More...
struct | pcieDebug1Reg_s
| Specification of the Debug 1 Register. More...
struct | pcieGen2Reg_s
| Specification of the Gen2 Register. More...
typedef struct pciePlAckTimerReg_s | pciePlAckTimerReg_t
| Specification of the Ack Latency Time and Replay Timer register.
typedef struct pciePlOMsgReg_s | pciePlOMsgReg_t
| Specification of the Other Message register.
typedef struct pciePlForceLinkReg_s | pciePlForceLinkReg_t
| Specification of the Port Force Link register.
typedef struct pcieAckFreqReg_s | pcieAckFreqReg_t
| Specification of the Ack Frequency register.
typedef struct pcieLnkCtrlReg_s | pcieLnkCtrlReg_t
| Specification of the Port Link Control Register.
typedef struct pcieLaneSkewReg_s | pcieLaneSkewReg_t
| Specification of the Lane Skew register.
typedef struct pcieSymNumReg_s | pcieSymNumReg_t
| Specification of the Symbol Number register.
typedef struct pcieSymTimerFltMaskReg_s | pcieSymTimerFltMaskReg_t
| Specification of the Symbol Timer and Filter Mask register.
typedef struct pcieFltMask2Reg_s | pcieFltMask2Reg_t
| Specification of the Filter Mask 2 register.
typedef struct pcieDebug0Reg_s | pcieDebug0Reg_t
| Specification of the Debug0 Register.
typedef struct pcieDebug1Reg_s | pcieDebug1Reg_t
| Specification of the Debug 1 Register.
typedef struct pcieGen2Reg_s | pcieGen2Reg_t
| Specification of the Gen2 Register.

## Typedef Documentation

typedef struct pcieAckFreqReg_s pcieAckFreqReg_t

Specification of the Ack Frequency register.

This register may be used for both endpoint and root complex modes.

typedef struct pcieDebug0Reg_s pcieDebug0Reg_t

Specification of the Debug0 Register.

This register may be used for both endpoint and root complex modes.

typedef struct pcieDebug1Reg_s pcieDebug1Reg_t

Specification of the Debug 1 Register.

This register may be used for both endpoint and root complex modes.

typedef struct pcieFltMask2Reg_s pcieFltMask2Reg_t

Specification of the Filter Mask 2 register.

This register may be used for both endpoint and root complex modes.

typedef struct pcieGen2Reg_s pcieGen2Reg_t

Specification of the Gen2 Register.

This register may be used for both endpoint and root complex modes.

typedef struct pcieLaneSkewReg_s pcieLaneSkewReg_t

Specification of the Lane Skew register.

This register may be used for both endpoint and root complex modes.

typedef struct pcieLnkCtrlReg_s pcieLnkCtrlReg_t

Specification of the Port Link Control Register.

This register may be used for both endpoint and root complex modes.

typedef struct pciePlAckTimerReg_s pciePlAckTimerReg_t

Specification of the Ack Latency Time and Replay Timer register.

This register may be used for both endpoint and root complex modes.

typedef struct pciePlForceLinkReg_s pciePlForceLinkReg_t

Specification of the Port Force Link register.

This register may be used for both endpoint and root complex modes.

typedef struct pciePlOMsgReg_s pciePlOMsgReg_t

Specification of the Other Message register.

This register may be used for both endpoint and root complex modes.

typedef struct pcieSymNumReg_s pcieSymNumReg_t

Specification of the Symbol Number register.

This register may be used for both endpoint and root complex modes.

typedef struct pcieSymTimerFltMaskReg_s pcieSymTimerFltMaskReg_t

Specification of the Symbol Timer and Filter Mask register.

This register may be used for both endpoint and root complex modes.

Copyright 2012, Texas Instruments Incorporated