- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

# EMAC_CHAN_MAC_ADDR_tag Struct Reference

This structure is used to for the driver to return the application the channel/MAC address configuration when an EMAC port is opened. More...

`#include <emac_drv.h>`

## Data Fields

Uint32 | chan_num
Uint32 | num_of_mac_addrs
EMAC_MAC_ADDR_T * | p_mac_addr

## Detailed Description

This structure is used to for the driver to return the application the channel/MAC address configuration when an EMAC port is opened.

## Field Documentation

Uint32 EMAC_CHAN_MAC_ADDR_tag::chan_num

channel number configured for this core

Uint32 EMAC_CHAN_MAC_ADDR_tag::num_of_mac_addrs

Total number of MAC addresses configured for this channel

EMAC_MAC_ADDR_T* EMAC_CHAN_MAC_ADDR_tag::p_mac_addr

Pointer to the MAC addresses configured for this channel

The documentation for this struct was generated from the following file:

- emac_drv.h

Copyright 2012, Texas Instruments Incorporated