# Tcp3d_SizeCfg Struct Reference
[TCP3D Driver Data Structures]

Parameters which determine buffer sizes. More...

`#include <tcp3d_drv.h>`

## Data Fields

uint32_t | maxCodeBlocks
uint32_t | mode

## Detailed Description

Parameters which determine buffer sizes.

These are configured and passed with getNumBuf() & getBufDesc() funcitons to get the buffer requirement of the TCP3.

## Field Documentation

uint32_t Tcp3d_SizeCfg::maxCodeBlocks

Maximum code blocks for which driver will be configured

uint32_t Tcp3d_SizeCfg::mode

TCP3 Decode mode for which the driver instance will be used

The documentation for this struct was generated from the following file:

- tcp3d_drv.h

Copyright 2012, Texas Instruments Incorporated