# pcieExpRomReg_s Struct Reference
[PCIE LLD Type0 (endpoint) Register Definitions]

Specification of the Expansion ROM Register. More...

`#include <pcie.h>`

## Data Fields

uint32_t | raw
| [ro] Raw image of register on read; actual value on write
uint32_t | expRomAddr
| [ro] Address of Expansion ROM
uint8_t | enable
| [ro] Expansion ROM Enable

## Detailed Description

Specification of the Expansion ROM Register.

## Field Documentation

uint8_t pcieExpRomReg_s::enable

[ro] Expansion ROM Enable

Field size: 1 bit

uint32_t pcieExpRomReg_s::expRomAddr

[ro] Address of Expansion ROM

Field size: 21 bits

The documentation for this struct was generated from the following file:

- pcie.h

Copyright 2012, Texas Instruments Incorporated