# pcieType0Bar32bitIdx_s Struct Reference
[PCIE LLD Type0 (endpoint) Register Definitions]

pcieBar32bitReg_s register plus an index (End Point BAR) More...

`#include <pcie.h>`

## Data Fields

pcieBar32bitReg_t | reg
| Register Structure.
uint8_t | idx
| Index in the array of registers of this type.

## Detailed Description

pcieBar32bitReg_s register plus an index (End Point BAR)

There are multiple instances of this register. The index is used to select which instance of the register will be accessed.

This structure is used to access an End Point BAR. For more details, please refer to pcieBar32bitReg_t

The documentation for this struct was generated from the following file:

- pcie.h

Copyright 2012, Texas Instruments Incorporated