# Srio_Type9AddrInfo Struct Reference
[SRIO LLD Data Structures]

SRIO Socket Type9 Information. More...

`#include <srio_drv.h>`

## Data Fields

uint16_t | tt
| Transport Type; 16 bit or 8 bit identifiers.
uint16_t | id
| This is the 8 bit or 16 bit SRIO identifier.
uint8_t | cos
| Class of service.
uint16_t | streamId
| Stream identifier.

## Detailed Description

SRIO Socket Type9 Information.

The structure describes the address information required to send & receive a Type11 message over a Type11 socket. This is populated to indicate the remote endpoint where the message has to be sent.

The documentation for this struct was generated from the following file:

- srio_drv.h

Copyright 2012, Texas Instruments Incorporated