# pcieTlpCfgReg_s Struct Reference
[PCIE LLD Application Register Definitions]

Specification of the TLP configuration Register. More...

`#include <pcie.h>`

## Data Fields

uint32_t | raw
| [ro] Raw image of register on read; actual value on write
uint8_t | relaxed
| [rw] Enable relaxed ordering for all outgoing TLPs
uint8_t | noSnoop
| [rw] Enable No Snoop attribute on all outgoing TLPs

## Detailed Description

Specification of the TLP configuration Register.

## Field Documentation

uint8_t pcieTlpCfgReg_s::noSnoop

[rw] Enable No Snoop attribute on all outgoing TLPs

Field size: 1 bit

uint8_t pcieTlpCfgReg_s::relaxed

[rw] Enable relaxed ordering for all outgoing TLPs

Field size: 1 bit

The documentation for this struct was generated from the following file:

- pcie.h

Copyright 2012, Texas Instruments Incorporated