# hyplnkRXPrivIDIdxReg_s Struct Reference
[HYPLNK LLD Register Definitions]

Specification of the Rx Address PrivID Index Register. More...

`#include <hyplnk.h>`

## Data Fields

uint32_t | raw
| [ro] Raw image of register on read; actual value on write
uint8_t | rxPrivIDIdx
| [rw] Selects PrivID array element number

## Detailed Description

Specification of the Rx Address PrivID Index Register.

## Field Documentation

uint8_t hyplnkRXPrivIDIdxReg_s::rxPrivIDIdx

[rw] Selects PrivID array element number

Field size: 4 bits

The specified array element can be read or written via hyplnkRXPrivIDValReg_s::rxPrivIDVal after the index is written.

The documentation for this struct was generated from the following file:

- hyplnk.h

Copyright 2012, Texas Instruments Incorporated