# hyplnkChipVerReg_s Struct Reference
[HYPLNK LLD Register Definitions]

Specification of the Chip Version Register. More...

`#include <hyplnk.h>`

## Data Fields

uint32_t | raw
| [ro] Raw image of register on read; actual value on write
uint16_t | devRev
| [ro] Device Revision
uint16_t | devID
| [ro] Device ID

## Detailed Description

Specification of the Chip Version Register.

## Field Documentation

uint16_t hyplnkChipVerReg_s::devID

[ro] Device ID

Field size: 16 bits

Reflects value of device_id pins (not brought out to chip pins)

uint16_t hyplnkChipVerReg_s::devRev

[ro] Device Revision

Field size: 16 bits

Reflects value of device_rev pins (not brought out to chip pins)

The documentation for this struct was generated from the following file:

- hyplnk.h

Copyright 2012, Texas Instruments Incorporated