# pcieObSizeReg_s Struct Reference
[PCIE LLD Application Register Definitions]

Specification of the Outbound Size Register. More...

`#include <pcie.h>`

## Data Fields

uint32_t | raw
| [ro] Raw image of register on read; actual value on write
uint8_t | size
| [rw] Set each outbound translation window size

## Detailed Description

Specification of the Outbound Size Register.

## Field Documentation

uint8_t pcieObSizeReg_s::size

[rw] Set each outbound translation window size

size | Window Size
--- | ---
0 | 1 MB
1 | 2 MB
2 | 4 MB
3 | 8 MB
others | reserved

Field size: 3 bits

The documentation for this struct was generated from the following file:

- pcie.h

Copyright 2012, Texas Instruments Incorporated