# pcieObOffsetHiReg_s Struct Reference
[PCIE LLD Application Register Definitions]

Specification of the Outbound Translation Region Offset High Register. More...

`#include <pcie.h>`

## Data Fields

uint32_t | raw
| [ro] Raw image of register on read; actual value on write
uint32_t | offsetHi
| [rw] Offset high bits [63:32] for translation region

## Detailed Description

Specification of the Outbound Translation Region Offset High Register.

There is one register per translation region (0-7)

## Field Documentation

uint32_t pcieObOffsetHiReg_s::offsetHi

[rw] Offset high bits [63:32] for translation region

Field size: 32 bits

The documentation for this struct was generated from the following file:

- pcie.h

Copyright 2012, Texas Instruments Incorporated