- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

# EMAC Driver Data Structures

Here are the data structures with brief descriptions:

EMAC_CHAN_MAC_ADDR_tag | This structure is used to for the driver to return the application the channel/MAC address configuration when an EMAC port is opened
EMAC_CONFIG_INFO_tag | EMAC configuration data structure
EMAC_LINK_INFO_tag | EMAC statistics and link status data structure
EMAC_OPEN_CONFIG_INFO_tag | EMAC open configuration data structure
EMAC_PKT_DESC_T | EMAC packet descriptor data structure
EMAC_STATISTICS_tag | The statistics structure is used to retrieve the current count of various packet events in the system. These values represent the delta values from the last time the statistics were read

Copyright 2012, Texas Instruments Incorporated