# Rm_Resource Struct Reference
[RM LLD Resource Table Definition Symbols and Structures]

Resource Table resource definition structure. More...

`#include <resource_table_defs.h>`

## Data Fields

uint32_t | resourceId
uint32_t | resourceStart
uint32_t | resourceEnd
uint32_t | resourceInitFlags
uint32_t | resourceUseFlags

## Detailed Description

Resource Table resource definition structure.

## Field Documentation

uint32_t Rm_Resource::resourceEnd

End range for identified resource

uint32_t Rm_Resource::resourceId

Resouce identifier.

uint32_t Rm_Resource::resourceInitFlags

Resource initialization permission flags Bits 0 : DSP 0 Permission Bit Bits 1 : DSP 1 Permission Bit Bits 2 : DSP 2 Permission Bit Bits 3 : DSP 3 Permission Bit Bits 31-8 : UNUSED

uint32_t Rm_Resource::resourceStart

Start range for identified resource

uint32_t Rm_Resource::resourceUseFlags

Resource usage permission flags Bits 0 : DSP 0 Permission Bit Bits 1 : DSP 1 Permission Bit Bits 2 : DSP 2 Permission Bit Bits 3 : DSP 3 Permission Bit Bits 31-8 : UNUSED

The documentation for this struct was generated from the following file:

- resource_table_defs.h

Copyright 2012, Texas Instruments Incorporated