# csl_edma3Aux.h File Reference

This is the EDMA Auxilary Header File which exposes the various CSL Functional Layer API's to configure the EDMA Module. More...

`#include <ti/csl/csl_edma3.h>`

## Functions

CSL_IDEF_INLINE void | CSL_edma3GetInfo (CSL_Edma3Handle hModule, CSL_Edma3QueryInfo *response)
CSL_IDEF_INLINE void | CSL_edma3MapDMAChannelToParamBlock (CSL_Edma3Handle hModule, Uint8 dmaChannel, Uint16 paramId)
CSL_IDEF_INLINE Uint16 | CSL_edma3GetDMAChannelToParamBlockMapping (CSL_Edma3Handle hModule, Uint8 dmaChannel)
CSL_IDEF_INLINE void | CSL_edma3MapQDMAChannelToParamBlock (CSL_Edma3Handle hModule, Uint8 qdmaChannel, Uint16 paramId)
CSL_IDEF_INLINE Uint16 | CSL_edma3GetQDMAChannelToParamBlockMapping (CSL_Edma3Handle hModule, Uint8 qdmaChannel)
CSL_IDEF_INLINE void | CSL_edma3SetQDMATriggerWord (CSL_Edma3Handle hModule, Uint8 qdmaChannel, Uint8 trword)
CSL_IDEF_INLINE void | CSL_edma3GetQDMATriggerWord (CSL_Edma3Handle hModule, Uint8 qdmaChannel, Uint8 *trword)
CSL_IDEF_INLINE void | CSL_edma3MapDMAChannelToEventQueue (CSL_Edma3Handle hModule, Uint8 dmaChannel, Uint8 eventQueue)
CSL_IDEF_INLINE Uint8 | CSL_edma3GetDMAChannelToEventQueueMapping (CSL_Edma3Handle hModule, Uint8 dmaChannel)
CSL_IDEF_INLINE void | CSL_edma3MapQDMAChannelToEventQueue (CSL_Edma3Handle hModule, Uint8 qdmaChannel, Uint8 eventQueue)
CSL_IDEF_INLINE Uint8 | CSL_edma3GetQDMAChannelToEventQueueMapping (CSL_Edma3Handle hModule, Uint8 qdmaChannel)
CSL_IDEF_INLINE void | CSL_edma3MapEventQueueToTC (CSL_Edma3Handle hModule, Uint8 eventQueue, Uint8 tcNum)
CSL_IDEF_INLINE Uint8 | CSL_edma3GetEventQueueToTCMapping (CSL_Edma3Handle hModule, Uint8 eventQueue)
CSL_IDEF_INLINE void | CSL_edma3SetEventQueuePriority (CSL_Edma3Handle hModule, Uint8 eventQueue, Uint8 priority)
CSL_IDEF_INLINE Uint8 | CSL_edma3GetEventQueuePriority (CSL_Edma3Handle hModule, Uint8 eventQueue)
CSL_IDEF_INLINE void | CSL_edma3GetEventMissed (CSL_Edma3Handle hModule, CSL_BitMask32 *missedLo, CSL_BitMask32 *missedHi, CSL_BitMask32 *missedQdma)
CSL_IDEF_INLINE void | CSL_edma3IsDMAChannelMissedEventSet (CSL_Edma3Handle hModule, Uint8 dmaChannel, Bool *response)
CSL_IDEF_INLINE void | CSL_edma3IsQDMAChannelMissedEventSet (CSL_Edma3Handle hModule, Uint8 qdmaChannel, Bool *response)
CSL_IDEF_INLINE void | CSL_edma3EventsMissedClear (CSL_Edma3Handle hModule, CSL_BitMask32 missedLo, CSL_BitMask32 missedHi, CSL_BitMask32 missedQdma)
CSL_IDEF_INLINE void | CSL_edma3ClearDMAMissedEvent (CSL_Edma3Handle hModule, Uint8 dmaChannel)
CSL_IDEF_INLINE void | CSL_edma3ClearQDMAMissedEvent (CSL_Edma3Handle hModule, Uint8 qdmaChannel)
CSL_IDEF_INLINE void | CSL_edma3GetControllerError (CSL_Edma3Handle hModule, CSL_Edma3CtrlErrStat *ccStat)
CSL_IDEF_INLINE void | CSL_edma3ClearControllerError (CSL_Edma3Handle hModule, CSL_Edma3CtrlErrStat *ccStat)
CSL_IDEF_INLINE void | CSL_edma3ErrorEval (CSL_Edma3Handle hModule)
CSL_IDEF_INLINE void | CSL_edma3DmaRegionAccessEnable (CSL_Edma3Handle hModule, Int edmaRegion, CSL_BitMask32 drae, CSL_BitMask32 draeh)
CSL_IDEF_INLINE void | CSL_edma3DmaRegionAccessDisable (CSL_Edma3Handle hModule, Int edmaRegion, CSL_BitMask32 drae, CSL_BitMask32 draeh)
CSL_IDEF_INLINE void | CSL_edma3QdmaRegionAccessEnable (CSL_Edma3Handle hModule, Int edmaRegion, CSL_BitMask32 qrae)
CSL_IDEF_INLINE void | CSL_edma3QdmaRegionAccessDisable (CSL_Edma3Handle hModule, Int edmaRegion, CSL_BitMask32 qrae)
CSL_IDEF_INLINE void | CSL_edma3GetWaterMark (CSL_Edma3Handle hModule, Uint8 eventQueue, Uint8 *waterMark)
CSL_IDEF_INLINE void | CSL_edma3GetNumberValidEntries (CSL_Edma3Handle hModule, Uint8 eventQueue, Uint8 *numValidEntries)
CSL_IDEF_INLINE void | CSL_edma3GetStartPointer (CSL_Edma3Handle hModule, Uint8 eventQueue, Uint8 *startPtr)
CSL_IDEF_INLINE void | CSL_edma3GetThresholdExceeded (CSL_Edma3Handle hModule, Uint8 eventQueue, Bool *thresholdExceeded)
CSL_IDEF_INLINE void | CSL_edma3EventQueueThresholdSet (CSL_Edma3Handle hModule, Uint8 eventQueue, Uint8 threshold)
CSL_IDEF_INLINE void | CSL_edma3GetActivityStatus (CSL_Edma3Handle hModule, CSL_Edma3ActivityStat *activityStat)
CSL_IDEF_INLINE void | CSL_edma3GetMemoryFaultError (CSL_Edma3Handle hModule, CSL_Edma3MemFaultStat *memFault)
CSL_IDEF_INLINE void | CSL_edma3MemFaultClear (CSL_Edma3Handle hModule)
CSL_IDEF_INLINE void | CSL_edma3GetMemoryProtectionAttrib (CSL_Edma3Handle hModule, Int region, CSL_BitMask32 *mppa)
CSL_IDEF_INLINE void | CSL_edma3SetMemoryProtectionAttrib (CSL_Edma3Handle hModule, Int region, CSL_BitMask32 mppa)
CSL_IDEF_INLINE void | CSL_edma3IsDMAChannelEventPending (CSL_Edma3Handle hModule, Uint8 dmaChannel, Bool *response)
CSL_IDEF_INLINE void | CSL_edma3ClearDMAChannelEvent (CSL_Edma3Handle hModule, Int region, Uint8 dmaChannel)
CSL_IDEF_INLINE void | CSL_edma3SetDMAChannelEvent (CSL_Edma3Handle hModule, Int region, Uint8 dmaChannel)
CSL_IDEF_INLINE void | CSL_edma3DMAChannelDisable (CSL_Edma3Handle hModule, Int region, Uint8 dmaChannel)
CSL_IDEF_INLINE void | CSL_edma3DMAChannelEnable (CSL_Edma3Handle hModule, Int region, Uint8 dmaChannel)
CSL_IDEF_INLINE void | CSL_edma3GetDMASecondaryEvents (CSL_Edma3Handle hModule, CSL_BitMask32 *secEventLo, CSL_BitMask32 *secEventHi)
CSL_IDEF_INLINE void | CSL_edma3IsDMAChannelSecondaryEventSet (CSL_Edma3Handle hModule, Uint8 dmaChannel, Bool *response)
CSL_IDEF_INLINE void | CSL_edma3ClearDMASecondaryEvents (CSL_Edma3Handle hModule, CSL_BitMask32 secEventLo, CSL_BitMask32 secEventHi)
CSL_IDEF_INLINE void | CSL_edma3ClearDMAChannelSecondaryEvents (CSL_Edma3Handle hModule, Uint8 dmaChannel)
CSL_IDEF_INLINE void | CSL_edma3InterruptLoDisable (CSL_Edma3Handle hModule, Int region, CSL_BitMask32 intrLo)
CSL_IDEF_INLINE void | CSL_edma3InterruptHiDisable (CSL_Edma3Handle hModule, Int region, CSL_BitMask32 intrHi)
CSL_IDEF_INLINE void | CSL_edma3InterruptLoEnable (CSL_Edma3Handle hModule, Int region, CSL_BitMask32 intrLo)
CSL_IDEF_INLINE void | CSL_edma3InterruptHiEnable (CSL_Edma3Handle hModule, Int region, CSL_BitMask32 intrHi)
CSL_IDEF_INLINE void | CSL_edma3GetLoPendingInterrupts (CSL_Edma3Handle hModule, Int region, CSL_BitMask32 *intrLo)
CSL_IDEF_INLINE void | CSL_edma3GetHiPendingInterrupts (CSL_Edma3Handle hModule, Int region, CSL_BitMask32 *intrHi)
CSL_IDEF_INLINE void | CSL_edma3ClearLoPendingInterrupts (CSL_Edma3Handle hModule, Int region, CSL_BitMask32 intrLo)
CSL_IDEF_INLINE void | CSL_edma3ClearHiPendingInterrupts (CSL_Edma3Handle hModule, Int region, CSL_BitMask32 intrHi)
CSL_IDEF_INLINE void | CSL_edma3InterruptEval (CSL_Edma3Handle hModule, Int region)
CSL_IDEF_INLINE void | CSL_edma3IsQDMAChannelEventPending (CSL_Edma3Handle hModule, Uint8 qdmaChannel, Bool *response)
CSL_IDEF_INLINE void | CSL_edma3QDMAChannelEnable (CSL_Edma3Handle hModule, Int region, Uint8 qdmaChannel)
CSL_IDEF_INLINE void | CSL_edma3QDMAChannelDisable (CSL_Edma3Handle hModule, Int region, Uint8 qdmaChannel)
CSL_IDEF_INLINE void | CSL_edma3GetQDMASecondaryEvents (CSL_Edma3Handle hModule, Uint32 *qdmaSecEvent)
CSL_IDEF_INLINE void | CSL_edma3IsQDMAChannelSecondaryEventSet (CSL_Edma3Handle hModule, Uint8 qdmaChannel, Bool *response)
CSL_IDEF_INLINE void | CSL_edma3ClearQDMASecondaryEvents (CSL_Edma3Handle hModule, Uint32 qdmaSecEvent)
CSL_IDEF_INLINE void | CSL_edma3ClearQDMAChannelSecondaryEvents (CSL_Edma3Handle hModule, Uint8 qdmaChannel)

## Detailed Description

This is the EDMA Auxilary Header File which exposes the various CSL Functional Layer API's to configure the EDMA Module.

  ============================================================================
  (C) Copyright 2002, 2003, 2004, 2005, 2008, 2009, Texas Instruments, Inc.

Redistribution and use in source and binary forms, with or without modification, are permitted provided that the following conditions are met:

Redistributions of source code must retain the above copyright notice, this list of conditions and the following disclaimer.

Redistributions in binary form must reproduce the above copyright notice, this list of conditions and the following disclaimer in the documentation and/or other materials provided with the distribution.

Neither the name of Texas Instruments Incorporated nor the names of its contributors may be used to endorse or promote products derived from this software without specific prior written permission.

THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT OWNER OR CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.

Copyright 2012, Texas Instruments Incorporated