# IDMA Data Structures
[IDMA]

## Data Structures

struct | CSL_IDMA_IDMA1CONFIG
| This structure holds the information required to initiate a iDMA Channel 1 Block Fill/Transfer request in the GEM. More...
struct | CSL_IDMA_IDMA0CONFIG
| This structure holds the information required to initiate a iDMA Channel 0 Configuration(CFG) space Transfer request from the GEM. More...
struct | CSL_IDMA_STATUS
| This structure holds the information required to interpret the IDMA Channel 0/1 Transfer Status. More...

## Defines

#define | hIdma ((CSL_CgemRegs *) CSL_CGEM0_5_REG_BASE_ADDRESS_REGS)

## Define Documentation

#define hIdma ((CSL_CgemRegs *) CSL_CGEM0_5_REG_BASE_ADDRESS_REGS)

Handle to access IDMA registers.

Copyright 2012, Texas Instruments Incorporated