# hyplnkRXSegIdxReg_s Struct Reference
[HYPLNK LLD Register Definitions]

Specification of the Rx Address Segment Index Register. More...

`#include <hyplnk.h>`

## Data Fields

uint32_t | raw
| [ro] Raw image of register on read; actual value on write
uint8_t | rxSegIdx
| [rw] Selects segment array element number

## Detailed Description

Specification of the Rx Address Segment Index Register.

## Field Documentation

uint8_t hyplnkRXSegIdxReg_s::rxSegIdx

[rw] Selects segment array element number

Field size: 6 bits

The specified array element can be read or written via hyplnkRXSegValReg_s after the index is written.

The documentation for this struct was generated from the following file:

- hyplnk.h

Copyright 2012, Texas Instruments Incorporated