# Srio_Type11BindAddrInfo Struct Reference
[SRIO LLD Data Structures]

SRIO Socket Type11 Binding Information. More...

`#include <srio_drv.h>`

## Data Fields

uint16_t | tt
| Transport Type; 16 bit or 8 bit identifiers.
uint16_t | id
| This is the 8 bit or 16 bit SRIO identifier.
uint16_t | letter
| Letter Identifier.
uint16_t | mbox
| Mailbox number.
uint16_t | segMap
| Segmentation Mapping Set to 0 for single segment and 1 for multi segment.

## Detailed Description

SRIO Socket Type11 Binding Information.

The structure describes the address information required for binding a Type11 socket. This includes information which describes the Type11 endpoint characteristics and is used to describe the local characteristics of the endpoint.

The documentation for this struct was generated from the following file:

- srio_drv.h

Copyright 2012, Texas Instruments Incorporated