# Qmss_QosSrioCfg Struct Reference

QoS SRIO Tracking configuration structure. More...

`#include <qmss_qos.h>`

## Data Fields

uint8_t | queCount
uint16_t | queBase
Qmss_QosSrioTXQCfg | TXQs [QMSS_QOS_SRIO_MAX_TX_Q]

## Detailed Description

QoS SRIO Tracking configuration structure.

## Field Documentation

uint16_t Qmss_QosSrioCfg::queBase

The Queue index of the base queue of the SRIO queue cluster. This value must be a multiple of 32.

uint8_t Qmss_QosSrioCfg::queCount

The number of queues to monitor. This controls both the number of valid TXQ entries in this structure, plus the number of queues considered valid from the SRIO base queue index.

The valid range is QMSS_QOS_SRIO_MIN_TX_Q to QMSS_QOS_SRIO_MAX_TX_Q.

Qmss_QosSrioTXQCfg Qmss_QosSrioCfg::TXQs[QMSS_QOS_SRIO_MAX_TX_Q]

Configurations for each queue requested via queCount

The documentation for this struct was generated from the following file:

- qmss_qos.h

Copyright 2012, Texas Instruments Incorporated