# hyplnkRXPrivIDValReg_s Struct Reference
[HYPLNK LLD Register Definitions]

Specification of the Rx Address PrivID Value Register. More...

`#include <hyplnk.h>`

## Data Fields

uint32_t | raw
| [ro] Raw image of register on read; actual value on write
uint8_t | rxPrivIDVal
| [rw] Selects PrivID value

## Detailed Description

Specification of the Rx Address PrivID Value Register.

## Field Documentation

uint8_t hyplnkRXPrivIDValReg_s::rxPrivIDVal

[rw] Selects PrivID value

Field size: 4 bits

Specifies the PrivID in the PrivID lookup table at the position specified by hyplnkRXPrivIDIdxReg_s::rxPrivIDIdx. This is used to dereference the PrivID from the address bits selected by hyplnkRXAddrSelReg_s::rxPrivIDSel.

The documentation for this struct was generated from the following file:

- hyplnk.h

Copyright 2012, Texas Instruments Incorporated