# hyplnkRevReg_s Struct Reference
[HYPLNK LLD Register Definitions]

Specification of the HyperLink Revision Register. More...

`#include <hyplnk.h>`

## Data Fields

uint32_t | raw
| [ro] Raw image of register on read; actual value on write
uint8_t | scheme
| [ro] Scheme
uint8_t | bu
| [ro] Business Unit
uint16_t | func
| [ro] Function identifier
uint8_t | rtl
| [ro] RTL Version
uint8_t | cust
| [ro] Customer special version
uint8_t | revMaj
| [ro] Major revision
uint8_t | revMin
| [ro] Minor revision

## Detailed Description

Specification of the HyperLink Revision Register.

The Revision Register contains the major and minor revisions for the HyperLink module.

## Field Documentation

uint8_t hyplnkRevReg_s::bu

[ro] Business Unit

Field size: 2 bits

uint8_t hyplnkRevReg_s::cust

[ro] Customer special version

Field size: 2 bits

uint16_t hyplnkRevReg_s::func

[ro] Function identifier

0xe90 is HyperLink

Field size: 12 bits

uint8_t hyplnkRevReg_s::revMaj

[ro] Major revision

Field size: 3 bits

uint8_t hyplnkRevReg_s::revMin

[ro] Minor revision

Field size: 6 bits

uint8_t hyplnkRevReg_s::rtl

[ro] RTL Version

Field size: 5 bits

uint8_t hyplnkRevReg_s::scheme

[ro] Scheme

Field size: 2 bits

The documentation for this struct was generated from the following file:

- hyplnk.h

Copyright 2012, Texas Instruments Incorporated