# CSL_Edma3CmdDrae Struct Reference
[EDMA3 Data Structures]

Edma Command Structure for setting region specific attributes. More...

`#include <csl_edma3.h>`

## Data Fields

Int | region
CSL_BitMask32 | drae
CSL_BitMask32 | draeh

## Detailed Description

Edma Command Structure for setting region specific attributes.

An object of this type is allocated by the user and its address is passed as a parameter to the CSL_edma3GetHwStatus when

## Field Documentation

CSL_BitMask32 CSL_Edma3CmdDrae::drae

DRAE Setting for the region

CSL_BitMask32 CSL_Edma3CmdDrae::draeh

DRAEH Setting for the region

Int CSL_Edma3CmdDrae::region

this field needs to be initialiazed by the user before issuing the command specifying the region for which attributes need to be set

The documentation for this struct was generated from the following file:

- csl_edma3.h

Copyright 2012, Texas Instruments Incorporated