# CHIP Enumerated Data Types
[CHIP]

## Enumerations

enum | CSL_ChipReg { CSL_CHIP_AMR = 0, CSL_CHIP_CSR = 1, CSL_CHIP_IFR = 2, CSL_CHIP_ISR = 2, CSL_CHIP_ICR = 3, CSL_CHIP_IER = 4, CSL_CHIP_ISTP = 5, CSL_CHIP_IRP = 6, CSL_CHIP_NRP = 7, CSL_CHIP_ERP = 7, CSL_CHIP_TSCL = 10, CSL_CHIP_TSCH = 11, CSL_CHIP_ARP = 12, CSL_CHIP_ILC = 13, CSL_CHIP_RILC = 14, CSL_CHIP_REP = 15,
CSL_CHIP_PCE1 = 16, CSL_CHIP_DNUM = 17, CSL_CHIP_SSR = 21, CSL_CHIP_GPLYA = 22,
CSL_CHIP_GPLYB = 23, CSL_CHIP_GFPGFR = 24, CSL_CHIP_DIER = 25, CSL_CHIP_TSR = 26,
CSL_CHIP_ITSR = 27, CSL_CHIP_NTSR = 28, CSL_CHIP_EFR = 29, CSL_CHIP_ECR = 29,
CSL_CHIP_IERR = 31
}

## Enumeration Type Documentation

enum CSL_ChipReg

Enum for the CHIP registers

Enumerator:

  CSL_CHIP_AMR | Addressing Mode Register
  CSL_CHIP_CSR | Control Status Register
  CSL_CHIP_IFR | Interrupt Flag Register
  CSL_CHIP_ISR | Interrupt Set Register
  CSL_CHIP_ICR | Interrupt Clear Register
  CSL_CHIP_IER | Interrupt Enable Register
  CSL_CHIP_ISTP | Interrupt Service Table Pointer Register
  CSL_CHIP_IRP | Interrupt Return Pointer Register
  CSL_CHIP_NRP | Nonmaskable Interrupt (NMI) Return Pointer Register
  CSL_CHIP_ERP | Exception Return Pointer Register
  CSL_CHIP_TSCL | Time Stamp Counter Register - Low
  CSL_CHIP_TSCH | Time Stamp Counter Registers - High
  CSL_CHIP_ARP | Analysis Return Pointer
  CSL_CHIP_ILC | SPLOOP Inner Loop Count Register
  CSL_CHIP_RILC | SPLOOP Reload Inner Loop Count Register
  CSL_CHIP_REP | Restricted Entry Point Address Register
  CSL_CHIP_PCE1 | E1 Phase Program Counter
  CSL_CHIP_DNUM | DSP Core Number Register
  CSL_CHIP_SSR | Saturation Status Register
  CSL_CHIP_GPLYA | GMPY Polynomial.A Side Register
  CSL_CHIP_GPLYB | GMPY Polynomial.B Side Register
  CSL_CHIP_GFPGFR | Galois Field Polynomial Generator Function Register
  CSL_CHIP_DIER | Debug interrupt enable register
  CSL_CHIP_TSR | Task State Register
  CSL_CHIP_ITSR | Interrupt Task State Register
  CSL_CHIP_NTSR | NMI/Exception Task State Register
  CSL_CHIP_EFR | Exception Flag Register
  CSL_CHIP_ECR | Exception Clear Register
  CSL_CHIP_IERR | Internal Exception Report Register

Copyright 2012, Texas Instruments Incorporated