# pcieType1Bar32bitIdx_s Struct Reference
[PCIE LLD Type1 (root) Register Definitions]

pcieBar32bitReg_s register plus an index (Root Complex BAR) More...

`#include <pcie.h>`

## Data Fields

pcieBar32bitReg_t | reg
| Register Structure.
uint8_t | idx
| Index in the array of registers of this type.

## Detailed Description

pcieBar32bitReg_s register plus an index (Root Complex BAR)

There are multiple instances of this register. The index is used to select which instance of the register will be accessed.

This structure is used to access a Root Complex BAR. For more details, please refer to pcieBar32bitReg_t.

The documentation for this struct was generated from the following file:

- pcie.h

Copyright 2012, Texas Instruments Incorporated