[10:30:51]  TESTING = false
[10:30:51]  RstdNet: Port 2777: Listening..
[10:30:51]  
[10:30:51]  ***Script completed successfully.***
[10:31:28]  [RadarAPI]: ar1.selectRadarMode(1)
[10:31:28]  [RadarAPI]: ar1.selectCascadeMode(1)
[10:31:28]  [RadarAPI]: Status: Passed
[10:31:28]  [RadarAPI]: Status: Passed
[10:31:32]  [RadarAPI]: ar1.SelectCaptureDevice("TDA2XX")
[10:31:32]  [RadarAPI]: Status: Passed
[10:31:34]  [RadarAPI]: TDAStatusCallback Event Registered
[10:31:34]  [RadarAPI]: registerTDAStatusCallback Status: Passed
[10:31:34]  [RadarAPI]: ar1.ConnectTDA("192.168.33.180", 5001, 15)
[10:31:34]  [RadarAPI]: Device 32 : CAPTURE_RESPONSE_ACK Async event recieved() with status 0 
[10:31:34]  [RadarAPI]: Device 32 : CAPTURE_RESPONSE_VERSION_INFO Async event recieved() with status 0. TDA Version : REL_VISION_SDK_03_07_01_00 Aug  5 2019 15:04:45[10:31:34]  [RadarAPI]: Device 32 : CAPTURE_RESPONSE_ACK Async event recieved() with status 0 
[10:31:35]  [RadarAPI]: Device 1 : CAPTURE_RESPONSE_ACK Async event recieved() with status 0 
[10:31:36]  [RadarAPI]: ConnectTDACaptureCard Status: Passed
[10:31:36]  TDA Capture Card Status : CONNECTED!
[10:33:01]  [RadarAPI]: Device 1 : CAPTURE_RESPONSE_ACK Async event recieved() with status 0 
[10:33:01]  [RadarAPI]: ar1.FullReset(1)
[10:33:01]  [RadarAPI]: Status: Passed
[10:33:03]  [RadarAPI]: Device 1 : CAPTURE_RESPONSE_ACK Async event recieved() with status 0 
[10:33:03]  [RadarAPI]: Device 1 : CAPTURE_RESPONSE_ACK Async event recieved() with status 0 
[10:33:04]  [RadarAPI]: ar1.FullReset(1)
[10:33:04]  [RadarAPI]: Status: Passed
[10:33:04]  [RadarAPI]: ar1.SOPControl_mult(1,4)
[10:33:04]  [RadarAPI]: Status: Passed
[10:33:05]  [RadarAPI]: ar1.PowerOn_mult(1, 0, 1000, 0,0)
[10:33:05]  [RadarAPI]: Status: Passed
[10:33:05]  [DeviceId-0] MSS power up done async event received!
[10:33:22]  [RadarAPI]: ar1.DownloadBSSFw_mult(1,"C:\\ti\\mmwave_dfp_02_02_02_01\\firmware\\xwr22xx_metaImage.bin")
[10:33:22]  [RadarAPI]: ar1.DownloadBssFwOvSPI_mult(1, C:\\ti\\mmwave_dfp_02_02_02_01\\firmware\\xwr22xx_metaImage.bin)
[10:33:34]  [RadarAPI]: ar1.SelectChipVersion("AR1243")
[10:33:34]  [RadarAPI]: Status: Passed
[10:33:34]  [RadarAPI]: ar1.SelectChipVersion("AR1243")
[10:33:34]  [RadarAPI]: Status: Passed
[10:33:34]  [RadarAPI]: ar1.deviceVariantSelection("XWR2243")
[10:33:34]  [RadarAPI]: Status: Passed
[10:33:34]  [RadarAPI]: ar1.frequencyBandSelection("77G")
[10:33:34]  [RadarAPI]: ar1.SelectChipVersion("XWR2243")
[10:33:34]  [RadarAPI]: Status: Passed
[10:33:34]  Device Status : XWR2243/ASIL-B/SOP:4/ES:1.1
[10:33:34]  [RadarAPI]: ar1.RfEnable_mult(1)
[10:33:35]  [RadarAPI]: Status: Passed
[10:33:35]  [DeviceId-0] BSS power up done async event received!
[10:33:42]  [RadarAPI]: Device 2 : CAPTURE_RESPONSE_ACK Async event recieved() with status 0 
[10:33:42]  [RadarAPI]: Device 2 : CAPTURE_RESPONSE_ACK Async event recieved() with status 0 
[10:33:42]  [RadarAPI]: ar1.FullReset(2)
[10:33:42]  [RadarAPI]: Status: Passed
[10:33:42]  [RadarAPI]: ar1.SOPControl_mult(2,4)
[10:33:42]  [RadarAPI]: Status: Passed
[10:33:44]  [RadarAPI]: ar1.DownloadBSSFw_mult(2,"C:\\ti\\mmwave_dfp_02_02_02_01\\firmware\\xwr22xx_metaImage.bin")
[10:33:44]  [RadarAPI]: ar1.DownloadBssFwOvSPI_mult(2, C:\\ti\\mmwave_dfp_02_02_02_01\\firmware\\xwr22xx_metaImage.bin)
[10:33:44]  [RadarAPI]: Error: Download FW failed with error -2
[10:33:50]  [RadarAPI]: ar1.AddDevice(2)
[10:33:50]  [RadarAPI]: Status: Passed
[10:33:50]  [DeviceId-1] MSS power up done async event received!
[10:33:53]  [RadarAPI]: ar1.DownloadBSSFw_mult(2,"C:\\ti\\mmwave_dfp_02_02_02_01\\firmware\\xwr22xx_metaImage.bin")
[10:33:53]  [RadarAPI]: ar1.DownloadBssFwOvSPI_mult(2, C:\\ti\\mmwave_dfp_02_02_02_01\\firmware\\xwr22xx_metaImage.bin)
[10:33:58]  [RadarAPI]: ar1.SelectChipVersion("AR1243")
[10:33:58]  [RadarAPI]: Status: Passed
[10:33:58]  [RadarAPI]: ar1.SelectChipVersion("XWR2243")
[10:33:58]  [RadarAPI]: Status: Passed
[10:33:58]  Slave1 Device Status : XWR2243/ASIL-B/SOP:4/ES:1.1
[10:33:58]  [RadarAPI]: ar1.RfEnable_mult(2)
[10:33:58]  [DeviceId-1] BSS power up done async event received!
[10:33:58]  [RadarAPI]: Status: Passed
[10:34:09]  [RadarAPI]: Device 4 : CAPTURE_RESPONSE_ACK Async event recieved() with status 0 
[10:34:11]  [RadarAPI]: Device 4 : CAPTURE_RESPONSE_ACK Async event recieved() with status 0 
[10:34:11]  [RadarAPI]: ar1.AddDevice(4)
[10:34:11]  [RadarAPI]: Status: Passed
[10:34:12]  [DeviceId-2] MSS power up done async event received!
[10:34:12]  [RadarAPI]: ar1.FullReset(4)
[10:34:12]  [RadarAPI]: Status: Passed
[10:34:12]  [RadarAPI]: ar1.SOPControl_mult(4,4)
[10:34:12]  [RadarAPI]: Status: Passed
[10:34:15]  [RadarAPI]: ar1.DownloadBSSFw_mult(4,"C:\\ti\\mmwave_dfp_02_02_02_01\\firmware\\xwr22xx_metaImage.bin")
[10:34:16]  [RadarAPI]: ar1.DownloadBssFwOvSPI_mult(4, C:\\ti\\mmwave_dfp_02_02_02_01\\firmware\\xwr22xx_metaImage.bin)
[10:34:25]  [RadarAPI]: Device 8 : CAPTURE_RESPONSE_ACK Async event recieved() with status 0 
[10:34:25]  [RadarAPI]: Device 8 : CAPTURE_RESPONSE_ACK Async event recieved() with status 0 
[10:34:25]  [RadarAPI]: ar1.FullReset(8)
[10:34:25]  [RadarAPI]: Status: Passed
[10:34:25]  [RadarAPI]: ar1.SOPControl_mult(8,4)
[10:34:25]  [RadarAPI]: Status: Passed
[10:34:30]  [RadarAPI]: ar1.AddDevice(8)
[10:34:30]  [RadarAPI]: Status: Passed
[10:34:30]  [DeviceId-3] MSS power up done async event received!
[10:34:32]  [RadarAPI]: ar1.DownloadBSSFw_mult(8,"C:\\ti\\mmwave_dfp_02_02_02_01\\firmware\\xwr22xx_metaImage.bin")
[10:34:33]  [RadarAPI]: ar1.DownloadBssFwOvSPI_mult(8, C:\\ti\\mmwave_dfp_02_02_02_01\\firmware\\xwr22xx_metaImage.bin)
[10:34:37]  [RadarAPI]: ar1.SelectChipVersion("AR1243")
[10:34:37]  [RadarAPI]: Status: Passed
[10:34:37]  [RadarAPI]: ar1.SelectChipVersion("XWR2243")
[10:34:37]  [RadarAPI]: Status: Passed
[10:34:37]  Slave3 Device Status : XWR2243/ASIL-B/SOP:4/ES:1.1
[10:34:37]  [RadarAPI]: ar1.RfEnable_mult(8)
[10:34:37]  [DeviceId-3] BSS power up done async event received!
[10:34:37]  [RadarAPI]: Status: Passed
[10:34:49]  [RadarAPI]: ar1.SelectChipVersion("AR1243")
[10:34:49]  [RadarAPI]: Status: Passed
[10:34:49]  [RadarAPI]: ar1.SelectChipVersion("XWR2243")
[10:34:49]  [RadarAPI]: Status: Passed
[10:34:49]  Slave2 Device Status : XWR2243/ASIL-B/SOP:4/ES:1.1
[10:34:49]  [RadarAPI]: ar1.RfEnable_mult(4)
[10:34:49]  [DeviceId-2] BSS power up done async event received!
[10:34:49]  [RadarAPI]: Status: Passed
[10:36:51]  [RadarAPI]: ar1.DownloadBSSFw_mult(2,"C:\\ti\\mmwave_dfp_02_02_02_01\\firmware\\xwr22xx_metaImage.bin")
[10:36:51]  [RadarAPI]: ar1.DownloadBssFwOvSPI_mult(2, C:\\ti\\mmwave_dfp_02_02_02_01\\firmware\\xwr22xx_metaImage.bin)