
**** Build of configuration Debug for project TDC7200_basic_spi_rw ****

"C:\\ti\\ccsv6\\utils\\bin\\gmake" -k all 
'Building file: C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/F5xx_F6xx_Core_Lib/HAL_PMM.c'
'Invoking: MSP430 Compiler'
"C:/ti/ccsv6/tools/compiler/ti-cgt-msp430_4.4.3/bin/cl430" -vmspx --abi=eabi --data_model=restricted --use_hw_mpy=F5 --include_path="C:/ti/ccsv6/ccs_base/msp430/include" --include_path="C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/include" --include_path="C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/F5xx_F6xx_Core_Lib" --include_path="C:/ti/ccsv6/tools/compiler/ti-cgt-msp430_4.4.3/include" --advice:power=all -g --define=__MSP430F5529__ --diag_warning=225 --display_error_number --diag_wrap=off --silicon_errata=CPU21 --silicon_errata=CPU22 --silicon_errata=CPU23 --silicon_errata=CPU40 --printf_support=minimal --preproc_with_compile --preproc_dependency="HAL_PMM.pp"  "C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/F5xx_F6xx_Core_Lib/HAL_PMM.c"
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/F5xx_F6xx_Core_Lib/HAL_PMM.c", line 135: remark #1528-D: (ULP 3.1) Detected flag polling using PMMIFG. Recommend using an interrupt combined with enter LPMx and ISR
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/F5xx_F6xx_Core_Lib/HAL_PMM.c", line 147: remark #1528-D: (ULP 3.1) Detected flag polling using PMMIFG. Recommend using an interrupt combined with enter LPMx and ISR
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/F5xx_F6xx_Core_Lib/HAL_PMM.c", line 162: remark #1528-D: (ULP 3.1) Detected flag polling using PMMIFG. Recommend using an interrupt combined with enter LPMx and ISR
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/F5xx_F6xx_Core_Lib/HAL_PMM.c", line 174: remark #1528-D: (ULP 3.1) Detected flag polling using PMMIFG. Recommend using an interrupt combined with enter LPMx and ISR
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/F5xx_F6xx_Core_Lib/HAL_PMM.c", line 201: remark #1528-D: (ULP 3.1) Detected flag polling using PMMIFG. Recommend using an interrupt combined with enter LPMx and ISR
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/F5xx_F6xx_Core_Lib/HAL_PMM.c", line 246: remark #1528-D: (ULP 3.1) Detected flag polling using PMMIFG. Recommend using an interrupt combined with enter LPMx and ISR
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/F5xx_F6xx_Core_Lib/HAL_PMM.c", line 276: remark #1528-D: (ULP 3.1) Detected flag polling using PMMIFG. Recommend using an interrupt combined with enter LPMx and ISR
'Finished building: C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/F5xx_F6xx_Core_Lib/HAL_PMM.c'
' '
'Building file: C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/library/TI_MSP430_spi_USCIB0_5xx.c'
'Invoking: MSP430 Compiler'
"C:/ti/ccsv6/tools/compiler/ti-cgt-msp430_4.4.3/bin/cl430" -vmspx --abi=eabi --data_model=restricted --use_hw_mpy=F5 --include_path="C:/ti/ccsv6/ccs_base/msp430/include" --include_path="C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/include" --include_path="C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/F5xx_F6xx_Core_Lib" --include_path="C:/ti/ccsv6/tools/compiler/ti-cgt-msp430_4.4.3/include" --advice:power=all -g --define=__MSP430F5529__ --diag_warning=225 --display_error_number --diag_wrap=off --silicon_errata=CPU21 --silicon_errata=CPU22 --silicon_errata=CPU23 --silicon_errata=CPU40 --printf_support=minimal --preproc_with_compile --preproc_dependency="TI_MSP430_spi_USCIB0_5xx.pp"  "C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/library/TI_MSP430_spi_USCIB0_5xx.c"
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/library/TI_MSP430_spi_USCIB0_5xx.c", line 119: remark #1528-D: (ULP 3.1) Detected flag polling using UCTXIFG. Recommend using an interrupt combined with enter LPMx and ISR
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/library/TI_MSP430_spi_USCIB0_5xx.c", line 123: remark #1528-D: (ULP 3.1) Detected flag polling using UCTXIFG. Recommend using an interrupt combined with enter LPMx and ISR
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/library/TI_MSP430_spi_USCIB0_5xx.c", line 127: remark #1528-D: (ULP 3.1) Detected flag polling using UCBUSY. Recommend using an interrupt combined with enter LPMx and ISR
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/library/TI_MSP430_spi_USCIB0_5xx.c", line 154: remark #1528-D: (ULP 3.1) Detected flag polling using UCTXIFG. Recommend using an interrupt combined with enter LPMx and ISR
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/library/TI_MSP430_spi_USCIB0_5xx.c", line 157: remark #1528-D: (ULP 3.1) Detected flag polling using UCTXIFG. Recommend using an interrupt combined with enter LPMx and ISR
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/library/TI_MSP430_spi_USCIB0_5xx.c", line 160: remark #1528-D: (ULP 3.1) Detected flag polling using UCBUSY. Recommend using an interrupt combined with enter LPMx and ISR
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/library/TI_MSP430_spi_USCIB0_5xx.c", line 166: remark #1528-D: (ULP 3.1) Detected flag polling using UCBUSY. Recommend using an interrupt combined with enter LPMx and ISR
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/library/TI_MSP430_spi_USCIB0_5xx.c", line 203: remark #1528-D: (ULP 3.1) Detected flag polling using UCTXIFG. Recommend using an interrupt combined with enter LPMx and ISR
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/library/TI_MSP430_spi_USCIB0_5xx.c", line 209: remark #1528-D: (ULP 3.1) Detected flag polling using UCTXIFG. Recommend using an interrupt combined with enter LPMx and ISR
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/library/TI_MSP430_spi_USCIB0_5xx.c", line 213: remark #1528-D: (ULP 3.1) Detected flag polling using UCBUSY. Recommend using an interrupt combined with enter LPMx and ISR
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/library/TI_MSP430_spi_USCIB0_5xx.c", line 207: remark #1544-D: (ULP 13.1) Detected loop counting up. Recommend loops count down as detecting zeros is easier
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/library/TI_MSP430_spi_USCIB0_5xx.c", line 244: remark #1528-D: (ULP 3.1) Detected flag polling using UCTXIFG. Recommend using an interrupt combined with enter LPMx and ISR
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/library/TI_MSP430_spi_USCIB0_5xx.c", line 250: remark #1528-D: (ULP 3.1) Detected flag polling using UCTXIFG. Recommend using an interrupt combined with enter LPMx and ISR
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/library/TI_MSP430_spi_USCIB0_5xx.c", line 253: remark #1528-D: (ULP 3.1) Detected flag polling using UCBUSY. Recommend using an interrupt combined with enter LPMx and ISR
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/library/TI_MSP430_spi_USCIB0_5xx.c", line 258: remark #1528-D: (ULP 3.1) Detected flag polling using UCRXIFG. Recommend using an interrupt combined with enter LPMx and ISR
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/library/TI_MSP430_spi_USCIB0_5xx.c", line 248: remark #1544-D: (ULP 13.1) Detected loop counting up. Recommend loops count down as detecting zeros is easier
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/library/TI_MSP430_spi_USCIB0_5xx.c", line 289: remark #1528-D: (ULP 3.1) Detected flag polling using UCTXIFG. Recommend using an interrupt combined with enter LPMx and ISR
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/library/TI_MSP430_spi_USCIB0_5xx.c", line 295: remark #1528-D: (ULP 3.1) Detected flag polling using UCTXIFG. Recommend using an interrupt combined with enter LPMx and ISR
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/library/TI_MSP430_spi_USCIB0_5xx.c", line 299: remark #1528-D: (ULP 3.1) Detected flag polling using UCBUSY. Recommend using an interrupt combined with enter LPMx and ISR
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/library/TI_MSP430_spi_USCIB0_5xx.c", line 304: remark #1528-D: (ULP 3.1) Detected flag polling using UCRXIFG. Recommend using an interrupt combined with enter LPMx and ISR
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/library/TI_MSP430_spi_USCIB0_5xx.c", line 293: remark #1544-D: (ULP 13.1) Detected loop counting up. Recommend loops count down as detecting zeros is easier
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/library/TI_MSP430_spi_USCIB0_5xx.c", line 279: remark #1535-D: (ULP 8.1) variable "inst" is used as a constant. Recommend declaring variable as either 'static const' or 'const'
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/library/TI_MSP430_spi_USCIB0_5xx.c", line 348: remark #1528-D: (ULP 3.1) Detected flag polling using UCTXIFG. Recommend using an interrupt combined with enter LPMx and ISR
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/library/TI_MSP430_spi_USCIB0_5xx.c", line 351: remark #1528-D: (ULP 3.1) Detected flag polling using UCTXIFG. Recommend using an interrupt combined with enter LPMx and ISR
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/library/TI_MSP430_spi_USCIB0_5xx.c", line 354: remark #1528-D: (ULP 3.1) Detected flag polling using UCBUSY. Recommend using an interrupt combined with enter LPMx and ISR
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/library/TI_MSP430_spi_USCIB0_5xx.c", line 358: remark #1528-D: (ULP 3.1) Detected flag polling using UCRXIFG. Recommend using an interrupt combined with enter LPMx and ISR
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/library/TI_MSP430_spi_USCIB0_5xx.c", line 363: remark #1528-D: (ULP 3.1) Detected flag polling using UCTXIFG. Recommend using an interrupt combined with enter LPMx and ISR
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/library/TI_MSP430_spi_USCIB0_5xx.c", line 366: remark #1528-D: (ULP 3.1) Detected flag polling using UCBUSY. Recommend using an interrupt combined with enter LPMx and ISR
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/library/TI_MSP430_spi_USCIB0_5xx.c", line 374: remark #1528-D: (ULP 3.1) Detected flag polling using UCTXIFG. Recommend using an interrupt combined with enter LPMx and ISR
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/library/TI_MSP430_spi_USCIB0_5xx.c", line 377: remark #1528-D: (ULP 3.1) Detected flag polling using UCBUSY. Recommend using an interrupt combined with enter LPMx and ISR
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/library/TI_MSP430_spi_USCIB0_5xx.c", line 417: remark #1528-D: (ULP 3.1) Detected flag polling using UCTXIFG. Recommend using an interrupt combined with enter LPMx and ISR
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/library/TI_MSP430_spi_USCIB0_5xx.c", line 421: remark #1528-D: (ULP 3.1) Detected flag polling using UCTXIFG. Recommend using an interrupt combined with enter LPMx and ISR
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/library/TI_MSP430_spi_USCIB0_5xx.c", line 424: remark #1528-D: (ULP 3.1) Detected flag polling using UCBUSY. Recommend using an interrupt combined with enter LPMx and ISR
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/library/TI_MSP430_spi_USCIB0_5xx.c", line 428: remark #1528-D: (ULP 3.1) Detected flag polling using UCRXIFG. Recommend using an interrupt combined with enter LPMx and ISR
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/library/TI_MSP430_spi_USCIB0_5xx.c", line 432: remark #1528-D: (ULP 3.1) Detected flag polling using UCTXIFG. Recommend using an interrupt combined with enter LPMx and ISR
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/library/TI_MSP430_spi_USCIB0_5xx.c", line 435: remark #1528-D: (ULP 3.1) Detected flag polling using UCBUSY. Recommend using an interrupt combined with enter LPMx and ISR
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/library/TI_MSP430_spi_USCIB0_5xx.c", line 439: remark #1528-D: (ULP 3.1) Detected flag polling using UCRXIFG. Recommend using an interrupt combined with enter LPMx and ISR
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/library/TI_MSP430_spi_USCIB0_5xx.c", line 443: remark #1528-D: (ULP 3.1) Detected flag polling using UCTXIFG. Recommend using an interrupt combined with enter LPMx and ISR
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/library/TI_MSP430_spi_USCIB0_5xx.c", line 446: remark #1528-D: (ULP 3.1) Detected flag polling using UCBUSY. Recommend using an interrupt combined with enter LPMx and ISR
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/library/TI_MSP430_spi_USCIB0_5xx.c", line 450: remark #1528-D: (ULP 3.1) Detected flag polling using UCRXIFG. Recommend using an interrupt combined with enter LPMx and ISR
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/library/TI_MSP430_spi_USCIB0_5xx.c", line 457: remark #1540-D: (ULP 11.2) Assignment of higher bits (constants) to "PAOUT_L" within a loop. Recommend using lower 4 bits to allow use of constant generators
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/library/TI_MSP430_spi_USCIB0_5xx.c", line 478: remark #1528-D: (ULP 3.1) Detected flag polling using UCTXIFG. Recommend using an interrupt combined with enter LPMx and ISR
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/library/TI_MSP430_spi_USCIB0_5xx.c", line 484: remark #1528-D: (ULP 3.1) Detected flag polling using UCTXIFG. Recommend using an interrupt combined with enter LPMx and ISR
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/library/TI_MSP430_spi_USCIB0_5xx.c", line 488: remark #1528-D: (ULP 3.1) Detected flag polling using UCBUSY. Recommend using an interrupt combined with enter LPMx and ISR
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/library/TI_MSP430_spi_USCIB0_5xx.c", line 490: remark #1528-D: (ULP 3.1) Detected flag polling using UCRXIFG. Recommend using an interrupt combined with enter LPMx and ISR
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/library/TI_MSP430_spi_USCIB0_5xx.c", line 482: remark #1544-D: (ULP 13.1) Detected loop counting up. Recommend loops count down as detecting zeros is easier
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/library/TI_MSP430_spi_USCIB0_5xx.c", line 470: remark #1535-D: (ULP 8.1) variable "inst" is used as a constant. Recommend declaring variable as either 'static const' or 'const'
'Finished building: C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/library/TI_MSP430_spi_USCIB0_5xx.c'
' '
'Building file: C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/demo_apps/demo1_tdc720x_basic_rw/main.c'
'Invoking: MSP430 Compiler'
"C:/ti/ccsv6/tools/compiler/ti-cgt-msp430_4.4.3/bin/cl430" -vmspx --abi=eabi --data_model=restricted --use_hw_mpy=F5 --include_path="C:/ti/ccsv6/ccs_base/msp430/include" --include_path="C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/include" --include_path="C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/F5xx_F6xx_Core_Lib" --include_path="C:/ti/ccsv6/tools/compiler/ti-cgt-msp430_4.4.3/include" --advice:power=all -g --define=__MSP430F5529__ --diag_warning=225 --display_error_number --diag_wrap=off --silicon_errata=CPU21 --silicon_errata=CPU22 --silicon_errata=CPU23 --silicon_errata=CPU40 --printf_support=minimal --preproc_with_compile --preproc_dependency="main.pp"  "C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/demo_apps/demo1_tdc720x_basic_rw/main.c"
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/demo_apps/demo1_tdc720x_basic_rw/main.c", line 141: remark #1527-D: (ULP 2.1) Detected SW delay loop using __delay_cycles. Recommend using a timer module instead
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/demo_apps/demo1_tdc720x_basic_rw/main.c", line 142: remark #1527-D: (ULP 2.1) Detected SW delay loop using __delay_cycles. Recommend using a timer module instead
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/demo_apps/demo1_tdc720x_basic_rw/main.c", line 184: remark #1527-D: (ULP 2.1) Detected SW delay loop using __delay_cycles. Recommend using a timer module instead
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/demo_apps/demo1_tdc720x_basic_rw/main.c", line 204: remark #1527-D: (ULP 2.1) Detected SW delay loop using __delay_cycles. Recommend using a timer module instead
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/demo_apps/demo1_tdc720x_basic_rw/main.c", line 213: remark #1527-D: (ULP 2.1) Detected SW delay loop using __delay_cycles. Recommend using a timer module instead
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/demo_apps/demo1_tdc720x_basic_rw/main.c", line 225: remark #1527-D: (ULP 2.1) Detected SW delay loop using __delay_cycles. Recommend using a timer module instead
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/demo_apps/demo1_tdc720x_basic_rw/main.c", line 68: remark #1535-D: (ULP 8.1) variable "tout" is used as a constant. Recommend declaring variable as either 'static const' or 'const'
"C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/demo_apps/demo1_tdc720x_basic_rw/main.c", line 70: remark #1535-D: (ULP 8.1) variable "TDC720x_Parallel_Read" is used as a constant. Recommend declaring variable as either 'static const' or 'const'
'Finished building: C:/Users/a0415888/Documents/pwd/GIT_REPOS/TDC7200/tdc7200evm_fw/code/demo_apps/demo1_tdc720x_basic_rw/main.c'
' '
'Building target: TDC7200_basic_spi_rw.out'
'Invoking: MSP430 Linker'
"C:/ti/ccsv6/tools/compiler/ti-cgt-msp430_4.4.3/bin/cl430" -vmspx --abi=eabi --data_model=restricted --use_hw_mpy=F5 --advice:power=all -g --define=__MSP430F5529__ --diag_warning=225 --display_error_number --diag_wrap=off --silicon_errata=CPU21 --silicon_errata=CPU22 --silicon_errata=CPU23 --silicon_errata=CPU40 --printf_support=minimal -z -m"TDC7200_basic_spi_rw.map" --heap_size=160 --stack_size=160 --cinit_hold_wdt=on -i"C:/ti/ccsv6/ccs_base/msp430/include" -i"C:/ti/ccsv6/tools/compiler/ti-cgt-msp430_4.4.3/lib" -i"C:/ti/ccsv6/tools/compiler/ti-cgt-msp430_4.4.3/include" -i"C:/ti/ccsv6/ccs_base/msp430/lib/5xx_6xx_FRxx" --reread_libs --warn_sections --display_error_number --diag_wrap=off --xml_link_info="TDC7200_basic_spi_rw_linkInfo.xml" --use_hw_mpy=F5 --rom_model -o "TDC7200_basic_spi_rw.out" "./HAL_PMM.obj" "./TI_MSP430_spi_USCIB0_5xx.obj" "./main.obj" "../lnk_msp430f5529.cmd"  -l"libmath.a" -l"libc.a" 
<Linking>
remark #10372-D: (ULP 4.1) Detected uninitialized Port D in this project. Recommend initializing all unused ports to eliminate wasted current consumption on unused pins.
'Finished building target: TDC7200_basic_spi_rw.out'
' '

**** Build Finished ****
