Unfortunately it is not possible to generate identical telegrams.
The main reason for this is that the telegrams which are provided from the customer are already decrypted and I don't have an encryption key.
Furthermore even if I know the encryption key I need more than 1 ore 2 ours to generate identical telegrams.

What I have done is the following:

I flashed the binary Serial_CC13xx_Collector_T2.out (v1.2.0) to a CC1350 Launchpad rev1.2.0.
I configured a meter to transmit periodical telegrams which have the same length as the telegrams from the customer (see picture below).
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The same data decrypted (see picture below):

[image: cid:b8255db49ccc088705757e6b9c76da0b2c6d3b6b@zimbra]

Using the CC1350 collector I was able to receive all telegrams (see picture below):

[image: cid:47e90e5c46859810f96b281d8977f72a378ba127@zimbra]

As you see in the screenshots from the sniffer the access number is increased in every telegram and the data collector was able to receive all telegrams.
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