MSP430™CapTIvateSoftwareLibraryAPIGuide 1_70_00_03

Data Fields
IQ16_t Union Reference
CAPT_TYPE

typedef IQ16_t More...

`#include <CAPT_Type.h>`

## Data Fields
struct {
uint16_t ui16Decimal
| Lower 16; Decimal Bits. More...
uint16_t ui16Natural
| Upper 16; Integer Bits. More...
}; |
uint32_t | ui32Full
| Full 32 bits. More...

## Detailed Description

typedef IQ16_t

IQ16_t is a fixed-point integer/fractional data type. Common type used mainly for filtered values. The upper 16bits will be the natural (integer) values, and the lower 16bits will be the decimal section.

## Field Documentation

## § ui16Decimal

uint16_t IQ16_t::ui16Decimal

Lower 16; Decimal Bits.

## § ui16Natural

uint16_t IQ16_t::ui16Natural

Upper 16; Integer Bits.

## § @10

struct { ... }

## § ui32Full

uint32_t IQ16_t::ui32Full

Full 32 bits.

The documentation for this union was generated from the following file:

- CAPT_Type.h

© Copyright 1995-2018, Texas Instruments Incorporated. All rights reserved.
Trademarks | Privacy policy | Terms of use | Terms of sale