MSP430™CapTIvateSoftwareLibraryAPIGuide 1_70_00_03

Functions | Variables
I2CSlave.c File Reference
`#include "I2CSlave.h"`
`#include "FunctionTimer.h"`
Include dependency graph for I2CSlave.c:

## Functions
void | I2CSlave_openPort (const tI2CSlavePort *pPort)
void | I2CSlave_closePort (void)
uint8_t | I2CSlave_getPortStatus (void)
void | I2CSlave_setTransmitBuffer (uint8_t *pBuffer, uint16_t ui16Length)
void | I2CSlave_setRequestFlag (void)
__interrupt void | I2CSlave_ISR (void)

## Variables
const tI2CSlavePort * | g_pI2CSlavePort
const EUSCI_B_I2C_initSlaveParam | g_I2CSlaveConfiguration
const uint8_t * | g_pI2CTransmitBuffer
| var g_pI2CTransmitBuffer stores a pointer to the current transmit buffer. More...
uint16_t | g_ui16I2CLength
volatile uint16_t | g_ui16I2CIndex
| var g_ui16I2CIndex stores the current transmit or receive buffer index. More...
volatile uint8_t | g_I2CSlaveStatus = eI2CSlaveIsClosed
volatile bool | g_bI2CSlaveRequestPending
const tFunctionTimer | g_I2CSlaveFunctionTimer

© Copyright 1995-2018, Texas Instruments Incorporated. All rights reserved.
Trademarks | Privacy policy | Terms of use | Terms of sale