MSP430™CapTIvateSoftwareLibraryAPIGuide 1_70_00_03

Data Fields
tCaptivateElementTuning Struct Reference
CAPT_TYPE

typedef tCaptivateElementTuning More...

`#include <CAPT_Type.h>`

## Data Fields
uint16_t | ui16OffsetTap
| Offset Correction Tap (16 Bit Selection) More...
uint8_t | ui8CoarseGainRatio
| Coarse Gain Ratio (3 Bit Selection) More...
uint8_t | ui8FineGainRatio
| Fine Gain Ratio (5 Bit Selection) More...

## Detailed Description

typedef tCaptivateElementTuning

Every element in the system has at a corresponding element tuning structure associated with it for each frequency it is measured at. This structure holds the CapTIvate™ block tuning configuration for the specific element at a specific conversion frequency.

## Field Documentation

## § ui16OffsetTap

uint16_t tCaptivateElementTuning::ui16OffsetTap

Offset Correction Tap (16 Bit Selection)

## § ui8CoarseGainRatio

uint8_t tCaptivateElementTuning::ui8CoarseGainRatio

Coarse Gain Ratio (3 Bit Selection)

## § ui8FineGainRatio

uint8_t tCaptivateElementTuning::ui8FineGainRatio

Fine Gain Ratio (5 Bit Selection)

The documentation for this struct was generated from the following file:

- CAPT_Type.h

© Copyright 1995-2018, Texas Instruments Incorporated. All rights reserved.
Trademarks | Privacy policy | Terms of use | Terms of sale