lwIP 2.1.2 Lightweight IP stack

Functions
api_lib.c File Reference
`#include "lwip/opt.h"`
`#include "lwip/api.h"`
`#include "lwip/memp.h"`
`#include "lwip/ip.h"`
`#include "lwip/raw.h"`
`#include "lwip/udp.h"`
`#include "lwip/priv/api_msg.h"`
`#include "lwip/priv/tcp_priv.h"`
`#include "lwip/priv/tcpip_priv.h"`
`#include "path/to/my/lwip_hooks.h"`
`#include <string.h>`

## Functions
struct netconn * | netconn_new_with_proto_and_callback (enum netconn_type t, u8_t proto, netconn_callback callback)
err_t | netconn_prepare_delete (struct netconn *conn)
err_t | netconn_delete (struct netconn *conn)
err_t | netconn_getaddr (struct netconn *conn, ip_addr_t *addr, u16_t *port, u8_t local)
err_t | netconn_bind (struct netconn *conn, const ip_addr_t *addr, u16_t port)
err_t | netconn_bind_if (struct netconn *conn, u8_t if_idx)
err_t | netconn_connect (struct netconn *conn, const ip_addr_t *addr, u16_t port)
err_t | netconn_disconnect (struct netconn *conn)
err_t | netconn_listen_with_backlog (struct netconn *conn, u8_t backlog)
err_t | netconn_accept (struct netconn *conn, struct netconn **new_conn)
err_t | netconn_recv_tcp_pbuf (struct netconn *conn, struct pbuf **new_buf)
err_t | netconn_recv_tcp_pbuf_flags (struct netconn *conn, struct pbuf **new_buf, u8_t apiflags)
err_t | netconn_recv_udp_raw_netbuf (struct netconn *conn, struct netbuf **new_buf)
err_t | netconn_recv_udp_raw_netbuf_flags (struct netconn *conn, struct netbuf **new_buf, u8_t apiflags)
err_t | netconn_recv (struct netconn *conn, struct netbuf **new_buf)
err_t | netconn_sendto (struct netconn *conn, struct netbuf *buf, const ip_addr_t *addr, u16_t port)
err_t | netconn_send (struct netconn *conn, struct netbuf *buf)
err_t | netconn_write_partly (struct netconn *conn, const void *dataptr, size_t size, u8_t apiflags, size_t *bytes_written)
err_t | netconn_write_vectors_partly (struct netconn *conn, struct netvector *vectors, u16_t vectorcnt, u8_t apiflags, size_t *bytes_written)
err_t | netconn_close (struct netconn *conn)
err_t | netconn_err (struct netconn *conn)
err_t | netconn_shutdown (struct netconn *conn, u8_t shut_rx, u8_t shut_tx)
err_t | netconn_join_leave_group (struct netconn *conn, const ip_addr_t *multiaddr, const ip_addr_t *netif_addr, enum netconn_igmp join_or_leave)
err_t | netconn_join_leave_group_netif (struct netconn *conn, const ip_addr_t *multiaddr, u8_t if_idx, enum netconn_igmp join_or_leave)
err_t | netconn_gethostbyname_addrtype (const char *name, ip_addr_t *addr, u8_t dns_addrtype)

## Detailed Description

Sequential API External module

## Function Documentation

## ◆ netconn_getaddr()

err_t netconn_getaddr | ( | struct netconn * | conn,
|  | ip_addr_t * | addr,
|  | u16_t * | port,
|  | u8_t | local
| ) |  |

Get the local or remote IP address and port of a netconn. For RAW netconns, this returns the protocol instead of a port!

Parameters

  conn | the netconn to query
  addr | a pointer to which to save the IP address
  port | a pointer to which to save the port (or protocol for RAW)
  local | 1 to get the local IP address, 0 to get the remote one

Returns
  ERR_CONN for invalid connections ERR_OK if the information was retrieved

## ◆ netconn_new_with_proto_and_callback()

struct netconn* netconn_new_with_proto_and_callback | ( | enum netconn_type | t,
|  | u8_t | proto,
|  | netconn_callback | callback
| ) |  |

Create a new netconn (of a specific type) that has a callback function. The corresponding pcb is also created.

Parameters

  t | the type of 'connection' to create (

See also
  enum netconn_type)

Parameters

  proto | the IP protocol for RAW IP pcbs
  callback | a function to call on status changes (RX available, TX'ed)

Returns
  a newly allocated struct netconn or NULL on memory error

## ◆ netconn_recv_udp_raw_netbuf()

err_t netconn_recv_udp_raw_netbuf | ( | struct netconn * | conn,
|  | struct netbuf ** | new_buf
| ) |  |

Receive data (in form of a netbuf) from a UDP or RAW netconn

Parameters

  conn | the netconn from which to receive data
  new_buf | pointer where a new netbuf is stored when received data

Returns
  ERR_OK if data has been received, an error code otherwise (timeout, memory error or another error) ERR_ARG if conn is not a UDP/RAW netconn

## ◆ netconn_recv_udp_raw_netbuf_flags()

err_t netconn_recv_udp_raw_netbuf_flags | ( | struct netconn * | conn,
|  | struct netbuf ** | new_buf,
|  | u8_t | apiflags
| ) |  |

Receive data (in form of a netbuf) from a UDP or RAW netconn

Parameters

  conn | the netconn from which to receive data
  new_buf | pointer where a new netbuf is stored when received data
  apiflags | flags that control function behaviour. For now only: NETCONN_DONTBLOCK: only read data that is available now, don't wait for more data

Returns
  ERR_OK if data has been received, an error code otherwise (timeout, memory error or another error) ERR_ARG if conn is not a UDP/RAW netconn

## ◆ netconn_write_vectors_partly()

err_t netconn_write_vectors_partly | ( | struct netconn * | conn,
|  | struct netvector * | vectors,
|  | u16_t | vectorcnt,
|  | u8_t | apiflags,
|  | size_t * | bytes_written
| ) |  |

Send vectorized data atomically over a TCP netconn.

Parameters

  conn | the TCP netconn over which to send data
  vectors | array of vectors containing data to send
  vectorcnt | number of vectors in the array
  apiflags | combination of following flags : NETCONN_COPY: data will be copied into memory belonging to the stack NETCONN_MORE: for TCP connection, PSH flag will be set on last segment sent NETCONN_DONTBLOCK: only write the data if all data can be written at once
  bytes_written | pointer to a location that receives the number of written bytes

Returns
  ERR_OK if data was sent, any other err_t on error