MotorWare f2806x Driver API Documentation

- Main Page
- Modules
- Data Structures
- Files

- File List
- Globals

adc_obj.h
Go to the documentation of this file.
1 /* --COPYRIGHT--,BSD
2 * Copyright (c) 2012, Texas Instruments Incorporated
3 * All rights reserved.
4 *
5 * Redistribution and use in source and binary forms, with or without
6 * modification, are permitted provided that the following conditions
7 * are met:
8 *
9 * * Redistributions of source code must retain the above copyright
10 * notice, this list of conditions and the following disclaimer.
11 *
12 * * Redistributions in binary form must reproduce the above copyright
13 * notice, this list of conditions and the following disclaimer in the
14 * documentation and/or other materials provided with the distribution.
15 *
16 * * Neither the name of Texas Instruments Incorporated nor the names of
17 * its contributors may be used to endorse or promote products derived
18 * from this software without specific prior written permission.
19 *
20 * THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS"
21 * AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO,
22 * THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR
23 * PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT OWNER OR
24 * CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL,
25 * EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO,
26 * PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS;
27 * OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY,
28 * WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR
29 * OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE,
30 * EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
31 * --/COPYRIGHT--*/
32 #ifndef _ADC_OBJ_H_
33 #define _ADC_OBJ_H_
34
40
41
42 // modules
43 #include "sw/modules/math/src/32b/math.h"
44 #include "sw/modules/types/src/types.h"
45
46
47
50 typedef struct _ADC_Obj_
51 {
52 volatile uint16_t ADCRESULT[16];
53 volatile uint16_t resvd_1[26096];
54 volatile uint16_t ADCCTL1;
55 volatile uint16_t rsvd_2[3];
56 volatile uint16_t ADCINTFLG;
57 volatile uint16_t ADCINTFLGCLR;
58 volatile uint16_t ADCINTOVF;
59 volatile uint16_t ADCINTOVFCLR;
60 volatile uint16_t INTSELxNy[5];
61 volatile uint16_t rsvd_3[3];
62 volatile uint16_t SOCPRICTRL;
63 volatile uint16_t rsvd_4;
64 volatile uint16_t ADCSAMPLEMODE;
65 volatile uint16_t rsvd_5;
66 volatile uint16_t ADCINTSOCSEL1;
67 volatile uint16_t ADCINTSOCSEL2;
68 volatile uint16_t rsvd_6[2];
69 volatile uint16_t ADCSOCFLG1;
70 volatile uint16_t rsvd_7;
71 volatile uint16_t ADCSOCFRC1;
72 volatile uint16_t rsvd_8;
73 volatile uint16_t ADCSOCOVF1;
74 volatile uint16_t rsvd_9;
75 volatile uint16_t ADCSOCOVFCLR1;
76 volatile uint16_t rsvd_10;
77 volatile uint16_t ADCSOCxCTL[16];
78 volatile uint16_t rsvd_11[16];
79 volatile uint16_t ADCREFTRIM;
80 volatile uint16_t ADCOFFTRIM;
81 volatile uint16_t resvd_12[13];
82 volatile uint16_t ADCREV;
83 } ADC_Obj;
84
85
88 typedef struct _ADC_Obj_ *ADC_Handle;
89
90
91
92 #ifdef __cplusplus
93 }
94 #endif // extern "C"
95
97 #endif // end of _ADC_OBJ_H_ definition
_ADC_Obj_::ADCSOCOVFCLR1
volatile uint16_t ADCSOCOVFCLR1
ADC SOC Overflow Clear 1 Register.
Definition: adc_obj.h:75
_ADC_Obj_::ADCINTSOCSEL2
volatile uint16_t ADCINTSOCSEL2
ADC Interrupt Trigger SOC Select 2 Register.
Definition: adc_obj.h:67
_ADC_Obj_::rsvd_8
volatile uint16_t rsvd_8
Reserved.
Definition: adc_obj.h:72
_ADC_Obj_::ADCINTFLGCLR
volatile uint16_t ADCINTFLGCLR
ADC Interrupt Flag Clear Register.
Definition: adc_obj.h:57
_ADC_Obj_::ADCINTFLG
volatile uint16_t ADCINTFLG
ADC Interrupt Flag Register.
Definition: adc_obj.h:56
_ADC_Obj_::ADCINTOVF
volatile uint16_t ADCINTOVF
ADC Interrupt Overflow Register.
Definition: adc_obj.h:58
_ADC_Obj_::ADCSOCFRC1
volatile uint16_t ADCSOCFRC1
ADC SOC Force 1 Register.
Definition: adc_obj.h:71
_ADC_Obj_::ADCSAMPLEMODE
volatile uint16_t ADCSAMPLEMODE
ADC Sample Mode Register.
Definition: adc_obj.h:64
_ADC_Obj_::rsvd_10
volatile uint16_t rsvd_10
Reserved.
Definition: adc_obj.h:76
_ADC_Obj_::rsvd_2
volatile uint16_t rsvd_2[3]
Reserved.
Definition: adc_obj.h:55
_ADC_Obj_::resvd_1
volatile uint16_t resvd_1[26096]
Reserved.
Definition: adc_obj.h:53
_ADC_Obj_::rsvd_6
volatile uint16_t rsvd_6[2]
Reserved.
Definition: adc_obj.h:68
_ADC_Obj_::rsvd_3
volatile uint16_t rsvd_3[3]
Reserved.
Definition: adc_obj.h:61
_ADC_Obj_::ADCSOCxCTL
volatile uint16_t ADCSOCxCTL[16]
ADC SOCx Control Registers.
Definition: adc_obj.h:77
_ADC_Obj_::ADCCTL1
volatile uint16_t ADCCTL1
ADC Control Register 1.
Definition: adc_obj.h:54
_ADC_Obj_::ADCINTOVFCLR
volatile uint16_t ADCINTOVFCLR
ADC Interrupt Overflow Clear Register.
Definition: adc_obj.h:59
_ADC_Obj_::resvd_12
volatile uint16_t resvd_12[13]
Reserved.
Definition: adc_obj.h:81
_ADC_Obj_::ADCINTSOCSEL1
volatile uint16_t ADCINTSOCSEL1
ADC Interrupt Trigger SOC Select 1 Register.
Definition: adc_obj.h:66
_ADC_Obj_
Defines the analog-to-digital converter (ADC) object.
Definition: adc_obj.h:50
ADC_Handle
struct _ADC_Obj_ * ADC_Handle
Defines the analog-to-digital converter (ADC) handle.
Definition: adc_obj.h:88
ADC_Obj
struct _ADC_Obj_ ADC_Obj
Defines the analog-to-digital converter (ADC) object.
_ADC_Obj_::SOCPRICTRL
volatile uint16_t SOCPRICTRL
ADC Start Of Conversion Priority Control Register.
Definition: adc_obj.h:62
_ADC_Obj_::ADCREFTRIM
volatile uint16_t ADCREFTRIM
ADC Reference/Gain Trim Register.
Definition: adc_obj.h:79
_ADC_Obj_::INTSELxNy
volatile uint16_t INTSELxNy[5]
ADC Interrupt Select x and y Register.
Definition: adc_obj.h:60
_ADC_Obj_::ADCREV
volatile uint16_t ADCREV
ADC Revision Register.
Definition: adc_obj.h:82
_ADC_Obj_::rsvd_11
volatile uint16_t rsvd_11[16]
Reserved.
Definition: adc_obj.h:78
_ADC_Obj_::rsvd_9
volatile uint16_t rsvd_9
Reserved.
Definition: adc_obj.h:74
_ADC_Obj_::ADCSOCFLG1
volatile uint16_t ADCSOCFLG1
ADC SOC Flag 1 Register.
Definition: adc_obj.h:69
_ADC_Obj_::rsvd_5
volatile uint16_t rsvd_5
Reserved.
Definition: adc_obj.h:65
_ADC_Obj_::rsvd_4
volatile uint16_t rsvd_4
Reserved.
Definition: adc_obj.h:63
_ADC_Obj_::ADCOFFTRIM
volatile uint16_t ADCOFFTRIM
ADC Offset Trim Register.
Definition: adc_obj.h:80
_ADC_Obj_::ADCSOCOVF1
volatile uint16_t ADCSOCOVF1
ADC SOC Overflow 1 Register.
Definition: adc_obj.h:73
_ADC_Obj_::rsvd_7
volatile uint16_t rsvd_7
Reserved.
Definition: adc_obj.h:70
_ADC_Obj_::ADCRESULT
volatile uint16_t ADCRESULT[16]
ADC result registers.
Definition: adc_obj.h:52