{"text_format":"1","workbook":"xlsx","n_sheets":12,"sheets":["Instructions","Design Converter","BOM & Schematic","Fsw & Ripple","Losses","EVM","Design EMI Filter","Variable Mgmt","Standard Value Calculator","Efficiency","Schematic Mgmt","Efficiency Plots"],"not_rendered":{"charts":6,"images":26,"macros":1,"external_links":0,"defined_names":205,"comments":4,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Instructions","index":0,"n_rows":74,"n_cols":3,"rows_kept":74,"cut":false,"hidden":true,"merged":[[0,0,0,16],[7,1,9,15],[16,2,17,15],[11,1,14,15],[18,2,19,15],[65,1,66,15],[69,1,70,15],[73,1,74,15],[77,1,78,15],[20,2,21,15],[50,1,52,15],[54,1,55,15],[56,1,57,15],[60,1,62,15],[24,1,26,15],[38,1,39,15],[41,1,43,15],[46,1,47,15],[28,1,28,15],[29,1,31,15],[33,1,35,15]]}
["                         LM5164 Low IQ DC/DC Converter Design Tool  "]
[]
[]
[null,"Design Regulator tab"]
[null,"Start with Step 1, and then work down towards the bottom of the worksheet."]
[]
[null,"Step 1. Operating Specifications"]
[null,"First, enter the values in the yellow shaded cells to define the power supply parameters.  If a particular specification is not known, enter an estimate. It can be changed later, if necessary, to optimize component values.  Cells  with a red mark in the upper right corner have a comment to provide additional information.  Hold the cursor over the cell to read the comment.  A red font indicates an erroneous entry and requires an adjustment to the entry.  Consult the entry's comments for the entry specific requirements."]
[]
[]
[]
[null,"Second, select a desired mode of operation. PFM mode requires the fewest external components and the lowest inductance.  As a result, it can provide the smallest solution size. At light loads, a PFM converter has a relatively longer sleep time interval and thus operates at lower input quiescent current levels.  COT mode offers nearly constant switching frequency, relatively higher conversion efficiencies at medium to heavy loads, and enables the lowest output voltage ripple.  Options COT1, COT2, and COT3 enable you to select a ripple generation method (a requirement for the stable operation in COT mode):"]
[]
[]
[]
[]
[null,"-COT1: ","Type 1 ripple generation method requires a single resistor in series with the output capacitor.  It is the simplest, the most compact, and the most economical method that works with fixed and adjustable device options, however, the output voltage ripple is the highest."]
[]
[null,"-COT2: ","Type 2 ripple generation method requires a feedforward capacitor in addition to the series resistor.  The feedforward capacitor reduces the required minimum value of the series resistor and ultimately the output voltage ripple by the VOUT / 1.223V factor.  It only works with an adjustable device option (i.e. external feedback resistor network)."]
[]
[null,"-COT3:","Type 3 ripple generation method three external components to generate and inject required voltage ripple into the FB node.  In return, it provides the lowest output voltage ripple. It also only works with an adjustable device option (i.e. external feedback resistor network)."]
[]
[]
[null,"Step 2. Filter Inductor"]
[null,"First, select an inductor current limit level.  In PFM Mode, 1.25A, 0.75A, 0.5A, and 1.25A - MOD options are available.  For the 500mA max load, select either 1.25A or 1.25A - MOD option.  The 1.25A - MOD option enables higher efficiency at the expense of slightly worse transient operation.  For the 300mA and 200mA max loads, select 0.75A and 0.5A options respectively. In COT Mode, 0.75A and 0.5A options are available.   For the 500mA and 300mA max loads, select 0.75A and 0.5A options respectively."]
[]
[]
[]
[null,"Second, select the filter inductance value based on the suggested value. Enter the inductor RDC for accurate efficiency estimates."]
[null,"In PFM mode, selected inductance defines the switching frequency.  You may select lower or higher inductance to increase or decrease the switching frequency.  Watch the minimum output capacitance.  At very low switching frequencies, the required minimum capacitance may become excessive."]
[]
[]
[]
[null,"In COT mode, the suggested inductance is  derived based on the target inductor (peak-to-peak) ripple current of 40% of the DC full load output current at nominal input voltage. It may be acceptable to use higher ripple current with the proviso that peak inductor current remains below the ILIM setting.  Pk-to-Pk Ripple Current value will turn red if this is violated.  If this happens, increase the selected inductance or decrease the Input Voltage (max) or both."]
[]
[]
[]
[null,"Step 3. Output Capacitors and Ripple Generation"]
[null,"First, select the output capacitance based on the minimum recommended value.  Make sure that the nominal capacitance is appropriately derated for applied voltage, especially with ceramics.  For PFM and COT3 modes, ensure that the capacitor ESR does not exceed the maximum allowable value.  "]
[]
[]
[null,"Second, for COT modes, select the values for the ripple generation components based on the minimum recommended values.  Ensure that the output voltage ripple meets any of your minimum ripple requirements by reviewing the VOUT Ripple vs. IOUT plot in the fSW&Ripple tab.  For accurate output voltage ripple estimates in COT3 mode, ensure that the Output Capacitor ESR is set to the levels of a typical ceramic capacitor ESR (e.g. 10 mW)."]
[]
[]
[]
[null,"Step 4. Input Capacitors"]
[null,"Select the input capacitance based on the minimum recommended value.  Make sure that the nominal capacitance is appropriately derated for applied voltage, especially with ceramics.  "]
[]
[]
[null,"Step 5. Feedback, Soft-Start, UVLO"]
[null,"First, review the feedback resistor network. With an adjustable device option, an external feedback resistor network is required. The resistor values are automatically calculated based on the selected VOUT in Step 1.  For lowering the leakage current through the resistors, adjust the upper FB resistor (R1) until the lower FB resistor (R2) reaches its upper end of the range (100kW).  Keeping the upper FB resistor below 1MW is recommended."]
[]
[]
[]
[null,"Second, select one out of three soft-start configurations.  If the external soft-start option is selected, enter a desired soft start time.  "]
[]
[null,"Third, select one out of the two UVLO options.  If the external UVLO option is selected, define desired UVLO thresholds and hysteresis.  Keeping the upper UVLO resistor at 1MW or higher is recommended for the minimum leakage current."]
[]
[]
[null,"Step 6. Efficiency and Thermals"]
[null,"Enter the LM5166's junction-to-ambient thermal impedance (dependent on your PCB design, air flow, etc.) and ambient temperature. Device power dissipation and junction temperature are derived at the maximum load.  Ensure that the junction temperature is within the recommended range."]
[]
[]
[]
[null,"BOM & Schematic tab"]
[null,"This tab summarizes the converter schematic and BOM.  It also helps you estimate the total solution size. Select a package size for each external component (i.e. inductor, capacitors, and resistors) for accurate solution size estimates."]
[]
[]
[null,"Design EMI Filter tab"]
[null,"In case an EMI filter is needed, a simple EMI filter design aid is given in this tab.  It is based on the guidelines documented in TI's literature number SNVA489C (aka AN-2162).  Suggest reviewing the note before using the design aid."]
[]
[]
[null,"fSW & Ripple tab"]
[null,"In this tab, the switching/burst frequency (COT/PFM mode) and the output voltage ripple as a function of the load current are plotted."]

{"sheet":"Design Converter","index":1,"n_rows":58,"n_cols":17,"rows_kept":58,"cut":false,"hidden":false,"merged":[[2,14,2,15],[0,0,0,16]]}
["                          LM5163/4 Low IQ DC/DC Converter Design Tool  "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"http://www.ti.com/ww/en/analog/power_management/widevin"]
["About",null,"xx",null,null,"= Input Box",null,null,null,null,null,null,null,null,"Terms Of Use",null,"                "]
[]
["Step 1: Operating Specifications"]
[null,null,null,"Input Voltage - Min, VIN(min) ",18,"V"]
[null,null,null,"Input Voltage - Nom, VIN(nom)",48,"V"]
[null,null,null,"Input Voltage - Max, VIN(max)",60,"V"]
[null,null,null,"Output Voltage, VOUT ",5,"V"]
[null,null,null,"Full Load Current, IOUT",0.1,"A"]
[null,null,null,"Mode of Operation",null,null,{"$f":"MODE","v":3}]
[null,null,null,"Switching Frequency at VIN(nom)",300,"kHz"]
[null,null,null,"Timing Resistance, RT",{"$f":"'Standard Value Calculator'!J4/1000","v":41.2},"kΩ"]
[]
["Step 2: Buck Inductor"]
[null,null,null,"Recommended Buck Inductance ",{"$f":"Lopt*1000000","v":373.26388888888891},"µH"]
[null,null,null,"Inductance, LF ",370,"µH"]
[null,null,null,"Inductor DCR ",120,"mΩ"]
[null,null,null,{"$f":"CHOOSE(MODE, \"Pk-to-Pk Ripple Current\",\"Pk-to-Pk Ripple Current\",\"Pk-to-Pk Ripple Current\", \"Resulting PFM Switching Frequency\")","v":"Pk-to-Pk Ripple Current"},{"$f":"Iripple_Vinnom*1000","v":40.617087951732877},"mApk-pk"]
[null,null,null,{"$f":"CHOOSE(MODE, 'Variable Mgmt'!H88,'Variable Mgmt'!H88,'Variable Mgmt'!H88, 'Variable Mgmt'!H89)","v":"% Ripple Current at Nom VIN"},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), 'Variable Mgmt'!B96*100, Ilim/2*1000)","v":40.61708795173287},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), \"%\", \"mA\")","v":"%"}]
[]
[{"$f":"IF(MODE=4, \"Step 3: Output Capacitors\", \"Step 3: Output Capacitors, Ripple Generation\")","v":"Step 3: Output Capacitors, Ripple Generation"}]
[null,null,null,"Minimum Output Capacitance ",{"$f":"'Variable Mgmt'!B116","v":2.2000000000000002},"µF"]
[null,null,null,"Output Capacitance, COUT ",33,"µF"]
[null,null,null,{"$f":"IF(OR(MODE=1,MODE=2),\"Recommended Series Resistance\",IF(MODE=3,\"Maximum Allowable ESR\",\"*Higher Cout Improves Light-Load Eff\"))","v":"Maximum Allowable ESR"},{"$f":"'Variable Mgmt'!B272","v":0.61499999999999999},"Ω"]
[null,null,null,{"$f":"IF(OR(MODE=1,MODE=2),\"Total ESR & Series Resistance, Rser\",IF(MODE=3,\"Output Capacitor ESR\",\"*PFM Hysteresis Sets Output Ripple\"))","v":"Output Capacitor ESR"},5.0000000000000001E-3,"Ω"]
[null,null,null,{"$f":"CHOOSE(MODE, \"Resulting Output Voltage Ripple\",\"Resulting Output Voltage Ripple\", \"Output Voltage Ripple\",\"Output Voltage Ripple\")","v":"Output Voltage Ripple"},{"$f":"CHOOSE(MODE, Vripple2*1000,Vripple2*1000,Vripple2*1000, PFM_Ripple)","v":0.55158918852872141},"mVpk-pk"]
[null,null,null,{"$f":"IF(MODE=1,\"\",IF(MODE=2,\"Minimum Feedforward Capacitance\", IF(MODE=3,\"Minimum Coupling Capacitance\",\"\")))","v":"Minimum Coupling Capacitance"},{"$f":"'Variable Mgmt'!B140","v":">47"},"pF"]
[null,null,null,{"$f":"IF(MODE=1,\"\",IF(MODE=2,\"Feedforward Capacitance, Cff\", IF(MODE=3,\"Coupling Capacitance, Cb\",\"\")))","v":"Coupling Capacitance, Cb"},56,"pF",null,null,null,null,null,"** Specify Inductor Core Loss **",100,"mW"]
[null,null,null,{"$f":"IF(MODE=3,\"Minimum Ripple Generation Capacitance\",\"\")","v":"Minimum Ripple Generation Capacitance"},{"$f":"'Variable Mgmt'!B144","v":">307"},"pF"]
[null,null,null,{"$f":"IF(MODE=3,\"Ripple Generation Capacitance, Ca\",\"\")","v":"Ripple Generation Capacitance, Ca"},2200,"pF"]
[null,null,null,{"$f":"IF(MODE=3,\"Ripple Generation Resistance, Ra\",\"\")","v":"Ripple Generation Resistance, Ra"},{"$f":"Ra","v":340},"kΩ"]
[null,null,null,{"$f":"IF(MODE=3,\"Amplitude of Injected Ripple\",\"\")","v":"Amplitude of Injected Ripple"},20,"mVpk-pk"]
[]
["Step 4: Input Capacitors"]
[null,null,null,"Minimum Input Capacitance ",{"$f":"'Variable Mgmt'!B157","v":2.2000000000000002},"µF"]
[null,null,null,"Input Capacitance, CIN ",2.2000000000000002,"µF"]
[null,null,null,"Maximum Allowable ESR",{"$f":"'Variable Mgmt'!B159","v":19.830325093869845},"Ω"]
[null,null,null,"Input Capacitor ESR ",3,"mΩ"]
[null,null,null,"Resulting Input Voltage Ripple ",{"$f":"CHOOSE(MODE, Vinripple2*1000,Vinripple2*1000,Vinripple2*1000, 'Variable Mgmt'!B165*1000)","v":14.60338702035974},"mVpk-pk"]
[]
["Step 5: Feedback, PGOOD, UVLO"]
[null,null,null,"Upper Feedback Resistor, RFB1 ",453,"kΩ"]
[null,null,null,"Lower Feedback Resistor, RFB2",{"$f":"IF(Vout=Vref,\"OPEN\",Rfb2_u/1000)","v":143},{"$f":"IF(Vout=Vref,\"\",\"kΩ\")","v":"kΩ"}]
[null,null,null,"Acutal Output Voltage Setpoint",{"$f":"'Variable Mgmt'!B201","v":5.0013986013986012},"V"]
[null,null,null,"PGOOD Pull-up Resistance",20,{"$f":"\"kΩ\"","v":"kΩ"},null,null,null,null,null,null,null,null,null,null," "]
[null,null,null,"BST Capacitance, CBST ",2.2000000000000002,"nF"]
[null,null,null,{"$f":"\"Required Input Voltage UVLO Turn-on\"","v":"Required Input Voltage UVLO Turn-on"},6,"V"]
[null,null,null,"Upper UVLO Resistor, RUV1",1,"MΩ"]
[null,null,null,"Lower UVLO Resistor, RUV2",{"$f":"'Variable Mgmt'!F276","v":332},{"$f":"'Variable Mgmt'!G276","v":"kΩ"}]
[null,null,null,"Actual UVLO Turn-on Threshold",{"$f":"'Variable Mgmt'!B186","v":6.0180722891566267},"V"]
[null,null,null,"Actual UVLO Turn-off Threshold",{"$f":"'Variable Mgmt'!B187","v":5.6168674698795176},"V"]
[]
["Step 6: Efficiency & Thermals"]
[null,null,null,"Estimated Thermal Impedance, JJA",41,"°C/W"]
[null,null,null,"Ambient Temp, TA",25,"°C"]
[null,null,null,"IC Power Dissipation at Full Load, PD",{"$f":"'Variable Mgmt'!B26","v":0.22273269936649198},"W"]
[null,null,null,"IC Junction Temp at Full Load, TJ",{"$f":"E56+E55*'Variable Mgmt'!B26","v":34.132040674026172},"°C"]

{"sheet":"BOM & Schematic","index":2,"n_rows":53,"n_cols":13,"rows_kept":53,"cut":false,"hidden":false,"merged":[[33,3,33,5],[0,0,0,16],[29,3,29,5],[41,3,41,5],[47,7,47,9],[30,3,30,5],[43,3,43,5],[44,3,44,5],[42,3,42,5],[39,3,39,5],[40,3,40,5],[38,3,38,5],[37,3,37,5],[36,3,36,5],[31,3,31,5],[34,3,34,5],[32,3,32,5]]}
["                         LM5163/4 100V Low IQ DC/DC Converter Design Tool  "]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[{"$f":"\"VIN = \"&Vin&\" V, VOUT = \"&Vout&\" V, IOUT = \"&Iout&\" A \"&'Variable Mgmt'!B35&\" Converter\"","v":"VIN = 48 V, VOUT = 5 V, IOUT = 0.1 A COT Converter"}]
["Low IQ, High Efficiency, Synchronous Buck Converter BOM"]
["Count","Ref Des","Value","Description",null,null,"Size","Part Number","MFR","Footprint (mm)","Area (mm2)"]
[{"$f":"ROUNDUP('Design Converter'!E37/10,0)","v":1},"CIN",{"$f":"Cin*1000000","v":2.2000000000000002},{"$f":"IF(VIN_max>35, \"Capacitor, Ceramic, \"&'Variable Mgmt'!B257&\", 100V, X7R, 10%\", \"Capacitor, Ceramic, \"&'Variable Mgmt'!B257&\", 50V, X7R, 10%\")","v":"Capacitor, Ceramic, 2.2µF, 100V, X7R, 10%"},null,null,5,"Std","Std",{"$f":"CHOOSE(G31,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45)","v":"3.2 x 2.5"},{"$f":"CHOOSE(G31,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45)","v":8}]
[{"$f":"'Variable Mgmt'!D252","v":1},"COUT",{"$f":"'Variable Mgmt'!F253","v":"47µF"},{"$f":"CHOOSE(Cout_Voltage_Rating, \"Capacitor, Ceramic, \"&'Variable Mgmt'!F253&\", 6.3V, X7R, 10%\", \"Capacitor, Ceramic, \"&'Variable Mgmt'!F253&\", 10V, X7R, 10%\", \"Capacitor, Ceramic, \"&'Variable Mgmt'!F253&\", 16V, X7R, 10%\", \"Capacitor, Ceramic, \"&'Variable Mgmt'!F253&\", 25V, X7R, 10%\",  \"Capacitor, Ceramic, \"&'Variable Mgmt'!F253&\", 50V, X7R, 10%\")","v":"Capacitor, Ceramic, 47µF, 6.3V, X7R, 10%"},null,null,5,"Std","Std",{"$f":"CHOOSE(G32,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45)","v":"3.2 x 2.5"},{"$f":"(CHOOSE(G32,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45))*A32","v":8}]
[{"$f":"CHOOSE(MODE, \"-\", \"-\", \"1\",\"-\")","v":"1"},{"$f":"CHOOSE(MODE,\"-\",\"-\",\"Ca\",\"-\")","v":"Ca"},{"$f":"CHOOSE(MODE, \"-\",\"-\",'Variable Mgmt'!B293, \"-\")","v":"2200pF"},{"$f":"CHOOSE(MODE,\"-\",\"-\", \"Capacitor, Ceramic, \"&'Variable Mgmt'!B293&\", 16V, X7R, 10%\", \"-\")","v":"Capacitor, Ceramic, 2200pF, 16V, X7R, 10%"},null,null,1,{"$f":"CHOOSE(MODE, \"-\", \"-\", \"Std\", \"-\")","v":"Std"},{"$f":"H33","v":"Std"},{"$f":"CHOOSE(MODE,\"\",\"\",CHOOSE(G33,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),\"\")","v":"1.0 x 0.5"},{"$f":"CHOOSE(MODE,\"\",\"\",CHOOSE(G33,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),\"\")","v":0.5}]
[{"$f":"CHOOSE(MODE, \"-\", \"1\", \"1\",\"-\")","v":"1"},{"$f":"CHOOSE(MODE,\"-\",\"Cff\",\"Cb\",\"-\")","v":"Cb"},{"$f":"CHOOSE(MODE, \"-\",'Variable Mgmt'!B290,'Variable Mgmt'!B290, \"-\")","v":"56pF"},{"$f":"CHOOSE(MODE,\"-\",\"Capacitor, Ceramic, \"&'Variable Mgmt'!B290&\", 50V, X7R, 10%\", \"Capacitor, Ceramic, \"&'Variable Mgmt'!B290&\", 50V, X7R, 10%\", \"-\")","v":"Capacitor, Ceramic, 56pF, 50V, X7R, 10%"},null,null,1,{"$f":"CHOOSE(MODE, \"-\", \"Std\", \"Std\", \"-\")","v":"Std"},{"$f":"H34","v":"Std"},{"$f":"CHOOSE(MODE,\"\",CHOOSE(G34,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),CHOOSE(G34,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),\"\")","v":"1.0 x 0.5"},{"$f":"CHOOSE(MODE,\"\",CHOOSE(G34,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),CHOOSE(G34,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),\"\")","v":0.5}]
[1,"CBST","2.2nF","Capacitor, Ceramic, 2.2nF, 25V, X7R, 10%",null,null,1,{"$f":"CHOOSE(MODE, \"-\", \"Std\", \"Std\", \"-\")","v":"Std"},{"$f":"H35","v":"Std"},{"$f":"CHOOSE(MODE,\"\",CHOOSE(G35,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),CHOOSE(G35,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),\"\")","v":"1.0 x 0.5"},{"$f":"CHOOSE(MODE,\"\",CHOOSE(G35,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),CHOOSE(G35,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),\"\")","v":0.5}]
[]
[1,"LF",{"$f":"'Design Converter'!E17","v":370},{"$f":"\"Inductor, \"&Lf*1000000&\" µH, \"&Rdcr*1000&\" mΩ, >\"&ROUNDUP(Isat_min,2)&\"A\"","v":"Inductor, 370 µH, 120 mΩ, >1.8A"},null,null,4,"Various","Various",{"$f":"CHOOSE(G37,'Variable Mgmt'!T50,'Variable Mgmt'!T51,'Variable Mgmt'!T52,'Variable Mgmt'!T53,'Variable Mgmt'!T54,'Variable Mgmt'!T55,'Variable Mgmt'!T56)","v":"6.0 x 6.0"},{"$f":"CHOOSE(G37,'Variable Mgmt'!U50,'Variable Mgmt'!U51,'Variable Mgmt'!U52,'Variable Mgmt'!U53,'Variable Mgmt'!U54,'Variable Mgmt'!U55,'Variable Mgmt'!U56)","v":36}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(MODE_RSET=2,CHOOSE(G38,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),\"\")","v":""}]
[{"$f":"CHOOSE(MODE, \"1\",\"1\",\"1\", \"-\")","v":"1"},"RT",{"$f":"CHOOSE(MODE, 'Design Converter'!E13, 'Design Converter'!E13,'Design Converter'!E13,\"-\")","v":41.2},{"$f":"C39","v":41.2},null,null,1,{"$f":"CHOOSE(MODE, \"Std\",\"Std\",\"Std\",\"-\")","v":"Std"},{"$f":"H39","v":"Std"},{"$f":"CHOOSE(MODE,CHOOSE(G39,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),CHOOSE(G39,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),CHOOSE(G39,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),\"\")","v":"1.0 x 0.5"},{"$f":"CHOOSE(MODE,CHOOSE(G39,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),CHOOSE(G39,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),CHOOSE(G39,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),\"\")","v":0.5}]
[1,"RFB1",{"$f":"Rfb1_/1000","v":453},453,null,null,1,{"$f":"CHOOSE(MODE_VOUT,\"-\",\"Std\")","v":"Std"},{"$f":"H40","v":"Std"},{"$f":"(CHOOSE(MODE_VOUT,\"\",CHOOSE(G40,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45)))","v":"1.0 x 0.5"},{"$f":"CHOOSE(MODE_VOUT,\"\",CHOOSE(G40,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45))","v":0.5}]
[1,"RFB2",{"$f":"Rfb2_u/1000","v":143},143,null,null,1,{"$f":"CHOOSE(MODE_VOUT,\"-\",\"Std\")","v":"Std"},{"$f":"H41","v":"Std"},{"$f":"CHOOSE(MODE_VOUT,\"\",CHOOSE(G41,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45))","v":"1.0 x 0.5"},{"$f":"CHOOSE(MODE_VOUT,\"\",CHOOSE(G41,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45))","v":0.5}]
[{"$f":"IF(MODE=3,\"1\",\"-\")","v":"1"},{"$f":"CHOOSE(MODE,\"-\",\"-\",\"Ra\",\"-\")","v":"Ra"},{"$f":"'Variable Mgmt'!F296","v":"340k"},{"$f":"\"Resistor, Chip, \"&'Variable Mgmt'!B296&\", 1/16W, 1%\"","v":"Resistor, Chip, 340kΩ, 1/16W, 1%"},null,null,1,{"$f":"CHOOSE(MODE, \"-\", \"-\", \"Std\", \"-\")","v":"Std"},{"$f":"H42","v":"Std"},{"$f":"CHOOSE(MODE,\"\",\"\",CHOOSE(G42,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),\"\")","v":"1.0 x 0.5"},{"$f":"CHOOSE(MODE,\"\",\"\",CHOOSE(G42,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),\"\")","v":0.5}]
[1,"RPGOOD",100,100,null,null,1,"Std","Std",{"$f":"CHOOSE(G43,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45)","v":"1.0 x 0.5"},{"$f":"CHOOSE(G43,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45)","v":0.5}]
[{"$f":"CHOOSE(MODE_UVLO, \"1\", \"-\")","v":"1"},"RUV1",{"$f":"CHOOSE(MODE_UVLO, 'Variable Mgmt'!H275, \"-\")","v":"1M"},{"$f":"CHOOSE(MODE_UVLO, \"Resistor, Chip, \"&'Variable Mgmt'!C275&\", 1/16W, 1%\", \"-\")","v":"Resistor, Chip, 1MΩ, 1/16W, 1%"},null,null,2,{"$f":"CHOOSE(MODE_UVLO,\"Std\",\"-\")","v":"Std"},{"$f":"H44","v":"Std"},{"$f":"CHOOSE(MODE_UVLO,CHOOSE(G44,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),\"\")","v":"1.6 x 0.8"},{"$f":"CHOOSE(MODE_UVLO,CHOOSE(G44,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),\"\")","v":1.3}]
[{"$f":"CHOOSE(MODE_UVLO, \"1\", \"-\")","v":"1"},"RUV2",{"$f":"CHOOSE(MODE_UVLO, 'Variable Mgmt'!H276, \"-\")","v":"332k"},{"$f":"CHOOSE(MODE_UVLO, \"Resistor, Chip, \"&'Variable Mgmt'!C276&\", 1/16W, 1%\", \"-\")","v":"Resistor, Chip, 332kΩ, 1/16W, 1%"},null,null,1,{"$f":"CHOOSE(MODE_UVLO,\"Std\",\"-\")","v":"Std"},{"$f":"H45","v":"Std"},{"$f":"CHOOSE(MODE_UVLO,CHOOSE(G45,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),\"\")","v":"1.0 x 0.5"},{"$f":"CHOOSE(MODE_UVLO,CHOOSE(G45,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),\"\")","v":0.5}]
[1,"U1",{"$f":"CHOOSE(VARIANT, \"LM5163-Q1\", \"LM5164-Q1\")","v":"LM5164-Q1"},{"$f":"CHOOSE(VARIANT, \"IC, LM51643-Q1, Buck Converter, 6V–100V Input\", \"IC, LM5164-Q1, Buck Converter, 6V–100V Input\")","v":"IC, LM5164-Q1, Buck Converter, 6V–100V Input"},null,null,"SOIC-8",{"$f":"CHOOSE(VARIANT, \"LM5163QDDATQ1\", \"LM5164QDDATQ1\")","v":"LM5164QDDATQ1"},"TI","5.0 x 6.0",30]
[]
[null,{"$f":"\"Total Solution Size (padded by 15%) = \"&ROUND(K48,1)&\" mm^2 = \"&ROUND(M48,3)&\" in^2\"","v":"Total Solution Size (padded by 15%) = 101 mm^2 = 0.157 in^2"},null,null,null,null,null,null,null,null,{"$f":"SUM(K31:K46)*1.15","v":100.96999999999998},null,{"$f":"K48/25.4/25.4","v":0.156503813007626}]
[]
["NOTES:"]
["* Inductor saturation current should be higher than the peak inductor current setting for all operating temperatures *"]
["** Effective input and output capacitances should be appropriately derated for applied voltage and temperature, particularly with ceramics **"]
["***Estimated total solution size does not include EMI filter***"]

{"sheet":"Fsw & Ripple","index":3,"n_rows":1,"n_cols":1,"rows_kept":1,"cut":false,"hidden":true,"merged":[[0,0,0,16]]}
["                         LM5164 Low IQ DC/DC Converter Design Tool  "]

{"sheet":"Losses","index":4,"n_rows":42,"n_cols":6,"rows_kept":42,"cut":false,"hidden":true,"merged":[[0,0,0,16]]}
["                         LM5166 Low IQ DC/DC Converter Design Tool  "]
[]
[]
[]
[null,null,null,"Load Current",500,"mA"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,"Inductor Core Loss Constant",0]

{"sheet":"EVM","index":5,"n_rows":85,"n_cols":15,"rows_kept":85,"cut":false,"hidden":false,"merged":[[0,0,0,16]]}
["LM5163/4 100V, Low IQ DC/DC Converter Design Tool  "]
[]
[null,"LM5164-Q1EVM-041 PCB Layout"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Top"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Layer"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Layer 2"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Layer 3"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bottom"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Layer"]

{"sheet":"Design EMI Filter","index":6,"n_rows":33,"n_cols":15,"rows_kept":33,"cut":false,"hidden":false,"merged":[[0,0,0,22],[32,10,32,12],[29,10,29,12],[31,10,31,12]]}
["                         LM5163/4 100V, Low IQ DC/DC Converter Design Tool  "]
[]
[]
[]
[]
[]
["Step 7: EMI Filter (Optional)"]
[null,null,null,"Desired Maximum Noise Level, Vnoise(MAX)",50,"dBmV"]
[null,null,null,"EMI Filter Inductance, LF(EMI)",22,"mH"]
[null,null,null,"Minimum EMI Filter Capacitance",{"$f":"'Variable Mgmt'!M164","v":0.31884179934871787},"mF"]
[null,null,null,"EMI Filter Capacitance, CF(EMI)",4.7,"mF"]
[null,null,null,"Minimum EMI Filter Damping Capacitance",{"$f":"'Variable Mgmt'!M168","v":8.8000000000000007},"mF"]
[null,null,null,"EMI Filter Damping Capacitance, CD(EMI)",10,"mF"]
[null,null,null,"Minimum Damping Capacitor ESR",{"$f":"'Variable Mgmt'!M169","v":3.1622776601683795},"Ω"]
[null,null,null,"Damping Capacitor ESR, ESR CD(EMI)",3.3,"Ω"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,"EMI Filter BOM"]
[null,null,null,null,null,null,null,"Count","Ref Des","Value","Description",null,null,"Part Number","MFR"]
[null,null,null,null,null,null,null,1,"LF(EMI)",{"$f":"'Variable Mgmt'!B298","v":"22µH"},{"$f":"\"Inductor, \"&Lf_emi*1000000&\" µH, \"&ROUNDUP(Isat_min,2)&\"A\"","v":"Inductor, 22 µH, 1.8A"},null,null,"Std","Std"]
[null,null,null,null,null,null,null,1,"CF(EMI)",{"$f":"'Variable Mgmt'!B299","v":"4.7µF"},{"$f":"IF(VIN_max>35, \"Capacitor, Ceramic, \"&'Variable Mgmt'!B299&\", 100V, X7R, 10%\", \"Capacitor, Ceramic, \"&'Variable Mgmt'!B299&\", 50V, X7R, 10%\")","v":"Capacitor, Ceramic, 4.7µF, 100V, X7R, 10%"},null,null,"Std","Std"]
[null,null,null,null,null,null,null,1,"CD(EMI)",{"$f":"'Variable Mgmt'!B300","v":"10µF"},{"$f":"IF(VIN_max>35, \"Capacitor, Electrolytic, \"&'Variable Mgmt'!B300&\", 100V, ESR>\"&ESR_Cd&ohm, \"Capacitor, Electrolytic, \"&'Variable Mgmt'!B300&\", 50V, ESR>\"&ESR_Cd&ohm)","v":"Capacitor, Electrolytic, 10µF, 100V, ESR>3.3Ω"},null,null,"Std","Std"]

{"sheet":"Variable Mgmt","index":7,"n_rows":320,"n_cols":21,"rows_kept":320,"cut":false,"hidden":true,"merged":[[4,4,4,7],[0,0,0,8]]}
["EXCEL Variables Names/Calculations",null,null,null,null,null,null,null,null,null,null,"LM5166"]
[null,"Input from user ="]
[null,"Output ="]
[null,"Constant"]
["Variable Name","Value","STD Units",null,"Notes",null,null,null,"Iteration"]
["Step 1: Operational Specs"]
["VIN_min",{"$f":"'Design Converter'!E6","v":18},"V","Minimum input voltage",null,null,null,null,1]
["VIN_nom",{"$f":"'Design Converter'!E7","v":48},"V","Nominal input voltage"]
["VIN_max",{"$f":"'Design Converter'!E8","v":60},"V","Maximum input voltage"]
[]
["Vout",{"$f":"'Design Converter'!E9","v":5},"V","Output Voltage",null,null,null,null,1]
["Iout",{"$f":"'Design Converter'!E10","v":0.1},"A","Maximum Output Current",null,null,null,null,1]
["Rout",{"$f":"Vout/Iout","v":50},"W","Load resistance"]
["Pout",{"$f":"Vout*Iout","v":0.5},"W","Output power"]
[]
["Efficiency",0.9,null,"Estimate of efficiency"]
["Pin",{"$f":"Pout/Efficiency","v":0.55555555555555558},"W","Calculate input power assuming 90% efficiency"]
["Iin_Vinmin",{"$f":"Pin/VIN_min","v":3.0864197530864199E-2},"A"]
["Iin_Vinnom",{"$f":"Pin/VIN_nom","v":1.1574074074074075E-2},"A","Input currents at min, nom, max Vin"]
["Iin_Vinmax",{"$f":"Pin/VIN_max","v":9.2592592592592605E-3},"A"]
[]
["Fsw",{"$f":"'Design Converter'!E12*1000","v":300000},"Hz","Nominal Switching Frequency",null,null,null,null,1]
["Vref",1.2,"V","Reference Voltage"]
["Rt",{"$f":"Vout*2500000000/Fsw","v":41666.666666666664},"W","Frequency Set Resistor"]
[null,null,null,null,null,null,null,null,null,null,{"$f":"B34&\"_\"&F35&\"_\"&F39&\"_\"&I41&\"_\"&I36","v":"COT3_VOUTadj_UVLOadj_SSAdj_RsetGND"},null,null,null,null,null,"Vout<5V",100,1]
["Internal PD at Full Load",{"$f":" IF(OR(MODE=1,MODE=2,MODE=3), Efficiency!AZ106,#REF!)","v":0.22273269936649198},"W",null,null,null,null,null,null,null,null,null,null,null,null,null,"Vout<=8V",47,2]
[null,null,null,null,null,null,null,null,null,null,{"$f":"\"SCH_\"&B34&\"_\"&B41","v":"SCH_COT3_LM5164"},null,null,null,null,null,"Vout<=12V",22,3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Vout<=20V",22,4]
["Step 2: Circuit Configuration for COT / PFM, Fixed / Adj Vout, ILIM, UVLO, SS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Vout>20V",10,5]
[null,"COT Type I",1,null,null,null,null,null,null,null,null,null,null,null,null,null,"Cout Capacitance",{"$f":"CHOOSE(S30,\"100\", \"47\",\"22\",\"22\",\"10\")","v":"47"},{"$f":"IF(Vout<5, 1, IF(Vout<=8, 2, IF(Vout<=12, 3, IF(Vout<=20, 4, 5))))","v":2}]
[null,"COT Type II",2]
["COT/PFM ","COT Type III",3]
[null,null,null,null,"VOUT Fixed/Adjustable","Fixed",1,null,"ILIM shorted",1,{"$f":"B34&\", \"&F35&\", \"&I36&\", \"&F39&\", \"&I41","v":"COT3, VOUTadj, RsetGND, UVLOadj, SSAdj"},null,null,null,null,null,"Vout<=5V","6.3V",1]
["MODE",{"$f":"CHOOSE(C34, \"COT1\", \"COT2\",\"COT3\")","v":"COT3"},3,null,null,"Adjustable",2,null,"ILIM resistor needed",2,{"$f":"C34&\", \"&G35&\", \"&J36&\", \"&G39&\", \"&J41","v":"3, 2, 1, 1, 1"},null,null,null,null,null,"Vout<=8V","10V",2]
[null,{"$f":"IF(MODE=4, \"PFM\", \"COT\")","v":"COT"},null,null,"MODE_VOUT",{"$f":"CHOOSE(G35, \"VOUTfixed\", \"VOUTadj\")","v":"VOUTadj"},{"$f":"IF(AND(OR(MODE=1,MODE=4),OR(Vout=3.3,Vout=5)),1,2)","v":2},null,null,null,{"$f":"C34&G35&J36&G39&J41","v":"32111"},null,null,null,null,null,"Vout<=12V","16V",3]
[null,null,null,null,null,null,null,"MODE_RSET",{"$f":"CHOOSE(J36, \"RsetGND\",\"Rset\")","v":"RsetGND"},1,null,null,null,null,null,null,"Vout<=20V","25V",4]
[null,null,null,null,"UVLO","Adjustable",1,null,null,null,null,null,null,null,null,null,"Vout>20V","50V",5]
[null,null,null,null,null,"Internal",2,"Soft Start","Adjustable",1,null,"Iout Linear Axis",1,null,null,null,"Cout Voltage Rating",{"$f":"CHOOSE(S38,\"6.3V\", \"10V\",\"16V\",\"25V\",\"50V\")","v":"6.3V"},{"$f":"IF(Vout<=5, 1, IF(Vout<=8, 2, IF(Vout<=12, 3, IF(Vout<=20, 4, 5))))","v":1}]
[null,"LM5163",1,null,"MODE_UVLO",{"$f":"CHOOSE(G39, \"UVLOadj\", \"UVLOint\")","v":"UVLOadj"},1,null,"3ms Fixed",2,null,"Iout Log Axis",2]
[null,"LM5164",2,null,null,null,null,null,null,null,null,"PLOT_TYPE",1]
["VARIANT",{"$f":"CHOOSE(VARIANT, \"LM5163\", \"LM5164\")","v":"LM5164"},2,null,"ESR","NO",1,"MODE_SS",{"$f":"CHOOSE(J41, \"SSAdj\", \"SSfix\")","v":"SSAdj"},1,null,null,null,null,null,null,null,"0402",1,"1.0 x 0.5",0.5]
[null,null,null,null,null,"YES",2,null,null,null,null,null,null,null,null,null,null,"0603",2,"1.6 x 0.8",1.3]
[null,null,null,null,"MODE_ESR",null,2,null,null,null,null,null,null,null,null,null,null,"0805",3,"2.0 x 1.25",2.5]
[null,null,null,null,null,{"$f":"CHOOSE(G44, \"\", \"_ESR\")","v":"_ESR"},{"$f":"IF(MODE=2, 1, MODE_ESR)","v":2},null,null,null,null,null,null,null,null,null,null,"1206",4,"3.2 x 1.6",5.0999999999999996]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1210",5,"3.2 x 2.5",8]
["Step 3: Buck Inductor",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Component Size",{"$f":"CHOOSE(S46,\"0402\", \"0603\",\"0805\",\"1206\",\"1210\")","v":"1210"},5,{"$f":"CHOOSE(S46,T41,T42,T43,T44,T45)","v":"3.2 x 2.5"}]
["Don1",{"$f":"Vout/VIN_nom","v":0.10416666666666667},{"$f":"(Vout-VIN_nom)/Vout","v":-8.6},null,"Ideal Duty Cycle at VIN(nom)",null,null,null,1]
["Doff1",{"$f":"1-47:47","v":0.89583333333333337},null,null,"Ideal 1- Duty Cycle at VIN(nom)",null,null,null,1]
[]
["Don_Vinmin",{"$f":"Vout/VIN_min","v":0.27777777777777779},{"$f":"IF(VIN_min>Vout, \"BUCK\", \"BOOST\")","v":"BUCK"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3mm x 3mm",1,"3.0 x 3.0",9]
["Don_Vinnom",{"$f":"Vout/VIN_nom","v":0.10416666666666667},{"$f":"IF(VIN_nom>Vout, \"BUCK\", \"BOOST\")","v":"BUCK"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4mm x 4mm",2,"4.0 x 4.0",16]
["Don_Vinmax",{"$f":"Vout/VIN_max","v":8.3333333333333329E-2},{"$f":"IF(VIN_max>Vout, \"BUCK\", \"BOOST\")","v":"BUCK"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5mm x 5mm",3,"5.0 x 5.0",25]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6mm x 6mm",4,"6.0 x 6.0",36]
["Lf_Vinmin",{"$f":"(VIN_min-Vout)*Don_Vinmin/(Fsw*Iout*0.4)","v":3.0092592592592595E-4},"H","COT",null,null,null,null,null,null,null,null,null,null,null,null,null,"7mm x 7mm",5,"7.0 x 7.0",49]
["Lf_Vinnom",{"$f":"(VIN_nom-Vout)*Don_Vinnom/(Fsw*Iout*0.4)","v":3.7326388888888891E-4},"H","COT",null,null,null,null,1,null,null,null,null,null,null,null,"Inductor Size","8mm x 8mm",6,"8.0 x 8.0",64]
["Lf_Vinmax",{"$f":"(VIN_max-Vout)*Don_Vinmax/(Fsw*Iout*0.7)","v":2.1825396825396823E-4},"H","COT",null,null,null,null,null,null,null,null,null,null,null,null,null,"10mm x 10mm",7,"10.0 x 10.0",100]
[]
["L_Vinmin_COT",{"$f":"(VIN_min-Vout)*Don_Vinmin/(Fsw*Iout*0.3)","v":4.012345679012346E-4},"H","COT","Calculated Inductance for 30% ripple at VIN(min)"]
["L_Vinnom_COT",{"$f":"(VIN_nom-Vout)*Don_Vinnom/(Fsw*Iout*0.4)","v":3.7326388888888891E-4},"H","COT","Calculated Inductance for 40% ripple at VIN(nom)",null,null,null,null,null,"Pk-to-Pk Ripple Current at VIN(nom), DIL"]
["L_Vinmax_COT",{"$f":"(VIN_max-Vout)*Don_Vinmax/(Fsw*Iout*0.7)","v":2.1825396825396823E-4},"H","COT","Calculated Inductance for 70% ripple at VIN(max)"]
[]
[]
["Lopt",{"$f":"B59","v":3.7326388888888891E-4},"H"]
[]
["Lf",{"$f":"'Design Converter'!E17/1000000","v":3.6999999999999999E-4},"H",null,"Chosen Inductance"]
["Rdcr",{"$f":"'Design Converter'!E18/1000","v":0.12},"W",null,"Chosen Inductor DCR"]
[]
["Don2",{"$f":"(Vout+Iout*Rdcr)/Vin","v":0.10441666666666666},null,null,"**Edit to add Rdson**"]
["Doff2",{"$f":"1-_Don2","v":0.8955833333333334}]
[]
["Rdson1",0.75,"W"]
["Rdson2",0.33,"W"]
[]
["Don_Vinmin_2",{"$f":"(Vout+Iout*(Rdcr+Rdson2))/(VIN_min+Iout*Rdson2)","v":0.2797648755060167},null,null,"Duty cycles adjusted for DCR and shunt voltage drops"]
["Don_Vinnom_2",{"$f":"(Vout+Iout*(Rdcr+Rdson2))/(VIN_nom+Iout*Rdson2)","v":0.10503195719609434},null,null,"need to include RDS(on) later"]
["Don_Vinmax_2",{"$f":"(Vout+Iout*(Rdcr+Rdson2))/(VIN_max+Iout*Rdson2)","v":8.4037112921226662E-2}]
[]
["Iripple_Vinmin",{"$f":"(VIN_min-Vout-Rdson1*Iout)*Don_Vinmin_2/(Fsw*Lf)","v":3.2576225368606E-2},"A","COT"]
["Iripple_Vinnom",{"$f":"(VIN_nom-Vout-Rdson1*Iout)*Don_Vinnom_2/(Fsw*Lf)","v":4.0617087951732876E-2},"A","COT"]
["Iripple_Vinmax",{"$f":"(VIN_max-Vout)*Don_Vinmax_2/(Fsw*Lf)","v":4.1640010906914111E-2},"A","COT"]
[]
["ILpk_Vinmin",{"$f":"Iout+Iripple_Vinmin/2","v":0.116288112684303},"A","COT"]
["ILpk_Vinnom",{"$f":"Iout+Iripple_Vinnom/2","v":0.12030854397586645},"A","COT"]
["ILpk_Vinmax",{"$f":"Iout+Iripple_Vinmax/2","v":0.12082000545345706},"A","COT"]
[]
["ILIM_Typ",{"$f":"CHOOSE(VARIANT, 0.75, 1.5)","v":1.5},"A",null,"Isat_min",{"$f":"B86*1.2","v":1.7999999999999998}]
[]
["Ripple current",{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), Iripple_Vinnom, Iripple)","v":4.0617087951732876E-2},"A",null,null,null,null,"% Ripple Current at Nom VIN"]
[null,null,null,null,null,null,null,"Maximum Load Current"]
["Max inductor ripple current",{"$f":"MAX(B78:B80)","v":4.1640010906914111E-2},"A"]
[null,null,null,null,null,"Ripple I","Iin"]
["% Ripple Current",{"$f":"B78/Iout","v":0.32576225368605999},null,"COT",null,{"$f":"B78","v":3.2576225368606E-2},{"$f":"Iin_Vinmin","v":3.0864197530864199E-2}]
[null,{"$f":"B79/Iout","v":0.40617087951732872},null,"COT",null,{"$f":"B79","v":4.0617087951732876E-2},{"$f":"Iin_Vinnom","v":1.1574074074074075E-2}]
[null,{"$f":"B80/Iout","v":0.4164001090691411},null,"COT",null,{"$f":"B80","v":4.1640010906914111E-2},{"$f":"Iin_Vinmax","v":9.2592592592592605E-3}]
[]
[null,{"$f":"IF(OR(MODE=1, MODE=2,MODE=3), B93, Ilim/Iout)","v":0.40617087951732872}]
[]
["Iripple1",{"$f":"(Vin-Vout)*Don_Vinnom_2/(Fsw*Lf)","v":4.0688055490378891E-2},"A","inductor ripple current with chosen inductance (pk-pk)",null,null,null,null,1]
["Temp",100]
["DCR at hot",{"$f":"Rdcr*(1+0.0039*(B99-25))","v":0.15509999999999999},"W"]
[]
[]
[]
["Step 4: Output Capacitor"]
["Icoutrms_VINmin",{"$f":"Iripple_Vinmin/SQRT(12)","v":9.403946242873296E-3},"A","Output Cap RMS current"]
["Icoutrms_VINnom",{"$f":"Iripple_Vinnom/SQRT(12)","v":1.1725143331315841E-2},"A"]
["Icoutrms_VINmax",{"$f":"Iripple_Vinmax/SQRT(12)","v":1.2020435753082908E-2},"A",null,null,null,{"$f":"Vripple1","v":2.5000000000000001E-2}]
[]
["Output Ripple Spec (pk-pk)",{"$f":"Vout*0.005","v":2.5000000000000001E-2},"V","Vout capacitive ripple spec at Vin(nom) = Vripple1"]
[]
["Coutmin"]
["COT",{"$f":"Iripple_Vinnom/(Fsw*8*Vripple1)","v":6.7695146586221459E-7},"F","COT","Min recommended Cout based on ripple spec above",null,null,null,1]
[null,{"$f":"Lf*B83^2/((1.05*Vout)^2-Vout^2)","v":2.0899254356407441E-6},"F","COT","Min recommended Cout based on 5% load-off transient spec"]
["CoutMinCOT",{"$f":"MAX(B112:B113, 0.0000022)","v":2.2000000000000001E-6},"F","COT","max of 2 results and 2.2uF"]
[]
["Reported Countmin",{"$f":"CoutMinCOT*1000000","v":2.2000000000000002},"µF"]
[]
["Cout",{"$f":"'Design Converter'!E24/1000000","v":3.3000000000000003E-5},"F","Chosen Output Capacitance",null,null,null,null,1]
["Resrmax",{"$f":"SQRT((Vripple1/Iripple_Vinnom)^2-(1/(Fsw*Cout*8))^2)","v":0.61537497068877833},"W","Max ESR before ripple exceeds Vripple1",null,null,null,null,1]
["Type1 ESR for sufficient (20mV) COT ripple at FB pin",{"$f":"0.02*Vout/Vref/Iripple_Vinnom","v":2.0516816329216438},"W","(a)"]
["Type2 ESR for sufficient (20mV) COT ripple at FB pin",{"$f":"0.02/Iripple_Vinnom","v":0.49240359190119454},"W","(b)"]
[]
["Type 1 Output Cap RC Time Constant",{"$f":"Cout*B130*1000000","v":0},"µs"]
["Type 2 Output Cap RC Time Constant",{"$f":"Cout*B131*1000000","v":0},"µs"]
["Ton @ Vin(min)",{"$f":"Vout/VIN_min/(Fsw)","v":9.2592592592592594E-7},"s"]
["Ton @ Vin(nom)",{"$f":"Vout/VIN_nom/(Fsw)","v":3.4722222222222224E-7},"s"]
["ESR so that RC > Ton/2",{"$f":"B125/2/Cout","v":1.4029180695847361E-2},"W","(c)"]
[]
[]
["Type1: Need ESR of…",{"$f":"IF(MODE=1, MAX(B120,B127), 0)","v":0},"W","Max of (a) and (c)"]
["Type2: Need ESR of…",{"$f":"IF(MODE=2, MAX(B121,B127), 0)","v":0},"W","Max of (b) and (c)"]
[]
["Reported Cout ESR max",{"$f":"IF(OR(CoutEsrMax>0.5, CoutEsrMax<0, (ISERROR(CoutEsrMax))), \"N/A\", CoutEsrMax*1000)","v":"N/A"},"mW"]
[]
["CoutEsr",{"$f":" 'Design Converter'!E26","v":5.0000000000000001E-3},"W","Chosen ESR",null,null,null,null,1]
[]
["Actual Output Ripple",{"$f":"Iripple_Vinnom*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2)","v":5.515891885287214E-4},"Vp-p","Vripple2"]
[]
["Minimum Feedforward / Coupling Capacitance",{"$f":"MAX(1000000000000*0.00005/(3*Rfb1_),47)","v":47},"pF",null,null,null,null,{"$f":"0.00005/3/Rfb1_","v":3.6791758646063281E-11}]
["Recommended Cff / Cb",{"$f":"IF(OR(MODE=2,MODE=3), \">\"&ROUND(B139,0),\"\")","v":">47"},"pF"]
["Selected Cff / Cb",{"$f":"'Design Converter'!$E$29","v":56},"pF"]
[]
["Minimum Ripple Generation Capacitance",{"$f":"10/(Fsw*Rfb)","v":3.0668375039235966E-10},"F",{"$f":"1000000000000*B143","v":306.68375039235968},"pF",{"$f":"Rfb","v":108689.59731543624}]
["Recommended Ca",{"$f":"IF(MODE=3, \">\"&ROUND(D143,0),\"\")","v":">307"},"pF"]
["Selected Ca",{"$f":"'Design Converter'!E31","v":2200},"pF",{"$f":"B145/1000000000000","v":2.1999999999999998E-9},"F"]
[]
["Maximum Ripple Generation Resistance",{"$f":"(VIN_nom-Vout)*B126/((B149/1000)*Ca)","v":339330.80808080814},"W",{"$f":"B147/1000","v":339.33080808080814},"kW"]
["Recommended Ra",{"$f":"IF(MODE=3, \"<\"&ROUND(D147,0),\"\")","v":"<339"},"kW",null,null,null,null,null,null,null,null,"Lf_emi",{"$f":"'Design EMI Filter'!$E$9","v":22},"uH",{"$f":"M148/1000000","v":2.1999999999999999E-5},"H"]
["Ripple amplitude",{"$f":"'Design Converter'!E33","v":20},"mVp-p",null,null,null,null,null,null,null,null,"Cf_emi",{"$f":"'Design EMI Filter'!$E$11","v":4.7},"uF",{"$f":"M149/1000000","v":4.6999999999999999E-6},"F"]
[null,null,null,null,null,null,null,null,null,null,null,"Cd_emi",{"$f":"'Design EMI Filter'!$E$13","v":10},"uF",{"$f":"M150/1000000","v":1.0000000000000001E-5},"F"]
[null,null,null,null,null,null,null,null,null,null,null,"ESR_Cd",{"$f":"'Design EMI Filter'!$E$15","v":3.3},"Ω",{"$f":"M151","v":3.3},"Ω",{"$f":"ESR_Cd&ohm","v":"3.3Ω"}]
["Step 5: Input Capacitor",null,null,null,null,null,null,null,null,null,null,"Min Noise",{"$f":"'Design EMI Filter'!$E$8","v":50},"dB","noise limit"]
["Vinripple1",{"$f":"0.05*VIN_nom","v":2.4000000000000004},"Vp-p","Input voltage ripple spec (pk-pk) at Vin(nom)",null,null,null,null,null,null,null,"Duty Cycle",{"$f":"Vout/VIN_nom/Efficiency_COT_Full_Load","v":0.17160900604063703},null,"calculated duty cycle"]
[null,null,null,null,null,null,null,null,null,null,null,"Target Atten.",{"$f":"20*LOG(Iout/(PI()^2*Fsw*Cin)*SIN(PI()*Duty_Cycle)/0.000001) - Min_Noise","v":27.932003566716915},"dB","calculated attenuation"]
["Icinrms",{"$f":"Iout*SQRT(Don_Vinnom_2*(1-Don_Vinnom_2))","v":3.065945941526891E-2},"A"]
["Cinmin",{"$f":"Iout*Don_Vinnom_2*(1-Don_Vinnom_2)/(Vinripple1*Fsw-Iout*RCinEsr)*1000000","v":1.3055589611502624E-2},"µF"]
["Reported Cinmin",{"$f":"IF(Cinmin<2.2, 2.2,Cinmin)","v":2.2000000000000002},"µF",null,null,null,null,null,null,null,null,"Filter Inductor"]
["Cin",{"$f":"'Design Converter'!E37/1000000","v":2.2000000000000001E-6},"F","Input capacitance",null,null,null,null,null,null,null,"Irms rating",{"$f":"Iout*1.5","v":0.15000000000000002},"A","calculated suggested IRMS rating"]
["CinEsrMax",{"$f":"-(Iout*Don_Vinnom_2*(1-Don_Vinnom_2)/(Cin*Fsw)-Vinripple1)/(Iout+Iripple_Vinnom/2)","v":19.830325093869845},"W"]
["RCinEsr",{"$f":"'Design Converter'!E39/1000","v":3.0000000000000001E-3},"W","Input capacitance series resistance (ESR)"]
["Reported Cin ESR max",{"$f":"IF(OR(CinEsrMax>12, CinEsrMax<0), \"N/A\",CinEsrMax*1000)","v":"N/A"},"mΩ",null,null,null,null,null,null,null,null,"Filter Capacitor"]
[null,null,null,null,null,null,null,null,null,null,null,"Cfa calculation",{"$f":"Cin/(Cin*Lf_emi*0.000001*(2*PI()*Fsw/10)^2 - 1) / 0.000001","v":-2.2000037833022223},"uF","calculated value"]
["COT input voltage ripple - Vinripple2",{"$f":"Iout*Don_Vinnom_2*(1-Don_Vinnom_2)/(Cin*Fsw)+(Iout +Iripple_Vinnom/2)*RCinEsr","v":1.4603387020359741E-2},"Vp-p",null,{"$f":"Iout*Don_Vinmax_2*(1-Don_Vinmax_2)/(Cin*Fsw)","v":1.1662860086832068E-2},"Vp-p",null,null,null,null,null,"Cfb calculation",{"$f":"1/(Lf_emi)*(10^(Target_Att/40)/(2*PI()*Fsw))^2/0.000001","v":0.31884179934871787},"uF","calculated value"]
[null,null,null,null,null,null,null,null,null,null,null,"Cf",{"$f":"MAX(M162,M163)","v":0.31884179934871787},"uF","calculated value"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,"Damping Capacitor"]
["Step 6: Soft Start",null,null,null,null,null,null,null,null,null,null,"Cd ≥",{"$f":"4*Cin*1000000","v":8.8000000000000007},"uF","calculated value"]
["Tss",{"$f":"'Design Converter'!#REF!/1000","v":{"$error":"#REF!"}},"s","Soft-start time",null,null,null,null,null,null,null,"Cd ESR ≥",{"$f":"SQRT(Lf_emi/Cin)","v":3.1622776601683795},"Ω","calculated value"]
["Iss",1.0000000000000001E-5,"A","Soft-start current"]
["Css",{"$f":"8.16*Tss/1000000","v":{"$error":"#NAME?"}},"F","Required soft-start cap"]
["Css_u",{"$f":"'Standard Value Calculator'!B4","v":{"$error":"#NAME?"}},"F","User selected SS cap",null,null,null,null,null,null,null,"CIN and Cd Capacitors Current Sharing and Rating"]
[null,null,null,null,null,null,null,null,null,null,null,"Cd impedance",{"$f":" 1/(2*PI()*Fsw*Cd_emi) + ESR_Cd","v":3.3530516476972982},"Ω","calculated Cd impedance at the sw. frequency"]
["Step 7: Other Components - UVLO, PGOOD",null,null,null,null,null,null,null,null,null,null,"Cin impedance",{"$f":" 1/(2*PI()*Fsw*Cin) + RCinEsr","v":0.24414385316953838},"Ω","calculated CIN impedance at the sw. frequency"]
[]
["Rising UVLO/EN Threshold",1.5,"V",null,null,null,null,null,null,null,null,"IRMS Total Input Cap",{"$f":"Iout*SQRT(Duty_Cycle*(1-Duty_Cycle))","v":3.7704025658592696E-2},"A","calculated total IRMS current for CIN and Cd combined"]
["Falling UVLO/EN Threshold",1.4,"V",null,null,null,null,null,null,null,null,"IRMS Cd Act",{"$f":"IRMSTOT*(ZCIN/(ZCIN+ZCd))","v":2.558995223382697E-3},"A","Calculated min IRMS current rating for Cd"]
["Voltage Hysteresis",{"$f":"B176-B177","v":0.10000000000000009},"V",null,null,null,null,null,null,null,null,"IRMS CIN",{"$f":"IRMSTOT*(ZCd/(ZCIN+ZCd))","v":3.5145030435210001E-2},"A","Calculated min IRMS current rating for CIN"]
[]
["VINUVLO_ON",{"$f":"'Design Converter'!E48","v":6},"V"]
["VINUVLO_OFF",null,"V"]
[]
["RUV1",{"$f":"'Design Converter'!E49*1000","v":1000},"kΩ",{"$f":"'Standard Value Calculator'!J16","v":1000},"kΩ",{"$f":"IF(Ruvlo1<0,\"N/A\",D183)","v":1000},{"$f":"IF(Ruvlo1<0,\"N/A\",D183&\"kΩ\")","v":"1000kΩ"}]
["RUV2",{"$f":"Vuvlo_on*Ruvlo1/(VINuvlo_on-Vuvlo_on)","v":333.33333333333331},"kΩ",{"$f":"'Standard Value Calculator'!J17","v":332},"kΩ",{"$f":"IF(F183=\"N/A\",\"N/A\",D184)","v":332},{"$f":"IF(G183=\"N/A\",\"N/A\",D184&\"kΩ\")","v":"332kΩ"}]
[]
["VINUVLO_ON_ACTUAL",{"$f":"(D183+D184)/D184*Vuvlo_on","v":6.0180722891566267},"V"]
["VINUVLO_OFF_ACTUAL",{"$f":"(D183+D184)/D184*Vuvlo_off","v":5.6168674698795176},"V"]
[]
["RPG",20,"kΩ"]
[]
[]
["Step 8: FB Divider"]
["Pi",3.1415926500000002,null,"p"]
["Toff_Vinmax",{"$f":"(1-Don_Vinmax_2)/Fsw","v":3.0532096235959111E-6},"sec"]
["Ton_Vinmin",{"$f":"IF(VIN_min>Vout, (1-Don_Vinmin_2)/Fsw, Don_Vinmin_2/Fsw)","v":2.4007837483132775E-6},"sec"]
[]
["Rfb1",{"$f":"'Design Converter'!E43*1000","v":453000},"W","Lower Feedback Resistance - chosen by user",null,null,null,null,1]
["Rfb2",{"$f":"IF(Vout=Vref,100000000,Vref*B197/((Vout-Vref)))","v":143052.63157894739},"W","Upper Feedback Resistance"]
["Rfb2_u",{"$f":"IF(Vout=Vref,\"N/A\",'Standard Value Calculator'!J10)","v":143000},"W","Std Value Upper Feedback Resistance"]
["Rfb",{"$f":"Rfb1_*Rfb2_u/(Rfb1_+Rfb2_u)","v":108689.59731543624},"W","Rfb1 || Rfb2_u"]
[null,{"$f":"1.2/Rfb2_u*(Rfb2_u+Rfb1_)","v":5.0013986013986012},"V"]
["Ifb",{"$f":"CHOOSE(MODE_VOUT, IF(Vout=5, 0.000007, 0.0000038), Vout/(Rfb1_+Rfb2_u))","v":8.3892617449664422E-6}]
[]
["Other Input Variables"]
["Rfets",0,"W","Series resistance due to FETs",null,null,null,{"$f":"_Don2*RdsonTop+Doff2*RdsonBot+B209*Vin^2*Fsw/2/(((Iripple1/SQRT(3))^2))","v":3131.6904581745416}]
["Diode loss eq res",{"$f":"0.00000002*Fsw*0.6*4/Iripple1","v":0.35391221886740271}]
["Fet loss eq res",{"$f":"_Don2*RdsonTop+Doff2*RdsonBot","v":0.34399158333333335}]
["cap loss eq res",{"$f":"B209*Vin^2*Fsw/2/(((Iripple1/SQRT(3))^2))","v":3131.3464665912084}]
["Sw cap",5.0000000000000001E-9]
[]
["Step 8: Efficiency"]
[]
["Design"]
["Ta",25,"°C","Ambient Temperature"]
["Components"]
["LTc",{"$f":"4000/1000000","v":4.0000000000000001E-3},"%/°C","Inductor DCR Temp Co"]
["θCA",40,"°C/W","Inductor Core to Ambient Thermal Resistance"]
["RCinEsr",{"$f":"RCinEsr","v":3.0000000000000001E-3},"W","Input Capacitor ESR"]
["Part Characteristics"]
["Vcc",{"$f":"IF(Vin>7.7,7.5,Vin-0.2)","v":7.5},"V"]
["Deadtime"]
["Deadtime",2E-8,"s","Total Deadtime",null,null,"20ns for LM5166"]
["IQ"]
["IQ ",1.0000000000000001E-5,"A","Quiescent Current Of Controller (Not Switching!)"]
[]
[]
["IC Power Disipation","Value","Units"]
["Power Dis",{"$f":"Efficiency!AZ106","v":0.22273269936649198},"W"]
["Temp rise",{"$f":"B228*ThetaJA","v":9.1543139439628209},"°C"]
["Current (switching)",{"$f":"(Qg_Q1+Qg_Q2)*Fsw+Iq","v":{"$error":"#NAME?"}},"A"]
["Qrr Current",{"$f":"Qrr_Q2*Fsw","v":{"$error":"#NAME?"}},"A"]
["Diode Current",{"$f":"C232/Vin","v":{"$error":"#NAME?"}},{"$f":"Deadtime*Fsw*(Ipp/2)*(Vsd_Q1+Vsd_Q2)","v":{"$error":"#NAME?"}}]
["Total Application Switching IQ",{"$f":"SUM(B230:B232)","v":{"$error":"#NAME?"}},"A"]
[]
[]
["SCHEMATIC LABELS"]
[]
[]
[{"$f":"\"RUV1 = \"&'Design Converter'!E49&\"MΩ\"","v":"RUV1 = 1MΩ"},{"$f":"C275","v":"1MΩ"}]
[{"$f":"\"RUV2 = \"&'Design Converter'!E50&\"kΩ\"","v":"RUV2 = 332kΩ"},{"$f":"C276","v":"332kΩ"}]
[{"$f":"\"Rhys = \"&'Design Converter'!E52&\"kΩ\"","v":"Rhys = 5.61686746987952kΩ"},{"$f":"C277","v":{"$error":"#REF!"}}]
[]
[{"$f":"\"LF = \"&'Design Converter'!E17&\"µH\"","v":"LF = 370µH"},{"$f":"'Design Converter'!E17&\"µH\"","v":"370µH"}]
[{"$f":"\"Rdcr = \"&Rdcr*1000&\"mΩ\"","v":"Rdcr = 120mΩ"},{"$f":"Rdcr*1000&\"mΩ\"","v":"120mΩ"}]
[{"$f":"\"Rt = \"&'Design Converter'!I43&\"kΩ\"","v":"Rt = kΩ"},{"$f":"'Design Converter'!I43&\"kΩ\"","v":"kΩ"}]
[{"$f":"\"Css = \"&ROUND(Css_u*1000000000,1)&\"nF\"","v":{"$error":"#NAME?"}},{"$f":"ROUND(Css_u*1000000000,1)&\"nF\"","v":{"$error":"#NAME?"}}]
[]
["VIN",{"$f":"VIN_nom&\"V\"","v":"48V"}]
["VIN range",{"$f":"VIN_min&\"V...\"&VIN_max&\"V\"","v":"18V...60V"}]
[]
[{"$f":"\"VOUT = \"&'Design Converter'!E9&\"V\"","v":"VOUT = 5V"},{"$f":"'Design Converter'!E9&\"V\"","v":"5V"}]
[null,null,{"$f":"R30","v":"47"},{"$f":"ROUNDUP('Design Converter'!$E$24/C252,0)","v":1}]
[{"$f":"\"COUT = \"&'Design Converter'!$E$24&\"µF\"","v":"COUT = 33µF"},{"$f":"'Design Converter'!$E$24&\"µF\"","v":"33µF"},{"$f":"IF('Design Converter'!$E$24=OR(10, 22, 47, 100), 'Design Converter'!$E$24,C252)","v":"47"},{"$f":"IF(D252=1, \"\",B255)","v":""},{"$f":"D253&C253&\"µF\"","v":"47µF"},{"$f":"C253&\"µF\"","v":"47µF"}]
["Capacitance per component (Cout)",{"$f":"C252&\"µF\"","v":"47µF"}]
["# of output caps",{"$f":"D252&\" x \"","v":"1 x "}]
[]
["CIN",{"$f":"Cin*1000000&\"µF\"","v":"2.2µF"}]
["Capacitance per component (Cin)",{"$f":"\"2.2µF\"","v":"2.2µF"}]
["# of input caps",{"$f":"ROUNDUP(Cin*1000000/2.2,0)&\" x \"","v":"1 x "}]
[]
["Fixed VOUT?",{"$f":"IF(MODE_VOUT=1, \"YES\", \"NO\")","v":"NO"}]
["FB resistor ref des shown or not?",{"$f":"IF(MODE_VOUT=2, \"YES\", \"NO\")","v":"YES"},{"$f":"IF(MODE_VOUT=2, \"R1\", \"\")","v":"R1"},{"$f":"IF(MODE_VOUT=2, \"R2\", \"\")","v":"R2"}]
[{"$f":"\"RFB1 = \"&'Design Converter'!E43&\"kΩ\"","v":"RFB1 = 453kΩ"},{"$f":"'Design Converter'!E43&\"kΩ\"","v":"453kΩ"},{"$f":"IF(MODE=1,'Design Converter'!E43&\"kΩ\", \"\")","v":""}]
[{"$f":"\"RFB2 = \"&IF(Vout=Vref,\"OPEN\",'Design Converter'!E44&\"kΩ\")","v":"RFB2 = 143kΩ"},{"$f":"IF(Vout=Vref,\"OPEN\",Rfb2_u/1000&\"kΩ\")","v":"143kΩ"},{"$f":"IF(MODE=1, IF(Vout=Vref, \"OPEN\",Rfb2_u/1000&\"kΩ\" ), \"\")","v":""}]
[]
[]
["Show Rt resistor ref des?",{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), \"YES\", \"NO\")","v":"YES"},{"$f":"IF(MODE=4,\"\", \"Rt\")","v":"Rt"}]
["Rt",{"$f":"IF(MODE=4, \"\", 'Standard Value Calculator'!J4/1000&\"kΩ\")","v":"41.2kΩ"}]
[]
["Show ESR resistor ref des?",{"$f":"IF(OR(MODE=3, MODE=4), \"NO\", \"YES\")","v":"NO"},{"$f":"IF(OR(MODE=3, MODE=4),\"\",\"Resr\")","v":""}]
[{"$f":"\"RESR = \"&'Design Converter'!E26&\"mΩ\"","v":"RESR = 0.005mΩ"},{"$f":"IF(OR(MODE=3,MODE=4), \"\", 'Design Converter'!E26&\"Ω\")","v":""},null,null,null,{"$f":"B120","v":2.0516816329216438}]
["Resr",{"$f":"IF(MODE=1, \">\"&ROUND(B130,3), IF(MODE=2,  \">\"&ROUND(B131,3),IF(MODE=3,ROUND(B119,3),\"\")))","v":0.61499999999999999}]
[]
["Adjustable UVLO?",{"$f":"IF(MODE_UVLO=1, \"YES\", \"NO\")","v":"YES"},{"$f":"IF(MODE_UVLO=1,\"Ren1\", \"\")","v":"Ren1"},{"$f":"IF(MODE_UVLO=1, \"Ren2\", \"\")","v":"Ren2"},{"$f":"IF(MODE_UVLO=1, \"Rhys\", \"\")","v":"Rhys"},"Value","Units","BOM display"]
[{"$f":"\"RUV1 = \"&C275","v":"RUV1 = 1MΩ"},{"$f":"'Design Converter'!E49&\" MΩ\"","v":"1 MΩ"},{"$f":"IF(MODE_UVLO=1,'Design Converter'!E49&\"MΩ\", \"\")","v":"1MΩ"},null,null,{"$f":"IF(MODE_UVLO=1,'Design Converter'!E49, \"\")","v":1},{"$f":"IF(MODE_UVLO=1,\"MΩ\", \"\")","v":"MΩ"},{"$f":"IF(MODE_UVLO=1,'Design Converter'!E49&\"M\", \"\")","v":"1M"}]
[{"$f":"\"RUV2 = \"&C276","v":"RUV2 = 332kΩ"},{"$f":"IF(D184>=1000, D184/1000&\" MΩ\", D184&\" kΩ\")","v":"332 kΩ"},{"$f":"IF(MODE_UVLO=1, IF(D184<1, D184*1000&\"Ω\", IF(D184<1000, D184&\"kΩ\", D184/1000&\"MΩ\")), \"\")","v":"332kΩ"},null,null,{"$f":"IF(MODE_UVLO=1, IF(D184<1, D184*1000, IF(D184<1000, D184, D184/1000)), \"\")","v":332},{"$f":"IF(MODE_UVLO=1, IF(D184<1, \"Ω\", IF(D184<1000,\"kΩ\", \"MΩ\")), \"\")","v":"kΩ"},{"$f":"IF(MODE_UVLO=1, IF(D184<1, D184*1000, IF(D184<1000, D184&\"k\", D184/1000&\"M\")), \"\")","v":"332k"}]
[{"$f":"\"RHYS = \"&C277","v":{"$error":"#REF!"}},{"$f":"IF(#REF!<1000,#REF!& \" kΩ\",#REF!& \" MΩ\")","v":{"$error":"#REF!"}},{"$f":"IF(MODE_UVLO=1, IF(#REF!<1,#REF!* 1000&\"Ω\", IF(#REF!<1000,#REF!& \"kΩ\",#REF!/ 1000&\"MΩ\")), \"\")","v":{"$error":"#REF!"}},null,null,{"$f":"IF(MODE_UVLO=1, IF(#REF!<1,#REF!* 1000, IF(#REF!<1000,#REF!,#REF!/ 1000)), \"\")","v":{"$error":"#REF!"}},{"$f":"IF(MODE_UVLO=1, IF(#REF!<1, \"Ω\", IF(#REF!<1000,\"kΩ\", \"MΩ\")), \"\")","v":{"$error":"#REF!"}},{"$f":"IF(MODE_UVLO=1, IF(#REF!<1,#REF!* 1000, IF(#REF!<1000,#REF!& \"k\",#REF!& \"M\")), \"\")","v":{"$error":"#REF!"}}]
[]
[{"$f":"\"Css = \"&Css*1000000000&\"nF\"","v":{"$error":"#NAME?"}},{"$f":"Css*1000000000&\"nF\"","v":{"$error":"#NAME?"}}]
["Cbst",{"$f":"\"2.2nF\"","v":"2.2nF"},null,{"$f":"B280","v":"2.2nF"}]
[]
[]
["Rset resistor ref des?",{"$f":"IF(MODE_RSET=2, \"YES\", \"NO\")","v":"NO"},{"$f":"IF(MODE_RSET=2, \"R3\", \"\")","v":""},null,null,{"$f":"MODE_RSET","v":1}]
["Rset",{"$f":"IF(MODE_RSET=2, C284&\"kΩ\", \"\")","v":""},{"$f":"IF(MODE_ILIM=3,100,IF(MODE_ILIM=2,56.2,IF(MODE_ILIM=4,24.9,0)))","v":{"$error":"#REF!"}}]
[]
[]
["Rpgood","100kΩ"]
[]
["Cff / Cb?",{"$f":"IF(MODE=2, \"Cff\", IF(MODE=3,\"Cb\",\"\"))","v":"Cb"}]
[{"$f":"\"Cff / Cb=\"&B290","v":"Cff / Cb=56pF"},{"$f":"IF(OR(MODE=2,MODE=3),B141&\"pF\",\"\")","v":"56pF"}]
[]
["Ca?",{"$f":"IF(MODE=3, \"Ca\",\"\")","v":"Ca"},null,{"$f":"Ca","v":2.1999999999999998E-9},{"$f":"Ton_Vinmin","v":2.4007837483132775E-6}]
["Ca=",{"$f":"IF(MODE=3,B145&\"pF\",\"\")","v":"2200pF"}]
[]
["Ra?",{"$f":"IF(MODE=3, \"Ra\",\"\")","v":"Ra"},"Injected Ripple"]
["Ra=",{"$f":"IF(MODE=3,Ra&\"kΩ\",\"\")","v":"340kΩ"},{"$f":"(VIN_nom-Vout)*Ton_Vin_nom/(Ra*Ca)/1000","v":1.9960635769459303E-2},{"$f":"ROUNDUP(1000*C296,0)","v":20},null,{"$f":"IF(MODE=3,Ra&\"k\",\"\")","v":"340k"}]
[]
["Lf(emi)",{"$f":"M148&\"µH\"","v":"22µH"}]
["Cf(emi)",{"$f":"M149&\"µF\"","v":"4.7µF"}]
["Df(emi)",{"$f":"M150&\"µF\"","v":"10µF"}]
[]
["Full-load efficiency",{"$f":"ROUND(Efficiency!CE106,1)&\"%\"","v":"60.7%"}]
["Full-load efficiency",{"$f":"ROUND(Efficiency!CE107,1)&\"%\"","v":"80.8%"}]
["10% load efficiency",{"$f":"ROUND(Efficiency!CE16,1)&\"%\"","v":"24.6%"},"linear scale only"]
["1% load efficiency",{"$f":"ROUND(Efficiency!CE56,1)&\"%\"","v":"45.3%"},"log scale only"]
[]
["Blank out",{"$f":"IF(C307=\"y\",\"\",\"|\")","v":"|"},"n"]
[]
["OUTPUT CURRENT",{"$f":"'Design Converter'!$E$10&\"A\"","v":"0.1A"}]
[]
["VIN ",2]
["RT",5]
["EN",7]
["PGOOD",6]
["SS",4]
["ILIM",3]
["GND",10]
["FB",8]
["SW",1]
["HYS",9]

{"sheet":"Standard Value Calculator","index":8,"n_rows":159,"n_cols":11,"rows_kept":159,"cut":false,"hidden":true,"merged":[]}
[]
["Capacitors","Css","Cout","Cin","Cb"]
["Inputs",{"$f":"Css","v":{"$error":"#NAME?"}},{"$f":"Cout","v":3.3000000000000003E-5},{"$f":"Cin","v":2.2000000000000001E-6},{"$f":"Cb","v":0},null,null,"Resistors","inputs","Standard Result"]
["Standard Result",{"$f":"SUM(B6:B158)/1000000000000","v":{"$error":"#NAME?"}},{"$f":"SUM(C6:C158)/1000000000000","v":3.3000000000000003E-5},{"$f":"SUM(D6:D158)/1000000000000","v":2.2000000000000001E-6},{"$f":"IF(E3=\"OPEN\",\"OPEN\",SUM(E6:E158)/1000000000000)","v":0},null,null,"Rt",{"$f":"Rt","v":41666.666666666664},{"$f":"IF(I4>(INT(0.5+100*POWER(10,IF(96*(LOG(I4)-INT(LOG(I4)))-ROUND(96*(LOG(I4)-INT(LOG(I4))),0)<0,ROUND(96*(LOG(I4)-INT(LOG(I4))),0)-1,ROUND(96*(LOG(I4)-INT(LOG(I4))),0))/96))*POWER(10,INT(LOG(I4))-2)+INT(0.5+100*POWER(10,(IF(96*(LOG(I4)-INT(LOG(I4)))-ROUND(96*(LOG(I4)-INT(LOG(I4))),0)<0,ROUND(96*(LOG(I4)-INT(LOG(I4))),0)-1,ROUND(96*(LOG(I4)-INT(LOG(I4))),0))+1)/96))*POWER(10,INT(LOG(I4))-2))/2,INT(0.5+100*POWER(10,(IF(96*(LOG(I4)-INT(LOG(I4)))-ROUND(96*(LOG(I4)-INT(LOG(I4))),0)<0,ROUND(96*(LOG(I4)-INT(LOG(I4))),0)-1,ROUND(96*(LOG(I4)-INT(LOG(I4))),0))+1)/96))*POWER(10,INT(LOG(I4))-2),INT(0.5+100*POWER(10,IF(96*(LOG(I4)-INT(LOG(I4)))-ROUND(96*(LOG(I4)-INT(LOG(I4))),0)<0,ROUND(96*(LOG(I4)-INT(LOG(I4))),0)-1,ROUND(96*(LOG(I4)-INT(LOG(I4))),0))/96))*POWER(10,INT(LOG(I4))-2))","v":41200},"Ω"]
["(pF)"]
[0.47,{"$f":"IF(IF((B$3*10^12-$A7)*(B$3*10^12-$A6)*-1<0,0,1)*IF(ABS(B$3*10^12-$A7)>(B$3*10^12-$A6),$A6,$A7)=B7,0,IF((B$3*10^12-$A7)*(B$3*10^12-$A6)*-1<0,0,1)*IF(ABS(B$3*10^12-$A7)>(B$3*10^12-$A6),$A6,$A7))","v":{"$error":"#NAME?"}},{"$f":"IF(IF((C$3*10^12-$A7)*(C$3*10^12-$A6)*-1<0,0,1)*IF(ABS(C$3*10^12-$A7)>(C$3*10^12-$A6),$A6,$A7)=C7,0,IF((C$3*10^12-$A7)*(C$3*10^12-$A6)*-1<0,0,1)*IF(ABS(C$3*10^12-$A7)>(C$3*10^12-$A6),$A6,$A7))","v":0},{"$f":"IF(IF((D$3*10^12-$A7)*(D$3*10^12-$A6)*-1<0,0,1)*IF(ABS(D$3*10^12-$A7)>(D$3*10^12-$A6),$A6,$A7)=D7,0,IF((D$3*10^12-$A7)*(D$3*10^12-$A6)*-1<0,0,1)*IF(ABS(D$3*10^12-$A7)>(D$3*10^12-$A6),$A6,$A7))","v":0},{"$f":"IF(IF((E$3*10^12-$A7)*(E$3*10^12-$A6)*-1<0,0,1)*IF(ABS(E$3*10^12-$A7)>(E$3*10^12-$A6),$A6,$A7)=E7,0,IF((E$3*10^12-$A7)*(E$3*10^12-$A6)*-1<0,0,1)*IF(ABS(E$3*10^12-$A7)>(E$3*10^12-$A6),$A6,$A7))","v":0},null,null,"Rshunt",{"$f":"Rshunt","v":{"$error":"#NAME?"}},{"$error":"#NAME?"},"Ω"]
[0.56000000000000005,{"$f":"IF(IF((B$3*10^12-$A8)*(B$3*10^12-$A7)*-1<0,0,1)*IF(ABS(B$3*10^12-$A8)>(B$3*10^12-$A7),$A7,$A8)=B8,0,IF((B$3*10^12-$A8)*(B$3*10^12-$A7)*-1<0,0,1)*IF(ABS(B$3*10^12-$A8)>(B$3*10^12-$A7),$A7,$A8))","v":{"$error":"#NAME?"}},{"$f":"IF(IF((C$3*10^12-$A8)*(C$3*10^12-$A7)*-1<0,0,1)*IF(ABS(C$3*10^12-$A8)>(C$3*10^12-$A7),$A7,$A8)=C8,0,IF((C$3*10^12-$A8)*(C$3*10^12-$A7)*-1<0,0,1)*IF(ABS(C$3*10^12-$A8)>(C$3*10^12-$A7),$A7,$A8))","v":0},{"$f":"IF(IF((D$3*10^12-$A8)*(D$3*10^12-$A7)*-1<0,0,1)*IF(ABS(D$3*10^12-$A8)>(D$3*10^12-$A7),$A7,$A8)=D8,0,IF((D$3*10^12-$A8)*(D$3*10^12-$A7)*-1<0,0,1)*IF(ABS(D$3*10^12-$A8)>(D$3*10^12-$A7),$A7,$A8))","v":0},{"$f":"IF(IF((E$3*10^12-$A8)*(E$3*10^12-$A7)*-1<0,0,1)*IF(ABS(E$3*10^12-$A8)>(E$3*10^12-$A7),$A7,$A8)=E8,0,IF((E$3*10^12-$A8)*(E$3*10^12-$A7)*-1<0,0,1)*IF(ABS(E$3*10^12-$A8)>(E$3*10^12-$A7),$A7,$A8))","v":0},null,null,"Rc1ea",{"$f":"Rcea1","v":{"$error":"#NAME?"}},{"$error":"#NAME?"},"Ω"]
[0.68,{"$error":"#NAME?"},0,0,0]
[0.82,{"$error":"#NAME?"},0,0,0,null,null,"Rfb1",{"$f":"Rfb1_","v":453000},453000,"Ω"]
[1,{"$error":"#NAME?"},0,0,0,null,null,"Rfb2",{"$f":"Rfb2_","v":143052.63157894739},{"$f":"IF(I10=\"OPEN\",\"OPEN\",IF(I10>(INT(0.5+100*POWER(10,IF(96*(LOG(I10)-INT(LOG(I10)))-ROUND(96*(LOG(I10)-INT(LOG(I10))),0)<0,ROUND(96*(LOG(I10)-INT(LOG(I10))),0)-1,ROUND(96*(LOG(I10)-INT(LOG(I10))),0))/96))*POWER(10,INT(LOG(I10))-2)+INT(0.5+100*POWER(10,(IF(96*(LOG(I10)-INT(LOG(I10)))-ROUND(96*(LOG(I10)-INT(LOG(I10))),0)<0,ROUND(96*(LOG(I10)-INT(LOG(I10))),0)-1,ROUND(96*(LOG(I10)-INT(LOG(I10))),0))+1)/96))*POWER(10,INT(LOG(I10))-2))/2,INT(0.5+100*POWER(10,(IF(96*(LOG(I10)-INT(LOG(I10)))-ROUND(96*(LOG(I10)-INT(LOG(I10))),0)<0,ROUND(96*(LOG(I10)-INT(LOG(I10))),0)-1,ROUND(96*(LOG(I10)-INT(LOG(I10))),0))+1)/96))*POWER(10,INT(LOG(I10))-2),INT(0.5+100*POWER(10,IF(96*(LOG(I10)-INT(LOG(I10)))-ROUND(96*(LOG(I10)-INT(LOG(I10))),0)<0,ROUND(96*(LOG(I10)-INT(LOG(I10))),0)-1,ROUND(96*(LOG(I10)-INT(LOG(I10))),0))/96))*POWER(10,INT(LOG(I10))-2)))","v":143000},"Ω"]
[1.2,{"$error":"#NAME?"},0,0,0]
[1.5,{"$error":"#NAME?"},0,0,0]
[1.8,{"$error":"#NAME?"},0,0,0,null,null,"Rs",{"$f":"Rs_ideal*1000","v":{"$error":"#NAME?"}},{"$f":"IF(I13=0,0,IF(I13>(INT(0.5+100*POWER(10,IF(96*(LOG(I13)-INT(LOG(I13)))-ROUND(96*(LOG(I13)-INT(LOG(I13))),0)<0,ROUND(96*(LOG(I13)-INT(LOG(I13))),0)-1,ROUND(96*(LOG(I13)-INT(LOG(I13))),0))/96))*POWER(10,INT(LOG(I13))-2)+INT(0.5+100*POWER(10,(IF(96*(LOG(I13)-INT(LOG(I13)))-ROUND(96*(LOG(I13)-INT(LOG(I13))),0)<0,ROUND(96*(LOG(I13)-INT(LOG(I13))),0)-1,ROUND(96*(LOG(I13)-INT(LOG(I13))),0))+1)/96))*POWER(10,INT(LOG(I13))-2))/2,INT(0.5+100*POWER(10,(IF(96*(LOG(I13)-INT(LOG(I13)))-ROUND(96*(LOG(I13)-INT(LOG(I13))),0)<0,ROUND(96*(LOG(I13)-INT(LOG(I13))),0)-1,ROUND(96*(LOG(I13)-INT(LOG(I13))),0))+1)/96))*POWER(10,INT(LOG(I13))-2),INT(0.5+100*POWER(10,IF(96*(LOG(I13)-INT(LOG(I13)))-ROUND(96*(LOG(I13)-INT(LOG(I13))),0)<0,ROUND(96*(LOG(I13)-INT(LOG(I13))),0)-1,ROUND(96*(LOG(I13)-INT(LOG(I13))),0))/96))*POWER(10,INT(LOG(I13))-2)))","v":{"$error":"#NAME?"}},"mΩ"]
[2.2000000000000002,{"$f":"IF(IF((B$3*10^12-$A15)*(B$3*10^12-$A14)*-1<0,0,1)*IF(ABS(B$3*10^12-$A15)>(B$3*10^12-$A14),$A14,$A15)=B15,0,IF((B$3*10^12-$A15)*(B$3*10^12-$A14)*-1<0,0,1)*IF(ABS(B$3*10^12-$A15)>(B$3*10^12-$A14),$A14,$A15))","v":{"$error":"#NAME?"}},{"$f":"IF(IF((C$3*10^12-$A15)*(C$3*10^12-$A14)*-1<0,0,1)*IF(ABS(C$3*10^12-$A15)>(C$3*10^12-$A14),$A14,$A15)=C15,0,IF((C$3*10^12-$A15)*(C$3*10^12-$A14)*-1<0,0,1)*IF(ABS(C$3*10^12-$A15)>(C$3*10^12-$A14),$A14,$A15))","v":0},{"$f":"IF(IF((D$3*10^12-$A15)*(D$3*10^12-$A14)*-1<0,0,1)*IF(ABS(D$3*10^12-$A15)>(D$3*10^12-$A14),$A14,$A15)=D15,0,IF((D$3*10^12-$A15)*(D$3*10^12-$A14)*-1<0,0,1)*IF(ABS(D$3*10^12-$A15)>(D$3*10^12-$A14),$A14,$A15))","v":0},{"$f":"IF(IF((E$3*10^12-$A15)*(E$3*10^12-$A14)*-1<0,0,1)*IF(ABS(E$3*10^12-$A15)>(E$3*10^12-$A14),$A14,$A15)=E15,0,IF((E$3*10^12-$A15)*(E$3*10^12-$A14)*-1<0,0,1)*IF(ABS(E$3*10^12-$A15)>(E$3*10^12-$A14),$A14,$A15))","v":0},null,null,"Cslope_ideal",{"$f":"Cslope_ideal","v":{"$error":"#NAME?"}},{"$f":"#REF!*1000000000000","v":{"$error":"#REF!"}},"pF"]
[2.7,{"$error":"#NAME?"},0,0,0]
[3.3,{"$error":"#NAME?"},0,0,0,null,null,"Ruv1",{"$f":"Ruvlo1","v":1000},{"$f":"IF(I16=\"OPEN\",\"OPEN\",IF(I16>(INT(0.5+100*POWER(10,IF(96*(LOG(I16)-INT(LOG(I16)))-ROUND(96*(LOG(I16)-INT(LOG(I16))),0)<0,ROUND(96*(LOG(I16)-INT(LOG(I16))),0)-1,ROUND(96*(LOG(I16)-INT(LOG(I16))),0))/96))*POWER(10,INT(LOG(I16))-2)+INT(0.5+100*POWER(10,(IF(96*(LOG(I16)-INT(LOG(I16)))-ROUND(96*(LOG(I16)-INT(LOG(I16))),0)<0,ROUND(96*(LOG(I16)-INT(LOG(I16))),0)-1,ROUND(96*(LOG(I16)-INT(LOG(I16))),0))+1)/96))*POWER(10,INT(LOG(I16))-2))/2,INT(0.5+100*POWER(10,(IF(96*(LOG(I16)-INT(LOG(I16)))-ROUND(96*(LOG(I16)-INT(LOG(I16))),0)<0,ROUND(96*(LOG(I16)-INT(LOG(I16))),0)-1,ROUND(96*(LOG(I16)-INT(LOG(I16))),0))+1)/96))*POWER(10,INT(LOG(I16))-2),INT(0.5+100*POWER(10,IF(96*(LOG(I16)-INT(LOG(I16)))-ROUND(96*(LOG(I16)-INT(LOG(I16))),0)<0,ROUND(96*(LOG(I16)-INT(LOG(I16))),0)-1,ROUND(96*(LOG(I16)-INT(LOG(I16))),0))/96))*POWER(10,INT(LOG(I16))-2)))","v":1000},"kΩ"]
[3.9,{"$error":"#NAME?"},0,0,0,null,null,"Ruv2",{"$f":"Ruvlo2","v":333.33333333333331},{"$f":"IF(I17=\"OPEN\",\"OPEN\",IF(I17>(INT(0.5+100*POWER(10,IF(96*(LOG(I17)-INT(LOG(I17)))-ROUND(96*(LOG(I17)-INT(LOG(I17))),0)<0,ROUND(96*(LOG(I17)-INT(LOG(I17))),0)-1,ROUND(96*(LOG(I17)-INT(LOG(I17))),0))/96))*POWER(10,INT(LOG(I17))-2)+INT(0.5+100*POWER(10,(IF(96*(LOG(I17)-INT(LOG(I17)))-ROUND(96*(LOG(I17)-INT(LOG(I17))),0)<0,ROUND(96*(LOG(I17)-INT(LOG(I17))),0)-1,ROUND(96*(LOG(I17)-INT(LOG(I17))),0))+1)/96))*POWER(10,INT(LOG(I17))-2))/2,INT(0.5+100*POWER(10,(IF(96*(LOG(I17)-INT(LOG(I17)))-ROUND(96*(LOG(I17)-INT(LOG(I17))),0)<0,ROUND(96*(LOG(I17)-INT(LOG(I17))),0)-1,ROUND(96*(LOG(I17)-INT(LOG(I17))),0))+1)/96))*POWER(10,INT(LOG(I17))-2),INT(0.5+100*POWER(10,IF(96*(LOG(I17)-INT(LOG(I17)))-ROUND(96*(LOG(I17)-INT(LOG(I17))),0)<0,ROUND(96*(LOG(I17)-INT(LOG(I17))),0)-1,ROUND(96*(LOG(I17)-INT(LOG(I17))),0))/96))*POWER(10,INT(LOG(I17))-2)))","v":332},"kΩ"]
[4.7,{"$error":"#NAME?"},0,0,0,null,null,"Rhys",{"$f":"Rhys","v":{"$error":"#NAME?"}},{"$f":"IF(I18=\"OPEN\",\"OPEN\",IF(I18>(INT(0.5+100*POWER(10,IF(96*(LOG(I18)-INT(LOG(I18)))-ROUND(96*(LOG(I18)-INT(LOG(I18))),0)<0,ROUND(96*(LOG(I18)-INT(LOG(I18))),0)-1,ROUND(96*(LOG(I18)-INT(LOG(I18))),0))/96))*POWER(10,INT(LOG(I18))-2)+INT(0.5+100*POWER(10,(IF(96*(LOG(I18)-INT(LOG(I18)))-ROUND(96*(LOG(I18)-INT(LOG(I18))),0)<0,ROUND(96*(LOG(I18)-INT(LOG(I18))),0)-1,ROUND(96*(LOG(I18)-INT(LOG(I18))),0))+1)/96))*POWER(10,INT(LOG(I18))-2))/2,INT(0.5+100*POWER(10,(IF(96*(LOG(I18)-INT(LOG(I18)))-ROUND(96*(LOG(I18)-INT(LOG(I18))),0)<0,ROUND(96*(LOG(I18)-INT(LOG(I18))),0)-1,ROUND(96*(LOG(I18)-INT(LOG(I18))),0))+1)/96))*POWER(10,INT(LOG(I18))-2),INT(0.5+100*POWER(10,IF(96*(LOG(I18)-INT(LOG(I18)))-ROUND(96*(LOG(I18)-INT(LOG(I18))),0)<0,ROUND(96*(LOG(I18)-INT(LOG(I18))),0)-1,ROUND(96*(LOG(I18)-INT(LOG(I18))),0))/96))*POWER(10,INT(LOG(I18))-2)))","v":{"$error":"#NAME?"}},"kΩ"]
[5.6,{"$error":"#NAME?"},0,0,0]
[6.8,{"$error":"#NAME?"},0,0,0,null,null,"Ra",{"$f":"'Variable Mgmt'!D147","v":339.33080808080814},{"$f":"IF(I20=\"OPEN\",\"OPEN\",IF(I20>(INT(0.5+100*POWER(10,IF(96*(LOG(I20)-INT(LOG(I20)))-ROUND(96*(LOG(I20)-INT(LOG(I20))),0)<0,ROUND(96*(LOG(I20)-INT(LOG(I20))),0)-1,ROUND(96*(LOG(I20)-INT(LOG(I20))),0))/96))*POWER(10,INT(LOG(I20))-2)+INT(0.5+100*POWER(10,(IF(96*(LOG(I20)-INT(LOG(I20)))-ROUND(96*(LOG(I20)-INT(LOG(I20))),0)<0,ROUND(96*(LOG(I20)-INT(LOG(I20))),0)-1,ROUND(96*(LOG(I20)-INT(LOG(I20))),0))+1)/96))*POWER(10,INT(LOG(I20))-2))/2,INT(0.5+100*POWER(10,(IF(96*(LOG(I20)-INT(LOG(I20)))-ROUND(96*(LOG(I20)-INT(LOG(I20))),0)<0,ROUND(96*(LOG(I20)-INT(LOG(I20))),0)-1,ROUND(96*(LOG(I20)-INT(LOG(I20))),0))+1)/96))*POWER(10,INT(LOG(I20))-2),INT(0.5+100*POWER(10,IF(96*(LOG(I20)-INT(LOG(I20)))-ROUND(96*(LOG(I20)-INT(LOG(I20))),0)<0,ROUND(96*(LOG(I20)-INT(LOG(I20))),0)-1,ROUND(96*(LOG(I20)-INT(LOG(I20))),0))/96))*POWER(10,INT(LOG(I20))-2)))","v":340},"kΩ"]
[8.1999999999999993,{"$error":"#NAME?"},0,0,0]
[10,{"$error":"#NAME?"},0,0,0]
[12,{"$error":"#NAME?"},0,0,0]
[15,{"$error":"#NAME?"},0,0,0]
[18,{"$error":"#NAME?"},0,0,0]
[22,{"$error":"#NAME?"},0,0,0]
[27,{"$error":"#NAME?"},0,0,0]
[33,{"$error":"#NAME?"},0,0,0]
[39,{"$error":"#NAME?"},0,0,0]
[47,{"$error":"#NAME?"},0,0,0]
[56,{"$error":"#NAME?"},0,0,0]
[68,{"$error":"#NAME?"},0,0,0]
[82,{"$error":"#NAME?"},0,0,0]
[{"$f":"A22*10","v":100},{"$error":"#NAME?"},0,0,0]
[{"$f":"A23*10","v":120},{"$error":"#NAME?"},0,0,0]
[150,{"$error":"#NAME?"},0,0,0]
[180,{"$error":"#NAME?"},0,0,0]
[220,{"$error":"#NAME?"},0,0,{"$f":"IF(IF((E$3*10^12-$A39)*(E$3*10^12-$A38)*-1<0,0,1)*IF(ABS(E$3*10^12-$A39)>(E$3*10^12-$A38),$A38,$A39)=E39,0,IF((E$3*10^12-$A39)*(E$3*10^12-$A38)*-1<0,0,1)*IF(ABS(E$3*10^12-$A39)>(E$3*10^12-$A38),$A38,$A39))","v":0}]
[270,{"$error":"#NAME?"},0,0,0]
[330,{"$error":"#NAME?"},0,0,0]
[390,{"$error":"#NAME?"},0,0,0]
[470,{"$error":"#NAME?"},0,0,0]
[560,{"$error":"#NAME?"},0,0,0]
[680,{"$error":"#NAME?"},0,0,0]
[{"$f":"A33*10","v":820},{"$error":"#NAME?"},0,0,0]
[1000,{"$error":"#NAME?"},0,0,0]
[1200,{"$error":"#NAME?"},0,0,0]
[1500,{"$error":"#NAME?"},0,0,0]
[1800,{"$error":"#NAME?"},0,0,0]
[2200,{"$error":"#NAME?"},0,0,0]
[2700,{"$error":"#NAME?"},0,0,0]
[3300,{"$error":"#NAME?"},0,0,0]
[3900,{"$error":"#NAME?"},0,0,0]
[4700,{"$error":"#NAME?"},0,0,0]
[5600,{"$error":"#NAME?"},0,0,0]
[6800,{"$error":"#NAME?"},0,0,0]
[8200,{"$error":"#NAME?"},0,0,0]
[10000,{"$error":"#NAME?"},0,0,0]
[12000,{"$error":"#NAME?"},0,0,0]
[15000,{"$error":"#NAME?"},0,0,0]
[18000,{"$error":"#NAME?"},0,0,0]
[22000,{"$error":"#NAME?"},0,0,0]
[27000,{"$error":"#NAME?"},0,0,0]
[33000,{"$error":"#NAME?"},0,0,0]
[39000,{"$error":"#NAME?"},0,0,0]
[47000,{"$error":"#NAME?"},0,0,0]
[56000,{"$error":"#NAME?"},0,0,0]
[68000,{"$error":"#NAME?"},0,0,0]
[82000,{"$error":"#NAME?"},0,0,0]
[100000,{"$error":"#NAME?"},{"$f":"IF(IF((C$3*10^12-$A71)*(C$3*10^12-$A70)*-1<0,0,1)*IF(ABS(C$3*10^12-$A71)>(C$3*10^12-$A70),$A70,$A71)=C71,0,IF((C$3*10^12-$A71)*(C$3*10^12-$A70)*-1<0,0,1)*IF(ABS(C$3*10^12-$A71)>(C$3*10^12-$A70),$A70,$A71))","v":0},{"$f":"IF(IF((D$3*10^12-$A71)*(D$3*10^12-$A70)*-1<0,0,1)*IF(ABS(D$3*10^12-$A71)>(D$3*10^12-$A70),$A70,$A71)=D71,0,IF((D$3*10^12-$A71)*(D$3*10^12-$A70)*-1<0,0,1)*IF(ABS(D$3*10^12-$A71)>(D$3*10^12-$A70),$A70,$A71))","v":0},{"$f":"IF(IF((E$3*10^12-$A71)*(E$3*10^12-$A70)*-1<0,0,1)*IF(ABS(E$3*10^12-$A71)>(E$3*10^12-$A70),$A70,$A71)=E71,0,IF((E$3*10^12-$A71)*(E$3*10^12-$A70)*-1<0,0,1)*IF(ABS(E$3*10^12-$A71)>(E$3*10^12-$A70),$A70,$A71))","v":0}]
[120000,{"$f":"IF(IF((B$3*10^12-$A72)*(B$3*10^12-$A71)*-1<0,0,1)*IF(ABS(B$3*10^12-$A72)>(B$3*10^12-$A71),$A71,$A72)=B72,0,IF((B$3*10^12-$A72)*(B$3*10^12-$A71)*-1<0,0,1)*IF(ABS(B$3*10^12-$A72)>(B$3*10^12-$A71),$A71,$A72))","v":{"$error":"#NAME?"}},{"$f":"IF(IF((C$3*10^12-$A72)*(C$3*10^12-$A71)*-1<0,0,1)*IF(ABS(C$3*10^12-$A72)>(C$3*10^12-$A71),$A71,$A72)=C72,0,IF((C$3*10^12-$A72)*(C$3*10^12-$A71)*-1<0,0,1)*IF(ABS(C$3*10^12-$A72)>(C$3*10^12-$A71),$A71,$A72))","v":0},{"$f":"IF(IF((D$3*10^12-$A72)*(D$3*10^12-$A71)*-1<0,0,1)*IF(ABS(D$3*10^12-$A72)>(D$3*10^12-$A71),$A71,$A72)=D72,0,IF((D$3*10^12-$A72)*(D$3*10^12-$A71)*-1<0,0,1)*IF(ABS(D$3*10^12-$A72)>(D$3*10^12-$A71),$A71,$A72))","v":0},0]
[150000,{"$error":"#NAME?"},0,0,0]
[180000,{"$error":"#NAME?"},0,0,0]
[220000,{"$error":"#NAME?"},0,0,0]
[270000,{"$error":"#NAME?"},0,0,0]
[330000,{"$error":"#NAME?"},0,0,0]
[390000,{"$error":"#NAME?"},0,0,0]
[470000,{"$error":"#NAME?"},0,0,0]
[560000,{"$error":"#NAME?"},0,0,0]
[680000,{"$error":"#NAME?"},0,0,0]
[820000,{"$error":"#NAME?"},0,0,0]
[1000000,{"$error":"#NAME?"},0,0,0]
[1200000,{"$error":"#NAME?"},0,0,0]
[1500000,{"$error":"#NAME?"},0,0,0]
[1800000,{"$error":"#NAME?"},0,0,0]
[2200000,{"$error":"#NAME?"},0,2200000,0]
[2700000,{"$error":"#NAME?"},0,0,0]
[3300000,{"$error":"#NAME?"},0,0,0]
[3900000,{"$error":"#NAME?"},0,0,0]
[4700000,{"$error":"#NAME?"},0,0,0]
[5600000,{"$error":"#NAME?"},0,0,0]
[6800000,{"$error":"#NAME?"},0,0,0]
[8200000,{"$error":"#NAME?"},0,0,0]
[10000000,{"$error":"#NAME?"},0,0,0]
[12000000,{"$error":"#NAME?"},0,0,0]
[15000000,{"$error":"#NAME?"},0,0,0]
[18000000,{"$error":"#NAME?"},0,0,0]
[22000000,{"$error":"#NAME?"},0,0,0]
[{"$f":"A87*10","v":27000000},{"$error":"#NAME?"},0,0,0]
[33000000,{"$error":"#NAME?"},33000000,0,0]
[39000000,{"$error":"#NAME?"},0,0,0]
[47000000,{"$error":"#NAME?"},0,0,{"$f":"IF(IF((E$3*10^12-$A103)*(E$3*10^12-$A102)*-1<0,0,1)*IF(ABS(E$3*10^12-$A103)>(E$3*10^12-$A102),$A102,$A103)=E103,0,IF((E$3*10^12-$A103)*(E$3*10^12-$A102)*-1<0,0,1)*IF(ABS(E$3*10^12-$A103)>(E$3*10^12-$A102),$A102,$A103))","v":0}]
[56000000,{"$error":"#NAME?"},0,{"$f":"IF(IF((D$3*10^12-$A104)*(D$3*10^12-$A103)*-1<0,0,1)*IF(ABS(D$3*10^12-$A104)>(D$3*10^12-$A103),$A103,$A104)=D104,0,IF((D$3*10^12-$A104)*(D$3*10^12-$A103)*-1<0,0,1)*IF(ABS(D$3*10^12-$A104)>(D$3*10^12-$A103),$A103,$A104))","v":0},0]
[68000000,{"$error":"#NAME?"},0,0,0]
[82000000,{"$error":"#NAME?"},0,0,0]
[100000000,{"$error":"#NAME?"},0,0,0]
[120000000,{"$error":"#NAME?"},0,0,0]
[150000000,{"$error":"#NAME?"},0,0,0]
[180000000,{"$error":"#NAME?"},0,0,0]
[220000000,{"$error":"#NAME?"},0,0,0]
[270000000,{"$error":"#NAME?"},0,0,0]
[330000000,{"$error":"#NAME?"},0,0,0]
[390000000,{"$error":"#NAME?"},0,0,0]
[470000000,{"$error":"#NAME?"},0,0,0]
[560000000,{"$error":"#NAME?"},0,0,0]
[680000000,{"$error":"#NAME?"},0,0,0]
[820000000,{"$error":"#NAME?"},0,0,0]
[1000000000,{"$error":"#NAME?"},0,0,0]
[1200000000,{"$error":"#NAME?"},0,0,0]
[1500000000,{"$error":"#NAME?"},0,0,0]
[1800000000,{"$error":"#NAME?"},0,0,0]
[2200000000,{"$error":"#NAME?"},0,0,0]
[2700000000,{"$error":"#NAME?"},0,0,0]
[3300000000,{"$error":"#NAME?"},0,0,0]
[3900000000,{"$error":"#NAME?"},0,0,0]
[4700000000,{"$error":"#NAME?"},0,0,0]
[5600000000,{"$error":"#NAME?"},0,0,0]
[6800000000,{"$error":"#NAME?"},0,0,0]
[8200000000,{"$error":"#NAME?"},0,0,0]
[10000000000,{"$error":"#NAME?"},0,0,0]
[12000000000,{"$error":"#NAME?"},0,0,0]
[15000000000,{"$error":"#NAME?"},0,0,0]
[18000000000,{"$error":"#NAME?"},0,0,0]
[22000000000,{"$error":"#NAME?"},{"$f":"IF(IF((C$3*10^12-$A135)*(C$3*10^12-$A134)*-1<0,0,1)*IF(ABS(C$3*10^12-$A135)>(C$3*10^12-$A134),$A134,$A135)=C135,0,IF((C$3*10^12-$A135)*(C$3*10^12-$A134)*-1<0,0,1)*IF(ABS(C$3*10^12-$A135)>(C$3*10^12-$A134),$A134,$A135))","v":0},0,{"$f":"IF(IF((E$3*10^12-$A135)*(E$3*10^12-$A134)*-1<0,0,1)*IF(ABS(E$3*10^12-$A135)>(E$3*10^12-$A134),$A134,$A135)=E135,0,IF((E$3*10^12-$A135)*(E$3*10^12-$A134)*-1<0,0,1)*IF(ABS(E$3*10^12-$A135)>(E$3*10^12-$A134),$A134,$A135))","v":0}]
[27000000000,{"$f":"IF(IF((B$3*10^12-$A136)*(B$3*10^12-$A135)*-1<0,0,1)*IF(ABS(B$3*10^12-$A136)>(B$3*10^12-$A135),$A135,$A136)=B136,0,IF((B$3*10^12-$A136)*(B$3*10^12-$A135)*-1<0,0,1)*IF(ABS(B$3*10^12-$A136)>(B$3*10^12-$A135),$A135,$A136))","v":{"$error":"#NAME?"}},0,0,0]
[33000000000,{"$error":"#NAME?"},0,0,0]
[39000000000,{"$error":"#NAME?"},0,0,0]
[47000000000,{"$error":"#NAME?"},0,0,0]
[56000000000,{"$error":"#NAME?"},0,0,0]
[68000000000,{"$error":"#NAME?"},0,0,0]
[82000000000,{"$error":"#NAME?"},0,0,0]
[100000000000,{"$error":"#NAME?"},0,0,0]
[120000000000,{"$error":"#NAME?"},0,0,0]
[150000000000,{"$error":"#NAME?"},0,0,0]
[180000000000,{"$error":"#NAME?"},0,0,0]
[220000000000,{"$error":"#NAME?"},0,0,0]
[270000000000,{"$error":"#NAME?"},0,0,0]
[330000000000,{"$error":"#NAME?"},0,0,0]
[390000000000,{"$error":"#NAME?"},0,0,0]
[470000000000,{"$error":"#NAME?"},0,0,0]
[560000000000,{"$error":"#NAME?"},0,0,0]
[680000000000,{"$error":"#NAME?"},0,0,0]
[820000000000,{"$error":"#NAME?"},0,0,0]
[1000000000000,{"$error":"#NAME?"},0,0,0]
[1200000000000,{"$error":"#NAME?"},0,0,0]
[1500000000000,{"$error":"#NAME?"},0,0,0]
[1800000000000,{"$error":"#NAME?"},0,0,0]
[2200000000000,{"$error":"#NAME?"},0,0,0]
[2700000000000,{"$error":"#NAME?"},2700000000000,2700000000000,2700000000000]

{"sheet":"Efficiency","index":9,"n_rows":114,"n_cols":88,"rows_kept":114,"cut":false,"hidden":true,"merged":[[0,0,2,4],[1,6,1,7],[3,0,3,4],[3,10,3,21]]}
["LM5164 (COT) Efficiency Calculator"]
[null,null,null,null,null,null,"TERMS OF USE",null,null,{"$f":"CoutEsr","v":5.0000000000000001E-3}]
[]
[null,null,null,null,null,null,null,"Currents",null,null,"Miscellaneous",null,null,null,null,null,null,null,null,null,null,null,"Inductor",null,null,null,"Cout",null,null,"Cin",null,null,"High-side MOSFET Losses ",null,null,null,null,null,null,null,null,"Low-side MOSFET Losses ",null,null,"Diode",null,null,null,null,null,null,null,"RESULTS"]
["Input Parameters",null,null,null,null,null,null,"Step","Iout (A)","Ripple Current pk-pk (A)","Peak Current (A)","Valley Current (A)","VOUT Hysteresis +Undershoot (2us Delay) (mV)","Vout Rise per Pulse (mV)","Number of Pulses in DCM","VOUT Ripple (mV)","Off Time (sec)","Duty Cycle","Switching Frequency (Hz)","Active Mode Duration (sec)","Sleep Mode Duration (sec)","Operating Quiescent Current (A)","Irms (A)","Inductor DCR Loss @ 25°C (W)","Inductor Core Loss  (W)","Total Inductor Loss (W)","Irms (A)","Cout ESR Loss (W)","Total Cout Loss (W)","Irms (A)","Cin ESR Loss (W)","Total Cin Loss (W)","Irms (A)","Rdson HS Loss @ 25°C (W)","HS Gate Qg Loss (W)     ","SW Rise Time (ns)","SW Fall Time (ns)","HS Switching  Loss (W)","Coss Loss (W)","Total HS FET AC Loss (W)","Total HS FET Loss (W)","Irms (A)","Rdson LS Loss @ 25°C (W)","LS Gate Qg Loss (W)","Reverse Recovery & Leakage Losses","DeadTime Loss @ 25°C (W)","Total LS FET AC Loss (W)","Total LS FET Loss (W)","Quiescent Loss (W)","LDO + Quiescent Loss (W)","Total Gate Drive Loss (W)","Total Power Loss in IC (W)","Total Converter Power Loss (W)","Pout (W)","EFF (%)","High-side MOSFET Rdson %","Low-side MOSFET Rdson %","Gate Drive (Qg) Loss from Vin %","High-side MOSFET AC Loss %","Reverse Recovery & Leakage Loss %","Deadtime Loss %","Low-side MOSFET AC Loss %","Inductor Cu Loss %","Inductor Core Loss %","Cin ESR %","Cout ESR %","LDO + Quiescent Current Loss %","Total Loss %","Overall Eff %","Overall Eff","Current (mA)","Keep for \"previous\" data series","Keep for \"previous\" data series","Frequency (kHz)",null,"Coss",null,"Total Power Loss in IC (mW)","LDO + Quiescent Loss (mW)","Total Inductor Loss (mW)",null,null,"Overall Eff","Total Power Loss in IC (W)","LDO + Quiescent Loss (mW)","Total Inductor Loss (mW)","Fsw (kHz)","Ripple (mV)"]
["Design","Input Value","Units","Std Units","Description",null,null,0.04,{"$f":"IF(PLOT_TYPE=1, H6/100*Iout, min_I*EXP(H6*rr/100))","v":4.0000000000000003E-5},{"$f":"IF(I6<Icrit, (Vin-(Rdcr+RdsonTop)*Iripple/2-Vout)/L*OnTime, (Vin-(Rdcr+RdsonTop)*I6-Vout)/L*OnTime)","v":4.0337601521892447E-2},{"$f":"IF(I6<Icrit, (Vin-(Rdcr+RdsonTop)*Iripple/2-Vout)/L*OnTime, I6+((Vin-(Rdcr+RdsonTop)*J6-Vout)/L*OnTime)/2)","v":4.0337601521892447E-2},{"$f":"IF(I6<Icrit, 0, I6-((Vin-(Rdcr+RdsonTop)*K6-Vout)/L*OnTime)/2)","v":0},{"$f":"1000*((((J6/2)-I6)*0.000002/Cout+Vout/306))","v":17.55979659989098},{"$f":"IF(I6<Icrit, 1000*SQRT((J6*CoutEsr)^2+(((J6/2)-I6)*(OnTime+OffTime)/Cout)^2), 1000*J6*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":2.0245779524335625},{"$f":"ROUNDUP(M6/N6,0)","v":9},{"$f":"IF(I6<Icrit, 1000*((N6/1000)*O6), 1000*J6*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":18.221201571902064},{"$f":"IF(I6<Icrit, L*J6/(Vout+J6/2*(RdsonBot+Rdcr)), L*J6/(Vout+I6*(RdsonBot+Rdcr)))","v":2.9798859710179457E-6},{"$f":"OnTime*S6","v":2.0697624517144954E-4},{"$f":"IF(I6<Icrit,I6/((OnTime+Q6)*J6/2),1/(OnTime+Q6))","v":596.09158609377482},{"$f":"IF(1/S6-OnTime-Q6>Tsleep, OnTime+Q6+Tsleep, 1/S6)","v":8.3271081932401676E-6},{"$f":"IF(1/S6-OnTime-Q6>Tsleep, 1/S6-OnTime-Q6-Tsleep, 0)","v":1.6692674482960772E-3},{"$f":"S6*(T6*Iq_active+U6*Iq_sleep)","v":1.3226417434813949E-5},{"$f":"IF(I6<Icrit,Iripple*SQRT((OnTime+OffTime)*S6/3), SQRT(I6^2+Iripple^2/12))","v":1.0317789897272495E-3},{"$f":"W6^2*Rdcr","v":1.2774814603711001E-7},{"$f":"Core_Loss/1000*S6/$S$106","v":1.9686920073852754E-4},{"$f":"(Y6+X6*(1+Ltc*(Ta-25)))/(1-X6*Ltc*ThetaCa)","v":1.9699695291112393E-4},{"$f":"Iripple/SQRT(12)*SQRT((OnTime+Q6)*S6)","v":5.1779488153911148E-4},{"$f":"RCoutEsr*AA6^2","v":1.3405576967405124E-9},{"$f":"AB6","v":1.3405576967405124E-9},{"$f":"SQRT($R6)*SQRT($I6^2*(1-R6)+(Iripple^2)/12)","v":1.6727483754877098E-4},{"$f":"RCinEsr*AD6^2","v":8.3942613830903157E-11},{"$f":"AE6","v":8.3942613830903157E-11},{"$f":"IF(I6<Icrit,Iripple*SQRT((OnTime)*S6/3), SQRT(OnTime*S6*(I6^2+Iripple^2/12)))","v":3.3454769575364353E-4},{"$f":"RdsonTop*AG6^2","v":7.6890524424307765E-8},{"$f":"QgTop*S6*Vdd","v":2.3933077181665062E-6},{"$f":"20*VIN_nom/24","v":40},{"$f":"IF(I6<Icrit, Csw*Vin/Iripple*1000000000, Csw*Vin/(I6+Iripple/2)*1000000000)","v":190.67897193104272},{"$f":"IF(I6<Icrit, Vin*(I6+Iripple/2)*AK6/1000000000/2*S6, Vin*(I6-Iripple/2)*AJ6/1000000000/2*S6 + Vin*(I6+Iripple/2)*AK6/1000000000/2*S6)","v":5.5044916219982862E-5},{"$f":"IF(I6<Icrit, Csw*(Vin)^2*S6/2, Csw*Vin^2*S6/2)","v":1.0987160114880457E-4},{"$f":"AI6+AL6+AM6","v":1.6730982508695393E-4},{"$f":"(AI6+AL6+AM6+AH6*(1+RdsonTopTc*(Ta-25)))/(1-AH6*RdsonTopTc*ThetaJA)","v":1.6738671799176842E-4},{"$f":"IF(I6<Icrit,Iripple*SQRT((OffTime)*S6/3), SQRT(OffTime*S6*(I6^2+Iripple^2/12)))","v":9.7603571804955535E-4},{"$f":"RdsonBot*AP6^2","v":2.8960429976418733E-7},{"$f":"QgBot*S6*Vdd","v":6.5570074470315237E-6},{"$f":"IF(I6<Icrit, Vin*Idss*R6, QrrBot*(I6-Iripple/2)/1*S6*Vin+Vin*Idss*R6)","v":0},{"$f":"IF(I6<Icrit, dead1*S6*(I6+Iripple/2)*((I6+Iripple/2)*BDserR+VSD), dead1*S6*(I6+Iripple/2)*((I6+Iripple/2)*BDserR+VSD)+dead2*S6*(I6-Iripple/2)*((I6-Iripple/2)*BDserR+VSD))","v":1.9293774787085806E-7},{"$f":"AR6+AS6+AT6","v":6.7499451949023821E-6},{"$f":"(AR6+AS6+AT6+AQ6*(1+RdsonBotTc*(Ta-25)))/(1-AQ6*RdsonBotTc*ThetaJA)","v":7.039549871721159E-6},{"$f":"Vin*V6+Vout*Ifb/0.8","v":6.8730092277710989E-4},{"$f":"(Vin-Vdd)*(S6*QgBot+S6*QgTop)+AW6","v":7.6427363319781297E-4},{"$f":"AI6+AR6","v":8.9503151651980307E-6},{"$f":"AO6+AV6+AX6+AY6","v":9.4765021622650054E-4},{"$f":"SUM(Z6,AC6,AF6,AZ6)","v":1.1446485936379351E-3},{"$f":"Vout*I6","v":2.0000000000000001E-4},{"$f":"BB6/(BB6+BA6)","v":0.14873774527135133},{"$f":"(AO6-AN6)/($BB6+$BA6)","v":5.7184386447359139E-5},{"$f":"(AV6-AU6)/($BB6+$BA6)","v":2.1537573325031636E-4},{"$f":"Vin*S6*(QgBot+QgTop)/($BB6+$BA6)","v":6.3899985462697803E-2},{"$f":"AN6/($BB6+$BA6)","v":0.12442643072588849},{"$f":"AS6/(BA6+BB6)","v":0},{"$f":"AT6/($BB6+$BA6)","v":1.4348562798021947E-4},{"$f":"AU6/($BB6+$BA6)","v":5.0198581449748614E-3},{"$f":"X6/($BB6+$BA6)","v":9.5004856020775288E-5},{"$f":"Y6/($BB6+$BA6)","v":0.1464094051561082},{"$f":"(AF6)/($BB6+$BA6)","v":6.242717556696143E-8},{"$f":"(AC6)/($BB6+$BA6)","v":9.969576460966988E-7},{"$f":"AX6/($BB6+$BA6)","v":0.56838168486093255},{"$f":"SUM(BD6:BO6)","v":0.90864947433912224},{"$f":"BC6","v":0.14873774527135133},{"$f":"100*BQ6","v":14.873774527135133},{"$f":"I6*1000","v":0.04},8.7924221262065743,{"$f":"BT6/100","v":8.7924221262065741E-2},{"$f":"S6/1000","v":0.59609158609377477},null,{"$f":"AM6/($BB6+$BA6)","v":8.1710271121132022E-2},null,{"$f":"AZ6","v":9.4765021622650054E-4},{"$f":"AX6","v":7.6427363319781297E-4},{"$f":"Z6","v":1.9699695291112393E-4},null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR6, IF(MODE_ILIM=4,#REF!,#REF!))","v":14.873774527135133},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ6, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.4765021622650054E-4},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA6, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.6427363319781297E-4},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB6, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.9699695291112393E-4},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S6, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":0.59609158609377477},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P6, IF(MODE_ILIM=4,#REF!,#REF!))","v":18.221201571902064}]
[null,null,null,null,null,null,null,1,1E-3,4.0337601521892447E-2,4.0337601521892447E-2,0,{"$f":"IF(I7<Icrit, 1000*((((J7/2)-I7)*0.000002/Cout+Vout/306)), 1000*J7*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":17.501614781709161},1.929002042806546,{"$f":"ROUNDUP(M7/N7,0)","v":10},19.290020428065461,2.9798859710179457E-6,{"$f":"OnTime*S7","v":5.1744061292862374E-3},14902.289652344369,{"$f":"IF(1/S7-OnTime-Q7>Tsleep, OnTime+Q7+Tsleep, 1/S7)","v":8.3271081932401676E-6},{"$f":"IF(1/S7-OnTime-Q7>Tsleep, 1/S7-OnTime-Q7-Tsleep, 0)","v":5.8776674066332544E-5},9.0660435870348728E-5,{"$f":"IF(I7<Icrit,Iripple*SQRT((OnTime+OffTime)*S7/3), SQRT(I7^2+Iripple^2/12))","v":5.1588949486362475E-3},3.1937036509277509E-6,4.9217300184631876E-3,4.9249262387149008E-3,{"$f":"Iripple/SQRT(12)*SQRT((OnTime+Q7)*S7)","v":2.5889744076955574E-3},{"$f":"RCoutEsr*AA7^2","v":3.3513942418512811E-8},{"$f":"AB7","v":3.3513942418512811E-8},{"$f":"SQRT($R7)*SQRT($I7^2*(1-R7)+(Iripple^2)/12)","v":8.3944096649999635E-4},{"$f":"RCinEsr*AD7^2","v":2.1139834087153441E-9},{"$f":"AE7","v":2.1139834087153441E-9},{"$f":"IF(I7<Icrit,Iripple*SQRT((OnTime)*S7/3), SQRT(OnTime*S7*(I7^2+Iripple^2/12)))","v":1.6727384787682178E-3},{"$f":"RdsonTop*AG7^2","v":1.9222631106076945E-6},{"$f":"QgTop*S7*Vdd","v":5.9832692954162644E-5},40,190.67897193104272,1.4415922928479202E-3,2.7467900287201142E-3,{"$f":"AI7+AL7+AM7","v":4.2482150145221973E-3},4.2501387886530375E-3,4.8801785902477766E-3,{"$f":"RdsonBot*AP7^2","v":7.2401074941046838E-6},1.639251861757881E-4,0,5.0535250476608728E-6,{"$f":"AR7+AS7+AT7","v":1.6897871122344897E-4},1.7621905468506762E-4,4.4041338076827793E-3,6.3284515682003554E-3,2.2375787912995074E-4,{"$f":"AO7+AV7+AX7+AY7","v":1.0978567290668411E-2},1.5903529157309138E-2,5.0000000000000001E-3,{"$f":"BB7/(BB7+BA7)","v":0.23919405964287602},{"$f":"(AO7-AN7)/($BB7+$BA7)","v":9.2031068838322033E-5},{"$f":"(AV7-AU7)/($BB7+$BA7)","v":3.463694291586637E-4},0.10276138653345192,{"$f":"AN7/($BB7+$BA7)","v":0.20322955911187679},{"$f":"AS7/(BA7+BB7)","v":0},{"$f":"AT7/($BB7+$BA7)","v":2.4175463433139254E-4},{"$f":"AU7/($BB7+$BA7)","v":8.0837407861515959E-3},1.5278298831233666E-4,0.2354497167164834,{"$f":"(AF7)/($BB7+$BA7)","v":1.0113045470966167E-7},{"$f":"(AC7)/($BB7+$BA7)","v":1.6032671883443332E-6},{"$f":"AX7/($BB7+$BA7)","v":0.30274560437023362},{"$f":"SUM(BD7:BO7)","v":0.85310465003648117},0.23919405964287602,{"$f":"100*BQ7","v":23.919405964287602},1,9.5725635821403898,{"$f":"BT7/100","v":9.5725635821403893E-2},14.902289652344368,null,0.13140317159122722,null,{"$f":"AZ7","v":1.0978567290668411E-2},{"$f":"AX7","v":6.3284515682003554E-3},{"$f":"Z7","v":4.9249262387149008E-3},null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR7, IF(MODE_ILIM=4,#REF!,#REF!))","v":23.919405964287602},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ7, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0978567290668411E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA7, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.3284515682003554E-3},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB7, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.9249262387149008E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S7, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":14.902289652344368},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P7, IF(MODE_ILIM=4,#REF!,#REF!))","v":19.290020428065461}]
["Vin",{"$f":"Vin","v":48},"V",{"$f":"B8","v":48},"Vin",null,null,2,2E-3,4.0337601521892447E-2,4.0337601521892447E-2,0,17.441008721103099,1.8294996889257871,10,18.29499688925787,2.9798859710179457E-6,{"$f":"OnTime*S8","v":1.0348812258572475E-2},29804.579304688737,8.3271081932401676E-6,2.522478293654619E-5,1.7132087174069746E-4,7.2957792032194322E-3,6.3874073018555E-6,9.8434600369263752E-3,9.8498575106365158E-3,3.6613627199999074E-3,6.7027884837025596E-8,{"$f":"AB8","v":6.7027884837025596E-8},1.1999974443929213E-3,4.3199815996486268E-9,{"$f":"AE8","v":4.3199815996486268E-9},2.365609442977353E-3,3.844526221215389E-6,1.1966538590832529E-4,40,190.67897193104272,3.0195791426715674E-3,5.4935800574402284E-3,8.6328245860201221E-3,8.6366752533071703E-3,6.9016147491312166E-3,1.4480214988209366E-5,3.2785037235157619E-4,0,1.0586503076958914E-5,3.3843687542853512E-4,3.5291803557209824E-4,8.2758347294595198E-3,1.2124470250494672E-2,4.4751575825990148E-4,{"$f":"AO8+AV8+AX8+AY8","v":2.1561579297633842E-2},3.1411508156136796E-2,0.01,{"$f":"BB8/(BB8+BA8)","v":0.24147876871077187},9.2985439519125256E-5,3.4968927209711272E-4,0.10374293211193769,0.20846438515282179,0,2.5564157279768361E-4,8.1725319964803533E-3,1.5424232505062595E-4,0.23769866095706699,1.043183837536341E-7,1.6185811099732356E-6,0.2927802147359837,0.85171300646324866,0.24147876871077187,{"$f":"100*BQ8","v":24.147876871077187},2,10.507357436577642,0.10507357436577643,29.804579304688737,null,0.13265829480847177,null,2.1561579297633842E-2,1.2124470250494672E-2,9.8498575106365158E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR8, IF(MODE_ILIM=4,#REF!,#REF!))","v":24.147876871077187},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ8, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.1561579297633842E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA8, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.2124470250494672E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB8, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.8498575106365158E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S8, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":29.804579304688737},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P8, IF(MODE_ILIM=4,#REF!,#REF!))","v":18.29499688925787}]
["Vout",{"$f":"Vout","v":5},"V",{"$f":"B9","v":5},"Vout",null,null,3,3.0000000000000001E-3,4.0337601521892447E-2,4.0337601521892447E-2,0,17.38040266049704,1.7300640689530626,11,19.030704758483687,2.9798859710179457E-6,1.5523218387858712E-2,44706.868957033104,8.3271081932401676E-6,1.4040819226617402E-5,2.519813076110462E-4,8.9354681619484132E-3,9.5811109527832501E-6,1.476519005538956E-2,1.477479381577256E-2,4.4842352136242455E-3,1.0054182725553843E-7,1.0054182725553843E-7,1.4953530507784884E-3,6.7082422394175979E-9,6.7082422394175979E-9,2.8972680330020266E-3,5.7667893318230822E-6,1.7949807886248793E-4,40,190.67897193104272,4.7339605494709416E-3,8.2403700861603413E-3,1.3153828714493771E-2,1.3159609539439902E-2,8.4527172683190061E-3,2.1720322482314051E-5,4.9177555852736418E-4,0,1.6599112915369954E-5,5.0837467144273412E-4,5.3009712341724072E-4,1.2147535651236259E-2,1.7920488932788987E-2,6.7127363738985206E-4,3.228146923303598E-2,4.7056370298878034E-2,1.4999999999999999E-2,{"$f":"BB9/(BB9+BA9)","v":0.24171571633591332},9.315441619110275E-5,3.5004386930602253E-4,0.10384472839622545,0.21196580868558451,0,2.6748443125862393E-4,8.1921431916543372E-3,1.5439367314972456E-4,0.23793189940495943,1.0809917188371041E-7,1.620169319786275E-6,0.28877758796525982,0.85157897230208079,0.24171571633591332,24.171571633591331,3,11.516667783884284,0.11516667783884284,44.706868957033102,null,0.13278846388328525,null,3.228146923303598E-2,1.7920488932788987E-2,1.477479381577256E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR9, IF(MODE_ILIM=4,#REF!,#REF!))","v":24.171571633591331},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ9, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.228146923303598E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA9, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7920488932788987E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB9, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.477479381577256E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S9, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":44.706868957033102},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P9, IF(MODE_ILIM=4,#REF!,#REF!))","v":19.030704758483687}]
["Iout",{"$f":"Iout","v":0.1},"A",{"$f":"B10","v":0.1},"Iout(max)",null,null,4,4.0000000000000001E-3,4.0337601521892447E-2,4.0337601521892447E-2,0,17.319796599890978,1.6307073906315788,11,17.937781296947367,2.9798859710179457E-6,2.069762451714495E-2,59609.158609377475,8.3271081932401676E-6,8.4488373716530061E-6,3.3264174348139489E-4,1.0317789897272495E-2,1.2774814603711003E-5,1.968692007385275E-2,1.9699735154130753E-2,5.1779488153911148E-3,1.3405576967405125E-7,1.3405576967405125E-7,1.7670205839366122E-3,9.3670852321670567E-9,9.3670852321670567E-9,3.3454769575364356E-3,7.6890524424307779E-6,2.3933077181665058E-4,40,190.67897193104272,6.5847365132460428E-3,1.0987160114880457E-2,1.781122739994315E-2,1.7818941792528957E-2,9.7603571804955533E-3,2.8960429976418735E-5,6.5570074470315239E-4,0,2.3091533390369816E-5,6.7879227809352217E-4,7.0775649897761208E-4,1.6019236573012997E-2,2.3716507615083302E-2,8.9503151651980297E-4,4.3138237423109675E-2,6.283811600009534E-2,0.02,0.24143475208896567,9.3126123073558034E-5,3.4964847443001452E-4,0.10372402190532941,0.21501246358527334,0,2.7875493197290047E-4,8.1942022690706887E-3,1.5421420984147323E-4,0.23765533337129602,1.1307699504122324E-7,1.6182860758675022E-6,0.28629945682318519,0.85176295305654337,0.24143475208896567,24.143475208896568,4,12.603144523181673,0.12603144523181672,59.609158609377474,null,0.13263411392489674,null,4.3138237423109675E-2,2.3716507615083302E-2,1.9699735154130753E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR10, IF(MODE_ILIM=4,#REF!,#REF!))","v":24.143475208896568},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ10, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.3138237423109675E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA10, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.3716507615083302E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB10, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.9699735154130753E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S10, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":59.609158609377474},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P10, IF(MODE_ILIM=4,#REF!,#REF!))","v":17.937781296947367}]
["Rt",{"$f":"Vout*2500/(Fsw/1000)","v":41.666666666666664},"kW",{"$f":"B11*1000","v":41666.666666666664},"RT pin resistance to get Fsw",null,null,5,5.000000000000001E-3,4.0337601521892447E-2,4.0337601521892447E-2,0,17.259190539284916,1.5314450187041093,12,18.377340224449313,2.9798859710179457E-6,2.5872030646431194E-2,74511.44826172186,8.3271081932401676E-6,5.0936482586743705E-6,4.1330217935174368E-4,1.1535639793930935E-2,1.5968518254638752E-5,2.4608650092315942E-2,2.4624681525718815E-2,5.7891227676145213E-3,1.6756971209256408E-7,1.6756971209256408E-7,2.0316580026806426E-3,1.2382902719568894E-8,1.2382902719568894E-8,3.7403569471053237E-3,9.6113155530384737E-6,2.9916346477081327E-4,40,190.67897193104272,8.5719070339968714E-3,1.3733950143600572E-2,2.2605020642368259E-2,2.2614672158052254E-2,1.091241107013312E-2,3.6200537470523415E-5,8.1962593087894059E-4,0,3.0063943329434342E-5,8.496898742083749E-4,8.8589634301129781E-4,1.9890937494789738E-2,2.951252629737762E-2,1.1187893956497539E-3,5.4131884194090922E-2,7.875674567242455E-2,2.5000000000000005E-2,0.24094818932475692,9.3020609131922691E-5,3.489553239963029E-4,0.10351498718113812,0.21786555173709538,0,2.8975410836757227E-4,8.1892494671235352E-3,1.5390342238618136E-4,0.2371763872588015,1.1934551955458931E-7,1.6150247485749651E-6,0.28443959095009635,0.85207313442840493,0.24094818932475692,24.094818932475693,5.0000000000000009,13.76888730592373,0.1376888730592373,74.511448261721867,null,0.13236681677508169,null,5.4131884194090922E-2,2.951252629737762E-2,2.4624681525718815E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR11, IF(MODE_ILIM=4,#REF!,#REF!))","v":24.094818932475693},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ11, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.4131884194090922E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA11, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.951252629737762E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB11, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.4624681525718815E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S11, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":74.511448261721867},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P11, IF(MODE_ILIM=4,#REF!,#REF!))","v":18.377340224449313}]
["Tamb",{"$f":"'Design Converter'!E56","v":25},"°C",{"$f":"B12","v":25},"Ambient temperature",null,null,6,6.0000000000000001E-3,4.0337601521892447E-2,4.0337601521892447E-2,0,17.198584478678857,1.4322965604378022,13,18.619855285691425,2.9798859710179457E-6,3.1046436775717424E-2,89413.737914066209,8.3271081932401676E-6,2.8568555166886163E-6,4.9396261522209237E-4,1.2636660260780438E-2,1.9162221905566504E-5,2.953038011077912E-2,2.9549632930544439E-2,6.3416662559784209E-3,2.010836545110768E-7,2.010836545110768E-7,2.2978365970931598E-3,1.5840159080822017E-8,1.5840159080822017E-8,4.0973557461014857E-3,1.1533578663646164E-5,3.5899615772497586E-4,40,190.67897193104272,1.0695472111723423E-2,1.6480740172320683E-2,2.7535208441769082E-2,2.7546800781487912E-2,1.1953947399761997E-2,4.3440644964628089E-5,9.8355111705472837E-4,0,3.751652156003933E-5,1.0210676386147677E-3,1.0645168362773505E-3,2.3762638416566475E-2,3.5308544979671931E-2,1.3425472747797041E-3,6.5262409872216889E-2,9.4812259726574921E-2,0.03,0.24036100352417883,9.2878213600378122E-5,3.4811642508329353E-4,0.10326272327830441,0.22061301111036857,0,3.0058362569691815E-4,8.1808280761169715E-3,1.5352836289916558E-4,0.23659839326257737,1.2691188442163381E-7,1.6110889663530564E-6,0.28289324347641842,0.85244504383191622,0.24036100352417883,24.036100352417883,6,15.015319606822954,0.15015319606822955,89.413737914066203,null,0.13204424155467492,null,6.5262409872216889E-2,3.5308544979671931E-2,2.9549632930544439E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR12, IF(MODE_ILIM=4,#REF!,#REF!))","v":24.036100352417883},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ12, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.5262409872216889E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA12, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.5308544979671931E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB12, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.9549632930544439E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S12, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":89.413737914066203},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P12, IF(MODE_ILIM=4,#REF!,#REF!))","v":18.619855285691425}]
["VDD",5,"V",{"$f":"B13","v":5},"Gate drive rail",null,null,7,7.000000000000001E-3,4.0337601521892447E-2,4.0337601521892447E-2,0,17.137978418072798,1.3332874292685124,13,17.332736580490664,2.9798859710179457E-6,3.6220842905003665E-2,104316.02756641059,8.3271081932401676E-6,1.2591464152702178E-6,5.7462305109244117E-4,1.3649153073998846E-2,2.2355925556494259E-5,3.4452110129242312E-2,3.4474589368615367E-2,6.8497824334731927E-3,2.3459759692958966E-7,2.3459759692958966E-7,2.5704338759991768E-3,1.9821390932652455E-8,1.9821390932652455E-8,4.4256500232692005E-3,1.345584177425386E-5,4.1882885067913851E-4,40,190.67897193104272,1.2955431746425704E-2,1.9227530201040798E-2,3.2601790798145638E-2,3.2615327808314283E-2,1.2911738903377401E-2,5.0680752458732796E-5,1.1474763032305166E-3,0,4.5449446909660644E-5,1.1929257501401773E-3,1.2436181595357927E-3,2.7634339338343215E-2,4.1104563661966249E-2,1.566305153909655E-3,7.6529814783725975E-2,0.11100465857132921,3.5000000000000003E-2,0.23971837845777422,9.271628933696858E-5,3.4719720515527362E-4,0.10298664182819024,0.22329281214145874,0,3.1128764899961559E-4,8.1704636126893482E-3,1.5311789209501475E-4,0.23596582784658926,1.3575861980437357E-7,1.606781586458621E-6,0.28152912423602566,0.8528509312407464,0.23971837845777422,23.971837845777422,7.0000000000000009,16.343061169118954,0.16343061169118955,104.31602756641058,null,0.13169121032975376,null,7.6529814783725975E-2,4.1104563661966249E-2,3.4474589368615367E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR13, IF(MODE_ILIM=4,#REF!,#REF!))","v":23.971837845777422},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ13, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.6529814783725975E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA13, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.1104563661966249E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB13, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.4474589368615367E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S13, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":104.31602756641058},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P13, IF(MODE_ILIM=4,#REF!,#REF!))","v":17.332736580490664}]
["K1",400,"pC",4,"RT constant",null,null,8,8.0000000000000002E-3,4.0337601521892447E-2,4.0337601521892447E-2,0,17.077372357466736,1.2344511498330217,14,17.282316097662303,2.9798859710179457E-6,4.1395249034289899E-2,119218.31721875495,8.3271081932401676E-6,6.086458920642013E-8,6.5528348696278986E-4,1.4591558406438864E-2,2.5549629207422E-5,3.9373840147705501E-2,3.9399550839939304E-2,7.3227254399998148E-3,2.6811153934810238E-7,2.6811153934810238E-7,2.8523211091619886E-3,2.4407207129313229E-8,2.4407207129313229E-8,4.731218885954706E-3,1.5378104884861556E-5,4.7866154363330115E-4,40,190.67897193104272,1.5351785938103711E-2,2.1974320229760914E-2,3.7804767711497926E-2,3.7820253384009905E-2,1.3803229498262433E-2,5.7920859952837463E-5,1.3114014894063048E-3,0,5.3862898205774088E-5,1.3652643876120789E-3,1.4232004935476137E-3,3.1506040260119952E-2,4.6900582344260561E-2,1.7900630330396059E-3,8.7934099254857678E-2,0.12733394261354347,0.04,0.23904295431787984,9.2543522671567537E-5,3.4623044811259754E-4,0.10269646939992286,0.22592408402644143,0,3.2188865788078668E-4,8.1589208159945584E-3,1.5268647118671364E-4,0.23530097679368672,1.4585927247098633E-7,1.6022543613121219E-6,0.28028134407002597,0.85327689231955683,0.23904295431787984,23.904295431787983,8,17.75180413241851,0.17751804132418511,119.21831721875495,null,0.13132016067123004,null,8.7934099254857678E-2,4.6900582344260561E-2,3.9399550839939304E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR14, IF(MODE_ILIM=4,#REF!,#REF!))","v":23.904295431787983},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ14, IF(MODE_ILIM=4,#REF!,#REF!))","v":8.7934099254857678E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA14, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.6900582344260561E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB14, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.9399550839939304E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S14, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":119.21831721875495},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P14, IF(MODE_ILIM=4,#REF!,#REF!))","v":17.282316097662303}]
["Outputs",null,null,null,null,null,null,9,8.9999999999999993E-3,4.0337601521892447E-2,4.0337601521892447E-2,0,17.016766296860673,1.1358328459231366,15,17.037492688847049,2.9798859710179457E-6,4.6569655163576133E-2,134120.6068710993,7.4559758066191912E-6,0,6.6E-4,1.547668484590874E-2,2.8743332858349749E-5,4.4295570166168682E-2,4.4324517344523966E-2,7.7669232230866718E-3,3.0162548176661527E-7,3.0162548176661527E-7,3.1451703060716494E-3,2.96762887625845E-8,2.96762887625845E-8,5.0182154363046525E-3,1.7300367995469245E-5,5.3849423658746363E-4,40,190.67897193104272,1.7884534686757443E-2,2.4721110258481022E-2,4.3144139181825927E-2,4.3161577654053526E-2,1.4640535770743328E-2,6.5160967446942144E-5,1.4753266755820926E-3,0,6.2757054275855493E-5,1.5380837298579479E-3,1.6032640190747711E-3,3.1732432885906041E-2,4.9051292730564224E-2,2.0138209121695564E-3,9.5829955315862081E-2,0.14015480396215657,4.4999999999999998E-2,0.24303987278233119,9.418320159364098E-5,3.5203131553716144E-4,0.10441360603735192,0.2330165799567592,0,3.3894369971995052E-4,8.3070149785166476E-3,1.5523946580518939E-4,0.2392353275112547,1.6027825434467247E-7,1.6290448603659452E-6,0.264920443223227,0.85083515871287996,0.24303987278233119,24.303987278233119,9,19.240199150848532,0.19240199150848533,134.12060687109931,null,0.13351589982798245,null,9.5829955315862081E-2,4.9051292730564224E-2,4.4324517344523966E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR15, IF(MODE_ILIM=4,#REF!,#REF!))","v":24.303987278233119},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ15, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.5829955315862081E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA15, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.9051292730564224E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB15, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.4324517344523966E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S15, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":134.12060687109931},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P15, IF(MODE_ILIM=4,#REF!,#REF!))","v":17.037492688847049}]
["Design","Value","Units","Std Units","Description",null,null,10,1.0000000000000002E-2,4.0337601521892447E-2,4.0337601521892447E-2,0,16.956160236254615,1.0374946779173302,17,17.637409524594613,2.9798859710179457E-6,5.1744061292862388E-2,149022.89652344372,6.7103782259572695E-6,0,6.6E-4,1.6313858247227905E-2,3.193703650927751E-5,4.9217300184631885E-2,4.9249488882377082E-2,8.1870559322033236E-3,3.3513942418512821E-7,3.3513942418512821E-7,3.4498980256317461E-3,3.5705389161773462E-8,3.5705389161773462E-8,5.289663522712775E-3,1.9222631106076954E-5,5.9832692954162655E-4,40,190.67897193104272,2.0553677992386915E-2,2.7467900287201145E-2,4.8619905209129691E-2,4.8639300763924136E-2,1.5432479733572559E-2,7.2401074941046844E-5,1.6392518617578812E-3,0,7.2132093947380711E-5,1.7113839557052618E-3,1.7838089168801927E-3,3.1732432885906041E-2,5.0975610491081805E-2,2.2375787912995077E-3,0.10363629896318564,0.15288615869037608,5.000000000000001E-2,0.24644362297925332,9.5598215864712731E-5,3.5697339652163428E-4,0.10587590861364271,0.23964131177291581,0,3.5552989130944741E-4,8.4351932470514129E-3,1.5741357969134068E-4,0.24258579541516306,1.7598730929823232E-7,1.6518594779872754E-6,0.25125228266002864,0.84875783463897603,0.24644362297925332,24.644362297925333,10.000000000000002,20.80575856495858,0.20805758564958579,149.02289652344373,null,0.13538577724821443,null,0.10363629896318564,5.0975610491081805E-2,4.9249488882377082E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR16, IF(MODE_ILIM=4,#REF!,#REF!))","v":24.644362297925333},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ16, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10363629896318564},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA16, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.0975610491081805E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB16, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.9249488882377082E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S16, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":149.02289652344373},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P16, IF(MODE_ILIM=4,#REF!,#REF!))","v":17.637409524594613}]
["On-Time",{"$f":"(Rt*k_RT/10000)/Vin","v":0.34722222222222215},"µs",{"$f":"B17/1000000","v":3.4722222222222213E-7},"On Time - fixed",null,null,11,1.1000000000000001E-2,4.0337601521892447E-2,4.0337601521892447E-2,0,16.895554175648556,0.93952461373338669,18,16.911443047200962,2.9798859710179457E-6,5.6918467422148615E-2,163925.18617578805,6.1003438417793372E-6,0,6.6E-4,1.7110118877486223E-2,3.5130740160205245E-5,5.4139030203095066E-2,5.4174465453506335E-2,8.5866567021587736E-3,3.6865336660364093E-7,3.6865336660364093E-7,3.7669321688306831E-3,4.2569333893714309E-8,4.2569333893714309E-8,5.5478459064640506E-3,2.1144894216684636E-5,6.5815962249578903E-4,40,190.67897193104272,2.3359215854992097E-2,3.0214690315921253E-2,5.423206579340914E-2,5.4253422859100828E-2,1.6185721293777443E-2,7.9641182435151531E-5,1.8031770479336687E-3,0,8.1988196047825531E-5,1.8851652439814944E-3,1.9648353677277708E-3,3.1732432885906041E-2,5.2899928251599379E-2,2.4613366704294578E-3,0.11157952314885743,0.16575439982506426,5.5000000000000007E-2,0.24914565709034331,9.6745821186857998E-5,3.608993696588184E-4,0.10703674334394851,0.2456669757721027,0,3.7140005414522501E-4,8.5396496988299399E-3,1.5913947893244449E-4,0.24524553189425566,1.9283572117904859E-7,1.6699706411096605E-6,0.23963249789594074,0.84711144613536316,0.24914565709034331,24.914565709034331,11.000000000000002,22.444784059665849,0.22444784059665848,163.92518617578804,null,0.13687016131893512,null,0.11157952314885743,5.2899928251599379E-2,5.4174465453506335E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR17, IF(MODE_ILIM=4,#REF!,#REF!))","v":24.914565709034331},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ17, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.11157952314885743},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA17, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.2899928251599379E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB17, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.4174465453506335E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S17, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":163.92518617578804},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P17, IF(MODE_ILIM=4,#REF!,#REF!))","v":16.911443047200962}]
["Off Time",{"$f":"L*Iripple*1000000/(Vout+(Rdcr+RdsonBot)*Iout)","v":2.9554447727713429},"µs",{"$f":"B18/1000000","v":2.9554447727713428E-6},"Off Time - depends on Vout, L, Iout, DCR, etc.",null,null,12,1.2E-2,4.0337601521892447E-2,4.0337601521892447E-2,0,16.834948115042494,0.84205114642170353,20,16.841022928434072,2.9798859710179457E-6,6.2092873551434849E-2,178827.47582813242,5.5919818549643924E-6,0,6.5999999999999989E-4,1.7870936323896826E-2,3.8324443811133E-5,5.9060760221558241E-2,5.909944705791946E-2,8.968470427248491E-3,4.0216730902215371E-7,4.0216730902215371E-7,4.0963813609399364E-3,5.0341020762768376E-8,5.0341020762768376E-8,5.7945360660040532E-3,2.3067157327292329E-5,7.1799231544995173E-4,40,190.67897193104272,2.630114827457301E-2,3.2961480344641365E-2,5.998062093466433E-2,6.0003944085063016E-2,1.6905434536638012E-2,8.6881289929256205E-5,1.9671022341094567E-3,0,9.2325539404665812E-5,2.0594277735141225E-3,2.1463435523823697E-3,3.1732432885906034E-2,5.4824246012116953E-2,2.6850945495594082E-3,0.11965962819912175,0.17875952776537099,0.06,0.25129887197197848,9.7684689767040111E-5,3.6403061976927388E-4,0.10796179703078193,0.25121770635099971,0,3.8668839844328276E-4,8.6255312731977028E-3,1.6051482497818657E-4,0.24736504035808471,2.1084402886002733E-7,1.6844031850212217E-6,0.22962118632598716,0.8458020751192229,0.25129887197197848,25.129887197197849,12,24.152326085424395,0.24152326085424394,178.82747582813241,null,0.13805304715224859,null,0.11965962819912175,5.4824246012116953E-2,5.909944705791946E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR18, IF(MODE_ILIM=4,#REF!,#REF!))","v":25.129887197197849},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ18, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.11965962819912175},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA18, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.4824246012116953E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB18, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.909944705791946E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S18, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":178.82747582813241},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P18, IF(MODE_ILIM=4,#REF!,#REF!))","v":16.841022928434072}]
["DIL",{"$f":"(Vin-Vout-(Rdcr+RdsonTop)*Iout)/L*OnTime*1000","v":40.27712087087086},"mA",{"$f":"B19/1000","v":4.0277120870870861E-2},"Inductor pk-pk ripple current in CCM",null,null,13,1.3000000000000001E-2,4.0337601521892447E-2,4.0337601521892447E-2,0,16.774342054436431,0.74526915060566656,23,17.141190463930329,2.9798859710179457E-6,6.7267279680721104E-2,193729.76548047681,5.1618294045825154E-6,0,6.6E-4,1.8600660262040151E-2,4.1518147462060749E-5,6.3982490240021436E-2,6.4024433695624203E-2,9.3346799778103434E-3,4.3568125144066659E-7,4.3568125144066659E-7,4.4381460022109853E-3,5.9091419810824056E-8,5.9091419810824056E-8,6.0311443556404411E-3,2.4989420437900031E-5,7.7782500840411443E-4,40,190.67897193104272,2.9379475251129657E-2,3.5708270373361488E-2,6.5865570632895262E-2,6.5890864587290293E-2,1.7595734140559923E-2,9.4121397423360879E-5,2.1310274202852452E-3,0,1.0314430284537738E-4,2.2341717231306227E-3,2.3283336516098196E-3,3.1732432885906041E-2,5.6748563772634535E-2,2.9088524286893596E-3,0.127876614440224,0.19190154290851946,6.5000000000000002E-2,0.25301521845334329,9.8457775335502259E-5,3.6652924467926295E-4,0.10869916544394485,0.25638448834209399,0,4.0149351256370703E-4,8.6966068706181062E-3,1.6161112538294495E-4,0.24905451915796814,2.3001582295621333E-7,1.6959074924505576E-6,0.22089615784379402,0.84476095523969585,0.25301521845334329,25.301521845334328,13.000000000000002,25.922181532084487,0.25922181532084487,193.7297654804768,null,0.13899593583241698,null,0.127876614440224,5.6748563772634535E-2,6.4024433695624203E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR19, IF(MODE_ILIM=4,#REF!,#REF!))","v":25.301521845334328},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ19, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.127876614440224},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA19, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.6748563772634535E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB19, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.4024433695624203E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S19, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":193.7297654804768},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P19, IF(MODE_ILIM=4,#REF!,#REF!))","v":17.141190463930329}]
["CCM Freq",{"$f":"'Design Converter'!E12","v":300},"kHz",{"$f":"B20*1000","v":300000},"Frequency in CCM",{"$f":"10000*Vout/(k_RT*Rt/1000+Vin*0.75)","v":246.71052631578948},null,14,1.4000000000000002E-2,4.0337601521892447E-2,4.0337601521892447E-2,0,16.713735993830372,0.64948781418440016,26,16.886683168794406,2.9798859710179457E-6,7.2441685810007331E-2,208632.05513282117,4.7931273042551931E-6,0,6.6E-4,1.9302817392155586E-2,4.4711851112988497E-5,6.8904220258484625E-2,6.8949425366628223E-2,9.6870552167227699E-3,4.6919519385917916E-7,4.6919519385917916E-7,4.7919923941681713E-3,6.8889573317296811E-8,6.8889573317296811E-8,6.2588142852241079E-3,2.6911683548507724E-5,8.3765770135827702E-4,40,190.67897193104272,3.2594196784662022E-2,3.8455060402081596E-2,7.1886914888101894E-2,7.1914184511262427E-2,1.8259956270976634E-2,1.0136150491746559E-4,2.2949526064610331E-3,0,1.1444466519743605E-4,2.4093972716584693E-3,2.5108058461769198E-3,3.1732432885906041E-2,5.8672881533152116E-2,3.1326103078193101E-3,0.13623048219841077,0.2051804456498062,7.0000000000000007E-2,0.25437853999655846,9.9097241797612088E-5,3.6851664470193761E-4,0.10928486900314226,0.26123554934417453,0,4.1588952633312461E-4,8.7556994319453237E-3,1.6248193438093584E-4,0.25039649927078006,2.5034327259199759E-7,1.7050455483900028E-6,0.21321602773991813,0.84393658552599482,0.25437853999655846,25.437853999655847,14.000000000000002,27.746934669307642,0.27746934669307644,208.63205513282116,null,0.13974488743658547,null,0.13623048219841077,5.8672881533152116E-2,6.8949425366628223E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR20, IF(MODE_ILIM=4,#REF!,#REF!))","v":25.437853999655847},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ20, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.13623048219841077},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA20, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.8672881533152116E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB20, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.8949425366628223E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S20, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":208.63205513282116},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P20, IF(MODE_ILIM=4,#REF!,#REF!))","v":16.886683168794406}]
["Icrit_Skip",{"$f":"1000*Iripple/2","v":20.13856043543543},"mA",{"$f":"Iripple/2","v":2.0138560435435431E-2},"CCM-DCM (critical conduction) boundary",null,null,15,1.4999999999999999E-2,4.0337601521892447E-2,4.0337601521892447E-2,0,16.653129933224314,0.55522524706529652,30,16.656757411958896,2.9798859710179457E-6,7.7616091939293558E-2,223534.34478516551,4.4735854839715144E-6,0,6.6E-4,1.9980314220901751E-2,4.7905554763916252E-5,7.3825950276947799E-2,7.3874422070939263E-2,1.0027054764762103E-2,5.0270913627769199E-7,5.0270913627769199E-7,5.1576026665861282E-3,7.9802595799129015E-8,7.9802595799129015E-8,6.4784882708296358E-3,2.8833946659115416E-5,8.974903943124395E-4,40,190.67897193104272,3.594531287517011E-2,4.1201850430801705E-2,7.8044653700284253E-2,7.8073904002459379E-2,1.8900850406547626E-2,1.0860161241157023E-4,2.4588777926368207E-3,0,1.2622680528831759E-4,2.5851045979251382E-3,2.6937603168514369E-3,3.1732432885906041E-2,6.0597199293669676E-2,3.3563681869492601E-3,0.14472123179992977,0.21859623638260112,7.4999999999999997E-2,0.25545286589526794,9.9627646919182733E-5,3.7008553060844963E-4,0.10974641566155433,0.26582307274055123,0,4.2993332218272924E-4,8.8049650423868125E-3,1.6316815008993486E-4,0.25145400767583825,2.7181069070358904E-7,1.7122465276516165E-6,0.20639637633059502,0.84328963615794428,0.25545286589526794,25.545286589526796,15,29.618044224570543,0.29618044224570544,223.5343447851655,null,0.1403350769698197,null,0.14472123179992977,6.0597199293669676E-2,7.3874422070939263E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR21, IF(MODE_ILIM=4,#REF!,#REF!))","v":25.545286589526796},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ21, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.14472123179992977},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA21, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.0597199293669676E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB21, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.3874422070939263E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S21, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":223.5343447851655},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P21, IF(MODE_ILIM=4,#REF!,#REF!))","v":16.656757411958896}]
["Tr",null,"ns",{"$f":"B22/1000000000","v":0},"Switch rise time",null,null,16,1.6E-2,4.0337601521892447E-2,4.0337601521892447E-2,0,16.592523872618251,0.46340918145690629,36,16.682730532448627,2.9798859710179457E-6,8.2790498068579799E-2,238436.6344375099,4.1939863912232943E-6,0,6.6E-4,2.063557979454499E-2,5.1099258414844014E-5,7.8747680295411002E-2,7.8799423808565069E-2,1.035589763078223E-2,5.3622307869620498E-7,5.3622307869620498E-7,5.5346085080094079E-3,9.1895674010790379E-8,9.1895674010790379E-8,6.6909539150728711E-3,3.0756209769723112E-5,9.5732308726660231E-4,40,190.67897193104272,3.9432823522653933E-2,4.3948640459521827E-2,8.4338787069442367E-2,8.4370023206361403E-2,1.9520714360991107E-2,1.1584171990567494E-4,2.6228029788126096E-3,0,1.3849090194549798E-4,2.7612938807581077E-3,2.877197244402109E-3,3.1732432885906041E-2,6.2521517054187264E-2,3.5801260660792119E-3,0.15334886357103,0.23214891549834776,0.08,0.25628793190672944,1.0006806164668841E-4,3.713079171169338E-4,0.11010517265289793,0.27018766646936748,0,4.4366933559386666E-4,8.8460787260775317E-3,1.6370154076384894E-4,0.25227600156703994,2.9439690304250563E-7,1.7178437984963727E-6,0.20029387881861213,0.84278955732981797,0.25628793190672944,25.628793190672944,16,31.525976771075946,0.31525976771075948,238.43663443750989,null,0.1407938271685408,null,0.15334886357103,6.2521517054187264E-2,7.8799423808565069E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR22, IF(MODE_ILIM=4,#REF!,#REF!))","v":25.628793190672944},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ22, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15334886357103},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA22, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.2521517054187264E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB22, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.8799423808565069E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S22, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":238.43663443750989},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P22, IF(MODE_ILIM=4,#REF!,#REF!))","v":16.682730532448627}]
["Tf",null,"ns",{"$f":"B23/1000000000","v":0},"Switch fall time",null,null,17,1.7000000000000001E-2,4.0337601521892447E-2,4.0337601521892447E-2,0,16.531917812012189,0.37583693833037679,44,16.536825286536576,2.9798859710179457E-6,8.7964904197866053E-2,253338.92408985429,3.9472813093866292E-6,0,6.5999999999999989E-4,2.1270668784692644E-2,5.4292962065771762E-5,8.366941031387419E-2,8.3724430579513315E-2,1.0674614944949702E-2,5.6973702111471776E-7,5.6973702111471776E-7,5.9226139202291838E-3,1.052320669442775E-7,1.052320669442775E-7,6.8968774319963667E-3,3.2678472880330808E-5,1.017155780220765E-3,40,190.67897193104272,4.305672872711349E-2,4.6695430488241943E-2,9.0769314995576195E-2,9.0802542268448874E-2,2.0121491799469472E-2,1.2308182739977961E-4,2.7867281649883975E-3,0,1.5123713399645293E-4,2.9379652989848506E-3,3.0611168095986373E-3,3.1732432885906034E-2,6.4445834814704839E-2,3.8038839452091628E-3,0.16211337783796151,0.24583848338656289,8.5000000000000006E-2,0.25692295264418535,1.0043351829132797E-4,3.722405850527741E-4,0.11037798716825795,0.27436141668415959,0,4.5713283548015279E-4,8.8803614044864077E-3,1.6410715437337447E-4,0.25290108169221659,3.1807686296675708E-7,1.7221002081823041E-6,0.19479546077898119,0.84241226199837049,0.25692295264418535,25.692295264418537,17,33.460383546927204,0.33460383546927203,253.33892408985429,null,0.14114268089447568,null,0.16211337783796151,6.4445834814704839E-2,8.3724430579513315E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR23, IF(MODE_ILIM=4,#REF!,#REF!))","v":25.692295264418537},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ23, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.16211337783796151},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA23, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.4445834814704839E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB23, IF(MODE_ILIM=4,#REF!,#REF!))","v":8.3724430579513315E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S23, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":253.33892408985429},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P23, IF(MODE_ILIM=4,#REF!,#REF!))","v":16.536825286536576}]
[null,null,null,null,null,null,null,18,1.7999999999999999E-2,4.0337601521892447E-2,4.0337601521892447E-2,0,16.47131175140613,0.29629559437105102,56,16.592553284778859,2.9798859710179457E-6,9.3139310327152267E-2,268241.2137421986,3.7279879033095956E-6,0,6.6E-4,2.1887337609658296E-2,5.7486665716699497E-5,8.8591140332337365E-2,8.8649442383791716E-2,1.0984088159999723E-2,6.0325096353323054E-7,6.0325096353323054E-7,6.3212104808365605E-3,1.1987310582911395E-7,1.1987310582911395E-7,7.0968283289320581E-3,3.460073599093849E-5,1.0769884731749273E-3,40,190.67897193104272,4.6817028488548747E-2,4.9442220516962045E-2,9.7336237478685722E-2,9.7371461334202394E-2,2.0704844247393651E-2,1.3032193489388429E-4,2.9506533511641851E-3,0,1.6446568026865825E-4,3.1151190314328433E-3,3.2455191932116946E-3,3.1732432885906041E-2,6.6370152575222413E-2,4.0276418243391128E-3,0.17101477492697564,0.25966494043483673,0.09,0.25738925923793698,1.0073602309933778E-4,3.7292890049739645E-4,0.11057831953518692,0.2783700229071871,0,4.7035221793792601E-4,8.9088686659833261E-3,1.6440500338755769E-4,0.25336008872427151,3.4282277679896076E-7,1.7252257626487773E-6,0.18981071563161506,0.84213850565770576,0.25738925923793698,25.738925923793698,18,35.410314704487,0.35410314704487,268.24121374219862,null,0.14139885015488435,null,0.17101477492697564,6.6370152575222413E-2,8.8649442383791716E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR24, IF(MODE_ILIM=4,#REF!,#REF!))","v":25.738925923793698},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ24, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.17101477492697564},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA24, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.6370152575222413E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB24, IF(MODE_ILIM=4,#REF!,#REF!))","v":8.8649442383791716E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S24, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":268.24121374219862},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P24, IF(MODE_ILIM=4,#REF!,#REF!))","v":16.592553284778859}]
["Components","Input Value","Units","Std Units","Description",null,null,19,1.9000000000000003E-2,4.0337601521892447E-2,4.0337601521892447E-2,0,16.410705690800068,0.23315465800405599,71,16.553980718287974,2.9798859710179457E-6,9.8313716456438521E-2,283143.50339454302,3.5317780136617212E-6,0,6.6E-4,2.2487101741447857E-2,6.0680369367627272E-5,9.3512870350800567E-2,9.3574459221408016E-2,1.1285077810558005E-2,6.3676490595174332E-7,6.3676490595174332E-7,6.7299874723100494E-3,1.3587819413235063E-7,1.3587819413235063E-7,7.2912979879226174E-3,3.6522999101546192E-5,1.1368211661290902E-3,40,190.67897193104272,5.0713722806959773E-2,5.2189010545682167E-2,0.10403955451877103,0.10407678054910284,2.1272205301320846E-2,1.3756204238798899E-4,3.1145785373399735E-3,0,1.7817671958958995E-4,3.2927552569295636E-3,3.4304045760129229E-3,3.1732432885906041E-2,6.8294470335739987E-2,4.2513997034690637E-3,0.18005305516432479,0.27362828702883291,9.5000000000000015E-2,0.25771218146525315,1.0098527878001972E-4,3.734095399808337E-4,0.11071705180918663,0.28223432161795381,0,4.8335064307111498E-4,8.9324541083631356E-3,1.6461126696682679E-4,0.25367795592823372,3.6860490340428666E-7,1.7273902420351632E-6,0.18526649402355336,0.84195273021123485,0.25771218146525315,25.771218146525314,19.000000000000004,37.364462120689176,0.37364462120689174,283.14350339454302,null,0.14157625006569316,null,0.18005305516432479,6.8294470335739987E-2,9.3574459221408016E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR25, IF(MODE_ILIM=4,#REF!,#REF!))","v":25.771218146525314},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ25, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.18005305516432479},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA25, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.8294470335739987E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB25, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.3574459221408016E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S25, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":283.14350339454302},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P25, IF(MODE_ILIM=4,#REF!,#REF!))","v":16.553980718287974}]
["L",{"$f":"'Design Converter'!E17","v":370},"µH",{"$f":"B26/1000000","v":3.6999999999999999E-4},"Filter inductance",null,null,20,2.0000000000000004E-2,4.0337601521892447E-2,4.0337601521892447E-2,0,16.350099630194009,0.20239429371756895,81,16.393937791123083,2.9798859710179457E-6,0.10348812258572478,298045.79304688744,3.3551891129786347E-6,0,6.6E-4,2.307127958786187E-2,6.3874073018555007E-5,9.8434600369263769E-2,9.8499481092369931E-2,1.1578245535229043E-2,6.7027884837025631E-7,6.7027884837025631E-7,7.1485384883570278E-3,1.5330480755856534E-7,1.5330480755856534E-7,7.4807138942106473E-3,3.8445262212153895E-5,1.1966538590832531E-3,40,190.67897193104272,5.4746811682346512E-2,5.493580057440229E-2,0.11087926611583206,0.11091850005863117,2.182482214026624E-2,1.4480214988209366E-4,3.2785037235157624E-3,0,1.9237043078672368E-4,3.4708741543024862E-3,3.61577313877493E-3,3.1732432885906041E-2,7.0218788096257576E-2,4.4751575825990155E-3,0.18922821887626268,0.28772852355228851,0.10000000000000002,0.25791241532560127,1.0118920950066535E-4,3.7371247063514756E-4,0.11080307530471592,0.28597139333464339,0,4.9614722441430306E-4,8.9518153642735784E-3,1.6473916448899337E-4,0.25387505532847138,3.9539213198456076E-7,1.7287323672483524E-6,0.18110297239142367,0.84184222391706642,0.25791241532560127,25.791241532560129,20.000000000000004,39.311419610679415,0.39311419610679416,298.04579304688747,null,0.14168625013989647,null,0.18922821887626268,7.0218788096257576E-2,9.8499481092369931E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR26, IF(MODE_ILIM=4,#REF!,#REF!))","v":25.791241532560129},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ26, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.18922821887626268},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA26, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0218788096257576E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB26, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.8499481092369931E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S26, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":298.04579304688747},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P26, IF(MODE_ILIM=4,#REF!,#REF!))","v":16.393937791123083}]
["Rdcr",{"$f":"'Design Converter'!E18","v":120},"mW",{"$f":"B27/1000","v":0.12},"Inductor DCR at 25°C",null,null,21,2.1000000000000001E-2,4.033694913663663E-2,4.1161152440900309E-2,8.3915965184864008E-4,0.54778484042090125,0.54778484042090125,1,0.54778484042090125,2.9796281143650491E-6,0.10436965510700053,300584.60670816159,3.3268503365872714E-6,0,6.6E-4,2.4003899797128005E-2,6.914246465646742E-5,9.9273085977816658E-2,9.9343327457274339E-2,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,7.4385909907706289E-3,1.6599790778392191E-7,1.6599790778392191E-7,7.7547701392129591E-3,4.1313747959563909E-5,1.2068471959332688E-3,40,186.68616302345612,5.5652332762257131E-2,5.5403754708448341E-2,0.11226293466663874,0.11230510653541127,2.2624375349784599E-2,1.5560615743025408E-4,3.3064306737897783E-3,3.7286708071318777E-5,2.030107092699779E-4,3.5467280911310748E-3,3.7024408024336798E-3,3.1732432885906041E-2,7.0546622565524242E-2,4.5132778697230466E-3,0.19106744777309226,0.29041161716430175,0.10500000000000001,0.26554606754603854,1.066530848915609E-4,3.9379903003179391E-4,0.10957560594720157,0.2839141031609882,9.4298463810246066E-5,5.1341614777499758E-4,8.9697114024278549E-3,1.7486199609491313E-4,0.25106264375779996,4.1981039650371811E-7,1.7094490854879043E-6,0.17841312572313892,0.83322034797364219,0.26554606754603854,26.554606754603853,21,41.239947953148963,0.41239947953148964,300.58460670816157,null,0.14011665895346451,null,0.19106744777309226,7.0546622565524242E-2,9.9343327457274339E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR27, IF(MODE_ILIM=4,#REF!,#REF!))","v":26.554606754603853},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ27, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.19106744777309226},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA27, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0546622565524242E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB27, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.9343327457274339E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S27, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":300.58460670816157},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P27, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54778484042090125}]
["Kcore",0,null,{"$f":"B28","v":0},"Core loss constant - consult inductor vendor",null,null,22,2.2000000000000002E-2,4.0336191816816809E-2,4.2161152727666962E-2,1.8395383118671345E-3,0.54777455584743873,0.54777455584743873,1,0.54777455584743873,2.9793199750988993E-6,0.10437932292031096,300612.45001049567,3.3265421973211215E-6,0,6.6E-4,2.4883472536415849E-2,7.4302464656467418E-5,9.9282281693381699E-2,9.9357765362334038E-2,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,7.7043585346307881E-3,1.780714212904148E-7,1.780714212904148E-7,8.0392997996054805E-3,4.4401044451072527E-5,1.2069589867921401E-3,40,182.25587017305139,5.5946075817662776E-2,5.5408886785934558E-2,0.11256192159038947,0.11260724736253476,2.3454484523790425E-2,1.6723430466012427E-4,3.3067369501154531E-3,8.0578354759232583E-5,2.1270081799516823E-4,3.6000161228698538E-3,3.7673669521319669E-3,3.1732432885906041E-2,7.0550217943311344E-2,4.513695936907593E-3,0.19143852819488566,0.29079714756466835,0.11000000000000001,0.27445305104685552,1.1308905869390626E-4,4.1754496078371208E-4,0.10811324695698188,0.28084511647435734,2.0104523010915722E-4,5.3069444053578023E-4,8.982140079450026E-3,1.8538671022971481E-4,0.24771204659674523,4.4429313524913024E-7,1.6864791365406289E-6,0.17602475060511283,0.82312719188527139,0.27445305104685552,27.445305104685552,22.000000000000004,43.139231734149426,0.43139231734149425,300.61245001049565,null,0.13824670939554123,null,0.19143852819488566,7.0550217943311344E-2,9.9357765362334038E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR28, IF(MODE_ILIM=4,#REF!,#REF!))","v":27.445305104685552},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ28, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.19143852819488566},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA28, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0550217943311344E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB28, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.9357765362334038E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S28, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":300.61245001049565},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P28, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54777455584743873}]
["Cin",{"$f":"'Design Converter'!E37","v":2.2000000000000002},"µF",{"$f":"B29/1000000","v":2.2000000000000001E-6},"Input capacitance",null,null,23,2.3000000000000003E-2,4.0335434496996989E-2,4.3161153014433615E-2,2.8399169718856358E-3,0.54776427127397631,0.54776427127397631,1,0.54776427127397631,2.9790118879914387E-6,0.1043889908879319,300640.29375724396,3.326234110213661E-6,0,6.6E-4,2.5771829688063706E-2,7.9702464656467413E-5,9.9291477555721958E-2,9.9372447257012886E-2,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,7.9730349710325273E-3,1.9070785994792297E-7,1.9070785994792297E-7,8.3266939501669829E-3,4.7632342680006489E-5,1.2070707794353344E-3,40,178.03097559304263,5.623987241534413E-2,5.5414018945335208E-2,0.11286096214011468,0.11290958917131227,2.429295078635019E-2,1.7940482720404182E-4,3.3070432313296837E-3,1.2387802050133827E-4,2.2239512372090054E-4,3.6533163755519227E-3,3.8328483802021391E-3,3.1732432885906041E-2,7.0553813378485208E-2,4.5141140107650178E-3,0.19181036494076464,0.29118367884166485,0.11500000000000002,0.28312314351958084,1.1971685158859123E-4,4.4199709146905462E-4,0.10668940373706363,0.27785695984133624,3.0498030067236493E-4,5.4752353505467348E-4,8.9942471001549732E-3,1.9622271599823774E-4,0.24444969782852091,4.6951138088998186E-7,1.6641141989762141E-6,0.17369928200878773,0.81330216463622629,0.28312314351958084,28.312314351958083,23.000000000000004,44.999115697666738,0.44999115697666736,300.64029375724397,null,0.1364260107726688,null,0.19181036494076464,7.0553813378485208E-2,9.9372447257012886E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR29, IF(MODE_ILIM=4,#REF!,#REF!))","v":28.312314351958083},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ29, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.19181036494076464},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA29, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0553813378485208E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB29, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.9372447257012886E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S29, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":300.64029375724397},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P29, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54776427127397631}]
["RCinESR",{"$f":"'Design Converter'!E39","v":3},"mW",{"$f":"B30/1000","v":3.0000000000000001E-3},"Input capacitor ESR",null,null,24,2.4E-2,4.0334677177177168E-2,4.4161153301200268E-2,3.8402956319041302E-3,0.5477539867005139,0.5477539867005139,1,0.5477539867005139,2.9787038530294245E-6,0.10439865900986707,300668.13794841722,3.3259260752516467E-6,0,6.6E-4,2.6668093397739588E-2,8.534246465646742E-5,9.9300673564840986E-2,9.9387373143638227E-2,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,8.2443386923597307E-3,2.0390736142301928E-7,2.0390736142301928E-7,8.6166693423910291E-3,5.1007682512041703E-5,1.2071825738628951E-3,40,173.99751881881318,5.6533722556583121E-2,5.5419151186652263E-2,0.11316005631709827,0.11321213202824598,2.513894776602903E-2,1.9211787521407331E-4,3.3073495174325896E-3,1.6718570548962861E-4,2.3209362715833698E-4,3.7066288500805554E-3,3.8988852612694895E-3,3.1732432885906041E-2,7.0557408871047222E-2,4.514532091295485E-3,0.19218295825185816,0.29157121123888519,0.12,0.29156558263340071,1.2652904218192002E-4,4.671279378609018E-4,0.10530257436126025,0.27494648125769328,4.0621331357549754E-4,5.6392094689933171E-4,9.0060450023292434E-3,2.0735771192444445E-4,0.24127215619851664,4.954364053045169E-7,1.6423306803169001E-6,0.17143426688824967,0.80373481042757688,0.29156558263340071,29.15655826334007,24,46.810309970062292,0.46810309970062292,300.66813794841721,null,0.13465264253987322,null,0.19218295825185816,7.0557408871047222E-2,9.9387373143638227E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR30, IF(MODE_ILIM=4,#REF!,#REF!))","v":29.15655826334007},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ30, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.19218295825185816},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA30, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0557408871047222E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB30, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.9387373143638227E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S30, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":300.66813794841721},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P30, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.5477539867005139}]
["Cout",{"$f":"'Design Converter'!E24","v":33},"µF",{"$f":"B31/1000000","v":3.3000000000000003E-5},"Output capacitance",null,null,25,2.5000000000000001E-2,4.0333919857357348E-2,4.5161153587966921E-2,4.8406742919226246E-3,0.54774370212705137,0.54774370212705137,1,0.54774370212705137,2.9783958701996205E-6,0.1044083272861201,300695.98258402594,3.3256180924218427E-6,0,6.6E-4,2.7571492623188934E-2,9.1222464656467425E-5,9.9309869720742225E-2,9.9402543024593545E-2,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,8.5180213543588259E-3,2.1767006337993891E-7,2.1767006337993891E-7,8.9089771886278531E-3,5.4527103814126629E-5,1.2072943700748642E-3,40,170.14277650668976,5.6827626242661682E-2,5.5424283509887665E-2,0.11345920412262421,0.11351487599988067,2.59917496302014E-2,2.0537359884707868E-4,3.3076558084242859E-3,2.1050140991610283E-4,2.4179632901866197E-4,3.7599535473590508E-3,3.9654777703074613E-3,3.1732432885906041E-2,7.0561004420998732E-2,4.5149501784991497E-3,0.19255630836968601,0.29195974500037031,0.125,0.29978913192180934,1.3351859004136172E-4,4.9291142709286711E-4,0.10395133399161434,0.27211069049968706,5.0484827957652341E-4,5.7990329262707892E-4,9.0175456802327799E-3,2.1878002792904242E-4,0.23817615707879433,5.2204095476829684E-7,1.6211061989981996E-6,0.16922737810321728,0.79441521011796645,0.29978913192180934,29.978913192180933,25,48.564555994658186,0.48564555994658187,300.69598258402596,null,0.13292478272653979,null,0.19255630836968601,7.0561004420998732E-2,9.9402543024593545E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR31, IF(MODE_ILIM=4,#REF!,#REF!))","v":29.978913192180933},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ31, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.19255630836968601},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA31, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0561004420998732E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB31, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.9402543024593545E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S31, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":300.69598258402596},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P31, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54774370212705137}]
["RCoutESR",{"$f":"'Design Converter'!E26","v":5.0000000000000001E-3},"mW",{"$f":"B32","v":5.0000000000000001E-3},"Output capacitor ESR",null,null,26,2.6000000000000002E-2,4.0333162537537527E-2,4.6161153874733574E-2,5.8410529519411225E-3,0.54773341755358884,0.54773341755358884,1,0.54773341755358884,2.9780879394887921E-6,0.10441799571669473,300723.82766408089,3.3253101617110143E-6,0,6.6E-4,2.8481348378729576E-2,9.7342464656467414E-5,9.931906602342927E-2,9.9417956902318694E-2,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,8.7938634566114525E-3,2.3199610348057895E-7,2.3199610348057895E-7,9.2033984020177401E-3,5.8190646454482471E-5,1.2074061680712848E-3,40,166.45512836810553,5.7121583474861834E-2,5.5429415915043391E-2,0.11375840555797651,0.11381782115280369,2.6850717197658903E-2,2.1917214826471128E-4,3.30796210430489E-3,2.5382513397276604E-4,2.5150323001308283E-4,3.8132904682907391E-3,4.0326260826379955E-3,3.1732432885906041E-2,7.056460002834114E-2,4.5153682723761751E-3,0.192930415536159,0.29234928037060853,0.13,0.30780211081672948,1.4067881156336754E-4,5.1932280825668967E-4,0.10263432999524498,0.26934674887608262,6.0098393857812725E-4,5.9548634673271025E-4,9.0287604253631096E-3,2.3047858533356582E-4,0.23515860127967422,5.4929915655829698E-7,1.6004195076636091E-6,0.16707640644355118,0.78533394722904482,0.30780211081672948,30.780211081672949,26.000000000000004,50.254747979561841,0.50254747979561842,300.72382766408089,null,0.13124070169222135,null,0.192930415536159,7.056460002834114E-2,9.9417956902318694E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR32, IF(MODE_ILIM=4,#REF!,#REF!))","v":30.780211081672949},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ32, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.192930415536159},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA32, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.056460002834114E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB32, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.9417956902318694E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S32, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":300.72382766408089},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P32, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54773341755358884}]
["Controller",null,"Units","Std Units","Description",null,null,27,2.7000000000000003E-2,4.0332405217717707E-2,4.7161154161500241E-2,6.8414316119596238E-3,0.54772313298012643,0.54772313298012643,1,0.54772313298012643,2.9777800608837114E-6,0.10442766430159463,300751.6731885926,3.3250022831059336E-6,0,6.6E-4,2.9397061170643602E-2,1.0370246465646741E-4,9.932826247290559E-2,9.943361477930962E-2,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,9.0716705441445198E-3,2.4688561938449801E-7,2.4688561938449801E-7,9.4997395430934314E-3,6.199835030260314E-5,1.2075179678521992E-3,40,162.92394016824323,5.7415594254465588E-2,5.5434548402121385E-2,0.11405766062443917,0.11412096755364499,2.7715286112909868E-2,2.335136736334182E-4,3.3082684050745187E-3,2.9715687785162931E-4,2.6121433085282957E-4,3.8666396137789776E-3,4.1003303739318491E-3,3.1732432885906041E-2,7.0568195693075819E-2,4.5157863729267181E-3,0.19330527999357938,0.29273981759453571,0.13500000000000001,0.31561242242818172,1.4800335765288177E-4,5.4633856971060004E-4,0.10135027742773861,0.26665195974941247,6.947140893329483E-4,6.1068509432161532E-4,9.0396999641596445E-3,2.4244285986667094E-4,0.23221654470115546,5.7718643256758129E-7,1.5802504222170497E-6,0.16497925325242696,0.77648207650263257,0.31561242242818172,31.561242242818171,27.000000000000004,51.875007795911799,0.51875007795911798,300.75167318859258,null,0.12959875635115423,null,0.19330527999357938,7.0568195693075819E-2,9.943361477930962E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR33, IF(MODE_ILIM=4,#REF!,#REF!))","v":31.561242242818171},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ33, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.19330527999357938},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA33, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0568195693075819E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB33, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.943361477930962E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S33, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":300.75167318859258},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P33, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54772313298012643}]
["Deadtime1",20,"ns",{"$f":"B34/1000000000","v":2E-8},"PMOS off to NMOS on deadtime",null,null,28,2.8000000000000004E-2,4.0331647897897886E-2,4.8161154448266894E-2,7.8418102719781217E-3,0.54771284840666401,0.54771284840666401,1,0.54771284840666401,2.9774722343711522E-6,0.10443733304082355,300779.51915757189,3.3246944565933744E-6,0,6.5999999999999989E-4,3.0318100294552789E-2,1.1030246465646743E-4,9.9337459069174738E-2,9.9449516658118617E-2,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,9.3512699449311131E-3,2.6233874874891584E-7,2.6233874874891584E-7,9.797829366987006E-3,6.5950255229255391E-5,1.2076297694176511E-3,40,159.53946130775134,5.7709658582755063E-2,5.5439680971123652E-2,0.11435696932329636,0.11442431526907731,2.8584956772729559E-2,2.4839832512444049E-4,3.3085747107332911E-3,3.4049664174471035E-4,2.7092963224915493E-4,3.9200009847271565E-3,4.1685908202089535E-3,3.1732432885906034E-2,7.0571791415204144E-2,4.5162044801509427E-3,0.19368090198464136,0.29313135691753611,0.14000000000000001,0.3232275792644923,1.5548619305753009E-4,5.7393636251814033E-4,0.10009795485138129,0.26402375975994918,7.8612789470594135E-4,6.255137798779533E-4,9.0503744929127487E-3,2.5466284741297986E-4,0.22934718875153523,6.0567941932419939E-7,1.5605797561350433E-6,0.16293392359639366,0.76785109478892011,0.3232275792644923,32.322757926449228,28.000000000000004,53.420714247122767,0.53420714247122769,300.77951915757188,null,0.12799738482494311,null,0.19368090198464136,7.0571791415204144E-2,9.9449516658118617E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR34, IF(MODE_ILIM=4,#REF!,#REF!))","v":32.322757926449228},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ34, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.19368090198464136},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA34, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0571791415204144E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB34, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.9449516658118617E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S34, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":300.77951915757188},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P34, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54771284840666401}]
["Deadtime2",20,"ns",{"$f":"B35/1000000000","v":2E-8},"NMOS off to PMOS on deadtime",null,null,29,2.8999999999999998E-2,4.0330890578078066E-2,4.916115473503354E-2,8.8421889319966092E-3,0.54770256383320148,0.54770256383320148,1,0.54770256383320148,2.9771644599378975E-6,0.10444700193438511,300807.36557102919,3.3243866821601198E-6,0,6.6E-4,3.1243994710512955E-2,1.1714246465646737E-4,9.9346655812240184E-2,9.9465662541354055E-2,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,9.6325079674456655E-3,2.783556292287127E-7,2.783556292287127E-7,1.0097515879566902E-2,7.0046401106478652E-5,1.2077415727676823E-3,40,156.29273491011145,5.8003776461012312E-2,5.54448136220521E-2,0.1146563316558321,0.11472786436581589,2.9459285737503192E-2,2.6382625291381315E-4,3.3088810212813218E-3,3.8384442584403207E-4,2.8064913491333414E-4,3.9733745820386881E-3,4.237407597838725E-3,3.1732432885906041E-2,7.0575387194727474E-2,4.5166225940490041E-3,0.19405728175243109,0.2935238985854417,0.14499999999999999,0.33065472706899296,1.631215772151486E-4,6.0209492949354719E-4,9.8876200459625085E-2,0.26145971069235246,8.7531016458215684E-4,6.399859524615E-4,9.0607937101163903E-3,2.6712903227016122E-4,0.22654787146767907,6.3475589386715732E-7,1.541389259589258E-6,0.16093851993559391,0.75943291406654279,0.33065472706899296,33.065472706899293,28.999999999999996,54.888490199331855,0.54888490199331852,300.80736557102921,null,0.12643510148683326,null,0.19405728175243109,7.0575387194727474E-2,9.9465662541354055E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR35, IF(MODE_ILIM=4,#REF!,#REF!))","v":33.065472706899293},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ35, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.19405728175243109},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA35, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0575387194727474E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB35, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.9465662541354055E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S35, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":300.80736557102921},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P35, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54770256383320148}]
["Sleep delay",5,"µs",{"$f":"B36/1000000","v":5.0000000000000004E-6},"Delay time to enter sleep mode",null,null,30,0.03,4.0330133258258252E-2,5.0161155021800193E-2,9.8425675920151105E-3,0.54769227925973907,0.54769227925973907,1,0.54769227925973907,2.9768567375707307E-6,0.10445667098228303,300835.21242897521,3.3240789597929529E-6,0,6.5999999999999989E-4,3.2174325252762669E-2,1.2422246465646739E-4,9.9355852702105424E-2,9.9482052431680637E-2,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,9.915247491892305E-3,2.9493639847642991E-7,2.9493639847642991E-7,1.0398663824112572E-2,7.428682780758546E-5,1.2078533779023353E-3,40,153.17551866870434,5.8297947890519543E-2,5.5449946354908713E-2,0.11495574762333059,0.11503161491061881,3.0337878398653151E-2,2.7979760718236551E-4,3.3091873367187274E-3,4.2720023034162476E-4,2.9037283955666551E-4,4.0267604066170177E-3,4.3067808835404202E-3,3.1732432885906034E-2,7.0578983031647169E-2,4.5170407146210628E-3,0.19443441954042745,0.29391744284453392,0.15,0.33790066693218918,1.709040464868242E-4,6.3079403938058251E-4,9.7683908481939835E-2,0.25895749193074552,9.6234161830679901E-4,6.541145076346057E-4,9.0709668464801583E-3,2.7983235770253755E-4,0.2238160592777185,6.6439470498509053E-7,1.5226615629733907E-6,0.15899123625192829,0.75121983641459167,0.33790066693218918,33.790066693218918,30,56.276153038808332,0.5627615303880833,300.83521242897518,null,0.12491049236451846,null,0.19443441954042745,7.0578983031647169E-2,9.9482052431680637E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR36, IF(MODE_ILIM=4,#REF!,#REF!))","v":33.790066693218918},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ36, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.19443441954042745},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA36, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0578983031647169E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB36, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.9482052431680637E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S36, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":300.83521242897518},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P36, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54769227925973907}]
["IQ(active)",660,"µA",{"$f":"B37/1000000","v":6.6E-4},"LM5164 quiescent current - active state ",null,null,31,3.1E-2,4.0329375938438432E-2,5.1161155308566852E-2,1.0842946252033608E-2,0.54768199468627665,0.54768199468627665,1,0.54768199468627665,2.9765490672564405E-6,0.10446634018452103,300863.05973142065,3.3237712894786627E-6,0,6.6E-4,3.3108717967788512E-2,1.3154246465646742E-4,9.9365049738774053E-2,9.9498686331819339E-2,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,1.0199365897647238E-2,3.1208119414226836E-7,3.1208119414226836E-7,1.070115253197557E-2,7.8671575207161124E-5,1.2079651848216539E-3,40,150.1802149807545,5.859217287255894E-2,5.5455079169695456E-2,0.11525521722707605,0.11533556697028691,3.1220382707988922E-2,2.9631253811572127E-4,3.3094936570456273E-3,4.7056405542952401E-4,3.0010074689046986E-4,4.0801584593656215E-3,4.3767108543834718E-3,3.1732432885906041E-2,7.0582578925964659E-2,4.517458841867281E-3,0.19481231559250231,0.29431198994154317,0.155,0.34497187582322464,1.7882839766042086E-4,6.6001442573663041E-4,9.6520025845667198E-2,0.25651489345314621,1.0472991283645597E-3,6.6791172639197509E-4,9.0809026927958503E-3,2.9276419859968899E-4,0.22114933935259937,6.9457570937038884E-7,1.5043801244670773E-6,0.15709035259697313,0.74320453077376891,0.34497187582322464,34.497187582322461,31,57.582635216683897,0.57582635216683897,300.86305973142066,null,0.12342221087158241,null,0.19481231559250231,7.0582578925964659E-2,9.9498686331819339E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR37, IF(MODE_ILIM=4,#REF!,#REF!))","v":34.497187582322461},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ37, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.19481231559250231},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA37, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0582578925964659E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB37, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.9498686331819339E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S37, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":300.86305973142066},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P37, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54768199468627665}]
["IQ(sleep)",10,"µA",{"$f":"B38/1000000","v":1.0000000000000001E-5},"LM5164 quiescent current - sleep state",null,null,32,{"$f":"IF(PLOT_TYPE=1, H38/100*Iout, min_I*EXP(H38*rr/100))","v":3.2000000000000001E-2},{"$f":"IF(I38<Icrit, (Vin-(Rdcr+RdsonTop)*Iripple/2-Vout)/L*OnTime, (Vin-(Rdcr+RdsonTop)*I38-Vout)/L*OnTime)","v":4.0328618618618611E-2},{"$f":"IF(I38<Icrit, (Vin-(Rdcr+RdsonTop)*Iripple/2-Vout)/L*OnTime, I38+((Vin-(Rdcr+RdsonTop)*J38-Vout)/L*OnTime)/2)","v":5.2161155595333505E-2},{"$f":"IF(I38<Icrit, 0, I38-((Vin-(Rdcr+RdsonTop)*K38-Vout)/L*OnTime)/2)","v":1.1843324912052106E-2},0.54767171011281413,{"$f":"IF(I38<Icrit, 1000*SQRT((J38*CoutEsr)^2+(((J38/2)-I38)*(OnTime+OffTime)/Cout)^2), 1000*J38*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":0.54767171011281413},1,{"$f":"IF(I38<Icrit, 1000*((N38/1000)*O38), 1000*J38*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":0.54767171011281413},{"$f":"IF(I38<Icrit, L*J38/(Vout+J38/2*(RdsonBot+Rdcr)), L*J38/(Vout+I38*(RdsonBot+Rdcr)))","v":2.97624144898182E-6},0.10447600954110284,{"$f":"IF(I38<Icrit,I38/((OnTime+Q38)*J38/2),1/(OnTime+Q38))","v":300890.90747837623},3.3234636712040418E-6,0,{"$f":"S38*(T38*Iq_active+U38*Iq_sleep)","v":6.6E-4},3.4046838406386011E-2,{"$f":"W38^2*Rdcr","v":1.3910246465646738E-4},{"$f":"Core_Loss/1000*S38/$S$106","v":9.9374246922249568E-2},{"$f":"(Y38+X38*(1+Ltc*(Ta-25)))/(1-X38*Ltc*ThetaCa)","v":9.9515564244547328E-2},1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,1.0484753277562757E-2,3.2979015387408894E-7,3.2979015387408894E-7,1.1004874081000052E-2,8.3200683181064051E-5,1.2080769935256805E-3,{"$f":"20*VIN_nom/24","v":40},{"$f":"IF(I38<Icrit, Csw*Vin/Iripple*1000000000, Csw*Vin/(I38+Iripple/2)*1000000000)","v":147.29980912131913},{"$f":"IF(I38<Icrit, Vin*(I38+Iripple/2)*AK38/1000000000/2*S38, Vin*(I38-Iripple/2)*AJ38/1000000000/2*S38 + Vin*(I38+Iripple/2)*AK38/1000000000/2*S38)","v":5.8886451408412789E-2},{"$f":"IF(I38<Icrit, Csw*(Vin)^2*S38/2, Csw*Vin^2*S38/2)","v":5.5460212066414306E-2},0.11555474046835278,{"$f":"(AI38+AL38+AM38+AH38*(1+RdsonTopTc*(Ta-25)))/(1-AH38*RdsonTopTc*ThetaJA)","v":0.11563972061166383},{"$f":"IF(I38<Icrit,Iripple*SQRT((OffTime)*S38/3), SQRT(OffTime*S38*(I38^2+Iripple^2/12)))","v":3.2106483804938427E-2},3.1337119590429914E-4,{"$f":"QgBot*S38*Vdd","v":3.3097999822621388E-3},{"$f":"IF(I38<Icrit, Vin*Idss*R38, QrrBot*(I38-Iripple/2)/1*S38*Vin+Vin*Idss*R38)","v":5.1393590129977199E-4},{"$f":"IF(I38<Icrit, dead1*S38*(I38+Iripple/2)*((I38+Iripple/2)*BDserR+VSD), dead1*S38*(I38+Iripple/2)*((I38+Iripple/2)*BDserR+VSD)+dead2*S38*(I38-Iripple/2)*((I38-Iripple/2)*BDserR+VSD))","v":3.0983285762609076E-4},4.1335687411880014E-3,{"$f":"(AR38+AS38+AT38+AQ38*(1+RdsonBotTc*(Ta-25)))/(1-AQ38*RdsonBotTc*ThetaJA)","v":4.4471976877878197E-3},{"$f":"Vin*V38+Vout*Ifb/0.8","v":3.1732432885906041E-2},{"$f":"(Vin-Vdd)*(S38*QgBot+S38*QgTop)+AW38","v":7.058617487768129E-2},{"$f":"AI38+AR38","v":4.5178769757878191E-3},0.19519097015292075,{"$f":"SUM(Z38,AC38,AF38,AZ38)","v":0.2947075401236493},{"$f":"Vout*I38","v":0.16},0.35187452567092015,1.8688967261890372E-4,6.8973773013425888E-4,{"$f":"Vin*S38*(QgBot+QgTop)/($BB38+$BA38)","v":9.5383549073694604E-2},0.25412980932079948,1.1302559468444632E-3,6.8138931134029016E-4,9.0906096258354403E-3,{"$f":"X38/($BB38+$BA38)","v":3.0591633606656497E-4},{"$f":"Y38/($BB38+$BA38)","v":0.21854541249794665},7.2527971228365509E-7,1.4865291813040983E-6,0.15523423002505451,0.73538001134922881,{"$f":"BC38","v":0.35187452567092015},35.187452567092016,{"$f":"I38*1000","v":32},58.807882255999409,0.58807882255999411,{"$f":"S38/1000","v":300.89090747837622},null,{"$f":"AM38/($BB38+$BA38)","v":0.1219689738404886},null,0.19519097015292075,7.058617487768129E-2,9.9515564244547328E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR38, IF(MODE_ILIM=4,#REF!,#REF!))","v":35.187452567092016},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ38, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.19519097015292075},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA38, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.058617487768129E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB38, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.9515564244547328E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S38, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":300.89090747837622},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P38, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54767171011281413}]
["High-side N-ch MOSFET",null,"Units","Std Units","Description",null,null,33,3.3000000000000002E-2,4.0327861298798791E-2,5.3161155882100158E-2,1.2843703572070604E-2,{"$f":"IF(I39<Icrit, 1000*((((J39/2)-I39)*0.000002/Cout+Vout/306)), 1000*J39*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":0.54766142553935171},0.54766142553935171,1,0.54766142553935171,2.9759338827336686E-6,0.10448567905203204,300918.75566985237,{"$f":"IF(1/S39-OnTime-Q39>Tsleep, OnTime+Q39+Tsleep, 1/S39)","v":3.3231561049558909E-6},{"$f":"IF(1/S39-OnTime-Q39>Tsleep, 1/S39-OnTime-Q39-Tsleep, 0)","v":0},6.6E-4,{"$f":"IF(I39<Icrit,Iripple*SQRT((OnTime+OffTime)*S39/3), SQRT(I39^2+Iripple^2/12))","v":3.4988386722890806E-2},1.4690246465646738E-4,9.9383444252535424E-2,9.9532686172697921E-2,{"$f":"Iripple/SQRT(12)*SQRT((OnTime+Q39)*S39)","v":1.1627003288490194E-2},6.7593602735280891E-7,6.7593602735280891E-7,{"$f":"SQRT($R39)*SQRT($I39^2*(1-R39)+(Iripple^2)/12)","v":1.0771310896967791E-2},3.4806341531741121E-7,3.4806341531741121E-7,{"$f":"IF(I39<Icrit,Iripple*SQRT((OnTime)*S39/3), SQRT(OnTime*S39*(I39^2+Iripple^2/12)))","v":1.1309731714342349E-2},{"$f":"RdsonTop*AG39^2","v":8.7874191606425583E-5},{"$f":"QgTop*S39*Vdd","v":1.2081888040144572E-3},40,144.52781439819725,5.9180783499363294E-2,5.5465345045067185E-2,0.11585431734844494,0.11594407590163593,3.2995899403488092E-2,{"$f":"RdsonBot*AP39^2","v":3.3097373074331219E-4},3.3101063123683766E-3,5.573157681444162E-4,3.1956917247489419E-4,4.1869912529876874E-3,4.5182415615242499E-3,3.1732432885906041E-2,7.0589770886798409E-2,4.5182951163828342E-3,0.1955703834663414,0.295104093638482,0.16500000000000001,0.35861450111253651,1.950831440798143E-4,7.1994644932856465E-4,9.4273521398739776E-2,0.25180023162209736,1.211281916092484E-3,6.9455842035169883E-4,9.1000956324408088E-3,3.1928093378776404E-4,0.21600208654223377,7.5648841236108483E-7,1.4690937044431355E-6,0.15342130588010583,0.72773961752137462,0.35861450111253651,35.861450111253653,33,59.95273560232264,0.59952735602322638,300.91875566985237,null,0.12054955783255433,null,0.1955703834663414,7.0589770886798409E-2,9.9532686172697921E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR39, IF(MODE_ILIM=4,#REF!,#REF!))","v":35.861450111253653},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ39, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.1955703834663414},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA39, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0589770886798409E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB39, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.9532686172697921E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S39, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":300.91875566985237},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P39, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54766142553935171}]
["RdsonTop",687,"mW",{"$f":"B40/1000","v":0.68700000000000006},"Drain-source resistance of high-side MOSFET @ VDD, 25°C",null,null,34,3.4000000000000002E-2,4.032710397897897E-2,5.4161156168866811E-2,1.3844082232089102E-2,0.54765114096588918,0.54765114096588918,1,0.54765114096588918,2.9756263684987879E-6,0.10449534871731243,300946.60430585989,3.3228485907210102E-6,0,6.6E-4,3.5933093458128007E-2,1.5494246465646742E-4,9.9392641729635176E-2,9.9550052119160765E-2,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,1.1058949861468381E-2,3.669011161154146E-7,3.669011161154146E-7,1.1615638479867497E-2,9.269214036165024E-5,1.2083006162880274E-3,40,141.85822338514183,5.9475169146692847E-2,5.5470478105656092E-2,0.11615394786863698,0.11624863290713257,3.3888375822651418E-2,3.4912029283276858E-4,3.3104126473644589E-3,6.0070365615551118E-4,3.2930969214826943E-4,4.2404259956682396E-3,4.5898426537147423E-3,3.1732432885906041E-2,7.0593366953317416E-2,4.5187132636524859E-3,0.19595055577781723,0.29550165073412149,0.17,0.36519741601753875,2.0340430231830382E-4,7.5062388607098065E-4,9.3189030076803819E-2,0.2495242448344831,1.2904436648251809E-3,7.0742969789458336E-4,9.1093683319508241E-3,3.328505160231219E-4,0.21351727018129271,7.881843502311786E-7,1.4520593563670954E-6,0.15165008940782018,0.72027699514318944,0.36519741601753875,36.519741601753871,34,61.018807215515402,0.61018807215515403,300.94660430585986,null,0.11916279570260625,null,0.19595055577781723,7.0593366953317416E-2,9.9550052119160765E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR40, IF(MODE_ILIM=4,#REF!,#REF!))","v":36.519741601753871},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ40, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.19595055577781723},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA40, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0593366953317416E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB40, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.9550052119160765E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S40, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":300.94660430585986},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P40, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54765114096588918}]
["RdsonTopTc",4500,"ppm/°C",{"$f":"B41/1000000","v":4.4999999999999997E-3},"Drain to Source Resistance Temp Co",null,null,35,3.4999999999999996E-2,4.032634665915915E-2,5.5161156455633464E-2,1.4844460892107589E-2,0.54764085639242666,0.54764085639242666,1,0.54764085639242666,2.9753189062639853E-6,0.10450501853694766,300974.45338640932,3.322541128486208E-6,0,6.6E-4,3.6880715902359619E-2,1.6322246465646739E-4,9.9401839353552332E-2,9.9567662086881753E-2,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,1.1347589963055836E-2,3.8630339390893669E-7,3.8630339390893669E-7,1.1922516056664384E-2,9.7654569326415598E-5,1.2084124303464335E-3,40,139.28546446171563,5.976960835168376E-2,5.5475611248182968E-2,0.11645363203021317,0.11655339169512589,3.478368456285217E-2,3.6781103237747213E-4,3.3107189872505025E-3,6.4409956552511684E-4,3.3905441735762793E-4,4.293872970133247E-3,4.6620011428328053E-3,3.1732432885906041E-2,7.0596963077239699E-2,4.5191314175969362E-3,0.19633148733279535,0.29590021165909836,0.17499999999999999,0.37162862888388082,2.1184884279675488E-4,7.8175410327923061E-4,9.2129203883937916E-2,0.24730002057106348,1.3678047908617288E-3,7.2001330422650492E-4,9.118434997098147E-3,3.466179471047467E-4,0.21108896724283682,8.2035086063753074E-7,1.4354124517619529E-6,0.14991915766720315,0.71298607911372081,0.37162862888388082,37.162862888388084,34.999999999999993,62.00835196729512,0.62008351967295117,300.97445338640932,null,0.11780757339804249,null,0.19633148733279535,7.0596963077239699E-2,9.9567662086881753E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR41, IF(MODE_ILIM=4,#REF!,#REF!))","v":37.162862888388084},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ41, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.19633148733279535},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA41, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0596963077239699E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB41, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.9567662086881753E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S41, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":300.97445338640932},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P41, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54764085639242666}]
["QgTop",0.80300000000000005,"nC",{"$f":"B42/1000000000","v":8.0300000000000002E-10},"Gate charge of high-side MOSFET @ VDD",null,null,36,3.5999999999999997E-2,4.0325589339339329E-2,5.6161156742400117E-2,1.5844839552126091E-2,0.54763057181896424,0.54763057181896424,1,0.54763057181896424,2.9750114960160725E-6,0.10451468851094142,301002.30291151139,3.3222337182382948E-6,0,6.5999999999999989E-4,3.7831034951089582E-2,1.7174246465646739E-4,9.9411037124290405E-2,9.9585516078862957E-2,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,1.1637158678653383E-2,4.0627038633647327E-7,4.0627038633647327E-7,1.2230293740568967E-2,1.0276151838167252E-4,1.2085242461897182E-3,40,136.80436299809853,6.0064101115618454E-2,5.5480744472649779E-2,0.11675336983445794,0.11685835233263096,3.5681619346210086E-2,3.8704609958702146E-4,3.3110253320266258E-3,6.8750349644530013E-4,3.4880334881440413E-4,4.3473321772863303E-3,4.7347172077038197E-3,3.1732432885906034E-2,7.0600559258566592E-2,4.519549578216344E-3,0.19671317837711774,0.29629977666239438,0.18,0.37791325719555319,2.2041265462829042E-4,8.1332188129928809E-4,9.1093210781894793E-2,0.24512581268165026,1.443426031527638E-3,7.3231894261760098E-4,9.1273025734961849E-3,3.6057641231732095E-4,0.20871527133793694,8.5297202779173555E-7,1.4191399208484588E-6,0.14822715171795875,0.70586107712727575,0.37791325719555319,37.791325719555317,36,62.924142868481049,0.62924142868481048,301.00230291151138,null,0.11648282697385147,null,0.19671317837711774,7.0600559258566592E-2,9.9585516078862957E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR42, IF(MODE_ILIM=4,#REF!,#REF!))","v":37.791325719555317},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ42, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.19671317837711774},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA42, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0600559258566592E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB42, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.9585516078862957E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S42, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.00230291151138},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P42, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54763057181896424}]
["Coss",100,"pF",{"$f":"B43/1000000000000","v":1E-10},"Capacitance (Coss)",null,null,37,3.6999999999999998E-2,4.0324832019519509E-2,5.7161157029166777E-2,1.6845218212144585E-2,0.54762028724550182,0.54762028724550182,1,0.54762028724550182,2.9747041377418646E-6,0.10452435863929745,301030.15288117673,3.3219263599640869E-6,0,6.600000000000001E-4,3.8783852380476096E-2,1.8050246465646736E-4,9.9420235041852947E-2,9.9603614098162749E-2,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,1.1927590299164629E-2,4.2680223103417855E-7,4.2680223103417855E-7,1.253890756506513E-2,1.0801302740964508E-4,1.2086360638179246E-3,40,134.41010661579637,6.0358647439779395E-2,5.5485877779058494E-2,0.1170531612826558,0.11716351488670596,3.6581993551788074E-2,4.0682564467581152E-4,3.3113316816929445E-3,7.3091544910813355E-4,3.5855648723005518E-4,4.4008036180311332E-3,4.807991027505374E-3,3.1732432885906048E-2,7.0604155497299523E-2,4.5199677455108689E-3,0.1970956291570217,0.29670034599344286,0.185,0.38405619082224679,2.2909180981085054E-4,8.4531267801867763E-4,9.0080255739519485E-2,0.24299995268064264,1.5173654226897381E-3,7.4435588475773283E-4,9.1359776978259411E-3,3.7471940005400048E-4,0.20639436086933247,8.8603264370498997E-7,1.403229275160226E-6,0.14657277306224029,0.69889645450681059,0.38405619082224679,38.405619082224682,37,63.769353027551922,0.63769353027551923,301.03015288117672,null,0.11518753980677812,null,0.1970956291570217,7.0604155497299523E-2,9.9603614098162749E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR43, IF(MODE_ILIM=4,#REF!,#REF!))","v":38.405619082224682},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ43, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.1970956291570217},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA43, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0604155497299523E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB43, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.9603614098162749E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S43, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.03015288117672},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P43, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54762028724550182}]
["Low-side N-ch MOSFET",null,"Units","Std Units","Description",null,null,38,3.8000000000000006E-2,4.0324074699699695E-2,5.8161157315933437E-2,1.784559687216309E-2,0.5476100026720393,0.5476100026720393,1,0.5476100026720393,2.9743968314281835E-6,0.10453402892201938,301058.0032954159,3.3216190536504053E-6,0,6.5999999999999989E-4,3.9738988480717045E-2,1.8950246465646744E-4,9.9429433106243401E-2,9.9621956147895707E-2,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,1.2218825170419936E-2,4.4789906563586332E-7,4.4789906563586332E-7,1.284829953767979E-2,1.1340913629383064E-4,1.2087478832310948E-3,40,132.09821403350475,6.0653247325449036E-2,5.5491011167411057E-2,0.1173530063760912,0.11746887942445185,3.7484637987791274E-2,4.2714981786303244E-4,3.3116380362495754E-3,7.7433542370569587E-4,3.6831383331606079E-4,4.454287293271332E-3,4.8818227817676125E-3,3.1732432885906034E-2,7.0607751793439796E-2,4.5203859194806705E-3,0.19747883991913995,0.29710191990212864,0.19000000000000003,0.39006210453487006,2.3788255317066528E-4,8.7771259161159403E-4,8.9089578697890887E-2,0.24092084547659026,1.5896784472976E-3,7.5613299448719991E-4,9.1444667148228714E-3,3.8904068514971848E-4,0.20412449436910726,9.1951816926908796E-7,1.3876685755798742E-6,0.14495478032118353,0.69208692003805639,0.39006210453487006,39.006210453487007,38.000000000000007,64.547447140017496,0.645474471400175,301.05800329541592,null,0.113920739993307,null,0.19747883991913995,7.0607751793439796E-2,9.9621956147895707E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR44, IF(MODE_ILIM=4,#REF!,#REF!))","v":39.006210453487007},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ44, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.19747883991913995},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA44, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0607751793439796E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB44, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.9621956147895707E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S44, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.05800329541592},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P44, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.5476100026720393}]
["RdsonBot",304,"mW",{"$f":"B45/1000","v":0.30399999999999999},"Drain-source resistance of low-side MOSFET @ VDD, 25°C",null,null,39,3.9000000000000007E-2,4.0323317379879868E-2,5.916115760270009E-2,1.8845975532181591E-2,0.54759971809857677,0.54759971809857677,1,0.54759971809857677,2.974089577061851E-6,0.10454369935911098,301085.8541542397,3.3213117992840737E-6,0,6.6E-4,4.0696279995480693E-2,1.9874246465646743E-4,9.9438631317465359E-2,9.9640542231232657E-2,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,1.251080903023457E-2,4.695610277729966E-7,4.695610277729966E-7,1.315841697511979E-2,1.189498849189999E-4,1.2088597044292726E-3,40,129.86450707376696,6.0947900773909935E-2,5.5496144637709459E-2,0.11765290511604867,0.11777444601301278,3.8389398951843262E-2,4.480187693726705E-4,3.3119443956966367E-3,8.1776342043007161E-4,3.7807538778392364E-4,4.5077832039106319E-3,4.9562126503735759E-3,3.1732432885906041E-2,7.0611348146988856E-2,4.5208041001259091E-3,0.19786281091050112,0.29750449863878892,0.19500000000000003,0.39593546970423976,2.4678129296285608E-4,9.1050832571547681E-4,8.8120452668268553E-2,0.23888696538046708,1.66041817423039E-3,7.6765874997866863E-4,9.1527756931550699E-3,4.0353431330223945E-4,0.20190400614065315,9.5341469787747161E-7,1.3724464024612935E-6,0.14337198612834681,0.68542741272818064,0.39593546970423976,39.593546970423979,39.000000000000007,65.262084299350803,0.65262084299350809,301.08585415423971,null,0.11268149791746625,null,0.19786281091050112,7.0611348146988856E-2,9.9640542231232657E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR45, IF(MODE_ILIM=4,#REF!,#REF!))","v":39.593546970423979},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ45, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.19786281091050112},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA45, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0611348146988856E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB45, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.9640542231232657E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S45, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.08585415423971},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P45, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54759971809857677}]
["RdsonBotTc",4500,"ppm/°C",{"$f":"B46/1000000","v":4.4999999999999997E-3},"Drain To Source Resitance Temp Co",null,null,40,4.0000000000000008E-2,4.0322560060060048E-2,6.016115788946675E-2,1.9846354192200089E-2,0.54758943352511436,0.54758943352511436,1,0.54758943352511436,2.9737823746296996E-6,0.1045533699505759,301113.70545765868,3.3210045968519214E-6,0,6.5999999999999989E-4,4.1655578323563848E-2,2.0822246465646745E-4,9.9447829675522306E-2,9.9659372351400724E-2,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,1.2803492428171094E-2,4.917882550747036E-7,4.917882550747036E-7,1.3469211923014266E-2,1.2463531317119685E-4,1.2089715274124996E-3,40,127.70508546251655,6.124260778644465E-2,5.550127818995565E-2,0.11795285750381279,0.11808021471957582,3.9296136538096854E-2,4.6943264943350821E-4,3.3122507600342457E-3,8.6119943947335169E-4,3.8784115134516875E-4,4.5612913508527664E-3,5.0311608135595477E-3,3.1732432885906034E-2,7.0614944557948034E-2,4.5212222874467453E-3,0.19824754237853015,0.2979080824542133,0.20000000000000004,0.40168056524447288,2.5578459207827497E-4,9.4368715685588312E-4,8.7172181952840821E-2,0.23689685237166139,1.7296353881793953E-3,7.7894126448697259E-4,9.1609104402763201E-3,4.1819458649903552E-4,0.19973130218199928,9.8770892139499957E-7,1.3575518276808986E-6,0.14182325422371839,0.67891308941934492,0.40168056524447288,40.168056524447287,40.000000000000007,65.91703305041338,0.65917033050413376,301.11370545765868,null,0.11146892397566058,null,0.19824754237853015,7.0614944557948034E-2,9.9659372351400724E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR46, IF(MODE_ILIM=4,#REF!,#REF!))","v":40.168056524447287},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ46, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.19824754237853015},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA46, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0614944557948034E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB46, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.9659372351400724E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S46, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.11370545765868},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P46, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54758943352511436}]
["QgBot",2.2000000000000002,"nC",{"$f":"B47/1000000000","v":2.2000000000000003E-9},"Gate charge of low-side MOSFET at VDD",null,null,41,4.1000000000000002E-2,4.0321802740240227E-2,6.1161158176233396E-2,2.0846732852218577E-2,0.54757914895165183,0.54757914895165183,1,0.54757914895165183,2.9734752241185616E-6,0.10456304069641784,301141.55720568344,3.3206974463407835E-6,0,6.6E-4,4.2616747945737977E-2,2.1794246465646746E-4,9.9457028180417725E-2,9.967844651168313E-2,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,1.3096830216605407E-2,5.1458088516776538E-7,5.1458088516776538E-7,1.3780640648312826E-2,1.3046546093773911E-4,1.2090833521808191E-3,40,125.61630410173564,6.15373683643358E-2,5.5506411824151572E-2,0.11825286354066819,0.11838618561137129,4.0204723156316673E-2,4.913916082791241E-4,3.3125571292625181E-3,9.046434810276332E-4,3.9761112471134403E-4,4.6148117350014945E-3,5.1066674519153884E-3,3.1732432885906041E-2,7.0618541026318732E-2,4.521640481443337E-3,0.19863303457104875,0.29831267159964442,0.20500000000000002,0.40730148785736403,2.648891598126724E-4,9.7723690395209485E-4,8.6244100479123939E-2,0.23494910860247797,1.7973787112342441E-3,7.8998830577351375E-4,9.1688765163303997E-3,4.3301604937502516E-4,0.19760485636954106,1.0223880983014156E-6,1.3429743884741218E-6,0.14030749673334594,0.67253931319345372,0.40730148785736403,40.730148785736404,41,66.516098897051677,0.66516098897051679,301.14155720568345,null,0.11028216644683178,null,0.19863303457104875,7.0618541026318732E-2,9.967844651168313E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR47, IF(MODE_ILIM=4,#REF!,#REF!))","v":40.730148785736404},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ47, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.19863303457104875},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA47, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0618541026318732E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB47, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.967844651168313E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S47, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.14155720568345},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P47, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54757914895165183}]
["VSD",0.8,"V",{"$f":"B48","v":0.8},"Body diode forward voltage",null,null,42,4.2000000000000003E-2,4.0321045420420414E-2,6.2161158463000056E-2,2.1847111512237078E-2,0.54756886437818941,0.54756886437818941,1,0.54756886437818941,2.9731681255152756E-6,0.10457271159664046,301169.40939832461,3.3203903477374983E-6,0,6.6E-4,4.3579665045414953E-2,2.2790246465646742E-4,9.9466226832155155E-2,9.9697764715419523E-2,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,1.3390781103388757E-2,5.3793905567662027E-7,5.3793905567662027E-7,1.4092663194219274E-2,1.3644036810721768E-4,1.2091951787342734E-3,40,123.59475253662887,6.1832182508865997E-2,5.551154554029919E-2,0.11855292322789945,0.11869235875567244,4.1115042233407895E-2,5.1389579614789414E-4,3.3128635033815709E-3,9.4809554528501954E-4,4.0738530859402025E-4,4.6683443572606113E-3,5.1827327463848981E-3,3.1732432885906041E-2,7.062213755210231E-2,4.5220586821158445E-3,0.19901928773627547,0.298718266326778,0.21000000000000002,0.4128021616292924,2.7409184415528361E-4,1.0111458997500722E-3,8.5335570239631078E-2,0.23304239512356401,1.8636947167845652E-3,8.0080731430298994E-4,9.1766792471766178E-3,4.4799347643253887E-4,0.19552320688296748,1.0574400238482339E-6,1.3287040629255048E-6,0.13882367162090026,0.66630164250975166,0.4128021616292924,41.280216162929243,42,67.063063929713536,0.6706306392971354,301.1694093983246,null,0.10912040949723052,null,0.19901928773627547,7.062213755210231E-2,9.9697764715419523E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR48, IF(MODE_ILIM=4,#REF!,#REF!))","v":41.280216162929243},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ48, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.19901928773627547},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA48, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.062213755210231E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB48, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.9697764715419523E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S48, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.1694093983246},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P48, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54756886437818941}]
["BDserR",100,"mW",{"$f":"B49*0.001","v":0.1},"Series resistance of body diode",null,null,43,4.3000000000000003E-2,4.0320288100600593E-2,6.3161158749766716E-2,2.2847490172255576E-2,0.547558579804727,0.547558579804727,1,0.547558579804727,2.9728610788066828E-6,0.10458238265124757,301197.2620355931,3.3200833010289051E-6,0,6.600000000000001E-4,4.4544216296513311E-2,2.3810246465646746E-4,9.9475425630738162E-2,9.9717326966005757E-2,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,1.3685307257826577E-2,5.6186290422336235E-7,5.6186290422336235E-7,1.4405242989072831E-2,1.4256007456949738E-4,1.2093070070729062E-3,40,121.63723637401354,6.2127050221317995E-2,5.5516679338400522E-2,0.11885303656679141,0.11899873421979594,4.2026987072335542E-2,5.3694536328299065E-4,3.3131698823915248E-3,9.915556324376208E-4,4.1716370370479112E-4,4.7218892185339366E-3,5.2593568782661453E-3,3.1732432885906048E-2,7.0625734135300156E-2,4.522476889464431E-3,0.19940630212282667,0.29912486688776402,0.21500000000000002,0.41818634702790125,2.833896245604711E-4,1.0454029640420807E-3,8.4445979829130519E-2,0.23117542881413983,1.9286280362978089E-3,8.1140542030202947E-4,9.184323736600641E-3,4.631218600605957E-4,0.19348495285378625,1.0928530020821183E-6,1.3147312469917332E-6,0.13737078029862754,0.66019582102179686,0.41818634702790125,41.818634702790128,43,67.561637846160409,0.67561637846160405,301.1972620355931,null,0.10798287130997708,null,0.19940630212282667,7.0625734135300156E-2,9.9717326966005757E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR49, IF(MODE_ILIM=4,#REF!,#REF!))","v":41.818634702790128},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ49, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.19940630212282667},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA49, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0625734135300156E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB49, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.9717326966005757E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S49, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.1972620355931},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P49, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.547558579804727}]
["QrrBot",3,"nC",{"$f":"B50*0.000000001","v":3.0000000000000004E-9},"Reverse recovery charge of body diode at 100mA",null,null,44,4.4000000000000004E-2,4.0319530780780773E-2,6.4161159036533369E-2,2.384786883227407E-2,0.54754829523126447,0.54754829523126447,1,0.54754829523126447,2.9725540839796323E-6,0.10459205386024277,301225.11511749926,3.3197763062018541E-6,0,6.5999999999999989E-4,4.5510297795889693E-2,2.4854246465646747E-4,9.9484624576170189E-2,9.9737133266893846E-2,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,1.3980373962901705E-2,5.8635256842773978E-7,5.8635256842773978E-7,1.4718346501873869E-2,1.4882462021571604E-4,1.2094188371967595E-3,40,119.74076043897196,6.2421971502974474E-2,5.5521813218457464E-2,0.1191532035586287,0.11930531207110139,4.2940459847128291E-2,5.6054045993238243E-4,3.3134762662924921E-3,1.0350237426775511E-3,4.2694631075527231E-4,4.7754463197253157E-3,5.336540029211816E-3,3.1732432885906034E-2,7.0629330775913601E-2,4.5228951034892518E-3,0.19979407797971604,0.29953247353520568,0.22000000000000003,0.423457649341898,2.9277960516625875E-4,1.0799973785439964E-3,8.3574743072445321E-2,0.22934697950224353,1.9922214594876781E-3,8.2178945976192305E-4,9.1918148777695441E-3,4.7839639929577029E-4,0.19148875122130107,1.1286158195999776E-6,1.3010467329469149E-6,0.13594786538618064,0.65421776802474818,0.423457649341898,42.345764934189802,44.000000000000007,68.015419380100283,0.68015419380100284,301.22511511749923,null,0.10686880233039961,null,0.19979407797971604,7.0629330775913601E-2,9.9737133266893846E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR50, IF(MODE_ILIM=4,#REF!,#REF!))","v":42.345764934189802},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ50, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.19979407797971604},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA50, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0629330775913601E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB50, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.9737133266893846E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S50, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.22511511749923},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P50, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54754829523126447}]
["TrrBot",20,"ns",{"$f":"B51*0.000000001","v":2E-8},"Reverse recovery time of body diode (not used)",null,null,45,4.5000000000000005E-2,4.0318773460960945E-2,6.5161159323300022E-2,2.4848247492292568E-2,0.54753801065780194,0.54753801065780194,1,0.54753801065780194,2.9722471410209741E-6,0.10460172522362979,301252.96864405385,3.3194693632431964E-6,0,6.600000000000001E-4,4.6477814121046637E-2,2.5922246465646742E-4,9.9493823668454801E-2,9.9757183621592166E-2,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,1.4275949307689452E-2,6.1140818590715675E-7,6.1140818590715675E-7,1.5031942938230987E-2,1.552340449382857E-4,1.2095306691058761E-3,40,117.90251348296719,6.2716946355118236E-2,5.5526947180472006E-2,0.11945342420469612,0.11961209237699175,4.3855370715810506E-2,5.8468123634883556E-4,3.3137826550845924E-3,1.0784998761969328E-3,4.3673313045710288E-4,4.8290156617386273E-3,5.4142823812295682E-3,3.1732432885906048E-2,7.0632927473944077E-2,4.5233133241904689E-3,0.20018261555635586,0.29994108652216128,0.22500000000000003,0.42861952660377489,3.022590084286048E-4,1.1149188633117839E-3,8.2721297736322821E-2,0.22755586726140778,2.054516028345596E-3,8.3196598946092481E-4,9.1991573639849996E-3,4.938124892716392E-4,0.18953331378121133,1.1647177209119925E-6,1.2876416891484318E-6,0.13455400860675854,0.64836356948791418,0.42861952660377489,42.86195266037749,45.000000000000007,68.427867006324419,0.68427867006324417,301.25296864405385,null,0.10577748361887432,null,0.20018261555635586,7.0632927473944077E-2,9.9757183621592166E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR51, IF(MODE_ILIM=4,#REF!,#REF!))","v":42.86195266037749},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ51, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.20018261555635586},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA51, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0632927473944077E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB51, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.9757183621592166E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S51, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.25296864405385},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P51, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54753801065780194}]
["Idss",0,"μA",{"$f":"B52/1000000","v":0},"Leakage current of low-side device",null,null,46,4.6000000000000006E-2,4.0318016141141139E-2,6.6161159610066675E-2,2.584862615231107E-2,0.54752772608433964,0.54752772608433964,1,0.54752772608433964,2.9719402499175659E-6,0.10461139674141227,301280.82261526742,3.3191624721397881E-6,0,6.6E-4,4.7446677496644191E-2,2.7014246465646745E-4,9.9503022907595454E-2,9.9777478033665226E-2,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,1.4572003914775207E-2,6.370298942766719E-7,6.370298942766719E-7,1.5346003971414585E-2,1.6178838863089182E-4,1.2096425028002987E-3,40,116.11985427921776,6.3011974779032059E-2,5.5532081224446091E-2,0.11975369850627846,0.1199190752049132,4.47716370357569E-2,6.093678427899139E-4,3.314089048767942E-3,1.1219840331878938E-3,4.4652416352194415E-4,4.8825972454777803E-3,5.4925841166823747E-3,3.1732432885906041E-2,7.0636524229392914E-2,4.5237315515682403E-3,0.2005719151025567,0.30035070610214354,0.23000000000000004,0.4336752970320415,3.1182516914174001E-4,1.1501575545882527E-3,8.1885104319425722E-2,0.22580095987128629,2.1155511254694246E-3,8.4194130107549117E-4,9.2063556987843631E-3,5.0936571130809252E-4,0.18761740441320643,1.2011483852988071E-6,1.2745076410299455E-6,0.13318832881083897,0.64262946963115108,0.4336752970320415,43.367529703204148,46.000000000000007,68.802277733330541,0.68802277733330541,301.28082261526743,null,0.10470822530356134,null,0.2005719151025567,7.0636524229392914E-2,9.9777478033665226E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR52, IF(MODE_ILIM=4,#REF!,#REF!))","v":43.367529703204148},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ52, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.2005719151025567},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA52, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0636524229392914E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB52, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.9777478033665226E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S52, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.28082261526743},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P52, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54752772608433964}]
["Csw",160,"pF",{"$f":"B53/1000000000000","v":1.5999999999999999E-10},"Effective SW node capacitance (CossHS + CossLS)",null,null,47,4.7E-2,4.0317258821321318E-2,6.7161159896833328E-2,2.684900481232956E-2,0.54751744151087711,0.54751744151087711,1,0.54751744151087711,2.9716334106562658E-6,0.10462106841359402,301308.67703115084,3.3188556328784876E-6,0,6.6E-4,4.8416807055717354E-2,2.8130246465646742E-4,9.9512222293595756E-2,9.9798016506734005E-2,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,1.4868510698217196E-2,6.6321783114899759E-7,6.6321783114899759E-7,1.5660503503968429E-2,1.6848769118849372E-4,1.2097543382800708E-3,40,114.3902989606928,6.3307056775998835E-2,5.5537215350381725E-2,0.12005402646466062,0.12022626062235527,4.5689182668199352E-2,6.3460042951797883E-4,3.3143954473426598E-3,1.1654762138425675E-3,4.5631941066148068E-4,4.9361910718467078E-3,5.5714454182888675E-3,3.1732432885906041E-2,7.0640121042261528E-2,4.5241497856227308E-3,0.2009619768685284,0.30076133252912091,0.23499999999999999,0.43862814602662048,3.2147552881726623E-4,1.1857039839799021E-3,8.1065644914972507E-2,0.22408117043074435,2.1753645570888958E-3,8.5172143444427813E-4,9.2134142054352258E-3,5.250518235956819E-4,0.18573983647501635,1.2378979050582172E-6,1.2616364532355814E-6,0.13184998011856697,0.63701186300701962,0.43862814602662048,43.862814602662048,47,69.1417728033842,0.69141772803384205,301.30867703115086,null,0.10366036512603874,null,0.2009619768685284,7.0640121042261528E-2,9.9798016506734005E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR53, IF(MODE_ILIM=4,#REF!,#REF!))","v":43.862814602662048},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ53, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.2009619768685284},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA53, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0640121042261528E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB53, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.9798016506734005E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S53, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.30867703115086},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P53, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54751744151087711}]
["ThetaJA",41.1,"°C/W",null,"Thermal resistance",null,null,48,4.8000000000000001E-2,4.0316501501501491E-2,6.8161160183599981E-2,2.7849383472348055E-2,0.54750715693741459,0.54750715693741459,1,0.54750715693741459,2.9713266232239394E-6,0.10463074024017865,301336.53189171461,3.3185488454461616E-6,0,6.6E-4,4.9388128183507442E-2,2.9270246465646748E-4,9.9521421826459164E-2,9.9818799044475534E-2,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,1.5165444648218097E-2,6.8997213413450088E-7,6.8997213413450088E-7,1.597541745597772E-2,1.7533199250732449E-4,1.2098661755452341E-3,40,112.71150947307099,6.3602192347301467E-2,5.5542349558280836E-2,0.12035440808112755,0.12053364869685082,4.6607937360503532E-2,6.6037914680018876E-4,3.3147018508088611E-3,1.2089764183530948E-3,4.6611887258741927E-4,4.9897971417493759E-3,5.6508664691236948E-3,3.1732432885906041E-2,7.0643717912551252E-2,4.5245680263540956E-3,0.20135280110487985,0.30117296605751687,0.24,0.44348113274840184,3.3120763039782934E-4,1.2215490588716126E-3,8.026242214098861E-2,0.22239545511284106,2.2339926311555677E-3,8.6131219004365283E-4,9.2203370358656302E-3,5.4086675243374691E-4,0.18389947035137347,1.2749567650450029E-6,1.2490203128161601E-6,0.13053815017256998,0.63150728705361903,0.44348113274840184,44.348113274840188,48,69.449289175978407,0.69449289175978413,301.33653189171463,null,0.10263326707339201,null,0.20135280110487985,7.0643717912551252E-2,9.9818799044475534E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR54, IF(MODE_ILIM=4,#REF!,#REF!))","v":44.348113274840188},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ54, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.20135280110487985},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA54, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0643717912551252E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB54, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.9818799044475534E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S54, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.33653189171463},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P54, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54750715693741459}]
["Inductor",null,"Units","Std Units","Description",null,null,49,4.9000000000000002E-2,4.031574418168167E-2,6.9161160470366634E-2,2.8849762132366553E-2,0.54749687236395217,0.54749687236395217,1,0.54749687236395217,2.9710198876074571E-6,0.10464041222116989,301364.38719696936,3.3182421098296794E-6,0,6.6E-4,5.0360571933513246E-2,3.0434246465646742E-4,9.9530621506189201E-2,9.983982565062316E-2,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,1.5462782639197495E-2,7.172929408412023E-7,7.172929408412023E-7,1.6290723576640066E-2,1.8232133248489112E-4,1.2099780145958319E-3,40,111.08128302977779,6.389738149422286E-2,5.5547483848145389E-2,0.12065484335696408,0.12084123949597593,4.7527836196431306E-2,6.86704144908501E-4,3.3150082591666633E-3,1.2524846469116214E-3,4.7592255001148979E-4,5.0434154560897743E-3,5.7308474526178571E-3,3.1732432885906041E-2,7.06473148402635E-2,4.5249862737624953E-3,0.20174438806261977,0.30158560694221115,0.245,0.44823719631150682,3.4101911328147385E-4,1.2576840439941605E-3,7.9474958133525689E-2,0.22074281105195762,2.291470230836215E-3,8.7071914072886969E-4,9.2271281790685701E-3,5.5680658398428082E-4,0.18209521114724903,1.312315823415086E-6,1.236651713414535E-6,0.1292520584936164,0.62611241508577908,0.44823719631150682,44.823719631150681,49,69.727575757335345,0.69727575757335347,301.36438719696935,null,0.10162632009082204,null,0.20174438806261977,7.06473148402635E-2,9.983982565062316E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR55, IF(MODE_ILIM=4,#REF!,#REF!))","v":44.823719631150681},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ55, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.20174438806261977},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA55, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.06473148402635E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB55, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.983982565062316E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S55, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.36438719696935},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P55, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54749687236395217}]
["Ltc",4000,"ppm",{"$f":"Ltc","v":4.0000000000000001E-3},"Inductor DCR Temp Co",null,null,50,0.05,4.0314986861861857E-2,7.0161160757133301E-2,2.9850140792385051E-2,0.54748658779048964,0.54748658779048964,1,0.54748658779048964,2.9707132037936918E-6,0.10465008435657142,301392.24294692575,3.3179354260159141E-6,0,6.6E-4,5.1334074506808457E-2,3.1622246465646739E-4,9.953982133278938E-2,9.9861096328966559E-2,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,1.5760503258407017E-2,7.4518038887477453E-7,7.4518038887477453E-7,1.6606401276250432E-2,1.8945575101997431E-4,1.2100898554319069E-3,40,109.49754246909106,6.4192624218046015E-2,5.5552618219977354E-2,0.12095533229345527,0.12114903308735024,4.844881910596037E-2,7.1357557411966949E-4,3.3153146724161837E-3,1.2960008997102992E-3,4.8573044364544446E-4,5.0970460157719272E-3,5.8113885525590729E-3,3.1732432885906041E-2,7.065091182539962E-2,4.5254045278480901E-3,0.20213673799315701,0.30199925543853978,0.25,0.45289916161460347,3.5090770863645759E-4,1.2941005440661893E-3,7.8702793598566287E-2,0.21912227435408665,2.347830883722265E-3,8.799476427908447E-4,9.2337914690166431E-3,5.7286755650647059E-4,0.18032600651555092,1.3499662934921183E-6,1.2245234403727714E-6,0.12799095493212304,0.62082404969479965,0.45289916161460347,45.289916161460347,50,69.979193442852676,0.69979193442852672,301.39224294692576,null,0.10063893686929555,null,0.20213673799315701,7.065091182539962E-2,9.9861096328966559E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR56, IF(MODE_ILIM=4,#REF!,#REF!))","v":45.289916161460347},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ56, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.20213673799315701},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA56, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.065091182539962E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB56, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.9861096328966559E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S56, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.39224294692576},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P56, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54748658779048964}]
["ThetaCA",20,"°C/W",{"$f":"ThetaCa","v":40},"Inductor Core-to-Ambient thermal resistance",null,null,51,5.1000000000000004E-2,4.0314229542042036E-2,7.116116104389994E-2,3.0850519452403549E-2,0.54747630321702723,0.54747630321702723,1,0.54747630321702723,2.970406571769522E-6,0.10465975664638692,301420.09914159443,3.3176287939917447E-6,0,6.6E-4,5.2308576786895683E-2,3.283424646564674E-4,9.9549021306263211E-2,9.9882611083351586E-2,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,1.605858665261407E-2,7.7363461583854429E-7,7.7363461583854429E-7,1.6922431476106101E-2,1.9673528801262898E-4,1.2102016980535017E-3,40,107.95832742455175,6.4487920520053935E-2,5.5557752673778688E-2,0.12125587489188612,0.12145702953863674,4.9370830427385271E-2,7.4099358471524791E-4,3.3156210905575393E-3,1.3395251769412868E-3,4.955425542010586E-4,5.150688821699884E-3,5.892489953092119E-3,3.1732432885906041E-2,7.0654508867960986E-2,4.5258227886110407E-3,0.20252985114830088,0.30241391180229565,0.255,0.45746974483558239,3.6087123498626669E-4,1.3307904874382435E-3,7.7945486918661905E-2,0.21753291822198606,2.4031068270437992E-3,8.8900284637463147E-4,9.2403305921197349E-3,5.8904605303953085E-4,0.17859084461022817,1.3878997266809124E-6,1.2126285566990852E-6,0.12675411820905688,0.61563911652921866,0.45746974483558239,45.74697448355824,51.000000000000007,70.206518151218702,0.702065181512187,301.42009914159445,null,9.9670552703184048E-2,null,0.20252985114830088,7.0654508867960986E-2,9.9882611083351586E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR57, IF(MODE_ILIM=4,#REF!,#REF!))","v":45.74697448355824},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ57, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.20252985114830088},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA57, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0654508867960986E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB57, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.9882611083351586E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S57, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.42009914159445},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P57, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54747630321702723}]
[null,null,null,null,null,null,null,52,5.2000000000000005E-2,4.0313472222222216E-2,7.2161161330666607E-2,3.1850898112422046E-2,0.54746601864356481,0.54746601864356481,1,0.54746601864356481,2.9700999915218293E-6,0.10466942909062017,301447.95578098617,3.3173222137440515E-6,0,6.5999999999999989E-4,5.3284023923410313E-2,3.4070246465646746E-4,9.9558221426614274E-2,9.990436991768048E-2,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,1.6357014390708052E-2,8.0265575933349104E-7,8.0265575933349104E-7,1.7238796474174093E-2,2.0415998336418406E-4,1.2103135424606595E-3,40,106.4617862297607,6.4783270401529702E-2,5.5562887209551368E-2,0.12155647115354173,0.12176522891754193,5.0293818515404924E-2,7.6895832698158811E-4,3.3159275135908484E-3,1.3830574787967495E-3,5.0535888239013028E-4,5.2043438747777287E-3,5.9741518387191883E-3,3.1732432885906034E-2,7.0658105967948998E-2,4.5262410560515075E-3,0.20292372778026163,0.30282957628972879,0.26,0.46195155861205012,3.7090759404715019E-4,1.3677461106720236E-3,7.7202613310652757E-2,0.21597385118753581,2.4573290691546571E-3,8.9788970530217075E-4,9.2467490942563374E-3,6.0533859450393097E-4,0.17688875215641564,1.4261079963578644E-6,1.2009603898371824E-6,0.12554085454026706,0.61055465843119372,0.46195155861205012,46.195155861205009,52.000000000000007,70.411746141009829,0.70411746141009823,301.44795578098615,null,9.8720624413222297E-2,null,0.20292372778026163,7.0658105967948998E-2,9.990436991768048E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR58, IF(MODE_ILIM=4,#REF!,#REF!))","v":46.195155861205009},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ58, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.20292372778026163},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA58, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0658105967948998E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB58, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.990436991768048E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S58, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.44795578098615},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P58, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54746601864356481}]
[null,null,null,null,null,null,null,53,5.3000000000000005E-2,4.0312714902402388E-2,7.316116161743326E-2,3.2851276772440541E-2,0.54745573407010228,0.54745573407010228,1,0.54745573407010228,2.9697934630375011E-6,0.1046791016892748,301475.81286511151,3.3170156852597234E-6,0,6.6E-4,5.4260364958877323E-2,3.5330246465646744E-4,9.9567421693846012E-2,9.9926372835911617E-2,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,1.6655769340364158E-2,8.3224395695824419E-7,8.3224395695824419E-7,1.7555479824650614E-2,2.1172987697724204E-4,1.2104253886534228E-3,40,105.00616848727394,6.5078673863756403E-2,5.5568021827297351E-2,0.12185712107970717,0.12207363129181575,5.1217735389739956E-2,7.9746995120983993E-4,3.316233941516227E-3,1.4265978054688573E-3,5.1517942892447997E-4,5.2580111759095646E-3,6.0563743943002303E-3,3.1732432885906041E-2,7.066170312536503E-2,4.52665933016965E-3,0.20331836814165066,0.30324624915754661,0.26500000000000001,0.46634711692840158,3.810147668014896E-4,1.4049599439930819E-3,7.6473764031094307E-2,0.21444421544421352,2.5105274475350427E-3,9.0661298633868531E-4,9.2530503874065657E-3,6.2174183319336628E-4,0.1752187926298848,1.4645832826738186E-6,1.1895125191849797E-6,0.12435049633873435,0.60556782990499713,0.46634711692840158,46.634711692840156,53.000000000000007,70.596901007914624,0.70596901007914625,301.47581286511149,null,9.7788629330470223E-2,null,0.20331836814165066,7.066170312536503E-2,9.9926372835911617E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR59, IF(MODE_ILIM=4,#REF!,#REF!))","v":46.634711692840156},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ59, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.20331836814165066},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA59, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.066170312536503E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB59, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.9926372835911617E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S59, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.47581286511149},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P59, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54745573407010228}]
[null,null,null,null,null,null,null,54,5.4000000000000006E-2,4.0311957582582575E-2,7.4161161904199913E-2,3.3851655432459042E-2,0.54744544949663976,0.54744544949663976,1,0.54744544949663976,2.9694869863034298E-6,0.1046887744423545,301503.67039398104,3.3167092085256524E-6,0,6.6E-4,5.5237552493485463E-2,3.661424646564674E-4,9.9576622107961962E-2,9.9948619842059702E-2,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,1.6954835557141078E-2,8.6239934630908619E-7,8.6239934630908619E-7,1.7872466229787807E-2,2.1944500875568015E-4,1.2105372366318339E-3,40,103.5898182388938,6.5374130908017164E-2,5.5573156527018587E-2,0.12215782467166758,0.12238223672925166,5.2142536419539483E-2,8.2652860769595236E-4,3.3165403743337916E-3,1.4701461571497872E-3,5.2500419451595079E-4,5.3116907259995296E-3,6.1391578050533158E-3,3.1732432885906041E-2,7.066530034021043E-2,4.5270776109656253E-3,0.20371377248548103,0.30366393066291442,0.27,0.47065883972867789,3.9119080979129633E-4,1.4424247975597525E-3,7.5758545626266896E-2,0.21294318527313452,2.5627306835396047E-3,9.1517727793913512E-4,9.2592377559130266E-3,6.3825254663189401E-4,0.17358006453864588,1.5033180582096472E-6,1.1782787643136477E-6,0.12318240098963698,0.60067589189588166,0.47065883972867789,47.065883972867788,54.000000000000007,70.763841860106652,0.70763841860106647,301.50367039398105,null,9.6874064337284321E-2,null,0.20371377248548103,7.066530034021043E-2,9.9948619842059702E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR60, IF(MODE_ILIM=4,#REF!,#REF!))","v":47.065883972867788},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ60, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.20371377248548103},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA60, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.066530034021043E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB60, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.9948619842059702E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S60, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.50367039398105},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P60, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54744544949663976}]
[null,null,null,null,null,null,null,55,5.5000000000000007E-2,4.0311200262762754E-2,7.5161162190966566E-2,3.4852034092477543E-2,0.54743516492317734,0.54743516492317734,1,0.54743516492317734,2.9691805613065103E-6,0.104698447349863,301531.52836760553,3.3164027835287325E-6,0,6.6E-4,5.6215542383495354E-2,3.7922246465646751E-4,9.9585822668965665E-2,9.997111094019577E-2,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,1.7254198184596045E-2,8.931220649799525E-7,8.931220649799525E-7,1.8189741442573348E-2,2.2730541860464955E-4,1.2106490863959363E-3,40,102.21116768132948,6.5669641535595194E-2,5.5578291308717047E-2,0.12245858193070819,0.12269104529768679,5.3068180039451004E-2,8.5613444674067412E-4,3.3168468120436615E-3,1.5137025340317221E-3,5.348331798764092E-4,5.3653825259517927E-3,6.2225022565549903E-3,3.1732432885906041E-2,7.0668897612486584E-2,4.5274958984395982E-3,0.20410994106516794,0.30408262106345607,0.27500000000000002,0.47488905727299563,4.0143385161809069E-4,1.4801337484954054E-3,7.5056579223877859E-2,0.21146996555658873,2.6139664341020691E-3,9.2358699850845973E-4,9.2653143623936379E-3,6.5486763177255176E-4,0.17197169980007571,1.5423050744292391E-6,1.1672531738415606E-6,0.12203594969351128,0.59587620685919207,0.47488905727299563,47.48890572729956,55.000000000000007,70.914272258910415,0.70914272258910416,301.53152836760552,null,9.5976444961602042E-2,null,0.20410994106516794,7.0668897612486584E-2,9.997111094019577E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR61, IF(MODE_ILIM=4,#REF!,#REF!))","v":47.48890572729956},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ61, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.20410994106516794},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA61, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0668897612486584E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB61, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.997111094019577E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S61, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.53152836760552},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P61, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54743516492317734}]
[null,null,null,null,null,null,null,56,5.6000000000000008E-2,4.0310442942942934E-2,7.6161162477733232E-2,3.5852412752496038E-2,0.54742488034971482,0.54742488034971482,1,0.54742488034971482,2.9688741880336433E-6,0.104708120411804,301559.38678599556,3.3160964102558656E-6,0,6.5999999999999989E-4,5.7194293469458667E-2,3.925424646564675E-4,9.9595023376860617E-2,9.9993846134447006E-2,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,1.7553843364179315E-2,9.2441225056242655E-7,9.2441225056242655E-7,1.8507292179029439E-2,2.3531114643057544E-4,1.2107609379457722E-3,40,100.86873137708646,6.5965205747773703E-2,5.5583426172394701E-2,0.12275939285811417,0.12300005706500175,5.3994627493754561E-2,8.8628761864955208E-4,3.3171532546459517E-3,1.5572669363068514E-3,5.4466638571774384E-4,5.4190865766705464E-3,6.3064079347406174E-3,3.1732432885906034E-2,7.0672494942194852E-2,4.5279141925917239E-3,0.20450687413452892,0.30450232061725385,0.28000000000000003,0.47904001425402504,4.1174208963521076E-4,1.5180801286349555E-3,7.436749986377629E-2,0.21002379037345165,2.6642613405919854E-3,9.3184640420684384E-4,9.2712832533287642E-3,6.7158409951551532E-4,0.17039286220743308,1.5815373488786433E-6,1.1564300149210665E-6,0.12091054637313046,0.5911662341010685,0.47904001425402504,47.904001425402505,56.000000000000007,71.049749591014816,0.71049749591014821,301.55938678599557,null,9.5095304521112506E-2,null,0.20450687413452892,7.0672494942194852E-2,9.9993846134447006E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR62, IF(MODE_ILIM=4,#REF!,#REF!))","v":47.904001425402505},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ62, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.20450687413452892},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA62, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0672494942194852E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB62, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.9993846134447006E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S62, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.55938678599557},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P62, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54742488034971482}]
[null,1500,null,null,null,"Eff (%)","Iout (mA)",57,5.6999999999999995E-2,4.0309685623123113E-2,7.7161162764499872E-2,3.6852791412514518E-2,0.5474145957762524,0.5474145957762524,1,0.5474145957762524,2.9685678664717325E-6,0.10471779362818118,301587.24564916187,3.3157900886939552E-6,0,6.600000000000001E-4,5.8173767330907504E-2,4.0610246465646731E-4,9.9604224231650357E-2,0.10001682542899704,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,1.7853758153824315E-2,9.5627004064574468E-7,9.5627004064574468E-7,1.8825106039053203E-2,2.4346223214115741E-4,1.210872791281385E-3,40,99.561100915645412,6.6260823545835984E-2,5.5588561118053513E-2,0.12306025745517088,0.12330927209912086,5.4921842605416313E-2,9.1698827373293322E-4,3.3174597021407804E-3,1.60083936416737E-3,5.5450381275186627E-4,5.4728028790600172E-3,6.3908750259047426E-3,3.1732432885906048E-2,7.0676092329336665E-2,4.5283324934221655E-3,0.20490457194778444,0.30492302958284945,0.28499999999999998,0.48311387368879494,4.2211378682074403E-4,1.5562575129401527E-3,7.3690955865196542E-2,0.20860392167125619,2.7136410750049321E-3,9.3995959632898367E-4,9.2771473643434195E-3,6.8839906952544868E-4,0.16884274598006996,1.6210081530838847E-6,1.1458037632990555E-6,0.11980561664004478,0.58654352537344756,0.48311387368879494,48.311387368879494,56.999999999999993,71.171694607053283,0.71171694607053282,301.58724564916184,null,9.4230193314137414E-2,null,0.20490457194778444,7.0676092329336665E-2,0.10001682542899704,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR63, IF(MODE_ILIM=4,#REF!,#REF!))","v":48.311387368879494},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ63, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.20490457194778444},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA63, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0676092329336665E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB63, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10001682542899704},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S63, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.58724564916184},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P63, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.5474145957762524}]
[null,null,null,null,null,{"$f":"BR56","v":45.289916161460347},{"$f":"I56*1000","v":50},58,5.7999999999999996E-2,4.0308928303303293E-2,7.8161163051266525E-2,3.7853170072533027E-2,0.54740431120278987,0.54740431120278987,1,0.54740431120278987,2.9682615966076882E-6,0.10472746699899825,301615.10495711502,3.3154838188299104E-6,0,6.6E-4,5.9153928064588926E-2,4.1990246465646737E-4,9.9613425233338382E-2,0.10004004882808561,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,1.8153930454282641E-2,9.8869557281679237E-7,9.8869557281679237E-7,1.9143171434854653E-2,2.5175871564536955E-4,1.2109846464028167E-3,40,98.286939984591257,6.6556494931065302E-2,5.559369614569544E-2,0.12336117572316356,0.12361869046801205,5.5849791567307794E-2,9.4823656230596436E-4,3.3177661545282654E-3,1.6444198178054798E-3,5.6434546169071079E-4,5.5265314340244565E-3,6.4759037167014446E-3,3.1732432885906041E-2,7.067968977391334E-2,4.5287508009310817E-3,0.20530303475955791,0.30534474821924368,0.28999999999999998,0.48711272060000371,4.3254726881987302E-4,1.5946597085414603E-3,7.3026608228225737E-2,0.20720964801008734,2.7621303836544474E-3,9.4793052828423205E-4,9.2829095252037683E-3,7.0530976532916809E-4,0.16732057439205697,1.6607110011033338E-6,1.1353690939151217E-6,0.11872060681701789,0.58200572070731593,0.48711272060000371,48.711272060000368,57.999999999999993,71.281400919850697,0.71281400919850701,301.61510495711502,null,9.3380677854274646E-2,null,0.20530303475955791,7.067968977391334E-2,0.10004004882808561,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR64, IF(MODE_ILIM=4,#REF!,#REF!))","v":48.711272060000368},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ64, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.20530303475955791},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA64, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.067968977391334E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB64, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10004004882808561},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S64, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.61510495711502},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P64, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54740431120278987}]
[null,null,null,null,null,{"$f":"BR81","v":54.532073534553106},{"$f":"I81*1000","v":75.000000000000014},59,5.8999999999999997E-2,4.0308170983483473E-2,7.9161163338033178E-2,3.8853548732551521E-2,0.54739402662932746,0.54739402662932746,1,0.54739402662932746,2.9679553784284237E-6,0.10473714052425889,301642.96470986569,3.3151776006506459E-6,0,6.6E-4,6.0134742083678729E-2,4.3394246465646737E-4,9.9622626381928203E-2,0.10006351633600885,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,1.845434894236862E-2,1.0216889846601054E-6,1.0216889846601054E-6,1.9461477526164277E-2,2.6020063685345992E-4,1.2110965033101107E-3,40,97.0449798144315,6.6852219904745019E-2,5.5598831255322445E-2,0.12366214766337758,0.12392831223968701,5.6778442753175527E-2,9.8003263468859165E-4,3.3180726118085227E-3,1.6880082974133884E-3,5.7419133324623447E-4,5.5802722424681452E-3,6.5614941941446927E-3,3.1732432885906041E-2,7.0683287275926293E-2,4.5291691151186329E-3,0.20570226282487664,0.3057674767858975,0.29499999999999998,0.49103856549999725,4.4304092114541381E-4,1.6332807443673204E-3,7.237413006735445E-2,0.20584028337380936,2.8097531285219083E-3,9.5576301220258258E-4,9.2885724645457995E-3,7.2231350967608468E-4,0.16582559847431935,1.7006396386937182E-6,1.1251208720036955E-6,0.11765498301286459,0.57755054446931753,0.49103856549999725,49.103856549999726,59,71.3800443047935,0.713800443047935,301.64296470986568,null,9.2546340146067607E-2,null,0.20570226282487664,7.0683287275926293E-2,0.10006351633600885,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR65, IF(MODE_ILIM=4,#REF!,#REF!))","v":49.103856549999726},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ65, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.20570226282487664},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA65, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0683287275926293E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB65, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10006351633600885},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S65, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.64296470986568},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P65, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54739402662932746}]
[null,null,null,null,null,{"$f":"BR106","v":60.681661652833171},{"$f":"I106*1000","v":100},60,0.06,4.0307413663663652E-2,8.016116362479983E-2,3.9853927392570015E-2,0.54738374205586493,0.54738374205586493,1,0.54738374205586493,2.967649211920857E-6,0.10474681420396682,301670.82490742451,3.3148714341430793E-6,0,6.6E-4,6.111617793571978E-2,4.4822246465646735E-4,9.9631827677423374E-2,0.10008722795711913,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,1.8755003010378048E-2,1.0552504137578691E-6,1.0552504137578691E-6,1.978001416148277E-2,2.687880356769513E-4,1.2112083620033096E-3,40,95.834014964462483,6.7147998468158554E-2,5.5603966446936486E-2,0.12396317327709835,0.12423813748220111,5.7707766546238264E-2,1.0123766412055615E-3,3.31837907398167E-3,1.7316048031833086E-3,5.8404142813041685E-4,5.6340253052953957E-3,6.6476466456087038E-3,3.1732432885906041E-2,7.0686884835376856E-2,4.5295874359849797E-3,0.20610225639917165,0.30619121554273188,0.3,0.49489334768964877,4.5359318652708834E-4,1.6721148613244058E-3,7.1733206075122541E-2,0.20449516604445073,2.8565323264095432E-3,9.6346072518968464E-4,9.2941388143527801E-3,7.3940772014514803E-4,0.16435709578572752,1.7407880330517294E-6,1.1150541446689121E-6,0.11660823024644107,0.57317580162786819,0.49489334768964877,49.489334768964873,60,71.468691685531624,0.71468691685531627,301.6708249074245,null,9.1726776999157683E-2,null,0.20610225639917165,7.0686884835376856E-2,0.10008722795711913,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR66, IF(MODE_ILIM=4,#REF!,#REF!))","v":49.489334768964873},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ66, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.20610225639917165},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA66, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0686884835376856E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB66, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10008722795711913},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S66, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.6708249074245},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P66, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54738374205586493}]
[null,null,null,null,null,null,null,61,6.0999999999999999E-2,4.0306656343843832E-2,8.1161163911566497E-2,4.0854306052588517E-2,0.54737345748240251,0.54737345748240251,1,0.54737345748240251,2.96734309707191E-6,0.10475648803812572,301698.68554980215,3.3145653192941323E-6,0,6.6E-4,6.2098206137299661E-2,4.6274246465646731E-4,9.9641029119827362E-2,0.10011118369582513,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,1.9055882711032812E-2,1.0893799976899177E-6,1.0893799976899177E-6,2.0098771824732235E-2,2.7752095202864083E-4,1.2113202224824557E-3,40,94.652899420260511,6.7443830622589268E-2,5.5609101720539532E-2,0.12426425256561124,0.12454816626365346,5.8637735183543108E-2,1.04526873218642E-3,3.3186855410478238E-3,1.7752093353074611E-3,5.9389574705526063E-4,5.6877906234105453E-3,6.7343612588282959E-3,3.1732432885906041E-2,7.0690482452266445E-2,4.5300057635302791E-3,0.20650301573827848,0.30661596475012864,0.30499999999999999,0.49867893838350924,4.6420256240075242E-4,1.7111565029950119E-3,7.1103532014010498E-2,0.2031736575358665,2.9024901860315402E-3,9.7102721525245417E-4,9.2996111141968821E-3,7.5658990498313336E-4,0.1629143692489044,1.7811503630958621E-6,1.1051641329031653E-6,0.11557985161676827,0.5688793742159054,0.49867893838350924,49.867893838350923,61,71.54830972155635,0.71548309721556347,301.69868554980212,null,9.092159937855486E-2,null,0.20650301573827848,7.0690482452266445E-2,0.10011118369582513,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR67, IF(MODE_ILIM=4,#REF!,#REF!))","v":49.867893838350923},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ67, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.20650301573827848},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA67, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0690482452266445E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB67, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10011118369582513},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S67, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.69868554980212},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P67, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54737345748240251}]
[null,null,null,null,null,null,null,62,6.2E-2,4.0305899024024018E-2,8.216116419833315E-2,4.1854684712607018E-2,0.5473631729089401,0.5473631729089401,1,0.5473631729089401,2.9670370338685104E-6,0.1047661620267393,301726.54663700925,3.3142592560907327E-6,0,6.6E-4,6.3080799023716896E-2,4.7750246465646753E-4,9.9650230709143708E-2,0.10013538355659179,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,1.935697870737868E-2,1.1240778740337347E-6,1.1240778740337347E-6,2.0417741586744035E-2,2.8639942582260006E-4,1.2114320847475921E-3,40,93.500542976240993,6.7739716369320677E-2,5.5614237076133541E-2,0.12456538553020181,0.12485839865218711,5.9568322614432297E-2,1.0787090579655141E-3,3.3189920130071021E-3,1.8188218939780708E-3,6.0375429073279078E-4,5.7415681977179634E-3,6.8216382218992538E-3,3.1732432885906041E-2,7.069408012659642E-2,4.530424097754694E-3,0.20690454109843748,0.30704172466893065,0.31,0.50239714367181298,4.7486759852829362E-4,1.750400306820085E-3,7.0484814234856544E-2,0.2018751415830696,2.9476481431688381E-3,9.7846590691534011E-4,9.3049918152594332E-3,7.7385765916019396E-4,0.16149674604680964,1.8217210102555882E-6,1.0954462240223345E-6,0.11456936751647846,0.56465921797830076,0.50239714367181298,50.2397143671813,62,71.619772941093288,0.71619772941093285,301.72654663700922,null,9.0130431788827528E-2,null,0.20690454109843748,7.069408012659642E-2,0.10013538355659179,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR68, IF(MODE_ILIM=4,#REF!,#REF!))","v":50.2397143671813},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ68, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.20690454109843748},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA68, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.069408012659642E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB68, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10013538355659179},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S68, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.72654663700922},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P68, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.5473631729089401}]
[null,null,null,null,null,null,null,63,6.3E-2,4.0305141704204198E-2,8.3161164485099803E-2,4.2855063372625513E-2,0.54735288833547757,0.54735288833547757,1,0.54735288833547757,2.9667310222975881E-6,0.10477583616981126,301754.40816905652,3.3139532445198103E-6,0,6.6E-4,6.4063930612089065E-2,4.925024646564674E-4,9.9659432445375964E-2,0.10015982754394043,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,1.9658282227129717E-2,1.1593441803644523E-6,1.1593441803644523E-6,2.073691506108416E-2,2.9542349697417531E-4,1.211543948798762E-3,40,92.375907879283162,6.8035655709636308E-2,5.5619372513720497E-2,0.12486657217215556,0.12516883471598883,6.0499504371664722E-2,1.1126977688819919E-3,3.3192984898596221E-3,1.8624424793873713E-3,6.1361705987505555E-4,5.795358029122049E-3,6.9094777232786824E-3,3.1732432885906041E-2,7.0697677858368141E-2,4.5308424386583841E-3,0.20730683273629405,0.3074684955604422,0.315,0.50604970732918519,4.855868947409527E-4,1.7898410957385576E-3,6.9876769220197393E-2,0.20059902318386635,2.992026894004512E-3,9.8578010654592672E-4,9.3102832841430363E-3,7.912086606295482E-4,0.16010357657642924,1.8624945497372225E-6,1.0858959644925114E-6,0.11357631488596892,0.56051335919277867,0.50604970732918519,50.604970732918517,63,71.68387138413388,0.71683871384133879,301.75440816905655,null,8.935291169016249E-2,null,0.20730683273629405,7.0697677858368141E-2,0.10015982754394043,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR69, IF(MODE_ILIM=4,#REF!,#REF!))","v":50.604970732918517},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ69, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.20730683273629405},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA69, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0697677858368141E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB69, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10015982754394043},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S69, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.75440816905655},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P69, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54735288833547757}]
[null,null,null,null,null,null,null,64,{"$f":"IF(PLOT_TYPE=1, H70/100*Iout, min_I*EXP(H70*rr/100))","v":6.4000000000000001E-2},{"$f":"IF(I70<Icrit, (Vin-(Rdcr+RdsonTop)*Iripple/2-Vout)/L*OnTime, (Vin-(Rdcr+RdsonTop)*I70-Vout)/L*OnTime)","v":4.0304384384384377E-2},{"$f":"IF(I70<Icrit, (Vin-(Rdcr+RdsonTop)*Iripple/2-Vout)/L*OnTime, I70+((Vin-(Rdcr+RdsonTop)*J70-Vout)/L*OnTime)/2)","v":8.4161164771866456E-2},{"$f":"IF(I70<Icrit, 0, I70-((Vin-(Rdcr+RdsonTop)*K70-Vout)/L*OnTime)/2)","v":4.3855442032644007E-2},0.54734260376201516,{"$f":"IF(I70<Icrit, 1000*SQRT((J70*CoutEsr)^2+(((J70/2)-I70)*(OnTime+OffTime)/Cout)^2), 1000*J70*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":0.54734260376201516},1,{"$f":"IF(I70<Icrit, 1000*((N70/1000)*O70), 1000*J70*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":0.54734260376201516},{"$f":"IF(I70<Icrit, L*J70/(Vout+J70/2*(RdsonBot+Rdcr)), L*J70/(Vout+I70*(RdsonBot+Rdcr)))","v":2.9664250623460796E-6},0.10478551046734531,{"$f":"IF(I70<Icrit,I70/((OnTime+Q70)*J70/2),1/(OnTime+Q70))","v":301782.27014595456},3.3136472845683019E-6,0,{"$f":"S70*(T70*Iq_active+U70*Iq_sleep)","v":6.600000000000001E-4},6.5047576476534169E-2,{"$f":"W70^2*Rdcr","v":5.0774246465646732E-4},{"$f":"Core_Loss/1000*S70/$S$106","v":9.96686343285276E-2},{"$f":"(Y70+X70*(1+Ltc*(Ta-25)))/(1-X70*Ltc*ThetaCa)","v":0.10018451566244853},1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,1.9959785021010368E-2,1.1951790542548496E-6,1.1951790542548496E-6,2.1056284363774467E-2,3.0459320539998747E-4,1.2116558146360076E-3,{"$f":"20*VIN_nom/24","v":40},{"$f":"IF(I70<Icrit, Csw*Vin/Iripple*1000000000, Csw*Vin/(I70+Iripple/2)*1000000000)","v":91.278005711701283},{"$f":"IF(I70<Icrit, Vin*(I70+Iripple/2)*AK70/1000000000/2*S70, Vin*(I70-Iripple/2)*AJ70/1000000000/2*S70 + Vin*(I70+Iripple/2)*AK70/1000000000/2*S70)","v":6.8331648644819679E-2},{"$f":"IF(I70<Icrit, Csw*(Vin)^2*S70/2, Csw*Vin^2*S70/2)","v":5.5624508033302343E-2},0.12516781249275802,{"$f":"(AI70+AL70+AM70+AH70*(1+RdsonTopTc*(Ta-25)))/(1-AH70*RdsonTopTc*ThetaJA)","v":0.12547947452328928},{"$f":"IF(I70<Icrit,Iripple*SQRT((OffTime)*S70/3), SQRT(OffTime*S70*(I70^2+Iripple^2/12)))","v":6.1431257453903432E-2},1.1472350152798008E-3,{"$f":"QgBot*S70*Vdd","v":3.3196049716055004E-3},{"$f":"IF(I70<Icrit, Vin*Idss*R70, QrrBot*(I70-Iripple/2)/1*S70*Vin+Vin*Idss*R70)","v":1.9060710917275995E-3},{"$f":"IF(I70<Icrit, dead1*S70*(I70+Iripple/2)*((I70+Iripple/2)*BDserR+VSD), dead1*S70*(I70+Iripple/2)*((I70+Iripple/2)*BDserR+VSD)+dead2*S70*(I70-Iripple/2)*((I70-Iripple/2)*BDserR+VSD))","v":6.2348405519412542E-4},5.8491601185272253E-3,{"$f":"(AR70+AS70+AT70+AQ70*(1+RdsonBotTc*(Ta-25)))/(1-AQ70*RdsonBotTc*ThetaJA)","v":6.9978799517853617E-3},{"$f":"Vin*V70+Vout*Ifb/0.8","v":3.1732432885906048E-2},{"$f":"(Vin-Vdd)*(S70*QgBot+S70*QgTop)+AW70","v":7.0701275647583023E-2},{"$f":"AI70+AR70","v":4.5312607862415082E-3},0.20770989090889916,{"$f":"SUM(Z70,AC70,AF70,AZ70)","v":0.3078962776864293},{"$f":"Vout*I70","v":0.32},0.50963831347923305,4.9635909879833045E-4,1.8294738702556951E-3,{"$f":"Vin*S70*(QgBot+QgTop)/($BB70+$BA70)","v":6.9279123151041164E-2},0.19934472768966896,3.0356464267486697E-3,9.9297300740727214E-4,9.3154878064881427E-3,{"$f":"X70/($BB70+$BA70)","v":8.0864066677909712E-4},{"$f":"Y70/($BB70+$BA70)","v":0.15873423345615373},1.9034657422379571E-6,1.076509053124807E-6,0.11260024650582681,0.55643989165396324,{"$f":"BC70","v":0.50963831347923305},50.963831347923303,{"$f":"I70*1000","v":64},71.741317737155555,0.71741317737155552,{"$f":"S70/1000","v":301.78227014595456},null,{"$f":"AM70/($BB70+$BA70)","v":8.8588688944388302E-2},null,0.20770989090889916,7.0701275647583023E-2,0.10018451566244853,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR70, IF(MODE_ILIM=4,#REF!,#REF!))","v":50.963831347923303},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ70, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.20770989090889916},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA70, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0701275647583023E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB70, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10018451566244853},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S70, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.78227014595456},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P70, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54734260376201516}]
[null,null,null,null,null,null,null,65,6.5000000000000002E-2,4.0303627064564557E-2,8.5161165058633109E-2,4.4855820692662501E-2,{"$f":"IF(I71<Icrit, 1000*((((J71/2)-I71)*0.000002/Cout+Vout/306)), 1000*J71*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":0.54733231918855274},0.54733231918855274,{"$f":"ROUNDUP(M71/N71,0)","v":1},0.54733231918855274,2.9661191540009238E-6,0.10479518491934514,301810.13256771408,{"$f":"IF(1/S71-OnTime-Q71>Tsleep, OnTime+Q71+Tsleep, 1/S71)","v":3.3133413762231464E-6},{"$f":"IF(1/S71-OnTime-Q71>Tsleep, 1/S71-OnTime-Q71-Tsleep, 0)","v":0},6.600000000000001E-4,{"$f":"IF(I71<Icrit,Iripple*SQRT((OnTime+OffTime)*S71/3), SQRT(I71^2+Iripple^2/12))","v":6.6031713634211869E-2},5.2322246465646733E-4,9.9677836358602181E-2,0.10020944791674999,{"$f":"Iripple/SQRT(12)*SQRT((OnTime+Q71)*S71)","v":1.1627003288490194E-2},{"$f":"RCoutEsr*AA71^2","v":6.7593602735280891E-7},6.7593602735280891E-7,{"$f":"SQRT($R71)*SQRT($I71^2*(1-R71)+(Iripple^2)/12)","v":2.0261479324696862E-2},{"$f":"RCinEsr*AD71^2","v":1.2315826332753554E-6},1.2315826332753554E-6,{"$f":"IF(I71<Icrit,Iripple*SQRT((OnTime)*S71/3), SQRT(OnTime*S71*(I71^2+Iripple^2/12)))","v":2.1375842076518301E-2},{"$f":"RdsonTop*AG71^2","v":3.1390859101793197E-4},{"$f":"QgTop*S71*Vdd","v":1.2117676822593721E-3},40,90.205894493883349,6.8627695176154413E-2,5.5629643634881057E-2,{"$f":"AI71+AL71+AM71","v":0.12546910649329485},0.12579031814236308,6.2363560218427282E-2,{"$f":"RdsonBot*AP71^2","v":1.1823209475076914E-3},3.3199114582448553E-3,1.9497077311910009E-3,6.3335527740209408E-4,{"$f":"AR71+AS71+AT71","v":5.9029744668379503E-3},7.086845096600119E-3,3.1732432885906048E-2,7.0704873494242398E-2,4.5316791405042274E-3,0.20811371587370983,0.30832507130912046,0.32500000000000001,0.51316458912356921,{"$f":"(AO71-AN71)/($BB71+$BA71)","v":5.0718290435631727E-4},{"$f":"(AV71-AU71)/($BB71+$BA71)","v":1.8692938009149673E-3},6.8691611495681024E-2,{"$f":"AN71/($BB71+$BA71)","v":0.19811169994256309},{"$f":"AS71/(BA71+BB71)","v":3.0785260516543885E-3},{"$f":"AT71/($BB71+$BA71)","v":1.0000476944531994E-3},{"$f":"AU71/($BB71+$BA71)","v":9.3206075904055906E-3},8.2615151106356084E-4,0.15738811058365679,{"$f":"(AF71)/($BB71+$BA71)","v":1.9446295260814496E-6},{"$f":"(AC71)/($BB71+$BA71)","v":1.0672813346163748E-6},{"$f":"AX71/($BB71+$BA71)","v":0.11164073032525182},{"$f":"SUM(BD71:BO71)","v":0.55243697381086143},0.51316458912356921,51.316458912356921,65,71.792753953912452,{"$f":"BT71/100","v":0.71792753953912447},301.81013256771411,null,8.7837425289182508E-2,null,{"$f":"AZ71","v":0.20811371587370983},{"$f":"AX71","v":7.0704873494242398E-2},{"$f":"Z71","v":0.10020944791674999},null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR71, IF(MODE_ILIM=4,#REF!,#REF!))","v":51.316458912356921},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ71, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.20811371587370983},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA71, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0704873494242398E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB71, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10020944791674999},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S71, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.81013256771411},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P71, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54733231918855274}]
[null,null,null,null,null,null,null,66,6.6000000000000003E-2,4.0302869744744736E-2,8.6161165345399762E-2,4.5856199352681003E-2,0.5473220346150901,0.5473220346150901,1,0.5473220346150901,2.965813297249067E-6,{"$f":"OnTime*S72","v":0.10480485952581445},301837.99543434568,3.3130355194712892E-6,0,6.6E-4,6.7016320441147484E-2,5.3894246465646743E-4,9.9687038535603179E-2,0.1002346243115349,1.1627003288490194E-2,6.7593602735280891E-7,{"$f":"AB72","v":6.7593602735280891E-7},2.0563357824003703E-2,1.268555054994043E-6,{"$f":"AE72","v":1.268555054994043E-6},2.1695581213082939E-2,3.2336969374717895E-4,1.211879551668898E-3,40,89.158675988745955,6.8923795304924096E-2,5.5634779318458595E-2,0.12577045417505159,0.12610136564152866,6.3296392283052297E-2,1.217955715919213E-3,3.3202179497778027E-3,1.9933523979698249E-3,6.4323072721107755E-4,5.9568010749587053E-3,7.1763733472661774E-3,3.1732432885906041E-2,7.0708471398347669E-2,4.5320975014467007E-3,{"$f":"AO72+AV72+AX72+AY72","v":0.20851830788858919},0.30875487669120644,0.33,0.51663010654325237,5.1805704903767197E-4,1.9092962211497142E-3,6.8113978619252863E-2,0.19689940345590951,3.1206844295193887E-3,1.0070071488816749E-3,9.3256447697359877E-3,8.4373909980652658E-4,0.15606462224130294,1.985981009750163E-6,1.058208793417286E-6,0.11069734882436021,0.54850282604875955,0.51663010654325237,{"$f":"100*BQ72","v":51.663010654325234},66,71.838757366287027,0.71838757366287032,301.83799543434566,null,8.7098793838804839E-2,null,0.20851830788858919,7.0708471398347669E-2,0.1002346243115349,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR72, IF(MODE_ILIM=4,#REF!,#REF!))","v":51.663010654325234},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ72, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.20851830788858919},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA72, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0708471398347669E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB72, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.1002346243115349},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S72, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.83799543434566},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P72, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.5473220346150901}]
[null,null,null,null,null,null,null,67,6.7000000000000004E-2,4.0302112424924916E-2,8.7161165632166429E-2,4.6856578012699504E-2,0.54731175004162769,0.54731175004162769,1,0.54731175004162769,2.9655074920774568E-6,0.10481453428675691,301865.85874585999,3.3127297142996791E-6,0,6.6E-4,6.8001376496881025E-2,5.5490246465646762E-4,9.9696240859534144E-2,0.10026004485154975,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,2.0865413623000102E-2,1.3060964569766348E-6,1.3060964569766348E-6,2.2015495188529757E-2,3.3297655350817356E-4,1.211991422864628E-3,40,88.135493191793415,6.9219949032412437E-2,5.5639915084036914E-2,0.12607185553931399,0.12641261708914858,6.4229734436361444E-2,1.2541394708727167E-3,3.3205244462044606E-3,2.037005092256329E-3,6.5311040533321452E-4,6.0106399437940038E-3,7.2664648936895219E-3,3.1732432885906041E-2,7.0712069359900209E-2,4.5325158690690884E-3,0.20892366721180738,0.30918569409584146,0.33500000000000002,{"$f":"BB73/(BB73+BA73)","v":0.52003638558008547},5.2898031259894951E-4,1.9494766204924095E-3,6.754597741282585E-2,0.19570731963593888,3.1621395987618205E-3,1.0138542524603864E-3,9.3306014071460348E-3,8.6140140916247921E-4,0.15476320224630977,2.027515464791298E-6,1.0492875479042285E-6,0.10976969840839049,0.5446357281070997,0.52003638558008547,52.003638558008547,67,71.879846296152991,0.71879846296152994,301.86585874586001,null,8.6372478609807263E-2,null,0.20892366721180738,7.0712069359900209E-2,0.10026004485154975,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR73, IF(MODE_ILIM=4,#REF!,#REF!))","v":52.003638558008547},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ73, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.20892366721180738},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA73, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0712069359900209E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB73, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10026004485154975},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S73, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.86585874586001},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P73, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54731175004162769}]
[null,null,null,null,null,null,null,68,6.8000000000000005E-2,4.0301355105105095E-2,8.8161165918933082E-2,4.7856956672717998E-2,0.54730146546816527,0.54730146546816527,1,0.54730146546816527,2.9652017384730456E-6,0.10482420920217629,301893.7225022678,3.3124239606952679E-6,0,6.6E-4,6.898686255708808E-2,5.7110246465646736E-4,9.9705443330398602E-2,0.10028570954159732,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,2.1167640214775164E-2,1.3442069767865005E-6,1.3442069767865005E-6,2.2335577791016893E-2,3.4272921022263558E-4,1.2121032958466052E-3,40,87.135527992040068,6.9516156359903172E-2,5.5645050931617999E-2,0.12637331058736778,0.1267240725536293,6.5163568555439519E-2,1.2908723627313577E-3,3.3208309475249464E-3,2.0806658142427763E-3,6.6299431248066708E-4,6.0644910742483895E-3,7.3571199261392699E-3,3.1732432885906041E-2,7.0715667378901392E-2,4.5329342433715518E-3,0.20932979410204153,0.30961752378664298,0.34,0.5233848958047318,5.3995151518837817E-4,1.9898306381208779E-3,6.6987368940895631E-2,0.19453494704196614,3.2029090011527141E-3,1.0205917916377167E-3,9.3354794970712321E-3,8.7913648222956073E-4,0.15348330314307429,2.0692283190746939E-6,1.0405138448432771E-6,0.1088573888319658,0.54083401662546626,0.5233848958047318,52.33848958047318,68,71.916485184007442,0.71916485184007439,301.89372250226779,null,8.5658174070276108E-2,null,0.20932979410204153,7.0715667378901392E-2,0.10028570954159732,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR74, IF(MODE_ILIM=4,#REF!,#REF!))","v":52.33848958047318},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ74, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.20932979410204153},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA74, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0715667378901392E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB74, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10028570954159732},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S74, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.89372250226779},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P74, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54730146546816527}]
[null,null,null,null,null,null,null,69,6.8999999999999992E-2,4.0300597785285275E-2,8.9161166205699721E-2,4.8857335332736479E-2,0.54729118089470274,0.54729118089470274,1,0.54729118089470274,2.9648960364227933E-6,0.10483388427207621,301921.58670357958,3.3121182586450151E-6,0,6.5999999999999989E-4,6.9972760453411872E-2,5.875424646564672E-4,9.9714645948200023E-2,0.10031161838653656,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,2.1470031454600882E-2,1.3828867519846538E-6,1.3828867519846538E-6,2.2655823155928827E-2,3.5262770381355924E-4,1.2122151706148721E-3,40,86.157998990378076,6.9812417288679998E-2,5.5650186861203786E-2,0.12667481932049865,0.12703573210342137,6.609787753039667E-2,1.3281545418630883E-3,3.321137453739376E-3,2.1243345641214326E-3,6.7288244936561901E-4,6.1183544672264271E-3,7.4483386352480075E-3,3.1732432885906034E-2,7.0719265455352565E-2,4.533352624354248E-3,0.2097366888183762,0.31005036602769209,0.34499999999999997,0.52667705857814173,5.5096951568982125E-4,2.0303540567220379E-3,6.6437922106223166E-2,0.19338180068300811,3.2430095062821887E-3,1.0272224614514193E-3,9.3402809685137634E-3,8.969424263044057E-4,0.15222439543524294,2.1111151503824863E-6,1.0318840541251356E-6,0.10796004265168661,0.53709608281032895,0.52667705857814173,52.66770585781417,68.999999999999986,71.94908925319227,0.71949089253192267,301.92158670357958,null,8.4955584711254389E-2,null,0.2097366888183762,7.0719265455352565E-2,0.10031161838653656,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR75, IF(MODE_ILIM=4,#REF!,#REF!))","v":52.66770585781417},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ75, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.2097366888183762},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA75, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0719265455352565E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB75, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10031161838653656},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S75, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.92158670357958},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P75, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54729118089470274}]
[null,null,null,null,null,null,null,70,6.9999999999999993E-2,4.0299840465465454E-2,9.0161166492466374E-2,4.985771399275498E-2,0.54728089632124033,0.54728089632124033,1,0.54728089632124033,2.9645903859136598E-6,0.10484355949646042,301949.4513498061,3.3118126081358821E-6,0,6.6E-4,7.0959053019826593E-2,6.0422246465646734E-4,9.9723848712941973E-2,0.10033777139128294,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,2.1772581535268589E-2,1.4221359201297563E-6,1.4221359201297563E-6,2.2976225742113717E-2,3.6267207420521497E-4,1.2123270471694715E-3,40,85.202159463163838,7.0108731820026762E-2,5.5655322872796259E-2,0.12697638173999248,0.12734759580701938,6.7032645195041374E-2,1.3659861586406681E-3,3.3214439648478677E-3,2.1680113420845773E-3,6.8277481670027797E-4,6.1722301236327238E-3,7.5401212120121963E-3,3.1732432885906041E-2,7.0722863589255155E-2,4.5337710120173392E-3,0.21014435162030409,0.31048422108353452,0.35,0.52991424901236794,5.6203321014680759E-4,2.071042796655197E-3,6.5897413331032106E-2,0.19224741134873108,3.282457434831557E-3,1.0337488692465286E-3,9.3450076877038581E-3,9.1481741027095421E-4,0.15098596685526186,2.1531716803116367E-6,1.0233946637573347E-6,0.10707729470544083,0.5334203702156648,0.52991424901236794,52.991424901236797,69.999999999999986,71.978028730187987,0.71978028730187982,301.94945134980611,null,8.4264424639082E-2,null,0.21014435162030409,7.0722863589255155E-2,0.10033777139128294,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR76, IF(MODE_ILIM=4,#REF!,#REF!))","v":52.991424901236797},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ76, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.21014435162030409},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA76, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0722863589255155E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB76, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10033777139128294},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S76, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.94945134980611},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P76, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54728089632124033}]
[null,null,null,null,null,null,null,71,7.0999999999999994E-2,4.0299083145645634E-2,9.1161166779233027E-2,5.0858092652773482E-2,0.5472706117477778,0.5472706117477778,1,0.5472706117477778,2.9642847869326131E-6,0.10485323487533259,301977.31644095795,3.3115070091548354E-6,0,6.5999999999999989E-4,7.1945724024924246E-2,6.2114246465646747E-4,9.9733051624627936E-2,0.1003641685608081,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,2.2075284964397882E-2,1.4619546187781135E-6,1.4619546187781135E-6,2.3296780310032031E-2,3.728623613231467E-4,1.2124389255104462E-3,40,84.267295459869402,7.0405099955227285E-2,5.5660458966397368E-2,0.12727799784713509,0.12765966373296211,6.7967856263129595E-2,1.4043673634416551E-3,3.3217504808505378E-3,2.211696148324489E-3,6.9267141519687369E-4,6.2261180443719012E-3,7.6324678477924911E-3,3.1732432885906034E-2,7.0726461780610497E-2,4.534189406360984E-3,0.21055278276772607,0.31091908921918032,0.35499999999999998,0.53309779783645073,5.7314153026390385E-4,2.1118929103978645E-3,6.5365626253640244E-2,0.1911313249727894,3.3212685807187188E-3,1.040173538213271E-3,9.3496614606322533E-3,9.3275966211568521E-4,0.14976752166929072,2.1953937684716627E-6,1.0150422750988771E-6,0.10620879161692214,0.52980537263102778,0.53309779783645073,53.30977978364507,71,72.003632642003467,0.72003632642003468,301.97731644095796,null,8.3584417187472018E-2,null,0.21055278276772607,7.0726461780610497E-2,0.1003641685608081,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR77, IF(MODE_ILIM=4,#REF!,#REF!))","v":53.30977978364507},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ77, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.21055278276772607},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA77, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0726461780610497E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB77, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.1003641685608081},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S77, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.97731644095796},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P77, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.5472706117477778}]
[null,null,null,null,null,null,null,72,7.1999999999999995E-2,4.0298325825825813E-2,9.2161167065999694E-2,5.1858471312791976E-2,0.54726032717431528,0.54726032717431528,1,0.54726032717431528,2.9639792394666225E-6,0.10486291040869647,302005.1819770459,3.3112014616888452E-6,0,6.600000000000001E-4,7.2932758109580373E-2,6.3830246465646737E-4,9.9742254683261491E-2,0.10039080990014006,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,2.2378136543537895E-2,1.5023429854836784E-6,1.5023429854836784E-6,2.361748190164108E-2,3.8319860509417438E-4,1.2125508056378394E-3,40,83.352724024613281,7.070152169556547E-2,5.5665595142009097E-2,0.12757966764321241,0.12797193594983244,6.8903496269678233E-2,1.4432983066484109E-3,3.3220570017475051E-3,2.2553889830334564E-3,7.0257224556765892E-4,6.2800182303486204E-3,7.7253787343141379E-3,3.1732432885906048E-2,7.0730060029420005E-2,4.5346078073853447E-3,0.21096198252095194,0.31135497070010487,0.36,0.5362289931726929,5.842934419789421E-4,2.1529005772583485E-3,6.4842351439660689E-2,0.19003310202674051,3.3594582321800391E-3,1.0464989107550659E-3,9.3542440354611039E-3,9.5076746656218313E-4,0.14856858001549897,2.2377774069610292E-6,1.0068235983237405E-6,0.10535419132394451,0.52624963207104569,0.5362289931726929,53.622899317269287,72,72.026192211331946,0.72026192211331941,302.00518197704588,null,8.2915294548217458E-2,null,0.21096198252095194,7.0730060029420005E-2,0.10039080990014006,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR78, IF(MODE_ILIM=4,#REF!,#REF!))","v":53.622899317269287},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ78, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.21096198252095194},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA78, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0730060029420005E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB78, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10039080990014006},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S78, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":302.00518197704588},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P78, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54726032717431528}]
[null,null,null,null,null,null,null,73,7.2999999999999995E-2,4.0297568506005993E-2,9.3161167352766347E-2,5.285884997281047E-2,0.54725004260085286,0.54725004260085286,1,0.54725004260085286,2.9636737435026643E-6,0.10487258609655571,302033.04795808054,3.3108959657248866E-6,0,6.600000000000001E-4,7.3920140729509989E-2,6.5570246465646736E-4,9.9751457888846123E-2,0.10041769541436313,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,2.2681131348899146E-2,1.5433011577980467E-6,1.5433011577980467E-6,2.3938325821857499E-2,3.936808454463923E-4,1.2126626875516933E-3,40,82.457791532260714,7.0997997042325206E-2,5.5670731399633404E-2,0.1278813911295103,0.12828441252625736,6.9839551516882425E-2,1.4827791386480993E-3,3.3223635275388863E-3,2.299089846403772E-3,7.1247730852490906E-4,6.3339306824675675E-3,7.8188540636673232E-3,3.1732432885906048E-2,7.073365833568504E-2,4.5350262150905801E-3,0.21137195114070031,0.3117918657922486,0.36499999999999999,0.53930908222830531,5.9548794410417571E-4,2.1940620983402527E-3,6.4327386106962564E-2,0.18895231694283604,3.3970411918477638E-3,1.0527273516960599E-3,9.3587571048199657E-3,9.6883916281840338E-4,0.14738867727388782,2.2803187151067001E-6,9.987354481005207E-7,0.10451316262922965,0.52275173686070597,0.53930908222830531,53.930908222830531,73,72.045963869077937,0.72045963869077934,302.03304795808054,null,8.2256797419492586E-2,null,0.21137195114070031,7.073365833568504E-2,0.10041769541436313,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR79, IF(MODE_ILIM=4,#REF!,#REF!))","v":53.930908222830531},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ79, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.21137195114070031},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA79, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.073365833568504E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB79, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10041769541436313},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S79, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":302.03304795808054},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P79, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54725004260085286}]
[null,null,null,null,null,null,null,74,7.3999999999999996E-2,4.0296811186186179E-2,9.4161167639533E-2,5.3859228632828979E-2,0.54723975802739055,0.54723975802739055,1,0.54723975802739055,2.9633682990277185E-6,0.10488226193891401,302060.91438407241,3.3105905212499407E-6,0,6.6E-4,7.490785810227496E-2,6.7334246465646712E-4,9.9760661241385287E-2,0.10044482510861785,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,2.2984264713570585E-2,1.5848292732704581E-6,1.5848292732704581E-6,2.4259307621456269E-2,4.043091223091706E-4,1.2127745712520507E-3,40,81.581872130573942,7.1294525996790453E-2,5.5675867739272224E-2,0.12818316830731472,0.12859709353090815,7.0776009024223693E-2,1.522810009832686E-3,3.3226700582247967E-3,2.3427987386277355E-3,7.2238660478092173E-4,6.3878554016334535E-3,7.9128940283075423E-3,3.1732432885906041E-2,7.073725669940692E-2,4.535444629476847E-3,0.21178268888809948,0.31222977476201796,0.37,0.54233927290708916,6.0672406703125847E-4,2.2353738917450026E-3,6.3820533863632498E-2,0.18788855756409756,3.4340317958784098E-3,1.0588611513370429E-3,9.3632023079932673E-3,9.869731424304209E-4,0.14622736346590087,2.3230139344523533E-6,9.9077473947629368E-7,0.10368538477242829,0.5193103198111485,0.54233927290708916,54.23392729070892,74,72.063171902227168,0.72063171902227163,302.06091438407242,null,8.16086746707788E-2,null,0.21178268888809948,7.073725669940692E-2,0.10044482510861785,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR80, IF(MODE_ILIM=4,#REF!,#REF!))","v":54.23392729070892},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ80, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.21178268888809948},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA80, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.073725669940692E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB80, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10044482510861785},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S80, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":302.06091438407242},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P80, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54723975802739055}]
[null,null,null,null,null,null,null,75,7.5000000000000011E-2,4.0296053866366359E-2,9.5161167926299667E-2,5.4859607292847487E-2,0.54722947345392792,0.54722947345392792,1,0.54722947345392792,2.9630629060287677E-6,0.10489193793577509,302088.78125503234,3.31028512825099E-6,0,6.6E-4,7.5895897158348186E-2,6.9122246465646762E-4,9.9769864740882605E-2,0.10047219898810132,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,2.3287532211090981E-2,1.6269274694478001E-6,1.6269274694478001E-6,2.4580423081278811E-2,4.1508347561315423E-4,1.2128864567389549E-3,40,80.724366280609559,7.1591108560245253E-2,5.5681004160927562E-2,0.12848499917791176,0.12890997903250032,7.1712856482397502E-2,1.5633910705989422E-3,3.3229765938053565E-3,2.3865156598976535E-3,7.3230013504801841E-4,6.4417923887510288E-3,8.0074988210559767E-3,3.1732432885906041E-2,7.0740855120587115E-2,4.5358630505443111E-3,0.21219419602468773,0.31266869787628587,0.37500000000000006,0.54532073534553105,6.1800087149671893E-4,2.2768324879993652E-3,6.3321604458225836E-2,0.18684142462018341,3.4704439321840358E-3,1.0649025283680454E-3,9.3675812330052139E-3,1.0051678472368405E-3,0.14508420268219271,2.3658594239816485E-6,9.8293848395352181E-7,0.10287054702221396,0.51592405648101414,0.54532073534553105,54.532073534553106,75.000000000000014,72.078010752951272,0.72078010752951271,302.08878125503236,null,8.097068302350556E-2,null,0.21219419602468773,7.0740855120587115E-2,0.10047219898810132,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR81, IF(MODE_ILIM=4,#REF!,#REF!))","v":54.532073534553106},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ81, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.21219419602468773},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA81, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0740855120587115E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB81, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10047219898810132},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S81, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":302.08878125503236},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P81, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54722947345392792}]
[null,null,null,null,null,null,null,76,7.6000000000000012E-2,4.0295296546546538E-2,9.616116821306632E-2,5.5859985952865981E-2,0.5472191888804655,0.5472191888804655,1,0.5472191888804655,2.9627575644928004E-6,0.10490161408714267,302116.64857097098,3.3099797867150227E-6,0,6.6E-4,7.6884245495878828E-2,7.0934246465646767E-4,9.9779068387341574E-2,0.10049981705806676,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,2.3590929640256511E-2,1.6695958838745997E-6,1.6695958838745997E-6,2.4901668197635441E-2,4.2600394529026316E-4,1.2129983440124486E-3,40,79.884699388209782,7.1887744733973621E-2,5.5686140664601369E-2,0.12878688374258745,0.12922306909979378,7.2650082210725192E-2,1.6045224713484394E-3,3.323283134280681E-3,2.4302406104058376E-3,7.422179000385427E-4,6.4957416447250617E-3,8.1026686350998429E-3,3.1732432885906041E-2,7.0744453599226959E-2,4.5362814782931296E-3,0.21260647281241371,0.3131086354023917,0.38000000000000006,0.54825460337741561,6.2931744740576424E-4,2.3184345256957624E-3,6.2830413541639984E-2,0.18581053122764635,3.5062910578151072E-3,1.0708536326453934E-3,9.3718954186076311E-3,1.0234217674183949E-3,0.14395877253702624,2.4088516555637741E-6,9.7522378574952674E-7,0.10206834828735829,0.51259166351870022,0.54825460337741561,54.825460337741561,76.000000000000014,72.090646982404948,0.72090646982404949,302.11664857097099,null,8.0342586746552619E-2,null,0.21260647281241371,7.0744453599226959E-2,0.10049981705806676,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR82, IF(MODE_ILIM=4,#REF!,#REF!))","v":54.825460337741561},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ82, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.21260647281241371},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA82, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0744453599226959E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB82, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10049981705806676},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S82, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":302.11664857097099},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P82, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.5472191888804655}]
[null,null,null,null,null,null,null,77,7.7000000000000013E-2,4.0294539226726718E-2,9.7161168499832987E-2,5.6860364612884476E-2,0.54720890430700309,0.54720890430700309,1,0.54720890430700309,2.9624522744068103E-6,0.10491129039302043,302144.51633189892,3.3096744966290322E-6,0,6.6E-4,7.7872891338838596E-2,7.2770246465646748E-4,9.9788272180765664E-2,0.10052767932382374,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,2.3894453011058366E-2,1.7128346540930286E-6,1.7128346540930286E-6,2.5223039168798856E-2,4.3707057127369303E-4,1.2131102330725741E-3,40,79.062320520022766,7.2184434519259641E-2,5.5691277250295608E-2,0.12908882200262783,0.1295363638015925,7.3587675117748982E-2,1.6462043624875531E-3,3.3235896796508886E-3,2.4739735903446052E-3,7.5213990046486053E-4,6.5497031704603538E-3,8.1984036639927756E-3,3.1732432885906041E-2,7.0748052135327824E-2,4.5366999127234627E-3,0.21301951951363654,0.31354958760814172,0.38500000000000006,0.55114197593080472,6.4067291270912736E-4,2.3601767473339008E-3,6.2346782439983831E-2,0.18479550241326814,3.5415862155406567E-3,1.0767165478405246E-3,9.3761463561760402E-3,1.0417334396376156E-3,0.14285066364786528,2.4519872096093196E-6,9.6762783822868961E-7,0.10127849674576665,0.50931189708116964,0.55114197593080472,55.114197593080469,77.000000000000014,72.101220909974245,0.7210122090997424,302.1445163318989,null,7.9724157365813481E-2,null,0.21301951951363654,7.0748052135327824E-2,0.10052767932382374,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR83, IF(MODE_ILIM=4,#REF!,#REF!))","v":55.114197593080469},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ83, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.21301951951363654},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA83, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0748052135327824E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB83, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10052767932382374},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S83, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":302.1445163318989},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P83, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54720890430700309}]
[null,null,null,null,null,null,null,78,7.8000000000000014E-2,4.0293781906906904E-2,9.816116878659964E-2,5.7860743272902977E-2,0.54719861973354067,0.54719861973354067,1,0.54719861973354067,2.9621470357577947E-6,0.10492096685341204,302172.38453782676,3.3093692579800165E-6,0,6.6E-4,7.8861823498259057E-2,7.4630246465646772E-4,9.9797476121158427E-2,0.10055578579073826,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,2.4198098531653972E-2,1.7566439176429022E-6,1.7566439176429022E-6,2.5544532382495107E-2,4.4828339349791438E-4,1.2132221239193745E-3,40,78.256701198023066,7.2481177917387438E-2,5.5696413918012229E-2,0.12939081395931903,0.12984986320674496,7.4525624664737194E-2,1.6884368944274626E-3,3.3238962299160946E-3,2.5177145999062804E-3,7.6206613703936092E-4,6.6036769668617358E-3,8.2947041016551912E-3,3.1732432885906041E-2,7.0751650728891086E-2,4.5371183538354693E-3,0.21343333639112672,0.31399155476180995,0.39000000000000007,0.55398391836100003,6.520664123325253E-4,2.4020559953529569E-3,6.1870537937855581E-2,0.18379597465923775,3.5763420496686626E-3,1.0824932939674254E-3,9.3803354915188396E-3,1.0601014452637479E-3,0.14175947913881454,2.4952627709252119E-6,9.6014792049814633E-7,0.10050070949051276,0.50608355132521621,0.55398391836100003,55.398391836100004,78.000000000000014,72.109847935853821,0.72109847935853821,302.17238453782676,null,7.9115173387068069E-2,null,0.21343333639112672,7.0751650728891086E-2,0.10055578579073826,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR84, IF(MODE_ILIM=4,#REF!,#REF!))","v":55.398391836100004},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ84, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.21343333639112672},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA84, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0751650728891086E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB84, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10055578579073826},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S84, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":302.17238453782676},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P84, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54719861973354067}]
[null,null,null,null,null,null,null,79,7.9000000000000015E-2,4.0293024587087077E-2,9.9161169073366293E-2,5.8861121932921479E-2,0.54718833516007803,0.54718833516007803,1,0.54718833516007803,2.9618418485327527E-6,0.10493064346832129,302200.25318876537,3.309064070754975E-6,0,6.600000000000001E-4,7.9851031336298742E-2,7.6514246465646761E-4,9.9806680208523429E-2,0.10058413646423263,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,2.4501862596284941E-2,1.8010238120616809E-6,1.8010238120616809E-6,2.58661444043078E-2,4.5964245189867404E-4,1.2133340165528929E-3,40,77.467334266989326,7.2777974929641207E-2,5.570155066775323E-2,0.12969285961394733,0.13016356738414409,7.5463920831853742E-2,1.731220217584152E-3,3.3242027850764197E-3,2.5614636392831949E-3,7.7199661047445652E-4,6.6576630348340708E-3,8.3915701423746634E-3,3.1732432885906048E-2,7.0755249379918145E-2,4.5375368016293124E-3,0.21384792370806618,0.3144345371321382,0.39500000000000007,0.55678146372288606,6.6349711715413858E-4,2.4440692083442191E-3,6.1401512071476608E-2,0.18281159546901357,3.610570821146956E-3,1.0881858297951254E-3,9.3844642266042149E-3,1.0785244086783912E-3,0.14068483416664218,2.5386751247581634E-6,9.5278139415830279E-7,9.9734712191971248E-2,0.50290545696734568,0.55678146372288606,55.678146372288609,79.000000000000014,72.116619551864289,0.72116619551864292,302.20025318876537,null,7.8515420031458574E-2,null,0.21384792370806618,7.0755249379918145E-2,0.10058413646423263,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR85, IF(MODE_ILIM=4,#REF!,#REF!))","v":55.678146372288609},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ85, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.21384792370806618},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA85, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0755249379918145E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB85, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10058413646423263},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S85, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":302.20025318876537},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P85, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54718833516007803}]
[null,null,null,null,null,null,null,80,8.0000000000000016E-2,4.0292267267267257E-2,0.10016116936013295,5.9861500592939973E-2,0.54717805058661562,0.54717805058661562,1,0.54717805058661562,2.9615367127186932E-6,0.10494032023775178,302228.12228472519,3.308758934940915E-6,0,6.6E-4,8.0840504732903329E-2,7.8422246465646782E-4,9.9815884442864114E-2,0.10061273134978538,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,2.4805741774062855E-2,1.8459744748844611E-6,1.8459744748844611E-6,2.6187871966918946E-2,4.7114778641299283E-4,1.2134459109731717E-3,40,76.693732829839263,7.3074825557305101E-2,5.5706687499520548E-2,0.12999495896779881,0.13047747640272711,7.640255408676859E-2,1.7745544823784063E-3,3.3245093451319775E-3,2.6052207086676837E-3,7.8193132148258104E-4,6.7116613752822418E-3,8.4890019808062742E-3,3.1732432885906041E-2,7.075884808841032E-2,4.537955256105149E-3,0.21426328172804884,0.31487853498833646,0.40000000000000008,0.55953561398584473,6.7496422302870782E-4,2.486213417434656E-3,6.093954193116205E-2,0.18184202295277996,3.6442844219825242E-3,1.0937960551512971E-3,9.3885339212090684E-3,1.0970009956576226E-3,0.13962635546819521,2.5822211530166853E-6,9.455257002000165E-7,9.8980238775199444E-2,0.49977647990865381,0.55953561398584473,55.953561398584469,80.000000000000014,72.121604042494241,0.72121604042494236,302.2281222847252,null,7.7924688982904514E-2,null,0.21426328172804884,7.075884808841032E-2,0.10061273134978538,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR86, IF(MODE_ILIM=4,#REF!,#REF!))","v":55.953561398584469},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ86, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.21426328172804884},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA86, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.075884808841032E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB86, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10061273134978538},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S86, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":302.2281222847252},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P86, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54717805058661562}]
[null,null,null,null,null,null,null,81,8.1000000000000016E-2,4.0291509947447436E-2,0.10116116964689961,6.0861879252958467E-2,0.54716776601315309,0.54716776601315309,1,0.54716776601315309,2.961231628302625E-6,0.10494999716170723,302255.99182571692,3.3084538505248477E-6,0,6.6E-4,8.1830234054844089E-2,8.0354246465646779E-4,9.9825088824184005E-2,0.10064157045293146,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,2.5109732798551675E-2,1.8914960436439853E-6,1.8914960436439853E-6,2.6509711960117484E-2,4.8279943697916808E-4,1.2135578071802535E-3,40,75.935429246125537,7.3371729801663413E-2,5.5711824413316145E-2,0.13029711202215982,0.13079159033147583,7.7341515355507734E-2,1.8184398392358165E-3,3.3248159100828867E-3,2.6489858082520898E-3,7.9187027077619245E-4,6.7656719891111688E-3,8.5869998119730145E-3,3.1732432885906041E-2,7.0762446854369054E-2,4.5383737172631404E-3,0.21467941071508104,0.31532354860008349,0.40500000000000008,0.56224734119424435,6.8646694985469549E-4,2.528485742832529E-3,6.0484469472640939E-2,0.18088692543147644,3.6774943890148732E-3,1.0993258131226679E-3,9.3925458944941441E-3,1.11552991182659E-3,0.13858368092809067,2.6258978306623777E-6,9.3837835604078213E-7,9.8237031111772871E-2,0.49669551992131311,0.56224734119424435,56.224734119424433,81.000000000000014,72.124846875437001,0.72124846875436999,302.25599182571693,null,7.734277814683356E-2,null,0.21467941071508104,7.0762446854369054E-2,0.10064157045293146,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR87, IF(MODE_ILIM=4,#REF!,#REF!))","v":56.224734119424433},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ87, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.21467941071508104},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA87, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0762446854369054E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB87, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10064157045293146},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S87, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":302.25599182571693},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P87, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54716776601315309}]
[null,null,null,null,null,"Eff (%)","Iout (mA)",82,8.2000000000000003E-2,4.0290752627627623E-2,0.10216116993366625,6.1862257912976955E-2,0.54715748143969078,0.54715748143969078,1,0.54715748143969078,2.9609265952715642E-6,0.10495967424019138,302283.86181175127,3.308148817493786E-6,0,6.6E-4,8.2820210126940408E-2,8.2310246465646753E-4,9.9834293352486655E-2,0.10067065377926222,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,2.5413832558081689E-2,1.9375886558706388E-6,1.9375886558706388E-6,2.6831661421512439E-2,4.9459744353677246E-4,1.2136697051741813E-3,40,75.191974189363449,7.3668687664000393E-2,5.5716961409141993E-2,0.13059931877831657,0.13110590923941631,7.8280795995359129E-2,1.8628764385867781E-3,3.3251224799292641E-3,2.6927589382287611E-3,8.0181345906777041E-4,6.8196948772257949E-3,8.6855638312661274E-3,3.1732432885906041E-2,7.076604567779568E-2,4.5387921851034454E-3,0.21509631093358156,0.31576957823752699,0.41000000000000003,0.56491758857632468,6.9800454068350047E-4,2.5708833905265702E-3,6.0036141336765797E-2,0.17994598105843246,3.7102119170769176E-3,1.1047768921575768E-3,9.3965014265090501E-3,1.134109901182832E-3,0.13755645916562967,2.669702222261667E-6,9.3133695269270596E-7,9.7504838725322882E-2,0.49366150939346215,0.56491758857632468,56.491758857632469,82,72.126370778645395,0.72126370778645399,302.28386181175125,null,7.6769491419640568E-2,null,0.21509631093358156,7.076604567779568E-2,0.10067065377926222,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR88, IF(MODE_ILIM=4,#REF!,#REF!))","v":56.491758857632469},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ88, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.21509631093358156},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA88, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.076604567779568E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB88, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10067065377926222},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S88, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":302.28386181175125},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P88, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54715748143969078}]
[null,null,null,null,null,{"$f":"BT51","v":68.427867006324419},{"$f":"I56*1000","v":50},83,8.3000000000000004E-2,4.0289995307807802E-2,0.1031611702204329,6.2862636572995456E-2,0.54714719686622826,0.54714719686622826,1,0.54714719686622826,2.9606216136125268E-6,0.10496935147320793,302311.73224283895,3.3078438358347491E-6,0,6.6E-4,8.3810424205289419E-2,8.4290246465646747E-4,9.9843498027775618E-2,0.10069998133442531,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,2.5718038086736221E-2,1.9842524490924447E-6,1.9842524490924447E-6,2.7153717527893851E-2,5.0654184602665444E-4,1.2137816049549984E-3,40,74.462935759198103,7.396569914560043E-2,5.5722098487000077E-2,0.13090157923755552,0.1314204331956195,7.9220387769668346E-2,1.9078644308664918E-3,3.3254290546712289E-3,2.7365400987900555E-3,8.1176088706981855E-4,6.8737300405311026E-3,8.7846942344455108E-3,3.1732432885906041E-2,7.07696445586916E-2,4.539210659626227E-3,0.21551398264838281,0.3162166241712846,0.41500000000000004,0.56754727160413676,7.0957626086799079E-4,2.6134036491308934E-3,5.9594408677180424E-2,0.17901887745770442,3.7424478715749653E-3,1.1101510280757331E-3,9.4004017596308886E-3,1.1527397446847718E-3,0.1365443491399447,2.7136314786897425E-6,9.2439915205548382E-7,9.6783418510072175E-2,0.49067341212949772,0.56754727160413676,56.75472716041368,83,72.126175499523185,0.72126175499523182,302.31173224283896,null,7.6204638468322608E-2,null,0.21551398264838281,7.07696445586916E-2,0.10069998133442531,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR89, IF(MODE_ILIM=4,#REF!,#REF!))","v":56.75472716041368},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ89, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.21551398264838281},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA89, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.07696445586916E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB89, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10069998133442531},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S89, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":302.31173224283896},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P89, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54714719686622826}]
[null,null,null,null,null,{"$f":"BT81","v":72.078010752951272},{"$f":"I81*1000","v":75.000000000000014},84,8.4000000000000005E-2,4.0289237987987975E-2,0.10416117050719956,6.3863015233013951E-2,0.54713691229276573,0.54713691229276573,1,0.54713691229276573,2.9603166833125381E-6,0.1049790288607606,302339.60311899061,3.3075389055347604E-6,0,6.6E-4,8.480086795234211E-2,8.6294246465646761E-4,9.985270285005439E-2,0.10072955312412472,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,2.6022346555957573E-2,2.0314875608350709E-6,2.0314875608350709E-6,2.7475877587189577E-2,5.1863268439093768E-4,1.2138935065227473E-3,40,73.747898644724415,7.4262764247747887E-2,5.5727235646892345E-2,0.13120389340116298,0.1317351622692006,8.0160282824372722E-2,1.9534039665149608E-3,3.3257356343088969E-3,2.7803292901283322E-3,8.2171255549486196E-4,6.9277774799320919E-3,8.8843912176400537E-3,3.1732432885906041E-2,7.0773243497058186E-2,4.539629140831644E-3,0.21593242612473049,0.31666468667244341,0.42000000000000004,0.57013727900703925,7.2118139724789484E-4,2.6560438868681192E-3,5.9159126995538679E-2,0.17810531137825877,3.7742128005174764E-3,1.1154499059899078E-3,9.4042480999398242E-3,1.1714182589020632E-3,0.13554701977244865,2.757682833978939E-6,9.1756268432799547E-7,9.6072534461703302E-2,0.48773022220293294,0.57013727900703925,57.013727900703927,84,72.124237241864293,0.72124237241864297,302.33960311899062,null,7.5648034519769716E-2,null,0.21593242612473049,7.0773243497058186E-2,0.10072955312412472,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR90, IF(MODE_ILIM=4,#REF!,#REF!))","v":57.013727900703927},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ90, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.21593242612473049},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA90, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0773243497058186E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB90, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10072955312412472},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S90, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":302.33960311899062},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P90, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54713691229276573}]
[null,null,null,null,null,{"$f":"BT106","v":71.049894896969974},{"$f":"I106*1000","v":100},85,8.5000000000000006E-2,4.0288480668168154E-2,0.10516117079396621,6.4863393893032445E-2,0.5471266277193032,0.5471266277193032,1,0.5471266277193032,2.9600118043586266E-6,0.10498870640285303,302367.47444021679,3.3072340265808489E-6,0,6.600000000000001E-4,8.5791533413679955E-2,8.8322246465646762E-4,9.9861907819326426E-2,0.10075936915412075,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,2.6326755266723248E-2,2.0792941286218209E-6,2.0792941286218209E-6,2.7798139030970836E-2,5.3086999857302169E-4,1.2140054098774705E-3,40,73.04646333555435,7.4559882971727123E-2,5.5732372888820755E-2,0.13150626127042536,0.13205009652931954,8.1100473666136416E-2,1.9994951959769925E-3,3.3260422188423847E-3,2.824126512435958E-3,8.3166846505544926E-4,6.9818371963337924E-3,8.984654977348034E-3,3.1732432885906048E-2,7.0776842492896799E-2,4.540047628719855E-3,0.21635164162828424,0.31711376601256097,0.42500000000000004,0.57268847374110898,7.3281925737107465E-4,2.6988015486837662E-3,5.8730155983891169E-2,0.17720498836319862,3.8055169460205875E-3,1.1206751621440378E-3,9.4080416185348299E-3,1.1901442947246424E-3,0.13456414958570675,2.8018536023041876E-6,9.1082534553249082E-7,9.5371957419933956E-2,0.48483096285915728,0.57268847374110898,57.268847374110898,85,72.120507778355574,0.72120507778355569,302.36747444021677,null,7.5099500159221455E-2,null,0.21635164162828424,7.0776842492896799E-2,0.10075936915412075,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR91, IF(MODE_ILIM=4,#REF!,#REF!))","v":57.268847374110898},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ91, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.21635164162828424},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA91, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0776842492896799E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB91, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10075936915412075},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S91, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":302.36747444021677},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P91, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.5471266277193032}]
[null,null,null,null,null,null,null,86,8.6000000000000007E-2,4.0287723348348341E-2,0.10616117108073286,6.5863772553050939E-2,0.5471163431458409,0.5471163431458409,1,0.5471163431458409,2.9597069767378238E-6,0.10499838409948893,302395.34620652819,3.3069291989600457E-6,0,6.5999999999999989E-4,8.6782412996358679E-2,9.0374246465646762E-4,9.9871112935595321E-2,0.10078942943023012,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,2.6631261642248209E-2,2.1276722899736425E-6,2.1276722899736425E-6,2.8120499407463497E-2,5.4325382851758142E-4,1.2141173150192106E-3,40,72.358245377482575,7.4857055318822641E-2,5.5737510212787278E-2,0.13180868284662911,0.1323652360451808,8.2040953141961095E-2,2.0461382697022027E-3,3.3263488082718104E-3,2.8679317659053051E-3,8.4162861646415129E-4,7.0359091906412666E-3,9.0854857104374961E-3,3.1732432885906034E-2,7.0780441546208828E-2,4.5404661232910214E-3,0.21677162942511813,0.31756386246366558,0.43000000000000005,0.57520169391668485,7.4448916874809588E-4,2.7416741534852435E-3,5.8307359373878744E-2,0.17631762243327473,3.8363702553167456E-3,1.1258283856719433E-3,9.4117834527926211E-3,1.2089167361275343E-3,0.13359542635790456,2.8461411750986765E-6,9.041849951456983E-7,9.4681464822209793E-2,0.48197468546558025,0.57520169391668485,57.520169391668489,86,72.229662267470047,0.72229662267470052,302.39534620652819,null,7.4558861137427351E-2,null,0.21677162942511813,7.0780441546208828E-2,0.10078942943023012,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR92, IF(MODE_ILIM=4,#REF!,#REF!))","v":57.520169391668489},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ92, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.21677162942511813},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA92, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0780441546208828E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB92, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10078942943023012},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S92, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":302.39534620652819},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P92, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.5471163431458409}]
[null,null,null,null,null,null,null,87,8.7000000000000008E-2,4.028696602852852E-2,0.10716117136749953,6.6864151213069448E-2,0.54710605857237837,0.54710605857237837,1,0.54710605857237837,2.9594022004371651E-6,0.10500806195067205,302423.2184179356,3.3066244226593869E-6,0,6.6E-4,8.7773499448697861E-2,9.2450246465646761E-4,9.9880318198864587E-2,0.10081973395832594,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,2.6935863221172376E-2,2.1766221824091201E-6,2.1766221824091201E-6,2.8442956375025922E-2,5.5578421417056825E-4,1.2142292219480114E-3,40,71.682874669836295,7.5154281290318925E-2,5.574264761879389E-2,0.13211115813106084,0.13268058088603374,8.298171442015756E-2,2.09333333814501E-3,3.3266554025972919E-3,2.9117450507287566E-3,8.5159301043356242E-4,7.0899934637596107E-3,9.1868836141466171E-3,3.1732432885906041E-2,7.0784040656995645E-2,4.5408846245453029E-3,0.21719238978172131,0.31801497629825703,0.43500000000000005,0.57767775368614127,7.5619047813912856E-4,2.7846592914992198E-3,5.7890604792392115E-2,0.17544293578396739,3.8667823912913271E-3,1.1309111202806412E-3,9.4154747075725874E-3,1.2277344989886192E-3,0.13264054679213128,2.890543018293165E-6,8.9763955383150514E-7,9.4000840467958008E-2,0.47916046850679239,0.57767775368614127,57.767775368614124,87.000000000000014,72.361493645121143,0.72361493645121144,302.42321841793557,null,7.4025948186075816E-2,null,0.21719238978172131,7.0784040656995645E-2,0.10081973395832594,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR93, IF(MODE_ILIM=4,#REF!,#REF!))","v":57.767775368614124},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ93, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.21719238978172131},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA93, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0784040656995645E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB93, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10081973395832594},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S93, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":302.42321841793557},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P93, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54710605857237837}]
[null,null,null,null,null,null,null,88,8.8000000000000009E-2,4.02862087087087E-2,0.10816117165426618,6.7864529873087942E-2,0.54709577399891585,0.54709577399891585,1,0.54709577399891585,2.9590974754436928E-6,0.10501773995640604,302451.09107444948,3.3063196976659155E-6,0,6.6E-4,8.8764785841405389E-2,9.4550246465646736E-4,9.988952360913772E-2,0.10085028274433756,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,2.7240557651196491E-2,2.2261439434444793E-6,2.2261439434444793E-6,2.8765507696057603E-2,5.6846119547920913E-4,1.2143411306639147E-3,40,71.019994801811478,7.5451560887500491E-2,5.5747785106842529E-2,0.13241368712500695,0.13299613112117206,8.3922750972574345E-2,2.1410805517646371E-3,3.3269620018189444E-3,2.9555663670986941E-3,8.615616476762985E-4,7.1440900165939368E-3,9.2888488860840713E-3,3.1732432885906041E-2,7.0787639825258625E-2,4.5413031324828589E-3,0.21761392296499762,0.31846710778930598,0.44000000000000006,0.58011744409386745,7.6792255087073248E-4,2.8277546217415211E-3,5.7479763623376652E-2,0.17458065849546378,3.8967627425706619E-3,1.1359248658619893E-3,9.4191164563704292E-3,1.2465965299567317E-3,0.13169921619974317,2.9350566696728503E-6,8.9118700127016794E-7,9.3329874292877923E-2,0.4763874166225045,0.58011744409386745,58.011744409386743,88.000000000000014,72.477313046906502,0.724773130469065,302.45109107444949,null,7.3500596841081026E-2,null,0.21761392296499762,7.0787639825258625E-2,0.10085028274433756,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR94, IF(MODE_ILIM=4,#REF!,#REF!))","v":58.011744409386743},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ94, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.21761392296499762},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA94, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0787639825258625E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB94, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10085028274433756},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S94, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":302.45109107444949},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P94, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54709577399891585}]
[null,null,null,null,null,null,null,89,8.900000000000001E-2,4.0285451388888872E-2,0.10916117194103284,6.8864908533106436E-2,0.54708548942545332,0.54708548942545332,1,0.54708548942545332,2.9587928017444509E-6,0.10502741811669467,302478.96417608071,3.3060150239666731E-6,0,6.5999999999999989E-4,8.975626554993564E-2,9.6674246465646763E-4,9.9898729166418274E-2,0.10088107579425083,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,2.7545342683132395E-2,2.2762377105935864E-6,2.2762377105935864E-6,2.9088151231305898E-2,5.812848123920068E-4,1.214453041166964E-3,40,70.369262425294309,7.5748894111651949E-2,5.5752922676935199E-2,0.1327162698297541,0.1333118868199345,8.4864056557987816E-2,2.1893800610251158E-3,3.3272686059368879E-3,2.9993957152075128E-3,8.7153452890500007E-4,7.1981988500494001E-3,9.3913817242294341E-3,3.1732432885906034E-2,7.0791239050999155E-2,4.5417216471038517E-3,0.21803622924226693,0.31892025721025574,0.44500000000000006,0.58252153389031225,7.7968477018206612E-4,2.8709578695939706E-3,5.7074710875479114E-2,0.17373052825489643,3.9263204331836188E-3,1.140871080036205E-3,9.4227097424230515E-3,1.2655018053676099E-3,0.130771148197112,2.9796797363459513E-6,8.848253740792859E-7,9.2668362152772563E-2,0.47365465968615705,0.58252153389031225,58.252153389031221,89.000000000000014,72.230234640211876,0.72230234640211877,302.47896417608069,null,7.2982647273339904E-2,null,0.21803622924226693,7.0791239050999155E-2,0.10088107579425083,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR95, IF(MODE_ILIM=4,#REF!,#REF!))","v":58.252153389031221},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ95, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.21803622924226693},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA95, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0791239050999155E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB95, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10088107579425083},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S95, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":302.47896417608069},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P95, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54708548942545332}]
[null,null,null,null,null,null,null,90,9.0000000000000011E-2,4.0284694069069066E-2,0.11016117222779949,6.9865287193124945E-2,0.54707520485199101,0.54707520485199101,1,0.54707520485199101,2.9584881793264907E-6,0.10503709643154156,302506.83772283979,3.3057104015487129E-6,0,6.6E-4,9.0747932237988563E-2,9.8822246465646757E-4,9.990793487070973E-2,0.10091211311410785,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,2.7850216165336675E-2,2.326903621367941E-6,2.326903621367941E-6,2.9410884934540971E-2,5.9425510485873988E-4,1.2145649534572019E-3,40,69.730346661849737,7.6046280964057883E-2,5.5758060329073829E-2,0.13301890624658891,0.13362784805170447,8.5805625206566399E-2,2.2382320163952816E-3,3.3275752149512384E-3,3.0432330952476078E-3,8.8151165483232874E-4,7.2523199650311749E-3,9.4944823269335413E-3,3.1732432885906041E-2,7.0794838334218624E-2,4.54214016840844E-3,0.21845930888126508,0.31937442483502165,0.45000000000000007,0.58489077031185999,7.9147653659807538E-4,2.914266824482965E-3,5.6675325055250206E-2,0.17289229009024101,3.9554643318175974E-3,1.1457511796305847E-3,9.4262555797670327E-3,1.2844493302053468E-3,0.12985606441510342,3.0244098923185586E-6,8.7855276382205067E-7,9.201610561645493E-2,0.47096135192220734,0.58489077031185999,58.489077031186,90.000000000000014,72.8349974854723,0.72834997485472297,302.5068377228398,null,7.2471944126593663E-2,null,0.21845930888126508,7.0794838334218624E-2,0.10091211311410785,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR96, IF(MODE_ILIM=4,#REF!,#REF!))","v":58.489077031186},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ96, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.21845930888126508},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA96, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0794838334218624E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB96, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10091211311410785},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S96, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":302.5068377228398},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P96, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54707520485199101}]
[null,null,null,null,null,null,null,91,9.1000000000000011E-2,4.0283936749249245E-2,0.11116117251456614,7.0865665853143439E-2,0.54706492027852849,0.54706492027852849,1,0.54706492027852849,2.9581836081768644E-6,0.10504677490095048,302534.71171473747,3.3054058303990863E-6,0,6.6E-4,9.173977984206505E-2,1.0099424646564676E-3,9.9917140722015657E-2,0.1009433947100072,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,2.8155176038499485E-2,2.3781418132766868E-6,2.3781418132766868E-6,2.9733706847571591E-2,6.0737211283046276E-4,1.2146768675346709E-3,40,69.102928541724268,7.634372144600296E-2,5.5763198063260411E-2,0.13332159637679802,0.13394401488591015,8.6747451205329229E-2,2.2876365683487765E-3,3.3278818288621126E-3,3.0870785074113855E-3,8.9149302617096929E-4,7.3064533624444669E-3,9.5981508929188601E-3,3.1732432885906041E-2,7.0798437674918377E-2,4.5425586963967835E-3,0.21888316215014417,0.319829610937992,0.45500000000000007,0.58722587982819452,8.0329726732905908E-4,2.9576793376547826E-3,5.6281488045633071E-2,0.17206569611530689,3.9842030606887036E-3,1.1505665420965868E-3,9.4297549542530154E-3,1.3034381371071415E-3,0.1289536942206663,3.0692448761705936E-6,8.7236731509852245E-7,9.1372911767286888E-2,0.46830667106021373,0.58722587982819452,58.722587982819455,91.000000000000014,73.305168165960453,0.73305168165960455,302.53471171473745,null,7.1968336362048274E-2,null,0.21888316215014417,7.0798437674918377E-2,0.1009433947100072,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR97, IF(MODE_ILIM=4,#REF!,#REF!))","v":58.722587982819455},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ97, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.21888316215014417},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA97, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0798437674918377E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB97, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.1009433947100072},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S97, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":302.53471171473745},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P97, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54706492027852849}]
[null,null,null,null,null,null,null,92,9.2000000000000012E-2,4.0283179429429418E-2,0.11216117280133281,7.1866044513161934E-2,0.54705463570506596,0.54705463570506596,1,0.54705463570506596,2.9578790882826312E-6,0.1050564535249251,302562.58615178434,3.3051013105048535E-6,0,6.600000000000001E-4,9.2731802557000725E-2,1.0319024646564679E-3,9.9926346720339523E-2,0.10097492058810373,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,2.8460220330762266E-2,2.4299524238266016E-6,2.4299524238266016E-6,3.0056615095576698E-2,6.2063587625950693E-4,1.2147887833994142E-3,40,68.486700472865579,7.664121555877193E-2,5.5768335879496887E-2,0.13362434022166822,0.13426038739202464,8.7689529084526069E-2,2.3375938673640467E-3,3.3281884476696285E-3,3.1309319518912542E-3,9.0147864363362984E-4,7.3605990431945129E-3,9.7023876212798954E-3,3.1732432885906048E-2,7.0802037073099816E-2,4.5429772310690425E-3,0.21930778931747341,0.32028581579402832,0.46000000000000008,0.58952756885872448,8.151463956949861E-4,3.0011933200430533E-3,5.5893084989481846E-2,0.17125050528528504,4.0125450040446771E-3,1.1553185068682481E-3,9.4332088245180738E-3,1.3224672854092463E-3,0.12806377444994721,3.1141824888279588E-6,8.6626722371592524E-7,9.0738593012934354E-2,0.46568981752393934,0.58952756885872448,58.952756885872446,92.000000000000014,73.638455592594738,0.73638455592594743,302.56258615178433,null,7.1471677109427326E-2,null,0.21930778931747341,7.0802037073099816E-2,0.10097492058810373,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR98, IF(MODE_ILIM=4,#REF!,#REF!))","v":58.952756885872446},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ98, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.21930778931747341},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA98, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0802037073099816E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB98, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10097492058810373},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S98, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":302.56258615178433},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P98, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54705463570506596}]
[null,null,null,null,null,null,null,93,9.3000000000000013E-2,4.0282422109609597E-2,0.11316117308809946,7.2866423173180428E-2,0.54704435113160355,0.54704435113160355,1,0.54704435113160355,2.9575746196308534E-6,0.10506613230346912,302590.46103399113,3.3047968418530757E-6,0,6.6E-4,9.3723994822406953E-2,1.0541024646564677E-3,9.9935552865684896E-2,0.10100669075460876,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,2.8765347153140719E-2,2.4823355905221027E-6,2.4823355905221027E-6,3.0379607882729674E-2,6.3404643509947835E-4,1.2149007010514743E-3,40,67.881365738100683,7.6938763303649446E-2,5.5773473777785243E-2,0.13392713778248616,0.13457696563956578,8.8631853604871386E-2,2.3881040639243474E-3,3.3284950713739028E-3,3.1747934288796319E-3,9.1146850793304059E-4,7.4147570081865748E-3,9.8071927114835311E-3,3.1732432885906041E-2,7.0805636528764287E-2,4.5433957724253776E-3,0.21973319065223898,0.32074303967846562,0.46500000000000008,0.59179652445955222,8.2702337057358796E-4,3.0448067402238346E-3,5.5510004177869644E-2,0.17044648316234598,4.0404983163182589E-3,1.1600083766647466E-3,9.4366181229181122E-3,1.341535860232141E-3,0.12718604915237883,3.159220591426302E-6,8.6025073493417014E-7,9.0112966902944125E-2,0.46311001365379556,0.59179652445955222,59.17965244595522,93.000000000000014,73.832411821820315,0.73832411821820321,302.59046103399112,null,7.0981823524148988E-2,null,0.21973319065223898,7.0805636528764287E-2,0.10100669075460876,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR99, IF(MODE_ILIM=4,#REF!,#REF!))","v":59.17965244595522},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ99, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.21973319065223898},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA99, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0805636528764287E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB99, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10100669075460876},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S99, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":302.59046103399112},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P99, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54704435113160355}]
[null,null,null,null,null,null,null,94,9.4E-2,4.0281664789789784E-2,0.1141611733748661,7.3866801833198908E-2,0.54703406655814113,0.54703406655814113,1,0.54703406655814113,2.9572702022085985E-6,0.10507581123658623,302618.33636136842,3.3044924244308208E-6,0,6.5999999999999989E-4,9.4716351309953678E-2,1.0765424646564676E-3,9.9944759158055244E-2,0.10103870521578991,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,2.9070554695230951E-2,2.5352914508652427E-6,2.5352914508652427E-6,3.0702683488094365E-2,6.4760382930526038E-4,1.2150126204908942E-3,40,67.286638018746814,7.7236364681920355E-2,5.5778611758127428E-2,0.13422998906053868,0.13489374969809645,8.9574419745570885E-2,2.4391673085177382E-3,3.3288016999750529E-3,3.2186629385689376E-3,9.2146261978195455E-4,7.468927258325945E-3,9.912566363369445E-3,3.1732432885906034E-2,7.0809236041913179E-2,4.5438143204659474E-3,0.22015936642384501,0.32120128286711314,0.47,0.59403341498239104,8.3892765587091742E-4,3.0885176224542642E-3,5.5132136942957204E-2,0.1696534016908102,4.0680709299475834E-3,1.1646374187397768E-3,9.4399837564221878E-3,1.3606429716030671E-3,0.12632026934521737,3.2043571032620022E-6,8.5431614178302121E-7,8.9495855953769993E-2,0.46056650296103763,0.59403341498239104,59.403341498239101,94,73.8844086186851,0.73884408618685105,302.61833636136839,null,7.0498636650334873E-2,null,0.22015936642384501,7.0809236041913179E-2,0.10103870521578991,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR100, IF(MODE_ILIM=4,#REF!,#REF!))","v":59.403341498239101},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ100, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.22015936642384501},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA100, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0809236041913179E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB100, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10103870521578991},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S100, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":302.61833636136839},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P100, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54703406655814113}]
[null,null,null,null,null,null,null,95,9.5000000000000001E-2,4.0280907469969963E-2,0.11516117366163275,7.4867180493217417E-2,0.5470237819846786,0.5470237819846786,1,0.5470237819846786,2.9569658360029375E-6,0.10508549032428018,302646.21213392698,3.3041880582251597E-6,0,6.6E-4,9.5708866911433876E-2,1.0992224646564676E-3,9.9953965597454161E-2,0.10107096397797127,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,2.9375841221178759E-2,2.5888201423557154E-6,2.5888201423557154E-6,3.1025840261773279E-2,6.613080988330124E-4,1.2151245417177168E-3,40,66.702240943047059,7.7534019694869449E-2,5.5783749820525419E-2,0.13453289405711258,0.13521073963722444,9.0517222693084071E-2,2.4907837516370897E-3,3.3291083334731969E-3,3.2625404811516042E-3,9.3146097989314845E-4,7.5231097945179497E-3,1.0018508777150482E-2,3.1732432885906041E-2,7.0812835612547892E-2,4.5442328751909133E-3,0.22058631690211372,0.32166054563625468,0.47499999999999998,0.59623889070675662,8.5085873001341475E-4,3.132324044790716E-3,5.4759377555206858E-2,0.16887103898143668,4.0952705628794122E-3,1.1692068660802515E-3,9.4433066074705654E-3,1.3797877536141459E-3,0.12546619277803661,3.249589999826273E-6,8.4846178344751734E-7,8.888708748089573E-2,0.45805854941220764,0.59623889070675662,59.623889070675659,95,73.791636151568156,0.73791636151568152,302.64621213392695,null,7.0021981289375396E-2,null,0.22058631690211372,7.0812835612547892E-2,0.10107096397797127,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR101, IF(MODE_ILIM=4,#REF!,#REF!))","v":59.623889070675659},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ101, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.22058631690211372},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA101, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0812835612547892E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB101, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10107096397797127},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S101, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":302.64621213392695},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P101, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.5470237819846786}]
[null,null,null,null,null,null,null,96,{"$f":"IF(PLOT_TYPE=1, H102/100*Iout, min_I*EXP(H102*rr/100))","v":9.6000000000000002E-2},{"$f":"IF(I102<Icrit, (Vin-(Rdcr+RdsonTop)*Iripple/2-Vout)/L*OnTime, (Vin-(Rdcr+RdsonTop)*I102-Vout)/L*OnTime)","v":4.0280150150150143E-2},{"$f":"IF(I102<Icrit, (Vin-(Rdcr+RdsonTop)*Iripple/2-Vout)/L*OnTime, I102+((Vin-(Rdcr+RdsonTop)*J102-Vout)/L*OnTime)/2)","v":0.11616117394839941},{"$f":"IF(I102<Icrit, 0, I102-((Vin-(Rdcr+RdsonTop)*K102-Vout)/L*OnTime)/2)","v":7.5867559153235911E-2},0.54701349741121619,{"$f":"IF(I102<Icrit, 1000*SQRT((J102*CoutEsr)^2+(((J102/2)-I102)*(OnTime+OffTime)/Cout)^2), 1000*J102*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":0.54701349741121619},1,{"$f":"IF(I102<Icrit, 1000*((N102/1000)*O102), 1000*J102*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":0.54701349741121619},2.9566615210009458E-6,0.10509516956655465,302674.08835167746,3.303883743223168E-6,0,{"$f":"S102*(T102*Iq_active+U102*Iq_sleep)","v":6.6E-4},9.6701536727554452E-2,{"$f":"W102^2*Rdcr","v":1.1221424646564674E-3},{"$f":"Core_Loss/1000*S102/$S$106","v":9.9963172183885146E-2},{"$f":"(Y102+X102*(1+Ltc*(Ta-25)))/(1-X102*Ltc*ThetaCa)","v":0.10110346704753331},1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,2.9681205065893387E-2,2.6429218024908457E-6,2.6429218024908457E-6,3.1349076621290224E-2,6.7515928364016999E-4,1.2152364647319851E-3,{"$f":"20*VIN_nom/24","v":40},66.127907657935182,{"$f":"IF(I102<Icrit, Vin*(I102+Iripple/2)*AK102/1000000000/2*S102, Vin*(I102-Iripple/2)*AJ102/1000000000/2*S102 + Vin*(I102+Iripple/2)*AK102/1000000000/2*S102)","v":7.7831728343781617E-2},5.5788887964981188E-2,0.1348358527734948,{"$f":"(AI102+AL102+AM102+AH102*(1+RdsonTopTc*(Ta-25)))/(1-AH102*RdsonTopTc*ThetaJA)","v":0.1355279355266025},9.1460257830570602E-2,2.5429535437800732E-3,3.3294149718684526E-3,{"$f":"IF(I102<Icrit, Vin*Idss*R102, QrrBot*(I102-Iripple/2)/1*S102*Vin+Vin*Idss*R102)","v":3.3064260568200663E-3},9.4146358897942081E-4,7.5773046176679393E-3,{"$f":"(AR102+AS102+AT102+AQ102*(1+RdsonBotTc*(Ta-25)))/(1-AQ102*RdsonBotTc*ThetaJA)","v":1.0125020153413012E-2},{"$f":"Vin*V102+Vout*Ifb/0.8","v":3.1732432885906041E-2},{"$f":"(Vin-Vdd)*(S102*QgBot+S102*QgTop)+AW102","v":7.0816435240669801E-2},4.5446514366004375E-3,0.22101404235728575,{"$f":"SUM(Z102,AC102,AF102,AZ102)","v":0.32212082826264893},0.48,0.59841358444669057,8.6281608546023218E-4,3.1762241372827694E-3,5.4391623124737401E-2,0.16809917910440264,4.1221047257700687E-3,1.1737179185567104E-3,9.4465875347981912E-3,1.3989693636144176E-3,0.12462358370670922,3.2949173109184487E-6,8.4268604371843882E-7,8.8286493437721145E-2,0.45558543674240748,0.59841358444669057,59.841358444669055,96,73.551124384272143,0.73551124384272137,302.67408835167748,null,6.9551725873790063E-2,null,0.22101404235728575,7.0816435240669801E-2,0.10110346704753331,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR102, IF(MODE_ILIM=4,#REF!,#REF!))","v":59.841358444669055},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ102, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.22101404235728575},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA102, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0816435240669801E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB102, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10110346704753331},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S102, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":302.67408835167748},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P102, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54701349741121619}]
[null,null,null,null,null,null,null,97,{"$f":"IF(PLOT_TYPE=1, H103/100*Iout, min_I*EXP(H103*rr/100))","v":9.7000000000000003E-2},4.0279392830330323E-2,0.11716117423516606,7.6867937813254406E-2,0.54700321283775366,0.54700321283775366,1,0.54700321283775366,2.9563572571897045E-6,0.10510484896341331,302701.9650146304,{"$f":"IF(1/S103-OnTime-Q103>Tsleep, OnTime+Q103+Tsleep, 1/S103)","v":3.3035794794119267E-6},0,6.6E-4,9.7694356057402634E-2,1.1453024646564676E-3,9.9972378917351654E-2,0.10113621443091272,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,2.998664463148884E-2,2.6975965687655954E-6,2.6975965687655954E-6,3.1672391048190932E-2,{"$f":"RdsonTop*AG103^2","v":6.8915742368544375E-4},1.2153483895337412E-3,40,65.563380422735094,7.8129490629941747E-2,5.5794026191496676E-2,0.13513886521097218,0.13584533743592839,9.2403520727972824E-2,{"$f":"RdsonBot*AP103^2","v":2.5956768354491707E-3},3.3297216151609347E-3,3.3503196657667621E-3,9.5147044775359282E-4,7.6315117286812903E-3,1.0232100693117339E-2,3.1732432885906041E-2,7.0820034926280251E-2,4.5450700046946761E-3,0.22144254306002065,0.32258213102352951,0.48499999999999999,0.6005581121332032,8.7479922823555209E-4,3.2202160802394949E-3,5.4028773506626313E-2,0.16733761189056673,4.1485807288982081E-3,1.1781717440276932E-3,9.4498273742252229E-3,1.418186981434212E-3,0.12379221267643289,3.3403371188347889E-6,8.3698734950478372E-7,8.7693910260895624E-2,0.45314646779605028,0.6005581121332032,60.055811213320318,97,73.159788011658193,0.73159788011658189,302.70196501463039,null,6.9087742346135531E-2,null,0.22144254306002065,7.0820034926280251E-2,0.10113621443091272,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR103, IF(MODE_ILIM=4,#REF!,#REF!))","v":60.055811213320318},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ103, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.22144254306002065},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA103, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0820034926280251E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB103, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10113621443091272},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S103, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":302.70196501463039},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P103, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54700321283775366}]
[null,null,null,null,null,null,null,98,{"$f":"IF(PLOT_TYPE=1, H104/100*Iout, min_I*EXP(H104*rr/100))","v":9.8000000000000004E-2},4.0278635510510502E-2,0.11816117452193273,7.78683164732729E-2,0.54699292826429124,0.54699292826429124,1,0.54699292826429124,2.9560530445562964E-6,0.10511452851485993,302729.84212279669,{"$f":"IF(1/S104-OnTime-Q104>Tsleep, OnTime+Q104+Tsleep, 1/S104)","v":3.3032752667785186E-6},0,6.600000000000001E-4,9.8687320388541125E-2,1.1687024646564676E-3,9.998158579785732E-2,0.1011692061346029,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,3.0292158383936965E-2,2.7528445786725677E-6,2.7528445786725677E-6,3.1995782084846665E-2,{"$f":"RdsonTop*AG104^2","v":7.0330255892882352E-4},1.2154603161230286E-3,40,65.008410223495474,7.8427306554634812E-2,5.5799164500073883E-2,0.13544193137083171,0.13616294543494495,9.3347007132690132E-2,{"$f":"RdsonBot*AP104^2","v":2.6489537771516728E-3},3.3300282633507644E-3,3.3942213081841408E-3,9.6148155692850942E-4,7.6857311284634147E-3,1.0339750597598073E-2,3.1732432885906048E-2,7.0823634669380658E-2,4.545488579473793E-3,0.22187181928139746,0.32304445419660638,0.49,0.60267307337356313,8.8680767747895183E-4,3.2642981025646067E-3,5.3670731209976869E-2,0.16658613274063341,4.1747056888028003E-3,1.1825694794002108E-3,9.4530269394161436E-3,1.4374398086403498E-3,0.12297185631338217,3.3858475566292815E-6,8.3136416940537592E-7,8.7109178721800171E-2,0.45074096389382168,0.60267307337356313,60.267307337356314,98,72.614496083320674,0.72614496083320679,302.7298421227967,null,6.8629906042727645E-2,null,0.22187181928139746,7.0823634669380658E-2,0.1011692061346029,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR104, IF(MODE_ILIM=4,#REF!,#REF!))","v":60.267307337356314},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ104, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.22187181928139746},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA104, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0823634669380658E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB104, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.1011692061346029},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S104, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":302.7298421227967},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P104, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54699292826429124}]
[null,null,null,null,null,null,null,99,{"$f":"IF(PLOT_TYPE=1, H105/100*Iout, min_I*EXP(H105*rr/100))","v":9.9000000000000005E-2},4.0277878190690682E-2,0.11916117480869938,7.8868695133291408E-2,0.54698264369082872,0.54698264369082872,1,0.54698264369082872,2.9557488830878114E-6,0.10512420822089817,302757.7196761868,{"$f":"IF(1/S105-OnTime-Q105>Tsleep, OnTime+Q105+Tsleep, 1/S105)","v":3.3029711053100336E-6},0,6.6E-4,9.9680425387688648E-2,1.1923424646564675E-3,9.99907928254056E-2,0.10120244216515334,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,3.0597744849917688E-2,2.808665969701993E-6,2.808665969701993E-6,3.2319248331446566E-2,{"$f":"RdsonTop*AG105^2","v":7.1759472933157192E-4},1.21557224449989E-3,40,64.462756406747161,7.8725176119145784E-2,5.5804302890714752E-2,0.13574505125436043,0.13648075959344011,9.4290712960804463E-2,{"$f":"RdsonBot*AP105^2","v":2.7027845193996732E-3},3.3303349164380551E-3,3.4381309842646543E-3,9.7149691721703721E-4,7.7399628179197471E-3,1.044797006856452E-2,3.1732432885906041E-2,7.0827234469972369E-2,4.5459071609379453E-3,0.22230187129291495,0.32350779806006535,0.495,0.60475905198850033,8.9884096501386464E-4,3.3084684801574097E-3,5.3317401310575843E-2,0.16584454244185334,4.2004865346589532E-3,1.1869122316483353E-3,9.456187022608864E-3,1.4567270678207621E-3,0.12216229712458754,3.4314468064431097E-6,8.258150123368843E-7,8.6532143783894386E-2,0.44836826422463805,0.60475905198850033,60.475905198850036,99,71.912167665597565,0.71912167665597559,302.75771967618681,null,6.8178095581955117E-2,null,0.22230187129291495,7.0827234469972369E-2,0.10120244216515334,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR105, IF(MODE_ILIM=4,#REF!,#REF!))","v":60.475905198850036},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ105, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.22230187129291495},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA105, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0827234469972369E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB105, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10120244216515334},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S105, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":302.75771967618681},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P105, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54698264369082872}]
[null,null,null,null,null,null,null,100,{"$f":"IF(PLOT_TYPE=1, H106/100*Iout, min_I*EXP(H106*rr/100))","v":0.1},4.0277120870870861E-2,0.12016117509546603,7.9869073793309903E-2,0.54697235911736619,0.54697235911736619,1,0.54697235911736619,2.9554447727713428E-6,0.10513388808153172,302785.59767481143,{"$f":"IF(1/S106-OnTime-Q106>Tsleep, OnTime+Q106+Tsleep, 1/S106)","v":3.3026669949935651E-6},0,6.600000000000001E-4,0.1006736668919463,1.2162224646564677E-3,0.1,0.1012359225291701,1.1627003288490194E-2,6.7593602735280891E-7,6.7593602735280891E-7,3.0903402613853288E-2,2.8650608793417426E-6,2.8650608793417426E-6,3.264278844316635E-2,{"$f":"RdsonTop*AG106^2","v":7.3203397485623121E-4},1.2156841746643679E-3,40,63.926186331551449,7.9023099324759677E-2,5.5809441363421246E-2,0.13604822486284529,0.13679877998124687,9.52346342888198E-2,{"$f":"RdsonBot*AP106^2","v":2.7571692127100764E-3},3.330641574422926E-3,3.4820486942007635E-3,9.8151652933206601E-4,7.794206797955755E-3,1.0556759308101047E-2,3.1732432885906048E-2,7.0830834328056785E-2,4.5463257490872943E-3,0.22273269936649198,0.3239721628925688,0.5,0.60681661652833174,9.1089863493293657E-4,3.352725534376432E-3,5.2968691366978272E-2,0.16511264699191486,4.225930014403606E-3,1.1912010787918307E-3,9.459308395315268E-3,1.4760480018971725E-3,0.12136332330566635,3.477133097899686E-6,8.2033842621566672E-7,8.5962654465660454E-2,{"$f":"SUM(BD106:BO106)","v":0.44602772526146128},0.60681661652833174,60.681661652833171,100,71.049894896969974,0.71049894896969978,302.78559767481141,null,6.7732192756975215E-2,null,0.22273269936649198,7.0830834328056785E-2,0.1012359225291701,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR106, IF(MODE_ILIM=4,#REF!,#REF!))","v":60.681661652833171},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ106, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.22273269936649198},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA106, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.0830834328056785E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB106, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.1012359225291701},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S106, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":302.78559767481141},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P106, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54697235911736619}]
[null,null,null,null,null,null,null,null,{"$f":"Losses!$E$5/1000","v":0.5},3.9974192942942938E-2,0.52016128980212795,0.48002053780070869,0.54285852973237891,0.54285852973237891,1,0.54285852973237891,{"$f":"IF(I107<Icrit, L*J107/(Vout+J107/2*(RdsonBot+Rdcr)), L*J107/(Vout+I107*(RdsonBot+Rdcr)))","v":2.837768877376993E-6},{"$f":"OnTime*S107","v":0.10901827080958405},{"$f":"IF(I107<Icrit,I107/((OnTime+Q107)*J107/2),1/(OnTime+Q107))","v":313972.61993160215},{"$f":"IF(1/S107-OnTime-Q107>Tsleep, OnTime+Q107+Tsleep, 1/S107)","v":3.1849910995992153E-6},{"$f":"IF(1/S107-OnTime-Q107>Tsleep, 1/S107-OnTime-Q107-Tsleep, 0)","v":0},6.6E-4,{"$f":"IF(I107<Icrit,Iripple*SQRT((OnTime+OffTime)*S107/3), SQRT(I107^2+Iripple^2/12))","v":0.50013516893482968},3.0016222464656475E-2,0.10369470091797611,0.1343561817893672,{"$f":"Iripple/SQRT(12)*SQRT((OnTime+Q107)*S107)","v":1.1627003288490194E-2},{"$f":"RCoutEsr*AA107^2","v":6.7593602735280891E-7},{"$f":"AB107","v":6.7593602735280891E-7},{"$f":"SQRT($R107)*SQRT($I107^2*(1-R107)+(Iripple^2)/12)","v":0.15587834915469834},{"$f":"RCinEsr*AD107^2","v":7.2894179205582133E-5},{"$f":"AE107","v":7.2894179205582133E-5},{"$f":"IF(I107<Icrit,Iripple*SQRT((OnTime)*S107/3), SQRT(OnTime*S107*(I107^2+Iripple^2/12)))","v":0.16513420474805332},{"$f":"RdsonTop*AG107^2","v":1.8734012931929361E-2},{"$f":"QgTop*S107*Vdd","v":1.2606000690253828E-3},40,{"$f":"IF(I107<Icrit, Csw*Vin/Iripple*1000000000, Csw*Vin/(I107+Iripple/2)*1000000000)","v":14.765296373279202},0.20250825255465996,{"$f":"IF(I107<Icrit, Csw*(Vin)^2*S107/2, Csw*Vin^2*S107/2)","v":5.7871433305792912E-2},0.26164028592947824,0.28134913300627629,{"$f":"IF(I107<Icrit,Iripple*SQRT((OffTime)*S107/3), SQRT(OffTime*S107*(I107^2+Iripple^2/12)))","v":0.48177549614479187},{"$f":"RdsonBot*AP107^2","v":7.0560719120410356E-2},{"$f":"QgBot*S107*Vdd","v":3.4536988192476244E-3},2.1695522887330062E-2,{"$f":"IF(I107<Icrit, dead1*S107*(I107+Iripple/2)*((I107+Iripple/2)*BDserR+VSD), dead1*S107*(I107+Iripple/2)*((I107+Iripple/2)*BDserR+VSD)+dead2*S107*(I107-Iripple/2)*((I107-Iripple/2)*BDserR+VSD))","v":5.3380438798102305E-3},3.0487265586387917E-2,0.10238411844133713,3.1732432885906041E-2,7.2275403325053902E-2,{"$f":"AI107+AR107","v":4.7142988882730077E-3},{"$f":"AO107+AV107+AX107+AY107","v":0.46072295366094029},0.59515270556554045,{"$f":"Vout*I107","v":2.5},{"$f":"BB107/(BB107+BA107)","v":0.80771459046419003},6.3676493380629114E-3,2.3228854823759769E-2,{"$f":"Vin*S107*(QgBot+QgTop)/($BB107+$BA107)","v":1.4621982704130117E-2},8.4532270559384837E-2,{"$f":"AS107/(BA107+BB107)","v":7.0095161535385043E-3},{"$f":"AT107/($BB107+$BA107)","v":1.7246463705043184E-3},9.8500036949929239E-3,{"$f":"X107/($BB107+$BA107)","v":9.6978163341288094E-3},{"$f":"Y107/($BB107+$BA107)","v":3.3502289154107898E-2},{"$f":"(AF107)/($BB107+$BA107)","v":2.3551076841704019E-5},{"$f":"(AC107)/($BB107+$BA107)","v":2.1838535660530624E-7},2.3351159118932027E-2,{"$f":"SUM(BD107:BO107)","v":0.21390995771374044},{"$f":"BC107","v":0.80771459046419003},{"$f":"100*BQ107","v":80.771459046418997},{"$f":"I107*1000","v":500},72.049894896970002,{"$f":"BT107/100","v":0.72049894896970001},{"$f":"S107/1000","v":313.97261993160214},null,{"$f":"AM107/($BB107+$BA107)","v":1.8697440420865682E-2},null,0.46072295366094029,7.2275403325053902E-2,0.1343561817893672,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR107, IF(MODE_ILIM=4,#REF!,#REF!))","v":80.771459046418997},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ107, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.46072295366094029},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA107, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.2275403325053902E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB107, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.1343561817893672},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S107, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":313.97261993160214},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P107, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54285852973237891}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(MODE=1, MODE=2,MODE=3),Efficiency!BD107,IF(AND(MODE=4,MODE_ILIM=4),#REF!,#REF!))","v":6.3676493380629114E-3},{"$f":"IF(OR(MODE=1, MODE=2,MODE=3),Efficiency!BE107,IF(AND(MODE=4,MODE_ILIM=4),#REF!,#REF!))","v":2.3228854823759769E-2},null,{"$f":"IF(OR(MODE=1, MODE=2,MODE=3),Efficiency!BG107,IF(AND(MODE=4,MODE_ILIM=4),#REF!,#REF!))","v":8.4532270559384837E-2},null,null,{"$f":"IF(OR(MODE=1, MODE=2,MODE=3),Efficiency!BJ107,IF(AND(MODE=4,MODE_ILIM=4),#REF!,#REF!))","v":9.8500036949929239E-3},{"$f":"IF(OR(MODE=1, MODE=2,MODE=3),Efficiency!BK107,IF(AND(MODE=4,MODE_ILIM=4),#REF!,#REF!))","v":9.6978163341288094E-3},{"$f":"IF(OR(MODE=1, MODE=2,MODE=3),Efficiency!BL107,IF(AND(MODE=4,MODE_ILIM=4),#REF!,#REF!))","v":3.3502289154107898E-2},null,null,{"$f":"IF(OR(MODE=1, MODE=2,MODE=3),Efficiency!BO107,IF(AND(MODE=4,MODE_ILIM=4),#REF!,#REF!))","v":2.3351159118932027E-2}]
[null,null,null,null,null,null,null,1.0000000000000001E-5,"A","min_I",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Load (A)","High-side MOSFET Rdson %","Low-side MOSFET Rdson %","Gate Drive (Qg) Loss from Vin %","High-side MOSFET Switching Loss %","Reverse Recovery & Leakage Loss %","Deadtime Loss %",null,"Inductor Cu Loss %","Inductor Core Loss %","Cin ESR %","Cout ESR %","Quiescent Current Loss %","Total Loss %","Overall Eff %"]
[null,null,null,null,null,null,null,{"$f":"Iout","v":0.1},"A","max_I",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"I107","v":0.5},{"$f":"BD107","v":6.3676493380629114E-3},{"$f":"BE107","v":2.3228854823759769E-2},1.4621982704130117E-2,8.4532270559384837E-2,7.0095161535385043E-3,1.7246463705043184E-3,null,9.6978163341288094E-3,3.3502289154107898E-2,2.3551076841704019E-5,2.1838535660530624E-7,2.3351159118932027E-2,0.21390995771374044,0.80771459046419003]
[null,null,null,null,null,null,null,{"$f":"LOG(max_I/min_I,EXP(1))","v":9.2103403719761836},null,"rr",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"10mA",{"$f":"BD70","v":4.9635909879833045E-4},{"$f":"BE70","v":1.8294738702556951E-3},6.9279123151041164E-2,0.19934472768966896,3.0356464267486697E-3,9.9297300740727214E-4,null,8.0864066677909712E-4,0.15873423345615373,1.9034657422379571E-6,1.076509053124807E-6,0.11260024650582681,0.55643989165396324,0.50963831347923305]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"50ma",{"$f":"BD85","v":6.6349711715413858E-4},{"$f":"BE85","v":2.4440692083442191E-3},6.1401512071476608E-2,0.18281159546901357,3.610570821146956E-3,1.0881858297951254E-3,null,1.0785244086783912E-3,0.14068483416664218,2.5386751247581634E-6,9.5278139415830279E-7,9.9734712191971248E-2,0.50290545696734568,0.55678146372288606]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"100mA",{"$f":"BD91","v":7.3281925737107465E-4},{"$f":"BE91","v":2.6988015486837662E-3},5.8730155983891169E-2,0.17720498836319862,3.8055169460205875E-3,1.1206751621440378E-3,null,1.1901442947246424E-3,0.13456414958570675,2.8018536023041876E-6,9.1082534553249082E-7,9.5371957419933956E-2,0.48483096285915728,0.57268847374110898]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"500mA",{"$f":"BD106","v":9.1089863493293657E-4},{"$f":"BE106","v":3.352725534376432E-3},5.2968691366978272E-2,0.16511264699191486,4.225930014403606E-3,1.1912010787918307E-3,null,1.4760480018971725E-3,0.12136332330566635,3.477133097899686E-6,8.2033842621566672E-7,8.5962654465660454E-2,0.44602772526146128,0.60681661652833174]

{"sheet":"Schematic Mgmt","index":10,"n_rows":2,"n_cols":1,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
[]
[{"$f":"'Variable Mgmt'!K27","v":"SCH_COT3_LM5164"}]

{"sheet":"Efficiency Plots","index":11,"n_rows":2,"n_cols":1,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
[]
[{"$f":"IF(PLOT_TYPE=1, \"EFF_LINEAR\", \"EFF_LOG\")","v":"EFF_LINEAR"}]