{"text_format":"1","workbook":"xlsx","n_sheets":12,"sheets":["Instructions","Design Converter","BOM & Schematic","Fsw & Ripple","Losses","EVM","Design EMI Filter","Variable Mgmt","Standard Value Calculator","Efficiency","Schematic Mgmt","Efficiency Plots"],"not_rendered":{"charts":6,"images":26,"macros":1,"external_links":0,"defined_names":205,"comments":4,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Instructions","index":0,"n_rows":74,"n_cols":3,"rows_kept":74,"cut":false,"hidden":true,"merged":[[65,1,66,15],[69,1,70,15],[73,1,74,15],[77,1,78,15],[20,2,21,15],[50,1,52,15],[54,1,55,15],[56,1,57,15],[60,1,62,15],[24,1,26,15],[38,1,39,15],[41,1,43,15],[46,1,47,15],[28,1,28,15],[29,1,31,15],[33,1,35,15],[0,0,0,16],[7,1,9,15],[16,2,17,15],[11,1,14,15],[18,2,19,15]]}
["                         LM5164 Low IQ DC/DC Converter Design Tool  "]
[]
[]
[null,"Design Regulator tab"]
[null,"Start with Step 1, and then work down towards the bottom of the worksheet."]
[]
[null,"Step 1. Operating Specifications"]
[null,"First, enter the values in the yellow shaded cells to define the power supply parameters.  If a particular specification is not known, enter an estimate. It can be changed later, if necessary, to optimize component values.  Cells  with a red mark in the upper right corner have a comment to provide additional information.  Hold the cursor over the cell to read the comment.  A red font indicates an erroneous entry and requires an adjustment to the entry.  Consult the entry's comments for the entry specific requirements."]
[]
[]
[]
[null,"Second, select a desired mode of operation. PFM mode requires the fewest external components and the lowest inductance.  As a result, it can provide the smallest solution size. At light loads, a PFM converter has a relatively longer sleep time interval and thus operates at lower input quiescent current levels.  COT mode offers nearly constant switching frequency, relatively higher conversion efficiencies at medium to heavy loads, and enables the lowest output voltage ripple.  Options COT1, COT2, and COT3 enable you to select a ripple generation method (a requirement for the stable operation in COT mode):"]
[]
[]
[]
[]
[null,"-COT1: ","Type 1 ripple generation method requires a single resistor in series with the output capacitor.  It is the simplest, the most compact, and the most economical method that works with fixed and adjustable device options, however, the output voltage ripple is the highest."]
[]
[null,"-COT2: ","Type 2 ripple generation method requires a feedforward capacitor in addition to the series resistor.  The feedforward capacitor reduces the required minimum value of the series resistor and ultimately the output voltage ripple by the VOUT / 1.223V factor.  It only works with an adjustable device option (i.e. external feedback resistor network)."]
[]
[null,"-COT3:","Type 3 ripple generation method three external components to generate and inject required voltage ripple into the FB node.  In return, it provides the lowest output voltage ripple. It also only works with an adjustable device option (i.e. external feedback resistor network)."]
[]
[]
[null,"Step 2. Filter Inductor"]
[null,"First, select an inductor current limit level.  In PFM Mode, 1.25A, 0.75A, 0.5A, and 1.25A - MOD options are available.  For the 500mA max load, select either 1.25A or 1.25A - MOD option.  The 1.25A - MOD option enables higher efficiency at the expense of slightly worse transient operation.  For the 300mA and 200mA max loads, select 0.75A and 0.5A options respectively. In COT Mode, 0.75A and 0.5A options are available.   For the 500mA and 300mA max loads, select 0.75A and 0.5A options respectively."]
[]
[]
[]
[null,"Second, select the filter inductance value based on the suggested value. Enter the inductor RDC for accurate efficiency estimates."]
[null,"In PFM mode, selected inductance defines the switching frequency.  You may select lower or higher inductance to increase or decrease the switching frequency.  Watch the minimum output capacitance.  At very low switching frequencies, the required minimum capacitance may become excessive."]
[]
[]
[]
[null,"In COT mode, the suggested inductance is  derived based on the target inductor (peak-to-peak) ripple current of 40% of the DC full load output current at nominal input voltage. It may be acceptable to use higher ripple current with the proviso that peak inductor current remains below the ILIM setting.  Pk-to-Pk Ripple Current value will turn red if this is violated.  If this happens, increase the selected inductance or decrease the Input Voltage (max) or both."]
[]
[]
[]
[null,"Step 3. Output Capacitors and Ripple Generation"]
[null,"First, select the output capacitance based on the minimum recommended value.  Make sure that the nominal capacitance is appropriately derated for applied voltage, especially with ceramics.  For PFM and COT3 modes, ensure that the capacitor ESR does not exceed the maximum allowable value.  "]
[]
[]
[null,"Second, for COT modes, select the values for the ripple generation components based on the minimum recommended values.  Ensure that the output voltage ripple meets any of your minimum ripple requirements by reviewing the VOUT Ripple vs. IOUT plot in the fSW&Ripple tab.  For accurate output voltage ripple estimates in COT3 mode, ensure that the Output Capacitor ESR is set to the levels of a typical ceramic capacitor ESR (e.g. 10 mW)."]
[]
[]
[]
[null,"Step 4. Input Capacitors"]
[null,"Select the input capacitance based on the minimum recommended value.  Make sure that the nominal capacitance is appropriately derated for applied voltage, especially with ceramics.  "]
[]
[]
[null,"Step 5. Feedback, Soft-Start, UVLO"]
[null,"First, review the feedback resistor network. With an adjustable device option, an external feedback resistor network is required. The resistor values are automatically calculated based on the selected VOUT in Step 1.  For lowering the leakage current through the resistors, adjust the upper FB resistor (R1) until the lower FB resistor (R2) reaches its upper end of the range (100kW).  Keeping the upper FB resistor below 1MW is recommended."]
[]
[]
[]
[null,"Second, select one out of three soft-start configurations.  If the external soft-start option is selected, enter a desired soft start time.  "]
[]
[null,"Third, select one out of the two UVLO options.  If the external UVLO option is selected, define desired UVLO thresholds and hysteresis.  Keeping the upper UVLO resistor at 1MW or higher is recommended for the minimum leakage current."]
[]
[]
[null,"Step 6. Efficiency and Thermals"]
[null,"Enter the LM5166's junction-to-ambient thermal impedance (dependent on your PCB design, air flow, etc.) and ambient temperature. Device power dissipation and junction temperature are derived at the maximum load.  Ensure that the junction temperature is within the recommended range."]
[]
[]
[]
[null,"BOM & Schematic tab"]
[null,"This tab summarizes the converter schematic and BOM.  It also helps you estimate the total solution size. Select a package size for each external component (i.e. inductor, capacitors, and resistors) for accurate solution size estimates."]
[]
[]
[null,"Design EMI Filter tab"]
[null,"In case an EMI filter is needed, a simple EMI filter design aid is given in this tab.  It is based on the guidelines documented in TI's literature number SNVA489C (aka AN-2162).  Suggest reviewing the note before using the design aid."]
[]
[]
[null,"fSW & Ripple tab"]
[null,"In this tab, the switching/burst frequency (COT/PFM mode) and the output voltage ripple as a function of the load current are plotted."]

{"sheet":"Design Converter","index":1,"n_rows":58,"n_cols":17,"rows_kept":58,"cut":false,"hidden":false,"merged":[[2,14,2,15],[0,0,0,16]]}
["                          LM5163/4 Low IQ DC/DC Converter Design Tool  "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"http://www.ti.com/ww/en/analog/power_management/widevin"]
["About",null,"xx",null,null,"= Input Box",null,null,null,null,null,null,null,null,"Terms Of Use",null,"                "]
[]
["Step 1: Operating Specifications"]
[null,null,null,"Input Voltage - Min, VIN(min) ",18,"V"]
[null,null,null,"Input Voltage - Nom, VIN(nom)",48,"V"]
[null,null,null,"Input Voltage - Max, VIN(max)",70,"V"]
[null,null,null,"Output Voltage, VOUT ",12,"V"]
[null,null,null,"Full Load Current, IOUT",1,"A"]
[null,null,null,"Mode of Operation",null,null,{"$f":"MODE","v":3}]
[null,null,null,"Switching Frequency at VIN(nom)",300,"kHz"]
[null,null,null,"Timing Resistance, RT",{"$f":"'Standard Value Calculator'!J4/1000","v":100},"kΩ"]
[]
["Step 2: Buck Inductor"]
[null,null,null,"Recommended Buck Inductance ",{"$f":"Lopt*1000000","v":75},"µH"]
[null,null,null,"Inductance, LF ",68,"µH"]
[null,null,null,"Inductor DCR ",120,"mΩ"]
[null,null,null,{"$f":"CHOOSE(MODE, \"Pk-to-Pk Ripple Current\",\"Pk-to-Pk Ripple Current\",\"Pk-to-Pk Ripple Current\", \"Resulting PFM Switching Frequency\")","v":"Pk-to-Pk Ripple Current"},{"$f":"Iripple_Vinnom*1000","v":445.12451162960531},"mApk-pk"]
[null,null,null,{"$f":"CHOOSE(MODE, 'Variable Mgmt'!H88,'Variable Mgmt'!H88,'Variable Mgmt'!H88, 'Variable Mgmt'!H89)","v":"% Ripple Current at Nom VIN"},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), 'Variable Mgmt'!B96*100, Ilim/2*1000)","v":44.512451162960531},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), \"%\", \"mA\")","v":"%"}]
[]
[{"$f":"IF(MODE=4, \"Step 3: Output Capacitors\", \"Step 3: Output Capacitors, Ripple Generation\")","v":"Step 3: Output Capacitors, Ripple Generation"}]
[null,null,null,"Minimum Output Capacitance ",{"$f":"'Variable Mgmt'!B116","v":6.8859604278673592},"µF"]
[null,null,null,"Output Capacitance, COUT ",33,"µF"]
[null,null,null,{"$f":"IF(OR(MODE=1,MODE=2),\"Recommended Series Resistance\",IF(MODE=3,\"Maximum Allowable ESR\",\"*Higher Cout Improves Light-Load Eff\"))","v":"Maximum Allowable ESR"},{"$f":"'Variable Mgmt'!B272","v":0.13400000000000001},"Ω"]
[null,null,null,{"$f":"IF(OR(MODE=1,MODE=2),\"Total ESR & Series Resistance, Rser\",IF(MODE=3,\"Output Capacitor ESR\",\"*PFM Hysteresis Sets Output Ripple\"))","v":"Output Capacitor ESR"},5.0000000000000001E-3,"Ω"]
[null,null,null,{"$f":"CHOOSE(MODE, \"Resulting Output Voltage Ripple\",\"Resulting Output Voltage Ripple\", \"Output Voltage Ripple\",\"Output Voltage Ripple\")","v":"Output Voltage Ripple"},{"$f":"CHOOSE(MODE, Vripple2*1000,Vripple2*1000,Vripple2*1000, PFM_Ripple)","v":6.0448909694310649},"mVpk-pk"]
[null,null,null,{"$f":"IF(MODE=1,\"\",IF(MODE=2,\"Minimum Feedforward Capacitance\", IF(MODE=3,\"Minimum Coupling Capacitance\",\"\")))","v":"Minimum Coupling Capacitance"},{"$f":"'Variable Mgmt'!B140","v":">47"},"pF"]
[null,null,null,{"$f":"IF(MODE=1,\"\",IF(MODE=2,\"Feedforward Capacitance, Cff\", IF(MODE=3,\"Coupling Capacitance, Cb\",\"\")))","v":"Coupling Capacitance, Cb"},56,"pF",null,null,null,null,null,"** Specify Inductor Core Loss **",100,"mW"]
[null,null,null,{"$f":"IF(MODE=3,\"Minimum Ripple Generation Capacitance\",\"\")","v":"Minimum Ripple Generation Capacitance"},{"$f":"'Variable Mgmt'!B144","v":">742"},"pF"]
[null,null,null,{"$f":"IF(MODE=3,\"Ripple Generation Capacitance, Ca\",\"\")","v":"Ripple Generation Capacitance, Ca"},2200,"pF"]
[null,null,null,{"$f":"IF(MODE=3,\"Ripple Generation Resistance, Ra\",\"\")","v":"Ripple Generation Resistance, Ra"},{"$f":"Ra","v":681},"kΩ"]
[null,null,null,{"$f":"IF(MODE=3,\"Amplitude of Injected Ripple\",\"\")","v":"Amplitude of Injected Ripple"},20,"mVpk-pk"]
[]
["Step 4: Input Capacitors"]
[null,null,null,"Minimum Input Capacitance ",{"$f":"'Variable Mgmt'!B157","v":2.2000000000000002},"µF"]
[null,null,null,"Input Capacitance, CIN ",2.2000000000000002,"µF"]
[null,null,null,"Maximum Allowable ESR",{"$f":"'Variable Mgmt'!B159","v":1.7260766085084038},"Ω"]
[null,null,null,"Input Capacitor ESR ",3,"mΩ"]
[null,null,null,"Resulting Input Voltage Ripple ",{"$f":"CHOOSE(MODE, Vinripple2*1000,Vinripple2*1000,Vinripple2*1000, 'Variable Mgmt'!B165*1000)","v":293.43157456024653},"mVpk-pk"]
[]
["Step 5: Feedback, PGOOD, UVLO"]
[null,null,null,"Upper Feedback Resistor, RFB1 ",453,"kΩ"]
[null,null,null,"Lower Feedback Resistor, RFB2",{"$f":"IF(Vout=Vref,\"OPEN\",Rfb2_u/1000)","v":49.9},{"$f":"IF(Vout=Vref,\"\",\"kΩ\")","v":"kΩ"}]
[null,null,null,"Acutal Output Voltage Setpoint",{"$f":"'Variable Mgmt'!B201","v":12.0937875751503},"V"]
[null,null,null,"PGOOD Pull-up Resistance",20,{"$f":"\"kΩ\"","v":"kΩ"},null,null,null,null,null,null,null,null,null,null," "]
[null,null,null,"BST Capacitance, CBST ",2.2000000000000002,"nF"]
[null,null,null,{"$f":"\"Required Input Voltage UVLO Turn-on\"","v":"Required Input Voltage UVLO Turn-on"},6,"V"]
[null,null,null,"Upper UVLO Resistor, RUV1",1,"MΩ"]
[null,null,null,"Lower UVLO Resistor, RUV2",{"$f":"'Variable Mgmt'!F276","v":332},{"$f":"'Variable Mgmt'!G276","v":"kΩ"}]
[null,null,null,"Actual UVLO Turn-on Threshold",{"$f":"'Variable Mgmt'!B186","v":6.0180722891566267},"V"]
[null,null,null,"Actual UVLO Turn-off Threshold",{"$f":"'Variable Mgmt'!B187","v":5.6168674698795176},"V"]
[]
["Step 6: Efficiency & Thermals"]
[null,null,null,"Estimated Thermal Impedance, JJA",41,"°C/W"]
[null,null,null,"Ambient Temp, TA",25,"°C"]
[null,null,null,"IC Power Dissipation at Full Load, PD",{"$f":"'Variable Mgmt'!B26","v":0.92081499923575372},"W"]
[null,null,null,"IC Junction Temp at Full Load, TJ",{"$f":"E56+E55*'Variable Mgmt'!B26","v":62.753414968665901},"°C"]

{"sheet":"BOM & Schematic","index":2,"n_rows":53,"n_cols":13,"rows_kept":53,"cut":false,"hidden":false,"merged":[[0,0,0,16],[29,3,29,5],[41,3,41,5],[47,7,47,9],[30,3,30,5],[43,3,43,5],[44,3,44,5],[42,3,42,5],[39,3,39,5],[40,3,40,5],[38,3,38,5],[37,3,37,5],[36,3,36,5],[31,3,31,5],[34,3,34,5],[32,3,32,5],[33,3,33,5]]}
["                         LM5163/4 100V Low IQ DC/DC Converter Design Tool  "]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[{"$f":"\"VIN = \"&Vin&\" V, VOUT = \"&Vout&\" V, IOUT = \"&Iout&\" A \"&'Variable Mgmt'!B35&\" Converter\"","v":"VIN = 48 V, VOUT = 12 V, IOUT = 1 A COT Converter"}]
["Low IQ, High Efficiency, Synchronous Buck Converter BOM"]
["Count","Ref Des","Value","Description",null,null,"Size","Part Number","MFR","Footprint (mm)","Area (mm2)"]
[{"$f":"ROUNDUP('Design Converter'!E37/10,0)","v":1},"CIN",{"$f":"Cin*1000000","v":2.2000000000000002},{"$f":"IF(VIN_max>35, \"Capacitor, Ceramic, \"&'Variable Mgmt'!B257&\", 100V, X7R, 10%\", \"Capacitor, Ceramic, \"&'Variable Mgmt'!B257&\", 50V, X7R, 10%\")","v":"Capacitor, Ceramic, 2.2µF, 100V, X7R, 10%"},null,null,5,"Std","Std",{"$f":"CHOOSE(G31,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45)","v":"3.2 x 2.5"},{"$f":"CHOOSE(G31,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45)","v":8}]
[{"$f":"'Variable Mgmt'!D252","v":2},"COUT",{"$f":"'Variable Mgmt'!F253","v":"22µF"},{"$f":"CHOOSE(Cout_Voltage_Rating, \"Capacitor, Ceramic, \"&'Variable Mgmt'!F253&\", 6.3V, X7R, 10%\", \"Capacitor, Ceramic, \"&'Variable Mgmt'!F253&\", 10V, X7R, 10%\", \"Capacitor, Ceramic, \"&'Variable Mgmt'!F253&\", 16V, X7R, 10%\", \"Capacitor, Ceramic, \"&'Variable Mgmt'!F253&\", 25V, X7R, 10%\",  \"Capacitor, Ceramic, \"&'Variable Mgmt'!F253&\", 50V, X7R, 10%\")","v":"Capacitor, Ceramic, 22µF, 16V, X7R, 10%"},null,null,5,"Std","Std",{"$f":"CHOOSE(G32,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45)","v":"3.2 x 2.5"},{"$f":"(CHOOSE(G32,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45))*A32","v":16}]
[{"$f":"CHOOSE(MODE, \"-\", \"-\", \"1\",\"-\")","v":"1"},{"$f":"CHOOSE(MODE,\"-\",\"-\",\"Ca\",\"-\")","v":"Ca"},{"$f":"CHOOSE(MODE, \"-\",\"-\",'Variable Mgmt'!B293, \"-\")","v":"2200pF"},{"$f":"CHOOSE(MODE,\"-\",\"-\", \"Capacitor, Ceramic, \"&'Variable Mgmt'!B293&\", 16V, X7R, 10%\", \"-\")","v":"Capacitor, Ceramic, 2200pF, 16V, X7R, 10%"},null,null,1,{"$f":"CHOOSE(MODE, \"-\", \"-\", \"Std\", \"-\")","v":"Std"},{"$f":"H33","v":"Std"},{"$f":"CHOOSE(MODE,\"\",\"\",CHOOSE(G33,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),\"\")","v":"1.0 x 0.5"},{"$f":"CHOOSE(MODE,\"\",\"\",CHOOSE(G33,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),\"\")","v":0.5}]
[{"$f":"CHOOSE(MODE, \"-\", \"1\", \"1\",\"-\")","v":"1"},{"$f":"CHOOSE(MODE,\"-\",\"Cff\",\"Cb\",\"-\")","v":"Cb"},{"$f":"CHOOSE(MODE, \"-\",'Variable Mgmt'!B290,'Variable Mgmt'!B290, \"-\")","v":"56pF"},{"$f":"CHOOSE(MODE,\"-\",\"Capacitor, Ceramic, \"&'Variable Mgmt'!B290&\", 50V, X7R, 10%\", \"Capacitor, Ceramic, \"&'Variable Mgmt'!B290&\", 50V, X7R, 10%\", \"-\")","v":"Capacitor, Ceramic, 56pF, 50V, X7R, 10%"},null,null,1,{"$f":"CHOOSE(MODE, \"-\", \"Std\", \"Std\", \"-\")","v":"Std"},{"$f":"H34","v":"Std"},{"$f":"CHOOSE(MODE,\"\",CHOOSE(G34,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),CHOOSE(G34,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),\"\")","v":"1.0 x 0.5"},{"$f":"CHOOSE(MODE,\"\",CHOOSE(G34,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),CHOOSE(G34,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),\"\")","v":0.5}]
[1,"CBST","2.2nF","Capacitor, Ceramic, 2.2nF, 25V, X7R, 10%",null,null,1,{"$f":"CHOOSE(MODE, \"-\", \"Std\", \"Std\", \"-\")","v":"Std"},{"$f":"H35","v":"Std"},{"$f":"CHOOSE(MODE,\"\",CHOOSE(G35,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),CHOOSE(G35,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),\"\")","v":"1.0 x 0.5"},{"$f":"CHOOSE(MODE,\"\",CHOOSE(G35,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),CHOOSE(G35,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),\"\")","v":0.5}]
[]
[1,"LF",{"$f":"'Design Converter'!E17","v":68},{"$f":"\"Inductor, \"&Lf*1000000&\" µH, \"&Rdcr*1000&\" mΩ, >\"&ROUNDUP(Isat_min,2)&\"A\"","v":"Inductor, 68 µH, 120 mΩ, >1.8A"},null,null,4,"Various","Various",{"$f":"CHOOSE(G37,'Variable Mgmt'!T50,'Variable Mgmt'!T51,'Variable Mgmt'!T52,'Variable Mgmt'!T53,'Variable Mgmt'!T54,'Variable Mgmt'!T55,'Variable Mgmt'!T56)","v":"6.0 x 6.0"},{"$f":"CHOOSE(G37,'Variable Mgmt'!U50,'Variable Mgmt'!U51,'Variable Mgmt'!U52,'Variable Mgmt'!U53,'Variable Mgmt'!U54,'Variable Mgmt'!U55,'Variable Mgmt'!U56)","v":36}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(MODE_RSET=2,CHOOSE(G38,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),\"\")","v":""}]
[{"$f":"CHOOSE(MODE, \"1\",\"1\",\"1\", \"-\")","v":"1"},"RT",{"$f":"CHOOSE(MODE, 'Design Converter'!E13, 'Design Converter'!E13,'Design Converter'!E13,\"-\")","v":100},{"$f":"C39","v":100},null,null,1,{"$f":"CHOOSE(MODE, \"Std\",\"Std\",\"Std\",\"-\")","v":"Std"},{"$f":"H39","v":"Std"},{"$f":"CHOOSE(MODE,CHOOSE(G39,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),CHOOSE(G39,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),CHOOSE(G39,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),\"\")","v":"1.0 x 0.5"},{"$f":"CHOOSE(MODE,CHOOSE(G39,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),CHOOSE(G39,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),CHOOSE(G39,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),\"\")","v":0.5}]
[1,"RFB1",{"$f":"Rfb1_/1000","v":453},453,null,null,1,{"$f":"CHOOSE(MODE_VOUT,\"-\",\"Std\")","v":"Std"},{"$f":"H40","v":"Std"},{"$f":"(CHOOSE(MODE_VOUT,\"\",CHOOSE(G40,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45)))","v":"1.0 x 0.5"},{"$f":"CHOOSE(MODE_VOUT,\"\",CHOOSE(G40,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45))","v":0.5}]
[1,"RFB2",{"$f":"Rfb2_u/1000","v":49.9},49.9,null,null,1,{"$f":"CHOOSE(MODE_VOUT,\"-\",\"Std\")","v":"Std"},{"$f":"H41","v":"Std"},{"$f":"CHOOSE(MODE_VOUT,\"\",CHOOSE(G41,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45))","v":"1.0 x 0.5"},{"$f":"CHOOSE(MODE_VOUT,\"\",CHOOSE(G41,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45))","v":0.5}]
[{"$f":"IF(MODE=3,\"1\",\"-\")","v":"1"},{"$f":"CHOOSE(MODE,\"-\",\"-\",\"Ra\",\"-\")","v":"Ra"},{"$f":"'Variable Mgmt'!F296","v":"681k"},{"$f":"\"Resistor, Chip, \"&'Variable Mgmt'!B296&\", 1/16W, 1%\"","v":"Resistor, Chip, 681kΩ, 1/16W, 1%"},null,null,1,{"$f":"CHOOSE(MODE, \"-\", \"-\", \"Std\", \"-\")","v":"Std"},{"$f":"H42","v":"Std"},{"$f":"CHOOSE(MODE,\"\",\"\",CHOOSE(G42,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),\"\")","v":"1.0 x 0.5"},{"$f":"CHOOSE(MODE,\"\",\"\",CHOOSE(G42,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),\"\")","v":0.5}]
[1,"RPGOOD",100,100,null,null,1,"Std","Std",{"$f":"CHOOSE(G43,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45)","v":"1.0 x 0.5"},{"$f":"CHOOSE(G43,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45)","v":0.5}]
[{"$f":"CHOOSE(MODE_UVLO, \"1\", \"-\")","v":"1"},"RUV1",{"$f":"CHOOSE(MODE_UVLO, 'Variable Mgmt'!H275, \"-\")","v":"1M"},{"$f":"CHOOSE(MODE_UVLO, \"Resistor, Chip, \"&'Variable Mgmt'!C275&\", 1/16W, 1%\", \"-\")","v":"Resistor, Chip, 1MΩ, 1/16W, 1%"},null,null,2,{"$f":"CHOOSE(MODE_UVLO,\"Std\",\"-\")","v":"Std"},{"$f":"H44","v":"Std"},{"$f":"CHOOSE(MODE_UVLO,CHOOSE(G44,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),\"\")","v":"1.6 x 0.8"},{"$f":"CHOOSE(MODE_UVLO,CHOOSE(G44,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),\"\")","v":1.3}]
[{"$f":"CHOOSE(MODE_UVLO, \"1\", \"-\")","v":"1"},"RUV2",{"$f":"CHOOSE(MODE_UVLO, 'Variable Mgmt'!H276, \"-\")","v":"332k"},{"$f":"CHOOSE(MODE_UVLO, \"Resistor, Chip, \"&'Variable Mgmt'!C276&\", 1/16W, 1%\", \"-\")","v":"Resistor, Chip, 332kΩ, 1/16W, 1%"},null,null,1,{"$f":"CHOOSE(MODE_UVLO,\"Std\",\"-\")","v":"Std"},{"$f":"H45","v":"Std"},{"$f":"CHOOSE(MODE_UVLO,CHOOSE(G45,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),\"\")","v":"1.0 x 0.5"},{"$f":"CHOOSE(MODE_UVLO,CHOOSE(G45,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),\"\")","v":0.5}]
[1,"U1",{"$f":"CHOOSE(VARIANT, \"LM5163-Q1\", \"LM5164-Q1\")","v":"LM5164-Q1"},{"$f":"CHOOSE(VARIANT, \"IC, LM51643-Q1, Buck Converter, 6V–100V Input\", \"IC, LM5164-Q1, Buck Converter, 6V–100V Input\")","v":"IC, LM5164-Q1, Buck Converter, 6V–100V Input"},null,null,"SOIC-8",{"$f":"CHOOSE(VARIANT, \"LM5163QDDATQ1\", \"LM5164QDDATQ1\")","v":"LM5164QDDATQ1"},"TI","5.0 x 6.0",30]
[]
[null,{"$f":"\"Total Solution Size (padded by 15%) = \"&ROUND(K48,1)&\" mm^2 = \"&ROUND(M48,3)&\" in^2\"","v":"Total Solution Size (padded by 15%) = 110.2 mm^2 = 0.171 in^2"},null,null,null,null,null,null,null,null,{"$f":"SUM(K31:K46)*1.15","v":110.16999999999999},null,{"$f":"K48/25.4/25.4","v":0.17076384152768304}]
[]
["NOTES:"]
["* Inductor saturation current should be higher than the peak inductor current setting for all operating temperatures *"]
["** Effective input and output capacitances should be appropriately derated for applied voltage and temperature, particularly with ceramics **"]
["***Estimated total solution size does not include EMI filter***"]

{"sheet":"Fsw & Ripple","index":3,"n_rows":1,"n_cols":1,"rows_kept":1,"cut":false,"hidden":true,"merged":[[0,0,0,16]]}
["                         LM5164 Low IQ DC/DC Converter Design Tool  "]

{"sheet":"Losses","index":4,"n_rows":42,"n_cols":6,"rows_kept":42,"cut":false,"hidden":true,"merged":[[0,0,0,16]]}
["                         LM5166 Low IQ DC/DC Converter Design Tool  "]
[]
[]
[]
[null,null,null,"Load Current",500,"mA"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,"Inductor Core Loss Constant",0]

{"sheet":"EVM","index":5,"n_rows":85,"n_cols":15,"rows_kept":85,"cut":false,"hidden":false,"merged":[[0,0,0,16]]}
["LM5163/4 100V, Low IQ DC/DC Converter Design Tool  "]
[]
[null,"LM5164-Q1EVM-041 PCB Layout"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Top"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Layer"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Layer 2"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Layer 3"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bottom"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Layer"]

{"sheet":"Design EMI Filter","index":6,"n_rows":33,"n_cols":15,"rows_kept":33,"cut":false,"hidden":false,"merged":[[0,0,0,22],[32,10,32,12],[29,10,29,12],[31,10,31,12]]}
["                         LM5163/4 100V, Low IQ DC/DC Converter Design Tool  "]
[]
[]
[]
[]
[]
["Step 7: EMI Filter (Optional)"]
[null,null,null,"Desired Maximum Noise Level, Vnoise(MAX)",50,"dBmV"]
[null,null,null,"EMI Filter Inductance, LF(EMI)",22,"mH"]
[null,null,null,"Minimum EMI Filter Capacitance",{"$f":"'Variable Mgmt'!M164","v":4.7076016396939151},"mF"]
[null,null,null,"EMI Filter Capacitance, CF(EMI)",4.7,"mF"]
[null,null,null,"Minimum EMI Filter Damping Capacitance",{"$f":"'Variable Mgmt'!M168","v":8.8000000000000007},"mF"]
[null,null,null,"EMI Filter Damping Capacitance, CD(EMI)",10,"mF"]
[null,null,null,"Minimum Damping Capacitor ESR",{"$f":"'Variable Mgmt'!M169","v":3.1622776601683795},"Ω"]
[null,null,null,"Damping Capacitor ESR, ESR CD(EMI)",3.3,"Ω"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,"EMI Filter BOM"]
[null,null,null,null,null,null,null,"Count","Ref Des","Value","Description",null,null,"Part Number","MFR"]
[null,null,null,null,null,null,null,1,"LF(EMI)",{"$f":"'Variable Mgmt'!B298","v":"22µH"},{"$f":"\"Inductor, \"&Lf_emi*1000000&\" µH, \"&ROUNDUP(Isat_min,2)&\"A\"","v":"Inductor, 22 µH, 1.8A"},null,null,"Std","Std"]
[null,null,null,null,null,null,null,1,"CF(EMI)",{"$f":"'Variable Mgmt'!B299","v":"4.7µF"},{"$f":"IF(VIN_max>35, \"Capacitor, Ceramic, \"&'Variable Mgmt'!B299&\", 100V, X7R, 10%\", \"Capacitor, Ceramic, \"&'Variable Mgmt'!B299&\", 50V, X7R, 10%\")","v":"Capacitor, Ceramic, 4.7µF, 100V, X7R, 10%"},null,null,"Std","Std"]
[null,null,null,null,null,null,null,1,"CD(EMI)",{"$f":"'Variable Mgmt'!B300","v":"10µF"},{"$f":"IF(VIN_max>35, \"Capacitor, Electrolytic, \"&'Variable Mgmt'!B300&\", 100V, ESR>\"&ESR_Cd&ohm, \"Capacitor, Electrolytic, \"&'Variable Mgmt'!B300&\", 50V, ESR>\"&ESR_Cd&ohm)","v":"Capacitor, Electrolytic, 10µF, 100V, ESR>3.3Ω"},null,null,"Std","Std"]

{"sheet":"Variable Mgmt","index":7,"n_rows":320,"n_cols":21,"rows_kept":320,"cut":false,"hidden":true,"merged":[[4,4,4,7],[0,0,0,8]]}
["EXCEL Variables Names/Calculations",null,null,null,null,null,null,null,null,null,null,"LM5166"]
[null,"Input from user ="]
[null,"Output ="]
[null,"Constant"]
["Variable Name","Value","STD Units",null,"Notes",null,null,null,"Iteration"]
["Step 1: Operational Specs"]
["VIN_min",{"$f":"'Design Converter'!E6","v":18},"V","Minimum input voltage",null,null,null,null,1]
["VIN_nom",{"$f":"'Design Converter'!E7","v":48},"V","Nominal input voltage"]
["VIN_max",{"$f":"'Design Converter'!E8","v":70},"V","Maximum input voltage"]
[]
["Vout",{"$f":"'Design Converter'!E9","v":12},"V","Output Voltage",null,null,null,null,1]
["Iout",{"$f":"'Design Converter'!E10","v":1},"A","Maximum Output Current",null,null,null,null,1]
["Rout",{"$f":"Vout/Iout","v":12},"W","Load resistance"]
["Pout",{"$f":"Vout*Iout","v":12},"W","Output power"]
[]
["Efficiency",0.9,null,"Estimate of efficiency"]
["Pin",{"$f":"Pout/Efficiency","v":13.333333333333332},"W","Calculate input power assuming 90% efficiency"]
["Iin_Vinmin",{"$f":"Pin/VIN_min","v":0.7407407407407407},"A"]
["Iin_Vinnom",{"$f":"Pin/VIN_nom","v":0.27777777777777773},"A","Input currents at min, nom, max Vin"]
["Iin_Vinmax",{"$f":"Pin/VIN_max","v":0.19047619047619047},"A"]
[]
["Fsw",{"$f":"'Design Converter'!E12*1000","v":300000},"Hz","Nominal Switching Frequency",null,null,null,null,1]
["Vref",1.2,"V","Reference Voltage"]
["Rt",{"$f":"Vout*2500000000/Fsw","v":100000},"W","Frequency Set Resistor"]
[null,null,null,null,null,null,null,null,null,null,{"$f":"B34&\"_\"&F35&\"_\"&F39&\"_\"&I41&\"_\"&I36","v":"COT3_VOUTadj_UVLOadj_SSAdj_RsetGND"},null,null,null,null,null,"Vout<5V",100,1]
["Internal PD at Full Load",{"$f":" IF(OR(MODE=1,MODE=2,MODE=3), Efficiency!AZ106,#REF!)","v":0.92081499923575372},"W",null,null,null,null,null,null,null,null,null,null,null,null,null,"Vout<=8V",47,2]
[null,null,null,null,null,null,null,null,null,null,{"$f":"\"SCH_\"&B34&\"_\"&B41","v":"SCH_COT3_LM5164"},null,null,null,null,null,"Vout<=12V",22,3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Vout<=20V",22,4]
["Step 2: Circuit Configuration for COT / PFM, Fixed / Adj Vout, ILIM, UVLO, SS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Vout>20V",10,5]
[null,"COT Type I",1,null,null,null,null,null,null,null,null,null,null,null,null,null,"Cout Capacitance",{"$f":"CHOOSE(S30,\"100\", \"47\",\"22\",\"22\",\"10\")","v":"22"},{"$f":"IF(Vout<5, 1, IF(Vout<=8, 2, IF(Vout<=12, 3, IF(Vout<=20, 4, 5))))","v":3}]
[null,"COT Type II",2]
["COT/PFM ","COT Type III",3]
[null,null,null,null,"VOUT Fixed/Adjustable","Fixed",1,null,"ILIM shorted",1,{"$f":"B34&\", \"&F35&\", \"&I36&\", \"&F39&\", \"&I41","v":"COT3, VOUTadj, RsetGND, UVLOadj, SSAdj"},null,null,null,null,null,"Vout<=5V","6.3V",1]
["MODE",{"$f":"CHOOSE(C34, \"COT1\", \"COT2\",\"COT3\")","v":"COT3"},3,null,null,"Adjustable",2,null,"ILIM resistor needed",2,{"$f":"C34&\", \"&G35&\", \"&J36&\", \"&G39&\", \"&J41","v":"3, 2, 1, 1, 1"},null,null,null,null,null,"Vout<=8V","10V",2]
[null,{"$f":"IF(MODE=4, \"PFM\", \"COT\")","v":"COT"},null,null,"MODE_VOUT",{"$f":"CHOOSE(G35, \"VOUTfixed\", \"VOUTadj\")","v":"VOUTadj"},{"$f":"IF(AND(OR(MODE=1,MODE=4),OR(Vout=3.3,Vout=5)),1,2)","v":2},null,null,null,{"$f":"C34&G35&J36&G39&J41","v":"32111"},null,null,null,null,null,"Vout<=12V","16V",3]
[null,null,null,null,null,null,null,"MODE_RSET",{"$f":"CHOOSE(J36, \"RsetGND\",\"Rset\")","v":"RsetGND"},1,null,null,null,null,null,null,"Vout<=20V","25V",4]
[null,null,null,null,"UVLO","Adjustable",1,null,null,null,null,null,null,null,null,null,"Vout>20V","50V",5]
[null,null,null,null,null,"Internal",2,"Soft Start","Adjustable",1,null,"Iout Linear Axis",1,null,null,null,"Cout Voltage Rating",{"$f":"CHOOSE(S38,\"6.3V\", \"10V\",\"16V\",\"25V\",\"50V\")","v":"16V"},{"$f":"IF(Vout<=5, 1, IF(Vout<=8, 2, IF(Vout<=12, 3, IF(Vout<=20, 4, 5))))","v":3}]
[null,"LM5163",1,null,"MODE_UVLO",{"$f":"CHOOSE(G39, \"UVLOadj\", \"UVLOint\")","v":"UVLOadj"},1,null,"3ms Fixed",2,null,"Iout Log Axis",2]
[null,"LM5164",2,null,null,null,null,null,null,null,null,"PLOT_TYPE",1]
["VARIANT",{"$f":"CHOOSE(VARIANT, \"LM5163\", \"LM5164\")","v":"LM5164"},2,null,"ESR","NO",1,"MODE_SS",{"$f":"CHOOSE(J41, \"SSAdj\", \"SSfix\")","v":"SSAdj"},1,null,null,null,null,null,null,null,"0402",1,"1.0 x 0.5",0.5]
[null,null,null,null,null,"YES",2,null,null,null,null,null,null,null,null,null,null,"0603",2,"1.6 x 0.8",1.3]
[null,null,null,null,"MODE_ESR",null,2,null,null,null,null,null,null,null,null,null,null,"0805",3,"2.0 x 1.25",2.5]
[null,null,null,null,null,{"$f":"CHOOSE(G44, \"\", \"_ESR\")","v":"_ESR"},{"$f":"IF(MODE=2, 1, MODE_ESR)","v":2},null,null,null,null,null,null,null,null,null,null,"1206",4,"3.2 x 1.6",5.0999999999999996]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1210",5,"3.2 x 2.5",8]
["Step 3: Buck Inductor",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Component Size",{"$f":"CHOOSE(S46,\"0402\", \"0603\",\"0805\",\"1206\",\"1210\")","v":"1210"},5,{"$f":"CHOOSE(S46,T41,T42,T43,T44,T45)","v":"3.2 x 2.5"}]
["Don1",{"$f":"Vout/VIN_nom","v":0.25},{"$f":"(Vout-VIN_nom)/Vout","v":-3},null,"Ideal Duty Cycle at VIN(nom)",null,null,null,1]
["Doff1",{"$f":"1-47:47","v":0.75},null,null,"Ideal 1- Duty Cycle at VIN(nom)",null,null,null,1]
[]
["Don_Vinmin",{"$f":"Vout/VIN_min","v":0.66666666666666663},{"$f":"IF(VIN_min>Vout, \"BUCK\", \"BOOST\")","v":"BUCK"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3mm x 3mm",1,"3.0 x 3.0",9]
["Don_Vinnom",{"$f":"Vout/VIN_nom","v":0.25},{"$f":"IF(VIN_nom>Vout, \"BUCK\", \"BOOST\")","v":"BUCK"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4mm x 4mm",2,"4.0 x 4.0",16]
["Don_Vinmax",{"$f":"Vout/VIN_max","v":0.17142857142857143},{"$f":"IF(VIN_max>Vout, \"BUCK\", \"BOOST\")","v":"BUCK"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5mm x 5mm",3,"5.0 x 5.0",25]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6mm x 6mm",4,"6.0 x 6.0",36]
["Lf_Vinmin",{"$f":"(VIN_min-Vout)*Don_Vinmin/(Fsw*Iout*0.4)","v":3.3333333333333335E-5},"H","COT",null,null,null,null,null,null,null,null,null,null,null,null,null,"7mm x 7mm",5,"7.0 x 7.0",49]
["Lf_Vinnom",{"$f":"(VIN_nom-Vout)*Don_Vinnom/(Fsw*Iout*0.4)","v":7.4999999999999993E-5},"H","COT",null,null,null,null,1,null,null,null,null,null,null,null,"Inductor Size","8mm x 8mm",6,"8.0 x 8.0",64]
["Lf_Vinmax",{"$f":"(VIN_max-Vout)*Don_Vinmax/(Fsw*Iout*0.7)","v":4.7346938775510206E-5},"H","COT",null,null,null,null,null,null,null,null,null,null,null,null,null,"10mm x 10mm",7,"10.0 x 10.0",100]
[]
["L_Vinmin_COT",{"$f":"(VIN_min-Vout)*Don_Vinmin/(Fsw*Iout*0.3)","v":4.4444444444444447E-5},"H","COT","Calculated Inductance for 30% ripple at VIN(min)"]
["L_Vinnom_COT",{"$f":"(VIN_nom-Vout)*Don_Vinnom/(Fsw*Iout*0.4)","v":7.4999999999999993E-5},"H","COT","Calculated Inductance for 40% ripple at VIN(nom)",null,null,null,null,null,"Pk-to-Pk Ripple Current at VIN(nom), DIL"]
["L_Vinmax_COT",{"$f":"(VIN_max-Vout)*Don_Vinmax/(Fsw*Iout*0.7)","v":4.7346938775510206E-5},"H","COT","Calculated Inductance for 70% ripple at VIN(max)"]
[]
[]
["Lopt",{"$f":"B59","v":7.4999999999999993E-5},"H"]
[]
["Lf",{"$f":"'Design Converter'!E17/1000000","v":6.7999999999999999E-5},"H",null,"Chosen Inductance"]
["Rdcr",{"$f":"'Design Converter'!E18/1000","v":0.12},"W",null,"Chosen Inductor DCR"]
[]
["Don2",{"$f":"(Vout+Iout*Rdcr)/Vin","v":0.2525},null,null,"**Edit to add Rdson**"]
["Doff2",{"$f":"1-_Don2","v":0.74750000000000005}]
[]
["Rdson1",0.75,"W"]
["Rdson2",0.33,"W"]
[]
["Don_Vinmin_2",{"$f":"(Vout+Iout*(Rdcr+Rdson2))/(VIN_min+Iout*Rdson2)","v":0.67921440261865795},null,null,"Duty cycles adjusted for DCR and shunt voltage drops"]
["Don_Vinnom_2",{"$f":"(Vout+Iout*(Rdcr+Rdson2))/(VIN_nom+Iout*Rdson2)","v":0.25760397268777158},null,null,"need to include RDS(on) later"]
["Don_Vinmax_2",{"$f":"(Vout+Iout*(Rdcr+Rdson2))/(VIN_max+Iout*Rdson2)","v":0.17702260770652636}]
[]
["Iripple_Vinmin",{"$f":"(VIN_min-Vout-Rdson1*Iout)*Don_Vinmin_2/(Fsw*Lf)","v":0.17479782420333112},"A","COT"]
["Iripple_Vinnom",{"$f":"(VIN_nom-Vout-Rdson1*Iout)*Don_Vinnom_2/(Fsw*Lf)","v":0.44512451162960531},"A","COT"]
["Iripple_Vinmax",{"$f":"(VIN_max-Vout)*Don_Vinmax_2/(Fsw*Lf)","v":0.50329957093032007},"A","COT"]
[]
["ILpk_Vinmin",{"$f":"Iout+Iripple_Vinmin/2","v":1.0873989121016656},"A","COT"]
["ILpk_Vinnom",{"$f":"Iout+Iripple_Vinnom/2","v":1.2225622558148026},"A","COT"]
["ILpk_Vinmax",{"$f":"Iout+Iripple_Vinmax/2","v":1.25164978546516},"A","COT"]
[]
["ILIM_Typ",{"$f":"CHOOSE(VARIANT, 0.75, 1.5)","v":1.5},"A",null,"Isat_min",{"$f":"B86*1.2","v":1.7999999999999998}]
[]
["Ripple current",{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), Iripple_Vinnom, Iripple)","v":0.44512451162960531},"A",null,null,null,null,"% Ripple Current at Nom VIN"]
[null,null,null,null,null,null,null,"Maximum Load Current"]
["Max inductor ripple current",{"$f":"MAX(B78:B80)","v":0.50329957093032007},"A"]
[null,null,null,null,null,"Ripple I","Iin"]
["% Ripple Current",{"$f":"B78/Iout","v":0.17479782420333112},null,"COT",null,{"$f":"B78","v":0.17479782420333112},{"$f":"Iin_Vinmin","v":0.7407407407407407}]
[null,{"$f":"B79/Iout","v":0.44512451162960531},null,"COT",null,{"$f":"B79","v":0.44512451162960531},{"$f":"Iin_Vinnom","v":0.27777777777777773}]
[null,{"$f":"B80/Iout","v":0.50329957093032007},null,"COT",null,{"$f":"B80","v":0.50329957093032007},{"$f":"Iin_Vinmax","v":0.19047619047619047}]
[]
[null,{"$f":"IF(OR(MODE=1, MODE=2,MODE=3), B93, Ilim/Iout)","v":0.44512451162960531}]
[]
["Iripple1",{"$f":"(Vin-Vout)*Don_Vinnom_2/(Fsw*Lf)","v":0.45459524591959694},"A","inductor ripple current with chosen inductance (pk-pk)",null,null,null,null,1]
["Temp",100]
["DCR at hot",{"$f":"Rdcr*(1+0.0039*(B99-25))","v":0.15509999999999999},"W"]
[]
[]
[]
["Step 4: Output Capacitor"]
["Icoutrms_VINmin",{"$f":"Iripple_Vinmin/SQRT(12)","v":5.0459785428777056E-2},"A","Output Cap RMS current"]
["Icoutrms_VINnom",{"$f":"Iripple_Vinnom/SQRT(12)","v":0.12849637830612667},"A"]
["Icoutrms_VINmax",{"$f":"Iripple_Vinmax/SQRT(12)","v":0.14529007137982172},"A",null,null,null,{"$f":"Vripple1","v":0.06}]
[]
["Output Ripple Spec (pk-pk)",{"$f":"Vout*0.005","v":0.06},"V","Vout capacitive ripple spec at Vin(nom) = Vripple1"]
[]
["Coutmin"]
["COT",{"$f":"Iripple_Vinnom/(Fsw*8*Vripple1)","v":3.0911424418722593E-6},"F","COT","Min recommended Cout based on ripple spec above",null,null,null,1]
[null,{"$f":"Lf*B83^2/((1.05*Vout)^2-Vout^2)","v":6.8859604278673595E-6},"F","COT","Min recommended Cout based on 5% load-off transient spec"]
["CoutMinCOT",{"$f":"MAX(B112:B113, 0.0000022)","v":6.8859604278673595E-6},"F","COT","max of 2 results and 2.2uF"]
[]
["Reported Countmin",{"$f":"CoutMinCOT*1000000","v":6.8859604278673592},"µF"]
[]
["Cout",{"$f":"'Design Converter'!E24/1000000","v":3.3000000000000003E-5},"F","Chosen Output Capacitance",null,null,null,null,1]
["Resrmax",{"$f":"SQRT((Vripple1/Iripple_Vinnom)^2-(1/(Fsw*Cout*8))^2)","v":0.13420108507532141},"W","Max ESR before ripple exceeds Vripple1",null,null,null,null,1]
["Type1 ESR for sufficient (20mV) COT ripple at FB pin",{"$f":"0.02*Vout/Vref/Iripple_Vinnom","v":0.44931248397846707},"W","(a)"]
["Type2 ESR for sufficient (20mV) COT ripple at FB pin",{"$f":"0.02/Iripple_Vinnom","v":4.4931248397846707E-2},"W","(b)"]
[]
["Type 1 Output Cap RC Time Constant",{"$f":"Cout*B130*1000000","v":0},"µs"]
["Type 2 Output Cap RC Time Constant",{"$f":"Cout*B131*1000000","v":0},"µs"]
["Ton @ Vin(min)",{"$f":"Vout/VIN_min/(Fsw)","v":2.2222222222222221E-6},"s"]
["Ton @ Vin(nom)",{"$f":"Vout/VIN_nom/(Fsw)","v":8.3333333333333333E-7},"s"]
["ESR so that RC > Ton/2",{"$f":"B125/2/Cout","v":3.3670033670033662E-2},"W","(c)"]
[]
[]
["Type1: Need ESR of…",{"$f":"IF(MODE=1, MAX(B120,B127), 0)","v":0},"W","Max of (a) and (c)"]
["Type2: Need ESR of…",{"$f":"IF(MODE=2, MAX(B121,B127), 0)","v":0},"W","Max of (b) and (c)"]
[]
["Reported Cout ESR max",{"$f":"IF(OR(CoutEsrMax>0.5, CoutEsrMax<0, (ISERROR(CoutEsrMax))), \"N/A\", CoutEsrMax*1000)","v":134.2010850753214},"mW"]
[]
["CoutEsr",{"$f":" 'Design Converter'!E26","v":5.0000000000000001E-3},"W","Chosen ESR",null,null,null,null,1]
[]
["Actual Output Ripple",{"$f":"Iripple_Vinnom*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2)","v":6.0448909694310647E-3},"Vp-p","Vripple2"]
[]
["Minimum Feedforward / Coupling Capacitance",{"$f":"MAX(1000000000000*0.00005/(3*Rfb1_),47)","v":47},"pF",null,null,null,null,{"$f":"0.00005/3/Rfb1_","v":3.6791758646063281E-11}]
["Recommended Cff / Cb",{"$f":"IF(OR(MODE=2,MODE=3), \">\"&ROUND(B139,0),\"\")","v":">47"},"pF"]
["Selected Cff / Cb",{"$f":"'Design Converter'!$E$29","v":56},"pF"]
[]
["Minimum Ripple Generation Capacitance",{"$f":"10/(Fsw*Rfb)","v":7.4158618930281455E-10},"F",{"$f":"1000000000000*B143","v":741.58618930281455},"pF",{"$f":"Rfb","v":44948.697554185725}]
["Recommended Ca",{"$f":"IF(MODE=3, \">\"&ROUND(D143,0),\"\")","v":">742"},"pF"]
["Selected Ca",{"$f":"'Design Converter'!E31","v":2200},"pF",{"$f":"B145/1000000000000","v":2.1999999999999998E-9},"F"]
[]
["Maximum Ripple Generation Resistance",{"$f":"(VIN_nom-Vout)*B126/((B149/1000)*Ca)","v":681818.18181818188},"W",{"$f":"B147/1000","v":681.81818181818187},"kW"]
["Recommended Ra",{"$f":"IF(MODE=3, \"<\"&ROUND(D147,0),\"\")","v":"<682"},"kW",null,null,null,null,null,null,null,null,"Lf_emi",{"$f":"'Design EMI Filter'!$E$9","v":22},"uH",{"$f":"M148/1000000","v":2.1999999999999999E-5},"H"]
["Ripple amplitude",{"$f":"'Design Converter'!E33","v":20},"mVp-p",null,null,null,null,null,null,null,null,"Cf_emi",{"$f":"'Design EMI Filter'!$E$11","v":4.7},"uF",{"$f":"M149/1000000","v":4.6999999999999999E-6},"F"]
[null,null,null,null,null,null,null,null,null,null,null,"Cd_emi",{"$f":"'Design EMI Filter'!$E$13","v":10},"uF",{"$f":"M150/1000000","v":1.0000000000000001E-5},"F"]
[null,null,null,null,null,null,null,null,null,null,null,"ESR_Cd",{"$f":"'Design EMI Filter'!$E$15","v":3.3},"Ω",{"$f":"M151","v":3.3},"Ω",{"$f":"ESR_Cd&ohm","v":"3.3Ω"}]
["Step 5: Input Capacitor",null,null,null,null,null,null,null,null,null,null,"Min Noise",{"$f":"'Design EMI Filter'!$E$8","v":50},"dB","noise limit"]
["Vinripple1",{"$f":"0.05*VIN_nom","v":2.4000000000000004},"Vp-p","Input voltage ripple spec (pk-pk) at Vin(nom)",null,null,null,null,null,null,null,"Duty Cycle",{"$f":"Vout/VIN_nom/Efficiency_COT_Full_Load","v":0.2738225629791895},null,"calculated duty cycle"]
[null,null,null,null,null,null,null,null,null,null,null,"Target Atten.",{"$f":"20*LOG(Iout/(PI()^2*Fsw*Cin)*SIN(PI()*Duty_Cycle)/0.000001) - Min_Noise","v":51.316492648461235},"dB","calculated attenuation"]
["Icinrms",{"$f":"Iout*SQRT(Don_Vinnom_2*(1-Don_Vinnom_2))","v":0.43731472184600578},"A"]
["Cinmin",{"$f":"Iout*Don_Vinnom_2*(1-Don_Vinnom_2)/(Vinripple1*Fsw-Iout*RCinEsr)*1000000","v":0.26561689825013901},"µF"]
["Reported Cinmin",{"$f":"IF(Cinmin<2.2, 2.2,Cinmin)","v":2.2000000000000002},"µF",null,null,null,null,null,null,null,null,"Filter Inductor"]
["Cin",{"$f":"'Design Converter'!E37/1000000","v":2.2000000000000001E-6},"F","Input capacitance",null,null,null,null,null,null,null,"Irms rating",{"$f":"Iout*1.5","v":1.5},"A","calculated suggested IRMS rating"]
["CinEsrMax",{"$f":"-(Iout*Don_Vinnom_2*(1-Don_Vinnom_2)/(Cin*Fsw)-Vinripple1)/(Iout+Iripple_Vinnom/2)","v":1.7260766085084038},"W"]
["RCinEsr",{"$f":"'Design Converter'!E39/1000","v":3.0000000000000001E-3},"W","Input capacitance series resistance (ESR)"]
["Reported Cin ESR max",{"$f":"IF(OR(CinEsrMax>12, CinEsrMax<0), \"N/A\",CinEsrMax*1000)","v":1726.0766085084038},"mΩ",null,null,null,null,null,null,null,null,"Filter Capacitor"]
[null,null,null,null,null,null,null,null,null,null,null,"Cfa calculation",{"$f":"Cin/(Cin*Lf_emi*0.000001*(2*PI()*Fsw/10)^2 - 1) / 0.000001","v":-2.2000037833022223},"uF","calculated value"]
["COT input voltage ripple - Vinripple2",{"$f":"Iout*Don_Vinnom_2*(1-Don_Vinnom_2)/(Cin*Fsw)+(Iout +Iripple_Vinnom/2)*RCinEsr","v":0.29343157456024654},"Vp-p",null,{"$f":"Iout*Don_Vinmax_2*(1-Don_Vinmax_2)/(Cin*Fsw)","v":0.22073576373834489},"Vp-p",null,null,null,null,null,"Cfb calculation",{"$f":"1/(Lf_emi)*(10^(Target_Att/40)/(2*PI()*Fsw))^2/0.000001","v":4.7076016396939151},"uF","calculated value"]
[null,null,null,null,null,null,null,null,null,null,null,"Cf",{"$f":"MAX(M162,M163)","v":4.7076016396939151},"uF","calculated value"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,"Damping Capacitor"]
["Step 6: Soft Start",null,null,null,null,null,null,null,null,null,null,"Cd ≥",{"$f":"4*Cin*1000000","v":8.8000000000000007},"uF","calculated value"]
["Tss",{"$f":"'Design Converter'!#REF!/1000","v":{"$error":"#REF!"}},"s","Soft-start time",null,null,null,null,null,null,null,"Cd ESR ≥",{"$f":"SQRT(Lf_emi/Cin)","v":3.1622776601683795},"Ω","calculated value"]
["Iss",1.0000000000000001E-5,"A","Soft-start current"]
["Css",{"$f":"8.16*Tss/1000000","v":{"$error":"#NAME?"}},"F","Required soft-start cap"]
["Css_u",{"$f":"'Standard Value Calculator'!B4","v":{"$error":"#NAME?"}},"F","User selected SS cap",null,null,null,null,null,null,null,"CIN and Cd Capacitors Current Sharing and Rating"]
[null,null,null,null,null,null,null,null,null,null,null,"Cd impedance",{"$f":" 1/(2*PI()*Fsw*Cd_emi) + ESR_Cd","v":3.3530516476972982},"Ω","calculated Cd impedance at the sw. frequency"]
["Step 7: Other Components - UVLO, PGOOD",null,null,null,null,null,null,null,null,null,null,"Cin impedance",{"$f":" 1/(2*PI()*Fsw*Cin) + RCinEsr","v":0.24414385316953838},"Ω","calculated CIN impedance at the sw. frequency"]
[]
["Rising UVLO/EN Threshold",1.5,"V",null,null,null,null,null,null,null,null,"IRMS Total Input Cap",{"$f":"Iout*SQRT(Duty_Cycle*(1-Duty_Cycle))","v":0.44591901392819894},"A","calculated total IRMS current for CIN and Cd combined"]
["Falling UVLO/EN Threshold",1.4,"V",null,null,null,null,null,null,null,null,"IRMS Cd Act",{"$f":"IRMSTOT*(ZCIN/(ZCIN+ZCd))","v":3.0264795515216481E-2},"A","Calculated min IRMS current rating for Cd"]
["Voltage Hysteresis",{"$f":"B176-B177","v":0.10000000000000009},"V",null,null,null,null,null,null,null,null,"IRMS CIN",{"$f":"IRMSTOT*(ZCd/(ZCIN+ZCd))","v":0.41565421841298245},"A","Calculated min IRMS current rating for CIN"]
[]
["VINUVLO_ON",{"$f":"'Design Converter'!E48","v":6},"V"]
["VINUVLO_OFF",null,"V"]
[]
["RUV1",{"$f":"'Design Converter'!E49*1000","v":1000},"kΩ",{"$f":"'Standard Value Calculator'!J16","v":1000},"kΩ",{"$f":"IF(Ruvlo1<0,\"N/A\",D183)","v":1000},{"$f":"IF(Ruvlo1<0,\"N/A\",D183&\"kΩ\")","v":"1000kΩ"}]
["RUV2",{"$f":"Vuvlo_on*Ruvlo1/(VINuvlo_on-Vuvlo_on)","v":333.33333333333331},"kΩ",{"$f":"'Standard Value Calculator'!J17","v":332},"kΩ",{"$f":"IF(F183=\"N/A\",\"N/A\",D184)","v":332},{"$f":"IF(G183=\"N/A\",\"N/A\",D184&\"kΩ\")","v":"332kΩ"}]
[]
["VINUVLO_ON_ACTUAL",{"$f":"(D183+D184)/D184*Vuvlo_on","v":6.0180722891566267},"V"]
["VINUVLO_OFF_ACTUAL",{"$f":"(D183+D184)/D184*Vuvlo_off","v":5.6168674698795176},"V"]
[]
["RPG",20,"kΩ"]
[]
[]
["Step 8: FB Divider"]
["Pi",3.1415926500000002,null,"p"]
["Toff_Vinmax",{"$f":"(1-Don_Vinmax_2)/Fsw","v":2.7432579743115788E-6},"sec"]
["Ton_Vinmin",{"$f":"IF(VIN_min>Vout, (1-Don_Vinmin_2)/Fsw, Don_Vinmin_2/Fsw)","v":1.0692853246044734E-6},"sec"]
[]
["Rfb1",{"$f":"'Design Converter'!E43*1000","v":453000},"W","Lower Feedback Resistance - chosen by user",null,null,null,null,1]
["Rfb2",{"$f":"IF(Vout=Vref,100000000,Vref*B197/((Vout-Vref)))","v":50333.333333333328},"W","Upper Feedback Resistance"]
["Rfb2_u",{"$f":"IF(Vout=Vref,\"N/A\",'Standard Value Calculator'!J10)","v":49900},"W","Std Value Upper Feedback Resistance"]
["Rfb",{"$f":"Rfb1_*Rfb2_u/(Rfb1_+Rfb2_u)","v":44948.697554185725},"W","Rfb1 || Rfb2_u"]
[null,{"$f":"1.2/Rfb2_u*(Rfb2_u+Rfb1_)","v":12.0937875751503},"V"]
["Ifb",{"$f":"CHOOSE(MODE_VOUT, IF(Vout=5, 0.000007, 0.0000038), Vout/(Rfb1_+Rfb2_u))","v":2.3861602704314974E-5}]
[]
["Other Input Variables"]
["Rfets",0,"W","Series resistance due to FETs",null,null,null,{"$f":"_Don2*RdsonTop+Doff2*RdsonBot+B209*Vin^2*Fsw/2/(((Iripple1/SQRT(3))^2))","v":25.485771511844959}]
["Diode loss eq res",{"$f":"0.00000002*Fsw*0.6*4/Iripple1","v":3.1676530120481924E-2}]
["Fet loss eq res",{"$f":"_Don2*RdsonTop+Doff2*RdsonBot","v":0.40070749999999999}]
["cap loss eq res",{"$f":"B209*Vin^2*Fsw/2/(((Iripple1/SQRT(3))^2))","v":25.08506401184496}]
["Sw cap",5.0000000000000001E-9]
[]
["Step 8: Efficiency"]
[]
["Design"]
["Ta",25,"°C","Ambient Temperature"]
["Components"]
["LTc",{"$f":"4000/1000000","v":4.0000000000000001E-3},"%/°C","Inductor DCR Temp Co"]
["θCA",40,"°C/W","Inductor Core to Ambient Thermal Resistance"]
["RCinEsr",{"$f":"RCinEsr","v":3.0000000000000001E-3},"W","Input Capacitor ESR"]
["Part Characteristics"]
["Vcc",{"$f":"IF(Vin>7.7,7.5,Vin-0.2)","v":7.5},"V"]
["Deadtime"]
["Deadtime",2E-8,"s","Total Deadtime",null,null,"20ns for LM5166"]
["IQ"]
["IQ ",1.0000000000000001E-5,"A","Quiescent Current Of Controller (Not Switching!)"]
[]
[]
["IC Power Disipation","Value","Units"]
["Power Dis",{"$f":"Efficiency!AZ106","v":0.92081499923575372},"W"]
["Temp rise",{"$f":"B228*ThetaJA","v":37.845496468589481},"°C"]
["Current (switching)",{"$f":"(Qg_Q1+Qg_Q2)*Fsw+Iq","v":{"$error":"#NAME?"}},"A"]
["Qrr Current",{"$f":"Qrr_Q2*Fsw","v":{"$error":"#NAME?"}},"A"]
["Diode Current",{"$f":"C232/Vin","v":{"$error":"#NAME?"}},{"$f":"Deadtime*Fsw*(Ipp/2)*(Vsd_Q1+Vsd_Q2)","v":{"$error":"#NAME?"}}]
["Total Application Switching IQ",{"$f":"SUM(B230:B232)","v":{"$error":"#NAME?"}},"A"]
[]
[]
["SCHEMATIC LABELS"]
[]
[]
[{"$f":"\"RUV1 = \"&'Design Converter'!E49&\"MΩ\"","v":"RUV1 = 1MΩ"},{"$f":"C275","v":"1MΩ"}]
[{"$f":"\"RUV2 = \"&'Design Converter'!E50&\"kΩ\"","v":"RUV2 = 332kΩ"},{"$f":"C276","v":"332kΩ"}]
[{"$f":"\"Rhys = \"&'Design Converter'!E52&\"kΩ\"","v":"Rhys = 5.61686746987952kΩ"},{"$f":"C277","v":{"$error":"#REF!"}}]
[]
[{"$f":"\"LF = \"&'Design Converter'!E17&\"µH\"","v":"LF = 68µH"},{"$f":"'Design Converter'!E17&\"µH\"","v":"68µH"}]
[{"$f":"\"Rdcr = \"&Rdcr*1000&\"mΩ\"","v":"Rdcr = 120mΩ"},{"$f":"Rdcr*1000&\"mΩ\"","v":"120mΩ"}]
[{"$f":"\"Rt = \"&'Design Converter'!I43&\"kΩ\"","v":"Rt = kΩ"},{"$f":"'Design Converter'!I43&\"kΩ\"","v":"kΩ"}]
[{"$f":"\"Css = \"&ROUND(Css_u*1000000000,1)&\"nF\"","v":{"$error":"#NAME?"}},{"$f":"ROUND(Css_u*1000000000,1)&\"nF\"","v":{"$error":"#NAME?"}}]
[]
["VIN",{"$f":"VIN_nom&\"V\"","v":"48V"}]
["VIN range",{"$f":"VIN_min&\"V...\"&VIN_max&\"V\"","v":"18V...70V"}]
[]
[{"$f":"\"VOUT = \"&'Design Converter'!E9&\"V\"","v":"VOUT = 12V"},{"$f":"'Design Converter'!E9&\"V\"","v":"12V"}]
[null,null,{"$f":"R30","v":"22"},{"$f":"ROUNDUP('Design Converter'!$E$24/C252,0)","v":2}]
[{"$f":"\"COUT = \"&'Design Converter'!$E$24&\"µF\"","v":"COUT = 33µF"},{"$f":"'Design Converter'!$E$24&\"µF\"","v":"33µF"},{"$f":"IF('Design Converter'!$E$24=OR(10, 22, 47, 100), 'Design Converter'!$E$24,C252)","v":"22"},{"$f":"IF(D252=1, \"\",B255)","v":"2 x "},{"$f":"D253&C253&\"µF\"","v":"2 x 22µF"},{"$f":"C253&\"µF\"","v":"22µF"}]
["Capacitance per component (Cout)",{"$f":"C252&\"µF\"","v":"22µF"}]
["# of output caps",{"$f":"D252&\" x \"","v":"2 x "}]
[]
["CIN",{"$f":"Cin*1000000&\"µF\"","v":"2.2µF"}]
["Capacitance per component (Cin)",{"$f":"\"2.2µF\"","v":"2.2µF"}]
["# of input caps",{"$f":"ROUNDUP(Cin*1000000/2.2,0)&\" x \"","v":"1 x "}]
[]
["Fixed VOUT?",{"$f":"IF(MODE_VOUT=1, \"YES\", \"NO\")","v":"NO"}]
["FB resistor ref des shown or not?",{"$f":"IF(MODE_VOUT=2, \"YES\", \"NO\")","v":"YES"},{"$f":"IF(MODE_VOUT=2, \"R1\", \"\")","v":"R1"},{"$f":"IF(MODE_VOUT=2, \"R2\", \"\")","v":"R2"}]
[{"$f":"\"RFB1 = \"&'Design Converter'!E43&\"kΩ\"","v":"RFB1 = 453kΩ"},{"$f":"'Design Converter'!E43&\"kΩ\"","v":"453kΩ"},{"$f":"IF(MODE=1,'Design Converter'!E43&\"kΩ\", \"\")","v":""}]
[{"$f":"\"RFB2 = \"&IF(Vout=Vref,\"OPEN\",'Design Converter'!E44&\"kΩ\")","v":"RFB2 = 49.9kΩ"},{"$f":"IF(Vout=Vref,\"OPEN\",Rfb2_u/1000&\"kΩ\")","v":"49.9kΩ"},{"$f":"IF(MODE=1, IF(Vout=Vref, \"OPEN\",Rfb2_u/1000&\"kΩ\" ), \"\")","v":""}]
[]
[]
["Show Rt resistor ref des?",{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), \"YES\", \"NO\")","v":"YES"},{"$f":"IF(MODE=4,\"\", \"Rt\")","v":"Rt"}]
["Rt",{"$f":"IF(MODE=4, \"\", 'Standard Value Calculator'!J4/1000&\"kΩ\")","v":"100kΩ"}]
[]
["Show ESR resistor ref des?",{"$f":"IF(OR(MODE=3, MODE=4), \"NO\", \"YES\")","v":"NO"},{"$f":"IF(OR(MODE=3, MODE=4),\"\",\"Resr\")","v":""}]
[{"$f":"\"RESR = \"&'Design Converter'!E26&\"mΩ\"","v":"RESR = 0.005mΩ"},{"$f":"IF(OR(MODE=3,MODE=4), \"\", 'Design Converter'!E26&\"Ω\")","v":""},null,null,null,{"$f":"B120","v":0.44931248397846707}]
["Resr",{"$f":"IF(MODE=1, \">\"&ROUND(B130,3), IF(MODE=2,  \">\"&ROUND(B131,3),IF(MODE=3,ROUND(B119,3),\"\")))","v":0.13400000000000001}]
[]
["Adjustable UVLO?",{"$f":"IF(MODE_UVLO=1, \"YES\", \"NO\")","v":"YES"},{"$f":"IF(MODE_UVLO=1,\"Ren1\", \"\")","v":"Ren1"},{"$f":"IF(MODE_UVLO=1, \"Ren2\", \"\")","v":"Ren2"},{"$f":"IF(MODE_UVLO=1, \"Rhys\", \"\")","v":"Rhys"},"Value","Units","BOM display"]
[{"$f":"\"RUV1 = \"&C275","v":"RUV1 = 1MΩ"},{"$f":"'Design Converter'!E49&\" MΩ\"","v":"1 MΩ"},{"$f":"IF(MODE_UVLO=1,'Design Converter'!E49&\"MΩ\", \"\")","v":"1MΩ"},null,null,{"$f":"IF(MODE_UVLO=1,'Design Converter'!E49, \"\")","v":1},{"$f":"IF(MODE_UVLO=1,\"MΩ\", \"\")","v":"MΩ"},{"$f":"IF(MODE_UVLO=1,'Design Converter'!E49&\"M\", \"\")","v":"1M"}]
[{"$f":"\"RUV2 = \"&C276","v":"RUV2 = 332kΩ"},{"$f":"IF(D184>=1000, D184/1000&\" MΩ\", D184&\" kΩ\")","v":"332 kΩ"},{"$f":"IF(MODE_UVLO=1, IF(D184<1, D184*1000&\"Ω\", IF(D184<1000, D184&\"kΩ\", D184/1000&\"MΩ\")), \"\")","v":"332kΩ"},null,null,{"$f":"IF(MODE_UVLO=1, IF(D184<1, D184*1000, IF(D184<1000, D184, D184/1000)), \"\")","v":332},{"$f":"IF(MODE_UVLO=1, IF(D184<1, \"Ω\", IF(D184<1000,\"kΩ\", \"MΩ\")), \"\")","v":"kΩ"},{"$f":"IF(MODE_UVLO=1, IF(D184<1, D184*1000, IF(D184<1000, D184&\"k\", D184/1000&\"M\")), \"\")","v":"332k"}]
[{"$f":"\"RHYS = \"&C277","v":{"$error":"#REF!"}},{"$f":"IF(#REF!<1000,#REF!& \" kΩ\",#REF!& \" MΩ\")","v":{"$error":"#REF!"}},{"$f":"IF(MODE_UVLO=1, IF(#REF!<1,#REF!* 1000&\"Ω\", IF(#REF!<1000,#REF!& \"kΩ\",#REF!/ 1000&\"MΩ\")), \"\")","v":{"$error":"#REF!"}},null,null,{"$f":"IF(MODE_UVLO=1, IF(#REF!<1,#REF!* 1000, IF(#REF!<1000,#REF!,#REF!/ 1000)), \"\")","v":{"$error":"#REF!"}},{"$f":"IF(MODE_UVLO=1, IF(#REF!<1, \"Ω\", IF(#REF!<1000,\"kΩ\", \"MΩ\")), \"\")","v":{"$error":"#REF!"}},{"$f":"IF(MODE_UVLO=1, IF(#REF!<1,#REF!* 1000, IF(#REF!<1000,#REF!& \"k\",#REF!& \"M\")), \"\")","v":{"$error":"#REF!"}}]
[]
[{"$f":"\"Css = \"&Css*1000000000&\"nF\"","v":{"$error":"#NAME?"}},{"$f":"Css*1000000000&\"nF\"","v":{"$error":"#NAME?"}}]
["Cbst",{"$f":"\"2.2nF\"","v":"2.2nF"},null,{"$f":"B280","v":"2.2nF"}]
[]
[]
["Rset resistor ref des?",{"$f":"IF(MODE_RSET=2, \"YES\", \"NO\")","v":"NO"},{"$f":"IF(MODE_RSET=2, \"R3\", \"\")","v":""},null,null,{"$f":"MODE_RSET","v":1}]
["Rset",{"$f":"IF(MODE_RSET=2, C284&\"kΩ\", \"\")","v":""},{"$f":"IF(MODE_ILIM=3,100,IF(MODE_ILIM=2,56.2,IF(MODE_ILIM=4,24.9,0)))","v":{"$error":"#REF!"}}]
[]
[]
["Rpgood","100kΩ"]
[]
["Cff / Cb?",{"$f":"IF(MODE=2, \"Cff\", IF(MODE=3,\"Cb\",\"\"))","v":"Cb"}]
[{"$f":"\"Cff / Cb=\"&B290","v":"Cff / Cb=56pF"},{"$f":"IF(OR(MODE=2,MODE=3),B141&\"pF\",\"\")","v":"56pF"}]
[]
["Ca?",{"$f":"IF(MODE=3, \"Ca\",\"\")","v":"Ca"},null,{"$f":"Ca","v":2.1999999999999998E-9},{"$f":"Ton_Vinmin","v":1.0692853246044734E-6}]
["Ca=",{"$f":"IF(MODE=3,B145&\"pF\",\"\")","v":"2200pF"}]
[]
["Ra?",{"$f":"IF(MODE=3, \"Ra\",\"\")","v":"Ra"},"Injected Ripple"]
["Ra=",{"$f":"IF(MODE=3,Ra&\"kΩ\",\"\")","v":"681kΩ"},{"$f":"(VIN_nom-Vout)*Ton_Vin_nom/(Ra*Ca)/1000","v":2.0024028834601523E-2},{"$f":"ROUNDUP(1000*C296,0)","v":21},null,{"$f":"IF(MODE=3,Ra&\"k\",\"\")","v":"681k"}]
[]
["Lf(emi)",{"$f":"M148&\"µH\"","v":"22µH"}]
["Cf(emi)",{"$f":"M149&\"µF\"","v":"4.7µF"}]
["Df(emi)",{"$f":"M150&\"µF\"","v":"10µF"}]
[]
["Full-load efficiency",{"$f":"ROUND(Efficiency!CE106,1)&\"%\"","v":"91.3%"}]
["Full-load efficiency",{"$f":"ROUND(Efficiency!CE107,1)&\"%\"","v":"91.8%"}]
["10% load efficiency",{"$f":"ROUND(Efficiency!CE16,1)&\"%\"","v":"88.4%"},"linear scale only"]
["1% load efficiency",{"$f":"ROUND(Efficiency!CE56,1)&\"%\"","v":"91.8%"},"log scale only"]
[]
["Blank out",{"$f":"IF(C307=\"y\",\"\",\"|\")","v":"|"},"n"]
[]
["OUTPUT CURRENT",{"$f":"'Design Converter'!$E$10&\"A\"","v":"1A"}]
[]
["VIN ",2]
["RT",5]
["EN",7]
["PGOOD",6]
["SS",4]
["ILIM",3]
["GND",10]
["FB",8]
["SW",1]
["HYS",9]

{"sheet":"Standard Value Calculator","index":8,"n_rows":159,"n_cols":11,"rows_kept":159,"cut":false,"hidden":true,"merged":[]}
[]
["Capacitors","Css","Cout","Cin","Cb"]
["Inputs",{"$f":"Css","v":{"$error":"#NAME?"}},{"$f":"Cout","v":3.3000000000000003E-5},{"$f":"Cin","v":2.2000000000000001E-6},{"$f":"Cb","v":0},null,null,"Resistors","inputs","Standard Result"]
["Standard Result",{"$f":"SUM(B6:B158)/1000000000000","v":{"$error":"#NAME?"}},{"$f":"SUM(C6:C158)/1000000000000","v":3.3000000000000003E-5},{"$f":"SUM(D6:D158)/1000000000000","v":2.2000000000000001E-6},{"$f":"IF(E3=\"OPEN\",\"OPEN\",SUM(E6:E158)/1000000000000)","v":0},null,null,"Rt",{"$f":"Rt","v":100000},{"$f":"IF(I4>(INT(0.5+100*POWER(10,IF(96*(LOG(I4)-INT(LOG(I4)))-ROUND(96*(LOG(I4)-INT(LOG(I4))),0)<0,ROUND(96*(LOG(I4)-INT(LOG(I4))),0)-1,ROUND(96*(LOG(I4)-INT(LOG(I4))),0))/96))*POWER(10,INT(LOG(I4))-2)+INT(0.5+100*POWER(10,(IF(96*(LOG(I4)-INT(LOG(I4)))-ROUND(96*(LOG(I4)-INT(LOG(I4))),0)<0,ROUND(96*(LOG(I4)-INT(LOG(I4))),0)-1,ROUND(96*(LOG(I4)-INT(LOG(I4))),0))+1)/96))*POWER(10,INT(LOG(I4))-2))/2,INT(0.5+100*POWER(10,(IF(96*(LOG(I4)-INT(LOG(I4)))-ROUND(96*(LOG(I4)-INT(LOG(I4))),0)<0,ROUND(96*(LOG(I4)-INT(LOG(I4))),0)-1,ROUND(96*(LOG(I4)-INT(LOG(I4))),0))+1)/96))*POWER(10,INT(LOG(I4))-2),INT(0.5+100*POWER(10,IF(96*(LOG(I4)-INT(LOG(I4)))-ROUND(96*(LOG(I4)-INT(LOG(I4))),0)<0,ROUND(96*(LOG(I4)-INT(LOG(I4))),0)-1,ROUND(96*(LOG(I4)-INT(LOG(I4))),0))/96))*POWER(10,INT(LOG(I4))-2))","v":100000},"Ω"]
["(pF)"]
[0.47,{"$f":"IF(IF((B$3*10^12-$A7)*(B$3*10^12-$A6)*-1<0,0,1)*IF(ABS(B$3*10^12-$A7)>(B$3*10^12-$A6),$A6,$A7)=B7,0,IF((B$3*10^12-$A7)*(B$3*10^12-$A6)*-1<0,0,1)*IF(ABS(B$3*10^12-$A7)>(B$3*10^12-$A6),$A6,$A7))","v":{"$error":"#NAME?"}},{"$f":"IF(IF((C$3*10^12-$A7)*(C$3*10^12-$A6)*-1<0,0,1)*IF(ABS(C$3*10^12-$A7)>(C$3*10^12-$A6),$A6,$A7)=C7,0,IF((C$3*10^12-$A7)*(C$3*10^12-$A6)*-1<0,0,1)*IF(ABS(C$3*10^12-$A7)>(C$3*10^12-$A6),$A6,$A7))","v":0},{"$f":"IF(IF((D$3*10^12-$A7)*(D$3*10^12-$A6)*-1<0,0,1)*IF(ABS(D$3*10^12-$A7)>(D$3*10^12-$A6),$A6,$A7)=D7,0,IF((D$3*10^12-$A7)*(D$3*10^12-$A6)*-1<0,0,1)*IF(ABS(D$3*10^12-$A7)>(D$3*10^12-$A6),$A6,$A7))","v":0},{"$f":"IF(IF((E$3*10^12-$A7)*(E$3*10^12-$A6)*-1<0,0,1)*IF(ABS(E$3*10^12-$A7)>(E$3*10^12-$A6),$A6,$A7)=E7,0,IF((E$3*10^12-$A7)*(E$3*10^12-$A6)*-1<0,0,1)*IF(ABS(E$3*10^12-$A7)>(E$3*10^12-$A6),$A6,$A7))","v":0},null,null,"Rshunt",{"$f":"Rshunt","v":{"$error":"#NAME?"}},{"$error":"#NAME?"},"Ω"]
[0.56000000000000005,{"$f":"IF(IF((B$3*10^12-$A8)*(B$3*10^12-$A7)*-1<0,0,1)*IF(ABS(B$3*10^12-$A8)>(B$3*10^12-$A7),$A7,$A8)=B8,0,IF((B$3*10^12-$A8)*(B$3*10^12-$A7)*-1<0,0,1)*IF(ABS(B$3*10^12-$A8)>(B$3*10^12-$A7),$A7,$A8))","v":{"$error":"#NAME?"}},{"$f":"IF(IF((C$3*10^12-$A8)*(C$3*10^12-$A7)*-1<0,0,1)*IF(ABS(C$3*10^12-$A8)>(C$3*10^12-$A7),$A7,$A8)=C8,0,IF((C$3*10^12-$A8)*(C$3*10^12-$A7)*-1<0,0,1)*IF(ABS(C$3*10^12-$A8)>(C$3*10^12-$A7),$A7,$A8))","v":0},{"$f":"IF(IF((D$3*10^12-$A8)*(D$3*10^12-$A7)*-1<0,0,1)*IF(ABS(D$3*10^12-$A8)>(D$3*10^12-$A7),$A7,$A8)=D8,0,IF((D$3*10^12-$A8)*(D$3*10^12-$A7)*-1<0,0,1)*IF(ABS(D$3*10^12-$A8)>(D$3*10^12-$A7),$A7,$A8))","v":0},{"$f":"IF(IF((E$3*10^12-$A8)*(E$3*10^12-$A7)*-1<0,0,1)*IF(ABS(E$3*10^12-$A8)>(E$3*10^12-$A7),$A7,$A8)=E8,0,IF((E$3*10^12-$A8)*(E$3*10^12-$A7)*-1<0,0,1)*IF(ABS(E$3*10^12-$A8)>(E$3*10^12-$A7),$A7,$A8))","v":0},null,null,"Rc1ea",{"$f":"Rcea1","v":{"$error":"#NAME?"}},{"$error":"#NAME?"},"Ω"]
[0.68,{"$error":"#NAME?"},0,0,0]
[0.82,{"$error":"#NAME?"},0,0,0,null,null,"Rfb1",{"$f":"Rfb1_","v":453000},453000,"Ω"]
[1,{"$error":"#NAME?"},0,0,0,null,null,"Rfb2",{"$f":"Rfb2_","v":50333.333333333328},{"$f":"IF(I10=\"OPEN\",\"OPEN\",IF(I10>(INT(0.5+100*POWER(10,IF(96*(LOG(I10)-INT(LOG(I10)))-ROUND(96*(LOG(I10)-INT(LOG(I10))),0)<0,ROUND(96*(LOG(I10)-INT(LOG(I10))),0)-1,ROUND(96*(LOG(I10)-INT(LOG(I10))),0))/96))*POWER(10,INT(LOG(I10))-2)+INT(0.5+100*POWER(10,(IF(96*(LOG(I10)-INT(LOG(I10)))-ROUND(96*(LOG(I10)-INT(LOG(I10))),0)<0,ROUND(96*(LOG(I10)-INT(LOG(I10))),0)-1,ROUND(96*(LOG(I10)-INT(LOG(I10))),0))+1)/96))*POWER(10,INT(LOG(I10))-2))/2,INT(0.5+100*POWER(10,(IF(96*(LOG(I10)-INT(LOG(I10)))-ROUND(96*(LOG(I10)-INT(LOG(I10))),0)<0,ROUND(96*(LOG(I10)-INT(LOG(I10))),0)-1,ROUND(96*(LOG(I10)-INT(LOG(I10))),0))+1)/96))*POWER(10,INT(LOG(I10))-2),INT(0.5+100*POWER(10,IF(96*(LOG(I10)-INT(LOG(I10)))-ROUND(96*(LOG(I10)-INT(LOG(I10))),0)<0,ROUND(96*(LOG(I10)-INT(LOG(I10))),0)-1,ROUND(96*(LOG(I10)-INT(LOG(I10))),0))/96))*POWER(10,INT(LOG(I10))-2)))","v":49900},"Ω"]
[1.2,{"$error":"#NAME?"},0,0,0]
[1.5,{"$error":"#NAME?"},0,0,0]
[1.8,{"$error":"#NAME?"},0,0,0,null,null,"Rs",{"$f":"Rs_ideal*1000","v":{"$error":"#NAME?"}},{"$f":"IF(I13=0,0,IF(I13>(INT(0.5+100*POWER(10,IF(96*(LOG(I13)-INT(LOG(I13)))-ROUND(96*(LOG(I13)-INT(LOG(I13))),0)<0,ROUND(96*(LOG(I13)-INT(LOG(I13))),0)-1,ROUND(96*(LOG(I13)-INT(LOG(I13))),0))/96))*POWER(10,INT(LOG(I13))-2)+INT(0.5+100*POWER(10,(IF(96*(LOG(I13)-INT(LOG(I13)))-ROUND(96*(LOG(I13)-INT(LOG(I13))),0)<0,ROUND(96*(LOG(I13)-INT(LOG(I13))),0)-1,ROUND(96*(LOG(I13)-INT(LOG(I13))),0))+1)/96))*POWER(10,INT(LOG(I13))-2))/2,INT(0.5+100*POWER(10,(IF(96*(LOG(I13)-INT(LOG(I13)))-ROUND(96*(LOG(I13)-INT(LOG(I13))),0)<0,ROUND(96*(LOG(I13)-INT(LOG(I13))),0)-1,ROUND(96*(LOG(I13)-INT(LOG(I13))),0))+1)/96))*POWER(10,INT(LOG(I13))-2),INT(0.5+100*POWER(10,IF(96*(LOG(I13)-INT(LOG(I13)))-ROUND(96*(LOG(I13)-INT(LOG(I13))),0)<0,ROUND(96*(LOG(I13)-INT(LOG(I13))),0)-1,ROUND(96*(LOG(I13)-INT(LOG(I13))),0))/96))*POWER(10,INT(LOG(I13))-2)))","v":{"$error":"#NAME?"}},"mΩ"]
[2.2000000000000002,{"$f":"IF(IF((B$3*10^12-$A15)*(B$3*10^12-$A14)*-1<0,0,1)*IF(ABS(B$3*10^12-$A15)>(B$3*10^12-$A14),$A14,$A15)=B15,0,IF((B$3*10^12-$A15)*(B$3*10^12-$A14)*-1<0,0,1)*IF(ABS(B$3*10^12-$A15)>(B$3*10^12-$A14),$A14,$A15))","v":{"$error":"#NAME?"}},{"$f":"IF(IF((C$3*10^12-$A15)*(C$3*10^12-$A14)*-1<0,0,1)*IF(ABS(C$3*10^12-$A15)>(C$3*10^12-$A14),$A14,$A15)=C15,0,IF((C$3*10^12-$A15)*(C$3*10^12-$A14)*-1<0,0,1)*IF(ABS(C$3*10^12-$A15)>(C$3*10^12-$A14),$A14,$A15))","v":0},{"$f":"IF(IF((D$3*10^12-$A15)*(D$3*10^12-$A14)*-1<0,0,1)*IF(ABS(D$3*10^12-$A15)>(D$3*10^12-$A14),$A14,$A15)=D15,0,IF((D$3*10^12-$A15)*(D$3*10^12-$A14)*-1<0,0,1)*IF(ABS(D$3*10^12-$A15)>(D$3*10^12-$A14),$A14,$A15))","v":0},{"$f":"IF(IF((E$3*10^12-$A15)*(E$3*10^12-$A14)*-1<0,0,1)*IF(ABS(E$3*10^12-$A15)>(E$3*10^12-$A14),$A14,$A15)=E15,0,IF((E$3*10^12-$A15)*(E$3*10^12-$A14)*-1<0,0,1)*IF(ABS(E$3*10^12-$A15)>(E$3*10^12-$A14),$A14,$A15))","v":0},null,null,"Cslope_ideal",{"$f":"Cslope_ideal","v":{"$error":"#NAME?"}},{"$f":"#REF!*1000000000000","v":{"$error":"#REF!"}},"pF"]
[2.7,{"$error":"#NAME?"},0,0,0]
[3.3,{"$error":"#NAME?"},0,0,0,null,null,"Ruv1",{"$f":"Ruvlo1","v":1000},{"$f":"IF(I16=\"OPEN\",\"OPEN\",IF(I16>(INT(0.5+100*POWER(10,IF(96*(LOG(I16)-INT(LOG(I16)))-ROUND(96*(LOG(I16)-INT(LOG(I16))),0)<0,ROUND(96*(LOG(I16)-INT(LOG(I16))),0)-1,ROUND(96*(LOG(I16)-INT(LOG(I16))),0))/96))*POWER(10,INT(LOG(I16))-2)+INT(0.5+100*POWER(10,(IF(96*(LOG(I16)-INT(LOG(I16)))-ROUND(96*(LOG(I16)-INT(LOG(I16))),0)<0,ROUND(96*(LOG(I16)-INT(LOG(I16))),0)-1,ROUND(96*(LOG(I16)-INT(LOG(I16))),0))+1)/96))*POWER(10,INT(LOG(I16))-2))/2,INT(0.5+100*POWER(10,(IF(96*(LOG(I16)-INT(LOG(I16)))-ROUND(96*(LOG(I16)-INT(LOG(I16))),0)<0,ROUND(96*(LOG(I16)-INT(LOG(I16))),0)-1,ROUND(96*(LOG(I16)-INT(LOG(I16))),0))+1)/96))*POWER(10,INT(LOG(I16))-2),INT(0.5+100*POWER(10,IF(96*(LOG(I16)-INT(LOG(I16)))-ROUND(96*(LOG(I16)-INT(LOG(I16))),0)<0,ROUND(96*(LOG(I16)-INT(LOG(I16))),0)-1,ROUND(96*(LOG(I16)-INT(LOG(I16))),0))/96))*POWER(10,INT(LOG(I16))-2)))","v":1000},"kΩ"]
[3.9,{"$error":"#NAME?"},0,0,0,null,null,"Ruv2",{"$f":"Ruvlo2","v":333.33333333333331},{"$f":"IF(I17=\"OPEN\",\"OPEN\",IF(I17>(INT(0.5+100*POWER(10,IF(96*(LOG(I17)-INT(LOG(I17)))-ROUND(96*(LOG(I17)-INT(LOG(I17))),0)<0,ROUND(96*(LOG(I17)-INT(LOG(I17))),0)-1,ROUND(96*(LOG(I17)-INT(LOG(I17))),0))/96))*POWER(10,INT(LOG(I17))-2)+INT(0.5+100*POWER(10,(IF(96*(LOG(I17)-INT(LOG(I17)))-ROUND(96*(LOG(I17)-INT(LOG(I17))),0)<0,ROUND(96*(LOG(I17)-INT(LOG(I17))),0)-1,ROUND(96*(LOG(I17)-INT(LOG(I17))),0))+1)/96))*POWER(10,INT(LOG(I17))-2))/2,INT(0.5+100*POWER(10,(IF(96*(LOG(I17)-INT(LOG(I17)))-ROUND(96*(LOG(I17)-INT(LOG(I17))),0)<0,ROUND(96*(LOG(I17)-INT(LOG(I17))),0)-1,ROUND(96*(LOG(I17)-INT(LOG(I17))),0))+1)/96))*POWER(10,INT(LOG(I17))-2),INT(0.5+100*POWER(10,IF(96*(LOG(I17)-INT(LOG(I17)))-ROUND(96*(LOG(I17)-INT(LOG(I17))),0)<0,ROUND(96*(LOG(I17)-INT(LOG(I17))),0)-1,ROUND(96*(LOG(I17)-INT(LOG(I17))),0))/96))*POWER(10,INT(LOG(I17))-2)))","v":332},"kΩ"]
[4.7,{"$error":"#NAME?"},0,0,0,null,null,"Rhys",{"$f":"Rhys","v":{"$error":"#NAME?"}},{"$f":"IF(I18=\"OPEN\",\"OPEN\",IF(I18>(INT(0.5+100*POWER(10,IF(96*(LOG(I18)-INT(LOG(I18)))-ROUND(96*(LOG(I18)-INT(LOG(I18))),0)<0,ROUND(96*(LOG(I18)-INT(LOG(I18))),0)-1,ROUND(96*(LOG(I18)-INT(LOG(I18))),0))/96))*POWER(10,INT(LOG(I18))-2)+INT(0.5+100*POWER(10,(IF(96*(LOG(I18)-INT(LOG(I18)))-ROUND(96*(LOG(I18)-INT(LOG(I18))),0)<0,ROUND(96*(LOG(I18)-INT(LOG(I18))),0)-1,ROUND(96*(LOG(I18)-INT(LOG(I18))),0))+1)/96))*POWER(10,INT(LOG(I18))-2))/2,INT(0.5+100*POWER(10,(IF(96*(LOG(I18)-INT(LOG(I18)))-ROUND(96*(LOG(I18)-INT(LOG(I18))),0)<0,ROUND(96*(LOG(I18)-INT(LOG(I18))),0)-1,ROUND(96*(LOG(I18)-INT(LOG(I18))),0))+1)/96))*POWER(10,INT(LOG(I18))-2),INT(0.5+100*POWER(10,IF(96*(LOG(I18)-INT(LOG(I18)))-ROUND(96*(LOG(I18)-INT(LOG(I18))),0)<0,ROUND(96*(LOG(I18)-INT(LOG(I18))),0)-1,ROUND(96*(LOG(I18)-INT(LOG(I18))),0))/96))*POWER(10,INT(LOG(I18))-2)))","v":{"$error":"#NAME?"}},"kΩ"]
[5.6,{"$error":"#NAME?"},0,0,0]
[6.8,{"$error":"#NAME?"},0,0,0,null,null,"Ra",{"$f":"'Variable Mgmt'!D147","v":681.81818181818187},{"$f":"IF(I20=\"OPEN\",\"OPEN\",IF(I20>(INT(0.5+100*POWER(10,IF(96*(LOG(I20)-INT(LOG(I20)))-ROUND(96*(LOG(I20)-INT(LOG(I20))),0)<0,ROUND(96*(LOG(I20)-INT(LOG(I20))),0)-1,ROUND(96*(LOG(I20)-INT(LOG(I20))),0))/96))*POWER(10,INT(LOG(I20))-2)+INT(0.5+100*POWER(10,(IF(96*(LOG(I20)-INT(LOG(I20)))-ROUND(96*(LOG(I20)-INT(LOG(I20))),0)<0,ROUND(96*(LOG(I20)-INT(LOG(I20))),0)-1,ROUND(96*(LOG(I20)-INT(LOG(I20))),0))+1)/96))*POWER(10,INT(LOG(I20))-2))/2,INT(0.5+100*POWER(10,(IF(96*(LOG(I20)-INT(LOG(I20)))-ROUND(96*(LOG(I20)-INT(LOG(I20))),0)<0,ROUND(96*(LOG(I20)-INT(LOG(I20))),0)-1,ROUND(96*(LOG(I20)-INT(LOG(I20))),0))+1)/96))*POWER(10,INT(LOG(I20))-2),INT(0.5+100*POWER(10,IF(96*(LOG(I20)-INT(LOG(I20)))-ROUND(96*(LOG(I20)-INT(LOG(I20))),0)<0,ROUND(96*(LOG(I20)-INT(LOG(I20))),0)-1,ROUND(96*(LOG(I20)-INT(LOG(I20))),0))/96))*POWER(10,INT(LOG(I20))-2)))","v":681},"kΩ"]
[8.1999999999999993,{"$error":"#NAME?"},0,0,0]
[10,{"$error":"#NAME?"},0,0,0]
[12,{"$error":"#NAME?"},0,0,0]
[15,{"$error":"#NAME?"},0,0,0]
[18,{"$error":"#NAME?"},0,0,0]
[22,{"$error":"#NAME?"},0,0,0]
[27,{"$error":"#NAME?"},0,0,0]
[33,{"$error":"#NAME?"},0,0,0]
[39,{"$error":"#NAME?"},0,0,0]
[47,{"$error":"#NAME?"},0,0,0]
[56,{"$error":"#NAME?"},0,0,0]
[68,{"$error":"#NAME?"},0,0,0]
[82,{"$error":"#NAME?"},0,0,0]
[{"$f":"A22*10","v":100},{"$error":"#NAME?"},0,0,0]
[{"$f":"A23*10","v":120},{"$error":"#NAME?"},0,0,0]
[150,{"$error":"#NAME?"},0,0,0]
[180,{"$error":"#NAME?"},0,0,0]
[220,{"$error":"#NAME?"},0,0,{"$f":"IF(IF((E$3*10^12-$A39)*(E$3*10^12-$A38)*-1<0,0,1)*IF(ABS(E$3*10^12-$A39)>(E$3*10^12-$A38),$A38,$A39)=E39,0,IF((E$3*10^12-$A39)*(E$3*10^12-$A38)*-1<0,0,1)*IF(ABS(E$3*10^12-$A39)>(E$3*10^12-$A38),$A38,$A39))","v":0}]
[270,{"$error":"#NAME?"},0,0,0]
[330,{"$error":"#NAME?"},0,0,0]
[390,{"$error":"#NAME?"},0,0,0]
[470,{"$error":"#NAME?"},0,0,0]
[560,{"$error":"#NAME?"},0,0,0]
[680,{"$error":"#NAME?"},0,0,0]
[{"$f":"A33*10","v":820},{"$error":"#NAME?"},0,0,0]
[1000,{"$error":"#NAME?"},0,0,0]
[1200,{"$error":"#NAME?"},0,0,0]
[1500,{"$error":"#NAME?"},0,0,0]
[1800,{"$error":"#NAME?"},0,0,0]
[2200,{"$error":"#NAME?"},0,0,0]
[2700,{"$error":"#NAME?"},0,0,0]
[3300,{"$error":"#NAME?"},0,0,0]
[3900,{"$error":"#NAME?"},0,0,0]
[4700,{"$error":"#NAME?"},0,0,0]
[5600,{"$error":"#NAME?"},0,0,0]
[6800,{"$error":"#NAME?"},0,0,0]
[8200,{"$error":"#NAME?"},0,0,0]
[10000,{"$error":"#NAME?"},0,0,0]
[12000,{"$error":"#NAME?"},0,0,0]
[15000,{"$error":"#NAME?"},0,0,0]
[18000,{"$error":"#NAME?"},0,0,0]
[22000,{"$error":"#NAME?"},0,0,0]
[27000,{"$error":"#NAME?"},0,0,0]
[33000,{"$error":"#NAME?"},0,0,0]
[39000,{"$error":"#NAME?"},0,0,0]
[47000,{"$error":"#NAME?"},0,0,0]
[56000,{"$error":"#NAME?"},0,0,0]
[68000,{"$error":"#NAME?"},0,0,0]
[82000,{"$error":"#NAME?"},0,0,0]
[100000,{"$error":"#NAME?"},{"$f":"IF(IF((C$3*10^12-$A71)*(C$3*10^12-$A70)*-1<0,0,1)*IF(ABS(C$3*10^12-$A71)>(C$3*10^12-$A70),$A70,$A71)=C71,0,IF((C$3*10^12-$A71)*(C$3*10^12-$A70)*-1<0,0,1)*IF(ABS(C$3*10^12-$A71)>(C$3*10^12-$A70),$A70,$A71))","v":0},{"$f":"IF(IF((D$3*10^12-$A71)*(D$3*10^12-$A70)*-1<0,0,1)*IF(ABS(D$3*10^12-$A71)>(D$3*10^12-$A70),$A70,$A71)=D71,0,IF((D$3*10^12-$A71)*(D$3*10^12-$A70)*-1<0,0,1)*IF(ABS(D$3*10^12-$A71)>(D$3*10^12-$A70),$A70,$A71))","v":0},{"$f":"IF(IF((E$3*10^12-$A71)*(E$3*10^12-$A70)*-1<0,0,1)*IF(ABS(E$3*10^12-$A71)>(E$3*10^12-$A70),$A70,$A71)=E71,0,IF((E$3*10^12-$A71)*(E$3*10^12-$A70)*-1<0,0,1)*IF(ABS(E$3*10^12-$A71)>(E$3*10^12-$A70),$A70,$A71))","v":0}]
[120000,{"$f":"IF(IF((B$3*10^12-$A72)*(B$3*10^12-$A71)*-1<0,0,1)*IF(ABS(B$3*10^12-$A72)>(B$3*10^12-$A71),$A71,$A72)=B72,0,IF((B$3*10^12-$A72)*(B$3*10^12-$A71)*-1<0,0,1)*IF(ABS(B$3*10^12-$A72)>(B$3*10^12-$A71),$A71,$A72))","v":{"$error":"#NAME?"}},{"$f":"IF(IF((C$3*10^12-$A72)*(C$3*10^12-$A71)*-1<0,0,1)*IF(ABS(C$3*10^12-$A72)>(C$3*10^12-$A71),$A71,$A72)=C72,0,IF((C$3*10^12-$A72)*(C$3*10^12-$A71)*-1<0,0,1)*IF(ABS(C$3*10^12-$A72)>(C$3*10^12-$A71),$A71,$A72))","v":0},{"$f":"IF(IF((D$3*10^12-$A72)*(D$3*10^12-$A71)*-1<0,0,1)*IF(ABS(D$3*10^12-$A72)>(D$3*10^12-$A71),$A71,$A72)=D72,0,IF((D$3*10^12-$A72)*(D$3*10^12-$A71)*-1<0,0,1)*IF(ABS(D$3*10^12-$A72)>(D$3*10^12-$A71),$A71,$A72))","v":0},0]
[150000,{"$error":"#NAME?"},0,0,0]
[180000,{"$error":"#NAME?"},0,0,0]
[220000,{"$error":"#NAME?"},0,0,0]
[270000,{"$error":"#NAME?"},0,0,0]
[330000,{"$error":"#NAME?"},0,0,0]
[390000,{"$error":"#NAME?"},0,0,0]
[470000,{"$error":"#NAME?"},0,0,0]
[560000,{"$error":"#NAME?"},0,0,0]
[680000,{"$error":"#NAME?"},0,0,0]
[820000,{"$error":"#NAME?"},0,0,0]
[1000000,{"$error":"#NAME?"},0,0,0]
[1200000,{"$error":"#NAME?"},0,0,0]
[1500000,{"$error":"#NAME?"},0,0,0]
[1800000,{"$error":"#NAME?"},0,0,0]
[2200000,{"$error":"#NAME?"},0,2200000,0]
[2700000,{"$error":"#NAME?"},0,0,0]
[3300000,{"$error":"#NAME?"},0,0,0]
[3900000,{"$error":"#NAME?"},0,0,0]
[4700000,{"$error":"#NAME?"},0,0,0]
[5600000,{"$error":"#NAME?"},0,0,0]
[6800000,{"$error":"#NAME?"},0,0,0]
[8200000,{"$error":"#NAME?"},0,0,0]
[10000000,{"$error":"#NAME?"},0,0,0]
[12000000,{"$error":"#NAME?"},0,0,0]
[15000000,{"$error":"#NAME?"},0,0,0]
[18000000,{"$error":"#NAME?"},0,0,0]
[22000000,{"$error":"#NAME?"},0,0,0]
[{"$f":"A87*10","v":27000000},{"$error":"#NAME?"},0,0,0]
[33000000,{"$error":"#NAME?"},33000000,0,0]
[39000000,{"$error":"#NAME?"},0,0,0]
[47000000,{"$error":"#NAME?"},0,0,{"$f":"IF(IF((E$3*10^12-$A103)*(E$3*10^12-$A102)*-1<0,0,1)*IF(ABS(E$3*10^12-$A103)>(E$3*10^12-$A102),$A102,$A103)=E103,0,IF((E$3*10^12-$A103)*(E$3*10^12-$A102)*-1<0,0,1)*IF(ABS(E$3*10^12-$A103)>(E$3*10^12-$A102),$A102,$A103))","v":0}]
[56000000,{"$error":"#NAME?"},0,{"$f":"IF(IF((D$3*10^12-$A104)*(D$3*10^12-$A103)*-1<0,0,1)*IF(ABS(D$3*10^12-$A104)>(D$3*10^12-$A103),$A103,$A104)=D104,0,IF((D$3*10^12-$A104)*(D$3*10^12-$A103)*-1<0,0,1)*IF(ABS(D$3*10^12-$A104)>(D$3*10^12-$A103),$A103,$A104))","v":0},0]
[68000000,{"$error":"#NAME?"},0,0,0]
[82000000,{"$error":"#NAME?"},0,0,0]
[100000000,{"$error":"#NAME?"},0,0,0]
[120000000,{"$error":"#NAME?"},0,0,0]
[150000000,{"$error":"#NAME?"},0,0,0]
[180000000,{"$error":"#NAME?"},0,0,0]
[220000000,{"$error":"#NAME?"},0,0,0]
[270000000,{"$error":"#NAME?"},0,0,0]
[330000000,{"$error":"#NAME?"},0,0,0]
[390000000,{"$error":"#NAME?"},0,0,0]
[470000000,{"$error":"#NAME?"},0,0,0]
[560000000,{"$error":"#NAME?"},0,0,0]
[680000000,{"$error":"#NAME?"},0,0,0]
[820000000,{"$error":"#NAME?"},0,0,0]
[1000000000,{"$error":"#NAME?"},0,0,0]
[1200000000,{"$error":"#NAME?"},0,0,0]
[1500000000,{"$error":"#NAME?"},0,0,0]
[1800000000,{"$error":"#NAME?"},0,0,0]
[2200000000,{"$error":"#NAME?"},0,0,0]
[2700000000,{"$error":"#NAME?"},0,0,0]
[3300000000,{"$error":"#NAME?"},0,0,0]
[3900000000,{"$error":"#NAME?"},0,0,0]
[4700000000,{"$error":"#NAME?"},0,0,0]
[5600000000,{"$error":"#NAME?"},0,0,0]
[6800000000,{"$error":"#NAME?"},0,0,0]
[8200000000,{"$error":"#NAME?"},0,0,0]
[10000000000,{"$error":"#NAME?"},0,0,0]
[12000000000,{"$error":"#NAME?"},0,0,0]
[15000000000,{"$error":"#NAME?"},0,0,0]
[18000000000,{"$error":"#NAME?"},0,0,0]
[22000000000,{"$error":"#NAME?"},{"$f":"IF(IF((C$3*10^12-$A135)*(C$3*10^12-$A134)*-1<0,0,1)*IF(ABS(C$3*10^12-$A135)>(C$3*10^12-$A134),$A134,$A135)=C135,0,IF((C$3*10^12-$A135)*(C$3*10^12-$A134)*-1<0,0,1)*IF(ABS(C$3*10^12-$A135)>(C$3*10^12-$A134),$A134,$A135))","v":0},0,{"$f":"IF(IF((E$3*10^12-$A135)*(E$3*10^12-$A134)*-1<0,0,1)*IF(ABS(E$3*10^12-$A135)>(E$3*10^12-$A134),$A134,$A135)=E135,0,IF((E$3*10^12-$A135)*(E$3*10^12-$A134)*-1<0,0,1)*IF(ABS(E$3*10^12-$A135)>(E$3*10^12-$A134),$A134,$A135))","v":0}]
[27000000000,{"$f":"IF(IF((B$3*10^12-$A136)*(B$3*10^12-$A135)*-1<0,0,1)*IF(ABS(B$3*10^12-$A136)>(B$3*10^12-$A135),$A135,$A136)=B136,0,IF((B$3*10^12-$A136)*(B$3*10^12-$A135)*-1<0,0,1)*IF(ABS(B$3*10^12-$A136)>(B$3*10^12-$A135),$A135,$A136))","v":{"$error":"#NAME?"}},0,0,0]
[33000000000,{"$error":"#NAME?"},0,0,0]
[39000000000,{"$error":"#NAME?"},0,0,0]
[47000000000,{"$error":"#NAME?"},0,0,0]
[56000000000,{"$error":"#NAME?"},0,0,0]
[68000000000,{"$error":"#NAME?"},0,0,0]
[82000000000,{"$error":"#NAME?"},0,0,0]
[100000000000,{"$error":"#NAME?"},0,0,0]
[120000000000,{"$error":"#NAME?"},0,0,0]
[150000000000,{"$error":"#NAME?"},0,0,0]
[180000000000,{"$error":"#NAME?"},0,0,0]
[220000000000,{"$error":"#NAME?"},0,0,0]
[270000000000,{"$error":"#NAME?"},0,0,0]
[330000000000,{"$error":"#NAME?"},0,0,0]
[390000000000,{"$error":"#NAME?"},0,0,0]
[470000000000,{"$error":"#NAME?"},0,0,0]
[560000000000,{"$error":"#NAME?"},0,0,0]
[680000000000,{"$error":"#NAME?"},0,0,0]
[820000000000,{"$error":"#NAME?"},0,0,0]
[1000000000000,{"$error":"#NAME?"},0,0,0]
[1200000000000,{"$error":"#NAME?"},0,0,0]
[1500000000000,{"$error":"#NAME?"},0,0,0]
[1800000000000,{"$error":"#NAME?"},0,0,0]
[2200000000000,{"$error":"#NAME?"},0,0,0]
[2700000000000,{"$error":"#NAME?"},2700000000000,2700000000000,2700000000000]

{"sheet":"Efficiency","index":9,"n_rows":114,"n_cols":88,"rows_kept":114,"cut":false,"hidden":true,"merged":[[0,0,2,4],[1,6,1,7],[3,0,3,4],[3,10,3,21]]}
["LM5164 (COT) Efficiency Calculator"]
[null,null,null,null,null,null,"TERMS OF USE",null,null,{"$f":"CoutEsr","v":5.0000000000000001E-3}]
[]
[null,null,null,null,null,null,null,"Currents",null,null,"Miscellaneous",null,null,null,null,null,null,null,null,null,null,null,"Inductor",null,null,null,"Cout",null,null,"Cin",null,null,"High-side MOSFET Losses ",null,null,null,null,null,null,null,null,"Low-side MOSFET Losses ",null,null,"Diode",null,null,null,null,null,null,null,"RESULTS"]
["Input Parameters",null,null,null,null,null,null,"Step","Iout (A)","Ripple Current pk-pk (A)","Peak Current (A)","Valley Current (A)","VOUT Hysteresis +Undershoot (2us Delay) (mV)","Vout Rise per Pulse (mV)","Number of Pulses in DCM","VOUT Ripple (mV)","Off Time (sec)","Duty Cycle","Switching Frequency (Hz)","Active Mode Duration (sec)","Sleep Mode Duration (sec)","Operating Quiescent Current (A)","Irms (A)","Inductor DCR Loss @ 25°C (W)","Inductor Core Loss  (W)","Total Inductor Loss (W)","Irms (A)","Cout ESR Loss (W)","Total Cout Loss (W)","Irms (A)","Cin ESR Loss (W)","Total Cin Loss (W)","Irms (A)","Rdson HS Loss @ 25°C (W)","HS Gate Qg Loss (W)     ","SW Rise Time (ns)","SW Fall Time (ns)","HS Switching  Loss (W)","Coss Loss (W)","Total HS FET AC Loss (W)","Total HS FET Loss (W)","Irms (A)","Rdson LS Loss @ 25°C (W)","LS Gate Qg Loss (W)","Reverse Recovery & Leakage Losses","DeadTime Loss @ 25°C (W)","Total LS FET AC Loss (W)","Total LS FET Loss (W)","Quiescent Loss (W)","LDO + Quiescent Loss (W)","Total Gate Drive Loss (W)","Total Power Loss in IC (W)","Total Converter Power Loss (W)","Pout (W)","EFF (%)","High-side MOSFET Rdson %","Low-side MOSFET Rdson %","Gate Drive (Qg) Loss from Vin %","High-side MOSFET AC Loss %","Reverse Recovery & Leakage Loss %","Deadtime Loss %","Low-side MOSFET AC Loss %","Inductor Cu Loss %","Inductor Core Loss %","Cin ESR %","Cout ESR %","LDO + Quiescent Current Loss %","Total Loss %","Overall Eff %","Overall Eff","Current (mA)","Keep for \"previous\" data series","Keep for \"previous\" data series","Frequency (kHz)",null,"Coss",null,"Total Power Loss in IC (mW)","LDO + Quiescent Loss (mW)","Total Inductor Loss (mW)",null,null,"Overall Eff","Total Power Loss in IC (W)","LDO + Quiescent Loss (mW)","Total Inductor Loss (mW)","Fsw (kHz)","Ripple (mV)"]
["Design","Input Value","Units","Std Units","Description",null,null,0.04,{"$f":"IF(PLOT_TYPE=1, H6/100*Iout, min_I*EXP(H6*rr/100))","v":4.0000000000000002E-4},{"$f":"IF(I6<Icrit, (Vin-(Rdcr+RdsonTop)*Iripple/2-Vout)/L*OnTime, (Vin-(Rdcr+RdsonTop)*I6-Vout)/L*OnTime)","v":0.43904382096128897},{"$f":"IF(I6<Icrit, (Vin-(Rdcr+RdsonTop)*Iripple/2-Vout)/L*OnTime, I6+((Vin-(Rdcr+RdsonTop)*J6-Vout)/L*OnTime)/2)","v":0.43904382096128897},{"$f":"IF(I6<Icrit, 0, I6-((Vin-(Rdcr+RdsonTop)*K6-Vout)/L*OnTime)/2)","v":0},{"$f":"1000*((((J6/2)-I6)*0.000002/Cout+Vout/306))","v":52.495802061215528},{"$f":"IF(I6<Icrit, 1000*SQRT((J6*CoutEsr)^2+(((J6/2)-I6)*(OnTime+OffTime)/Cout)^2), 1000*J6*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":21.320896553465481},{"$f":"ROUNDUP(M6/N6,0)","v":3},{"$f":"IF(I6<Icrit, 1000*((N6/1000)*O6), 1000*J6*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":63.96268966039645},{"$f":"IF(I6<Icrit, L*J6/(Vout+J6/2*(RdsonBot+Rdcr)), L*J6/(Vout+I6*(RdsonBot+Rdcr)))","v":2.468766146888617E-6},{"$f":"OnTime*S6","v":4.598442059952765E-4},{"$f":"IF(I6<Icrit,I6/((OnTime+Q6)*J6/2),1/(OnTime+Q6))","v":551.81304719433183},{"$f":"IF(1/S6-OnTime-Q6>Tsleep, OnTime+Q6+Tsleep, 1/S6)","v":8.3020994802219518E-6},{"$f":"IF(1/S6-OnTime-Q6>Tsleep, 1/S6-OnTime-Q6-Tsleep, 0)","v":1.8039058667584421E-3},{"$f":"S6*(T6*Iq_active+U6*Iq_sleep)","v":1.2977784427989642E-5},{"$f":"IF(I6<Icrit,Iripple*SQRT((OnTime+OffTime)*S6/3), SQRT(I6^2+Iripple^2/12))","v":1.0453486351041886E-2},{"$f":"W6^2*Rdcr","v":1.311304522697028E-5},{"$f":"Core_Loss/1000*S6/$S$106","v":1.762427684874202E-4},{"$f":"(Y6+X6*(1+Ltc*(Ta-25)))/(1-X6*Ltc*ThetaCa)","v":1.8935621100023988E-4},{"$f":"Iripple/SQRT(12)*SQRT((OnTime+Q6)*S6)","v":5.314550847443332E-3},{"$f":"RCoutEsr*AA6^2","v":1.4122225355030321E-7},{"$f":"AB6","v":1.4122225355030321E-7},{"$f":"SQRT($R6)*SQRT($I6^2*(1-R6)+(Iripple^2)/12)","v":2.6698269183892055E-3},{"$f":"RCinEsr*AD6^2","v":2.1383927322466804E-8},{"$f":"AE6","v":2.1383927322466804E-8},{"$f":"IF(I6<Icrit,Iripple*SQRT((OnTime)*S6/3), SQRT(OnTime*S6*(I6^2+Iripple^2/12)))","v":5.3396262913862104E-3},{"$f":"RdsonTop*AG6^2","v":1.9587475336052383E-5},{"$f":"QgTop*S6*Vdd","v":2.2155293844852424E-6},{"$f":"20*VIN_nom/24","v":40},{"$f":"IF(I6<Icrit, Csw*Vin/Iripple*1000000000, Csw*Vin/(I6+Iripple/2)*1000000000)","v":17.80717756372006},{"$f":"IF(I6<Icrit, Vin*(I6+Iripple/2)*AK6/1000000000/2*S6, Vin*(I6-Iripple/2)*AJ6/1000000000/2*S6 + Vin*(I6+Iripple/2)*AK6/1000000000/2*S6)","v":5.0949422265397957E-5},{"$f":"IF(I6<Icrit, Csw*(Vin)^2*S6/2, Csw*Vin^2*S6/2)","v":1.0171018085885925E-4},{"$f":"AI6+AL6+AM6","v":1.5487513250874243E-4},{"$f":"(AI6+AL6+AM6+AH6*(1+RdsonTopTc*(Ta-25)))/(1-AH6*RdsonTopTc*ThetaJA)","v":1.7446323987339559E-4},{"$f":"IF(I6<Icrit,Iripple*SQRT((OffTime)*S6/3), SQRT(OffTime*S6*(I6^2+Iripple^2/12)))","v":8.9868664149277411E-3},{"$f":"RdsonBot*AP6^2","v":2.455218545976588E-5},{"$f":"QgBot*S6*Vdd","v":6.0699435191376506E-6},{"$f":"IF(I6<Icrit, Vin*Idss*R6, QrrBot*(I6-Iripple/2)/1*S6*Vin+Vin*Idss*R6)","v":0},{"$f":"IF(I6<Icrit, dead1*S6*(I6+Iripple/2)*((I6+Iripple/2)*BDserR+VSD), dead1*S6*(I6+Iripple/2)*((I6+Iripple/2)*BDserR+VSD)+dead2*S6*(I6-Iripple/2)*((I6-Iripple/2)*BDserR+VSD))","v":1.9589603786657919E-6},{"$f":"AR6+AS6+AT6","v":8.0289038978034433E-6},{"$f":"(AR6+AS6+AT6+AQ6*(1+RdsonBotTc*(Ta-25)))/(1-AQ6*RdsonBotTc*ThetaJA)","v":3.2581237306579754E-5},{"$f":"Vin*V6+Vout*Ifb/0.8","v":9.8085769310822741E-4},{"$f":"(Vin-Vdd)*(S6*QgBot+S6*QgTop)+AW6","v":1.0521127600793842E-3},{"$f":"AI6+AR6","v":8.2854729036228938E-6},{"$f":"AO6+AV6+AX6+AY6","v":1.2674427101629826E-3},{"$f":"SUM(Z6,AC6,AF6,AZ6)","v":1.4569615273440951E-3},{"$f":"Vout*I6","v":4.8000000000000004E-3},{"$f":"BB6/(BB6+BA6)","v":0.76714551927850283},{"$f":"(AO6-AN6)/($BB6+$BA6)","v":3.1306101658208144E-3},{"$f":"(AV6-AU6)/($BB6+$BA6)","v":3.9240026171613821E-3},{"$f":"Vin*S6*(QgBot+QgTop)/($BB6+$BA6)","v":1.2712326826235498E-2},{"$f":"AN6/($BB6+$BA6)","v":2.4752450823280446E-2},{"$f":"AS6/(BA6+BB6)","v":0},{"$f":"AT6/($BB6+$BA6)","v":3.1308493269532943E-4},{"$f":"AU6/($BB6+$BA6)","v":1.2831953437328369E-3},{"$f":"X6/($BB6+$BA6)","v":2.0957528937430433E-3},{"$f":"Y6/($BB6+$BA6)","v":2.8167468781325606E-2},{"$f":"(AF6)/($BB6+$BA6)","v":3.4176216729182417E-6},{"$f":"(AC6)/($BB6+$BA6)","v":2.2570420631984944E-5},{"$f":"AX6/($BB6+$BA6)","v":0.16815074784804959},{"$f":"SUM(BD6:BO6)","v":0.24455562827434946},{"$f":"BC6","v":0.76714551927850283},{"$f":"100*BQ6","v":76.71455192785028},{"$f":"I6*1000","v":0.4},8.7924221262065743,{"$f":"BT6/100","v":8.7924221262065741E-2},{"$f":"S6/1000","v":0.55181304719433188},null,{"$f":"AM6/($BB6+$BA6)","v":1.6255522814766669E-2},null,{"$f":"AZ6","v":1.2674427101629826E-3},{"$f":"AX6","v":1.0521127600793842E-3},{"$f":"Z6","v":1.8935621100023988E-4},null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR6, IF(MODE_ILIM=4,#REF!,#REF!))","v":76.71455192785028},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ6, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.2674427101629826E-3},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA6, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0521127600793842E-3},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB6, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.8935621100023988E-4},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S6, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":0.55181304719433188},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P6, IF(MODE_ILIM=4,#REF!,#REF!))","v":63.96268966039645}]
[null,null,null,null,null,null,null,1,0.01,0.43904382096128897,0.43904382096128897,0,{"$f":"IF(I7<Icrit, 1000*((((J7/2)-I7)*0.000002/Cout+Vout/306)), 1000*J7*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":51.913983879397342},20.396928522527151,{"$f":"ROUNDUP(M7/N7,0)","v":3},61.19078556758145,2.468766146888617E-6,{"$f":"OnTime*S7","v":1.1496105149881912E-2},13795.326179858293,{"$f":"IF(1/S7-OnTime-Q7>Tsleep, OnTime+Q7+Tsleep, 1/S7)","v":8.3020994802219518E-6},{"$f":"IF(1/S7-OnTime-Q7>Tsleep, 1/S7-OnTime-Q7-Tsleep, 0)","v":6.4186219169324628E-5},8.4444610699740974E-5,{"$f":"IF(I7<Icrit,Iripple*SQRT((OnTime+OffTime)*S7/3), SQRT(I7^2+Iripple^2/12))","v":5.2267431755209433E-2},3.2782613067425703E-4,4.4060692121855038E-3,4.7341436590194073E-3,{"$f":"Iripple/SQRT(12)*SQRT((OnTime+Q7)*S7)","v":2.6572754237216657E-2},{"$f":"RCoutEsr*AA7^2","v":3.530556338757579E-6},{"$f":"AB7","v":3.530556338757579E-6},{"$f":"SQRT($R7)*SQRT($I7^2*(1-R7)+(Iripple^2)/12)","v":1.3391562653197693E-2},{"$f":"RCinEsr*AD7^2","v":5.3800185088355776E-7},{"$f":"AE7","v":5.3800185088355776E-7},{"$f":"IF(I7<Icrit,Iripple*SQRT((OnTime)*S7/3), SQRT(OnTime*S7*(I7^2+Iripple^2/12)))","v":2.6698131456931048E-2},{"$f":"RdsonTop*AG7^2","v":4.8968688340130938E-4},{"$f":"QgTop*S7*Vdd","v":5.5388234612131045E-5},40,17.80717756372006,1.3303346582159419E-3,2.5427545214714805E-3,{"$f":"AI7+AL7+AM7","v":3.9284774142995535E-3},4.4185644764327099E-3,4.4934332074638698E-2,{"$f":"RdsonBot*AP7^2","v":6.1380463649414691E-4},1.5174858797844124E-4,0,5.1209961257249137E-5,{"$f":"AR7+AS7+AT7","v":2.0295854923569039E-4},8.1685591780103321E-4,4.411265354152291E-3,6.1926420284312122E-3,2.0713682259057228E-4,{"$f":"AO7+AV7+AX7+AY7","v":1.1635199245255527E-2},1.6373411462464574E-2,0.12,{"$f":"BB7/(BB7+BA7)","v":0.8799369225505429},{"$f":"(AO7-AN7)/($BB7+$BA7)","v":3.5937141769607195E-3},{"$f":"(AV7-AU7)/($BB7+$BA7)","v":4.5015913438105348E-3},1.4581387057379675E-2,{"$f":"AN7/($BB7+$BA7)","v":2.8806769385400527E-2},{"$f":"AS7/(BA7+BB7)","v":0},{"$f":"AT7/($BB7+$BA7)","v":3.7551279760530281E-4},{"$f":"AU7/($BB7+$BA7)","v":1.488256010164802E-3},2.4038859713096487E-3,3.230885819262673E-2,{"$f":"(AF7)/($BB7+$BA7)","v":3.9450641082747821E-6},{"$f":"(AC7)/($BB7+$BA7)","v":2.5888890663480465E-5},{"$f":"AX7/($BB7+$BA7)","v":4.5409453074624267E-2},{"$f":"SUM(BD7:BO7)","v":0.13349926196465395},0.8799369225505429,{"$f":"100*BQ7","v":87.993692255054285},10,9.5725635821403898,{"$f":"BT7/100","v":9.5725635821403893E-2},13.795326179858293,null,1.864552990354244E-2,null,{"$f":"AZ7","v":1.1635199245255527E-2},{"$f":"AX7","v":6.1926420284312122E-3},{"$f":"Z7","v":4.7341436590194073E-3},null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR7, IF(MODE_ILIM=4,#REF!,#REF!))","v":87.993692255054285},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ7, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.1635199245255527E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA7, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.1926420284312122E-3},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB7, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.7341436590194073E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S7, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":13.795326179858293},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P7, IF(MODE_ILIM=4,#REF!,#REF!))","v":61.19078556758145}]
["Vin",{"$f":"Vin","v":48},"V",{"$f":"B8","v":48},"Vin",null,null,2,0.02,0.43904382096128897,0.43904382096128897,0,51.307923273336741,19.434985238929613,3,58.304955716788839,2.468766146888617E-6,{"$f":"OnTime*S8","v":2.2992210299763824E-2},27590.652359716587,8.3020994802219518E-6,2.7942059844551336E-5,1.5888922139948195E-4,7.3917310858627364E-2,6.5565226134851407E-4,8.8121384243710077E-3,9.4687840024624704E-3,3.7579549431878918E-2,7.0611126775151555E-6,{"$f":"AB8","v":7.0611126775151555E-6},1.9114929742792771E-2,1.0961416172157112E-6,{"$f":"AE8","v":1.0961416172157112E-6},3.7756859596411646E-2,9.7937376680261876E-4,1.1077646922426209E-4,40,17.80717756372006,2.7785841113922866E-3,5.085509042942961E-3,7.9748696235595103E-3,8.9558656126755495E-3,6.3546741836130419E-2,1.2276092729882938E-3,3.0349717595688249E-4,0,1.070889709473157E-4,4.1058614690419817E-4,1.6385674506268714E-3,7.9846066677398582E-3,1.1547360016297702E-2,4.1427364518114456E-4,{"$f":"AO8+AV8+AX8+AY8","v":2.2556066724781269E-2},3.2033007981538471E-2,0.24,{"$f":"BB8/(BB8+BA8)","v":0.88224587810420274},3.606165282643254E-3,4.5140893483264733E-3,1.4619648634730711E-2,2.9315816057515806E-2,0,3.9366168003620835E-4,1.509324732137148E-3,2.4101937710184419E-3,3.2393636675770776E-2,4.0294434316959837E-6,2.5956823144029487E-5,4.2448378239016364E-2,0.13124090068777092,0.88224587810420274,{"$f":"100*BQ8","v":88.224587810420275},20,10.507357436577642,0.10507357436577643,27.590652359716586,null,1.8694455796658651E-2,null,2.2556066724781269E-2,1.1547360016297702E-2,9.4687840024624704E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR8, IF(MODE_ILIM=4,#REF!,#REF!))","v":88.224587810420275},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ8, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.2556066724781269E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA8, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.1547360016297702E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB8, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.4687840024624704E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S8, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":27.590652359716586},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P8, IF(MODE_ILIM=4,#REF!,#REF!))","v":58.304955716788839}]
["Vout",{"$f":"Vout","v":12},"V",{"$f":"B9","v":12},"Vout",null,null,3,0.03,0.43904382096128897,0.43904382096128897,0,50.701862667276139,18.473658372914446,3,55.420975118743335,2.468766146888617E-6,3.4488315449645729E-2,41385.978539574877,8.3020994802219518E-6,1.5860673402960243E-5,2.3333383209922292E-4,9.0529847381161682E-2,9.834783920227711E-4,1.3218207636556512E-2,1.4203921108498035E-2,4.6025360435900407E-2,1.0591669016272734E-5,1.0591669016272734E-5,2.3760506136466467E-2,1.6936849555831821E-6,1.6936849555831821E-6,4.6242520150557472E-2,1.4690606502039286E-3,1.6616470383639314E-4,40,17.80717756372006,4.344748359529034E-3,7.6282635644144411E-3,1.2139176627779868E-2,1.3611935678575365E-2,7.7828546157446069E-2,1.8414139094824406E-3,4.552457639353237E-4,0,1.676535834616155E-4,6.2289934739693923E-4,2.4651528127465484E-3,1.1557947981327425E-2,1.6902078004164191E-2,6.2141046777171684E-4,3.3600576963257821E-2,4.7816783425727712E-2,0.36,{"$f":"BB9/(BB9+BA9)","v":0.8827493488030117},3.6113252584262959E-3,4.5173556857429423E-3,1.4627991620396213E-2,2.9766250731048386E-2,0,4.1110025451453463E-4,1.5273999813457475E-3,2.4115691947775952E-3,3.2412122731981269E-2,4.1530535878291999E-6,2.5971635907921643E-5,4.1445273198871244E-2,0.13076051334659999,0.8827493488030117,88.274934880301174,30,11.516667783884284,0.11516667783884284,41.385978539574879,null,1.8705124149957193E-2,null,3.3600576963257821E-2,1.6902078004164191E-2,1.4203921108498035E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR9, IF(MODE_ILIM=4,#REF!,#REF!))","v":88.274934880301174},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ9, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.3600576963257821E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA9, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.6902078004164191E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB9, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.4203921108498035E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S9, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":41.385978539574879},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P9, IF(MODE_ILIM=4,#REF!,#REF!))","v":55.420975118743335}]
["Iout",{"$f":"Iout","v":1},"A",{"$f":"B10","v":1},"Iout(max)",null,null,4,0.04,0.43904382096128897,0.43904382096128897,0,50.095802061215529,17.513049434016406,3,52.539148302049213,2.468766146888617E-6,4.5984420599527648E-2,55181.304719433174,8.3020994802219518E-6,9.8199801821646906E-6,3.0777844279896392E-4,0.10453486351041887,1.3113045226970281E-3,1.7624276848742015E-2,1.8939555055311346E-2,5.3145508474433313E-2,1.4122225355030316E-5,1.4122225355030316E-5,2.7981815329785463E-2,2.3489459674506504E-6,2.3489459674506504E-6,5.3396262913862097E-2,1.9587475336052375E-3,2.2155293844852418E-4,40,17.80717756372006,6.0288274026261846E-3,1.0171018085885922E-2,1.642139842696063E-2,1.838680695567366E-2,8.9868664149277397E-2,2.4552185459765876E-3,6.0699435191376497E-4,0,2.3292035319156441E-4,8.3991470510532936E-4,3.296630226703822E-3,1.5131289294914993E-2,2.2256795992030679E-2,8.2854729036228912E-4,4.4768780464770452E-2,6.3724806691404276E-2,0.48,0.88279952301758446,3.6147118993386574E-3,4.5183068555355119E-3,1.4628823054586819E-2,3.0201672288755328E-2,0,4.2837911812208416E-4,1.5447422938384165E-3,2.4117062649327871E-3,3.2413964990831892E-2,4.3201007909573184E-6,2.5973112098682503E-5,4.093393517846744E-2,0.13072653515729857,0.88279952301758446,88.279952301758442,40,12.603144523181673,0.12603144523181672,55.181304719433172,null,1.8706187322548577E-2,null,4.4768780464770452E-2,2.2256795992030679E-2,1.8939555055311346E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR10, IF(MODE_ILIM=4,#REF!,#REF!))","v":88.279952301758442},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ10, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.4768780464770452E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA10, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.2256795992030679E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB10, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.8939555055311346E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S10, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":55.181304719433172},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P10, IF(MODE_ILIM=4,#REF!,#REF!))","v":52.539148302049213}]
["Rt",{"$f":"Vout*2500/(Fsw/1000)","v":100},"kW",{"$f":"B11*1000","v":100000},"RT pin resistance to get Fsw",null,null,5,0.05,0.43904382096128897,0.43904382096128897,0,49.489741455154928,16.553283409488969,3,49.659850228466901,2.468766146888617E-6,5.748052574940956E-2,68976.630899291471,8.3020994802219518E-6,6.195564249687362E-6,3.8222305349870493E-4,0.11687353041397945,1.6391306533712856E-3,2.2030346060927519E-2,2.3675685921104066E-2,5.9418484823812019E-2,1.7652781693787895E-5,1.7652781693787895E-5,3.2037931680851631E-2,3.0792871991607496E-6,3.0792871991607496E-6,5.9698836809923328E-2,2.4484344170065475E-3,2.7694117306065527E-4,40,17.80717756372006,7.8308212406837385E-3,1.2713772607357404E-2,2.0821535021101796E-2,2.3280511737211872E-2,0.10047622104244129,3.0690231824707349E-3,7.5874293989220624E-4,0,3.0290583452857826E-4,1.0616487744207845E-3,4.1330179233218739E-3,1.8704630608502561E-2,2.7611513979897168E-2,1.0356841129528615E-3,5.6060727753383777E-2,7.9757145743380789E-2,0.60000000000000009,0.88266817606432291,3.6174341549891974E-3,4.5183330078012599E-3,1.4626646511342373E-2,3.0630843899892238E-2,0,4.4560890080430285E-4,1.5618059788981959E-3,2.4113474402372571E-3,3.240914229277455E-2,4.5299813594357261E-6,2.596924770019571E-5,4.0619674471683971E-2,0.13087133588748298,0.88266817606432291,88.266817606432284,50,13.76888730592373,0.1376888730592373,68.976630899291465,null,1.8703404130387846E-2,null,5.6060727753383777E-2,2.7611513979897168E-2,2.3675685921104066E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR11, IF(MODE_ILIM=4,#REF!,#REF!))","v":88.266817606432284},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ11, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.6060727753383777E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA11, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.7611513979897168E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB11, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.3675685921104066E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S11, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":68.976630899291465},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P11, IF(MODE_ILIM=4,#REF!,#REF!))","v":49.659850228466901}]
["Tamb",{"$f":"'Design Converter'!E56","v":25},"°C",{"$f":"B12","v":25},"Ambient temperature",null,null,6,0.06,0.43904382096128897,0.43904382096128897,0,48.883680849094311,15.594515931853522,4,62.378063727414087,2.468766146888617E-6,6.8976630899291458E-2,82771.957079149754,8.3020994802219518E-6,3.779286961369148E-6,4.5666766419844582E-4,0.12802853796600527,1.9669567840455422E-3,2.6436415273113023E-2,2.8412313784094253E-2,6.508968894156042E-2,2.1183338032545464E-5,2.1183338032545464E-5,3.606068792990539E-2,3.9011196419340726E-6,3.9011196419340726E-6,6.5396799155229515E-2,2.9381213004078571E-3,3.3232940767278629E-4,40,17.80717756372006,9.7507298737016922E-3,1.5256527128828882E-2,2.5339586410203362E-2,2.8293082328136689E-2,0.11006618551564067,3.6828278189648821E-3,9.104915278706474E-4,0,3.7762658186407276E-4,1.2881181097347202E-3,4.9743341417080077E-3,2.2277971922090124E-2,3.2966231967763653E-2,1.2428209355434337E-3,6.7476469373151785E-2,9.5913867614920517E-2,0.72,0.88244608723798756,3.6198623839633791E-3,4.5178984918455116E-3,1.4622966289436778E-2,3.1056692888767834E-2,0,4.6282652722639812E-4,1.5787427581052732E-3,2.4107407192322278E-3,3.2400987803273835E-2,4.7812885609333078E-6,2.5962713557582494E-5,4.0404058904073475E-2,0.13110552076804322,0.88244608723798756,88.244608723798763,60,15.015319606822954,0.15015319606822955,82.771957079149757,null,1.8698698152326745E-2,null,6.7476469373151785E-2,3.2966231967763653E-2,2.8412313784094253E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR12, IF(MODE_ILIM=4,#REF!,#REF!))","v":88.244608723798763},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ12, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.7476469373151785E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA12, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.2966231967763653E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB12, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.8412313784094253E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S12, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":82.771957079149757},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P12, IF(MODE_ILIM=4,#REF!,#REF!))","v":62.378063727414087}]
["VDD",5,"V",{"$f":"B13","v":5},"Gate drive rail",null,null,7,7.0000000000000007E-2,0.43904382096128897,0.43904382096128897,0,48.277620243033709,14.636943226651317,4,58.547772906605267,2.468766146888617E-6,8.0472736049173391E-2,96567.283259008065,8.3020994802219518E-6,2.053374612570416E-6,5.3111227489818693E-4,0.13828662609232437,2.294782914719799E-3,3.084248448529853E-2,3.3149438722516404E-2,7.0304899361713122E-2,2.4713894371303053E-5,2.4713894371303053E-5,4.0124401270171292E-2,4.829902731869171E-6,4.829902731869171E-6,7.0636616305150113E-2,3.4278081838091663E-3,3.8771764228491741E-4,40,17.80717756372006,1.1788553301680053E-2,1.7799281650300366E-2,2.9975552594265334E-2,3.342455104510534E-2,0.11888506799828705,4.2966324554590297E-3,1.0622401158490889E-3,0,4.5709914958946401E-4,1.5193392654385528E-3,5.8205971292583647E-3,2.5851313235677697E-2,3.8320949955630151E-2,1.4499577581340063E-3,7.9016055888127851E-2,0.11219503840774742,0.84000000000000008,0.88217220854735912,3.6221554531594619E-3,4.5172025586400228E-3,1.4618427860496613E-2,3.1480475517274481E-2,0,4.8004781704578226E-4,1.5956177087198217E-3,2.4099925143037035E-3,3.2390931732718405E-2,5.0723880476689869E-6,2.5954655689688762E-5,4.024485363808461E-2,0.13139073184418026,0.88217220854735912,88.217220854735913,70,16.343061169118954,0.16343061169118955,96.567283259008065,null,1.8692894766668994E-2,null,7.9016055888127851E-2,3.8320949955630151E-2,3.3149438722516404E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR13, IF(MODE_ILIM=4,#REF!,#REF!))","v":88.217220854735913},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ13, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.9016055888127851E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA13, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.8320949955630151E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB13, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.3149438722516404E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S13, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":96.567283259008065},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P13, IF(MODE_ILIM=4,#REF!,#REF!))","v":58.547772906605267}]
["K1",400,"pC",4,"RT constant",null,null,8,0.08,0.43904382096128897,0.43904382096128897,0,47.6715596369731,13.680816176274156,4,54.723264705096625,2.468766146888617E-6,9.1968841199055296E-2,110362.60943886635,8.3020994802219518E-6,7.5894035097137113E-7,6.0555688559792782E-4,0.14783462171725473,2.6226090453940563E-3,3.5248553697484031E-2,3.7887060814621419E-2,7.5159098863757837E-2,2.8244450710060622E-5,2.8244450710060622E-5,4.4272430661163334E-2,5.8801443499425457E-6,5.8801443499425457E-6,7.5513719192823292E-2,3.917495067210475E-3,4.4310587689704836E-4,40,17.80717756372006,1.3944291524618815E-2,2.0342036171771844E-2,3.4729433573287706E-2,3.8674950216490922E-2,0.12709348367226084,4.9104370919531752E-3,1.2139887038275299E-3,0,5.4134009209616735E-4,1.7553287959236972E-3,6.6718251416626193E-3,2.942465454926526E-2,4.3675667943496629E-2,1.6570945807245782E-3,9.0679537882374747E-2,0.12860072329205618,0.96,0.88186603174104783,3.6243928180311252E-3,4.5163449192564022E-3,1.4613354221231794E-2,3.1902820593634952E-2,0,4.9728066545747971E-4,1.6124633746479402E-3,2.4091560746560773E-3,3.237968976438696E-2,5.4015620457795587E-6,2.5945647569152899E-5,4.0120924971844864E-2,0.13170777461276251,0.88186603174104783,88.186603174104789,80,17.75180413241851,0.17751804132418511,110.36260943886634,null,1.8686406996180516E-2,null,9.0679537882374747E-2,4.3675667943496629E-2,3.7887060814621419E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR14, IF(MODE_ILIM=4,#REF!,#REF!))","v":88.186603174104789},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ14, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.0679537882374747E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA14, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.3675667943496629E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB14, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7887060814621419E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S14, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":110.36260943886634},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P14, IF(MODE_ILIM=4,#REF!,#REF!))","v":54.723264705096625}]
["Outputs",null,null,null,null,null,null,9,0.09,0.43904382096128897,0.43904382096128897,0,47.065499030912498,12.72646061696674,4,50.905842467866961,2.468766146888617E-6,0.1034649463489372,124157.93561872464,8.054257627727397E-6,0,6.600000000000001E-4,0.15680229526562831,2.9504351760683135E-3,3.9654622909669542E-2,4.2625180138676638E-2,7.9718262711649973E-2,3.1775007048818214E-5,3.1775007048818214E-5,4.8529718805451788E-2,7.0654008220086634E-6,7.0654008220086634E-6,8.0094394370793145E-2,4.4071819506117851E-3,4.9849411150917943E-4,40,17.80717756372006,1.621794454251798E-2,2.2884790693243326E-2,3.9601229347270485E-2,4.4044312182387697E-2,0.13480299622391612,5.5242417284473233E-3,1.3657372918059714E-3,0,6.3036596377559918E-4,1.9961032555815706E-3,7.5280364429087115E-3,3.2037924040564734E-2,4.807031410907503E-2,1.8642314033151509E-3,0.1015068941376866,0.14417091468423407,1.08,0.88222974998436243,3.6294628322085833E-3,4.5189222525794633E-3,1.4619381376530866E-2,3.2349428394551696E-2,0,5.1493296909296154E-4,1.6305756260321302E-3,2.4101497108590889E-3,3.2393044495668447E-2,5.7715803710555662E-6,2.5956348633731707E-5,3.926764925751762E-2,0.13136527484404564,0.88222974998436243,88.222974998436243,90,19.240199150848532,0.19240199150848533,124.15793561872465,null,1.8694114047911593E-2,null,0.1015068941376866,4.807031410907503E-2,4.2625180138676638E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR15, IF(MODE_ILIM=4,#REF!,#REF!))","v":88.222974998436243},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ15, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.1015068941376866},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA15, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.807031410907503E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB15, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.2625180138676638E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S15, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":124.15793561872465},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P15, IF(MODE_ILIM=4,#REF!,#REF!))","v":50.905842467866961}]
["Design","Value","Units","Std Units","Description",null,null,10,0.1,0.43904382096128897,0.43904382096128897,0,46.459438424851896,11.774307316305975,4,47.097229265223902,2.468766146888617E-6,0.11496105149881912,137953.26179858294,7.2488318649546564E-6,0,6.5999999999999989E-4,0.16528413179387413,3.2782613067425703E-3,4.4060692121855038E-2,4.7363796772965809E-2,8.4030427093494869E-2,3.5305563387575783E-5,3.5305563387575783E-5,5.290959874729706E-2,8.3982769187999363E-6,8.3982769187999363E-6,8.4426904674491723E-2,4.8968688340130942E-3,5.5388234612131055E-4,40,17.80717756372006,1.8609512355377548E-2,2.5427545214714808E-2,4.459093991621367E-2,4.9532669294616381E-2,0.14209483449421742,6.138046364941468E-3,1.5174858797844125E-3,0,7.2419331901917515E-4,2.2416791988035876E-3,8.3892493052875328E-3,3.2037924040564721E-2,4.9851690783353941E-2,2.071368225905723E-3,0.10984497760916359,0.15725247822243577,1.2000000000000002,0.88413911136976819,3.6409801843757072E-3,4.529422642525054E-3,1.4651021300574872E-2,3.2853828327219892E-2,0,5.3357303128128038E-4,1.6516302123385812E-3,2.4153658654843921E-3,3.2463150982461546E-2,6.1877042433541744E-6,2.6012524533250227E-5,3.6729857991229173E-2,0.12950103076626709,0.88413911136976819,88.413911136976822,100,20.80575856495858,0.20805758564958579,137.95326179858293,null,1.8734572692043788E-2,null,0.10984497760916359,4.9851690783353941E-2,4.7363796772965809E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR16, IF(MODE_ILIM=4,#REF!,#REF!))","v":88.413911136976822},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ16, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10984497760916359},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA16, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.9851690783353941E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB16, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.7363796772965809E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S16, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":137.95326179858293},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P16, IF(MODE_ILIM=4,#REF!,#REF!))","v":47.097229265223902}]
["On-Time",{"$f":"(Rt*k_RT/10000)/Vin","v":0.83333333333333337},"µs",{"$f":"B17/1000000","v":8.3333333333333333E-7},"On Time - fixed",null,null,11,0.11,0.43904382096128897,0.43904382096128897,0,45.853377818791287,10.824937416901657,5,54.124687084508288,2.468766146888617E-6,0.12645715664870102,151748.58797844124,6.5898471499587784E-6,0,6.5999999999999989E-4,0.17335145988753667,3.606087437416828E-3,4.8466761334040542E-2,5.2102910795789138E-2,8.813185545117426E-2,3.8836119726333372E-5,3.8836119726333372E-5,5.741784233704926E-2,9.8904258559267401E-6,9.8904258559267401E-6,8.8547684646224853E-2,5.3865557174144051E-3,6.0927058073344156E-4,40,17.80717756372006,2.1118994963197517E-2,2.797029973618629E-2,4.9698565280117249E-2,5.5140053916729506E-2,0.14903031969680852,6.7518510014356178E-3,1.6692344677628538E-3,0,8.228387122183108E-4,2.4920731799811646E-3,9.2554820093976829E-3,3.2037924040564721E-2,5.163306745763286E-2,2.2785050484962952E-3,0.11830710843225635,0.17045874577362774,1.32,0.88563336874839127,3.6508817517037907E-3,4.537803443802094E-3,1.4675782558618114E-2,3.3344475599236416E-2,0,5.5207077321097777E-4,1.672017549662299E-3,2.4194480039399385E-3,3.2518015994386813E-2,6.6358266432883252E-6,2.6056487532082179E-5,3.4642399599482059E-2,0.12804558758821785,0.88563336874839127,88.563336874839123,110,22.444784059665849,0.22444784059665848,151.74858797844124,null,1.8766235439591591E-2,null,0.11830710843225635,5.163306745763286E-2,5.2102910795789138E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR17, IF(MODE_ILIM=4,#REF!,#REF!))","v":88.563336874839123},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ17, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.11830710843225635},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA17, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.163306745763286E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB17, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.2102910795789138E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S17, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":151.74858797844124},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P17, IF(MODE_ILIM=4,#REF!,#REF!))","v":54.124687084508288}]
["Off Time",{"$f":"L*Iripple*1000000/(Vout+(Rdcr+RdsonBot)*Iout)","v":2.360552157115261},"µs",{"$f":"B18/1000000","v":2.3605521571152612E-6},"Off Time - depends on Vout, L, Iout, DCR, etc.",null,null,12,0.12,0.43904382096128897,0.43904382096128897,0,45.247317212730685,9.879153391777491,5,49.39576695888745,2.468766146888617E-6,0.13795326179858292,165543.91415829951,6.0406932207955486E-6,0,6.6E-4,0.18105969476232336,3.9339135680910844E-3,5.2872830546226046E-2,5.6842522285463257E-2,9.2050720871800815E-2,4.2366676065090934E-5,4.2366676065090934E-5,6.2055215450643651E-2,1.1552549293877409E-5,1.1552549293877409E-5,9.2485040301114943E-2,5.8762426008157143E-3,6.6465881534557257E-4,40,17.80717756372006,2.3746392365977885E-2,3.0513054257657764E-2,5.4924105438981227E-2,6.0866498424016702E-2,0.15565709231489214,7.3656556379297624E-3,1.8209830557412948E-3,0,9.2631869776442206E-4,2.7473017535057168E-3,1.0126752844150152E-2,3.2037924040564728E-2,5.3414444131911785E-2,2.4856418710868674E-3,0.12689333727116553,0.18378977878198777,1.44,0.88681430245247062,3.6595827013352006E-3,4.5445852579388667E-3,1.4695351747030362E-2,3.3824640453261168E-2,0,5.7046713181016452E-4,1.6919072834455705E-3,2.4226741783298644E-3,3.256137662467995E-2,7.1145596830539425E-6,2.6091232140203749E-5,3.2894925703977645E-2,0.12689871687363205,0.88681430245247062,88.681430245247057,120,24.152326085424395,0.24152326085424394,165.54391415829951,null,1.8791258977221639E-2,null,0.12689333727116553,5.3414444131911785E-2,5.6842522285463257E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR18, IF(MODE_ILIM=4,#REF!,#REF!))","v":88.681430245247057},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ18, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.12689333727116553},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA18, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.3414444131911785E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB18, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.6842522285463257E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S18, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":165.54391415829951},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P18, IF(MODE_ILIM=4,#REF!,#REF!))","v":49.39576695888745}]
["DIL",{"$f":"(Vin-Vout-(Rdcr+RdsonTop)*Iout)/L*OnTime*1000","v":431.28676470588232},"mA",{"$f":"B19/1000","v":0.43128676470588234},"Inductor pk-pk ripple current in CCM",null,null,13,0.13,0.43904382096128897,0.43904382096128897,0,44.641256606670069,8.9380936308650263,5,44.690468154325131,2.468766146888617E-6,0.14944936694846486,179339.24033815783,5.5760245115035816E-6,0,6.6E-4,0.1884529052302224,4.2617396987653421E-3,5.727889975841155E-2,6.1582631320321254E-2,9.5809427932587649E-2,4.589723240384853E-5,4.589723240384853E-5,6.6819152289390393E-2,1.3394397338018237E-5,1.3394397338018237E-5,9.6261481927043008E-2,6.3659294842170243E-3,7.200470499577038E-4,40,17.80717756372006,2.6491704563718667E-2,3.3055808779129253E-2,6.0267560392805619E-2,6.6712035203510059E-2,0.16201303832383601,7.9794602744239097E-3,1.9727316437197365E-3,0,1.0346498300489251E-3,3.0073814737686614E-3,1.1003080106773077E-2,3.2037924040564728E-2,5.5195820806190718E-2,2.6927786936774404E-3,0.13560371481015129,0.19724563776021442,1.56,0.88775295068501414,3.6673727748834065E-3,4.5501314450242334E-3,1.4710906036023909E-2,3.4296605493141334E-2,0,5.8879066637928309E-4,1.7114178058804971E-3,2.4252384568143564E-3,3.2595841200333972E-2,7.6223818970981982E-6,2.6118848394097677E-5,3.1410418452677634E-2,0.1259904635614498,0.88775295068501414,88.775295068501407,130,25.922181532084487,0.25922181532084487,179.33924033815782,null,1.881114857753307E-2,null,0.13560371481015129,5.5195820806190718E-2,6.1582631320321254E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR19, IF(MODE_ILIM=4,#REF!,#REF!))","v":88.775295068501407},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ19, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.13560371481015129},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA19, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.5195820806190718E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB19, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.1582631320321254E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S19, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":179.33924033815782},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P19, IF(MODE_ILIM=4,#REF!,#REF!))","v":44.690468154325131}]
["CCM Freq",{"$f":"'Design Converter'!E12","v":300},"kHz",{"$f":"B20*1000","v":300000},"Frequency in CCM",{"$f":"10000*Vout/(k_RT*Rt/1000+Vin*0.75)","v":275.22935779816515},null,14,0.14000000000000001,0.43904382096128897,0.43904382096128897,0,44.035196000609467,8.0034247748923928,6,48.02054864935436,2.468766146888617E-6,0.16094547209834678,193134.56651801613,5.1777370463961831E-6,0,6.6E-4,0.19556682211458226,4.5895658294395989E-3,6.1684968970597061E-2,6.6323237978712646E-2,9.9426142178610247E-2,4.9427788742606106E-5,4.9427788742606106E-5,7.170487788752232E-2,1.5424768538593463E-5,1.5424768538593463E-5,9.9895260778887801E-2,6.8556163676183335E-3,7.7543528456983481E-4,40,17.80717756372006,2.9354931556419848E-2,3.5598563300600732E-2,6.5728930141590411E-2,7.2676696653989417E-2,0.16812887552682518,8.5932649109180612E-3,2.1244802316981778E-3,0,1.1478486634632357E-3,3.2723288951614134E-3,1.1884482102816457E-2,3.2037924040564728E-2,5.6977197480469637E-2,2.8999155162680126E-3,0.1444382917535435,0.21082638228953735,1.6800000000000002,0.88850040158935439,3.6744603192949907E-3,4.5547033235419955E-3,1.4723292004453306E-2,3.4762012396929581E-2,0,6.0706190383981462E-4,1.7306342485020024E-3,2.4272804062963464E-3,3.2623285537144255E-2,8.1576863339066252E-6,2.6140839373499577E-5,3.0133489787400724E-2,0.12527051845311041,0.88850040158935439,88.850040158935442,140,27.746934669307642,0.27746934669307644,193.13456651801613,null,1.882698677892131E-2,null,0.1444382917535435,5.6977197480469637E-2,6.6323237978712646E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR20, IF(MODE_ILIM=4,#REF!,#REF!))","v":88.850040158935442},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ20, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.1444382917535435},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA20, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.6977197480469637E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB20, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.6323237978712646E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S20, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":193.13456651801613},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P20, IF(MODE_ILIM=4,#REF!,#REF!))","v":48.02054864935436}]
["Icrit_Skip",{"$f":"1000*Iripple/2","v":215.64338235294116},"mA",{"$f":"Iripple/2","v":0.21564338235294117},"CCM-DCM (critical conduction) boundary",null,null,15,0.15,0.43904382096128897,0.43904382096128897,0,43.429135394548858,7.0776791999936606,7,49.543754399955617,2.468766146888617E-6,0.17244157724822867,206929.8926978744,4.8325545766364382E-6,0,6.6E-4,0.20243089273695883,4.9173919601138557E-3,6.6091038182782558E-2,7.1064342339003383E-2,0.10291583462360268,5.2958345081363682E-5,5.2958345081363682E-5,7.6706170744222132E-2,1.7651509890725278E-5,1.7651509890725278E-5,0.10340141850755032,7.3453032510196426E-3,8.3082351918196571E-4,40,17.80717756372006,3.2336073344081416E-2,3.814131782207221E-2,7.1308214685335589E-2,7.8760515185987631E-2,0.17402991979802948,9.2070695474122059E-3,2.2762288196766186E-3,0,1.265931752398769E-3,3.5421605720753879E-3,1.2770977146156876E-2,3.2037924040564728E-2,5.8758574154748555E-2,3.1070523388585843E-3,0.15339711882575166,0.22453207101972711,1.7999999999999998,0.88909433728721643,3.6809989860513443E-3,4.5584936421545893E-3,1.473313408071557E-2,3.5222072154885008E-2,0,6.252959735832379E-4,1.7496193924412637E-3,2.4289029699771751E-3,3.2645093218747326E-2,8.7188097157850768E-6,2.6158313735523759E-5,2.9023286415587744E-2,0.12470177395759456,0.88909433728721643,88.909433728721638,150,29.618044224570543,0.29618044224570544,206.92989269787441,null,1.8839572051264662E-2,null,0.15339711882575166,5.8758574154748555E-2,7.1064342339003383E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR21, IF(MODE_ILIM=4,#REF!,#REF!))","v":88.909433728721638},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ21, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15339711882575166},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA21, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.8758574154748555E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB21, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.1064342339003383E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S21, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":206.92989269787441},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P21, IF(MODE_ILIM=4,#REF!,#REF!))","v":49.543754399955617}]
["Tr",null,"ns",{"$f":"B22/1000000000","v":0},"Switch rise time",null,null,16,0.16,0.43904382096128897,0.43904382096128897,0,42.823074788488256,6.1648780966126591,7,43.154146676288612,2.468766146888617E-6,0.18393768239811059,220725.2188777327,4.5305199155966606E-6,0,6.5999999999999989E-4,0.20906972702083773,5.2452180907881125E-3,7.0497107394968062E-2,7.5805944479575935E-2,0.10629101694886663,5.6488901420121264E-5,5.6488901420121264E-5,8.1815884428420235E-2,2.0081516834413852E-5,2.0081516834413852E-5,0.10679252582772419,7.8349901344209501E-3,8.8621175379409672E-4,40,17.80717756372006,3.5435129926703404E-2,4.0684072343543688E-2,7.700541402404118E-2,8.4963523221796067E-2,0.17973732829855479,9.8208741839063505E-3,2.4279774076550599E-3,0,1.3889156512469415E-3,3.8168930589020014E-3,1.3662583559002257E-2,3.2037924040564721E-2,6.0539950829027467E-2,3.3141891614491565E-3,0.16248024677127493,0.23836276166910542,1.92,0.889563160603839,3.6871045679090202E-3,4.5616476872897792E-3,1.4740902926488492E-2,3.5677697647308992E-2,0,6.4350426902883787E-4,1.7684205485227705E-3,2.4301837410926602E-3,3.26623071185917E-2,9.3040508254897852E-6,2.6172107128292585E-5,2.8049015626182644E-2,0.12425626029036867,0.889563160603839,88.956316060383898,160,31.525976771075946,0.31525976771075948,220.72521887773269,null,1.8849506239665605E-2,null,0.16248024677127493,6.0539950829027467E-2,7.5805944479575935E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR22, IF(MODE_ILIM=4,#REF!,#REF!))","v":88.956316060383898},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ22, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.16248024677127493},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA22, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.0539950829027467E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB22, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.5805944479575935E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S22, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":220.72521887773269},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P22, IF(MODE_ILIM=4,#REF!,#REF!))","v":43.154146676288612}]
["Tf",null,"ns",{"$f":"B23/1000000000","v":0},"Switch fall time",null,null,17,0.17,0.43904382096128897,0.43904382096128897,0,42.217014182427647,5.2717497466757894,9,47.44574772008211,2.468766146888617E-6,0.19543378754799251,234520.54505759102,4.2640187440909743E-6,0,6.6E-4,0.21550414190649117,5.5730442214623702E-3,7.4903176607153579E-2,8.0548044478829212E-2,0.10956227248362353,6.0019457758878853E-5,6.0019457758878853E-5,8.7026304940014745E-2,2.2720733254537305E-5,2.2720733254537305E-5,0.11007921600355225,8.3246770178222636E-3,9.4159998840622795E-4,40,17.80717756372006,3.8652101304285799E-2,4.3226826865015174E-2,8.2820528157707199E-2,9.1285753195469846E-2,0.18526899736031496,1.0434678820400502E-2,2.5797259956335016E-3,0,1.5168169143991693E-3,4.0965429100326706E-3,1.45593196718966E-2,3.2037924040564728E-2,6.2321327503306406E-2,3.5213259840397295E-3,0.17168772635471258,0.25231851102455521,2.04,0.88992868582133411,3.692865976979395E-3,4.5642770459448827E-3,1.4746960025058788E-2,3.6129590089420176E-2,0,6.6169553101118816E-4,1.7870740433019992E-3,2.4311823137402877E-3,3.2675728196984062E-2,9.9116824931899355E-6,2.6182861356405948E-5,2.7187027982185509E-2,0.12391249574847588,0.88992868582133411,88.992868582133411,170,33.460383546927204,0.33460383546927203,234.52054505759102,null,1.8857251580494751E-2,null,0.17168772635471258,6.2321327503306406E-2,8.0548044478829212E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR23, IF(MODE_ILIM=4,#REF!,#REF!))","v":88.992868582133411},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ23, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.17168772635471258},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA23, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.2321327503306406E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB23, IF(MODE_ILIM=4,#REF!,#REF!))","v":8.0548044478829212E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S23, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":234.52054505759102},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P23, IF(MODE_ILIM=4,#REF!,#REF!))","v":47.44574772008211}]
[null,null,null,null,null,null,null,18,0.18,0.43904382096128897,0.43904382096128897,0,41.610953576367045,4.4102622591483298,10,44.102622591483296,2.468766146888617E-6,0.2069298926978744,248315.87123744929,4.0271288138636985E-6,0,6.600000000000001E-4,0.2217519325758821,5.9008703521366279E-3,7.9309245819339083E-2,8.5290642415178503E-2,0.11273864829563676,6.3550014097636415E-5,6.3550014097636415E-5,9.2329394887456603E-2,2.5574151480851696E-5,2.5574151480851696E-5,0.11327057878923497,8.8143639012235736E-3,9.9698822301835886E-4,40,17.80717756372006,4.1986987476828594E-2,4.5769581386486652E-2,8.8753557086333604E-2,9.7727237552833052E-2,0.19064022550839127,1.1048483456894643E-2,2.7314745836119429E-3,0,1.6496520962468674E-3,4.3811266798588107E-3,1.5461203823724689E-2,3.2037924040564734E-2,6.4102704177585332E-2,3.7284628066303017E-3,0.18101960836077338,0.26639937494153038,2.16,0.89020794445763896,3.6983526121769166E-3,4.5664688419781996E-3,1.4751587604787201E-2,3.6578297044967012E-2,0,6.7987657484729579E-4,1.8056082296692743E-3,2.4319452160585981E-3,3.2685981804314555E-2,1.0539959639359847E-5,2.6191077509310595E-5,2.6418859500048308E-2,0.12365370846599605,0.89020794445763896,89.020794445763897,180,35.410314704487,0.35410314704487,248.3158712374493,null,1.886316896516245E-2,null,0.18101960836077338,6.4102704177585332E-2,8.5290642415178503E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR24, IF(MODE_ILIM=4,#REF!,#REF!))","v":89.020794445763897},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ24, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.18101960836077338},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA24, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.4102704177585332E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB24, IF(MODE_ILIM=4,#REF!,#REF!))","v":8.5290642415178503E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S24, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":248.3158712374493},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P24, IF(MODE_ILIM=4,#REF!,#REF!))","v":44.102622591483296}]
["Components","Input Value","Units","Std Units","Description",null,null,19,0.19,0.43904382096128897,0.43904382096128897,0,41.004892970306443,3.6031826701917398,12,43.238192042300881,2.468766146888617E-6,0.21842599784775632,262111.19741730759,3.8151746657656087E-6,0,6.6E-4,0.22782845305936666,6.2286964828108847E-3,8.3715315031524573E-2,9.0033738367055638E-2,0.11582795037156964,6.7080570436393991E-5,6.7080570436393991E-5,9.7716959101258452E-2,2.8645812287991048E-5,2.8645812287991048E-5,0.11637445700212676,9.3040507846248784E-3,1.05237645763049E-3,40,17.80717756372006,4.5439788444331781E-2,4.8312335907958137E-2,9.4804500809920408E-2,0.10428800875148427,0.19586421260884845,1.1662288093388795E-2,2.8832231715903837E-3,0,1.7874377511814519E-3,4.6706609227718356E-3,1.6368254361716891E-2,3.2037924040564728E-2,6.5884080851864243E-2,3.9355996292208739E-3,0.1904759435942863,0.28060540834406633,2.2800000000000002,0.89041442799828618,3.7036194294757831E-3,4.5682920924977046E-3,1.4755009232349353E-2,3.7024252351021199E-2,0,6.9805279070209441E-4,1.8240455587385223E-3,2.4325093052267499E-3,3.2693563310741788E-2,1.1187124808314835E-5,2.6197152524087937E-5,2.5729884283291902E-2,0.12346661263137748,0.89041442799828618,89.041442799828616,190,37.364462120689176,0.37364462120689174,262.11119741730761,null,1.8867544273134036E-2,null,0.1904759435942863,6.5884080851864243E-2,9.0033738367055638E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR25, IF(MODE_ILIM=4,#REF!,#REF!))","v":89.041442799828616},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ25, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.1904759435942863},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA25, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.5884080851864243E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB25, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.0033738367055638E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S25, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":262.11119741730761},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P25, IF(MODE_ILIM=4,#REF!,#REF!))","v":43.238192042300881}]
["L",{"$f":"'Design Converter'!E17","v":68},"µH",{"$f":"B26/1000000","v":6.7999999999999999E-5},"Filter inductance",null,null,20,0.2,0.43904382096128897,0.43904382096128897,0,40.398832364245834,2.8963566549170263,14,40.548993168838372,2.468766146888617E-6,0.22992210299763824,275906.52359716588,3.6244159324773282E-6,0,6.5999999999999989E-4,0.2337470608279589,6.5565226134851424E-3,8.8121384243710077E-2,9.4777332412908991E-2,0.11883696964762404,7.061112677515158E-5,7.061112677515158E-5,0.10318075546578018,3.193880489546738E-5,3.193880489546738E-5,0.11939767361984666,9.7937376680261902E-3,1.1077646922426211E-3,40,17.80717756372006,4.9010504206795383E-2,5.0855090429429615E-2,0.10097335932846763,0.11096809926080189,0.20095244208488258,1.2276092729882939E-2,3.034971759568825E-3,0,1.9301904335943393E-3,4.9651621931631647E-3,1.7280489641453848E-2,3.2037924040564721E-2,6.7665457526143155E-2,4.1427364518114461E-3,0.20005678288021034,0.29493666522478995,2.4000000000000004,0.89055896228262987,3.7087105093434863E-3,4.5698021802168904E-3,1.4757404302142502E-2,3.746780420906301E-2,0,7.1622849564568082E-4,1.8424040376284726E-3,2.4329041561866353E-3,3.2698870211244721E-2,1.1851412060106169E-5,2.6201404911035919E-5,2.5108366515358922E-2,0.12334054743380146,0.89055896228262987,89.055896228262981,200,39.311419610679415,0.39311419610679416,275.90652359716586,null,1.8870606899842556E-2,null,0.20005678288021034,6.7665457526143155E-2,9.4777332412908991E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR26, IF(MODE_ILIM=4,#REF!,#REF!))","v":89.055896228262981},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ26, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.20005678288021034},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA26, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.7665457526143155E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB26, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.4777332412908991E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S26, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":275.90652359716586},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P26, IF(MODE_ILIM=4,#REF!,#REF!))","v":40.548993168838372}]
["Rdcr",{"$f":"'Design Converter'!E18","v":120},"mW",{"$f":"B27/1000","v":0.12},"Inductor DCR at 25°C",null,null,21,0.21,0.43904382096128897,0.43904382096128897,0,39.792771758185225,2.38081556354211,17,40.473864580215867,2.468766146888617E-6,0.24141820814752016,289701.84977702418,3.4518246975974558E-6,0,6.6E-4,0.23951946239918584,6.8843487441593992E-3,9.2527453455895581E-2,9.9521424631203267E-2,0.12177165771550387,7.4141683113909169E-5,7.4141683113909169E-5,0.10871256745453517,3.5455266967670577E-5,3.5455266967670577E-5,0.12234620831526818,1.02834245514275E-2,1.163152926854752E-3,40,17.80717756372006,5.2699134764219377E-2,5.3397844950901094E-2,0.10726013264197523,0.11776754156194931,0.20591497803431394,1.2889897366377086E-2,3.1867203475472667E-3,0,2.0779266978769449E-3,5.264647045424212E-3,1.8197928026871282E-2,3.2037924040564728E-2,6.9446834200422081E-2,4.3498732744020191E-3,0.20976217706364469,0.30939319864492953,2.52,0.89065033492230561,3.7136616165637042E-3,4.5710440626071901E-3,1.4758918433202834E-2,3.7909235341819905E-2,0,7.3440718627305619E-4,1.860698275497937E-3,2.4331537756775885E-3,3.2702225162698988E-2,1.2531049761712523E-5,2.6204093213137562E-5,2.4544780214245936E-2,0.12326685921156197,0.89065033492230561,89.065033492230555,210,41.239947953148963,0.41239947953148964,289.70184977702417,null,1.8872543051448178E-2,null,0.20976217706364469,6.9446834200422081E-2,9.9521424631203267E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR27, IF(MODE_ILIM=4,#REF!,#REF!))","v":89.065033492230555},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ27, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.20976217706364469},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA27, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.9446834200422081E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB27, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.9521424631203267E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S27, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":289.70184977702417},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P27, IF(MODE_ILIM=4,#REF!,#REF!))","v":40.473864580215867}]
["Kcore",0,null,{"$f":"B28","v":0},"Core loss constant - consult inductor vendor",null,null,22,0.22,0.43900073529411765,0.43841744121701987,1.5796744795474049E-3,5.9617287096541691,5.9617287096541691,1,5.9617287096541691,2.46848249606393E-6,0.25238637658523061,302863.65190227673,3.3018158293972636E-6,0,6.5999999999999989E-4,0.25278585690436134,7.66808273410467E-3,9.6731182339495556E-2,0.10452750916772631,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.11421312328471692,3.9133912591349839E-5,3.9133912591349839E-5,0.12699473796895569,1.1079704805129154E-2,1.2159975623876411E-3,40,17.629098274188785,5.7090511003936591E-2,5.5823828318627644E-2,0.11413033688495187,0.12546714789098709,0.21373869316788272,1.3888005602962751E-2,3.3315001709250443E-3,1.9000240279634038E-4,2.2471296573694406E-3,5.7686322310908254E-3,1.9707257632646281E-2,3.2037924040564721E-2,7.1146404547053815E-2,4.5474977333126859E-3,0.22086830780399985,0.32551245433157189,2.64,0.89023399518821367,3.8228843009835006E-3,4.7002417343403905E-3,1.4721225728131991E-2,3.848587340048009E-2,6.4070681112403906E-5,7.5775424719163589E-4,1.945239590096774E-3,2.5857530029605152E-3,3.2618707164154812E-2,1.31963406642211E-5,2.6134925564435249E-5,2.3991268167879016E-2,0.12373234928355981,0.89023399518821367,89.023399518821364,220,43.139231734149426,0.43139231734149425,302.86365190227673,null,1.8824344587421524E-2,null,0.22086830780399985,7.1146404547053815E-2,0.10452750916772631,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR28, IF(MODE_ILIM=4,#REF!,#REF!))","v":89.023399518821364},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ28, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.22086830780399985},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA28, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.1146404547053815E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB28, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10452750916772631},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S28, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":302.86365190227673},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P28, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.9617287096541691}]
["Cin",{"$f":"'Design Converter'!E37","v":2.2000000000000002},"µF",{"$f":"B29/1000000","v":2.2000000000000001E-6},"Input capacitance",null,null,23,0.23,0.43890183823529416,0.44841793024843213,1.1629125427147613E-2,5.9603856653549538,5.9603856653549538,1,5.9603856653549538,2.4670614307725882E-6,0.25249504768229863,302994.05721875833,3.3003947641059217E-6,0,6.6E-4,0.26153525469976752,8.2080827341046714E-3,9.6772832304314341E-2,0.10511896706699654,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.11789089030452661,4.1694786050381785E-5,4.1694786050381785E-5,0.13141855022941049,1.1865063881602861E-2,1.2165211397333147E-3,40,17.233510704120775,6.0023835662229477E-2,5.5847864626561536E-2,0.11708822142852432,0.1292368883681547,0.22118419733988084,1.4872424542477756E-2,3.3329346294063422E-3,6.2639565535019259E-4,2.3505092050744446E-3,6.309839489830979E-3,2.1240689840303709E-2,3.2037924040564728E-2,7.116324365516577E-2,4.5494557691396573E-3,0.22619027763276384,0.33142844293306511,2.7600000000000002,0.89279116465053465,3.9297907630376988E-3,4.8297577078338372E-3,1.4127700572717523E-2,3.7875119411605762E-2,2.0262337198265697E-4,7.6033110533341142E-4,2.0410757053928022E-3,2.6551100520758163E-3,3.1303597702717276E-2,1.3487223404991019E-5,2.5070432224149462E-5,2.3019534486668554E-2,0.12078319853499447,0.89279116465053465,89.279116465053463,230,44.999115697666738,0.44999115697666736,302.99405721875831,null,1.8065391341736691E-2,null,0.22619027763276384,7.116324365516577E-2,0.10511896706699654,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR29, IF(MODE_ILIM=4,#REF!,#REF!))","v":89.279116465053463},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ29, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.22619027763276384},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA29, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.116324365516577E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB29, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10511896706699654},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S29, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":302.99405721875831},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P29, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.9603856653549538}]
["RCinESR",{"$f":"'Design Converter'!E39","v":3},"mW",{"$f":"B30/1000","v":3.0000000000000001E-3},"Input capacitor ESR",null,null,24,0.24,0.43880294117647056,0.45841841927984428,2.1678576374747766E-2,5.9590426210557359,5.9590426210557359,1,5.9590426210557359,2.4656413612565444E-6,0.2526037361547363,303124.48338568356,3.298974694589878E-6,0,6.6E-4,0.27037139170199248,8.7720827341046699E-3,9.6814488928526066E-2,0.10573497421330073,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.12161467499304494,4.4370387520991855E-5,4.4370387520991855E-5,0.13588784813506119,1.2685803495024111E-2,1.2170448007935194E-3,40,16.855287045628756,6.2959668433285029E-2,5.5871904777649195E-2,0.12004861801172774,0.1330465806304621,0.22870625619845536,1.5901191693791304E-2,3.3343693172425194E-3,1.0631645483453753E-3,2.4542195751571221E-3,6.8517534407450172E-3,2.2820057220531594E-2,3.2037924040564728E-2,7.1180085455674669E-2,4.5514141180360386E-3,0.23159813742470439,0.33745498547278047,2.88,0.89511741827113889,4.0398273409952331E-3,4.963023213031886E-3,1.3580166849397444E-2,3.7311669799193016E-2,3.3043649503899784E-4,7.6278287846706064E-4,2.1295568925382199E-3,2.7264041839627105E-3,3.0090394229493757E-2,1.379052316856951E-5,2.4088432504665729E-5,2.2123102196320334E-2,0.11809524303411187,0.89511741827113889,89.511741827113894,240,46.810309970062292,0.46810309970062292,303.12448338568356,null,1.7365248318909812E-2,null,0.23159813742470439,7.1180085455674669E-2,0.10573497421330073,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR30, IF(MODE_ILIM=4,#REF!,#REF!))","v":89.511741827113894},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ30, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.23159813742470439},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA30, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.1180085455674669E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB30, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10573497421330073},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S30, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":303.12448338568356},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P30, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.9590426210557359}]
["Cout",{"$f":"'Design Converter'!E24","v":33},"µF",{"$f":"B31/1000000","v":3.3000000000000003E-5},"Output capacitance",null,null,25,0.25,0.43870404411764707,0.46841890831125654,3.1728027322347946E-2,5.9576995767565206,5.9576995767565206,1,5.9576995767565206,2.4642222864695191E-6,0.25271244200671134,303254.93040805362,3.2975556198028517E-6,0,6.6E-4,0.27928603518771261,9.3600827341046682E-3,9.6856152213728064E-2,0.10637554437122475,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.12538050511453064,4.7160813188324528E-5,4.7160813188324528E-5,0.14039852103685799,1.3541968615314558E-2,1.2175685455883354E-3,40,16.493308594212625,6.5898009918682776E-2,5.5895948772812447E-2,0.12301152723708356,0.13689636472088557,0.23629795130926784,1.6974363425058963E-2,3.3358042344885904E-3,1.5003091718805506E-3,2.5582611018748558E-3,7.3943745082439968E-3,2.4445482288564319E-2,3.2037924040564728E-2,7.1196929949226287E-2,4.5533727800769258E-3,0.23709214973875312,0.34359235837042057,3,0.89723856213803577,4.1526705398289392E-3,5.0996371425584266E-3,1.3073477267439014E-2,3.6790228608201553E-2,4.4871174804687078E-4,7.6512350420662083E-4,2.2115059838956628E-3,2.7994090579470422E-3,2.8967691582156032E-2,1.410483340478427E-5,2.3179693858414748E-5,2.129354368542875E-2,0.11563928364697212,0.89723856213803577,89.723856213803572,250,48.564555994658186,0.48564555994658187,303.25493040805361,null,1.6717333568753181E-2,null,0.23709214973875312,7.1196929949226287E-2,0.10637554437122475,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR31, IF(MODE_ILIM=4,#REF!,#REF!))","v":89.723856213803572},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ31, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.23709214973875312},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA31, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.1196929949226287E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB31, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10637554437122475},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S31, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":303.25493040805361},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P31, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.9576995767565206}]
["RCoutESR",{"$f":"'Design Converter'!E26","v":5.0000000000000001E-3},"mW",{"$f":"B32","v":5.0000000000000001E-3},"Output capacitor ESR",null,null,26,0.26,0.43860514705882347,0.4784193973426687,4.1777478269948154E-2,5.9563565324573036,5.9563565324573036,1,5.9563565324573036,2.4628042053666978E-6,0.25282116524239245,303385.39829087094,3.2961375387000313E-6,0,6.6E-4,0.28827190194479979,9.9720827341046713E-3,9.6897822161518044E-2,0.10704069187727328,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.12918482777643081,5.0066159182878269E-5,5.0066159182878269E-5,0.14494693214903073,1.44336042267786E-2,1.2180923741378468E-3,40,16.146550724637681,6.88388607201946E-2,5.5919996612973331E-2,0.12597694970730577,0.1407863824925403,0.24395316177431658,1.8091996122464506E-2,3.3372393811995811E-3,1.9378296160831902E-3,2.6626341195919298E-3,7.9377031168747017E-3,2.6117090017720813E-2,3.2037924040564728E-2,7.1213777136466594E-2,4.5553317553374282E-3,0.24267258140206513,0.34984084288577566,3.12,0.89917668886656421,4.2680438255830516E-3,5.2392567048483961E-3,1.2603224998316991E-2,3.6306261702347721E-2,5.5847795441578462E-4,7.6736491388391362E-4,2.2876274377683333E-3,2.8739308762678437E-3,2.7925725285120183E-2,1.4428949755873976E-5,2.2336311883949044E-5,2.0523643694631239E-2,0.11339032265482328,0.89917668886656421,89.917668886656415,260,50.254747979561841,0.50254747979561842,303.38539829087097,null,1.6116011985859886E-2,null,0.24267258140206513,7.1213777136466594E-2,0.10704069187727328,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR32, IF(MODE_ILIM=4,#REF!,#REF!))","v":89.917668886656415},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ32, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.24267258140206513},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA32, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.1213777136466594E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB32, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10704069187727328},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S32, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":303.38539829087097},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P32, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.9563565324573036}]
["Controller",null,"Units","Std Units","Description",null,null,27,0.27,0.43850624999999999,0.48841988637408085,5.1826929217548334E-2,5.9550134881580865,5.9550134881580865,1,5.9550134881580865,2.4613871169047287E-6,0.25292990586594993,303515.88703913993,3.2947204502380623E-6,0,6.6E-4,0.29732253438122086,1.0608082734104671E-2,9.6939498773494351E-2,0.10773043164069106,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.13302446088401629,5.3086521580449539E-5,5.3086521580449539E-5,0.14952985675541255,1.5360755328109117E-2,1.2186162864621468E-3,40,15.81407320489042,7.1782221439784938E-2,5.5944048299054271E-2,0.12894488602530135,0.14471677762285318,0.25166646022999306,1.9254146190227181E-2,3.3386747574305395E-3,2.375725971109599E-3,2.7673389627795794E-3,8.4817396913197188E-3,2.783500785702114E-2,3.2037924040564728E-2,7.1230627018041837E-2,4.5572910438926861E-3,0.24833970354180884,0.35620072515133472,3.24,0.90095082216626121,4.385709475904772E-3,5.3815873041644525E-3,1.2165615149173496E-2,3.5855864530441386E-2,6.6062107003485575E-4,7.6951738078055265E-4,2.3585278852761454E-3,2.9498027348454701E-3,2.6956086765544753E-2,1.4761834957979314E-5,2.1551479791523545E-5,1.9807188881272558E-2,0.11132683449218794,0.90095082216626121,90.095082216626125,270,51.875007795911799,0.51875007795911798,303.5158870391399,null,1.555643095998209E-2,null,0.24833970354180884,7.1230627018041837E-2,0.10773043164069106,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR33, IF(MODE_ILIM=4,#REF!,#REF!))","v":90.095082216626125},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ33, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.24833970354180884},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA33, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.1230627018041837E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB33, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10773043164069106},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S33, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":303.5158870391399},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P33, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.9550134881580865}]
["Deadtime1",20,"ns",{"$f":"B34/1000000000","v":2E-8},"PMOS off to NMOS on deadtime",null,null,28,0.28000000000000003,0.4384073529411765,0.49842037540549311,6.1876380165148515E-2,5.9536704438588712,5.9536704438588712,1,5.9536704438588712,2.4599710200417207E-6,0.25303866388155538,303646.39665786648,3.2933043533750534E-6,0,6.6E-4,0.30643219388777065,1.1268082734104672E-2,9.6981182051255832E-2,0.10844477914431729,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.13689655023907249,5.6221996402076695E-5,5.6221996402076695E-5,0.1541444290144979,1.6323466932393237E-2,1.2191402825813338E-3,40,15.49501168267626,7.4728092679610739E-2,5.596810383197795E-2,0.13191533679417003,0.14868769562795389,0.25943302331725088,2.0460870050608888E-2,3.3401103632365319E-3,2.8139983271449182E-3,2.8723759660160306E-3,9.0264846563974811E-3,2.9599365749159754E-2,3.2037924040564728E-2,7.1247479594598373E-2,4.5592506458178653E-3,0.25409379161752987,0.36267229620550362,3.3600000000000003,0.90257743165435944,4.5054620711255785E-3,5.5263744578678275E-3,1.175736210905934E-2,3.5435656511756487E-2,7.5590814964110833E-4,7.7158979825966013E-4,2.4247325410829525E-3,3.0268801112550672E-3,2.605149589721022E-2,1.5102590808055658E-5,2.0819304275952543E-5,1.913879974533898E-2,0.10943018328768124,0.90257743165435944,90.25774316543594,280,53.420714247122767,0.53420714247122769,303.64639665786649,null,1.5034389110485465E-2,null,0.25409379161752987,7.1247479594598373E-2,0.10844477914431729,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR34, IF(MODE_ILIM=4,#REF!,#REF!))","v":90.25774316543594},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ34, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.25409379161752987},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA34, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.1247479594598373E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB34, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10844477914431729},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S34, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":303.64639665786649},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P34, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.9536704438588712}]
["Deadtime2",20,"ns",{"$f":"B35/1000000000","v":2E-8},"NMOS off to PMOS on deadtime",null,null,29,0.28999999999999998,0.43830845588235301,0.50842086443690526,7.1925831112748639E-2,5.952327399559656,5.952327399559656,1,5.952327399559656,2.4585559137372394E-6,0.25314743929338157,303776.92715205788,3.2918892470705725E-6,0,6.6E-4,0.31559576906364295,1.1952082734104669E-2,9.7022871996401736E-2,0.10918375044547347,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.1407985317323823,5.9472679613984002E-5,5.9472679613984002E-5,0.15878809617330775,1.7321784067118075E-2,1.2196643625155125E-3,40,15.188570182135456,7.7676475042021548E-2,5.5992163212667305E-2,0.13488830261720436,0.15269928387728859,0.26724855462117986,2.1712224143921363E-2,3.3415461986726373E-3,3.2526467744031372E-3,2.977745463986541E-3,9.5719384370623155E-3,3.1410296148840118E-2,3.2037924040564728E-2,7.1264334866782825E-2,4.5612105611881493E-3,0.25993512545409964,0.36925585202644146,3.4799999999999995,0.90407084739975219,4.6271232531107653E-3,5.6733972880189292E-3,1.137560688888847E-2,3.5042695991796026E-2,8.4500664529503315E-4,7.7358990372617265E-4,2.4866984178313761E-3,3.1050372314982634E-3,2.5205617845673739E-2,1.5450435590732324E-5,2.0134657251624267E-5,1.8513795290917259E-2,0.1076841538495984,0.90407084739975219,90.407084739975218,290,54.888490199331855,0.54888490199331852,303.77692715205785,null,1.4546230587190049E-2,null,0.25993512545409964,7.1264334866782825E-2,0.10918375044547347,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR35, IF(MODE_ILIM=4,#REF!,#REF!))","v":90.407084739975218},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ35, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.25993512545409964},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA35, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.1264334866782825E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB35, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10918375044547347},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S35, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":303.77692715205785},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P35, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.952327399559656}]
["Sleep delay",5,"µs",{"$f":"B36/1000000","v":5.0000000000000004E-6},"Delay time to enter sleep mode",null,null,30,0.3,0.43820955882352941,0.51842135346831741,8.1975282060348847E-2,5.950984355260438,5.950984355260438,1,5.950984355260438,2.4571417969523053E-6,0.25325623210560283,303907.4785267234,3.2904751302856384E-6,0,6.6E-4,0.32480869669833695,1.2660082734104669E-2,9.7064568610531962E-2,0.10994736217688558,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.14472809808686701,6.2838667127525393E-5,6.2838667127525393E-5,0.16345857914123452,1.8355751774176535E-2,1.2201885262847945E-3,40,14.894014473637304,8.0627369129559784E-2,5.6016226442045659E-2,0.13786378409789024,0.15675169160845892,0.27510921831475393,2.3008264928533504E-2,3.3429822637939576E-3,3.691671403127119E-3,3.08344779148345E-3,1.0118101458404527E-2,3.326793404147551E-2,3.2037924040564728E-2,7.1281192835242008E-2,4.5631707900787525E-3,0.26586398927525517,0.37595169356652264,3.5999999999999996,0.90544359626530446,4.7505374728599335E-3,5.822463240820976E-3,1.1017850054777859E-2,3.4674411241204788E-2,9.2850006429922259E-4,7.7552446033807938E-4,2.5448250477430605E-3,3.184164122162228E-3,2.4412914464627903E-2,1.5804685763462492E-5,1.9493055556929792E-5,1.7928083218561718E-2,0.10607457112871617,0.90544359626530446,90.544359626530451,300,56.276153038808332,0.5627615303880833,303.90747852672342,null,1.4088759310804852E-2,null,0.26586398927525517,7.1281192835242008E-2,0.10994736217688558,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR36, IF(MODE_ILIM=4,#REF!,#REF!))","v":90.544359626530451},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ36, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.26586398927525517},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA36, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.1281192835242008E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB36, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10994736217688558},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S36, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":303.90747852672342},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P36, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.950984355260438}]
["IQ(active)",660,"µA",{"$f":"B37/1000000","v":6.6E-4},"LM5164 quiescent current - active state ",null,null,31,0.31,0.43811066176470592,0.52842184249972968,9.2024733007949028E-2,5.9496413109612218,5.9496413109612218,1,5.9496413109612218,2.4557286686493938E-6,0.25336504232239454,304038.05078687344,3.2890620019827269E-6,0,6.6E-4,0.33406689367680875,1.3392082734104669E-2,9.7106271895246787E-2,0.11073563154763934,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.14868316963611852,6.6320054799128399E-5,6.6320054799128399E-5,0.16815383851083704,1.9425415109872994E-2,1.220712773909297E-3,40,14.610666200384683,8.358077554496042E-2,5.6040293521036511E-2,0.14084178183990623,0.16084506994228764,0.28301158197007659,2.4349048880878434E-2,3.3444185586556079E-3,4.131072303588587E-3,3.189483283406209E-3,1.0664974145650404E-2,3.5172416962260297E-2,3.2037924040564728E-2,7.1298053500622904E-2,4.5651313325649045E-3,0.27188067173773578,0.3827601267874286,3.7199999999999998,0.90670667673492766,4.8755685158821437E-3,5.9734037719138804E-3,1.0681896927505593E-2,3.4328544074593299E-2,1.0069007633705673E-3,7.7739940548356167E-4,2.599463243297474E-3,3.2641642017202281E-3,2.3668522871036969E-2,1.6164740991343012E-5,1.8890562660081372E-5,1.7378070200865289E-2,0.10458898927932042,0.90670667673492766,90.670667673492773,310,57.582635216683897,0.57582635216683897,304.03805078687344,null,1.3659168898308848E-2,null,0.27188067173773578,7.1298053500622904E-2,0.11073563154763934,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR37, IF(MODE_ILIM=4,#REF!,#REF!))","v":90.670667673492773},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ37, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.27188067173773578},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA37, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.1298053500622904E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB37, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.11073563154763934},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S37, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":304.03805078687344},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P37, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.9496413109612218}]
["IQ(sleep)",10,"µA",{"$f":"B38/1000000","v":1.0000000000000001E-5},"LM5164 quiescent current - sleep state",null,null,32,{"$f":"IF(PLOT_TYPE=1, H38/100*Iout, min_I*EXP(H38*rr/100))","v":0.32},{"$f":"IF(I38<Icrit, (Vin-(Rdcr+RdsonTop)*Iripple/2-Vout)/L*OnTime, (Vin-(Rdcr+RdsonTop)*I38-Vout)/L*OnTime)","v":0.43801176470588232},{"$f":"IF(I38<Icrit, (Vin-(Rdcr+RdsonTop)*Iripple/2-Vout)/L*OnTime, I38+((Vin-(Rdcr+RdsonTop)*J38-Vout)/L*OnTime)/2)","v":0.53842233153114183},{"$f":"IF(I38<Icrit, 0, I38-((Vin-(Rdcr+RdsonTop)*K38-Vout)/L*OnTime)/2)","v":0.10207418395554921},5.9482982666620048,{"$f":"IF(I38<Icrit, 1000*SQRT((J38*CoutEsr)^2+(((J38/2)-I38)*(OnTime+OffTime)/Cout)^2), 1000*J38*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":5.9482982666620048},1,{"$f":"IF(I38<Icrit, 1000*((N38/1000)*O38), 1000*J38*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":5.9482982666620048},{"$f":"IF(I38<Icrit, L*J38/(Vout+J38/2*(RdsonBot+Rdcr)), L*J38/(Vout+I38*(RdsonBot+Rdcr)))","v":2.4543165277924267E-6},0.25347386994793375,{"$f":"IF(I38<Icrit,I38/((OnTime+Q38)*J38/2),1/(OnTime+Q38))","v":304168.64393752051},3.2876498611257598E-6,0,{"$f":"S38*(T38*Iq_active+U38*Iq_sleep)","v":6.6E-4},0.34336669822636012,{"$f":"W38^2*Rdcr","v":1.414808273410467E-2},{"$f":"Core_Loss/1000*S38/$S$106","v":9.7147981852147153E-2},{"$f":"(Y38+X38*(1+Ltc*(Ta-25)))/(1-X38*Ltc*ThetaCa)","v":0.11154857634417005},0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.15266186866212728,6.9916938430237787E-5,6.9916938430237787E-5,0.17287204523763267,2.0530819144929137E-2,1.221237105409145E-3,{"$f":"20*VIN_nom/24","v":40},{"$f":"IF(I38<Icrit, Csw*Vin/Iripple*1000000000, Csw*Vin/(I38+Iripple/2)*1000000000)","v":14.337897662925975},{"$f":"IF(I38<Icrit, Vin*(I38+Iripple/2)*AK38/1000000000/2*S38, Vin*(I38-Iripple/2)*AJ38/1000000000/2*S38 + Vin*(I38+Iripple/2)*AK38/1000000000/2*S38)","v":8.6536694891151497E-2},{"$f":"IF(I38<Icrit, Csw*(Vin)^2*S38/2, Csw*Vin^2*S38/2)","v":5.6064364450563779E-2},0.14382229644712441,{"$f":"(AI38+AL38+AM38+AH38*(1+RdsonTopTc*(Ta-25)))/(1-AH38*RdsonTopTc*ThetaJA)","v":0.16497957189811677},{"$f":"IF(I38<Icrit,Iripple*SQRT((OffTime)*S38/3), SQRT(OffTime*S38*(I38^2+Iripple^2/12)))","v":0.29095256721095908},2.5734632495460888E-2,{"$f":"QgBot*S38*Vdd","v":3.3458550833127261E-3},{"$f":"IF(I38<Icrit, Vin*Idss*R38, QrrBot*(I38-Iripple/2)/1*S38*Vin+Vin*Idss*R38)","v":4.5708495660881591E-3},{"$f":"IF(I38<Icrit, dead1*S38*(I38+Iripple/2)*((I38+Iripple/2)*BDserR+VSD), dead1*S38*(I38+Iripple/2)*((I38+Iripple/2)*BDserR+VSD)+dead2*S38*(I38-Iripple/2)*((I38-Iripple/2)*BDserR+VSD))","v":3.2958522747614403E-3},1.1212556924162325E-2,{"$f":"(AR38+AS38+AT38+AQ38*(1+RdsonBotTc*(Ta-25)))/(1-AQ38*RdsonBotTc*ThetaJA)","v":3.7123885015617253E-2},{"$f":"Vin*V38+Vout*Ifb/0.8","v":3.2037924040564728E-2},{"$f":"(Vin-Vdd)*(S38*QgBot+S38*QgTop)+AW38","v":7.1314916863572816E-2},{"$f":"AI38+AR38","v":4.5670921887218715E-3},0.27798546596602869,{"$f":"SUM(Z38,AC38,AF38,AZ38)","v":0.38968146269588333},{"$f":"Vout*I38","v":3.84},0.90786978496307125,5.0020966442960672E-3,6.1260707975252012E-3,{"$f":"Vin*S38*(QgBot+QgTop)/($BB38+$BA38)","v":1.0365812508203622E-2},3.4003103476131752E-2,1.0806604720476575E-3,7.7921997290565583E-4,2.6509223030274599E-3,{"$f":"X38/($BB38+$BA38)","v":3.3449522993362888E-3},{"$f":"Y38/($BB38+$BA38)","v":2.2968155571277394E-2},1.653007183800424E-5,1.8323707810602539E-5,1.6860588082706032E-2,0.10321643590710573,{"$f":"BC38","v":0.90786978496307125},90.786978496307128,{"$f":"I38*1000","v":320},58.807882255999409,0.58807882255999411,{"$f":"S38/1000","v":304.16864393752053},null,{"$f":"AM38/($BB38+$BA38)","v":1.3254985025475155E-2},null,0.27798546596602869,7.1314916863572816E-2,0.11154857634417005,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR38, IF(MODE_ILIM=4,#REF!,#REF!))","v":90.786978496307128},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ38, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.27798546596602869},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA38, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.1314916863572816E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB38, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.11154857634417005},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S38, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":304.16864393752053},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P38, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.9482982666620048}]
["High-side N-ch MOSFET",null,"Units","Std Units","Description",null,null,33,0.33,0.43791286764705883,0.54842282056255409,0.11212363490314942,{"$f":"IF(I39<Icrit, 1000*((((J39/2)-I39)*0.000002/Cout+Vout/306)), 1000*J39*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":5.9469552223627886},5.9469552223627886,1,5.9469552223627886,2.4529053733467767E-6,0.25358271498639856,304299.25798367825,{"$f":"IF(1/S39-OnTime-Q39>Tsleep, OnTime+Q39+Tsleep, 1/S39)","v":3.2862387066801103E-6},{"$f":"IF(1/S39-OnTime-Q39>Tsleep, 1/S39-OnTime-Q39-Tsleep, 0)","v":0},6.6E-4,{"$f":"IF(I39<Icrit,Iripple*SQRT((OnTime+OffTime)*S39/3), SQRT(I39^2+Iripple^2/12))","v":0.35270481914891988},1.4928082734104673E-2,9.7189698482834347E-2,0.11238621493128576,{"$f":"Iripple/SQRT(12)*SQRT((OnTime+Q39)*S39)","v":0.12450176485043199},7.750344725436132E-5,7.750344725436132E-5,{"$f":"SQRT($R39)*SQRT($I39^2*(1-R39)+(Iripple^2)/12)","v":0.15666249686003297},7.3629413767259532E-5,7.3629413767259532E-5,{"$f":"IF(I39<Icrit,Iripple*SQRT((OnTime)*S39/3), SQRT(OnTime*S39*(I39^2+Iripple^2/12)))","v":0.17761155530294762},{"$f":"RdsonTop*AG39^2","v":2.1672008964489703E-2},{"$f":"QgTop*S39*Vdd","v":1.2217615208044684E-3},40,14.075127177172119,8.949512777125386E-2,5.6088439231551573E-2,0.14680532852360989,0.16915535240933813,0.29892940706919063,{"$f":"RdsonBot*AP39^2","v":2.7165072284864315E-2},3.3472918378204615E-3,5.0110032809553432E-3,3.4025551006629635E-3,1.1760850219438769E-2,3.912248089502518E-2,3.2037924040564728E-2,7.1331782924739129E-2,4.5690533586249301E-3,0.28417866958772736,0.39671601738003476,3.96,0.90894150185657385,5.1300162316222529E-3,6.2803337574526301E-3,1.0067884174185131E-2,3.3696327219393356E-2,1.1501790020201437E-3,7.8099079377432824E-4,2.6994759751431544E-3,3.4264530151960331E-3,2.2308017804034099E-2,1.6900209578391914E-5,1.7789419127889125E-5,1.6372832803464517E-2,0.10194720040499193,0.90894150185657385,90.894150185657381,330,59.95273560232264,0.59952735602322638,304.29925798367827,null,1.2874017725231734E-2,null,0.28417866958772736,7.1331782924739129E-2,0.11238621493128576,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR39, IF(MODE_ILIM=4,#REF!,#REF!))","v":90.894150185657381},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ39, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.28417866958772736},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA39, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.1331782924739129E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB39, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.11238621493128576},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S39, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":304.29925798367827},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P39, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.9469552223627886}]
["RdsonTop",687,"mW",{"$f":"B40/1000","v":0.68700000000000006},"Drain-source resistance of high-side MOSFET @ VDD, 25°C",null,null,34,0.34,0.43781397058823524,0.55842330959396624,0.1221730858507496,5.9456121780635716,5.9456121780635716,1,5.9456121780635716,2.451495204279258E-6,0.25369157744196863,304429.89293036237,3.2848285376125915E-6,0,6.6E-4,0.36207829188018475,1.5732082734104674E-2,9.7231421788910352E-2,0.11324856625322534,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.16068351554272173,7.7457576501504291E-5,7.7457576501504291E-5,0.18237088778234711,2.2849029668128237E-2,1.2222860201154049E-3,40,13.821814933668573,9.2456074788581477E-2,5.611251786492439E-2,0.14979087867362126,0.17337256833916151,0.30693960907257584,2.8640424779758204E-2,3.3487288222339867E-3,5.4515335385485648E-3,3.5095920963318528E-3,1.2309854457114404E-2,4.1168349903232586E-2,3.2037924040564728E-2,7.1348651684769504E-2,4.5710148423493916E-3,0.29046058476951303,0.40386411204649425,4.08,0.90992944880700999,5.2592337939468149E-3,6.4360771702661581E-3,9.7865906258532784E-3,3.3406649918579875E-2,1.2158114970304962E-3,7.827159808217357E-4,2.745367421827604E-3,3.508599355595624E-3,2.1684738734094388E-2,1.7274737718612893E-5,1.7284967902157883E-5,1.5912313554079818E-2,0.10077265775771656,0.90992944880700999,90.992944880701003,340,61.018807215515402,0.61018807215515403,304.42989293036237,null,1.2514321679412783E-2,null,0.29046058476951303,7.1348651684769504E-2,0.11324856625322534,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR40, IF(MODE_ILIM=4,#REF!,#REF!))","v":90.992944880701003},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ40, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.29046058476951303},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA40, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.1348651684769504E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB40, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.11324856625322534},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S40, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":304.42989293036237},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P40, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.9456121780635716}]
["RdsonTopTc",4500,"ppm/°C",{"$f":"B41/1000000","v":4.4999999999999997E-3},"Drain to Source Resistance Temp Co",null,null,35,0.35,0.43771507352941186,0.5684237986253784,0.13222253679834972,5.9442691337643572,5.9442691337643572,1,5.9442691337643572,2.4500860195581315E-6,0.25380045731882472,304560.54878258967,3.283419352891465E-6,0,6.600000000000001E-4,0.37148444038865508,1.656008273410467E-2,9.7273151771977442E-2,0.11413564983475,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.16472352824164804,8.1401522269131061E-5,8.1401522269131061E-5,0.18714870582759713,2.4061926369852864E-2,1.2228106033620977E-3,40,13.577459296090474,9.5419536546641301E-2,5.6136600351606926E-2,0.15277894750161033,0.17763137849662247,0.31498092323659499,3.0160746528905234E-2,3.350166036608487E-3,5.8924404292551563E-3,3.6169635970964677E-3,1.285957006296011E-2,4.3261639972862018E-2,3.2037924040564734E-2,7.1365523144311771E-2,4.5729766399705846E-3,0.29683151825376686,0.41112607305804033,4.1999999999999993,0.91084041803580829,5.389666342072128E-3,6.5931985871164108E-3,9.5205758958143861E-3,3.3132676287961328E-2,1.2778745009128249E-3,7.8439919876182088E-4,2.7888133742636555E-3,3.5913315905332071E-3,2.1095313862773468E-2,1.7653284898182501E-5,1.680792197532826E-5,1.5476810222406927E-2,9.9685121069489652E-2,0.91084041803580829,91.084041803580831,350,62.00835196729512,0.62008351967295117,304.56054878258965,null,1.2174162983658752E-2,null,0.29683151825376686,7.1365523144311771E-2,0.11413564983475,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR41, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.084041803580831},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ41, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.29683151825376686},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA41, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.1365523144311771E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB41, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.11413564983475},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S41, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":304.56054878258965},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P41, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.9442691337643572}]
["QgTop",0.80300000000000005,"nC",{"$f":"B42/1000000000","v":8.0300000000000002E-10},"Gate charge of high-side MOSFET @ VDD",null,null,36,0.36,0.43761617647058826,0.57842428765679066,0.14227198774594993,5.9429260894651392,5.9429260894651392,1,5.9429260894651392,2.4486778181530929E-6,0.25390935462114927,304691.2255453791,3.282011151486426E-6,0,6.6E-4,0.38092084407508114,1.7412082734104675E-2,9.7314888433638641E-2,0.11504748578226998,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.16878126540100274,8.5461346651091188E-5,8.5461346651091188E-5,0.1919438001435701,2.5310744198112137E-2,1.223335270564697E-3,40,13.341593485550055,9.8385513649133602E-2,5.6160686692524275E-2,0.15576953561222256,0.18193194365283386,0.32305131425518463,3.1726094099168621E-2,3.3516034809991705E-3,6.3337240434914004E-3,3.7246699383925073E-3,1.3409997462883079E-2,4.5402501687411063E-2,3.2037924040564728E-2,7.1382397304013995E-2,4.5749387515638673E-3,0.3032917813958228,0.41850223197199821,4.32,0.91168048225275766,5.5212399952217417E-3,6.7516068703451521E-3,9.2686274828946147E-3,3.2873158645194252E-2,1.3366510625986404E-3,7.8604372353380323E-4,2.8300076282336811E-3,3.6745962926049689E-3,2.0537056578137265E-2,1.8035518918712246E-5,1.6356106520626687E-5,1.5064337592241071E-2,9.8677717496444523E-2,0.91168048225275766,91.168048225275768,360,62.924142868481049,0.62924142868481048,304.6912255453791,null,1.1851991186918185E-2,null,0.3032917813958228,7.1382397304013995E-2,0.11504748578226998,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR42, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.168048225275768},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ42, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.3032917813958228},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA42, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.1382397304013995E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB42, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.11504748578226998},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S42, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":304.6912255453791},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P42, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.9429260894651392}]
["Coss",100,"pF",{"$f":"B43/1000000000000","v":1E-10},"Capacitance (Coss)",null,null,37,0.37,0.43751727941176477,0.58842477668820281,0.15232143869355014,5.9415830451659239,5.9415830451659239,1,5.9415830451659239,2.4472705990352794E-6,0.2540182693531256,304821.92322375072,3.2806039323686129E-6,0,6.6E-4,0.39038530895881862,1.828808273410467E-2,9.735663177549729E-2,0.1159840947850049,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.17285557089959153,8.9637145173071138E-5,8.9637145173071138E-5,0.19675507460427474,2.6595528295800669E-2,1.2238600217433593E-3,40,13.113782604601525,0.10135400669995176,5.6184776888601733E-2,0.15876264361029685,0.18627442655748272,0.3311489372917738,3.3336524075519229E-2,3.3530411554612586E-3,6.7753844717025041E-3,3.8327114557630436E-3,1.3961137082926806E-2,4.7591088302654586E-2,3.2037924040564728E-2,7.1399274164524434E-2,4.5769011772046177E-3,0.3098416902018663,0.42599292557929863,4.4399999999999995,0.91245508735946557,5.6538888091191754E-3,6.9112207383088473E-3,9.0296578669878513E-3,3.2626977892984937E-2,1.3923950518065936E-3,7.8765249238556137E-4,2.8691239992431204E-3,3.7583455245010387E-3,2.0007557196336647E-2,1.8421141695844083E-5,1.5927570886292339E-5,1.4673115077746301E-2,9.7744283362002207E-2,0.91245508735946557,91.245508735946558,370,63.769353027551922,0.63769353027551923,304.82192322375073,null,1.1546415654090356E-2,null,0.3098416902018663,7.1399274164524434E-2,0.1159840947850049,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR43, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.245508735946558},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ43, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.3098416902018663},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA43, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.1399274164524434E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB43, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.1159840947850049},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S43, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":304.82192322375073},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P43, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.9415830451659239}]
["Low-side N-ch MOSFET",null,"Units","Std Units","Description",null,null,38,0.38,0.43741838235294117,0.59842526571961507,0.16237088964115032,5.9402400008667069,5.9402400008667069,1,5.9402400008667069,2.4458643611772598E-6,0.25412720151893886,304952.64182272664,3.2791976945105933E-6,0,6.5999999999999989E-4,0.39987584254474823,1.9188082734104672E-2,9.7398381799157371E-2,0.11694549811617955,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.1769453901683011,9.3929013305436913E-5,9.3929013305436913E-5,0.20158153370559287,2.7916323820265068E-2,1.2243848569182475E-3,40,12.893620961022126,0.1043250163031826,5.6208870940764974E-2,0.16175827210086582,0.19065899195557823,0.33927211686159309,3.499209306104293E-2,3.3544790600499932E-3,7.217421804362645E-3,3.9410884848585697E-3,1.4512989349271206E-2,4.9827555768454719E-2,3.2037924040564721E-2,7.1416153726491599E-2,4.5788639169682408E-3,0.31648156536749283,0.43359849594423217,4.5600000000000005,0.91316913117936938,5.78755378074256E-3,7.0719675296013022E-3,8.8026888102030569E-3,3.2393127367417465E-2,1.4453348242203666E-3,7.8922814640774487E-4,2.9063188322125937E-3,3.8425361489693461E-3,1.9504648176713383E-2,1.8809884972074831E-5,1.5520560436989297E-5,1.43015410198668E-2,9.6879275081763694E-2,0.91316913117936938,91.316913117936934,380,64.547447140017496,0.645474471400175,304.95264182272666,null,1.1256185491568343E-2,null,0.31648156536749283,7.1416153726491599E-2,0.11694549811617955,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR44, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.316913117936934},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ44, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.31648156536749283},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA44, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.1416153726491599E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB44, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.11694549811617955},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S44, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":304.95264182272666},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P44, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.9402400008667069}]
["RdsonBot",304,"mW",{"$f":"B45/1000","v":0.30399999999999999},"Drain-source resistance of low-side MOSFET @ VDD, 25°C",null,null,39,0.39,0.43731948529411768,0.60842575475102723,0.1724203405887505,5.9388969565674898,5.9388969565674898,1,5.9388969565674898,2.4444591035530393E-6,0.25423615112277514,305083.38134733017,3.2777924368863728E-6,0,6.6E-4,0.4093906318552884,2.0112082734104673E-2,9.7440138506223309E-2,0.11793171763425361,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.18104975970082277,9.8337046463177006E-5,9.8337046463177006E-5,0.20642227159759982,2.9273175943309613E-2,1.2249097761095307E-3,40,12.6807296567214,0.10729854306310627,5.6232968849939897E-2,0.16475642168915569,0.19508580660445157,0.34741932837250417,3.6692857676947771E-2,3.3559171948206322E-3,7.659836131974955E-3,4.0498013614370413E-3,1.5065554688232629E-2,5.2112062750983505E-2,3.2037924040564728E-2,7.1433035990564137E-2,4.5808269709301632E-3,0.3232117323169294,0.44131929044490054,4.68,0.91382703061137172,5.9221819994474713E-3,7.2337821490392898E-3,8.5868379663376314E-3,3.2170699061187212E-2,1.4956763477462325E-3,7.9077306681365426E-4,2.9417331421497548E-3,3.9271292402386993E-3,1.9026374451603167E-2,1.9201506659943917E-5,1.5133492535597879E-5,1.3948170762139417E-2,9.6077693185898067E-2,0.91382703061137172,91.382703061137178,390,65.262084299350803,0.65262084299350809,305.08338134733015,null,1.0980172424487679E-2,null,0.3232117323169294,7.1433035990564137E-2,0.11793171763425361,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR45, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.382703061137178},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ45, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.3232117323169294},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA45, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.1433035990564137E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB45, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.11793171763425361},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S45, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":305.08338134733015},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P45, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.9388969565674898}]
["RdsonBotTc",4500,"ppm/°C",{"$f":"B46/1000000","v":4.4999999999999997E-3},"Drain To Source Resitance Temp Co",null,null,40,0.4,0.43722058823529408,0.61842624378243949,0.18246979153635071,5.9375539122682728,5.9375539122682728,1,5.9375539122682728,2.4430548251380485E-6,0.25434511816882222,305214.14180258667,3.2763881584713812E-6,0,6.6E-4,0.41892802418896768,2.1060082734104674E-2,9.7481901898300125E-2,0.11894277578418705,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.18516779778158493,1.0286134000584579E-4,1.0286134000584579E-4,0.21127646247770215,3.0666129851202126E-2,1.2254347793373855E-3,40,12.474754411632974,0.11027458758419648,5.6257070617052776E-2,0.16775709298058664,0.19955503929101298,0.35558918195615546,3.8438874562571342E-2,3.3573555598284538E-3,8.1026275450715533E-3,4.1588504213639224E-3,1.561883352626393E-2,5.4444770655364537E-2,3.2037924040564728E-2,7.1449920957390944E-2,4.5827903391658393E-3,0.33003252124293431,0.4491556618143816,4.8000000000000007,0.91443277914545029,6.0577259199502036E-3,7.3966061649770815E-3,8.3813074121686787E-3,3.1958871824083232E-2,1.5436058800875534E-3,7.922894060120913E-4,2.9754944475899286E-3,4.0120895799125936E-3,1.8570968014426398E-2,1.959578771003555E-5,1.4764935972116339E-5,1.3611697873081197E-2,9.5335017245971113E-2,0.91443277914545029,91.443277914545035,400,65.91703305041338,0.65917033050413376,305.21414180258665,null,1.0717356131444462E-2,null,0.33003252124293431,7.1449920957390944E-2,0.11894277578418705,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR46, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.443277914545035},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ46, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.33003252124293431},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA46, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.1449920957390944E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB46, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.11894277578418705},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S46, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":305.21414180258665},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P46, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.9375539122682728}]
["QgBot",2.2000000000000002,"nC",{"$f":"B47/1000000000","v":2.2000000000000003E-9},"Gate charge of low-side MOSFET at VDD",null,null,41,0.41,0.43712169117647059,0.62842673281385164,0.19251924248395083,5.9362108679690575,5.9362108679690575,1,5.9362108679690575,2.4416515249091494E-6,0.25445410266126872,305344.9231935225,3.2749848582424826E-6,0,6.6E-4,0.42848651023208684,2.2032082734104671E-2,9.7523671976993201E-2,0.11997869559873969,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.18929869627787296,1.0750198923750718E-4,1.0750198923750718E-4,0.21614335215826547,3.2095230744679619E-2,1.2259598666219929E-3,40,12.275363596297929,0.11325315047112029,5.6281176243030064E-2,0.17076028658077236,0.20406686084926812,0.36378040827586444,4.0230200375387798E-2,3.358794155128748E-3,8.5457961342135357E-3,4.2682360006122185E-3,1.6172826289954503E-2,5.6825843648738987E-2,3.2037924040564728E-2,7.1466808627621101E-2,4.5847540217507409E-3,0.33694426714737896,0.45710796818261051,4.92,0.91498999631634581,6.1941427372441118E-3,7.5603870332037722E-3,8.1853737862889013E-3,3.1756901217381922E-2,1.589292271009001E-3,7.937791143246887E-4,3.0077183470468231E-3,4.0973852235202963E-3,1.8136826069712505E-2,1.9992529417972871E-5,1.4413593275969952E-5,1.3290938000595125E-2,9.4647149923021104E-2,0.91498999631634581,91.498999631634575,410,66.516098897051677,0.66516098897051679,305.3449231935225,null,1.0466811634814976E-2,null,0.33694426714737896,7.1466808627621101E-2,0.11997869559873969,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR47, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.498999631634575},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ47, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.33694426714737896},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA47, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.1466808627621101E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB47, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.11997869559873969},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S47, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":305.3449231935225},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P47, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.9362108679690575}]
["VSD",0.8,"V",{"$f":"B48","v":0.8},"Body diode forward voltage",null,null,42,0.42,0.43702279411764711,0.63842722184526379,0.20256869343155101,5.9348678236698413,5.9348678236698413,1,5.9348678236698413,2.4402492018446261E-6,0.25456310460430515,305475.7255251662,3.2735825351779592E-6,0,6.6E-4,0.43806470920501261,2.3028082734104671E-2,9.7565448743908559E-2,0.12103950069980682,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.19344171336320573,1.1225908940667795E-4,1.1225908940667795E-4,0.22102225064983994,3.3560523838954304E-2,1.2264850379835423E-3,40,12.082246450157612,0.11623423232873875,5.6305285728798636E-2,0.17376600309552093,0.20862144417809911,0.37199184604380409,4.2066891791015477E-2,3.3602329807768281E-3,8.9893419899910176E-3,4.3779584352625373E-3,1.6727533406030386E-2,5.9255448683762937E-2,3.2037924040564728E-2,7.1483699001903905E-2,4.58671801876037E-3,0.34394730988252636,0.46517657311899424,5.04,0.91550197038358649,6.3313938471605824E-3,7.7250774271965042E-3,7.9983797786076574E-3,3.1564110757863056E-2,1.6328889492636285E-3,7.9524396304370951E-4,3.0385098795393025E-3,4.1829871264343404E-3,1.7722492175874426E-2,2.0391551100254141E-5,1.4078285450969873E-5,1.2984814937807588E-2,9.401036867934201E-2,0.91550197038358649,91.550197038358647,420,67.063063929713536,0.6706306392971354,305.47572552516618,null,1.02276984181996E-2,null,0.34394730988252636,7.1483699001903905E-2,0.12103950069980682,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR48, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.550197038358647},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ48, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.34394730988252636},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA48, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.1483699001903905E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB48, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.12103950069980682},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S48, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":305.47572552516618},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P48, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.9348678236698413}]
["BDserR",100,"mW",{"$f":"B49*0.001","v":0.1},"Series resistance of body diode",null,null,43,0.43,0.43692389705882362,0.64842771087667606,0.21261814437915119,5.9335247793706252,5.9335247793706252,1,5.9335247793706252,2.4388478549241854E-6,0.25467212400212308,305606.54880254768,3.2721811882575193E-6,0,6.6E-4,0.44766135577115906,2.4048082734104668E-2,9.7607232200652733E-2,0.12212521529978934,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.19759616705650851,1.1713273570627085E-4,1.1713273570627085E-4,0.2259125256242856,3.5062054363719189E-2,1.227010293442229E-3,40,11.895111465421518,0.11921783376210632,5.6329399075285586E-2,0.17677424313083412,0.21321896425931111,0.38022243101910541,4.3949005503223823E-2,3.361672036828025E-3,9.4332652030231119E-3,4.4880180615031141E-3,1.728295530135425E-2,6.173375552254106E-2,3.2037924040564728E-2,7.1500592080888908E-2,4.588682330270254E-3,0.35104199419301135,0.47336184567576134,5.16,0.91597169529610112,6.4694443791947099E-3,7.8906346581141054E-3,7.8197267595030845E-3,3.1379884334347921E-2,1.6745356434478293E-3,7.966855644020404E-4,3.0679647029279436E-3,4.2688688198796029E-3,1.7326639913176758E-2,2.0792688081306796E-5,1.3757938754432032E-5,1.2692348554846277E-2,9.342128395667601E-2,0.91597169529610112,91.597169529610113,430,67.561637846160409,0.67561637846160405,305.60654880254771,null,9.9992510011627841E-3,null,0.35104199419301135,7.1500592080888908E-2,0.12212521529978934,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR49, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.597169529610113},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ49, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.35104199419301135},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA49, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.1500592080888908E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB49, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.12212521529978934},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S49, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":305.60654880254771},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P49, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.9335247793706252}]
["QrrBot",3,"nC",{"$f":"B50*0.000000001","v":3.0000000000000004E-9},"Reverse recovery charge of body diode at 100mA",null,null,44,0.44,0.43682500000000002,0.65842819990808821,0.2226675953267514,5.9321817350714081,5.9321817350714081,1,5.9321817350714081,2.4374474831289554E-6,0.2547811608589155,305737.39303069859,3.2707808164622889E-6,0,6.600000000000001E-4,0.45727528847606913,2.5092082734104668E-2,9.7649022348832729E-2,0.12323586420299988,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.2017614294767775,1.2212302327353799E-4,1.2212302327353799E-4,0.23081359664173343,3.6599867563153969E-2,1.2275356330182549E-3,40,11.713684918832534,0.12220395537647148,5.6353516283418364E-2,0.17978500729290808,0.21785959817595135,0.38847118629153538,4.5876598223940843E-2,3.363111323337685E-3,9.877565863957969E-3,4.5984152156298671E-3,1.783909240292552E-2,6.4260936761004042E-2,3.2037924040564734E-2,7.1517487865225812E-2,4.5906469563559401E-3,0.35822866975853712,0.48166416043206489,5.28,0.91640190281483791,6.6082627905525246E-3,8.0570201708176897E-3,7.6488683744649578E-3,3.1203659617575846E-2,1.7143598774450701E-3,7.981053889272563E-4,3.0961701179035351E-3,4.3550061293789501E-3,1.6948058690999798E-2,2.1195789944199042E-5,1.3451573208069344E-5,1.2412644311407199E-2,9.2876802832625116E-2,0.91640190281483791,91.640190281483797,440,68.015419380100283,0.68015419380100284,305.73739303069857,null,9.7807707485665796E-3,null,0.35822866975853712,7.1517487865225812E-2,0.12323586420299988,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR50, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.640190281483797},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ50, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.35822866975853712},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA50, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.1517487865225812E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB50, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.12323586420299988},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S50, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":305.73739303069857},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P50, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.9321817350714081}]
["TrrBot",20,"ns",{"$f":"B51*0.000000001","v":2E-8},"Reverse recovery time of body diode (not used)",null,null,45,0.45,0.43672610294117653,0.66842868893950047,0.23271704627435158,5.9308386907721919,5.9308386907721919,1,5.9308386907721919,2.4360480854414807E-6,0.25489021517887667,305868.25821465201,3.2693814187748134E-6,0,6.6E-4,0.46690543951733127,2.6160082734104674E-2,9.7690819190056108E-2,0.12437147280710419,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.20593692172605826,1.2723004719001395E-4,1.2723004719001395E-4,0.23572493004193745,3.8174008695930829E-2,1.2280610567318279E-3,40,11.53770953577642,0.1251925977772764,5.6377637354124661E-2,0.18279829618813287,0.22254352513090098,0.39673721368337894,4.7849726683260325E-2,3.3645508403611726E-3,1.0322244063472763E-2,4.709150234046432E-3,1.8395945137880367E-2,6.6837167853735599E-2,3.2037924040564728E-2,7.1534386355564528E-2,4.5926118970930005E-3,0.3655076912372941,0.49008389753884263,5.4,0.91679509051753527,6.7478205122639343E-3,8.2241991045486247E-3,7.4853049598351765E-3,3.1034922314861199E-2,1.752478274169556E-3,7.9950478057097605E-4,3.1232059607108598E-3,4.4413769292888337E-3,1.6585641374459194E-2,2.1600719005577614E-5,1.3158292581663556E-5,1.2144884113697428E-2,9.2374097335993027E-2,0.91679509051753527,91.679509051753527,450,68.427867006324419,0.68427867006324417,305.86825821465203,null,9.5716187298591649E-3,null,0.3655076912372941,7.1534386355564528E-2,0.12437147280710419,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR51, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.679509051753527},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ51, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.3655076912372941},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA51, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.1534386355564528E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB51, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.12437147280710419},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S51, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":305.86825821465203},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P51, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.9308386907721919}]
["Idss",0,"μA",{"$f":"B52/1000000","v":0},"Leakage current of low-side device",null,null,46,0.46,0.43662720588235293,0.67842917797091262,0.24276649722195176,5.9294956464729749,5.9294956464729749,1,5.9294956464729749,2.434649660845721E-6,0.25499928696620222,305999.14435944264,3.2679829941790541E-6,0,6.5999999999999989E-4,0.47655082567431595,2.7252082734104673E-2,9.7732622725930862E-2,0.12553206710459838,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.2101221093249187,1.3245390248145926E-4,1.3245390248145926E-4,0.24064603441466753,3.9784523035220176E-2,1.2285865646031622E-3,40,11.366943273024079,0.12818376157015726,5.640176228833247E-2,0.1858141104230929,0.2272709264657469,0.40501968612587652,4.9868447629449073E-2,3.3659905879538693E-3,1.0767299892273719E-2,4.8202234532642094E-3,1.8953513933491796E-2,6.9462627139255814E-2,3.2037924040564721E-2,7.1551287552555187E-2,4.594577152557032E-3,0.3728794183101149,0.49862144276444909,5.5200000000000005,0.91715354628859591,6.8880916397380558E-3,8.3921399087968501E-3,7.3285786594160709E-3,3.0873201145833404E-2,1.7889976956796481E-3,8.0088496993926288E-4,3.1491453838283175E-3,4.527960928140274E-3,1.6238373463980597E-2,2.200734898199895E-5,1.287727563386388E-5,1.1888318318902365E-2,9.1910576738870708E-2,0.91715354628859591,91.715354628859586,460,68.802277733330541,0.68802277733330541,305.99914435944265,null,9.3712094745779916E-3,null,0.3728794183101149,7.1551287552555187E-2,0.12553206710459838,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR52, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.715354628859586},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ52, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.3728794183101149},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA52, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.1551287552555187E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB52, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.12553206710459838},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S52, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":305.99914435944265},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P52, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.9294956464729749}]
["Csw",160,"pF",{"$f":"B53/1000000000000","v":1.5999999999999999E-10},"Effective SW node capacitance (CossHS + CossLS)",null,null,47,0.47,0.43652830882352944,0.68842966700232477,0.25281594816955189,5.9281526021737587,5.9281526021737587,1,5.9281526021737587,2.4332522083270491E-6,0.25510837622508908,306130.05147010693,3.2665855416603822E-6,0,6.6E-4,0.48621054025069455,2.8368082734104669E-2,9.7774432958065594E-2,0.1267176736843223,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.21431649813442041,1.377946841178031E-4,1.377946841178031E-4,0.24557645657575478,4.1431455868696558E-2,1.2291121566524793E-3,40,11.201158207994855,0.13117744736094428,5.6425891086970111E-2,0.18883245060456685,0.23204198567993478,0.41331784088670109,5.1932817828954286E-2,3.3674305661711766E-3,1.1212733441096127E-2,4.9316352099024064E-3,1.9511799217169709E-2,7.213749586576769E-2,3.2037924040564728E-2,7.1568191456848174E-2,4.5965427228236554E-3,0.3803442157253743,0.50727718754106876,5.64,0.91747936979819489,7.0290526613868021E-3,8.5608140064444421E-3,7.1782691414242171E-3,3.0718063435838081E-2,1.824016243129791E-3,8.0224708589642709E-4,3.1740555406733649E-3,4.614739480366916E-3,1.590532360509608E-2,2.2415563820202719E-5,1.2607768429808345E-5,1.1642258722593196E-2,9.1483863255099315E-2,0.91747936979819489,91.747936979819485,470,69.1417728033842,0.69141772803384205,306.13005147010693,null,9.1790054955274685E-3,null,0.3803442157253743,7.1568191456848174E-2,0.1267176736843223,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR53, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.747936979819485},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ53, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.3803442157253743},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA53, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.1568191456848174E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB53, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.1267176736843223},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S53, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":306.13005147010693},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P53, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.9281526021737587}]
["ThetaJA",41.1,"°C/W",null,"Thermal resistance",null,null,48,0.48,0.4364294117647059,0.69843015603373704,0.26286539911715212,5.9268095578745417,5.9268095578745417,1,5.9268095578745417,2.4318557268722471E-6,0.25521748295973579,306260.97955168295,3.2651890602055802E-6,0,6.6E-4,0.49588374590308187,2.9508082734104671E-2,9.781624988806939E-2,0.12792831973300872,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.2185196307070883,1.4325248701308675E-4,1.4325248701308675E-4,0.25051577798556973,4.3114852498544395E-2,1.229637832900007E-3,40,11.040139523822107,0.13417365575566181,5.6450023750966201E-2,0.19185331733952801,0.236856888450209,0.42163097354207202,5.4042894066410767E-2,3.3688707750685128E-3,1.1658544800704346E-2,5.0433858406880878E-3,2.0070801416460948E-2,7.4861958217373778E-2,3.2037924040564728E-2,7.1585098069093994E-2,4.5985086079685196E-3,0.38790245334464524,0.51605152901192142,5.76,0.91777449139376865,7.1706822199667604E-3,8.7301954975406246E-3,7.0339898314136255E-3,3.0569111240189691E-2,1.8576241362600516E-3,8.0359216577084096E-4,3.197998187822531E-3,4.7016954207114861E-3,1.5585635241504976E-2,2.2825256668286135E-5,1.2349077584224867E-5,1.1406072390926352E-2,9.1091770666359442E-2,0.91777449139376865,91.77744913937687,480,69.449289175978407,0.69449289175978413,306.26097955168296,null,8.9945124717377024E-3,null,0.38790245334464524,7.1585098069093994E-2,0.12792831973300872,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR54, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.77744913937687},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ54, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.38790245334464524},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA54, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.1585098069093994E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB54, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.12792831973300872},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S54, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":306.26097955168296},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P54, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.9268095578745417}]
["Inductor",null,"Units","Std Units","Description",null,null,49,0.49,0.43633051470588236,0.70843064506514919,0.27291485006475225,5.9254665135753255,5.9254665135753255,1,5.9254665135753255,2.4304602154695045E-6,0.25532660717434186,306391.92860921024,3.2637935488028376E-6,0,6.6E-4,0.50556966824649618,3.0672082734104666E-2,9.7858073517551811E-2,0.12916403303686888,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.22273108301672248,1.4882740602540636E-4,1.4882740602540636E-4,0.25546361155537162,4.4834758241463782E-2,1.2301635933659792E-3,40,10.88368458071743,0.13717238736052839,5.647416028124963E-2,0.194876711235144,0.24171582265034214,0.4299584326016761,5.6198733144648176E-2,3.3703112147013131E-3,1.2104734061891815E-2,5.155475682456204E-3,2.0630520959049332E-2,7.7636201340769539E-2,3.2037924040564728E-2,7.1602007389943448E-2,4.6004748080672921E-3,0.39555450618912241,0.52494487007927104,5.88,0.91804068876040545,7.312960902131611E-3,8.9002608981105357E-3,6.8953845900783534E-3,3.0425977926135075E-2,1.8899044890205276E-3,8.0492116435537675E-4,3.2210302161108217E-3,4.7888129181859846E-3,1.5278519253880895E-2,2.3236328968365406E-5,1.2100564302499937E-5,1.1179176221240022E-2,9.0732285472520074E-2,0.91804068876040545,91.804068876040546,490,69.727575757335345,0.69727575757335347,306.39192860921025,null,8.8172750002999904E-3,null,0.39555450618912241,7.1602007389943448E-2,0.12916403303686888,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR55, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.804068876040546},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ55, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.39555450618912241},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA55, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.1602007389943448E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB55, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.12916403303686888},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S55, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":306.39192860921025},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P55, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.9254665135753255}]
["Ltc",4000,"ppm",{"$f":"Ltc","v":4.0000000000000001E-3},"Inductor DCR Temp Co",null,null,50,0.5,0.43623161764705881,0.71843113409656145,0.28296430101235248,5.9241234692761084,5.9241234692761084,1,5.9241234692761084,2.4290656731084177E-6,0.25543574887310838,306522.89864773006,3.2623990064417509E-6,0,6.6E-4,0.51526759014212431,3.1860082734104664E-2,9.7899903848123013E-2,0.13042484198321452,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.2269504615232556,1.5451953595685614E-4,1.5451953595685614E-4,0.26041959879434984,4.6591218428676369E-2,1.2306894380706361E-3,40,10.731602065192263,0.14017364278195671,5.6498300678749606E-2,0.19790263289877696,0.24661897837115918,0.4382996147069918,5.8400391884698429E-2,3.3717518851250315E-3,1.2551301315481069E-2,5.2679050721496472E-3,2.1190958272755748E-2,8.0460415372421407E-2,3.2037924040564728E-2,7.1618919420047472E-2,4.6024413231956678E-3,0.40330075448682368,0.53395761945324938,6,0.91827960165160505,7.4558710523835187E-3,9.0709889092646465E-3,6.7621247758224076E-3,3.0288325150682124E-2,1.9209339953648705E-3,8.0623496186534136E-4,3.2432041202203224E-3,4.8760773469434691E-3,1.4983247451230806E-2,2.3648689654308787E-5,1.1861639111893517E-5,1.09610321326266E-2,9.0403550225170298E-2,0.91827960165160505,91.827960165160505,500,69.979193442852676,0.69979193442852672,306.52289864773007,null,8.6468728402124672E-3,null,0.40330075448682368,7.1618919420047472E-2,0.13042484198321452,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR56, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.827960165160505},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ56, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.40330075448682368},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA56, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.1618919420047472E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB56, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.13042484198321452},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S56, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":306.52289864773007},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P56, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.9241234692761084}]
["ThetaCA",20,"°C/W",{"$f":"ThetaCa","v":40},"Inductor Core-to-Ambient thermal resistance",null,null,51,0.51,0.43613272058823532,0.7284316231279736,0.29301375195995272,5.9227804249768932,5.9227804249768932,1,5.9227804249768932,2.4276720987799851E-6,0.25554490806023761,306653.88967228512,3.2610054321133182E-6,0,6.6E-4,0.5249768465855158,3.3072082734104662E-2,9.7941740881393555E-2,0.13171077556211636,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.23117740053435962,1.6032897155347119E-4,1.6032897155347119E-4,0.26538340725648474,4.8384278405931076E-2,1.2312153670342248E-3,40,10.583711209626347,0.14317742262655386,5.6522444944395595E-2,0.20093108293798367,0.25156654794086014,0.44665396033422355,6.0647927125802824E-2,3.3731927863951371E-3,1.2998246652323742E-2,5.3806743468192836E-3,2.1752113785538162E-2,8.3334793466235985E-2,3.2037924040564728E-2,7.1635834160057241E-2,4.604408153429362E-3,0.41114158372058279,0.54309019170150696,6.12,0.91849274494619715,7.5993966081893969E-3,9.2423602125925718E-3,6.6339066410917415E-3,3.0155840181817096E-2,1.9507835371210052E-3,8.0753437099209647E-4,3.2645684149119219E-3,4.9634751718195301E-3,1.4699146801790906E-2,2.4062254440612505E-5,1.1631757191413585E-5,1.0751142802970839E-2,9.0103848754929133E-2,0.91849274494619715,91.849274494619721,510,70.206518151218702,0.702065181512187,306.65388967228512,null,8.4829175830144141E-3,null,0.41114158372058279,7.1635834160057241E-2,0.13171077556211636,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR57, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.849274494619721},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ57, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.41114158372058279},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA57, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.1635834160057241E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB57, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.13171077556211636},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S57, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":306.65388967228512},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P57, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.9227804249768932}]
[null,null,null,null,null,null,null,52,0.52,0.43603382352941172,0.73843211215938587,0.30306320290755284,5.9214373806776761,5.9214373806776761,1,5.9214373806776761,2.4262794914766028E-6,0.25565408473993345,306784.90168792015,3.2596128248099363E-6,0,6.6E-4,0.53469682012414499,3.430808273410467E-2,9.7983584618974662E-2,0.13302186336809974,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.23541155983027576,1.662558075051705E-4,1.662558075051705E-4,0.27035472825175205,5.0213983533510073E-2,1.2317413802769995E-3,40,10.439841075489143,0.14618372750112146,5.6546593079117441E-2,0.20396206196051592,0.25655872594564644,0.45502094994214137,6.294139572541961E-2,3.3746339185671218E-3,1.3445570163300604E-2,5.4937838436240165E-3,2.2313987925491743E-2,8.6259531821728949E-2,3.2037924040564728E-2,7.1652751610624177E-2,4.6063752988441216E-3,0.41907738467684369,0.55234300729970298,6.24,0.91868152024918326,7.7435229535088414E-3,9.4143572884224473E-3,6.5104490190467752E-3,3.0028233518436677E-2,1.979518724076612E-3,8.0882014317001808E-4,3.2851680048417743E-3,5.0509938466349411E-3,1.4425594307247457E-2,2.4476945190561795E-5,1.1410414222466192E-5,1.0549047881359828E-2,8.9831593046158412E-2,0.91868152024918326,91.868152024918331,520,70.411746141009829,0.70411746141009823,306.78490168792013,null,8.3250496946851854E-3,null,0.41907738467684369,7.1652751610624177E-2,0.13302186336809974,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR58, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.868152024918331},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ58, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.41907738467684369},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA58, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.1652751610624177E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB58, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.13302186336809974},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S58, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":306.78490168792013},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P58, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.9214373806776761}]
[null,null,null,null,null,null,null,53,0.53,0.43593492647058824,0.74843260119079802,0.31311265385515308,5.9200943363784591,5.9200943363784591,1,5.9200943363784591,2.4248878501920698E-6,0.25576327891640083,306915.93469968101,3.258221183525403E-6,0,6.5999999999999989E-4,0.54442693674254605,3.5568082734104667E-2,9.8025435062477934E-2,0.13435813560187662,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.23965262252247493,1.7230013844569958E-4,1.7230013844569958E-4,0.27533327479081954,5.2080379186234378E-2,1.2322674778192193E-3,40,10.299829894238593,0.14919255801265541,5.65707450838452E-2,0.20699557057431983,0.26159570925065184,0.46340010051289887,6.5280854559230897E-2,3.3760752816964917E-3,1.3893271939321532E-2,5.6072338998307989E-3,2.2876581120848824E-2,8.9234829712699831E-2,3.2037924040564721E-2,7.1669671772399829E-2,4.6083427595157113E-3,0.42710855349526722,0.56171649268284396,6.36,0.91884722622247661,7.8882367883821112E-3,9.5869642540257639E-3,6.3914912634919913E-3,2.9905236770841614E-2,2.0072003749371319E-3,8.1009297415725941E-4,3.3050445138907885E-3,5.1386217236295021E-3,1.4162012438114678E-2,2.4892689353550274E-5,1.119714269376571E-5,1.0354320615148571E-2,8.9585311548666724E-2,0.91884722622247661,91.884722622247665,530,70.596901007914624,0.70596901007914625,306.91593469968103,null,8.1729358813883591E-3,null,0.42710855349526722,7.1669671772399829E-2,0.13435813560187662,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR59, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.884722622247665},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ59, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.42710855349526722},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA59, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.1669671772399829E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB59, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.13435813560187662},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S59, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":306.91593469968103},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P59, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.9200943363784591}]
[null,null,null,null,null,null,null,54,0.54,0.43583602941176469,0.75843309022221028,0.32316210480275326,5.9187512920792429,5.9187512920792429,1,5.9187512920792429,2.4234971739215761E-6,0.25587249059384626,307046.98871261551,3.2568305072549092E-6,0,6.6E-4,0.55416666216118804,3.6852082734104674E-2,9.8067292213515594E-2,0.13571962307211549,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.24390029312034725,1.7846205895257392E-4,1.7846205895257392E-4,0.28031877973636016,5.3983510753469938E-2,1.2327936596811511E-3,40,10.163524460554164,0.15220391476834635,5.6594900959509288E-2,0.21003160938753679,0.26667769702118843,0.47179096244059826,6.7666360521150312E-2,3.377516875838771E-3,1.4341352071325565E-2,5.7210248528147085E-3,2.3439893799979045E-2,9.2260889516422501E-2,3.2037924040564728E-2,7.1686594646036064E-2,4.6103105355199221E-3,0.43523549171916687,0.57121108029748924,6.48,0.91899106780485285,8.0335260125643203E-3,9.7601667192666001E-3,6.2767914102954316E-3,2.9786600769108669E-2,2.033884946572966E-3,8.1135350901640271E-4,3.3242365790856622E-3,5.2263479726308076E-3,1.3907865059881053E-2,2.5309419462882483E-5,1.0991508603525092E-5,1.0166564839668877E-2,8.9363638746157187E-2,0.91899106780485285,91.899106780485283,540,70.763841860106652,0.70763841860106647,307.04698871261553,null,8.0262667384397111E-3,null,0.43523549171916687,7.1686594646036064E-2,0.13571962307211549,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR60, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.899106780485283},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ60, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.43523549171916687},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA60, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.1686594646036064E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB60, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.13571962307211549},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S60, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":307.04698871261553},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P60, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.9187512920792429}]
[null,null,null,null,null,null,null,55,0.55000000000000004,0.4357371323529412,0.76843357925362243,0.33321155575035344,5.9174082477800276,5.9174082477800276,1,5.9174082477800276,2.4221074616617076E-6,0.25598171977647738,307178.06373177288,3.2554407949950407E-6,0,6.6E-4,0.56391549850210032,3.8160082734104671E-2,9.8109156073700299E-2,0.13710635719724795,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.24815429578323564,1.8474166354702081E-4,1.8474166354702081E-4,0.2853109941375197,5.5923423639133253E-2,1.2333199258830682E-3,40,10.030779573119494,0.15521779837557953,5.6619060707040376E-2,0.21307017900850297,0.2718048907443058,0.48019311672811338,7.0097970523330083E-2,3.3789587010495024E-3,1.4789810650280873E-2,5.8351570400589662E-3,2.4003926391389343E-2,9.5337916743357384E-2,3.2037924040564728E-2,7.1703520232184834E-2,4.612278626932571E-3,0.44345860634678064,0.58082720865482995,6.6000000000000005,0.91911416445799221,8.1793796214747645E-3,9.9339516575459967E-3,6.1661245330044872E-3,2.9672093871259853E-2,2.0596249179280026E-3,8.1260234656893441E-4,3.3427801134746911E-3,5.3141625087582524E-3,1.366265378944815E-2,2.5727072686605991E-5,1.0793108509970662E-5,9.9854122858941356E-3,8.916530582655384E-2,0.91911416445799221,91.911416445799219,550,70.914272258910415,0.70914272258910416,307.17806373177291,null,7.8847546475981443E-3,null,0.44345860634678064,7.1703520232184834E-2,0.13710635719724795,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR61, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.911416445799219},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ61, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.44345860634678064},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA61, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.1703520232184834E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB61, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.13710635719724795},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S61, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":307.17806373177291},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P61, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.9174082477800276}]
[null,null,null,null,null,null,null,56,0.56000000000000005,0.4356382352941176,0.7784340682850347,0.34326100669795362,5.9160652034808097,5.9160652034808097,1,5.9160652034808097,2.4207187124104388E-6,0.25609096646850343,307309.1597622041,3.2540520457437723E-6,0,6.6E-4,0.57367298128016475,3.9492082734104664E-2,9.8151026644645256E-2,0.13851837000731346,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.25241437273784745,1.9113904669392295E-4,1.9113904669392295E-4,0.29030968572702615,5.7900163261697266E-2,1.2338462764452495E-3,40,9.9014575186633493,0.15823420944193484,5.6643224327369457E-2,0.21611128004574953,0.27697749425067197,0.48860617245764737,7.2575741496168522E-2,3.3804007573842456E-3,1.5238647767184806E-2,5.9496307991549965E-3,2.4568679323724047E-2,9.846612006739501E-2,3.2037924040564728E-2,7.1720448531498393E-2,4.6142470338294949E-3,0.4517783098833949,0.59056532238465664,6.7200000000000006,0.919217557556545,8.3257876129705782E-3,1.010830729018999E-2,6.05928126914183E-3,2.9561500447034577E-2,2.0844691340797788E-3,8.1384004338726939E-4,3.3607085417177982E-3,5.4020559276286738E-3,1.342591472975568E-2,2.6145590424951525E-5,1.060156688800097E-5,9.8105201675571189E-3,8.8989132320776265E-2,0.919217557556545,91.921755755654502,560,71.049749591014816,0.71049749591014821,307.3091597622041,null,7.7481318926089313E-3,null,0.4517783098833949,7.1720448531498393E-2,0.13851837000731346,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR62, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.921755755654502},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ62, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.4517783098833949},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA62, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.1720448531498393E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB62, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.13851837000731346},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S62, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":307.3091597622041},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P62, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.9160652034808097}]
[null,1500,null,null,null,"Eff (%)","Iout (mA)",57,0.56999999999999995,0.43553933823529412,0.78843455731644674,0.35331045764555369,5.9147221591815935,5.9147221591815935,1,5.9147221591815935,2.4193309251671337E-6,0.25620023067413483,307440.27680896182,3.2526642585004668E-6,0,6.600000000000001E-4,0.58343867668408156,4.0848082734104667E-2,9.8192903927964259E-2,0.13995569414584147,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.25668028284343686,1.9765430280176024E-4,1.9765430280176024E-4,0.29531463756296944,5.9913775054197281E-2,1.2343727113879818E-3,40,9.7754275954046648,0.16125314857518708,5.666739182142784E-2,0.21915491310800289,0.28219571373677999,0.49702976450477787,7.5099730388317174E-2,3.3818430448985803E-3,1.5687863513063886E-2,6.0644464678024611E-3,2.5134153025764928E-2,0.10164571135663847,3.2037924040564734E-2,7.1737379544629165E-2,4.6162157562865619E-3,0.46019502039433419,0.60042587229023181,6.84,0.91930221702411574,8.4727409036564408E-3,1.0283222982681578E-2,5.956066496864411E-3,2.9454619516361771E-2,2.1084631151946438E-3,8.1506711737936702E-4,3.3780530116387553E-3,5.4900194471706031E-3,1.319721553757508E-2,2.6564917948832467E-5,1.0416533755547657E-5,9.6415690144558541E-3,8.8834018594682887E-2,0.91930221702411574,91.930221702411572,570,71.171694607053283,0.71171694607053282,307.44027680896181,null,7.6161489670194234E-3,null,0.46019502039433419,7.1737379544629165E-2,0.13995569414584147,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR63, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.930221702411572},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ63, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.46019502039433419},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA63, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.1737379544629165E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB63, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.13995569414584147},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S63, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":307.44027680896181},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P63, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.9147221591815935}]
[null,null,null,null,null,{"$f":"BR56","v":91.827960165160505},{"$f":"I56*1000","v":500},58,0.57999999999999996,0.43544044117647057,0.79843504634785889,0.36335990859315392,5.9133791148823773,5.9133791148823773,1,5.9133791148823773,2.4179440989325425E-6,0.25630951239758332,307571.41487709997,3.251277432265876E-6,0,6.600000000000001E-4,0.59321217911542601,4.2228082734104673E-2,9.8234787925271461E-2,0.14141836287177145,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.26095180028921944,2.0428752622255399E-4,2.0428752622255399E-4,0.30032564679948071,6.1964304464236668E-2,1.2348992307315565E-3,40,9.6525656724349052,0.16427461638330587,5.6691563190147065E-2,0.22220107880418449,0.287459757787484,0.50546355146944666,7.7669994166688211E-2,3.3832855636481002E-3,1.613745797897382E-2,6.1796043838093047E-3,2.5700347926431225E-2,0.10487690570473351,3.2037924040564734E-2,7.1754313272229781E-2,4.6181847943796567E-3,0.46870916155882697,0.61040931540407528,6.9599999999999991,0.91936904730342262,8.6202312536143629E-3,1.0458689151350889E-2,5.8562981443861769E-3,2.935126352442469E-2,2.131649334486807E-3,8.1628405101362282E-4,3.394842584553099E-3,5.5780448552735524E-3,1.297615278547566E-2,2.6985004074598054E-5,1.0237682538070867E-5,9.4782607231323601E-3,8.8698939094323886E-2,0.91936904730342262,91.936904730342263,580,71.281400919850697,0.71281400919850701,307.57141487709998,null,7.4885730517625423E-3,null,0.46870916155882697,7.1754313272229781E-2,0.14141836287177145,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR64, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.936904730342263},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ64, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.46870916155882697},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA64, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.1754313272229781E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB64, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.14141836287177145},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S64, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":307.57141487709998},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P64, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.9133791148823773}]
[null,null,null,null,null,{"$f":"BR81","v":91.842313069274653},{"$f":"I81*1000","v":750},59,0.59,0.43534154411764708,0.80843553537927115,0.37340935954075405,5.9120360705831612,5.9120360705831612,1,5.9120360705831612,2.4165582327087976E-6,0.25641881164306213,307702.57397167454,3.2498915660421307E-6,0,6.6E-4,0.60299310895803127,4.3632082734104655E-2,9.8276678638181666E-2,0.14290641006141167,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.26522871341027365,2.1103881125180722E-4,2.1103881125180722E-4,0.30534252357244762,6.4051796953992837E-2,1.2354258344962731E-3,40,9.5327537819152575,0.16729861347445585,5.6715738434459054E-2,0.22524977774341115,0.2927698373988703,0.51390721380056137,8.0286589816461779E-2,3.3847283136884203E-3,1.6587431255999523E-2,6.2951048850918021E-3,2.6267264454779744E-2,0.10815992146275534,3.2037924040564728E-2,7.1771249714953092E-2,4.6201541481846933E-3,0.47732116272476338,0.62051611504468118,7.08,0.91941889273728494,8.7682511985844175E-3,1.0634697179320224E-2,5.7598061168807387E-3,2.9251257237594152E-2,2.1540674687495639E-3,8.1749129422544885E-4,3.4111044068151175E-3,5.6661244626005801E-3,1.276234958409816E-2,2.7405800870865742E-5,1.0064708143775063E-5,9.3203167999001899E-3,8.8582936257783212E-2,0.91941889273728494,91.941889273728492,590,71.3800443047935,0.713800443047935,307.70257397167455,null,7.3651866429643807E-3,null,0.47732116272476338,7.1771249714953092E-2,0.14290641006141167,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR65, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.941889273728492},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ65, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.47732116272476338},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA65, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.1771249714953092E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB65, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.14290641006141167},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S65, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":307.70257397167455},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P65, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.9120360705831612}]
[null,null,null,null,null,{"$f":"BR106","v":91.27033478138263},{"$f":"I106*1000","v":1000},60,0.6,0.43524264705882348,0.81843602441068342,0.38345881048835428,5.9106930262839441,5.9106930262839441,1,5.9106930262839441,2.4151733254994122E-6,0.25652812841478578,307833.75409774296,3.2485066588327457E-6,0,6.6E-4,0.61278111055324824,4.5060082734104667E-2,9.8318576068310168E-2,0.14441987021043579,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.26951082360976997,2.1790825212844963E-4,2.1790825212844963E-4,0.31036508998805573,6.6176298000222927E-2,1.235952522702438E-3,40,9.4158797412724518,0.1703251404569967,5.6739917555295984E-2,0.22830101053499513,0.29812616600146863,0.52236045209365822,8.2949574341093263E-2,3.3861712950751729E-3,1.7037783435255111E-2,6.4109483096745981E-3,2.6834903040004882E-2,0.11149498027166044,3.2037924040564728E-2,7.1788188873452174E-2,4.6221238177776109E-3,0.48603145896435884,0.63074674087417737,7.1999999999999993,0.91945254242716512,8.9167939887529347E-3,1.081123934065637E-2,5.6664313275583741E-3,2.9154436746540599E-2,2.1757546245651047E-3,8.1868926704158984E-4,3.4268638647109661E-3,5.7542510599792986E-3,1.2555453435253671E-2,2.7827263393800382E-5,9.897325225679475E-6,9.1674767744357143E-3,8.8485115018114097E-2,0.91945254242716512,91.945254242716516,600,71.468691685531624,0.71468691685531627,307.83375409774294,null,7.2457863129617552E-3,null,0.48603145896435884,7.1788188873452174E-2,0.14441987021043579,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR66, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.945254242716516},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ66, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.48603145896435884},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA66, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.1788188873452174E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB66, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.14441987021043579},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S66, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":307.83375409774294},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P66, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.9106930262839441}]
[null,null,null,null,null,null,null,61,0.61,0.43514375000000005,0.82843651344209557,0.39350826143595447,5.9093499819847288,5.9093499819847288,1,5.9093499819847288,2.413789376309281E-6,0.25663746271697008,307964.95526036411,3.2471227096426142E-6,0,6.5999999999999989E-4,0.62257585035951424,4.6512082734104669E-2,9.8360480217272742E-2,0.14595877843591826,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.2737979443767356,2.2489594303477803E-4,2.2489594303477803E-4,0.31539317920338755,6.8337853094269832E-2,1.2364792953703618E-3,40,9.3018368028498255,0.17335419793948312,5.676410055359031E-2,0.23135477778844377,0.30352895948380776,0.53082298554350282,8.5659004762320606E-2,3.3876145078640054E-3,1.748851460788392E-2,6.5271349956907455E-3,2.7403264111438671E-2,0.11488230709531276,3.2037924040564721E-2,7.1805130748380269E-2,4.6240938032343672E-3,0.49484049113073514,0.64110166895694254,7.32,0.91947073462749296,9.0658535334118152E-3,1.0988308731815949E-2,5.5760248213066787E-3,2.906064856457934E-2,2.1967455429036434E-3,8.1987836195363223E-4,3.4421447245540611E-3,5.8424178798609219E-3,1.2355134290121415E-2,2.8249349447668054E-5,9.7352666097173159E-6,9.0194967649230035E-3,8.8404637831487845E-2,0.91947073462749296,91.947073462749302,610,71.54830972155635,0.71548309721556347,307.96495526036409,null,7.1301815896828635E-3,null,0.49484049113073514,7.1805130748380269E-2,0.14595877843591826,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR67, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.947073462749302},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ67, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.49484049113073514},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA67, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.1805130748380269E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB67, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.14595877843591826},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S67, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":307.96495526036409},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P67, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.9093499819847288}]
[null,null,null,null,null,null,null,62,0.62,0.43504485294117645,0.83843700247350783,0.40355771238355465,5.9080069376855109,5.9080069376855109,1,5.9080069376855109,2.412406384144671E-6,0.2567468145538323,308096.17746459879,3.2457397174780045E-6,0,6.6E-4,0.63237701527717805,4.7988082734104667E-2,9.840239108668572E-2,0.14752317047840885,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.27808990038978404,2.3200197809640003E-4,2.3200197809640003E-4,0.32042663458956216,7.053650774206785E-2,1.2370061525203641E-3,40,9.1905233287137857,0.17638578653066506,5.678828743027485E-2,0.23441108011346029,0.30897843621632154,0.53929455053561137,8.841493812017176E-2,3.389057952110587E-3,1.793962486505854E-2,6.6436652813817634E-3,2.7972348098550891E-2,0.11832213025409401,3.2037924040564728E-2,7.1822075340390909E-2,4.6260641046309506E-3,0.50374870591543741,0.651581381819197,7.4399999999999995,0.9194741607267003,9.2154243508450733E-3,1.1165899209584438E-2,5.4884469807399468E-3,2.8969748810801509E-2,2.2170727844827349E-3,8.2105894606822772E-4,3.4569692596062088E-3,5.9306185614011221E-3,1.2161082790044474E-2,2.8672019367892706E-5,9.5782818706491889E-6,8.8761481781257767E-3,8.8340720172938064E-2,0.9194741607267003,91.947416072670023,620,71.619772941093288,0.71619772941093285,308.09617746459878,null,7.0181939414057249E-3,null,0.50374870591543741,7.1822075340390909E-2,0.14752317047840885,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR68, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.947416072670023},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ68, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.50374870591543741},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA68, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.1822075340390909E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB68, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.14752317047840885},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S68, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":308.09617746459878},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P68, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.9080069376855109}]
[null,null,null,null,null,null,null,63,0.63,0.43494595588235296,0.84843749150491998,0.41360716333115483,5.9066638933862956,5.9066638933862956,1,5.9066638933862956,2.4110243480132257E-6,0.25685618392959109,308227.42071550927,3.2443576813465588E-6,0,6.6E-4,0.64218431112171548,4.9488082734104669E-2,9.8444308678165948E-2,0.14911308270404583,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.28238652669829262,2.3922645138217658E-4,2.3922645138217658E-4,0.32546530896899506,7.2772307464148714E-2,1.2375330941727697E-3,40,9.081842488533356,0.17941990683948789,5.6812478186282669E-2,0.23746991811994334,0.31447481707561042,0.547774899362519,9.1217431472971802E-2,3.3905016278706025E-3,1.8391114297980782E-2,6.7605395050976645E-3,2.854215543094905E-2,0.12181468145910657,3.2037924040564728E-2,7.1839022650137724E-2,4.6280347220433726E-3,0.51275655590689806,0.66218636850958035,7.5600000000000005,0.91946346885960772,9.3655015228784715E-3,1.1344005334807904E-2,5.4035668057558217E-3,2.8881602468832025E-2,2.2367668979649392E-3,8.2223136305813681E-4,3.4713583652474212E-3,6.0188471187713147E-3,1.1973008670200059E-2,2.9095235824183913E-5,9.426136039824431E-6,8.7372165298121116E-3,8.8292626449192224E-2,0.91946346885960772,91.946346885960779,630,71.68387138413388,0.71683871384133879,308.22742071550925,null,6.9096558555119389E-3,null,0.51275655590689806,7.1839022650137724E-2,0.14911308270404583,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR69, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.946346885960779},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ69, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.51275655590689806},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA69, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.1839022650137724E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB69, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.14911308270404583},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S69, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":308.22742071550925},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P69, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.9066638933862956}]
[null,null,null,null,null,null,null,64,{"$f":"IF(PLOT_TYPE=1, H70/100*Iout, min_I*EXP(H70*rr/100))","v":0.64},{"$f":"IF(I70<Icrit, (Vin-(Rdcr+RdsonTop)*Iripple/2-Vout)/L*OnTime, (Vin-(Rdcr+RdsonTop)*I70-Vout)/L*OnTime)","v":0.43484705882352942},{"$f":"IF(I70<Icrit, (Vin-(Rdcr+RdsonTop)*Iripple/2-Vout)/L*OnTime, I70+((Vin-(Rdcr+RdsonTop)*J70-Vout)/L*OnTime)/2)","v":0.85843798053633225},{"$f":"IF(I70<Icrit, 0, I70-((Vin-(Rdcr+RdsonTop)*K70-Vout)/L*OnTime)/2)","v":0.42365661427875501},5.9053208490870794,{"$f":"IF(I70<Icrit, 1000*SQRT((J70*CoutEsr)^2+(((J70/2)-I70)*(OnTime+OffTime)/Cout)^2), 1000*J70*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":5.9053208490870794},1,{"$f":"IF(I70<Icrit, 1000*((N70/1000)*O70), 1000*J70*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":5.9053208490870794},{"$f":"IF(I70<Icrit, L*J70/(Vout+J70/2*(RdsonBot+Rdcr)), L*J70/(Vout+I70*(RdsonBot+Rdcr)))","v":2.4096432669239594E-6},0.25696557084846616,{"$f":"IF(I70<Icrit,I70/((OnTime+Q70)*J70/2),1/(OnTime+Q70))","v":308358.68501815939},3.242976600257293E-6,0,{"$f":"S70*(T70*Iq_active+U70*Iq_sleep)","v":6.6E-4},0.65199746123038871,{"$f":"W70^2*Rdcr","v":5.1012082734104659E-2},{"$f":"Core_Loss/1000*S70/$S$106","v":9.8486232993330758E-2},{"$f":"(Y70+X70*(1+Ltc*(Ta-25)))/(1-X70*Ltc*ThetaCa)","v":0.15072855210670888},0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.28668766797344897,2.4656945690416357E-4,2.4656945690416357E-4,0.33050906391931206,7.5045297795647281E-2,1.2380601203479101E-3,{"$f":"20*VIN_nom/24","v":40},{"$f":"IF(I70<Icrit, Csw*Vin/Iripple*1000000000, Csw*Vin/(I70+Iripple/2)*1000000000)","v":8.9757019786452403},{"$f":"IF(I70<Icrit, Vin*(I70+Iripple/2)*AK70/1000000000/2*S70, Vin*(I70-Iripple/2)*AJ70/1000000000/2*S70 + Vin*(I70+Iripple/2)*AK70/1000000000/2*S70)","v":0.18245655947509204},{"$f":"IF(I70<Icrit, Csw*(Vin)^2*S70/2, Csw*Vin^2*S70/2)","v":5.6836672822547139E-2},0.2405312924179871,{"$f":"(AI70+AL70+AM70+AH70*(1+RdsonTopTc*(Ta-25)))/(1-AH70*RdsonTopTc*ThetaJA)","v":0.32001832546906234},{"$f":"IF(I70<Icrit,Iripple*SQRT((OffTime)*S70/3), SQRT(OffTime*S70*(I70^2+Iripple^2/12)))","v":0.55626379905223167},9.4066541897350558E-2,{"$f":"QgBot*S70*Vdd","v":3.3919455351997538E-3},{"$f":"IF(I70<Icrit, Vin*Idss*R70, QrrBot*(I70-Iripple/2)/1*S70*Vin+Vin*Idss*R70)","v":1.8842982997881737E-2},{"$f":"IF(I70<Icrit, dead1*S70*(I70+Iripple/2)*((I70+Iripple/2)*BDserR+VSD), dead1*S70*(I70+Iripple/2)*((I70+Iripple/2)*BDserR+VSD)+dead2*S70*(I70-Iripple/2)*((I70-Iripple/2)*BDserR+VSD))","v":6.8777580052970079E-3},2.9112686538378497E-2,{"$f":"(AR70+AS70+AT70+AQ70*(1+RdsonBotTc*(Ta-25)))/(1-AQ70*RdsonBotTc*ThetaJA)","v":0.1253601958469798},{"$f":"Vin*V70+Vout*Ifb/0.8","v":3.2037924040564728E-2},{"$f":"(Vin-Vdd)*(S70*QgBot+S70*QgTop)+AW70","v":7.1855972678274649E-2},{"$f":"AI70+AR70","v":4.6300056555476643E-3},0.52186449964986448,{"$f":"SUM(Z70,AC70,AF70,AZ70)","v":0.67291712466073184},{"$f":"Vout*I70","v":7.68},0.91943926719037539,9.5160806535960624E-3,1.1522622321301981E-2,{"$f":"Vin*S70*(QgBot+QgTop)/($BB70+$BA70)","v":5.3212612587800467E-3},2.8796082713170305E-2,2.2558565728194122E-3,8.233959349352889E-4,3.4853316636445091E-3,{"$f":"X70/($BB70+$BA70)","v":6.1070979123567688E-3},{"$f":"Y70/($BB70+$BA70)","v":1.1790639308818828E-2},2.9518963641600649E-5,9.2786084307653492E-6,8.6025003727297489E-3,8.825966628422531E-2,{"$f":"BC70","v":0.91943926719037539},91.943926719037535,{"$f":"I70*1000","v":640},71.741317737155555,0.71741317737155552,{"$f":"S70/1000","v":308.35868501815941},null,{"$f":"AM70/($BB70+$BA70)","v":6.8044100012372224E-3},null,0.52186449964986448,7.1855972678274649E-2,0.15072855210670888,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR70, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.943926719037535},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ70, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.52186449964986448},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA70, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.1855972678274649E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB70, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15072855210670888},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S70, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":308.35868501815941},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P70, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.9053208490870794}]
[null,null,null,null,null,null,null,65,0.65,0.43474816176470593,0.8684384695677444,0.43370606522635524,{"$f":"IF(I71<Icrit, 1000*((((J71/2)-I71)*0.000002/Cout+Vout/306)), 1000*J71*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":5.9039778047878624},5.9039778047878624,{"$f":"ROUNDUP(M71/N71,0)","v":1},5.9039778047878624,2.4082631398872561E-6,0.25707497531467893,308489.97037761472,{"$f":"IF(1/S71-OnTime-Q71>Tsleep, OnTime+Q71+Tsleep, 1/S71)","v":3.2415964732205896E-6},{"$f":"IF(1/S71-OnTime-Q71>Tsleep, 1/S71-OnTime-Q71-Tsleep, 0)","v":0},6.6E-4,{"$f":"IF(I71<Icrit,Iripple*SQRT((OnTime+OffTime)*S71/3), SQRT(I71^2+Iripple^2/12))","v":0.66181620518907835},5.2560082734104674E-2,9.8528164033798035E-2,0.15236961631021129,{"$f":"Iripple/SQRT(12)*SQRT((OnTime+Q71)*S71)","v":0.12450176485043199},{"$f":"RCoutEsr*AA71^2","v":7.750344725436132E-5},7.750344725436132E-5,{"$f":"SQRT($R71)*SQRT($I71^2*(1-R71)+(Iripple^2)/12)","v":0.29099317782241002},{"$f":"RCinEsr*AD71^2","v":2.5403108861755421E-4},2.5403108861755421E-4,{"$f":"IF(I71<Icrit,Iripple*SQRT((OnTime)*S71/3), SQRT(OnTime*S71*(I71^2+Iripple^2/12)))","v":0.3355577691372908},{"$f":"RdsonTop*AG71^2","v":7.7355524286307611E-2},{"$f":"QgTop*S71*Vdd","v":1.238587231066123E-3},40,8.8720137605911944,0.18549574504681357,5.6860871340001944E-2,{"$f":"AI71+AL71+AM71","v":0.24359520361788164},0.32560918735984118,0.56476103029770597,{"$f":"RdsonBot*AP71^2","v":9.6962326488249609E-2},3.3933896741537625E-3,1.9295231056021746E-2,6.9953211205469427E-3,{"$f":"AR71+AS71+AT71","v":2.9683941850722453E-2},0.12895891201528878,3.2037924040564728E-2,7.1872925425455744E-2,4.6319769052198855E-3,0.53107300170580563,0.68377415255188878,7.8000000000000007,0.91940212690053613,{"$f":"(AO71-AN71)/($BB71+$BA71)","v":9.6671578317876379E-3},{"$f":"(AV71-AU71)/($BB71+$BA71)","v":1.1701745989396094E-2},5.2414146688164005E-3,{"$f":"AN71/($BB71+$BA71)","v":2.8713070296031991E-2},{"$f":"AS71/(BA71+BB71)","v":2.2743687784543163E-3},{"$f":"AT71/($BB71+$BA71)","v":8.2455296366449997E-4},{"$f":"AU71/($BB71+$BA71)","v":3.4989075990187251E-3},6.1953656225389713E-3,1.1613718406702412E-2,{"$f":"(AF71)/($BB71+$BA71)","v":2.9943169637671522E-5},{"$f":"(AC71)/($BB71+$BA71)","v":9.1354915702286292E-6},{"$f":"AX71/($BB71+$BA71)","v":8.4718103208625151E-3},{"$f":"SUM(BD71:BO71)","v":8.8241191138481459E-2},0.91940212690053613,91.940212690053613,650,71.792753953912452,{"$f":"BT71/100","v":0.71792753953912447},308.48997037761472,null,6.7023084676173742E-3,null,{"$f":"AZ71","v":0.53107300170580563},{"$f":"AX71","v":7.1872925425455744E-2},{"$f":"Z71","v":0.15236961631021129},null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR71, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.940212690053613},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ71, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.53107300170580563},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA71, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.1872925425455744E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB71, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15236961631021129},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S71, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":308.48997037761472},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P71, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.9039778047878624}]
[null,null,null,null,null,null,null,66,0.66,0.43464926470588233,0.87843895859915655,0.44375551617395542,5.9026347604886453,5.9026347604886453,1,5.9026347604886453,2.4068839659148654E-6,{"$f":"OnTime*S72","v":0.25718439733245202},308621.27679894242,3.240217299248199E-6,0,6.6E-4,0.67164029766748834,5.4132082734104678E-2,9.8570101801186152E-2,0.15403631357053188,0.12450176485043199,7.750344725436132E-5,{"$f":"AB72","v":7.750344725436132E-5},0.29530291815954146,2.6161144042062252E-4,{"$f":"AE72","v":2.6161144042062252E-4},0.34061130185693511,7.9703032500488533E-2,1.2391144263477539E-3,40,8.7706938175711127,0.18853746416418404,5.6885073739581064E-2,0.24666165233011286,0.33124763129224549,0.57326638647743966,9.9904842358929963E-2,3.3948340447883672E-3,1.9747858563690449E-2,7.1132291895232482E-3,3.0255921798002065E-2,0.13261107205859618,3.2037924040564728E-2,7.1889880892335362E-2,4.6339484711361211E-3,{"$f":"AO72+AV72+AX72+AY72","v":0.54038253271431314},0.69475796117251998,7.92,0.91935258491255867,9.8187295967419111E-3,1.188137272363517E-2,5.163918188231021E-3,2.8632452988445974E-2,2.2923288910374272E-3,8.2570273263430087E-4,3.5121035244830086E-3,6.2836452257954067E-3,1.1442004783587695E-2,3.036782247391378E-5,8.996590223854952E-6,8.3449681600283425E-3,8.8236591227318029E-2,0.91935258491255867,{"$f":"100*BQ72","v":91.935258491255865},660,71.838757366287027,0.71838757366287032,308.6212767989424,null,6.6032120688668382E-3,null,0.54038253271431314,7.1889880892335362E-2,0.15403631357053188,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR72, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.935258491255865},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ72, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54038253271431314},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA72, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.1889880892335362E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB72, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15403631357053188},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S72, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":308.6212767989424},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P72, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.9026347604886453}]
[null,null,null,null,null,null,null,67,0.67,0.43455036764705884,0.88843944763056881,0.4538049671215556,5.90129171618943,5.90129171618943,1,5.90129171618943,2.4055057440199025E-6,0.25729383690600932,308752.6042872112,3.2388390773532365E-6,0,6.6E-4,0.68146950735221623,5.5728082734104678E-2,9.8612046297114023E-2,0.15572868277808757,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.299616758629344,2.6931060615466377E-4,2.6931060615466377E-4,0.34566954631643648,8.2087868017169774E-2,1.2396417062131529E-3,40,8.6716619273957516,0.19158171743693053,5.6909280022218768E-2,0.24973063916536245,0.33693388841744487,0.58177967275833897,0.10289414664097919,3.3962786471593239E-3,2.0200865612206766E-2,7.2314825510103754E-3,3.0828626810376465E-2,0.13631692160512729,3.2037924040564728E-2,7.1906839079568019E-2,4.6359203533724771E-3,0.54979356945551261,0.70586906628700918,8.0400000000000009,{"$f":"BB73/(BB73+BA73)","v":0.91929114637584197},9.9707929070454136E-3,1.2061499434216324E-2,5.0886692969061278E-3,2.8554125070086787E-2,2.3097608092574481E-3,8.268455079994062E-4,3.5249357813064673E-3,6.371931972880952E-3,1.1275271279470341E-2,3.0792892520285291E-5,8.8617205067837577E-6,8.2218060360347359E-3,8.824529270823106E-2,0.91929114637584197,91.929114637584192,670,71.879846296152991,0.71879846296152994,308.75260428721123,null,6.5069897103295134E-3,null,0.54979356945551261,7.1906839079568019E-2,0.15572868277808757,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR73, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.929114637584192},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ73, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.54979356945551261},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA73, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.1906839079568019E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB73, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15572868277808757},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S73, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":308.75260428721123},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P73, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.90129171618943}]
[null,null,null,null,null,null,null,68,0.68,0.4344514705882353,0.89843993666198096,0.46385441806915584,5.899948671890213,5.899948671890213,1,5.899948671890213,2.4041284732168432E-6,0.2574032940395764,308883.95284749172,3.2374618065501763E-6,0,6.600000000000001E-4,0.69130361596831846,5.7348082734104674E-2,9.8653997523201156E-2,0.15744676346004563,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.30393457607624375,2.7712867960393798E-4,2.7712867960393798E-4,0.3507323932693403,8.4510076429957726E-2,1.2401690706826793E-3,40,8.574841450649588,0.19462850547497595,5.6933490188849675E-2,0.25280216473450828,0.34266819251959918,0.59030070527298684,0.10593029648431883,3.3977234813224091E-3,2.0654252292918944E-2,7.3500815439015051E-3,3.1402057318142856E-2,0.14007670985408885,3.2037924040564734E-2,7.1923799987808498E-2,4.6378925520050886E-3,0.55930659491350165,0.71710799050040563,8.16,0.91921828693896712,1.0123345112085892E-2,1.2242123521786734E-2,5.0155713490130736E-3,2.8477986862955548E-2,2.3266870601350719E-3,8.2798153990770349E-4,3.5374197713655066E-3,6.4602213688820902E-3,1.111330375036251E-2,3.1218351731273256E-5,8.7307090707130656E-6,8.1021657126144897E-3,8.8266755109910611E-2,0.91921828693896712,91.921828693896714,680,71.916485184007442,0.71916485184007439,308.88395284749174,null,6.4135178089278055E-3,null,0.55930659491350165,7.1923799987808498E-2,0.15744676346004563,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR74, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.921828693896714},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ74, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.55930659491350165},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA74, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.1923799987808498E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB74, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15744676346004563},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S74, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":308.88395284749174},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P74, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.899948671890213}]
[null,null,null,null,null,null,null,69,0.69,0.43435257352941181,0.90844042569339312,0.47390386901675585,5.8986056275909968,5.8986056275909968,1,5.8986056275909968,2.4027521525215251E-6,0.25751276873737972,309015.32248485566,3.2360854858548587E-6,0,6.5999999999999989E-4,0.70114241738099981,5.8992082734104653E-2,9.8695955481067368E-2,0.1591905957826765,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.30825625405691925,2.8506575449561186E-4,2.8506575449561186E-4,0.35579973953573779,8.6969703347091129E-2,1.2406965197766955E-3,40,8.4801591328881418,0.1976778288884386,5.6957704240408594E-2,0.25587622964862389,0.34845078004236568,0.59882931036427578,0.10901334905721165,3.3991685473334123E-3,2.1108018697204502E-2,7.4690265071985576E-3,3.1976213751736468E-2,0.14389068961364243,3.2037924040564721E-2,7.1940763617711651E-2,4.6398650671101074E-3,0.56892209834082985,0.72847526332525625,8.2799999999999994,0.91913445482933398,1.0276383925993064E-2,1.2423242845270965E-2,4.944533158191212E-3,2.8403944304574082E-2,2.3431288958674456E-3,8.2911106362316316E-4,3.549570023455139E-3,6.5485091549587256E-3,1.0955900149148681E-2,3.1644173532468232E-5,8.603392359846792E-6,7.9858978922429207E-3,8.8300468979217714E-2,0.91913445482933398,91.913445482933398,690,71.94908925319227,0.71949089253192267,309.01532248485563,null,6.3226797627220291E-3,null,0.56892209834082985,7.1940763617711651E-2,0.1591905957826765,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR75, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.913445482933398},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ75, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.56892209834082985},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA75, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.1940763617711651E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB75, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.1591905957826765},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S75, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":309.01532248485563},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P75, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.8986056275909968}]
[null,null,null,null,null,null,null,70,0.7,0.43425367647058821,0.91844091472480538,0.48395331996435609,5.8972625832917798,5.8972625832917798,1,5.8972625832917798,2.4013767809511418E-6,0.25762226100364749,309146.71320437698,3.2347101142844749E-6,0,6.6E-4,0.71098571676994482,6.0660082734104663E-2,9.8737920172333252E-2,0.16096022055374834,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.3125816823912862,2.9312192449970078E-4,2.9312192449970078E-4,0.36087148758974624,8.9466794391447405E-2,1.2412240535155737E-3,40,8.3875449197968326,0.20072968828763302,5.6981922177830768E-2,0.25895283451897932,0.35428189011580247,0.60736532389111586,0.11214336154626947,3.4006138452481473E-3,2.1562164916470342E-2,7.5883177800122889E-3,3.255109654173078E-2,0.14775911733954411,3.2037924040564728E-2,7.1957729969932716E-2,4.6418378987637208E-3,0.578640575324043,0.7399714212495454,8.3999999999999986,0.91904007275896027,1.0429907403779443E-2,1.2604855692433118E-2,4.8754686173886966E-3,2.8331908556840688E-2,2.3591063825801912E-3,8.3023430055483417E-4,3.5614002540590712E-3,6.6367912916090602E-3,1.0802869683243998E-2,3.207033271660137E-5,8.4796159290141037E-6,7.8728615937067366E-3,8.8345953724841428E-2,0.91904007275896027,91.904007275896021,700,71.978028730187987,0.71978028730187982,309.14671320437697,null,6.2343654647927385E-3,null,0.578640575324043,7.1957729969932716E-2,0.16096022055374834,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR76, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.904007275896021},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ76, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.578640575324043},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA76, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.1957729969932716E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB76, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.16096022055374834},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S76, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":309.14671320437697},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P76, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.8972625832917798}]
[null,null,null,null,null,null,null,71,0.71,0.43415477941176478,0.92844140375621753,0.49400277091195621,5.8959195389925645,5.8959195389925645,1,5.8959195389925645,2.4000023575242421E-6,0.2577317708426089,309278.1250111307,3.2333356908575757E-6,0,6.6E-4,0.72083332986958382,6.2352082734104669E-2,9.877989159861969E-2,0.16275567922496118,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.31691075674865221,3.0129728322901024E-4,3.0129728322901024E-4,0.36594754517992573,9.200139520054787E-2,1.2417516719196897E-3,40,8.2969317843312478,0.20378408428306932,5.7006144002051611E-2,0.26203197995704064,0.36016176458367044,0.61590859058957625,0.11532039115645963,3.4020593751224381E-3,2.2016691042152661E-2,7.7079557015622812E-3,3.3126706118837383E-2,0.15168225317445941,3.2037924040564728E-2,7.197469904512703E-2,4.6438110470421283E-3,0.58846252785029896,0.75159700780574346,8.52,0.91893553967315711,1.0583913919469804E-2,1.2786960752911315E-2,4.8082963500324814E-3,2.8261795647118431E-2,2.3746384817649908E-3,8.3135145920093002E-4,3.572923423111257E-3,6.7250639433110116E-3,1.0654032041670604E-2,3.2496805348134577E-5,8.3592338179831678E-6,7.7629235809679436E-3,8.8402755638724878E-2,0.91893553967315711,91.893553967315711,710,72.003632642003467,0.72003632642003468,309.27812501113073,null,6.1484708571843908E-3,null,0.58846252785029896,7.197469904512703E-2,0.16275567922496118,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR77, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.893553967315711},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ77, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.58846252785029896},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA77, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.197469904512703E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB77, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.16275567922496118},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S77, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":309.27812501113073},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P77, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.8959195389925645}]
[null,null,null,null,null,null,null,72,0.72,0.43405588235294118,0.93844189278762968,0.50405222185955645,5.8945764946933474,5.8945764946933474,1,5.8945764946933474,2.3986288812607272E-6,0.25784129825849506,309409.55791019404,3.2319622145940607E-6,0,6.6E-4,0.7306850822692853,6.4068082734104664E-2,9.8821869761548276E-2,0.16457701389442411,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.32124337826590771,3.0959192423907916E-4,3.0959192423907916E-4,0.37102782497963477,9.4573551426564414E-2,1.2422793750094291E-3,40,8.2082555649423377,0.20684101748545392,5.7030369714006962E-2,0.26511366657447033,0.36609064803114449,0.62445896348441576,0.1185444951111134,3.4035051370121345E-3,2.2471597165717047E-2,7.8279406111770207E-3,3.3703042913906203E-2,0.15566036098796901,3.2037924040564728E-2,7.1991670843950167E-2,4.6457845120215641E-3,0.5983884643750853,0.76335257364100284,8.64,0.91882123235697943,1.0738402146031159E-2,1.2969557093491031E-2,4.7429393895562465E-3,2.8193526138499091E-2,2.389743125096498E-3,8.3246273601607834E-4,3.5841517852240115E-3,6.8133234644096015E-3,1.0509216684968369E-2,3.2923568675592513E-5,8.2421079766396314E-6,7.655957838457907E-3,8.8470446078402223E-2,0.91882123235697943,91.882123235697946,720,72.026192211331946,0.72026192211331941,309.40955791019405,null,6.0648975211108833E-3,null,0.5983884643750853,7.1991670843950167E-2,0.16457701389442411,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR78, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.882123235697946},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ78, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.5983884643750853},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA78, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.1991670843950167E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB78, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.16457701389442411},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S78, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":309.40955791019405},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P78, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.8945764946933474}]
[null,null,null,null,null,null,null,73,0.73,0.43395698529411769,0.94844238181904195,0.51410167280715657,5.8932334503941313,5.8932334503941313,1,5.8932334503941313,2.39725635118185E-6,0.25795084325553774,309541.01190664532,3.2305896845151835E-6,0,6.6E-4,0.74054080876807338,6.5808082734104656E-2,9.8863854662741002E-2,0.16642426730917284,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.32557945319492576,3.1800594102812061E-4,3.1800594102812061E-4,0.37611224426462209,9.7183308736324511E-2,1.2428071628051811E-3,40,8.1214548140660536,0.2099004885056889,5.7054599314632866E-2,0.26819789498312696,0.3720687878129349,0.63301630334645342,0.12181573065193237,3.4049511309730989E-3,2.2926883378658412E-2,7.948272848293924E-3,3.4280107357925436E-2,0.15969370841727204,3.2037924040564728E-2,7.2008645367057936E-2,4.6477582937782796E-3,0.60841889989104325,0.77523867658849854,8.76,0.9186975069127622,1.0893371036934619E-2,1.3152644135407931E-2,4.6793248846325689E-3,2.8127024826512508E-2,2.404437283248074E-3,8.3356831620890728E-4,3.5950969368068421E-3,6.9015663861336464E-3,1.0368262192060025E-2,3.3350601050911107E-5,8.1281077362701504E-6,7.5518450884567755E-3,8.8548619795189076E-2,0.9186975069127622,91.869750691276224,730,72.045963869077937,0.72045963869077934,309.54101190664534,null,5.9835523000296579E-3,null,0.60841889989104325,7.2008645367057936E-2,0.16642426730917284,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR79, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.869750691276224},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ79, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.60841889989104325},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA79, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.2008645367057936E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB79, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.16642426730917284},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S79, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":309.54101190664534},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P79, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.8932334503941313}]
[null,null,null,null,null,null,null,74,0.74,0.43385808823529409,0.95844287085045421,0.52415112375475681,5.8918904060949133,5.8918904060949133,1,5.8918904060949133,2.3958847663102087E-6,0.25806040583797085,309672.48700556502,3.2292180996435414E-6,0,6.6E-4,0.7504003527790164,6.7572082734104658E-2,9.8905846303820502E-2,0.16829748286772994,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.32991889257662749,3.265394270369648E-4,3.265394270369648E-4,0.38120072461543575,9.9830712811317973E-2,1.2433350353273434E-3,40,8.0364706561255712,0.21296249795487299,5.7078832804865746E-2,0.27128466579506605,0.37809643408183197,0.64158047819170749,0.1251341550389968,3.4063973570612159E-3,2.3382549772501086E-2,8.0689527524594011E-3,3.4857899882021703E-2,0.16378256690860432,3.2037924040564728E-2,7.2025622615106338E-2,4.6497323923885593E-3,0.61855435599793118,0.78725588173995242,8.879999999999999,0.91856470012064495,1.1048819809199207E-2,1.3336221633494016E-2,4.6173838277358339E-3,2.8062220459839443E-2,2.4187370292605313E-3,8.3466837447641027E-4,3.6057698594554881E-3,6.989789404637417E-3,1.0231015658811654E-2,3.3777881855155047E-5,8.01710932269354E-6,7.4504723466720614E-3,8.8636893394759914E-2,0.91856470012064495,91.856470012064491,740,72.063171902227168,0.72063171902227163,309.67248700556502,null,5.9043469525493176E-3,null,0.61855435599793118,7.2025622615106338E-2,0.16829748286772994,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR80, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.856470012064491},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ80, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.61855435599793118},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA80, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.2025622615106338E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB80, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.16829748286772994},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S80, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":309.67248700556502},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P80, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.8918904060949133}]
[null,null,null,null,null,null,null,75,0.75,0.4337591911764706,0.96844335988186636,0.53420057470235704,5.890547361795698,5.890547361795698,1,5.890547361795698,2.3945141256697519E-6,0.25816998601002877,309803.98321203451,3.227847459003085E-6,0,6.600000000000001E-4,0.76026356577891607,6.9360082734104669E-2,9.8947844686409686E-2,0.17019670462270683,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.33426161193941084,3.3519247564899989E-4,3.3519247564899989E-4,0.38629319164246045,0.10251580934770194,1.2438629925963186E-3,40,7.9532466543564757,0.2160270464443004,5.7103070185642202E-2,0.27437397962253895,0.38417383981767267,0.65015136281861907,0.12849982555077194,3.40784381533238E-3,2.3838596438798737E-2,8.1899806633288635E-3,3.5436420917459979E-2,0.167927211759378,3.2037924040564734E-2,7.2042602588751545E-2,4.6517068079286981E-3,0.6287953609737309,0.79940476151934114,9,0.9184231306927465,1.1204747927782288E-2,1.3520289656999133E-2,4.5570508049094811E-3,2.7999045482840008E-2,2.4326575969602772E-3,8.3576307568083909E-4,3.616180959951058E-3,7.0779893699738135E-3,1.0097332143576892E-2,3.4205391430022966E-5,7.9089954074256306E-6,7.3517325125349508E-3,8.8734903918046171E-2,0.9184231306927465,91.842313069274653,750,72.078010752951272,0.72078010752951271,309.8039832120345,null,5.8271978324516823E-3,null,0.6287953609737309,7.2042602588751545E-2,0.17019670462270683,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR81, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.842313069274653},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ81, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.6287953609737309},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA81, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.2042602588751545E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB81, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.17019670462270683},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S81, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":309.8039832120345},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P81, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.890547361795698}]
[null,null,null,null,null,null,null,76,0.76,0.43366029411764706,0.97844384891327851,0.54425002564995717,5.8892043174964819,5.8892043174964819,1,5.8892043174964819,2.3931444282857663E-6,0.25827958377594795,309935.50053113757,3.2264777616190994E-6,0,6.6E-4,0.77013030679935734,7.1172082734104664E-2,9.8989849812132283E-2,0.17212197728344902,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.33860753101986901,3.4396518019011468E-4,3.4396518019011468E-4,0.39138957473162089,0.10523864405630756,1.2443910346325172E-3,40,7.8717286858219513,0.21909413458546242,5.7127311457899274E-2,0.27746583707799422,0.39030126085674421,0.65872883838005791,0.1319127994841163,3.4092905058425139E-3,2.4295023469134477E-2,8.3113569206668125E-3,3.6015670895643802E-2,0.17212792216106121,3.2037924040564728E-2,7.2059585288650002E-2,4.6536815404750308E-3,0.63914244984693047,0.81168589575782391,9.120000000000001,0.91827310043055999,1.1361155091196149E-2,1.3704848571938402E-2,4.4982637648299691E-3,2.7937435797935343E-2,2.4462134348722953E-3,8.3685257547430972E-4,3.6263401071742886E-3,7.1661632759151984E-3,9.9670741554980461E-3,3.4633111014619825E-5,7.8036546934560013E-6,7.2555239910908984E-3,8.8842307531632983E-2,0.91827310043055999,91.827310043056002,760,72.090646982404948,0.72090646982404949,309.93550053113756,null,5.7520255933889708E-3,null,0.63914244984693047,7.2059585288650002E-2,0.17212197728344902,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR82, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.827310043056002},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ82, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.63914244984693047},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA82, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.2059585288650002E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB82, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.17212197728344902},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S82, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":309.93550053113756},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P82, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.8892043174964819}]
[null,null,null,null,null,null,null,77,0.77,0.43356139705882352,0.98844433794469078,0.55429947659755741,5.8878612731972648,5.8878612731972648,1,5.8878612731972648,2.391775673184883E-6,0.25838919913996605,310067.03896795923,3.2251090065182161E-6,0,6.6E-4,0.78000044195556206,7.3008082734104654E-2,9.9031861682612382E-2,0.17407334621872328,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.34295657350391584,3.5285763392864052E-4,3.5285763392864052E-4,0.39648980680896967,0.10799926266264549,1.2449191614563562E-3,40,7.7918648240362565,0.22216376299004628,5.7151556622574248E-2,0.28056023877407688,0.39647895592162363,0.66731279198711146,0.1353731341542887,3.410737428647552E-3,2.4751830955120804E-2,8.4330818643468548E-3,3.6595650248115209E-2,0.17638498124280552,3.2037924040564728E-2,7.2076570715458338E-2,4.6556565901039078E-3,0.64959616446999147,0.82409987176989774,9.24,0.91811489529416113,1.1518041218241707E-2,1.3889899024830187E-2,4.4409638054533204E-3,2.7877330546078619E-2,2.459418256028086E-3,8.3793702087574696E-4,3.6362566662088785E-3,7.2543082505465307E-3,9.8401111817659655E-3,3.5061022687028053E-5,7.7009815325621732E-6,7.1617503436780553E-3,8.8958778317926673E-2,0.91811489529416113,91.811489529416107,770,72.101220909974245,0.7210122090997424,310.06703896795921,null,5.6787549160641857E-3,null,0.64959616446999147,7.2076570715458338E-2,0.17407334621872328,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR83, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.811489529416107},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ83, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.64959616446999147},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA83, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.2076570715458338E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB83, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.17407334621872328},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S83, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":310.06703896795921},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P83, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.8878612731972648}]
[null,null,null,null,null,null,null,78,0.78,0.43346249999999997,0.99844482697610293,0.56434892754515753,5.8865182288980478,5.8865182288980478,1,5.8865182288980478,2.3904078593950717E-6,0.25849883210632174,310198.59852758609,3.2237411927284048E-6,0,6.5999999999999989E-4,0.7898738440098344,7.4868082734104655E-2,9.9073880299474587E-2,0.17605085745944868,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.34730866678661687,3.6186993007529181E-4,3.6186993007529181E-4,0.40159382412255723,0.11079771090691166,1.2454473730882582E-3,40,7.713605228661633,0.2252359322699356,5.7175805680604666E-2,0.28365718532362855,0.40270718665146565,0.67590311634196099,0.13888088689495542,3.4121845838034478E-3,2.5209018988399653E-2,8.5551558343517457E-3,3.7176359406554851E-2,0.18069867611583695,3.2037924040564721E-2,7.2093558869833402E-2,4.6576319568917062E-3,0.66015705359402777,0.83664728443080605,9.36,0.91794878639096633,1.167540643576186E-2,1.4075441927703571E-2,4.3850949767020751E-3,2.7818671903728873E-2,2.4722850840286632E-3,8.3901655080435681E-4,3.6459395298804927E-3,7.3424215475630158E-3,9.7163192504216428E-3,3.5489109310256192E-5,7.6008755713950053E-6,7.0703199648685109E-3,8.9084007156344694E-2,0.91794878639096633,91.794878639096638,780,72.109847935853821,0.72109847935853821,310.19859852758611,null,5.6073142559227322E-3,null,0.66015705359402777,7.2093558869833402E-2,0.17605085745944868,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR84, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.794878639096638},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ84, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.66015705359402777},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA84, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.2093558869833402E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB84, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.17605085745944868},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S84, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":310.19859852758611},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P84, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.8865182288980478}]
[null,null,null,null,null,null,null,79,0.79,0.43336360294117648,1.0084453160075153,0.57439837849275777,5.8851751845988325,5.8851751845988325,1,5.8851751845988325,2.3890409859456371E-6,0.25860848267925551,310330.17921510659,3.2223743192789703E-6,0,6.6E-4,0.79975039196668873,7.6752082734104665E-2,9.9115905664344098E-2,0.17805455770147077,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.35166374174918347,3.710021617831092E-4,3.710021617831092E-4,0.40670156604013191,0.11363403454399361,1.2459756695486529E-3,40,7.6369020417862439,0.22831064303721094,5.7200058632928444E-2,0.28675667733968802,0.40898621763274434,0.68449970939740012,0.14243611505819806,3.4136319713661727E-3,2.5666587660642379E-2,8.6775791707734504E-3,3.7757798802782003E-2,0.1850692979186237,3.2037924040564728E-2,7.2110549752432224E-2,4.6596076409148261E-3,0.67082567294471507,0.84932873625522332,9.48,0.91777503089100654,1.1833251067326297E-2,1.4261478444266043E-2,4.3306040978031129E-3,2.7761404894898162E-2,2.484826295687003E-3,8.400912965733922E-4,3.6553971479535508E-3,7.430500538211181E-3,9.5955805256206211E-3,3.5917354482185997E-5,7.5032414238429278E-6,6.9811457833972518E-3,8.9217700687642662E-2,0.91777503089100654,91.777503089100648,790,72.116619551864289,0.72116619551864292,310.33017921510657,null,5.5376356095784059E-3,null,0.67082567294471507,7.2110549752432224E-2,0.17805455770147077,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR85, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.777503089100648},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ85, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.67082567294471507},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA85, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.2110549752432224E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB85, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.17805455770147077},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S85, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":310.33017921510657},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P85, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.8851751845988325}]
[null,null,null,null,null,null,null,80,0.8,0.43326470588235289,1.0184458050389273,0.58444782944035789,5.8838321402996145,5.8838321402996145,1,5.8838321402996145,2.3876750518672197E-6,0.25871815086300887,310461.78103561065,3.2210083852005532E-6,0,6.6E-4,0.80962997069702924,7.86600827341047E-2,9.9157937778846544E-2,0.1800844943083795,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.35602173255172687,3.802544221474E-4,3.802544221474E-4,0.41181297486135271,0.11650827934347595,1.246504050857977E-3,40,7.5617092903295875,0.23138789590414899,5.7224315480483755E-2,0.28985871543549069,0.41531631643045391,0.69310247404077929,0.14603887601452054,3.4150795913917174E-3,2.6124537063549787E-2,8.8003522138131694E-3,3.8339968868754674E-2,0.1894971418628332,3.2037924040564728E-2,7.2127543363912111E-2,4.6615836422496948E-3,0.68160258529944895,0.86214483747723025,9.6000000000000014,0.91759387287500782,1.1991575622768305E-2,1.4448009977132711E-2,4.2774405880226813E-3,2.7705477216981945E-2,2.4970536605426383E-3,8.4116138234760138E-4,3.6646375541862322E-3,7.5185427038182975E-3,9.4777829325823782E-3,3.6345742489175088E-5,7.4079883674263836E-6,6.8941449850262676E-3,8.9359580354265666E-2,0.91759387287500782,91.759387287500786,800,72.121604042494241,0.72121604042494236,310.46178103561067,null,5.4696542983706607E-3,null,0.68160258529944895,7.2127543363912111E-2,0.1800844943083795,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR86, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.759387287500786},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ86, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.68160258529944895},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA86, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.2127543363912111E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB86, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.1800844943083795},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S86, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":310.46178103561067},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P86, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.8838321402996145}]
[null,null,null,null,null,null,null,81,0.81,0.4331658088235294,1.0284462940703396,0.59449728038795813,5.8824890960003993,5.8824890960003993,1,5.8824890960003993,2.3863100561917907E-6,0.25882783666182496,310593.40399418998,3.2196433895251238E-6,0,6.6E-4,0.81951247058899135,8.0592082734104675E-2,9.9199976644608195E-2,0.18214071531437123,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.36038257644050142,3.8962680420568161E-4,3.8962680420568161E-4,0.41692799564332378,0.11942049108964652,1.2470325170366729E-3,40,7.4879827941571833,0.23446769148322349,5.7248576224209098E-2,0.29296330022446926,0.42169775361977918,0.70171131780037121,0.1496892271528566,3.4165274439360901E-3,2.6582867288852154E-2,8.923475303781396E-3,3.8922870036569641E-2,0.19398250728009359,3.2037924040564728E-2,7.2144539704930483E-2,4.6635599609727626E-3,0.69248836056577612,0.87509620613160743,9.7200000000000006,0.91740554412095188,1.2150380788501813E-2,1.4635038156028035E-2,4.2255563096660767E-3,2.7650839079207717E-2,2.5089783775128047E-3,8.4222692556743287E-4,3.6736683914247188E-3,7.6065456288602947E-3,9.3628198097152771E-3,3.6774258263006268E-5,7.3150300616910323E-6,6.8092387554894405E-3,8.9509381510298316E-2,0.91740554412095188,91.740554412095193,810,72.124846875437001,0.72124846875436999,310.59340399419,null,5.4033087676049725E-3,null,0.69248836056577612,7.2144539704930483E-2,0.18214071531437123,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR87, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.740554412095193},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ87, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.69248836056577612},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA87, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.2144539704930483E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB87, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.18214071531437123},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S87, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":310.59340399419},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P87, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.8824890960003993}]
[null,null,null,null,null,"Eff (%)","Iout (mA)",82,0.82,0.43306691176470585,1.0384467831017516,0.60454673133555825,5.8811460517011831,5.8811460517011831,1,5.8811460517011831,2.3849459979526517E-6,0.25893754007994807,310725.0480959377,3.2182793312859853E-6,0,6.6E-4,0.82939778722327928,8.2548082734104633E-2,9.9242022263255694E-2,0.18422326942715553,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.36474621356847575,3.9911940093762037E-4,3.9911940093762037E-4,0.42204657603836698,0.12237071558150214,1.2475610681051898E-3,40,7.4156800795186282,0.23755003038710459,5.7272840865043237E-2,0.29607043232025304,0.42813080281823995,0.71032615257233422,0.15338722588057738,3.4179755290553149E-3,2.7041578428309204E-2,9.0469487810979493E-3,3.9506502738462471E-2,0.19852569766957356,3.2037924040564728E-2,7.2161538776145062E-2,4.6655365971605047E-3,0.70348357586111909,0.88818346813646665,9.84,0.91721026483426205,1.2309667418553796E-2,1.4822564826879631E-2,4.1749054223175885E-3,2.759744305264774E-2,2.520611108919304E-3,8.432880373427697E-4,3.6824969349004738E-3,7.6945069945232401E-3,9.2505895856472044E-3,3.7202887340903128E-5,7.224284286762297E-6,6.7263520418410451E-3,8.9666852595200464E-2,0.91721026483426205,91.721026483426201,820,72.126370778645395,0.72126370778645399,310.72504809593772,null,5.3385404001663472E-3,null,0.70348357586111909,7.2161538776145062E-2,0.18422326942715553,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR88, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.721026483426201},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ88, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.70348357586111909},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA88, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.2161538776145062E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB88, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.18422326942715553},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S88, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":310.72504809593772},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P88, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.8811460517011831}]
[null,null,null,null,null,{"$f":"BT51","v":68.427867006324419},{"$f":"I56*1000","v":500},83,0.83,0.43296801470588236,1.0484472721331639,0.61459618228315849,5.879803007401966,5.879803007401966,1,5.879803007401966,2.3835828761844313E-6,0.25904726112162402,310856.71334594884,3.2169162095177644E-6,0,6.6E-4,0.83928582107102956,8.4528082734104656E-2,9.9284074636416392E-2,0.18633220603090642,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.36911258682818165,4.0873230526497582E-4,4.0873230526497582E-4,0.42716866614304949,0.12535899863275485,1.2480897040839847E-3,40,7.344760297452666,0.24063491322865979,5.7297109403925288E-2,0.29918011233666908,0.43461574071832071,0.71894689436661696,0.15713292962349865,3.4194238468054374E-3,2.7500670573710181E-2,9.1707729862920296E-3,4.0090867406807645E-2,0.20312702074639472,3.2037924040564728E-2,7.2178540578213754E-2,4.6675135508894225E-3,0.71458881559381859,0.90140725737724436,9.9599999999999991,0.91700824432625949,1.2469436526253222E-2,1.5010592041731084E-2,4.1254442473929011E-3,2.7545243930841571E-2,2.5319620121077111E-3,8.4434482281870913E-4,3.6911301138788698E-3,7.7824245727174824E-3,9.1409954791061756E-3,3.7631615828359464E-5,7.1356727003970626E-6,6.6454133306887032E-3,8.9831754366065164E-2,0.91700824432625949,91.70082443262595,830,72.126175499523185,0.72126175499523182,310.85671334594883,null,5.2752933433195927E-3,null,0.71458881559381859,7.2178540578213754E-2,0.18633220603090642,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR89, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.70082443262595},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ89, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.71458881559381859},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA89, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.2178540578213754E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB89, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.18633220603090642},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S89, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":310.85671334594883},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P89, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.879803007401966}]
[null,null,null,null,null,{"$f":"BT81","v":72.078010752951272},{"$f":"I81*1000","v":750},84,0.84,0.43286911764705877,1.0584477611645762,0.62464563323075861,5.878459963102749,5.878459963102749,1,5.878459963102749,2.3822206899230828E-6,0.25915699979109985,310988.39974931983,3.2155540232564163E-6,0,6.6E-4,0.84917647721240619,8.6532082734104662E-2,9.9326133765717986E-2,0.18846757518925833,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.373481641695876,4.1846561005154013E-4,4.1846561005154013E-4,0.43229421835756909,0.12838538607183719,1.2486184249935193E-3,40,7.2751841468298881,0.2437223406209531,5.7321381841794632E-2,0.30229234088774126,0.44115284712058811,0.72757346307029802,0.16092639582588833,3.4208723972425185E-3,2.796014381687377E-2,9.2949482600022532E-3,4.0675964474118545E-2,0.20778678849089224,3.2037924040564728E-2,7.2195545111794657E-2,4.669490822236038E-3,0.72580467154551109,0.91476821579207535,10.08,0.91679968164511472,1.2629689276523162E-2,1.5199122049407827E-2,4.0771311421626518E-3,2.7494198600162469E-2,2.543040768855307E-3,8.4539738151566261E-4,3.6995745317936388E-3,7.8702962205075278E-3,9.033945219786739E-3,3.8060430364551658E-5,7.0491206120235515E-6,6.5663544419334186E-3,9.0003859183624982E-2,0.91679968164511472,91.679968164511479,840,72.124237241864293,0.72124237241864297,310.98839974931985,null,5.2135143476205736E-3,null,0.72580467154551109,7.2195545111794657E-2,0.18846757518925833,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR90, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.679968164511479},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ90, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.72580467154551109},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA90, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.2195545111794657E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB90, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.18846757518925833},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S90, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":310.98839974931985},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P90, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.878459963102749}]
[null,null,null,null,null,{"$f":"BT106","v":71.049894896969974},{"$f":"I106*1000","v":1000},85,0.85,0.43277022058823533,1.0684482501959882,0.63469508417835874,5.8771169188035346,5.8771169188035346,1,5.8771169188035346,2.3808594382058836E-6,0.25926675609262401,311120.10731114884,3.2141927715392167E-6,0,6.6E-4,0.85906966507430127,8.856008273410465E-2,9.9368199652788786E-2,0.19062942764834825,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.37785332608614192,4.2831940810308087E-4,4.2831940810308087E-4,0.43742318725468549,0.13144992374190873,1.2491472308542625E-3,40,7.20691380172845,0.24681231317724567,5.7345658179590954E-2,0.30540711858769087,0.44774240496730994,0.73620578222698907,0.16476768195047367,3.4223211804226376E-3,2.841999824964821E-2,9.4194749429766939E-3,4.1261794373047542E-2,0.21250531719873778,3.2037924040564728E-2,7.2212552377546063E-2,4.6714684112769004E-3,0.73713174295487061,0.92826699345857633,10.199999999999999,0.91658476616312035,1.2790426978727835E-2,1.5388157286875906E-2,4.0299263824834274E-3,2.7444265919142258E-2,2.553856612746088E-3,8.4644580764584954E-4,3.7078364849892687E-3,7.9581198749241085E-3,8.9293507885099682E-3,3.8489318090126325E-5,6.9645567723994613E-6,6.4891103367661906E-3,9.018295034767343E-2,0.91658476616312035,91.658476616312029,850,72.120507778355574,0.72120507778355569,311.12010731114884,null,5.1531526169618248E-3,null,0.73713174295487061,7.2212552377546063E-2,0.19062942764834825,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR91, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.658476616312029},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ91, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.73713174295487061},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA91, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.2212552377546063E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB91, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.19062942764834825},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S91, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":311.12010731114884},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P91, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.8771169188035346}]
[null,null,null,null,null,null,null,86,0.86,0.43267132352941173,1.0784487392274005,0.64474453512595897,5.8757738745043167,5.8757738745043167,1,5.8757738745043167,2.3794991200714295E-6,0.25937653003044642,311251.83603653568,3.212832453404763E-6,0,6.6E-4,0.86896529818564805,9.0612082734104676E-2,9.9410272299257613E-2,0.19281781483990351,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.38222759021612668,4.3829379216728183E-4,4.3829379216728183E-4,0.44255552945745119,0.13455265750086173,1.2496761216866908E-3,40,7.1399128428608041,0.24990483151099571,5.7369938418254253E-2,0.30852444605093665,0.45438470037657952,0.74484377883105046,0.16865684547844892,3.4237701964018926E-3,2.8880233963911227E-2,9.5443533760729421E-3,4.1848357536386063E-2,0.21728292753194239,3.2037924040564728E-2,7.2229562376126544E-2,4.6734463180885836E-3,0.74857063660273704,0.94190424868206213,10.32,0.9163636781237694,1.2951651080030479E-2,1.5577700371239329E-2,3.9837920535419928E-3,2.7395406606040187E-2,2.5644183546748738E-3,8.4749019040806367E-4,3.7159219801822961E-3,8.045893548127854E-3,8.8271281751388722E-3,3.8918266617172996E-5,6.8819131776432258E-6,6.4136189387846458E-3,9.0368821477963393E-2,0.9163636781237694,91.636367812376946,860,72.229662267470047,0.72229662267470052,311.25183603653568,null,5.0941596688648845E-3,null,0.74857063660273704,7.2229562376126544E-2,0.19281781483990351,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR92, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.636367812376946},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ92, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.74857063660273704},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA92, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.2229562376126544E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB92, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.19281781483990351},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S92, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":311.25183603653568},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P92, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.8757738745043167}]
[null,null,null,null,null,null,null,87,0.87,0.43257242647058824,1.0884492282588127,0.65479398607355921,5.8744308302051005,5.8744308302051005,1,5.8744308302051005,2.3781397345596364E-6,0.25948632160881824,311383.5859305819,3.2114730678929696E-6,0,6.6E-4,0.87886329394899199,9.2688082734104671E-2,9.9452351706753858E-2,0.19503278888437506,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.38660438647868617,4.4838885493368399E-4,4.4838885493368399E-4,0.44769120352506592,0.13769363322132702,1.2502050975112865E-3,40,7.07414619279026,0.25299989623585878,5.7394222558724853E-2,0.3116443238920949,0.46108002267695547,0.75348738313547836,0.17259394390948277,3.4252194452364009E-3,2.9340851051570093E-2,9.6695839002581378E-3,4.2435654397064634E-2,0.22211994457075271,3.2037924040564728E-2,7.2246575108194849E-2,4.6754245427476871E-3,0.76012196689865075,0.9556806480852138,10.44,0.9161365891518034,1.3113363159222076E-2,1.5767754092326201E-2,3.9386919479811469E-3,2.7347583134006103E-2,2.5747344066280203E-3,8.4853061426242175E-4,3.7238367507424833E-3,8.1336153228968224E-3,8.7271971528497146E-3,3.9347264001209587E-5,6.8011248865054871E-6,6.3398209671955185E-3,9.0561275936998212E-2,0.9161365891518034,91.613658915180338,870,72.361493645121143,0.72361493645121144,311.38358593058189,null,5.0364892042116553E-3,null,0.76012196689865075,7.2246575108194849E-2,0.19503278888437506,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR93, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.613658915180338},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ93, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.76012196689865075},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA93, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.2246575108194849E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB93, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.19503278888437506},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S93, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":311.38358593058189},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P93, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.8744308302051005}]
[null,null,null,null,null,null,null,88,0.88,0.4324735294117647,1.098449717290225,0.66484343702115933,5.8730877859058834,5.8730877859058834,1,5.8730877859058834,2.3767812807117365E-6,0.25959613083199201,311515.3569983904,3.2101146140450692E-6,0,6.5999999999999989E-4,0.88876357342707979,9.4788082734104662E-2,9.9494437876907302E-2,0.19727440259411796,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.39098366932376605,4.586046890336281E-4,4.586046890336281E-4,0.4528301698462342,0.14087289679067994,1.2507341583485377E-3,40,7.0095800546952329,0.25609750796568731,5.7418510601943321E-2,0.31476675272597915,0.46782866444262428,0.76213652847241964,0.17657903476172535,3.4266689269822951E-3,2.9801849604561607E-2,9.7951668566090052E-3,4.3023685388152912E-2,0.22701669786645895,3.2037924040564721E-2,7.2263590574409883E-2,4.6774030853308328E-3,0.77178635596882394,0.96959686669922984,10.56,0.91590366272911916,1.3275564920984502E-2,1.5958321405818657E-2,3.8945914708318112E-3,2.7300759633245762E-2,2.5848128038750309E-3,8.4956715918665341E-4,3.7315862718858461E-3,8.2212833484126176E-3,8.629481067484299E-3,3.9776298715023549E-5,6.7221298498487335E-6,6.2676597811609338E-3,9.0760126291451013E-2,0.91590366272911916,91.590366272911922,880,72.477313046906502,0.724773130469065,311.51535699839042,null,4.9800969856790382E-3,null,0.77178635596882394,7.2263590574409883E-2,0.19727440259411796,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR94, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.590366272911922},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ94, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.77178635596882394},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA94, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.2263590574409883E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB94, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.19727440259411796},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S94, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":311.51535699839042},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P94, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.8730877859058834}]
[null,null,null,null,null,null,null,89,0.89,0.43237463235294121,1.108450206321637,0.67489288796875957,5.8717447416066681,5.8717447416066681,1,5.8717447416066681,2.3754237575702737E-6,0.25970595770422161,311647.14924506593,3.2087570909036072E-6,0,6.6E-4,0.8986660611433327,9.6912082734104649E-2,9.9536530811348375E-2,0.19954270947661867,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.39536539514740632,4.6894138704019423E-4,4.6894138704019423E-4,0.45797239053946087,0.14409049411104638,1.2512633042189398E-3,40,6.9461818544565812,0.25919766731453131,5.7442802548850549E-2,0.31789173316760078,0.47463092152909608,0.77079115108536433,0.1806121755718163,3.4281186416957252E-3,3.0263229714852118E-2,9.9211025863119133E-3,4.361245094285976E-2,0.23197352149513029,3.2037924040564728E-2,7.2280608775430855E-2,4.679381945914665E-3,0.78356443374557194,0.98365358805648517,10.68,0.91566505463916203,1.3438258190554917E-2,1.614940542688538E-2,3.8514575507267068E-3,2.725490179964879E-2,2.5946612256935934E-3,8.5059990091535865E-4,3.7391757748634321E-3,8.3088958363219962E-3,8.5339066408207809E-3,4.0205359624225085E-5,6.6448687513940231E-6,6.1970812344294742E-3,9.0965193809236039E-2,0.91566505463916203,91.566505463916201,890,72.230234640211876,0.72230234640211877,311.64714924506592,null,4.9249407242059774E-3,null,0.78356443374557194,7.2280608775430855E-2,0.19954270947661867,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR95, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.566505463916201},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ95, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.78356443374557194},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA95, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.2280608775430855E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB95, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.19954270947661867},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S95, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":311.64714924506592},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P95, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.8717447416066681}]
[null,null,null,null,null,null,null,90,0.9,0.43227573529411761,1.1184506953530493,0.68494233891635981,5.8704016973074511,5.8704016973074511,1,5.8704016973074511,2.3740671641791044E-6,0.25981580222976247,311778.96267571498,3.207400497512438E-6,0,6.6E-4,0.90857068489516668,9.9060082734104674E-2,9.9578630511707997E-2,0.20183776373776949,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.39974952218780874,4.7939904146814422E-4,4.7939904146814422E-4,0.46311782935976498,0.1473464710993086,1.2517925351429957E-3,40,6.8839201858595169,0.26230037489663821,5.7467098400387787E-2,0.321019265832169,0.4814870931094401,0.77945118997214036,0.18469342389489163,3.429568589432865E-3,3.0724991474437573E-2,1.0047391430662925E-2,4.4201951494533362E-2,0.2369907541122945,3.2037924040564728E-2,7.2297629711917138E-2,4.6813611245758602E-3,0.79545683805822753,0.99785150428471958,10.8,0.9154209133822101,1.3601444908760947E-2,1.6341009424279032E-2,3.8092585569166268E-3,2.7209976809386173E-2,2.604287014739839E-3,8.5162891116352267E-4,3.7466102602223962E-3,8.3964510570529068E-3,8.4404037867016057E-3,4.0634435964381909E-5,6.5692848588756837E-6,6.1280335394677775E-3,9.1176307989514094E-2,0.9154209133822101,91.542091338221013,900,72.8349974854723,0.72834997485472297,311.77896267571498,null,4.8709799728804013E-3,null,0.79545683805822753,7.2297629711917138E-2,0.20183776373776949,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR96, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.542091338221013},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ96, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.79545683805822753},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA96, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.2297629711917138E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB96, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.20183776373776949},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S96, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":311.77896267571498},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P96, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.8704016973074511}]
[null,null,null,null,null,null,null,91,0.91,0.43217683823529413,1.1284511843844616,0.69499178986395993,5.869058653008234,5.869058653008234,1,5.869058653008234,2.3727114995833953E-6,0.25992566441287118,311910.7972954454,3.2060448329167292E-6,0,6.6E-4,0.9184773755792095,0.10123208273410467,9.9620736979617569E-2,0.20415962028519002,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.40413601042795094,4.8997774477386265E-4,4.8997774477386265E-4,0.46826645161133867,0.15064087368711118,1.2523218511412133E-3,40,6.8227647587164197,0.26540563132645278,5.7491398157496494E-2,0.32414935133509049,0.48839748171106906,0.78811658673791396,0.18882283730459162,3.4310187702498995E-3,3.118713497534345E-2,1.0174033731067813E-2,4.4792187476661166E-2,0.24206873900858047,3.2037924040564728E-2,7.2314653384528305E-2,4.6833406213911133E-3,0.80746421472556884,1.0121913162027871,10.92,0.91517138056374214,1.3765127127399069E-2,1.6533136814864544E-2,3.767964221651657E-3,2.7165953239027131E-2,2.6136971951660104E-3,8.5265425783547725E-4,3.7538945102093373E-3,8.4839473363657082E-3,8.3489054390489068E-3,4.1063517319615825E-5,6.4953238848189582E-6,6.060467140376123E-3,9.1393306123148402E-2,0.91517138056374214,91.517138056374208,910,73.305168165960453,0.73305168165960455,311.91079729544538,null,4.8181760276864334E-3,null,0.80746421472556884,7.2314653384528305E-2,0.20415962028519002,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR97, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.517138056374208},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ97, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.80746421472556884},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA97, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.2314653384528305E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB97, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.20415962028519002},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S97, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":311.91079729544538},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P97, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.869058653008234}]
[null,null,null,null,null,null,null,92,0.92,0.43207794117647058,1.1384516734158736,0.70504124081156005,5.8677156087090179,5.8677156087090179,1,5.8677156087090179,2.3713567628296187E-6,0.26003554425780584,312042.65310936701,3.2046900961629518E-6,0,6.5999999999999989E-4,0.92838606702754445,0.10342808273410467,9.966285021670912E-2,0.2065083347315981,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.40852482150427438,5.0067758935529779E-4,5.0067758935529779E-4,0.47341822406571515,0.15397374782086704,1.2528512522341087E-3,40,6.7626863497304903,0.26851343721861765,5.7515701821118523E-2,0.3272819902919703,0.49536239325308434,0.79678728545746169,0.19300047339306786,3.4324691842030374E-3,3.164966030962487E-2,1.0301029829042133E-2,4.5383159322870043E-2,0.24720782416633955,3.2037924040564721E-2,7.2331679793924186E-2,4.6853204364371466E-3,0.81958721764978515,1.026673733417993,11.040000000000001,0.91491659125789759,1.3929307004930823E-2,1.6725791158546627E-2,3.7275455675269899E-3,2.7122800990763567E-2,2.6228984895790182E-3,8.5367600522039415E-4,3.7610331003799214E-3,8.5713830521219978E-3,8.2593473908802468E-3,4.149259360255167E-5,6.4229338562225104E-6,5.9943345939325061E-3,9.1616032881340861E-2,0.91491659125789759,91.491659125789766,920,73.638455592594738,0.73638455592594743,312.042653109367,null,4.7664918345999467E-3,null,0.81958721764978515,7.2331679793924186E-2,0.2065083347315981,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR98, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.491659125789766},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ98, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.81958721764978515},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA98, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.2331679793924186E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB98, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.2065083347315981},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S98, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":312.042653109367},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P98, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.8677156087090179}]
[null,null,null,null,null,null,null,93,0.93,0.43197904411764709,1.1484521624472859,0.71509069175916029,5.8663725644098026,5.8663725644098026,1,5.8663725644098026,2.3700029529655522E-6,0.26014544176882576,312174.53012259089,3.2033362862988858E-6,0,6.6E-4,0.93829669585418041,0.10564808273410468,9.9704970224615067E-2,0.20888396339822754,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.41291591862101157,5.1149866755190155E-4,5.1149866755190155E-4,0.47857311488504656,0.15734513946176309,1.2533807384422025E-3,40,6.7036567559328013,0.27162379318797247,5.7540009392195952E-2,0.33041718331861064,0.50238213708418533,0.80546323254604379,0.19722638977099075,3.4339198313485001E-3,3.2112567569366493E-2,1.0428380066211249E-2,4.5974867466926236E-2,0.25240836231726543,3.2037924040564728E-2,7.2348708940764769E-2,4.6873005697907026E-3,0.83182650891200616,1.0412994744250399,11.16,0.91465667434786824,1.4093986802473608E-2,1.6918976153568011E-2,3.6879748394267804E-3,2.7080491222364726E-2,2.6318973349254448E-3,8.5469421417530317E-4,3.7680304104733648E-3,8.6587566312548957E-3,8.1716681435125126E-3,4.1921655035518652E-5,6.3520649924883109E-6,5.9295904581650348E-3,9.1844339930367683E-2,0.91465667434786824,91.465667434786823,930,73.832411821820315,0.73832411821820321,312.17453012259091,null,4.7158919025637146E-3,null,0.83182650891200616,7.2348708940764769E-2,0.20888396339822754,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR99, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.465667434786823},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ99, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.83182650891200616},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA99, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.2348708940764769E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB99, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.20888396339822754},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S99, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":312.17453012259091},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P99, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.8663725644098026}]
[null,null,null,null,null,null,null,94,0.94,0.43188014705882349,1.1584526514786981,0.72514014270676042,5.8650295201105846,5.8650295201105846,1,5.8650295201105846,2.3686500690402755E-6,0.26025535695019181,312306.4283402302,3.201983402373609E-6,0,6.6E-4,0.9482092013110146,0.10789208273410465,9.9747097004968477E-2,0.2112865633182959,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.41730926646975453,5.2244107164457375E-4,5.2244107164457375E-4,0.48373109355012556,0.16075509458576664,1.2539103097860241E-3,40,6.6456487505368482,0.2747366998495554,5.756432087167123E-2,0.33355493103101264,0.50945702602116072,0.81414437663826045,0.20150064406755733,3.4353707117425326E-3,3.2575856846682634E-2,1.0556084784310391E-2,4.6567312342735562E-2,0.25767071100103156,3.2037924040564728E-2,7.2365740825710317E-2,4.6892810215285567E-3,0.84418275886943117,1.056069266706626,11.28,0.91439175284490226,1.4259168880064895E-2,1.7112695632152081E-2,3.6492254407300695E-3,2.7038996281516681E-2,2.6406998973814494E-3,8.5570894229654087E-4,3.7748906346054987E-3,8.7460665469259909E-3,8.0858087652095414E-3,4.2350692132912323E-5,6.2826695909962658E-6,5.8661911879025856E-3,9.2078085570509227E-2,0.91439175284490226,91.439175284490233,940,73.8844086186851,0.73884408618685105,312.30642834023018,null,4.6663422219125755E-3,null,0.84418275886943117,7.2365740825710317E-2,0.2112865633182959,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR100, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.439175284490233},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ100, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.84418275886943117},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA100, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.2365740825710317E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB100, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.2112865633182959},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S100, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":312.30642834023018},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P100, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.8650295201105846}]
[null,null,null,null,null,null,null,95,0.95,0.43178125000000001,1.1684531405101102,0.73518959365436065,5.8636864758113694,5.8636864758113694,1,5.8636864758113694,2.3672981101041701E-6,0.26036528980616613,312438.34776739933,3.2006314434375032E-6,0,6.6E-4,0.95812352515261423,0.11016008273410466,9.9789230559402864E-2,0.21371619224052088,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.42170483115389251,5.3350489385559899E-4,5.3350489385559899E-4,0.48889213079281268,0.16420365918363092,1.2544399662861084E-3,40,6.5886360410654312,0.27785215781860184,5.7588636260487047E-2,0.33669523404537499,0.51658737638796171,0.82283066847432362,0.20582329393049831,3.4368218254413928E-3,3.3039528233717218E-2,1.0684144325184684E-2,4.7160494384343297E-2,0.26299523262496238,3.2037924040564728E-2,7.2382775449421233E-2,4.6912617917275017E-3,0.8566566462540729,1.0709838468357038,11.399999999999999,0.91412194418747106,1.4424855693180234E-2,1.7306953556465669E-2,3.611271873470605E-3,2.6998289644229283E-2,2.649312086319511E-3,8.5672024408047019E-4,3.7816177908296675E-3,8.8333113158554754E-3,8.0017127585906272E-3,4.2779695684632505E-5,6.2147019197708676E-6,5.804095036799131E-3,9.2317134397425074E-2,0.91412194418747106,91.412194418747106,950,73.791636151568156,0.73791636151568152,312.43834776739931,null,4.6178101878545192E-3,null,0.8566566462540729,7.2382775449421233E-2,0.21371619224052088,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR101, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.412194418747106},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ101, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.8566566462540729},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA101, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.2382775449421233E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB101, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.21371619224052088},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S101, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":312.43834776739931},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P101, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.8636864758113694}]
[null,null,null,null,null,null,null,96,{"$f":"IF(PLOT_TYPE=1, H102/100*Iout, min_I*EXP(H102*rr/100))","v":0.96},{"$f":"IF(I102<Icrit, (Vin-(Rdcr+RdsonTop)*Iripple/2-Vout)/L*OnTime, (Vin-(Rdcr+RdsonTop)*I102-Vout)/L*OnTime)","v":0.43168235294117646},{"$f":"IF(I102<Icrit, (Vin-(Rdcr+RdsonTop)*Iripple/2-Vout)/L*OnTime, I102+((Vin-(Rdcr+RdsonTop)*J102-Vout)/L*OnTime)/2)","v":1.1784536295415224},{"$f":"IF(I102<Icrit, 0, I102-((Vin-(Rdcr+RdsonTop)*K102-Vout)/L*OnTime)/2)","v":0.74523904460196078},5.8623434315121523,{"$f":"IF(I102<Icrit, 1000*SQRT((J102*CoutEsr)^2+(((J102/2)-I102)*(OnTime+OffTime)/Cout)^2), 1000*J102*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":5.8623434315121523},1,{"$f":"IF(I102<Icrit, 1000*((N102/1000)*O102), 1000*J102*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":5.8623434315121523},2.3659470752089133E-6,0.26047524034101216,312570.28840921458,3.1992804085422469E-6,0,{"$f":"S102*(T102*Iq_active+U102*Iq_sleep)","v":6.6E-4},0.96803961150919449,{"$f":"W102^2*Rdcr","v":0.11245208273410466},{"$f":"Core_Loss/1000*S102/$S$106","v":9.9831370889552282E-2},{"$f":"(Y102+X102*(1+Ltc*(Ta-25)))/(1-X102*Ltc*ThetaCa)","v":0.21617290863268654},0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.42610258011758573,5.4469022634859071E-4,5.4469022634859071E-4,0.49405619853255978,0.16769087926090112,1.2549697079629967E-3,{"$f":"20*VIN_nom/24","v":40},6.532593229614573,{"$f":"IF(I102<Icrit, Vin*(I102+Iripple/2)*AK102/1000000000/2*S102, Vin*(I102-Iripple/2)*AJ102/1000000000/2*S102 + Vin*(I102+Iripple/2)*AK102/1000000000/2*S102)","v":0.28097016771054517},5.7612955559586433E-2,0.33983809297809464,{"$f":"(AI102+AL102+AM102+AH102*(1+RdsonTopTc*(Ta-25)))/(1-AH102*RdsonTopTc*ThetaJA)","v":0.5237735080553747},0.83152206079322266,0.21019439702608561,3.4382731725013608E-3,{"$f":"IF(I102<Icrit, Vin*Idss*R102, QrrBot*(I102-Iripple/2)/1*S102*Vin+Vin*Idss*R102)","v":3.3503581822643805E-2},1.0812559030789211E-2,4.7754414025934375E-2,{"$f":"(AR102+AS102+AT102+AQ102*(1+RdsonBotTc*(Ta-25)))/(1-AQ102*RdsonBotTc*ThetaJA)","v":0.26838229452476176},{"$f":"Vin*V102+Vout*Ifb/0.8","v":3.2037924040564728E-2},{"$f":"(Vin-Vdd)*(S102*QgBot+S102*QgTop)+AW102","v":7.2399812812558209E-2},4.6932428804643579E-3,0.86924885827315912,{"$f":"SUM(Z102,AC102,AF102,AZ102)","v":1.0860439605794485},11.52,0.91384736052201365,1.4591049789487272E-2,1.7501754014880178E-2,3.5740896821675715E-3,2.6958345857019658E-2,2.6577395674180866E-3,8.5772817107423462E-4,3.7882157301107251E-3,8.9204894958129031E-3,7.9193259361728767E-3,4.3208656740520639E-5,6.1481181167322216E-6,5.7432619653684184E-3,9.2561356984369209E-2,0.91384736052201365,91.384736052201362,960,73.551124384272143,0.73551124384272137,312.57028840921458,null,4.5702645286458451E-3,null,0.86924885827315912,7.2399812812558209E-2,0.21617290863268654,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR102, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.384736052201362},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ102, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.86924885827315912},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA102, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.2399812812558209E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB102, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.21617290863268654},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S102, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":312.57028840921458},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P102, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.8623434315121523}]
[null,null,null,null,null,null,null,97,{"$f":"IF(PLOT_TYPE=1, H103/100*Iout, min_I*EXP(H103*rr/100))","v":0.97},0.43158345588235297,1.1884541185729347,0.75528849554956101,5.8610003872129361,5.8610003872129361,1,5.8610003872129361,2.3645969634074812E-6,0.26058520855899481,312702.2502707938,{"$f":"IF(1/S103-OnTime-Q103>Tsleep, OnTime+Q103+Tsleep, 1/S103)","v":3.1979302967408143E-6},0,6.6E-4,0.97795740676722331,0.11476808273410467,9.9873517997051325E-2,0.2186567716852594,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.43050248207895792,5.5599716122843037E-4,5.5599716122843037E-4,0.49922326981674436,{"$f":"RdsonTop*AG103^2","v":0.1712168008379206},1.2554995348372372E-3,40,6.4774957751282969,0.28409073014101682,5.763727876991271E-2,0.34298350844576675,0.53101574448130029,0.84021850823230382,{"$f":"RdsonBot*AP103^2","v":0.21461401103913985},3.4397247529787322E-3,3.3968017705665619E-2,1.0941329243189036E-2,4.834907170183339E-2,0.2738322690263148,3.2037924040564728E-2,7.2416852915782065E-2,4.6952242878159694E-3,0.88196009071121306,1.1012503630049553,11.64,0.91356810896656526,1.4757753805819349E-2,1.7697101218510428E-2,3.5376554010671532E-3,2.6919140482604562E-2,2.6659877749748923E-3,8.587327720172499E-4,3.7946881447536774E-3,9.007599683257244E-3,7.8385963034711681E-3,4.3637566595724713E-5,6.0828760950650174E-6,5.6836535546031719E-3,9.2810629583769691E-2,0.91356810896656526,91.356810896656526,970,73.159788011658193,0.73159788011658189,312.7022502707938,null,4.5236752381278278E-3,null,0.88196009071121306,7.2416852915782065E-2,0.2186567716852594,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR103, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.356810896656526},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ103, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.88196009071121306},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA103, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.2416852915782065E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB103, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.2186567716852594},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S103, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":312.7022502707938},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P103, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.8610003872129361}]
[null,null,null,null,null,null,null,98,{"$f":"IF(PLOT_TYPE=1, H104/100*Iout, min_I*EXP(H104*rr/100))","v":0.98},0.43148455882352937,1.1984546076043467,0.76533794649716125,5.8596573429137191,5.8596573429137191,1,5.8596573429137191,2.3632477737541393E-6,0.2606951944643805,312834.23335725657,{"$f":"IF(1/S104-OnTime-Q104>Tsleep, OnTime+Q104+Tsleep, 1/S104)","v":3.1965811070874729E-6},0,6.600000000000001E-4,0.98787685945712489,0.11710808273410464,9.9915671883535145E-2,0.22116784131505529,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.43490450696722277,5.6742579054120941E-4,5.6742579054120941E-4,0.50439331876455118,{"$f":"RdsonTop*AG104^2","v":0.17478146994983657},1.2560294469293851E-3,40,6.423319957566533,0.2872138457258463,5.7661605892409533E-2,0.34613148106518521,0.53831441275164849,0.84891996723282026,{"$f":"RdsonBot*AP104^2","v":0.21908219367303805},3.4411765669298227E-3,3.4432835975015529E-2,1.1070455304559275E-2,4.8944467846504622E-2,0.27934553350858687,3.2037924040564734E-2,7.2433895759753925E-2,4.6972060138592078E-3,0.89479104803384857,1.1166038185866993,11.76,0.91328429185846816,1.4924970465353399E-2,1.7892999498012856E-2,3.5019465045557103E-3,2.6880650048855481E-2,2.6740619234796635E-3,8.5973409297408505E-4,3.8010385763252159E-3,9.0946405111156179E-3,7.7594739491256342E-3,4.4066416776926862E-5,6.0189354542763192E-6,5.6252329247871566E-3,9.306483384681602E-2,0.91328429185846816,91.328429185846815,980,72.614496083320674,0.72614496083320679,312.83423335725655,null,4.4780135123189896E-3,null,0.89479104803384857,7.2433895759753925E-2,0.22116784131505529,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR104, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.328429185846815},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ104, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.89479104803384857},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA104, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.2433895759753925E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB104, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.22116784131505529},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S104, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":312.83423335725655},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P104, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.8596573429137191}]
[null,null,null,null,null,null,null,99,{"$f":"IF(PLOT_TYPE=1, H105/100*Iout, min_I*EXP(H105*rr/100))","v":0.99},0.43138566176470594,1.208455096635759,0.77538739744476137,5.8583142986145038,5.8583142986145038,1,5.8583142986145038,2.3618995053044507E-6,0.26080519806143654,312966.23767372384,{"$f":"IF(1/S105-OnTime-Q105>Tsleep, OnTime+Q105+Tsleep, 1/S105)","v":3.1952328386377839E-6},0,6.6E-4,0.99779792014759794,0.11947208273410466,9.9957832550639281E-2,0.22370617816895705,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.43930862586347658,5.7897620627416814E-4,5.7897620627416814E-4,0.50956632051415796,{"$f":"RdsonTop*AG105^2","v":0.17838493264660593},1.2565594442600012E-3,40,6.3700428438562522,0.29033951508106109,5.7685936928020778E-2,0.34928201145334187,0.54566984362186,0.85762639595104329,{"$f":"RdsonBot*AP105^2","v":0.2235990026497206},3.4426286144109627E-3,3.4898036722956056E-2,1.1199937557185097E-2,4.9540602894552116E-2,0.28492247046763702,3.2037924040564728E-2,7.2450941345135023E-2,4.6991880586709639E-3,0.90774244349330313,1.1321051013157888,11.879999999999999,0.9129960069872699,1.5092702574978382E-2,1.8089453300625662E-2,3.4669413605243242E-3,2.6842852000789817E-2,2.6819670184978109E-3,8.6073217745932253E-4,3.8072704231033728E-3,9.1816106466911032E-3,7.6819109415686721E-3,4.4495199029373189E-5,5.9562573965471698E-6,5.5679646591394938E-3,9.3323856559803881E-2,0.9129960069872699,91.299600698726991,990,71.912167665597565,0.71912167665597559,312.96623767372381,null,4.4332516897813527E-3,null,0.90774244349330313,7.2450941345135023E-2,0.22370617816895705,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR105, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.299600698726991},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ105, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.90774244349330313},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA105, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.2450941345135023E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB105, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.22370617816895705},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S105, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":312.96623767372381},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P105, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.8583142986145038}]
[null,null,null,null,null,null,null,100,{"$f":"IF(PLOT_TYPE=1, H106/100*Iout, min_I*EXP(H106*rr/100))","v":1},0.43128676470588234,1.2184555856671713,0.78543684839236161,5.8569712543152859,5.8569712543152859,1,5.8569712543152859,2.3605521571152607E-6,0.26091521935443224,313098.26322531869,{"$f":"IF(1/S106-OnTime-Q106>Tsleep, OnTime+Q106+Tsleep, 1/S106)","v":3.1938854904485943E-6},0,6.6E-4,1.0077205413460977,0.12186008273410466,0.1,0.22627184362768354,0.12450176485043199,7.750344725436132E-5,7.750344725436132E-5,0.44371481094491316,5.906485003556401E-4,5.906485003556401E-4,0.51474225117300354,{"$f":"RdsonTop*AG106^2","v":0.18202723499300155},1.2570895268496545E-3,40,6.3176422555231291,0.29346773882288707,5.771027187769074E-2,0.35243510022742747,0.55308237155906781,0.86633775417456038,{"$f":"RdsonBot*AP106^2","v":0.22816449570969916},3.444080895478506E-3,3.5363620041779453E-2,1.1329776343461832E-2,5.0137477280719794E-2,0.29056346758177071,3.2037924040564728E-2,7.2467989672586913E-2,4.7011704223281605E-3,0.92081499923575372,1.1477549948110473,12,0.91270334781382634,1.5260953022841445E-2,1.8286467187435311E-2,3.4326191864818023E-3,2.6805724655389541E-2,2.6897078669123526E-3,8.6172706655495888E-4,3.8133869470877179E-3,9.2685087896905993E-3,7.6058612317818873E-3,4.4923905304650726E-5,5.8948046480139902E-6,5.5118147319589894E-3,{"$f":"SUM(BD106:BO106)","v":9.3587589396087259E-2},0.91270334781382634,91.27033478138263,1000,71.049894896969974,0.71049894896969978,313.0982632253187,null,4.3893631955012049E-3,null,0.92081499923575372,7.2467989672586913E-2,0.22627184362768354,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR106, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.27033478138263},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ106, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.92081499923575372},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA106, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.2467989672586913E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB106, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.22627184362768354},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S106, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":313.0982632253187},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P106, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.8569712543152859}]
[null,null,null,null,null,null,null,null,{"$f":"Losses!$E$5/1000","v":0.5},0.43623161764705881,0.71843113409656145,0.28296430101235248,5.9241234692761084,5.9241234692761084,1,5.9241234692761084,{"$f":"IF(I107<Icrit, L*J107/(Vout+J107/2*(RdsonBot+Rdcr)), L*J107/(Vout+I107*(RdsonBot+Rdcr)))","v":2.4290656731084177E-6},{"$f":"OnTime*S107","v":0.25543574887310838},{"$f":"IF(I107<Icrit,I107/((OnTime+Q107)*J107/2),1/(OnTime+Q107))","v":306522.89864773006},{"$f":"IF(1/S107-OnTime-Q107>Tsleep, OnTime+Q107+Tsleep, 1/S107)","v":3.2623990064417509E-6},{"$f":"IF(1/S107-OnTime-Q107>Tsleep, 1/S107-OnTime-Q107-Tsleep, 0)","v":0},6.6E-4,{"$f":"IF(I107<Icrit,Iripple*SQRT((OnTime+OffTime)*S107/3), SQRT(I107^2+Iripple^2/12))","v":0.51526759014212431},3.1860082734104664E-2,9.7899903848123013E-2,0.13042484198321452,{"$f":"Iripple/SQRT(12)*SQRT((OnTime+Q107)*S107)","v":0.12450176485043199},{"$f":"RCoutEsr*AA107^2","v":7.750344725436132E-5},{"$f":"AB107","v":7.750344725436132E-5},{"$f":"SQRT($R107)*SQRT($I107^2*(1-R107)+(Iripple^2)/12)","v":0.2269504615232556},{"$f":"RCinEsr*AD107^2","v":1.5451953595685614E-4},{"$f":"AE107","v":1.5451953595685614E-4},{"$f":"IF(I107<Icrit,Iripple*SQRT((OnTime)*S107/3), SQRT(OnTime*S107*(I107^2+Iripple^2/12)))","v":0.26041959879434984},{"$f":"RdsonTop*AG107^2","v":4.6591218428676369E-2},{"$f":"QgTop*S107*Vdd","v":1.2306894380706361E-3},40,{"$f":"IF(I107<Icrit, Csw*Vin/Iripple*1000000000, Csw*Vin/(I107+Iripple/2)*1000000000)","v":10.731602065192263},0.14017364278195671,{"$f":"IF(I107<Icrit, Csw*(Vin)^2*S107/2, Csw*Vin^2*S107/2)","v":5.6498300678749606E-2},0.19790263289877696,0.24661897837115918,{"$f":"IF(I107<Icrit,Iripple*SQRT((OffTime)*S107/3), SQRT(OffTime*S107*(I107^2+Iripple^2/12)))","v":0.4382996147069918},{"$f":"RdsonBot*AP107^2","v":5.8400391884698429E-2},{"$f":"QgBot*S107*Vdd","v":3.3717518851250315E-3},1.2551301315481069E-2,{"$f":"IF(I107<Icrit, dead1*S107*(I107+Iripple/2)*((I107+Iripple/2)*BDserR+VSD), dead1*S107*(I107+Iripple/2)*((I107+Iripple/2)*BDserR+VSD)+dead2*S107*(I107-Iripple/2)*((I107-Iripple/2)*BDserR+VSD))","v":5.2679050721496472E-3},2.1190958272755748E-2,8.0460415372421407E-2,3.2037924040564728E-2,7.1618919420047472E-2,{"$f":"AI107+AR107","v":4.6024413231956678E-3},{"$f":"AO107+AV107+AX107+AY107","v":0.40330075448682368},0.53395761945324938,{"$f":"Vout*I107","v":6},{"$f":"BB107/(BB107+BA107)","v":0.91827960165160505},7.4558710523835187E-3,9.0709889092646465E-3,{"$f":"Vin*S107*(QgBot+QgTop)/($BB107+$BA107)","v":6.7621247758224076E-3},3.0288325150682124E-2,{"$f":"AS107/(BA107+BB107)","v":1.9209339953648705E-3},{"$f":"AT107/($BB107+$BA107)","v":8.0623496186534136E-4},3.2432041202203224E-3,{"$f":"X107/($BB107+$BA107)","v":4.8760773469434691E-3},{"$f":"Y107/($BB107+$BA107)","v":1.4983247451230806E-2},{"$f":"(AF107)/($BB107+$BA107)","v":2.3648689654308787E-5},{"$f":"(AC107)/($BB107+$BA107)","v":1.1861639111893517E-5},1.09610321326266E-2,{"$f":"SUM(BD107:BO107)","v":9.0403550225170298E-2},{"$f":"BC107","v":0.91827960165160505},{"$f":"100*BQ107","v":91.827960165160505},{"$f":"I107*1000","v":500},72.049894896970002,{"$f":"BT107/100","v":0.72049894896970001},{"$f":"S107/1000","v":306.52289864773007},null,{"$f":"AM107/($BB107+$BA107)","v":8.6468728402124672E-3},null,0.40330075448682368,7.1618919420047472E-2,0.13042484198321452,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR107, IF(MODE_ILIM=4,#REF!,#REF!))","v":91.827960165160505},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ107, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.40330075448682368},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA107, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.1618919420047472E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB107, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.13042484198321452},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S107, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":306.52289864773007},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P107, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.9241234692761084}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(MODE=1, MODE=2,MODE=3),Efficiency!BD107,IF(AND(MODE=4,MODE_ILIM=4),#REF!,#REF!))","v":7.4558710523835187E-3},{"$f":"IF(OR(MODE=1, MODE=2,MODE=3),Efficiency!BE107,IF(AND(MODE=4,MODE_ILIM=4),#REF!,#REF!))","v":9.0709889092646465E-3},null,{"$f":"IF(OR(MODE=1, MODE=2,MODE=3),Efficiency!BG107,IF(AND(MODE=4,MODE_ILIM=4),#REF!,#REF!))","v":3.0288325150682124E-2},null,null,{"$f":"IF(OR(MODE=1, MODE=2,MODE=3),Efficiency!BJ107,IF(AND(MODE=4,MODE_ILIM=4),#REF!,#REF!))","v":3.2432041202203224E-3},{"$f":"IF(OR(MODE=1, MODE=2,MODE=3),Efficiency!BK107,IF(AND(MODE=4,MODE_ILIM=4),#REF!,#REF!))","v":4.8760773469434691E-3},{"$f":"IF(OR(MODE=1, MODE=2,MODE=3),Efficiency!BL107,IF(AND(MODE=4,MODE_ILIM=4),#REF!,#REF!))","v":1.4983247451230806E-2},null,null,{"$f":"IF(OR(MODE=1, MODE=2,MODE=3),Efficiency!BO107,IF(AND(MODE=4,MODE_ILIM=4),#REF!,#REF!))","v":1.09610321326266E-2}]
[null,null,null,null,null,null,null,1.0000000000000001E-5,"A","min_I",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Load (A)","High-side MOSFET Rdson %","Low-side MOSFET Rdson %","Gate Drive (Qg) Loss from Vin %","High-side MOSFET Switching Loss %","Reverse Recovery & Leakage Loss %","Deadtime Loss %",null,"Inductor Cu Loss %","Inductor Core Loss %","Cin ESR %","Cout ESR %","Quiescent Current Loss %","Total Loss %","Overall Eff %"]
[null,null,null,null,null,null,null,{"$f":"Iout","v":1},"A","max_I",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"I107","v":0.5},{"$f":"BD107","v":7.4558710523835187E-3},{"$f":"BE107","v":9.0709889092646465E-3},6.7621247758224076E-3,3.0288325150682124E-2,1.9209339953648705E-3,8.0623496186534136E-4,null,4.8760773469434691E-3,1.4983247451230806E-2,2.3648689654308787E-5,1.1861639111893517E-5,1.09610321326266E-2,9.0403550225170298E-2,0.91827960165160505]
[null,null,null,null,null,null,null,{"$f":"LOG(max_I/min_I,EXP(1))","v":11.512925464970229},null,"rr",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"10mA",{"$f":"BD70","v":9.5160806535960624E-3},{"$f":"BE70","v":1.1522622321301981E-2},5.3212612587800467E-3,2.8796082713170305E-2,2.2558565728194122E-3,8.233959349352889E-4,null,6.1070979123567688E-3,1.1790639308818828E-2,2.9518963641600649E-5,9.2786084307653492E-6,8.6025003727297489E-3,8.825966628422531E-2,0.91943926719037539]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"50ma",{"$f":"BD85","v":1.1833251067326297E-2},{"$f":"BE85","v":1.4261478444266043E-2},4.3306040978031129E-3,2.7761404894898162E-2,2.484826295687003E-3,8.400912965733922E-4,null,7.430500538211181E-3,9.5955805256206211E-3,3.5917354482185997E-5,7.5032414238429278E-6,6.9811457833972518E-3,8.9217700687642662E-2,0.91777503089100654]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"100mA",{"$f":"BD91","v":1.2790426978727835E-2},{"$f":"BE91","v":1.5388157286875906E-2},4.0299263824834274E-3,2.7444265919142258E-2,2.553856612746088E-3,8.4644580764584954E-4,null,7.9581198749241085E-3,8.9293507885099682E-3,3.8489318090126325E-5,6.9645567723994613E-6,6.4891103367661906E-3,9.018295034767343E-2,0.91658476616312035]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"500mA",{"$f":"BD106","v":1.5260953022841445E-2},{"$f":"BE106","v":1.8286467187435311E-2},3.4326191864818023E-3,2.6805724655389541E-2,2.6897078669123526E-3,8.6172706655495888E-4,null,9.2685087896905993E-3,7.6058612317818873E-3,4.4923905304650726E-5,5.8948046480139902E-6,5.5118147319589894E-3,9.3587589396087259E-2,0.91270334781382634]

{"sheet":"Schematic Mgmt","index":10,"n_rows":2,"n_cols":1,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
[]
[{"$f":"'Variable Mgmt'!K27","v":"SCH_COT3_LM5164"}]

{"sheet":"Efficiency Plots","index":11,"n_rows":2,"n_cols":1,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
[]
[{"$f":"IF(PLOT_TYPE=1, \"EFF_LINEAR\", \"EFF_LOG\")","v":"EFF_LINEAR"}]