Just USB-C Cable Attached – showing CC lines add Rd fixed resistor

TI TPS25751EVM

Vbus=0V , CC-yellow = open Vbus=5V, CC- Yellow = 3V **State -Attached.SRC**

 

Custom design

 

Vbus=9V , CC-yellow = open Vbus=9V, CC- Yellow = open **STATE Attach.Wait.Src**