{"text_format":"1","workbook":"xlsx","n_sheets":12,"sheets":["Instructions","Design Converter","BOM & Schematic","Fsw & Ripple","Losses","EVM","Design EMI Filter","Variable Mgmt","Standard Value Calculator","Efficiency","Schematic Mgmt","Efficiency Plots"],"not_rendered":{"charts":6,"images":26,"macros":1,"external_links":0,"defined_names":205,"comments":4,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Instructions","index":0,"n_rows":74,"n_cols":3,"rows_kept":74,"cut":false,"hidden":true,"merged":[[0,0,0,16],[7,1,9,15],[16,2,17,15],[11,1,14,15],[18,2,19,15],[65,1,66,15],[69,1,70,15],[73,1,74,15],[77,1,78,15],[20,2,21,15],[50,1,52,15],[54,1,55,15],[56,1,57,15],[60,1,62,15],[24,1,26,15],[38,1,39,15],[41,1,43,15],[46,1,47,15],[28,1,28,15],[29,1,31,15],[33,1,35,15]]}
["                         LM5164 Low IQ DC/DC Converter Design Tool  "]
[]
[]
[null,"Design Regulator tab"]
[null,"Start with Step 1, and then work down towards the bottom of the worksheet."]
[]
[null,"Step 1. Operating Specifications"]
[null,"First, enter the values in the yellow shaded cells to define the power supply parameters.  If a particular specification is not known, enter an estimate. It can be changed later, if necessary, to optimize component values.  Cells  with a red mark in the upper right corner have a comment to provide additional information.  Hold the cursor over the cell to read the comment.  A red font indicates an erroneous entry and requires an adjustment to the entry.  Consult the entry's comments for the entry specific requirements."]
[]
[]
[]
[null,"Second, select a desired mode of operation. PFM mode requires the fewest external components and the lowest inductance.  As a result, it can provide the smallest solution size. At light loads, a PFM converter has a relatively longer sleep time interval and thus operates at lower input quiescent current levels.  COT mode offers nearly constant switching frequency, relatively higher conversion efficiencies at medium to heavy loads, and enables the lowest output voltage ripple.  Options COT1, COT2, and COT3 enable you to select a ripple generation method (a requirement for the stable operation in COT mode):"]
[]
[]
[]
[]
[null,"-COT1: ","Type 1 ripple generation method requires a single resistor in series with the output capacitor.  It is the simplest, the most compact, and the most economical method that works with fixed and adjustable device options, however, the output voltage ripple is the highest."]
[]
[null,"-COT2: ","Type 2 ripple generation method requires a feedforward capacitor in addition to the series resistor.  The feedforward capacitor reduces the required minimum value of the series resistor and ultimately the output voltage ripple by the VOUT / 1.223V factor.  It only works with an adjustable device option (i.e. external feedback resistor network)."]
[]
[null,"-COT3:","Type 3 ripple generation method three external components to generate and inject required voltage ripple into the FB node.  In return, it provides the lowest output voltage ripple. It also only works with an adjustable device option (i.e. external feedback resistor network)."]
[]
[]
[null,"Step 2. Filter Inductor"]
[null,"First, select an inductor current limit level.  In PFM Mode, 1.25A, 0.75A, 0.5A, and 1.25A - MOD options are available.  For the 500mA max load, select either 1.25A or 1.25A - MOD option.  The 1.25A - MOD option enables higher efficiency at the expense of slightly worse transient operation.  For the 300mA and 200mA max loads, select 0.75A and 0.5A options respectively. In COT Mode, 0.75A and 0.5A options are available.   For the 500mA and 300mA max loads, select 0.75A and 0.5A options respectively."]
[]
[]
[]
[null,"Second, select the filter inductance value based on the suggested value. Enter the inductor RDC for accurate efficiency estimates."]
[null,"In PFM mode, selected inductance defines the switching frequency.  You may select lower or higher inductance to increase or decrease the switching frequency.  Watch the minimum output capacitance.  At very low switching frequencies, the required minimum capacitance may become excessive."]
[]
[]
[]
[null,"In COT mode, the suggested inductance is  derived based on the target inductor (peak-to-peak) ripple current of 40% of the DC full load output current at nominal input voltage. It may be acceptable to use higher ripple current with the proviso that peak inductor current remains below the ILIM setting.  Pk-to-Pk Ripple Current value will turn red if this is violated.  If this happens, increase the selected inductance or decrease the Input Voltage (max) or both."]
[]
[]
[]
[null,"Step 3. Output Capacitors and Ripple Generation"]
[null,"First, select the output capacitance based on the minimum recommended value.  Make sure that the nominal capacitance is appropriately derated for applied voltage, especially with ceramics.  For PFM and COT3 modes, ensure that the capacitor ESR does not exceed the maximum allowable value.  "]
[]
[]
[null,"Second, for COT modes, select the values for the ripple generation components based on the minimum recommended values.  Ensure that the output voltage ripple meets any of your minimum ripple requirements by reviewing the VOUT Ripple vs. IOUT plot in the fSW&Ripple tab.  For accurate output voltage ripple estimates in COT3 mode, ensure that the Output Capacitor ESR is set to the levels of a typical ceramic capacitor ESR (e.g. 10 mW)."]
[]
[]
[]
[null,"Step 4. Input Capacitors"]
[null,"Select the input capacitance based on the minimum recommended value.  Make sure that the nominal capacitance is appropriately derated for applied voltage, especially with ceramics.  "]
[]
[]
[null,"Step 5. Feedback, Soft-Start, UVLO"]
[null,"First, review the feedback resistor network. With an adjustable device option, an external feedback resistor network is required. The resistor values are automatically calculated based on the selected VOUT in Step 1.  For lowering the leakage current through the resistors, adjust the upper FB resistor (R1) until the lower FB resistor (R2) reaches its upper end of the range (100kW).  Keeping the upper FB resistor below 1MW is recommended."]
[]
[]
[]
[null,"Second, select one out of three soft-start configurations.  If the external soft-start option is selected, enter a desired soft start time.  "]
[]
[null,"Third, select one out of the two UVLO options.  If the external UVLO option is selected, define desired UVLO thresholds and hysteresis.  Keeping the upper UVLO resistor at 1MW or higher is recommended for the minimum leakage current."]
[]
[]
[null,"Step 6. Efficiency and Thermals"]
[null,"Enter the LM5166's junction-to-ambient thermal impedance (dependent on your PCB design, air flow, etc.) and ambient temperature. Device power dissipation and junction temperature are derived at the maximum load.  Ensure that the junction temperature is within the recommended range."]
[]
[]
[]
[null,"BOM & Schematic tab"]
[null,"This tab summarizes the converter schematic and BOM.  It also helps you estimate the total solution size. Select a package size for each external component (i.e. inductor, capacitors, and resistors) for accurate solution size estimates."]
[]
[]
[null,"Design EMI Filter tab"]
[null,"In case an EMI filter is needed, a simple EMI filter design aid is given in this tab.  It is based on the guidelines documented in TI's literature number SNVA489C (aka AN-2162).  Suggest reviewing the note before using the design aid."]
[]
[]
[null,"fSW & Ripple tab"]
[null,"In this tab, the switching/burst frequency (COT/PFM mode) and the output voltage ripple as a function of the load current are plotted."]

{"sheet":"Design Converter","index":1,"n_rows":58,"n_cols":17,"rows_kept":58,"cut":false,"hidden":false,"merged":[[2,14,2,15],[0,0,0,16]]}
["                          LM5163/4 Low IQ DC/DC Converter Design Tool  "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"http://www.ti.com/ww/en/analog/power_management/widevin"]
["About",null,"xx",null,null,"= Input Box",null,null,null,null,null,null,null,null,"Terms Of Use",null,"                "]
[]
["Step 1: Operating Specifications"]
[null,null,null,"Input Voltage - Min, VIN(min) ",40,"V"]
[null,null,null,"Input Voltage - Nom, VIN(nom)",42,"V"]
[null,null,null,"Input Voltage - Max, VIN(max)",45,"V"]
[null,null,null,"Output Voltage, VOUT ",19,"V"]
[null,null,null,"Full Load Current, IOUT",7.0000000000000007E-2,"A"]
[null,null,null,"Mode of Operation",null,null,{"$f":"MODE","v":3}]
[null,null,null,"Switching Frequency at VIN(nom)",300,"kHz"]
[null,null,null,"Timing Resistance, RT",{"$f":"'Standard Value Calculator'!J4/1000","v":158},"kΩ"]
[]
["Step 2: Buck Inductor"]
[null,null,null,"Recommended Buck Inductance ",{"$f":"Lopt*1000000","v":1238.6621315192742},"µH"]
[null,null,null,"Inductance, LF ",470,"µH"]
[null,null,null,"Inductor DCR ",820,"mΩ"]
[null,null,null,{"$f":"CHOOSE(MODE, \"Pk-to-Pk Ripple Current\",\"Pk-to-Pk Ripple Current\",\"Pk-to-Pk Ripple Current\", \"Resulting PFM Switching Frequency\")","v":"Pk-to-Pk Ripple Current"},{"$f":"Iripple_Vinnom*1000","v":73.895489488548947},"mApk-pk"]
[null,null,null,{"$f":"CHOOSE(MODE, 'Variable Mgmt'!H88,'Variable Mgmt'!H88,'Variable Mgmt'!H88, 'Variable Mgmt'!H89)","v":"% Ripple Current at Nom VIN"},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), 'Variable Mgmt'!B96*100, Ilim/2*1000)","v":105.56498498364135},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), \"%\", \"mA\")","v":"%"}]
[]
[{"$f":"IF(MODE=4, \"Step 3: Output Capacitors\", \"Step 3: Output Capacitors, Ripple Generation\")","v":"Step 3: Output Capacitors, Ripple Generation"}]
[null,null,null,"Minimum Output Capacitance ",{"$f":"'Variable Mgmt'!B116","v":2.2000000000000002},"µF"]
[null,null,null,"Output Capacitance, COUT ",0.47,"µF"]
[null,null,null,{"$f":"IF(OR(MODE=1,MODE=2),\"Recommended Series Resistance\",IF(MODE=3,\"Maximum Allowable ESR\",\"*Higher Cout Improves Light-Load Eff\"))","v":"Maximum Allowable ESR"},{"$f":"'Variable Mgmt'!B272","v":0.93100000000000005},"Ω"]
[null,null,null,{"$f":"IF(OR(MODE=1,MODE=2),\"Total ESR & Series Resistance, Rser\",IF(MODE=3,\"Output Capacitor ESR\",\"*PFM Hysteresis Sets Output Ripple\"))","v":"Output Capacitor ESR"},1.0999999999999999E-2,"Ω"]
[null,null,null,{"$f":"CHOOSE(MODE, \"Resulting Output Voltage Ripple\",\"Resulting Output Voltage Ripple\", \"Output Voltage Ripple\",\"Output Voltage Ripple\")","v":"Output Voltage Ripple"},{"$f":"CHOOSE(MODE, Vripple2*1000,Vripple2*1000,Vripple2*1000, PFM_Ripple)","v":65.515228446498128},"mVpk-pk"]
[null,null,null,{"$f":"IF(MODE=1,\"\",IF(MODE=2,\"Minimum Feedforward Capacitance\", IF(MODE=3,\"Minimum Coupling Capacitance\",\"\")))","v":"Minimum Coupling Capacitance"},{"$f":"'Variable Mgmt'!B140","v":">47"},"pF"]
[null,null,null,{"$f":"IF(MODE=1,\"\",IF(MODE=2,\"Feedforward Capacitance, Cff\", IF(MODE=3,\"Coupling Capacitance, Cb\",\"\")))","v":"Coupling Capacitance, Cb"},47,"pF",null,null,null,null,null,"** Specify Inductor Core Loss **",100,"mW"]
[null,null,null,{"$f":"IF(MODE=3,\"Minimum Ripple Generation Capacitance\",\"\")","v":"Minimum Ripple Generation Capacitance"},{"$f":"'Variable Mgmt'!B144","v":">750"},"pF"]
[null,null,null,{"$f":"IF(MODE=3,\"Ripple Generation Capacitance, Ca\",\"\")","v":"Ripple Generation Capacitance, Ca"},2200,"pF"]
[null,null,null,{"$f":"IF(MODE=3,\"Ripple Generation Resistance, Ra\",\"\")","v":"Ripple Generation Resistance, Ra"},{"$f":"Ra","v":787},"kΩ"]
[null,null,null,{"$f":"IF(MODE=3,\"Amplitude of Injected Ripple\",\"\")","v":"Amplitude of Injected Ripple"},20,"mVpk-pk"]
[]
["Step 4: Input Capacitors"]
[null,null,null,"Minimum Input Capacitance ",{"$f":"'Variable Mgmt'!B157","v":2.2000000000000002},"µF"]
[null,null,null,"Input Capacitance, CIN ",2.2000000000000002,"µF"]
[null,null,null,"Maximum Allowable ESR",{"$f":"'Variable Mgmt'!B159","v":19.389925524959228},"Ω"]
[null,null,null,"Input Capacitor ESR ",2,"mΩ"]
[null,null,null,"Resulting Input Voltage Ripple ",{"$f":"CHOOSE(MODE, Vinripple2*1000,Vinripple2*1000,Vinripple2*1000, 'Variable Mgmt'!B165*1000)","v":26.50508983565658},"mVpk-pk"]
[]
["Step 5: Feedback, PGOOD, UVLO"]
[null,null,null,"Upper Feedback Resistor, RFB1 ",698,"kΩ"]
[null,null,null,"Lower Feedback Resistor, RFB2",{"$f":"IF(Vout=Vref,\"OPEN\",Rfb2_u/1000)","v":47.5},{"$f":"IF(Vout=Vref,\"\",\"kΩ\")","v":"kΩ"}]
[null,null,null,"Acutal Output Voltage Setpoint",{"$f":"'Variable Mgmt'!B201","v":18.833684210526314},"V"]
[null,null,null,"PGOOD Pull-up Resistance",20,{"$f":"\"kΩ\"","v":"kΩ"},null,null,null,null,null,null,null,null,null,null," "]
[null,null,null,"BST Capacitance, CBST ",2.2000000000000002,"nF"]
[null,null,null,{"$f":"\"Required Input Voltage UVLO Turn-on\"","v":"Required Input Voltage UVLO Turn-on"},6,"V"]
[null,null,null,"Upper UVLO Resistor, RUV1",1,"MΩ"]
[null,null,null,"Lower UVLO Resistor, RUV2",{"$f":"'Variable Mgmt'!F276","v":332},{"$f":"'Variable Mgmt'!G276","v":"kΩ"}]
[null,null,null,"Actual UVLO Turn-on Threshold",{"$f":"'Variable Mgmt'!B186","v":6.0180722891566267},"V"]
[null,null,null,"Actual UVLO Turn-off Threshold",{"$f":"'Variable Mgmt'!B187","v":5.6168674698795176},"V"]
[]
["Step 6: Efficiency & Thermals"]
[null,null,null,"Estimated Thermal Impedance, JJA",41,"°C/W"]
[null,null,null,"Ambient Temp, TA",25,"°C"]
[null,null,null,"IC Power Dissipation at Full Load, PD",{"$f":"'Variable Mgmt'!B26","v":0.16785335632632201},"W"]
[null,null,null,"IC Junction Temp at Full Load, TJ",{"$f":"E56+E55*'Variable Mgmt'!B26","v":31.881987609379202},"°C"]

{"sheet":"BOM & Schematic","index":2,"n_rows":53,"n_cols":13,"rows_kept":53,"cut":false,"hidden":false,"merged":[[33,3,33,5],[0,0,0,16],[29,3,29,5],[41,3,41,5],[47,7,47,9],[30,3,30,5],[43,3,43,5],[44,3,44,5],[42,3,42,5],[39,3,39,5],[40,3,40,5],[38,3,38,5],[37,3,37,5],[36,3,36,5],[31,3,31,5],[34,3,34,5],[32,3,32,5]]}
["                         LM5163/4 100V Low IQ DC/DC Converter Design Tool  "]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[{"$f":"\"VIN = \"&Vin&\" V, VOUT = \"&Vout&\" V, IOUT = \"&Iout&\" A \"&'Variable Mgmt'!B35&\" Converter\"","v":"VIN = 42 V, VOUT = 19 V, IOUT = 0.07 A COT Converter"}]
["Low IQ, High Efficiency, Synchronous Buck Converter BOM"]
["Count","Ref Des","Value","Description",null,null,"Size","Part Number","MFR","Footprint (mm)","Area (mm2)"]
[{"$f":"ROUNDUP('Design Converter'!E37/10,0)","v":1},"CIN",{"$f":"Cin*1000000","v":2.2000000000000002},{"$f":"IF(VIN_max>35, \"Capacitor, Ceramic, \"&'Variable Mgmt'!B257&\", 100V, X7R, 10%\", \"Capacitor, Ceramic, \"&'Variable Mgmt'!B257&\", 50V, X7R, 10%\")","v":"Capacitor, Ceramic, 2.2µF, 100V, X7R, 10%"},null,null,5,"Std","Std",{"$f":"CHOOSE(G31,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45)","v":"3.2 x 2.5"},{"$f":"CHOOSE(G31,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45)","v":8}]
[{"$f":"'Variable Mgmt'!D252","v":1},"COUT",{"$f":"'Variable Mgmt'!F253","v":"22µF"},{"$f":"CHOOSE(Cout_Voltage_Rating, \"Capacitor, Ceramic, \"&'Variable Mgmt'!F253&\", 6.3V, X7R, 10%\", \"Capacitor, Ceramic, \"&'Variable Mgmt'!F253&\", 10V, X7R, 10%\", \"Capacitor, Ceramic, \"&'Variable Mgmt'!F253&\", 16V, X7R, 10%\", \"Capacitor, Ceramic, \"&'Variable Mgmt'!F253&\", 25V, X7R, 10%\",  \"Capacitor, Ceramic, \"&'Variable Mgmt'!F253&\", 50V, X7R, 10%\")","v":"Capacitor, Ceramic, 22µF, 25V, X7R, 10%"},null,null,5,"Std","Std",{"$f":"CHOOSE(G32,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45)","v":"3.2 x 2.5"},{"$f":"(CHOOSE(G32,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45))*A32","v":8}]
[{"$f":"CHOOSE(MODE, \"-\", \"-\", \"1\",\"-\")","v":"1"},{"$f":"CHOOSE(MODE,\"-\",\"-\",\"Ca\",\"-\")","v":"Ca"},{"$f":"CHOOSE(MODE, \"-\",\"-\",'Variable Mgmt'!B293, \"-\")","v":"2200pF"},{"$f":"CHOOSE(MODE,\"-\",\"-\", \"Capacitor, Ceramic, \"&'Variable Mgmt'!B293&\", 16V, X7R, 10%\", \"-\")","v":"Capacitor, Ceramic, 2200pF, 16V, X7R, 10%"},null,null,1,{"$f":"CHOOSE(MODE, \"-\", \"-\", \"Std\", \"-\")","v":"Std"},{"$f":"H33","v":"Std"},{"$f":"CHOOSE(MODE,\"\",\"\",CHOOSE(G33,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),\"\")","v":"1.0 x 0.5"},{"$f":"CHOOSE(MODE,\"\",\"\",CHOOSE(G33,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),\"\")","v":0.5}]
[{"$f":"CHOOSE(MODE, \"-\", \"1\", \"1\",\"-\")","v":"1"},{"$f":"CHOOSE(MODE,\"-\",\"Cff\",\"Cb\",\"-\")","v":"Cb"},{"$f":"CHOOSE(MODE, \"-\",'Variable Mgmt'!B290,'Variable Mgmt'!B290, \"-\")","v":"47pF"},{"$f":"CHOOSE(MODE,\"-\",\"Capacitor, Ceramic, \"&'Variable Mgmt'!B290&\", 50V, X7R, 10%\", \"Capacitor, Ceramic, \"&'Variable Mgmt'!B290&\", 50V, X7R, 10%\", \"-\")","v":"Capacitor, Ceramic, 47pF, 50V, X7R, 10%"},null,null,1,{"$f":"CHOOSE(MODE, \"-\", \"Std\", \"Std\", \"-\")","v":"Std"},{"$f":"H34","v":"Std"},{"$f":"CHOOSE(MODE,\"\",CHOOSE(G34,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),CHOOSE(G34,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),\"\")","v":"1.0 x 0.5"},{"$f":"CHOOSE(MODE,\"\",CHOOSE(G34,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),CHOOSE(G34,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),\"\")","v":0.5}]
[1,"CBST","2.2nF","Capacitor, Ceramic, 2.2nF, 25V, X7R, 10%",null,null,1,{"$f":"CHOOSE(MODE, \"-\", \"Std\", \"Std\", \"-\")","v":"Std"},{"$f":"H35","v":"Std"},{"$f":"CHOOSE(MODE,\"\",CHOOSE(G35,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),CHOOSE(G35,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),\"\")","v":"1.0 x 0.5"},{"$f":"CHOOSE(MODE,\"\",CHOOSE(G35,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),CHOOSE(G35,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),\"\")","v":0.5}]
[]
[1,"LF",{"$f":"'Design Converter'!E17","v":470},{"$f":"\"Inductor, \"&Lf*1000000&\" µH, \"&Rdcr*1000&\" mΩ, >\"&ROUNDUP(Isat_min,2)&\"A\"","v":"Inductor, 470 µH, 820 mΩ, >0.9A"},null,null,4,"Various","Various",{"$f":"CHOOSE(G37,'Variable Mgmt'!T50,'Variable Mgmt'!T51,'Variable Mgmt'!T52,'Variable Mgmt'!T53,'Variable Mgmt'!T54,'Variable Mgmt'!T55,'Variable Mgmt'!T56)","v":"6.0 x 6.0"},{"$f":"CHOOSE(G37,'Variable Mgmt'!U50,'Variable Mgmt'!U51,'Variable Mgmt'!U52,'Variable Mgmt'!U53,'Variable Mgmt'!U54,'Variable Mgmt'!U55,'Variable Mgmt'!U56)","v":36}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(MODE_RSET=2,CHOOSE(G38,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),\"\")","v":""}]
[{"$f":"CHOOSE(MODE, \"1\",\"1\",\"1\", \"-\")","v":"1"},"RT",{"$f":"CHOOSE(MODE, 'Design Converter'!E13, 'Design Converter'!E13,'Design Converter'!E13,\"-\")","v":158},{"$f":"C39","v":158},null,null,1,{"$f":"CHOOSE(MODE, \"Std\",\"Std\",\"Std\",\"-\")","v":"Std"},{"$f":"H39","v":"Std"},{"$f":"CHOOSE(MODE,CHOOSE(G39,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),CHOOSE(G39,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),CHOOSE(G39,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),\"\")","v":"1.0 x 0.5"},{"$f":"CHOOSE(MODE,CHOOSE(G39,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),CHOOSE(G39,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),CHOOSE(G39,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),\"\")","v":0.5}]
[1,"RFB1",{"$f":"Rfb1_/1000","v":698},698,null,null,1,{"$f":"CHOOSE(MODE_VOUT,\"-\",\"Std\")","v":"Std"},{"$f":"H40","v":"Std"},{"$f":"(CHOOSE(MODE_VOUT,\"\",CHOOSE(G40,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45)))","v":"1.0 x 0.5"},{"$f":"CHOOSE(MODE_VOUT,\"\",CHOOSE(G40,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45))","v":0.5}]
[1,"RFB2",{"$f":"Rfb2_u/1000","v":47.5},47.5,null,null,1,{"$f":"CHOOSE(MODE_VOUT,\"-\",\"Std\")","v":"Std"},{"$f":"H41","v":"Std"},{"$f":"CHOOSE(MODE_VOUT,\"\",CHOOSE(G41,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45))","v":"1.0 x 0.5"},{"$f":"CHOOSE(MODE_VOUT,\"\",CHOOSE(G41,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45))","v":0.5}]
[{"$f":"IF(MODE=3,\"1\",\"-\")","v":"1"},{"$f":"CHOOSE(MODE,\"-\",\"-\",\"Ra\",\"-\")","v":"Ra"},{"$f":"'Variable Mgmt'!F296","v":"787k"},{"$f":"\"Resistor, Chip, \"&'Variable Mgmt'!B296&\", 1/16W, 1%\"","v":"Resistor, Chip, 787kΩ, 1/16W, 1%"},null,null,1,{"$f":"CHOOSE(MODE, \"-\", \"-\", \"Std\", \"-\")","v":"Std"},{"$f":"H42","v":"Std"},{"$f":"CHOOSE(MODE,\"\",\"\",CHOOSE(G42,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),\"\")","v":"1.0 x 0.5"},{"$f":"CHOOSE(MODE,\"\",\"\",CHOOSE(G42,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),\"\")","v":0.5}]
[1,"RPGOOD",100,100,null,null,1,"Std","Std",{"$f":"CHOOSE(G43,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45)","v":"1.0 x 0.5"},{"$f":"CHOOSE(G43,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45)","v":0.5}]
[{"$f":"CHOOSE(MODE_UVLO, \"1\", \"-\")","v":"1"},"RUV1",{"$f":"CHOOSE(MODE_UVLO, 'Variable Mgmt'!H275, \"-\")","v":"1M"},{"$f":"CHOOSE(MODE_UVLO, \"Resistor, Chip, \"&'Variable Mgmt'!C275&\", 1/16W, 1%\", \"-\")","v":"Resistor, Chip, 1MΩ, 1/16W, 1%"},null,null,2,{"$f":"CHOOSE(MODE_UVLO,\"Std\",\"-\")","v":"Std"},{"$f":"H44","v":"Std"},{"$f":"CHOOSE(MODE_UVLO,CHOOSE(G44,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),\"\")","v":"1.6 x 0.8"},{"$f":"CHOOSE(MODE_UVLO,CHOOSE(G44,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),\"\")","v":1.3}]
[{"$f":"CHOOSE(MODE_UVLO, \"1\", \"-\")","v":"1"},"RUV2",{"$f":"CHOOSE(MODE_UVLO, 'Variable Mgmt'!H276, \"-\")","v":"332k"},{"$f":"CHOOSE(MODE_UVLO, \"Resistor, Chip, \"&'Variable Mgmt'!C276&\", 1/16W, 1%\", \"-\")","v":"Resistor, Chip, 332kΩ, 1/16W, 1%"},null,null,1,{"$f":"CHOOSE(MODE_UVLO,\"Std\",\"-\")","v":"Std"},{"$f":"H45","v":"Std"},{"$f":"CHOOSE(MODE_UVLO,CHOOSE(G45,'Variable Mgmt'!T$41,'Variable Mgmt'!T$42,'Variable Mgmt'!T$43,'Variable Mgmt'!T$44,'Variable Mgmt'!T$45),\"\")","v":"1.0 x 0.5"},{"$f":"CHOOSE(MODE_UVLO,CHOOSE(G45,'Variable Mgmt'!U$41,'Variable Mgmt'!U$42,'Variable Mgmt'!U$43,'Variable Mgmt'!U$44,'Variable Mgmt'!U$45),\"\")","v":0.5}]
[1,"U1",{"$f":"CHOOSE(VARIANT, \"LM5163-Q1\", \"LM5164-Q1\")","v":"LM5163-Q1"},{"$f":"CHOOSE(VARIANT, \"IC, LM51643-Q1, Buck Converter, 6V–100V Input\", \"IC, LM5164-Q1, Buck Converter, 6V–100V Input\")","v":"IC, LM51643-Q1, Buck Converter, 6V–100V Input"},null,null,"SOIC-8",{"$f":"CHOOSE(VARIANT, \"LM5163QDDATQ1\", \"LM5164QDDATQ1\")","v":"LM5163QDDATQ1"},"TI","5.0 x 6.0",30]
[]
[null,{"$f":"\"Total Solution Size (padded by 15%) = \"&ROUND(K48,1)&\" mm^2 = \"&ROUND(M48,3)&\" in^2\"","v":"Total Solution Size (padded by 15%) = 101 mm^2 = 0.157 in^2"},null,null,null,null,null,null,null,null,{"$f":"SUM(K31:K46)*1.15","v":100.96999999999998},null,{"$f":"K48/25.4/25.4","v":0.156503813007626}]
[]
["NOTES:"]
["* Inductor saturation current should be higher than the peak inductor current setting for all operating temperatures *"]
["** Effective input and output capacitances should be appropriately derated for applied voltage and temperature, particularly with ceramics **"]
["***Estimated total solution size does not include EMI filter***"]

{"sheet":"Fsw & Ripple","index":3,"n_rows":1,"n_cols":1,"rows_kept":1,"cut":false,"hidden":true,"merged":[[0,0,0,16]]}
["                         LM5164 Low IQ DC/DC Converter Design Tool  "]

{"sheet":"Losses","index":4,"n_rows":42,"n_cols":6,"rows_kept":42,"cut":false,"hidden":true,"merged":[[0,0,0,16]]}
["                         LM5166 Low IQ DC/DC Converter Design Tool  "]
[]
[]
[]
[null,null,null,"Load Current",500,"mA"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,"Inductor Core Loss Constant",0]

{"sheet":"EVM","index":5,"n_rows":85,"n_cols":15,"rows_kept":85,"cut":false,"hidden":false,"merged":[[0,0,0,16]]}
["LM5163/4 100V, Low IQ DC/DC Converter Design Tool  "]
[]
[null,"LM5164-Q1EVM-041 PCB Layout"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Top"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Layer"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Layer 2"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Layer 3"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Bottom"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Layer"]

{"sheet":"Design EMI Filter","index":6,"n_rows":33,"n_cols":15,"rows_kept":33,"cut":false,"hidden":false,"merged":[[0,0,0,22],[32,10,32,12],[29,10,29,12],[31,10,31,12]]}
["                         LM5163/4 100V, Low IQ DC/DC Converter Design Tool  "]
[]
[]
[]
[]
[]
["Step 7: EMI Filter (Optional)"]
[null,null,null,"Desired Maximum Noise Level, Vnoise(MAX)",50,"dBmV"]
[null,null,null,"EMI Filter Inductance, LF(EMI)",22,"mH"]
[null,null,null,"Minimum EMI Filter Capacitance",{"$f":"'Variable Mgmt'!M164","v":0.43039553812788961},"mF"]
[null,null,null,"EMI Filter Capacitance, CF(EMI)",4.7,"mF"]
[null,null,null,"Minimum EMI Filter Damping Capacitance",{"$f":"'Variable Mgmt'!M168","v":8.8000000000000007},"mF"]
[null,null,null,"EMI Filter Damping Capacitance, CD(EMI)",10,"mF"]
[null,null,null,"Minimum Damping Capacitor ESR",{"$f":"'Variable Mgmt'!M169","v":3.1622776601683795},"Ω"]
[null,null,null,"Damping Capacitor ESR, ESR CD(EMI)",3.3,"Ω"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,"EMI Filter BOM"]
[null,null,null,null,null,null,null,"Count","Ref Des","Value","Description",null,null,"Part Number","MFR"]
[null,null,null,null,null,null,null,1,"LF(EMI)",{"$f":"'Variable Mgmt'!B298","v":"22µH"},{"$f":"\"Inductor, \"&Lf_emi*1000000&\" µH, \"&ROUNDUP(Isat_min,2)&\"A\"","v":"Inductor, 22 µH, 0.9A"},null,null,"Std","Std"]
[null,null,null,null,null,null,null,1,"CF(EMI)",{"$f":"'Variable Mgmt'!B299","v":"4.7µF"},{"$f":"IF(VIN_max>35, \"Capacitor, Ceramic, \"&'Variable Mgmt'!B299&\", 100V, X7R, 10%\", \"Capacitor, Ceramic, \"&'Variable Mgmt'!B299&\", 50V, X7R, 10%\")","v":"Capacitor, Ceramic, 4.7µF, 100V, X7R, 10%"},null,null,"Std","Std"]
[null,null,null,null,null,null,null,1,"CD(EMI)",{"$f":"'Variable Mgmt'!B300","v":"10µF"},{"$f":"IF(VIN_max>35, \"Capacitor, Electrolytic, \"&'Variable Mgmt'!B300&\", 100V, ESR>\"&ESR_Cd&ohm, \"Capacitor, Electrolytic, \"&'Variable Mgmt'!B300&\", 50V, ESR>\"&ESR_Cd&ohm)","v":"Capacitor, Electrolytic, 10µF, 100V, ESR>3.3Ω"},null,null,"Std","Std"]

{"sheet":"Variable Mgmt","index":7,"n_rows":320,"n_cols":21,"rows_kept":320,"cut":false,"hidden":true,"merged":[[4,4,4,7],[0,0,0,8]]}
["EXCEL Variables Names/Calculations",null,null,null,null,null,null,null,null,null,null,"LM5166"]
[null,"Input from user ="]
[null,"Output ="]
[null,"Constant"]
["Variable Name","Value","STD Units",null,"Notes",null,null,null,"Iteration"]
["Step 1: Operational Specs"]
["VIN_min",{"$f":"'Design Converter'!E6","v":40},"V","Minimum input voltage",null,null,null,null,1]
["VIN_nom",{"$f":"'Design Converter'!E7","v":42},"V","Nominal input voltage"]
["VIN_max",{"$f":"'Design Converter'!E8","v":45},"V","Maximum input voltage"]
[]
["Vout",{"$f":"'Design Converter'!E9","v":19},"V","Output Voltage",null,null,null,null,1]
["Iout",{"$f":"'Design Converter'!E10","v":7.0000000000000007E-2},"A","Maximum Output Current",null,null,null,null,1]
["Rout",{"$f":"Vout/Iout","v":271.42857142857139},"W","Load resistance"]
["Pout",{"$f":"Vout*Iout","v":1.33},"W","Output power"]
[]
["Efficiency",0.9,null,"Estimate of efficiency"]
["Pin",{"$f":"Pout/Efficiency","v":1.4777777777777779},"W","Calculate input power assuming 90% efficiency"]
["Iin_Vinmin",{"$f":"Pin/VIN_min","v":3.6944444444444446E-2},"A"]
["Iin_Vinnom",{"$f":"Pin/VIN_nom","v":3.5185185185185187E-2},"A","Input currents at min, nom, max Vin"]
["Iin_Vinmax",{"$f":"Pin/VIN_max","v":3.2839506172839511E-2},"A"]
[]
["Fsw",{"$f":"'Design Converter'!E12*1000","v":300000},"Hz","Nominal Switching Frequency",null,null,null,null,1]
["Vref",1.2,"V","Reference Voltage"]
["Rt",{"$f":"Vout*2500000000/Fsw","v":158333.33333333334},"W","Frequency Set Resistor"]
[null,null,null,null,null,null,null,null,null,null,{"$f":"B34&\"_\"&F35&\"_\"&F39&\"_\"&I41&\"_\"&I36","v":"COT3_VOUTadj_UVLOadj_SSAdj_RsetGND"},null,null,null,null,null,"Vout<5V",100,1]
["Internal PD at Full Load",{"$f":" IF(OR(MODE=1,MODE=2,MODE=3), Efficiency!AZ106,#REF!)","v":0.16785335632632201},"W",null,null,null,null,null,null,null,null,null,null,null,null,null,"Vout<=8V",47,2]
[null,null,null,null,null,null,null,null,null,null,{"$f":"\"SCH_\"&B34&\"_\"&B41","v":"SCH_COT3_LM5163"},null,null,null,null,null,"Vout<=12V",22,3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Vout<=20V",22,4]
["Step 2: Circuit Configuration for COT / PFM, Fixed / Adj Vout, ILIM, UVLO, SS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Vout>20V",10,5]
[null,"COT Type I",1,null,null,null,null,null,null,null,null,null,null,null,null,null,"Cout Capacitance",{"$f":"CHOOSE(S30,\"100\", \"47\",\"22\",\"22\",\"10\")","v":"22"},{"$f":"IF(Vout<5, 1, IF(Vout<=8, 2, IF(Vout<=12, 3, IF(Vout<=20, 4, 5))))","v":4}]
[null,"COT Type II",2]
["COT/PFM ","COT Type III",3]
[null,null,null,null,"VOUT Fixed/Adjustable","Fixed",1,null,"ILIM shorted",1,{"$f":"B34&\", \"&F35&\", \"&I36&\", \"&F39&\", \"&I41","v":"COT3, VOUTadj, RsetGND, UVLOadj, SSAdj"},null,null,null,null,null,"Vout<=5V","6.3V",1]
["MODE",{"$f":"CHOOSE(C34, \"COT1\", \"COT2\",\"COT3\")","v":"COT3"},3,null,null,"Adjustable",2,null,"ILIM resistor needed",2,{"$f":"C34&\", \"&G35&\", \"&J36&\", \"&G39&\", \"&J41","v":"3, 2, 1, 1, 1"},null,null,null,null,null,"Vout<=8V","10V",2]
[null,{"$f":"IF(MODE=4, \"PFM\", \"COT\")","v":"COT"},null,null,"MODE_VOUT",{"$f":"CHOOSE(G35, \"VOUTfixed\", \"VOUTadj\")","v":"VOUTadj"},{"$f":"IF(AND(OR(MODE=1,MODE=4),OR(Vout=3.3,Vout=5)),1,2)","v":2},null,null,null,{"$f":"C34&G35&J36&G39&J41","v":"32111"},null,null,null,null,null,"Vout<=12V","16V",3]
[null,null,null,null,null,null,null,"MODE_RSET",{"$f":"CHOOSE(J36, \"RsetGND\",\"Rset\")","v":"RsetGND"},1,null,null,null,null,null,null,"Vout<=20V","25V",4]
[null,null,null,null,"UVLO","Adjustable",1,null,null,null,null,null,null,null,null,null,"Vout>20V","50V",5]
[null,null,null,null,null,"Internal",2,"Soft Start","Adjustable",1,null,"Iout Linear Axis",1,null,null,null,"Cout Voltage Rating",{"$f":"CHOOSE(S38,\"6.3V\", \"10V\",\"16V\",\"25V\",\"50V\")","v":"25V"},{"$f":"IF(Vout<=5, 1, IF(Vout<=8, 2, IF(Vout<=12, 3, IF(Vout<=20, 4, 5))))","v":4}]
[null,"LM5163",1,null,"MODE_UVLO",{"$f":"CHOOSE(G39, \"UVLOadj\", \"UVLOint\")","v":"UVLOadj"},1,null,"3ms Fixed",2,null,"Iout Log Axis",2]
[null,"LM5164",2,null,null,null,null,null,null,null,null,"PLOT_TYPE",1]
["VARIANT",{"$f":"CHOOSE(VARIANT, \"LM5163\", \"LM5164\")","v":"LM5163"},1,null,"ESR","NO",1,"MODE_SS",{"$f":"CHOOSE(J41, \"SSAdj\", \"SSfix\")","v":"SSAdj"},1,null,null,null,null,null,null,null,"0402",1,"1.0 x 0.5",0.5]
[null,null,null,null,null,"YES",2,null,null,null,null,null,null,null,null,null,null,"0603",2,"1.6 x 0.8",1.3]
[null,null,null,null,"MODE_ESR",null,2,null,null,null,null,null,null,null,null,null,null,"0805",3,"2.0 x 1.25",2.5]
[null,null,null,null,null,{"$f":"CHOOSE(G44, \"\", \"_ESR\")","v":"_ESR"},{"$f":"IF(MODE=2, 1, MODE_ESR)","v":2},null,null,null,null,null,null,null,null,null,null,"1206",4,"3.2 x 1.6",5.0999999999999996]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1210",5,"3.2 x 2.5",8]
["Step 3: Buck Inductor",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Component Size",{"$f":"CHOOSE(S46,\"0402\", \"0603\",\"0805\",\"1206\",\"1210\")","v":"1210"},5,{"$f":"CHOOSE(S46,T41,T42,T43,T44,T45)","v":"3.2 x 2.5"}]
["Don1",{"$f":"Vout/VIN_nom","v":0.45238095238095238},{"$f":"(Vout-VIN_nom)/Vout","v":-1.2105263157894737},null,"Ideal Duty Cycle at VIN(nom)",null,null,null,1]
["Doff1",{"$f":"1-47:47","v":0.54761904761904767},null,null,"Ideal 1- Duty Cycle at VIN(nom)",null,null,null,1]
[]
["Don_Vinmin",{"$f":"Vout/VIN_min","v":0.47499999999999998},{"$f":"IF(VIN_min>Vout, \"BUCK\", \"BOOST\")","v":"BUCK"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3mm x 3mm",1,"3.0 x 3.0",9]
["Don_Vinnom",{"$f":"Vout/VIN_nom","v":0.45238095238095238},{"$f":"IF(VIN_nom>Vout, \"BUCK\", \"BOOST\")","v":"BUCK"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4mm x 4mm",2,"4.0 x 4.0",16]
["Don_Vinmax",{"$f":"Vout/VIN_max","v":0.42222222222222222},{"$f":"IF(VIN_max>Vout, \"BUCK\", \"BOOST\")","v":"BUCK"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5mm x 5mm",3,"5.0 x 5.0",25]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"6mm x 6mm",4,"6.0 x 6.0",36]
["Lf_Vinmin",{"$f":"(VIN_min-Vout)*Don_Vinmin/(Fsw*Iout*0.4)","v":1.1874999999999998E-3},"H","COT",null,null,null,null,null,null,null,null,null,null,null,null,null,"7mm x 7mm",5,"7.0 x 7.0",49]
["Lf_Vinnom",{"$f":"(VIN_nom-Vout)*Don_Vinnom/(Fsw*Iout*0.4)","v":1.2386621315192742E-3},"H","COT",null,null,null,null,1,null,null,null,null,null,null,null,"Inductor Size","8mm x 8mm",6,"8.0 x 8.0",64]
["Lf_Vinmax",{"$f":"(VIN_max-Vout)*Don_Vinmax/(Fsw*Iout*0.7)","v":7.4678760393046104E-4},"H","COT",null,null,null,null,null,null,null,null,null,null,null,null,null,"10mm x 10mm",7,"10.0 x 10.0",100]
[]
["L_Vinmin_COT",{"$f":"(VIN_min-Vout)*Don_Vinmin/(Fsw*Iout*0.3)","v":1.5833333333333331E-3},"H","COT","Calculated Inductance for 30% ripple at VIN(min)"]
["L_Vinnom_COT",{"$f":"(VIN_nom-Vout)*Don_Vinnom/(Fsw*Iout*0.4)","v":1.2386621315192742E-3},"H","COT","Calculated Inductance for 40% ripple at VIN(nom)",null,null,null,null,null,"Pk-to-Pk Ripple Current at VIN(nom), DIL"]
["L_Vinmax_COT",{"$f":"(VIN_max-Vout)*Don_Vinmax/(Fsw*Iout*0.7)","v":7.4678760393046104E-4},"H","COT","Calculated Inductance for 70% ripple at VIN(max)"]
[]
[]
["Lopt",{"$f":"B59","v":1.2386621315192742E-3},"H"]
[]
["Lf",{"$f":"'Design Converter'!E17/1000000","v":4.6999999999999999E-4},"H",null,"Chosen Inductance"]
["Rdcr",{"$f":"'Design Converter'!E18/1000","v":0.82},"W",null,"Chosen Inductor DCR"]
[]
["Don2",{"$f":"(Vout+Iout*Rdcr)/Vin","v":0.45374761904761907},null,null,"**Edit to add Rdson**"]
["Doff2",{"$f":"1-_Don2","v":0.54625238095238093}]
[]
["Rdson1",0.75,"W"]
["Rdson2",0.33,"W"]
[]
["Don_Vinmin_2",{"$f":"(Vout+Iout*(Rdcr+Rdson2))/(VIN_min+Iout*Rdson2)","v":0.47673718427608058},null,null,"Duty cycles adjusted for DCR and shunt voltage drops"]
["Don_Vinnom_2",{"$f":"(Vout+Iout*(Rdcr+Rdson2))/(VIN_nom+Iout*Rdson2)","v":0.45404789270663043},null,null,"need to include RDS(on) later"]
["Don_Vinmax_2",{"$f":"(Vout+Iout*(Rdcr+Rdson2))/(VIN_max+Iout*Rdson2)","v":0.42379356374838695}]
[]
["Iripple_Vinmin",{"$f":"(VIN_min-Vout-Rdson1*Iout)*Don_Vinmin_2/(Fsw*Lf)","v":7.0825901898036864E-2},"A","COT"]
["Iripple_Vinnom",{"$f":"(VIN_nom-Vout-Rdson1*Iout)*Don_Vinnom_2/(Fsw*Lf)","v":7.3895489488548946E-2},"A","COT"]
["Iripple_Vinmax",{"$f":"(VIN_max-Vout)*Don_Vinmax_2/(Fsw*Lf)","v":7.8146330903957867E-2},"A","COT"]
[]
["ILpk_Vinmin",{"$f":"Iout+Iripple_Vinmin/2","v":0.10541295094901844},"A","COT"]
["ILpk_Vinnom",{"$f":"Iout+Iripple_Vinnom/2","v":0.10694774474427449},"A","COT"]
["ILpk_Vinmax",{"$f":"Iout+Iripple_Vinmax/2","v":0.10907316545197894},"A","COT"]
[]
["ILIM_Typ",{"$f":"CHOOSE(VARIANT, 0.75, 1.5)","v":0.75},"A",null,"Isat_min",{"$f":"B86*1.2","v":0.89999999999999991}]
[]
["Ripple current",{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), Iripple_Vinnom, Iripple)","v":7.3895489488548946E-2},"A",null,null,null,null,"% Ripple Current at Nom VIN"]
[null,null,null,null,null,null,null,"Maximum Load Current"]
["Max inductor ripple current",{"$f":"MAX(B78:B80)","v":7.8146330903957867E-2},"A"]
[null,null,null,null,null,"Ripple I","Iin"]
["% Ripple Current",{"$f":"B78/Iout","v":1.0117985985433837},null,"COT",null,{"$f":"B78","v":7.0825901898036864E-2},{"$f":"Iin_Vinmin","v":3.6944444444444446E-2}]
[null,{"$f":"B79/Iout","v":1.0556498498364135},null,"COT",null,{"$f":"B79","v":7.3895489488548946E-2},{"$f":"Iin_Vinnom","v":3.5185185185185187E-2}]
[null,{"$f":"B80/Iout","v":1.1163761557708265},null,"COT",null,{"$f":"B80","v":7.8146330903957867E-2},{"$f":"Iin_Vinmax","v":3.2839506172839511E-2}]
[]
[null,{"$f":"IF(OR(MODE=1, MODE=2,MODE=3), B93, Ilim/Iout)","v":1.0556498498364135}]
[]
["Iripple1",{"$f":"(Vin-Vout)*Don_Vinnom_2/(Fsw*Lf)","v":7.4064549874131205E-2},"A","inductor ripple current with chosen inductance (pk-pk)",null,null,null,null,1]
["Temp",100]
["DCR at hot",{"$f":"Rdcr*(1+0.0039*(B99-25))","v":1.05985},"W"]
[]
[]
[]
["Step 4: Output Capacitor"]
["Icoutrms_VINmin",{"$f":"Iripple_Vinmin/SQRT(12)","v":2.0445676763214807E-2},"A","Output Cap RMS current"]
["Icoutrms_VINnom",{"$f":"Iripple_Vinnom/SQRT(12)","v":2.1331790374056449E-2},"A"]
["Icoutrms_VINmax",{"$f":"Iripple_Vinmax/SQRT(12)","v":2.2558902591790823E-2},"A",null,null,null,{"$f":"Vripple1","v":9.5000000000000001E-2}]
[]
["Output Ripple Spec (pk-pk)",{"$f":"Vout*0.005","v":9.5000000000000001E-2},"V","Vout capacitive ripple spec at Vin(nom) = Vripple1"]
[]
["Coutmin"]
["COT",{"$f":"Iripple_Vinnom/(Fsw*8*Vripple1)","v":3.2410302407258311E-7},"F","COT","Min recommended Cout based on ripple spec above",null,null,null,1]
[null,{"$f":"Lf*B83^2/((1.05*Vout)^2-Vout^2)","v":1.4528141206044594E-7},"F","COT","Min recommended Cout based on 5% load-off transient spec"]
["CoutMinCOT",{"$f":"MAX(B112:B113, 0.0000022)","v":2.2000000000000001E-6},"F","COT","max of 2 results and 2.2uF"]
[]
["Reported Countmin",{"$f":"CoutMinCOT*1000000","v":2.2000000000000002},"µF"]
[]
["Cout",{"$f":"'Design Converter'!E24/1000000","v":4.6999999999999995E-7},"F","Chosen Output Capacitance",null,null,null,null,1]
["Resrmax",{"$f":"SQRT((Vripple1/Iripple_Vinnom)^2-(1/(Fsw*Cout*8))^2)","v":0.93104224510987044},"W","Max ESR before ripple exceeds Vripple1",null,null,null,null,1]
["Type1 ESR for sufficient (20mV) COT ripple at FB pin",{"$f":"0.02*Vout/Vref/Iripple_Vinnom","v":4.2853314709517996},"W","(a)"]
["Type2 ESR for sufficient (20mV) COT ripple at FB pin",{"$f":"0.02/Iripple_Vinnom","v":0.27065251395485046},"W","(b)"]
[]
["Type 1 Output Cap RC Time Constant",{"$f":"Cout*B130*1000000","v":0},"µs"]
["Type 2 Output Cap RC Time Constant",{"$f":"Cout*B131*1000000","v":0},"µs"]
["Ton @ Vin(min)",{"$f":"Vout/VIN_min/(Fsw)","v":1.5833333333333333E-6},"s"]
["Ton @ Vin(nom)",{"$f":"Vout/VIN_nom/(Fsw)","v":1.507936507936508E-6},"s"]
["ESR so that RC > Ton/2",{"$f":"B125/2/Cout","v":1.6843971631205676},"W","(c)"]
[]
[]
["Type1: Need ESR of…",{"$f":"IF(MODE=1, MAX(B120,B127), 0)","v":0},"W","Max of (a) and (c)"]
["Type2: Need ESR of…",{"$f":"IF(MODE=2, MAX(B121,B127), 0)","v":0},"W","Max of (b) and (c)"]
[]
["Reported Cout ESR max",{"$f":"IF(OR(CoutEsrMax>0.5, CoutEsrMax<0, (ISERROR(CoutEsrMax))), \"N/A\", CoutEsrMax*1000)","v":"N/A"},"mW"]
[]
["CoutEsr",{"$f":" 'Design Converter'!E26","v":1.0999999999999999E-2},"W","Chosen ESR",null,null,null,null,1]
[]
["Actual Output Ripple",{"$f":"Iripple_Vinnom*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2)","v":6.5515228446498125E-2},"Vp-p","Vripple2"]
[]
["Minimum Feedforward / Coupling Capacitance",{"$f":"MAX(1000000000000*0.00005/(3*Rfb1_),47)","v":47},"pF",null,null,null,null,{"$f":"0.00005/3/Rfb1_","v":2.387774594078319E-11}]
["Recommended Cff / Cb",{"$f":"IF(OR(MODE=2,MODE=3), \">\"&ROUND(B139,0),\"\")","v":">47"},"pF"]
["Selected Cff / Cb",{"$f":"'Design Converter'!$E$29","v":47},"pF"]
[]
["Minimum Ripple Generation Capacitance",{"$f":"10/(Fsw*Rfb)","v":7.4950987784647872E-10},"F",{"$f":"1000000000000*B143","v":749.50987784647873},"pF",{"$f":"Rfb","v":44473.507712944331}]
["Recommended Ca",{"$f":"IF(MODE=3, \">\"&ROUND(D143,0),\"\")","v":">750"},"pF"]
["Selected Ca",{"$f":"'Design Converter'!E31","v":2200},"pF",{"$f":"B145/1000000000000","v":2.1999999999999998E-9},"F"]
[]
["Maximum Ripple Generation Resistance",{"$f":"(VIN_nom-Vout)*B126/((B149/1000)*Ca)","v":788239.53823953832},"W",{"$f":"B147/1000","v":788.23953823953832},"kW"]
["Recommended Ra",{"$f":"IF(MODE=3, \"<\"&ROUND(D147,0),\"\")","v":"<788"},"kW",null,null,null,null,null,null,null,null,"Lf_emi",{"$f":"'Design EMI Filter'!$E$9","v":22},"uH",{"$f":"M148/1000000","v":2.1999999999999999E-5},"H"]
["Ripple amplitude",{"$f":"'Design Converter'!E33","v":20},"mVp-p",null,null,null,null,null,null,null,null,"Cf_emi",{"$f":"'Design EMI Filter'!$E$11","v":4.7},"uF",{"$f":"M149/1000000","v":4.6999999999999999E-6},"F"]
[null,null,null,null,null,null,null,null,null,null,null,"Cd_emi",{"$f":"'Design EMI Filter'!$E$13","v":10},"uF",{"$f":"M150/1000000","v":1.0000000000000001E-5},"F"]
[null,null,null,null,null,null,null,null,null,null,null,"ESR_Cd",{"$f":"'Design EMI Filter'!$E$15","v":3.3},"Ω",{"$f":"M151","v":3.3},"Ω",{"$f":"ESR_Cd&ohm","v":"3.3Ω"}]
["Step 5: Input Capacitor",null,null,null,null,null,null,null,null,null,null,"Min Noise",{"$f":"'Design EMI Filter'!$E$8","v":50},"dB","noise limit"]
["Vinripple1",{"$f":"0.05*VIN_nom","v":2.1},"Vp-p","Input voltage ripple spec (pk-pk) at Vin(nom)",null,null,null,null,null,null,null,"Duty Cycle",{"$f":"Vout/VIN_nom/Efficiency_COT_Full_Load","v":0.54503729202524387},null,"calculated duty cycle"]
[null,null,null,null,null,null,null,null,null,null,null,"Target Atten.",{"$f":"20*LOG(Iout/(PI()^2*Fsw*Cin)*SIN(PI()*Duty_Cycle)/0.000001) - Min_Noise","v":30.537853747346375},"dB","calculated attenuation"]
["Icinrms",{"$f":"Iout*SQRT(Don_Vinnom_2*(1-Don_Vinnom_2))","v":3.4851874824648438E-2},"A"]
["Cinmin",{"$f":"Iout*Don_Vinnom_2*(1-Don_Vinnom_2)/(Vinripple1*Fsw-Iout*RCinEsr)*1000000","v":2.7543155987820547E-2},"µF"]
["Reported Cinmin",{"$f":"IF(Cinmin<2.2, 2.2,Cinmin)","v":2.2000000000000002},"µF",null,null,null,null,null,null,null,null,"Filter Inductor"]
["Cin",{"$f":"'Design Converter'!E37/1000000","v":2.2000000000000001E-6},"F","Input capacitance",null,null,null,null,null,null,null,"Irms rating",{"$f":"Iout*1.5","v":0.10500000000000001},"A","calculated suggested IRMS rating"]
["CinEsrMax",{"$f":"-(Iout*Don_Vinnom_2*(1-Don_Vinnom_2)/(Cin*Fsw)-Vinripple1)/(Iout+Iripple_Vinnom/2)","v":19.389925524959228},"W"]
["RCinEsr",{"$f":"'Design Converter'!E39/1000","v":2E-3},"W","Input capacitance series resistance (ESR)"]
["Reported Cin ESR max",{"$f":"IF(OR(CinEsrMax>12, CinEsrMax<0), \"N/A\",CinEsrMax*1000)","v":"N/A"},"mΩ",null,null,null,null,null,null,null,null,"Filter Capacitor"]
[null,null,null,null,null,null,null,null,null,null,null,"Cfa calculation",{"$f":"Cin/(Cin*Lf_emi*0.000001*(2*PI()*Fsw/10)^2 - 1) / 0.000001","v":-2.2000037833022223},"uF","calculated value"]
["COT input voltage ripple - Vinripple2",{"$f":"Iout*Don_Vinnom_2*(1-Don_Vinnom_2)/(Cin*Fsw)+(Iout +Iripple_Vinnom/2)*RCinEsr","v":2.6505089835656581E-2},"Vp-p",null,{"$f":"Iout*Don_Vinmax_2*(1-Don_Vinmax_2)/(Cin*Fsw)","v":2.5899212932072761E-2},"Vp-p",null,null,null,null,null,"Cfb calculation",{"$f":"1/(Lf_emi)*(10^(Target_Att/40)/(2*PI()*Fsw))^2/0.000001","v":0.43039553812788961},"uF","calculated value"]
[null,null,null,null,null,null,null,null,null,null,null,"Cf",{"$f":"MAX(M162,M163)","v":0.43039553812788961},"uF","calculated value"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,"Damping Capacitor"]
["Step 6: Soft Start",null,null,null,null,null,null,null,null,null,null,"Cd ≥",{"$f":"4*Cin*1000000","v":8.8000000000000007},"uF","calculated value"]
["Tss",{"$f":"'Design Converter'!#REF!/1000","v":{"$error":"#REF!"}},"s","Soft-start time",null,null,null,null,null,null,null,"Cd ESR ≥",{"$f":"SQRT(Lf_emi/Cin)","v":3.1622776601683795},"Ω","calculated value"]
["Iss",1.0000000000000001E-5,"A","Soft-start current"]
["Css",{"$f":"8.16*Tss/1000000","v":{"$error":"#NAME?"}},"F","Required soft-start cap"]
["Css_u",{"$f":"'Standard Value Calculator'!B4","v":{"$error":"#NAME?"}},"F","User selected SS cap",null,null,null,null,null,null,null,"CIN and Cd Capacitors Current Sharing and Rating"]
[null,null,null,null,null,null,null,null,null,null,null,"Cd impedance",{"$f":" 1/(2*PI()*Fsw*Cd_emi) + ESR_Cd","v":3.3530516476972982},"Ω","calculated Cd impedance at the sw. frequency"]
["Step 7: Other Components - UVLO, PGOOD",null,null,null,null,null,null,null,null,null,null,"Cin impedance",{"$f":" 1/(2*PI()*Fsw*Cin) + RCinEsr","v":0.24314385316953838},"Ω","calculated CIN impedance at the sw. frequency"]
[]
["Rising UVLO/EN Threshold",1.5,"V",null,null,null,null,null,null,null,null,"IRMS Total Input Cap",{"$f":"Iout*SQRT(Duty_Cycle*(1-Duty_Cycle))","v":3.4857725792174991E-2},"A","calculated total IRMS current for CIN and Cd combined"]
["Falling UVLO/EN Threshold",1.4,"V",null,null,null,null,null,null,null,null,"IRMS Cd Act",{"$f":"IRMSTOT*(ZCIN/(ZCIN+ZCd))","v":2.3567800359556882E-3},"A","Calculated min IRMS current rating for Cd"]
["Voltage Hysteresis",{"$f":"B176-B177","v":0.10000000000000009},"V",null,null,null,null,null,null,null,null,"IRMS CIN",{"$f":"IRMSTOT*(ZCd/(ZCIN+ZCd))","v":3.2500945756219306E-2},"A","Calculated min IRMS current rating for CIN"]
[]
["VINUVLO_ON",{"$f":"'Design Converter'!E48","v":6},"V"]
["VINUVLO_OFF",null,"V"]
[]
["RUV1",{"$f":"'Design Converter'!E49*1000","v":1000},"kΩ",{"$f":"'Standard Value Calculator'!J16","v":1000},"kΩ",{"$f":"IF(Ruvlo1<0,\"N/A\",D183)","v":1000},{"$f":"IF(Ruvlo1<0,\"N/A\",D183&\"kΩ\")","v":"1000kΩ"}]
["RUV2",{"$f":"Vuvlo_on*Ruvlo1/(VINuvlo_on-Vuvlo_on)","v":333.33333333333331},"kΩ",{"$f":"'Standard Value Calculator'!J17","v":332},"kΩ",{"$f":"IF(F183=\"N/A\",\"N/A\",D184)","v":332},{"$f":"IF(G183=\"N/A\",\"N/A\",D184&\"kΩ\")","v":"332kΩ"}]
[]
["VINUVLO_ON_ACTUAL",{"$f":"(D183+D184)/D184*Vuvlo_on","v":6.0180722891566267},"V"]
["VINUVLO_OFF_ACTUAL",{"$f":"(D183+D184)/D184*Vuvlo_off","v":5.6168674698795176},"V"]
[]
["RPG",20,"kΩ"]
[]
[]
["Step 8: FB Divider"]
["Pi",3.1415926500000002,null,"p"]
["Toff_Vinmax",{"$f":"(1-Don_Vinmax_2)/Fsw","v":1.9206881208387102E-6},"sec"]
["Ton_Vinmin",{"$f":"IF(VIN_min>Vout, (1-Don_Vinmin_2)/Fsw, Don_Vinmin_2/Fsw)","v":1.744209385746398E-6},"sec"]
[]
["Rfb1",{"$f":"'Design Converter'!E43*1000","v":698000},"W","Lower Feedback Resistance - chosen by user",null,null,null,null,1]
["Rfb2",{"$f":"IF(Vout=Vref,100000000,Vref*B197/((Vout-Vref)))","v":47056.1797752809},"W","Upper Feedback Resistance"]
["Rfb2_u",{"$f":"IF(Vout=Vref,\"N/A\",'Standard Value Calculator'!J10)","v":47500},"W","Std Value Upper Feedback Resistance"]
["Rfb",{"$f":"Rfb1_*Rfb2_u/(Rfb1_+Rfb2_u)","v":44473.507712944331},"W","Rfb1 || Rfb2_u"]
[null,{"$f":"1.2/Rfb2_u*(Rfb2_u+Rfb1_)","v":18.833684210526314},"V"]
["Ifb",{"$f":"CHOOSE(MODE_VOUT, IF(Vout=5, 0.000007, 0.0000038), Vout/(Rfb1_+Rfb2_u))","v":2.5486250838363514E-5}]
[]
["Other Input Variables"]
["Rfets",0,"W","Series resistance due to FETs",null,null,null,{"$f":"_Don2*RdsonTop+Doff2*RdsonBot+B209*Vin^2*Fsw/2/(((Iripple1/SQRT(3))^2))","v":724.01408319451764}]
["Diode loss eq res",{"$f":"0.00000002*Fsw*0.6*4/Iripple1","v":0.19442499852455783}]
["Fet loss eq res",{"$f":"_Don2*RdsonTop+Doff2*RdsonBot","v":0.4777853380952381}]
["cap loss eq res",{"$f":"B209*Vin^2*Fsw/2/(((Iripple1/SQRT(3))^2))","v":723.53629785642238}]
["Sw cap",5.0000000000000001E-9]
[]
["Step 8: Efficiency"]
[]
["Design"]
["Ta",25,"°C","Ambient Temperature"]
["Components"]
["LTc",{"$f":"4000/1000000","v":4.0000000000000001E-3},"%/°C","Inductor DCR Temp Co"]
["θCA",40,"°C/W","Inductor Core to Ambient Thermal Resistance"]
["RCinEsr",{"$f":"RCinEsr","v":2E-3},"W","Input Capacitor ESR"]
["Part Characteristics"]
["Vcc",{"$f":"IF(Vin>7.7,7.5,Vin-0.2)","v":7.5},"V"]
["Deadtime"]
["Deadtime",2E-8,"s","Total Deadtime",null,null,"20ns for LM5166"]
["IQ"]
["IQ ",1.0000000000000001E-5,"A","Quiescent Current Of Controller (Not Switching!)"]
[]
[]
["IC Power Disipation","Value","Units"]
["Power Dis",{"$f":"Efficiency!AZ106","v":0.16785335632632201},"W"]
["Temp rise",{"$f":"B228*ThetaJA","v":6.8987729450118351},"°C"]
["Current (switching)",{"$f":"(Qg_Q1+Qg_Q2)*Fsw+Iq","v":{"$error":"#NAME?"}},"A"]
["Qrr Current",{"$f":"Qrr_Q2*Fsw","v":{"$error":"#NAME?"}},"A"]
["Diode Current",{"$f":"C232/Vin","v":{"$error":"#NAME?"}},{"$f":"Deadtime*Fsw*(Ipp/2)*(Vsd_Q1+Vsd_Q2)","v":{"$error":"#NAME?"}}]
["Total Application Switching IQ",{"$f":"SUM(B230:B232)","v":{"$error":"#NAME?"}},"A"]
[]
[]
["SCHEMATIC LABELS"]
[]
[]
[{"$f":"\"RUV1 = \"&'Design Converter'!E49&\"MΩ\"","v":"RUV1 = 1MΩ"},{"$f":"C275","v":"1MΩ"}]
[{"$f":"\"RUV2 = \"&'Design Converter'!E50&\"kΩ\"","v":"RUV2 = 332kΩ"},{"$f":"C276","v":"332kΩ"}]
[{"$f":"\"Rhys = \"&'Design Converter'!E52&\"kΩ\"","v":"Rhys = 5.61686746987952kΩ"},{"$f":"C277","v":{"$error":"#REF!"}}]
[]
[{"$f":"\"LF = \"&'Design Converter'!E17&\"µH\"","v":"LF = 470µH"},{"$f":"'Design Converter'!E17&\"µH\"","v":"470µH"}]
[{"$f":"\"Rdcr = \"&Rdcr*1000&\"mΩ\"","v":"Rdcr = 820mΩ"},{"$f":"Rdcr*1000&\"mΩ\"","v":"820mΩ"}]
[{"$f":"\"Rt = \"&'Design Converter'!I43&\"kΩ\"","v":"Rt = kΩ"},{"$f":"'Design Converter'!I43&\"kΩ\"","v":"kΩ"}]
[{"$f":"\"Css = \"&ROUND(Css_u*1000000000,1)&\"nF\"","v":{"$error":"#NAME?"}},{"$f":"ROUND(Css_u*1000000000,1)&\"nF\"","v":{"$error":"#NAME?"}}]
[]
["VIN",{"$f":"VIN_nom&\"V\"","v":"42V"}]
["VIN range",{"$f":"VIN_min&\"V...\"&VIN_max&\"V\"","v":"40V...45V"}]
[]
[{"$f":"\"VOUT = \"&'Design Converter'!E9&\"V\"","v":"VOUT = 19V"},{"$f":"'Design Converter'!E9&\"V\"","v":"19V"}]
[null,null,{"$f":"R30","v":"22"},{"$f":"ROUNDUP('Design Converter'!$E$24/C252,0)","v":1}]
[{"$f":"\"COUT = \"&'Design Converter'!$E$24&\"µF\"","v":"COUT = 0.47µF"},{"$f":"'Design Converter'!$E$24&\"µF\"","v":"0.47µF"},{"$f":"IF('Design Converter'!$E$24=OR(10, 22, 47, 100), 'Design Converter'!$E$24,C252)","v":"22"},{"$f":"IF(D252=1, \"\",B255)","v":""},{"$f":"D253&C253&\"µF\"","v":"22µF"},{"$f":"C253&\"µF\"","v":"22µF"}]
["Capacitance per component (Cout)",{"$f":"C252&\"µF\"","v":"22µF"}]
["# of output caps",{"$f":"D252&\" x \"","v":"1 x "}]
[]
["CIN",{"$f":"Cin*1000000&\"µF\"","v":"2.2µF"}]
["Capacitance per component (Cin)",{"$f":"\"2.2µF\"","v":"2.2µF"}]
["# of input caps",{"$f":"ROUNDUP(Cin*1000000/2.2,0)&\" x \"","v":"1 x "}]
[]
["Fixed VOUT?",{"$f":"IF(MODE_VOUT=1, \"YES\", \"NO\")","v":"NO"}]
["FB resistor ref des shown or not?",{"$f":"IF(MODE_VOUT=2, \"YES\", \"NO\")","v":"YES"},{"$f":"IF(MODE_VOUT=2, \"R1\", \"\")","v":"R1"},{"$f":"IF(MODE_VOUT=2, \"R2\", \"\")","v":"R2"}]
[{"$f":"\"RFB1 = \"&'Design Converter'!E43&\"kΩ\"","v":"RFB1 = 698kΩ"},{"$f":"'Design Converter'!E43&\"kΩ\"","v":"698kΩ"},{"$f":"IF(MODE=1,'Design Converter'!E43&\"kΩ\", \"\")","v":""}]
[{"$f":"\"RFB2 = \"&IF(Vout=Vref,\"OPEN\",'Design Converter'!E44&\"kΩ\")","v":"RFB2 = 47.5kΩ"},{"$f":"IF(Vout=Vref,\"OPEN\",Rfb2_u/1000&\"kΩ\")","v":"47.5kΩ"},{"$f":"IF(MODE=1, IF(Vout=Vref, \"OPEN\",Rfb2_u/1000&\"kΩ\" ), \"\")","v":""}]
[]
[]
["Show Rt resistor ref des?",{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), \"YES\", \"NO\")","v":"YES"},{"$f":"IF(MODE=4,\"\", \"Rt\")","v":"Rt"}]
["Rt",{"$f":"IF(MODE=4, \"\", 'Standard Value Calculator'!J4/1000&\"kΩ\")","v":"158kΩ"}]
[]
["Show ESR resistor ref des?",{"$f":"IF(OR(MODE=3, MODE=4), \"NO\", \"YES\")","v":"NO"},{"$f":"IF(OR(MODE=3, MODE=4),\"\",\"Resr\")","v":""}]
[{"$f":"\"RESR = \"&'Design Converter'!E26&\"mΩ\"","v":"RESR = 0.011mΩ"},{"$f":"IF(OR(MODE=3,MODE=4), \"\", 'Design Converter'!E26&\"Ω\")","v":""},null,null,null,{"$f":"B120","v":4.2853314709517996}]
["Resr",{"$f":"IF(MODE=1, \">\"&ROUND(B130,3), IF(MODE=2,  \">\"&ROUND(B131,3),IF(MODE=3,ROUND(B119,3),\"\")))","v":0.93100000000000005}]
[]
["Adjustable UVLO?",{"$f":"IF(MODE_UVLO=1, \"YES\", \"NO\")","v":"YES"},{"$f":"IF(MODE_UVLO=1,\"Ren1\", \"\")","v":"Ren1"},{"$f":"IF(MODE_UVLO=1, \"Ren2\", \"\")","v":"Ren2"},{"$f":"IF(MODE_UVLO=1, \"Rhys\", \"\")","v":"Rhys"},"Value","Units","BOM display"]
[{"$f":"\"RUV1 = \"&C275","v":"RUV1 = 1MΩ"},{"$f":"'Design Converter'!E49&\" MΩ\"","v":"1 MΩ"},{"$f":"IF(MODE_UVLO=1,'Design Converter'!E49&\"MΩ\", \"\")","v":"1MΩ"},null,null,{"$f":"IF(MODE_UVLO=1,'Design Converter'!E49, \"\")","v":1},{"$f":"IF(MODE_UVLO=1,\"MΩ\", \"\")","v":"MΩ"},{"$f":"IF(MODE_UVLO=1,'Design Converter'!E49&\"M\", \"\")","v":"1M"}]
[{"$f":"\"RUV2 = \"&C276","v":"RUV2 = 332kΩ"},{"$f":"IF(D184>=1000, D184/1000&\" MΩ\", D184&\" kΩ\")","v":"332 kΩ"},{"$f":"IF(MODE_UVLO=1, IF(D184<1, D184*1000&\"Ω\", IF(D184<1000, D184&\"kΩ\", D184/1000&\"MΩ\")), \"\")","v":"332kΩ"},null,null,{"$f":"IF(MODE_UVLO=1, IF(D184<1, D184*1000, IF(D184<1000, D184, D184/1000)), \"\")","v":332},{"$f":"IF(MODE_UVLO=1, IF(D184<1, \"Ω\", IF(D184<1000,\"kΩ\", \"MΩ\")), \"\")","v":"kΩ"},{"$f":"IF(MODE_UVLO=1, IF(D184<1, D184*1000, IF(D184<1000, D184&\"k\", D184/1000&\"M\")), \"\")","v":"332k"}]
[{"$f":"\"RHYS = \"&C277","v":{"$error":"#REF!"}},{"$f":"IF(#REF!<1000,#REF!& \" kΩ\",#REF!& \" MΩ\")","v":{"$error":"#REF!"}},{"$f":"IF(MODE_UVLO=1, IF(#REF!<1,#REF!* 1000&\"Ω\", IF(#REF!<1000,#REF!& \"kΩ\",#REF!/ 1000&\"MΩ\")), \"\")","v":{"$error":"#REF!"}},null,null,{"$f":"IF(MODE_UVLO=1, IF(#REF!<1,#REF!* 1000, IF(#REF!<1000,#REF!,#REF!/ 1000)), \"\")","v":{"$error":"#REF!"}},{"$f":"IF(MODE_UVLO=1, IF(#REF!<1, \"Ω\", IF(#REF!<1000,\"kΩ\", \"MΩ\")), \"\")","v":{"$error":"#REF!"}},{"$f":"IF(MODE_UVLO=1, IF(#REF!<1,#REF!* 1000, IF(#REF!<1000,#REF!& \"k\",#REF!& \"M\")), \"\")","v":{"$error":"#REF!"}}]
[]
[{"$f":"\"Css = \"&Css*1000000000&\"nF\"","v":{"$error":"#NAME?"}},{"$f":"Css*1000000000&\"nF\"","v":{"$error":"#NAME?"}}]
["Cbst",{"$f":"\"2.2nF\"","v":"2.2nF"},null,{"$f":"B280","v":"2.2nF"}]
[]
[]
["Rset resistor ref des?",{"$f":"IF(MODE_RSET=2, \"YES\", \"NO\")","v":"NO"},{"$f":"IF(MODE_RSET=2, \"R3\", \"\")","v":""},null,null,{"$f":"MODE_RSET","v":1}]
["Rset",{"$f":"IF(MODE_RSET=2, C284&\"kΩ\", \"\")","v":""},{"$f":"IF(MODE_ILIM=3,100,IF(MODE_ILIM=2,56.2,IF(MODE_ILIM=4,24.9,0)))","v":{"$error":"#REF!"}}]
[]
[]
["Rpgood","100kΩ"]
[]
["Cff / Cb?",{"$f":"IF(MODE=2, \"Cff\", IF(MODE=3,\"Cb\",\"\"))","v":"Cb"}]
[{"$f":"\"Cff / Cb=\"&B290","v":"Cff / Cb=47pF"},{"$f":"IF(OR(MODE=2,MODE=3),B141&\"pF\",\"\")","v":"47pF"}]
[]
["Ca?",{"$f":"IF(MODE=3, \"Ca\",\"\")","v":"Ca"},null,{"$f":"Ca","v":2.1999999999999998E-9},{"$f":"Ton_Vinmin","v":1.744209385746398E-6}]
["Ca=",{"$f":"IF(MODE=3,B145&\"pF\",\"\")","v":"2200pF"}]
[]
["Ra?",{"$f":"IF(MODE=3, \"Ra\",\"\")","v":"Ra"},"Injected Ripple"]
["Ra=",{"$f":"IF(MODE=3,Ra&\"kΩ\",\"\")","v":"787kΩ"},{"$f":"(VIN_nom-Vout)*Ton_Vin_nom/(Ra*Ca)/1000","v":2.0031500336455867E-2},{"$f":"ROUNDUP(1000*C296,0)","v":21},null,{"$f":"IF(MODE=3,Ra&\"k\",\"\")","v":"787k"}]
[]
["Lf(emi)",{"$f":"M148&\"µH\"","v":"22µH"}]
["Cf(emi)",{"$f":"M149&\"µF\"","v":"4.7µF"}]
["Df(emi)",{"$f":"M150&\"µF\"","v":"10µF"}]
[]
["Full-load efficiency",{"$f":"ROUND(Efficiency!CE106,1)&\"%\"","v":"83%"}]
["Full-load efficiency",{"$f":"ROUND(Efficiency!CE107,1)&\"%\"","v":"92.8%"}]
["10% load efficiency",{"$f":"ROUND(Efficiency!CE16,1)&\"%\"","v":"71%"},"linear scale only"]
["1% load efficiency",{"$f":"ROUND(Efficiency!CE56,1)&\"%\"","v":"73%"},"log scale only"]
[]
["Blank out",{"$f":"IF(C307=\"y\",\"\",\"|\")","v":"|"},"n"]
[]
["OUTPUT CURRENT",{"$f":"'Design Converter'!$E$10&\"A\"","v":"0.07A"}]
[]
["VIN ",2]
["RT",5]
["EN",7]
["PGOOD",6]
["SS",4]
["ILIM",3]
["GND",10]
["FB",8]
["SW",1]
["HYS",9]

{"sheet":"Standard Value Calculator","index":8,"n_rows":159,"n_cols":11,"rows_kept":159,"cut":false,"hidden":true,"merged":[]}
[]
["Capacitors","Css","Cout","Cin","Cb"]
["Inputs",{"$f":"Css","v":{"$error":"#NAME?"}},{"$f":"Cout","v":4.6999999999999995E-7},{"$f":"Cin","v":2.2000000000000001E-6},{"$f":"Cb","v":0},null,null,"Resistors","inputs","Standard Result"]
["Standard Result",{"$f":"SUM(B6:B158)/1000000000000","v":{"$error":"#NAME?"}},{"$f":"SUM(C6:C158)/1000000000000","v":4.7E-7},{"$f":"SUM(D6:D158)/1000000000000","v":2.2000000000000001E-6},{"$f":"IF(E3=\"OPEN\",\"OPEN\",SUM(E6:E158)/1000000000000)","v":0},null,null,"Rt",{"$f":"Rt","v":158333.33333333334},{"$f":"IF(I4>(INT(0.5+100*POWER(10,IF(96*(LOG(I4)-INT(LOG(I4)))-ROUND(96*(LOG(I4)-INT(LOG(I4))),0)<0,ROUND(96*(LOG(I4)-INT(LOG(I4))),0)-1,ROUND(96*(LOG(I4)-INT(LOG(I4))),0))/96))*POWER(10,INT(LOG(I4))-2)+INT(0.5+100*POWER(10,(IF(96*(LOG(I4)-INT(LOG(I4)))-ROUND(96*(LOG(I4)-INT(LOG(I4))),0)<0,ROUND(96*(LOG(I4)-INT(LOG(I4))),0)-1,ROUND(96*(LOG(I4)-INT(LOG(I4))),0))+1)/96))*POWER(10,INT(LOG(I4))-2))/2,INT(0.5+100*POWER(10,(IF(96*(LOG(I4)-INT(LOG(I4)))-ROUND(96*(LOG(I4)-INT(LOG(I4))),0)<0,ROUND(96*(LOG(I4)-INT(LOG(I4))),0)-1,ROUND(96*(LOG(I4)-INT(LOG(I4))),0))+1)/96))*POWER(10,INT(LOG(I4))-2),INT(0.5+100*POWER(10,IF(96*(LOG(I4)-INT(LOG(I4)))-ROUND(96*(LOG(I4)-INT(LOG(I4))),0)<0,ROUND(96*(LOG(I4)-INT(LOG(I4))),0)-1,ROUND(96*(LOG(I4)-INT(LOG(I4))),0))/96))*POWER(10,INT(LOG(I4))-2))","v":158000},"Ω"]
["(pF)"]
[0.47,{"$f":"IF(IF((B$3*10^12-$A7)*(B$3*10^12-$A6)*-1<0,0,1)*IF(ABS(B$3*10^12-$A7)>(B$3*10^12-$A6),$A6,$A7)=B7,0,IF((B$3*10^12-$A7)*(B$3*10^12-$A6)*-1<0,0,1)*IF(ABS(B$3*10^12-$A7)>(B$3*10^12-$A6),$A6,$A7))","v":{"$error":"#NAME?"}},{"$f":"IF(IF((C$3*10^12-$A7)*(C$3*10^12-$A6)*-1<0,0,1)*IF(ABS(C$3*10^12-$A7)>(C$3*10^12-$A6),$A6,$A7)=C7,0,IF((C$3*10^12-$A7)*(C$3*10^12-$A6)*-1<0,0,1)*IF(ABS(C$3*10^12-$A7)>(C$3*10^12-$A6),$A6,$A7))","v":0},{"$f":"IF(IF((D$3*10^12-$A7)*(D$3*10^12-$A6)*-1<0,0,1)*IF(ABS(D$3*10^12-$A7)>(D$3*10^12-$A6),$A6,$A7)=D7,0,IF((D$3*10^12-$A7)*(D$3*10^12-$A6)*-1<0,0,1)*IF(ABS(D$3*10^12-$A7)>(D$3*10^12-$A6),$A6,$A7))","v":0},{"$f":"IF(IF((E$3*10^12-$A7)*(E$3*10^12-$A6)*-1<0,0,1)*IF(ABS(E$3*10^12-$A7)>(E$3*10^12-$A6),$A6,$A7)=E7,0,IF((E$3*10^12-$A7)*(E$3*10^12-$A6)*-1<0,0,1)*IF(ABS(E$3*10^12-$A7)>(E$3*10^12-$A6),$A6,$A7))","v":0},null,null,"Rshunt",{"$f":"Rshunt","v":{"$error":"#NAME?"}},{"$error":"#NAME?"},"Ω"]
[0.56000000000000005,{"$f":"IF(IF((B$3*10^12-$A8)*(B$3*10^12-$A7)*-1<0,0,1)*IF(ABS(B$3*10^12-$A8)>(B$3*10^12-$A7),$A7,$A8)=B8,0,IF((B$3*10^12-$A8)*(B$3*10^12-$A7)*-1<0,0,1)*IF(ABS(B$3*10^12-$A8)>(B$3*10^12-$A7),$A7,$A8))","v":{"$error":"#NAME?"}},{"$f":"IF(IF((C$3*10^12-$A8)*(C$3*10^12-$A7)*-1<0,0,1)*IF(ABS(C$3*10^12-$A8)>(C$3*10^12-$A7),$A7,$A8)=C8,0,IF((C$3*10^12-$A8)*(C$3*10^12-$A7)*-1<0,0,1)*IF(ABS(C$3*10^12-$A8)>(C$3*10^12-$A7),$A7,$A8))","v":0},{"$f":"IF(IF((D$3*10^12-$A8)*(D$3*10^12-$A7)*-1<0,0,1)*IF(ABS(D$3*10^12-$A8)>(D$3*10^12-$A7),$A7,$A8)=D8,0,IF((D$3*10^12-$A8)*(D$3*10^12-$A7)*-1<0,0,1)*IF(ABS(D$3*10^12-$A8)>(D$3*10^12-$A7),$A7,$A8))","v":0},{"$f":"IF(IF((E$3*10^12-$A8)*(E$3*10^12-$A7)*-1<0,0,1)*IF(ABS(E$3*10^12-$A8)>(E$3*10^12-$A7),$A7,$A8)=E8,0,IF((E$3*10^12-$A8)*(E$3*10^12-$A7)*-1<0,0,1)*IF(ABS(E$3*10^12-$A8)>(E$3*10^12-$A7),$A7,$A8))","v":0},null,null,"Rc1ea",{"$f":"Rcea1","v":{"$error":"#NAME?"}},{"$error":"#NAME?"},"Ω"]
[0.68,{"$error":"#NAME?"},0,0,0]
[0.82,{"$error":"#NAME?"},0,0,0,null,null,"Rfb1",{"$f":"Rfb1_","v":698000},698000,"Ω"]
[1,{"$error":"#NAME?"},0,0,0,null,null,"Rfb2",{"$f":"Rfb2_","v":47056.1797752809},{"$f":"IF(I10=\"OPEN\",\"OPEN\",IF(I10>(INT(0.5+100*POWER(10,IF(96*(LOG(I10)-INT(LOG(I10)))-ROUND(96*(LOG(I10)-INT(LOG(I10))),0)<0,ROUND(96*(LOG(I10)-INT(LOG(I10))),0)-1,ROUND(96*(LOG(I10)-INT(LOG(I10))),0))/96))*POWER(10,INT(LOG(I10))-2)+INT(0.5+100*POWER(10,(IF(96*(LOG(I10)-INT(LOG(I10)))-ROUND(96*(LOG(I10)-INT(LOG(I10))),0)<0,ROUND(96*(LOG(I10)-INT(LOG(I10))),0)-1,ROUND(96*(LOG(I10)-INT(LOG(I10))),0))+1)/96))*POWER(10,INT(LOG(I10))-2))/2,INT(0.5+100*POWER(10,(IF(96*(LOG(I10)-INT(LOG(I10)))-ROUND(96*(LOG(I10)-INT(LOG(I10))),0)<0,ROUND(96*(LOG(I10)-INT(LOG(I10))),0)-1,ROUND(96*(LOG(I10)-INT(LOG(I10))),0))+1)/96))*POWER(10,INT(LOG(I10))-2),INT(0.5+100*POWER(10,IF(96*(LOG(I10)-INT(LOG(I10)))-ROUND(96*(LOG(I10)-INT(LOG(I10))),0)<0,ROUND(96*(LOG(I10)-INT(LOG(I10))),0)-1,ROUND(96*(LOG(I10)-INT(LOG(I10))),0))/96))*POWER(10,INT(LOG(I10))-2)))","v":47500},"Ω"]
[1.2,{"$error":"#NAME?"},0,0,0]
[1.5,{"$error":"#NAME?"},0,0,0]
[1.8,{"$error":"#NAME?"},0,0,0,null,null,"Rs",{"$f":"Rs_ideal*1000","v":{"$error":"#NAME?"}},{"$f":"IF(I13=0,0,IF(I13>(INT(0.5+100*POWER(10,IF(96*(LOG(I13)-INT(LOG(I13)))-ROUND(96*(LOG(I13)-INT(LOG(I13))),0)<0,ROUND(96*(LOG(I13)-INT(LOG(I13))),0)-1,ROUND(96*(LOG(I13)-INT(LOG(I13))),0))/96))*POWER(10,INT(LOG(I13))-2)+INT(0.5+100*POWER(10,(IF(96*(LOG(I13)-INT(LOG(I13)))-ROUND(96*(LOG(I13)-INT(LOG(I13))),0)<0,ROUND(96*(LOG(I13)-INT(LOG(I13))),0)-1,ROUND(96*(LOG(I13)-INT(LOG(I13))),0))+1)/96))*POWER(10,INT(LOG(I13))-2))/2,INT(0.5+100*POWER(10,(IF(96*(LOG(I13)-INT(LOG(I13)))-ROUND(96*(LOG(I13)-INT(LOG(I13))),0)<0,ROUND(96*(LOG(I13)-INT(LOG(I13))),0)-1,ROUND(96*(LOG(I13)-INT(LOG(I13))),0))+1)/96))*POWER(10,INT(LOG(I13))-2),INT(0.5+100*POWER(10,IF(96*(LOG(I13)-INT(LOG(I13)))-ROUND(96*(LOG(I13)-INT(LOG(I13))),0)<0,ROUND(96*(LOG(I13)-INT(LOG(I13))),0)-1,ROUND(96*(LOG(I13)-INT(LOG(I13))),0))/96))*POWER(10,INT(LOG(I13))-2)))","v":{"$error":"#NAME?"}},"mΩ"]
[2.2000000000000002,{"$f":"IF(IF((B$3*10^12-$A15)*(B$3*10^12-$A14)*-1<0,0,1)*IF(ABS(B$3*10^12-$A15)>(B$3*10^12-$A14),$A14,$A15)=B15,0,IF((B$3*10^12-$A15)*(B$3*10^12-$A14)*-1<0,0,1)*IF(ABS(B$3*10^12-$A15)>(B$3*10^12-$A14),$A14,$A15))","v":{"$error":"#NAME?"}},{"$f":"IF(IF((C$3*10^12-$A15)*(C$3*10^12-$A14)*-1<0,0,1)*IF(ABS(C$3*10^12-$A15)>(C$3*10^12-$A14),$A14,$A15)=C15,0,IF((C$3*10^12-$A15)*(C$3*10^12-$A14)*-1<0,0,1)*IF(ABS(C$3*10^12-$A15)>(C$3*10^12-$A14),$A14,$A15))","v":0},{"$f":"IF(IF((D$3*10^12-$A15)*(D$3*10^12-$A14)*-1<0,0,1)*IF(ABS(D$3*10^12-$A15)>(D$3*10^12-$A14),$A14,$A15)=D15,0,IF((D$3*10^12-$A15)*(D$3*10^12-$A14)*-1<0,0,1)*IF(ABS(D$3*10^12-$A15)>(D$3*10^12-$A14),$A14,$A15))","v":0},{"$f":"IF(IF((E$3*10^12-$A15)*(E$3*10^12-$A14)*-1<0,0,1)*IF(ABS(E$3*10^12-$A15)>(E$3*10^12-$A14),$A14,$A15)=E15,0,IF((E$3*10^12-$A15)*(E$3*10^12-$A14)*-1<0,0,1)*IF(ABS(E$3*10^12-$A15)>(E$3*10^12-$A14),$A14,$A15))","v":0},null,null,"Cslope_ideal",{"$f":"Cslope_ideal","v":{"$error":"#NAME?"}},{"$f":"#REF!*1000000000000","v":{"$error":"#REF!"}},"pF"]
[2.7,{"$error":"#NAME?"},0,0,0]
[3.3,{"$error":"#NAME?"},0,0,0,null,null,"Ruv1",{"$f":"Ruvlo1","v":1000},{"$f":"IF(I16=\"OPEN\",\"OPEN\",IF(I16>(INT(0.5+100*POWER(10,IF(96*(LOG(I16)-INT(LOG(I16)))-ROUND(96*(LOG(I16)-INT(LOG(I16))),0)<0,ROUND(96*(LOG(I16)-INT(LOG(I16))),0)-1,ROUND(96*(LOG(I16)-INT(LOG(I16))),0))/96))*POWER(10,INT(LOG(I16))-2)+INT(0.5+100*POWER(10,(IF(96*(LOG(I16)-INT(LOG(I16)))-ROUND(96*(LOG(I16)-INT(LOG(I16))),0)<0,ROUND(96*(LOG(I16)-INT(LOG(I16))),0)-1,ROUND(96*(LOG(I16)-INT(LOG(I16))),0))+1)/96))*POWER(10,INT(LOG(I16))-2))/2,INT(0.5+100*POWER(10,(IF(96*(LOG(I16)-INT(LOG(I16)))-ROUND(96*(LOG(I16)-INT(LOG(I16))),0)<0,ROUND(96*(LOG(I16)-INT(LOG(I16))),0)-1,ROUND(96*(LOG(I16)-INT(LOG(I16))),0))+1)/96))*POWER(10,INT(LOG(I16))-2),INT(0.5+100*POWER(10,IF(96*(LOG(I16)-INT(LOG(I16)))-ROUND(96*(LOG(I16)-INT(LOG(I16))),0)<0,ROUND(96*(LOG(I16)-INT(LOG(I16))),0)-1,ROUND(96*(LOG(I16)-INT(LOG(I16))),0))/96))*POWER(10,INT(LOG(I16))-2)))","v":1000},"kΩ"]
[3.9,{"$error":"#NAME?"},0,0,0,null,null,"Ruv2",{"$f":"Ruvlo2","v":333.33333333333331},{"$f":"IF(I17=\"OPEN\",\"OPEN\",IF(I17>(INT(0.5+100*POWER(10,IF(96*(LOG(I17)-INT(LOG(I17)))-ROUND(96*(LOG(I17)-INT(LOG(I17))),0)<0,ROUND(96*(LOG(I17)-INT(LOG(I17))),0)-1,ROUND(96*(LOG(I17)-INT(LOG(I17))),0))/96))*POWER(10,INT(LOG(I17))-2)+INT(0.5+100*POWER(10,(IF(96*(LOG(I17)-INT(LOG(I17)))-ROUND(96*(LOG(I17)-INT(LOG(I17))),0)<0,ROUND(96*(LOG(I17)-INT(LOG(I17))),0)-1,ROUND(96*(LOG(I17)-INT(LOG(I17))),0))+1)/96))*POWER(10,INT(LOG(I17))-2))/2,INT(0.5+100*POWER(10,(IF(96*(LOG(I17)-INT(LOG(I17)))-ROUND(96*(LOG(I17)-INT(LOG(I17))),0)<0,ROUND(96*(LOG(I17)-INT(LOG(I17))),0)-1,ROUND(96*(LOG(I17)-INT(LOG(I17))),0))+1)/96))*POWER(10,INT(LOG(I17))-2),INT(0.5+100*POWER(10,IF(96*(LOG(I17)-INT(LOG(I17)))-ROUND(96*(LOG(I17)-INT(LOG(I17))),0)<0,ROUND(96*(LOG(I17)-INT(LOG(I17))),0)-1,ROUND(96*(LOG(I17)-INT(LOG(I17))),0))/96))*POWER(10,INT(LOG(I17))-2)))","v":332},"kΩ"]
[4.7,{"$error":"#NAME?"},0,0,0,null,null,"Rhys",{"$f":"Rhys","v":{"$error":"#NAME?"}},{"$f":"IF(I18=\"OPEN\",\"OPEN\",IF(I18>(INT(0.5+100*POWER(10,IF(96*(LOG(I18)-INT(LOG(I18)))-ROUND(96*(LOG(I18)-INT(LOG(I18))),0)<0,ROUND(96*(LOG(I18)-INT(LOG(I18))),0)-1,ROUND(96*(LOG(I18)-INT(LOG(I18))),0))/96))*POWER(10,INT(LOG(I18))-2)+INT(0.5+100*POWER(10,(IF(96*(LOG(I18)-INT(LOG(I18)))-ROUND(96*(LOG(I18)-INT(LOG(I18))),0)<0,ROUND(96*(LOG(I18)-INT(LOG(I18))),0)-1,ROUND(96*(LOG(I18)-INT(LOG(I18))),0))+1)/96))*POWER(10,INT(LOG(I18))-2))/2,INT(0.5+100*POWER(10,(IF(96*(LOG(I18)-INT(LOG(I18)))-ROUND(96*(LOG(I18)-INT(LOG(I18))),0)<0,ROUND(96*(LOG(I18)-INT(LOG(I18))),0)-1,ROUND(96*(LOG(I18)-INT(LOG(I18))),0))+1)/96))*POWER(10,INT(LOG(I18))-2),INT(0.5+100*POWER(10,IF(96*(LOG(I18)-INT(LOG(I18)))-ROUND(96*(LOG(I18)-INT(LOG(I18))),0)<0,ROUND(96*(LOG(I18)-INT(LOG(I18))),0)-1,ROUND(96*(LOG(I18)-INT(LOG(I18))),0))/96))*POWER(10,INT(LOG(I18))-2)))","v":{"$error":"#NAME?"}},"kΩ"]
[5.6,{"$error":"#NAME?"},0,0,0]
[6.8,{"$error":"#NAME?"},0,0,0,null,null,"Ra",{"$f":"'Variable Mgmt'!D147","v":788.23953823953832},{"$f":"IF(I20=\"OPEN\",\"OPEN\",IF(I20>(INT(0.5+100*POWER(10,IF(96*(LOG(I20)-INT(LOG(I20)))-ROUND(96*(LOG(I20)-INT(LOG(I20))),0)<0,ROUND(96*(LOG(I20)-INT(LOG(I20))),0)-1,ROUND(96*(LOG(I20)-INT(LOG(I20))),0))/96))*POWER(10,INT(LOG(I20))-2)+INT(0.5+100*POWER(10,(IF(96*(LOG(I20)-INT(LOG(I20)))-ROUND(96*(LOG(I20)-INT(LOG(I20))),0)<0,ROUND(96*(LOG(I20)-INT(LOG(I20))),0)-1,ROUND(96*(LOG(I20)-INT(LOG(I20))),0))+1)/96))*POWER(10,INT(LOG(I20))-2))/2,INT(0.5+100*POWER(10,(IF(96*(LOG(I20)-INT(LOG(I20)))-ROUND(96*(LOG(I20)-INT(LOG(I20))),0)<0,ROUND(96*(LOG(I20)-INT(LOG(I20))),0)-1,ROUND(96*(LOG(I20)-INT(LOG(I20))),0))+1)/96))*POWER(10,INT(LOG(I20))-2),INT(0.5+100*POWER(10,IF(96*(LOG(I20)-INT(LOG(I20)))-ROUND(96*(LOG(I20)-INT(LOG(I20))),0)<0,ROUND(96*(LOG(I20)-INT(LOG(I20))),0)-1,ROUND(96*(LOG(I20)-INT(LOG(I20))),0))/96))*POWER(10,INT(LOG(I20))-2)))","v":787},"kΩ"]
[8.1999999999999993,{"$error":"#NAME?"},0,0,0]
[10,{"$error":"#NAME?"},0,0,0]
[12,{"$error":"#NAME?"},0,0,0]
[15,{"$error":"#NAME?"},0,0,0]
[18,{"$error":"#NAME?"},0,0,0]
[22,{"$error":"#NAME?"},0,0,0]
[27,{"$error":"#NAME?"},0,0,0]
[33,{"$error":"#NAME?"},0,0,0]
[39,{"$error":"#NAME?"},0,0,0]
[47,{"$error":"#NAME?"},0,0,0]
[56,{"$error":"#NAME?"},0,0,0]
[68,{"$error":"#NAME?"},0,0,0]
[82,{"$error":"#NAME?"},0,0,0]
[{"$f":"A22*10","v":100},{"$error":"#NAME?"},0,0,0]
[{"$f":"A23*10","v":120},{"$error":"#NAME?"},0,0,0]
[150,{"$error":"#NAME?"},0,0,0]
[180,{"$error":"#NAME?"},0,0,0]
[220,{"$error":"#NAME?"},0,0,{"$f":"IF(IF((E$3*10^12-$A39)*(E$3*10^12-$A38)*-1<0,0,1)*IF(ABS(E$3*10^12-$A39)>(E$3*10^12-$A38),$A38,$A39)=E39,0,IF((E$3*10^12-$A39)*(E$3*10^12-$A38)*-1<0,0,1)*IF(ABS(E$3*10^12-$A39)>(E$3*10^12-$A38),$A38,$A39))","v":0}]
[270,{"$error":"#NAME?"},0,0,0]
[330,{"$error":"#NAME?"},0,0,0]
[390,{"$error":"#NAME?"},0,0,0]
[470,{"$error":"#NAME?"},0,0,0]
[560,{"$error":"#NAME?"},0,0,0]
[680,{"$error":"#NAME?"},0,0,0]
[{"$f":"A33*10","v":820},{"$error":"#NAME?"},0,0,0]
[1000,{"$error":"#NAME?"},0,0,0]
[1200,{"$error":"#NAME?"},0,0,0]
[1500,{"$error":"#NAME?"},0,0,0]
[1800,{"$error":"#NAME?"},0,0,0]
[2200,{"$error":"#NAME?"},0,0,0]
[2700,{"$error":"#NAME?"},0,0,0]
[3300,{"$error":"#NAME?"},0,0,0]
[3900,{"$error":"#NAME?"},0,0,0]
[4700,{"$error":"#NAME?"},0,0,0]
[5600,{"$error":"#NAME?"},0,0,0]
[6800,{"$error":"#NAME?"},0,0,0]
[8200,{"$error":"#NAME?"},0,0,0]
[10000,{"$error":"#NAME?"},0,0,0]
[12000,{"$error":"#NAME?"},0,0,0]
[15000,{"$error":"#NAME?"},0,0,0]
[18000,{"$error":"#NAME?"},0,0,0]
[22000,{"$error":"#NAME?"},0,0,0]
[27000,{"$error":"#NAME?"},0,0,0]
[33000,{"$error":"#NAME?"},0,0,0]
[39000,{"$error":"#NAME?"},0,0,0]
[47000,{"$error":"#NAME?"},0,0,0]
[56000,{"$error":"#NAME?"},0,0,0]
[68000,{"$error":"#NAME?"},0,0,0]
[82000,{"$error":"#NAME?"},0,0,0]
[100000,{"$error":"#NAME?"},{"$f":"IF(IF((C$3*10^12-$A71)*(C$3*10^12-$A70)*-1<0,0,1)*IF(ABS(C$3*10^12-$A71)>(C$3*10^12-$A70),$A70,$A71)=C71,0,IF((C$3*10^12-$A71)*(C$3*10^12-$A70)*-1<0,0,1)*IF(ABS(C$3*10^12-$A71)>(C$3*10^12-$A70),$A70,$A71))","v":0},{"$f":"IF(IF((D$3*10^12-$A71)*(D$3*10^12-$A70)*-1<0,0,1)*IF(ABS(D$3*10^12-$A71)>(D$3*10^12-$A70),$A70,$A71)=D71,0,IF((D$3*10^12-$A71)*(D$3*10^12-$A70)*-1<0,0,1)*IF(ABS(D$3*10^12-$A71)>(D$3*10^12-$A70),$A70,$A71))","v":0},{"$f":"IF(IF((E$3*10^12-$A71)*(E$3*10^12-$A70)*-1<0,0,1)*IF(ABS(E$3*10^12-$A71)>(E$3*10^12-$A70),$A70,$A71)=E71,0,IF((E$3*10^12-$A71)*(E$3*10^12-$A70)*-1<0,0,1)*IF(ABS(E$3*10^12-$A71)>(E$3*10^12-$A70),$A70,$A71))","v":0}]
[120000,{"$f":"IF(IF((B$3*10^12-$A72)*(B$3*10^12-$A71)*-1<0,0,1)*IF(ABS(B$3*10^12-$A72)>(B$3*10^12-$A71),$A71,$A72)=B72,0,IF((B$3*10^12-$A72)*(B$3*10^12-$A71)*-1<0,0,1)*IF(ABS(B$3*10^12-$A72)>(B$3*10^12-$A71),$A71,$A72))","v":{"$error":"#NAME?"}},{"$f":"IF(IF((C$3*10^12-$A72)*(C$3*10^12-$A71)*-1<0,0,1)*IF(ABS(C$3*10^12-$A72)>(C$3*10^12-$A71),$A71,$A72)=C72,0,IF((C$3*10^12-$A72)*(C$3*10^12-$A71)*-1<0,0,1)*IF(ABS(C$3*10^12-$A72)>(C$3*10^12-$A71),$A71,$A72))","v":0},{"$f":"IF(IF((D$3*10^12-$A72)*(D$3*10^12-$A71)*-1<0,0,1)*IF(ABS(D$3*10^12-$A72)>(D$3*10^12-$A71),$A71,$A72)=D72,0,IF((D$3*10^12-$A72)*(D$3*10^12-$A71)*-1<0,0,1)*IF(ABS(D$3*10^12-$A72)>(D$3*10^12-$A71),$A71,$A72))","v":0},0]
[150000,{"$error":"#NAME?"},0,0,0]
[180000,{"$error":"#NAME?"},0,0,0]
[220000,{"$error":"#NAME?"},0,0,0]
[270000,{"$error":"#NAME?"},0,0,0]
[330000,{"$error":"#NAME?"},0,0,0]
[390000,{"$error":"#NAME?"},470000,0,0]
[470000,{"$error":"#NAME?"},0,0,0]
[560000,{"$error":"#NAME?"},0,0,0]
[680000,{"$error":"#NAME?"},0,0,0]
[820000,{"$error":"#NAME?"},0,0,0]
[1000000,{"$error":"#NAME?"},0,0,0]
[1200000,{"$error":"#NAME?"},0,0,0]
[1500000,{"$error":"#NAME?"},0,0,0]
[1800000,{"$error":"#NAME?"},0,0,0]
[2200000,{"$error":"#NAME?"},0,2200000,0]
[2700000,{"$error":"#NAME?"},0,0,0]
[3300000,{"$error":"#NAME?"},0,0,0]
[3900000,{"$error":"#NAME?"},0,0,0]
[4700000,{"$error":"#NAME?"},0,0,0]
[5600000,{"$error":"#NAME?"},0,0,0]
[6800000,{"$error":"#NAME?"},0,0,0]
[8200000,{"$error":"#NAME?"},0,0,0]
[10000000,{"$error":"#NAME?"},0,0,0]
[12000000,{"$error":"#NAME?"},0,0,0]
[15000000,{"$error":"#NAME?"},0,0,0]
[18000000,{"$error":"#NAME?"},0,0,0]
[22000000,{"$error":"#NAME?"},0,0,0]
[{"$f":"A87*10","v":27000000},{"$error":"#NAME?"},0,0,0]
[33000000,{"$error":"#NAME?"},0,0,0]
[39000000,{"$error":"#NAME?"},0,0,0]
[47000000,{"$error":"#NAME?"},0,0,{"$f":"IF(IF((E$3*10^12-$A103)*(E$3*10^12-$A102)*-1<0,0,1)*IF(ABS(E$3*10^12-$A103)>(E$3*10^12-$A102),$A102,$A103)=E103,0,IF((E$3*10^12-$A103)*(E$3*10^12-$A102)*-1<0,0,1)*IF(ABS(E$3*10^12-$A103)>(E$3*10^12-$A102),$A102,$A103))","v":0}]
[56000000,{"$error":"#NAME?"},0,{"$f":"IF(IF((D$3*10^12-$A104)*(D$3*10^12-$A103)*-1<0,0,1)*IF(ABS(D$3*10^12-$A104)>(D$3*10^12-$A103),$A103,$A104)=D104,0,IF((D$3*10^12-$A104)*(D$3*10^12-$A103)*-1<0,0,1)*IF(ABS(D$3*10^12-$A104)>(D$3*10^12-$A103),$A103,$A104))","v":0},0]
[68000000,{"$error":"#NAME?"},0,0,0]
[82000000,{"$error":"#NAME?"},0,0,0]
[100000000,{"$error":"#NAME?"},0,0,0]
[120000000,{"$error":"#NAME?"},0,0,0]
[150000000,{"$error":"#NAME?"},0,0,0]
[180000000,{"$error":"#NAME?"},0,0,0]
[220000000,{"$error":"#NAME?"},0,0,0]
[270000000,{"$error":"#NAME?"},0,0,0]
[330000000,{"$error":"#NAME?"},0,0,0]
[390000000,{"$error":"#NAME?"},0,0,0]
[470000000,{"$error":"#NAME?"},0,0,0]
[560000000,{"$error":"#NAME?"},0,0,0]
[680000000,{"$error":"#NAME?"},0,0,0]
[820000000,{"$error":"#NAME?"},0,0,0]
[1000000000,{"$error":"#NAME?"},0,0,0]
[1200000000,{"$error":"#NAME?"},0,0,0]
[1500000000,{"$error":"#NAME?"},0,0,0]
[1800000000,{"$error":"#NAME?"},0,0,0]
[2200000000,{"$error":"#NAME?"},0,0,0]
[2700000000,{"$error":"#NAME?"},0,0,0]
[3300000000,{"$error":"#NAME?"},0,0,0]
[3900000000,{"$error":"#NAME?"},0,0,0]
[4700000000,{"$error":"#NAME?"},0,0,0]
[5600000000,{"$error":"#NAME?"},0,0,0]
[6800000000,{"$error":"#NAME?"},0,0,0]
[8200000000,{"$error":"#NAME?"},0,0,0]
[10000000000,{"$error":"#NAME?"},0,0,0]
[12000000000,{"$error":"#NAME?"},0,0,0]
[15000000000,{"$error":"#NAME?"},0,0,0]
[18000000000,{"$error":"#NAME?"},0,0,0]
[22000000000,{"$error":"#NAME?"},{"$f":"IF(IF((C$3*10^12-$A135)*(C$3*10^12-$A134)*-1<0,0,1)*IF(ABS(C$3*10^12-$A135)>(C$3*10^12-$A134),$A134,$A135)=C135,0,IF((C$3*10^12-$A135)*(C$3*10^12-$A134)*-1<0,0,1)*IF(ABS(C$3*10^12-$A135)>(C$3*10^12-$A134),$A134,$A135))","v":0},0,{"$f":"IF(IF((E$3*10^12-$A135)*(E$3*10^12-$A134)*-1<0,0,1)*IF(ABS(E$3*10^12-$A135)>(E$3*10^12-$A134),$A134,$A135)=E135,0,IF((E$3*10^12-$A135)*(E$3*10^12-$A134)*-1<0,0,1)*IF(ABS(E$3*10^12-$A135)>(E$3*10^12-$A134),$A134,$A135))","v":0}]
[27000000000,{"$f":"IF(IF((B$3*10^12-$A136)*(B$3*10^12-$A135)*-1<0,0,1)*IF(ABS(B$3*10^12-$A136)>(B$3*10^12-$A135),$A135,$A136)=B136,0,IF((B$3*10^12-$A136)*(B$3*10^12-$A135)*-1<0,0,1)*IF(ABS(B$3*10^12-$A136)>(B$3*10^12-$A135),$A135,$A136))","v":{"$error":"#NAME?"}},0,0,0]
[33000000000,{"$error":"#NAME?"},0,0,0]
[39000000000,{"$error":"#NAME?"},0,0,0]
[47000000000,{"$error":"#NAME?"},0,0,0]
[56000000000,{"$error":"#NAME?"},0,0,0]
[68000000000,{"$error":"#NAME?"},0,0,0]
[82000000000,{"$error":"#NAME?"},0,0,0]
[100000000000,{"$error":"#NAME?"},0,0,0]
[120000000000,{"$error":"#NAME?"},0,0,0]
[150000000000,{"$error":"#NAME?"},0,0,0]
[180000000000,{"$error":"#NAME?"},0,0,0]
[220000000000,{"$error":"#NAME?"},0,0,0]
[270000000000,{"$error":"#NAME?"},0,0,0]
[330000000000,{"$error":"#NAME?"},0,0,0]
[390000000000,{"$error":"#NAME?"},0,0,0]
[470000000000,{"$error":"#NAME?"},0,0,0]
[560000000000,{"$error":"#NAME?"},0,0,0]
[680000000000,{"$error":"#NAME?"},0,0,0]
[820000000000,{"$error":"#NAME?"},0,0,0]
[1000000000000,{"$error":"#NAME?"},0,0,0]
[1200000000000,{"$error":"#NAME?"},0,0,0]
[1500000000000,{"$error":"#NAME?"},0,0,0]
[1800000000000,{"$error":"#NAME?"},0,0,0]
[2200000000000,{"$error":"#NAME?"},0,0,0]
[2700000000000,{"$error":"#NAME?"},2700000000000,2700000000000,2700000000000]

{"sheet":"Efficiency","index":9,"n_rows":114,"n_cols":88,"rows_kept":114,"cut":false,"hidden":true,"merged":[[0,0,2,4],[1,6,1,7],[3,0,3,4],[3,10,3,21]]}
["LM5164 (COT) Efficiency Calculator"]
[null,null,null,null,null,null,"TERMS OF USE",null,null,{"$f":"CoutEsr","v":1.0999999999999999E-2}]
[]
[null,null,null,null,null,null,null,"Currents",null,null,"Miscellaneous",null,null,null,null,null,null,null,null,null,null,null,"Inductor",null,null,null,"Cout",null,null,"Cin",null,null,"High-side MOSFET Losses ",null,null,null,null,null,null,null,null,"Low-side MOSFET Losses ",null,null,"Diode",null,null,null,null,null,null,null,"RESULTS"]
["Input Parameters",null,null,null,null,null,null,"Step","Iout (A)","Ripple Current pk-pk (A)","Peak Current (A)","Valley Current (A)","VOUT Hysteresis +Undershoot (2us Delay) (mV)","Vout Rise per Pulse (mV)","Number of Pulses in DCM","VOUT Ripple (mV)","Off Time (sec)","Duty Cycle","Switching Frequency (Hz)","Active Mode Duration (sec)","Sleep Mode Duration (sec)","Operating Quiescent Current (A)","Irms (A)","Inductor DCR Loss @ 25°C (W)","Inductor Core Loss  (W)","Total Inductor Loss (W)","Irms (A)","Cout ESR Loss (W)","Total Cout Loss (W)","Irms (A)","Cin ESR Loss (W)","Total Cin Loss (W)","Irms (A)","Rdson HS Loss @ 25°C (W)","HS Gate Qg Loss (W)     ","SW Rise Time (ns)","SW Fall Time (ns)","HS Switching  Loss (W)","Coss Loss (W)","Total HS FET AC Loss (W)","Total HS FET Loss (W)","Irms (A)","Rdson LS Loss @ 25°C (W)","LS Gate Qg Loss (W)","Reverse Recovery & Leakage Losses","DeadTime Loss @ 25°C (W)","Total LS FET AC Loss (W)","Total LS FET Loss (W)","Quiescent Loss (W)","LDO + Quiescent Loss (W)","Total Gate Drive Loss (W)","Total Power Loss in IC (W)","Total Converter Power Loss (W)","Pout (W)","EFF (%)","High-side MOSFET Rdson %","Low-side MOSFET Rdson %","Gate Drive (Qg) Loss from Vin %","High-side MOSFET AC Loss %","Reverse Recovery & Leakage Loss %","Deadtime Loss %","Low-side MOSFET AC Loss %","Inductor Cu Loss %","Inductor Core Loss %","Cin ESR %","Cout ESR %","LDO + Quiescent Current Loss %","Total Loss %","Overall Eff %","Overall Eff","Current (mA)","Keep for \"previous\" data series","Keep for \"previous\" data series","Frequency (kHz)",null,"Coss",null,"Total Power Loss in IC (mW)","LDO + Quiescent Loss (mW)","Total Inductor Loss (mW)",null,null,"Overall Eff","Total Power Loss in IC (W)","LDO + Quiescent Loss (mW)","Total Inductor Loss (mW)","Fsw (kHz)","Ripple (mV)"]
["Design","Input Value","Units","Std Units","Description",null,null,0.04,{"$f":"IF(PLOT_TYPE=1, H6/100*Iout, min_I*EXP(H6*rr/100))","v":2.8000000000000003E-5},{"$f":"IF(I6<Icrit, (Vin-(Rdcr+RdsonTop)*Iripple/2-Vout)/L*OnTime, (Vin-(Rdcr+RdsonTop)*I6-Vout)/L*OnTime)","v":7.3615061321327738E-2},{"$f":"IF(I6<Icrit, (Vin-(Rdcr+RdsonTop)*Iripple/2-Vout)/L*OnTime, I6+((Vin-(Rdcr+RdsonTop)*J6-Vout)/L*OnTime)/2)","v":7.3615061321327738E-2},{"$f":"IF(I6<Icrit, 0, I6-((Vin-(Rdcr+RdsonTop)*K6-Vout)/L*OnTime)/2)","v":0},{"$f":"1000*((((J6/2)-I6)*0.000002/Cout+Vout/306))","v":218.60014437718181},{"$f":"IF(I6<Icrit, 1000*SQRT((J6*CoutEsr)^2+(((J6/2)-I6)*(OnTime+OffTime)/Cout)^2), 1000*J6*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":259.6074474148997},{"$f":"ROUNDUP(M6/N6,0)","v":1},{"$f":"IF(I6<Icrit, 1000*((N6/1000)*O6), 1000*J6*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":259.6074474148997},{"$f":"IF(I6<Icrit, L*J6/(Vout+J6/2*(RdsonBot+Rdcr)), L*J6/(Vout+I6*(RdsonBot+Rdcr)))","v":1.8170476072160916E-6},{"$f":"OnTime*S6","v":3.4499661172981538E-4},{"$f":"IF(I6<Icrit,I6/((OnTime+Q6)*J6/2),1/(OnTime+Q6))","v":228.78722672608808},{"$f":"IF(1/S6-OnTime-Q6>Tsleep, OnTime+Q6+Tsleep, 1/S6)","v":8.3249841151525998E-6},{"$f":"IF(1/S6-OnTime-Q6>Tsleep, 1/S6-OnTime-Q6-Tsleep, 0)","v":4.3625484003384047E-3},{"$f":"S6*(T6*Iq_active+U6*Iq_sleep)","v":1.1238022518358926E-5},{"$f":"IF(I6<Icrit,Iripple*SQRT((OnTime+OffTime)*S6/3), SQRT(I6^2+Iripple^2/12))","v":1.1683559245390636E-3},{"$f":"W6^2*Rdcr","v":1.1193455644525347E-6},{"$f":"Core_Loss/1000*S6/$S$106","v":7.5899424559203101E-5},{"$f":"(Y6+X6*(1+Ltc*(Ta-25)))/(1-X6*Ltc*ThetaCa)","v":7.7018783917357094E-5},{"$f":"Iripple/SQRT(12)*SQRT((OnTime+Q6)*S6)","v":5.8483937221605851E-4},{"$f":"RCoutEsr*AA6^2","v":3.7624080042348076E-9},{"$f":"AB6","v":3.7624080042348076E-9},{"$f":"SQRT($R6)*SQRT($I6^2*(1-R6)+(Iripple^2)/12)","v":3.9385260404998476E-4},{"$f":"RCinEsr*AD6^2","v":3.1023974743390813E-10},{"$f":"AE6","v":3.1023974743390813E-10},{"$f":"IF(I6<Icrit,Iripple*SQRT((OnTime)*S6/3), SQRT(OnTime*S6*(I6^2+Iripple^2/12)))","v":7.8770452158896307E-4},{"$f":"RdsonTop*AG6^2","v":4.2626866995887603E-7},{"$f":"QgTop*S6*Vdd","v":9.1858071530524358E-7},{"$f":"20*VIN_nom/24","v":35},{"$f":"IF(I6<Icrit, Csw*Vin/Iripple*1000000000, Csw*Vin/(I6+Iripple/2)*1000000000)","v":91.485596098664772},{"$f":"IF(I6<Icrit, Vin*(I6+Iripple/2)*AK6/1000000000/2*S6, Vin*(I6-Iripple/2)*AJ6/1000000000/2*S6 + Vin*(I6+Iripple/2)*AK6/1000000000/2*S6)","v":1.6155533990453052E-5},{"$f":"IF(I6<Icrit, Csw*(Vin)^2*S6/2, Csw*Vin^2*S6/2)","v":3.2286453435585543E-5},{"$f":"AI6+AL6+AM6","v":4.9360568141343841E-5},{"$f":"(AI6+AL6+AM6+AH6*(1+RdsonTopTc*(Ta-25)))/(1-AH6*RdsonTopTc*ThetaJA)","v":4.9786840736417111E-5},{"$f":"IF(I6<Icrit,Iripple*SQRT((OffTime)*S6/3), SQRT(OffTime*S6*(I6^2+Iripple^2/12)))","v":8.6288884166724103E-4},{"$f":"RdsonBot*AP6^2","v":2.2635145453444522E-7},{"$f":"QgBot*S6*Vdd","v":2.516659493986969E-6},{"$f":"IF(I6<Icrit, Vin*Idss*R6, QrrBot*(I6-Iripple/2)/1*S6*Vin+Vin*Idss*R6)","v":0},{"$f":"IF(I6<Icrit, dead1*S6*(I6+Iripple/2)*((I6+Iripple/2)*BDserR+VSD), dead1*S6*(I6+Iripple/2)*((I6+Iripple/2)*BDserR+VSD)+dead2*S6*(I6-Iripple/2)*((I6-Iripple/2)*BDserR+VSD))","v":1.3516368708294145E-7},{"$f":"AR6+AS6+AT6","v":2.6518231810699106E-6},{"$f":"(AR6+AS6+AT6+AQ6*(1+RdsonBotTc*(Ta-25)))/(1-AQ6*RdsonBotTc*ThetaJA)","v":2.8781747560954044E-6},{"$f":"Vin*V6+Vout*Ifb/0.8","v":1.0772954031822084E-3},{"$f":"(Vin-Vdd)*(S6*QgBot+S6*QgTop)+AW6","v":1.1027161807309707E-3},{"$f":"AI6+AR6","v":3.4352402092922126E-6},{"$f":"AO6+AV6+AX6+AY6","v":1.1588164364327753E-3},{"$f":"SUM(Z6,AC6,AF6,AZ6)","v":1.2358392929978841E-3},{"$f":"Vout*I6","v":5.3200000000000003E-4},{"$f":"BB6/(BB6+BA6)","v":0.30093233140996645},{"$f":"(AO6-AN6)/($BB6+$BA6)","v":2.4112632678867585E-4},{"$f":"(AV6-AU6)/($BB6+$BA6)","v":1.2803854735101466E-4},{"$f":"Vin*S6*(QgBot+QgTop)/($BB6+$BA6)","v":1.6322760712666844E-2},{"$f":"AN6/($BB6+$BA6)","v":2.7921411373111122E-2},{"$f":"AS6/(BA6+BB6)","v":0},{"$f":"AT6/($BB6+$BA6)","v":7.645699901473071E-5},{"$f":"AU6/($BB6+$BA6)","v":1.5000363390345146E-3},{"$f":"X6/($BB6+$BA6)","v":6.3317156083478592E-4},{"$f":"Y6/($BB6+$BA6)","v":4.2933441325706492E-2},{"$f":"(AF6)/($BB6+$BA6)","v":1.7549092197617506E-7},{"$f":"(AC6)/($BB6+$BA6)","v":2.1282522790035705E-6},{"$f":"AX6/($BB6+$BA6)","v":0.62376494577230246},{"$f":"SUM(BD6:BO6)","v":0.71352369270001159},{"$f":"BC6","v":0.30093233140996645},{"$f":"100*BQ6","v":30.093233140996645},{"$f":"I6*1000","v":2.8000000000000004E-2},8.7924221262065743,{"$f":"BT6/100","v":8.7924221262065741E-2},{"$f":"S6/1000","v":0.22878722672608809},null,{"$f":"AM6/($BB6+$BA6)","v":1.8263228769417439E-2},null,{"$f":"AZ6","v":1.1588164364327753E-3},{"$f":"AX6","v":1.1027161807309707E-3},{"$f":"Z6","v":7.7018783917357094E-5},null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR6, IF(MODE_ILIM=4,#REF!,#REF!))","v":30.093233140996645},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ6, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.1588164364327753E-3},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA6, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.1027161807309707E-3},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB6, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.7018783917357094E-5},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S6, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":0.22878722672608809},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P6, IF(MODE_ILIM=4,#REF!,#REF!))","v":259.6074474148997}]
[null,null,null,null,null,null,null,1,7.000000000000001E-4,7.3615061321327738E-2,7.3615061321327738E-2,0,{"$f":"IF(I7<Icrit, 1000*((((J7/2)-I7)*0.000002/Cout+Vout/306)), 1000*J7*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":215.74056990909671},254.86419788488402,{"$f":"ROUNDUP(M7/N7,0)","v":1},254.86419788488402,1.8170476072160916E-6,{"$f":"OnTime*S7","v":8.6249152932453849E-3},5719.6806681522021,{"$f":"IF(1/S7-OnTime-Q7>Tsleep, OnTime+Q7+Tsleep, 1/S7)","v":8.3249841151525998E-6},{"$f":"IF(1/S7-OnTime-Q7>Tsleep, 1/S7-OnTime-Q7-Tsleep, 0)","v":1.665099512629897E-4},4.0950562958973125E-5,{"$f":"IF(I7<Icrit,Iripple*SQRT((OnTime+OffTime)*S7/3), SQRT(I7^2+Iripple^2/12))","v":5.841779622695319E-3},2.7983639111313374E-5,1.8974856139800775E-3,1.9254778741918627E-3,{"$f":"Iripple/SQRT(12)*SQRT((OnTime+Q7)*S7)","v":2.9241968610802926E-3},{"$f":"RCoutEsr*AA7^2","v":9.4060200105870192E-8},{"$f":"AB7","v":9.4060200105870192E-8},{"$f":"SQRT($R7)*SQRT($I7^2*(1-R7)+(Iripple^2)/12)","v":1.9703248059968512E-3},{"$f":"RCinEsr*AD7^2","v":7.7643596822530581E-9},{"$f":"AE7","v":7.7643596822530581E-9},{"$f":"IF(I7<Icrit,Iripple*SQRT((OnTime)*S7/3), SQRT(OnTime*S7*(I7^2+Iripple^2/12)))","v":3.9385226079448159E-3},{"$f":"RdsonTop*AG7^2","v":1.0656716748971904E-5},{"$f":"QgTop*S7*Vdd","v":2.2964517882631092E-5},35,91.485596098664772,4.1127271335749202E-4,8.0716133588963862E-4,{"$f":"AI7+AL7+AM7","v":1.2413985671297617E-3},1.2520577516341826E-3,4.3144442083362057E-3,{"$f":"RdsonBot*AP7^2","v":5.6587863633611313E-6},6.2916487349674239E-5,0,3.4411604406881777E-6,{"$f":"AR7+AS7+AT7","v":6.6357647790362423E-5},7.2016509525665024E-5,2.3252221016880044E-3,2.960741540407064E-3,8.5881005232305339E-5,{"$f":"AO7+AV7+AX7+AY7","v":4.3706968067992171E-3},6.2962765055508685E-3,1.3300000000000003E-2,{"$f":"BB7/(BB7+BA7)","v":0.67870036413461632},{"$f":"(AO7-AN7)/($BB7+$BA7)","v":5.4393927853598216E-4},{"$f":"(AV7-AU7)/($BB7+$BA7)","v":2.8877229476220457E-4},3.6813138646365789E-2,{"$f":"AN7/($BB7+$BA7)","v":6.3348696206553382E-2},{"$f":"AS7/(BA7+BB7)","v":0},{"$f":"AT7/($BB7+$BA7)","v":1.7560277023614303E-4},{"$f":"AU7/($BB7+$BA7)","v":3.3862375728147057E-3},1.4280079740345919E-3,9.6828885499885289E-2,{"$f":"(AF7)/($BB7+$BA7)","v":3.9621607094866792E-7},{"$f":"(AC7)/($BB7+$BA7)","v":4.7999016588292455E-6},{"$f":"AX7/($BB7+$BA7)","v":0.15108694447990667},{"$f":"SUM(BD7:BO7)","v":0.35390542084082455},0.67870036413461632,{"$f":"100*BQ7","v":67.870036413461634},0.70000000000000007,9.5725635821403898,{"$f":"BT7/100","v":9.5725635821403893E-2},5.7196806681522023,null,4.1189525758171502E-2,null,{"$f":"AZ7","v":4.3706968067992171E-3},{"$f":"AX7","v":2.960741540407064E-3},{"$f":"Z7","v":1.9254778741918627E-3},null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR7, IF(MODE_ILIM=4,#REF!,#REF!))","v":67.870036413461634},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ7, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.3706968067992171E-3},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA7, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.960741540407064E-3},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB7, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.9254778741918627E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S7, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":5.7196806681522023},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P7, IF(MODE_ILIM=4,#REF!,#REF!))","v":254.86419788488402}]
["Vin",{"$f":"Vin","v":42},"V",{"$f":"B8","v":42},"Vin",null,null,2,1.4000000000000002E-3,7.3615061321327738E-2,7.3615061321327738E-2,0,212.76184650484143,249.92331390647766,1,249.92331390647766,1.8170476072160916E-6,{"$f":"OnTime*S8","v":1.724983058649077E-2},11439.361336304404,8.3249841151525998E-6,7.909248357391856E-5,7.1901125917946251E-5,8.2615239708105012E-3,5.5967278222626735E-5,3.7949712279601549E-3,3.8509729907390696E-3,4.1354388599885838E-3,1.8812040021174044E-7,{"$f":"AB8","v":1.8812040021174044E-7},2.7909150154656129E-3,1.5578413247102845E-8,{"$f":"AE8","v":1.5578413247102845E-8},5.5699120878686106E-3,2.1313433497943804E-5,4.5929035765262185E-5,35,91.485596098664772,8.3792951754032966E-4,1.6143226717792772E-3,2.4981812250848691E-3,2.5195045902671517E-3,6.1015455135311125E-3,1.1317572726722261E-5,1.2583297469934848E-4,0,7.0116517366321131E-6,1.3284462643598058E-4,1.4416250092149824E-4,3.625145745964876E-3,4.8961846234029946E-3,1.7176201046461068E-4,{"$f":"AO8+AV8+AX8+AY8","v":7.7316137250562546E-3},1.1582790414608784E-2,2.6600000000000006E-2,{"$f":"BB8/(BB8+BA8)","v":0.6966489277279958},5.5845486803720462E-4,2.964129746051098E-4,3.7786680130918668E-2,6.5426889914495662E-2,0,1.8363382195213911E-4,3.4791754346260154E-3,1.4657723444228314E-3,9.9389572808911156E-2,4.0799567234202256E-7,4.9268374094462547E-6,0.1282301416485713,0.33682206877962184,0.6966489277279958,{"$f":"100*BQ8","v":69.664892772799575},1.4000000000000001,10.507357436577642,0.10507357436577643,11.439361336304405,null,4.2278802943685204E-2,null,7.7316137250562546E-3,4.8961846234029946E-3,3.8509729907390696E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR8, IF(MODE_ILIM=4,#REF!,#REF!))","v":69.664892772799575},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ8, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.7316137250562546E-3},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA8, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.8961846234029946E-3},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB8, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.8509729907390696E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S8, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":11.439361336304405},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P8, IF(MODE_ILIM=4,#REF!,#REF!))","v":249.92331390647766}]
["Vout",{"$f":"Vout","v":19},"V",{"$f":"B9","v":19},"Vout",null,null,3,2.1000000000000003E-3,7.3615061321327738E-2,7.3615061321327738E-2,0,209.78312310058612,244.9824309539168,1,244.9824309539168,1.8170476072160916E-6,2.5874745879736153E-2,17159.042004456605,8.3249841151525998E-6,4.9953327677561511E-5,1.0285168887691936E-4,1.0118259113128837E-2,8.3950917333940099E-5,5.6924568419402322E-3,5.7764853498732264E-3,5.0648575347244963E-3,2.8218060031761052E-7,2.8218060031761052E-7,3.4271161890702096E-3,2.3490250746774234E-8,2.3490250746774234E-8,6.8217212637190989E-3,3.1970150246915706E-5,6.8893553647893271E-5,35,91.485596098664772,1.2799704125485126E-3,2.4214840076689156E-3,3.7703479738653216E-3,3.8023406068932583E-3,7.4728365752595892E-3,1.6976359090083391E-5,1.8874946204902268E-4,0,1.0711507519554133E-5,1.9946096956857681E-4,2.1643800822587317E-4,4.9250693902417458E-3,6.8316277063989236E-3,2.5764301569691593E-4,1.1108049337214971E-2,1.6884840357939263E-2,3.9900000000000005E-2,{"$f":"BB9/(BB9+BA9)","v":0.70265232319916981},5.6340095043454187E-4,2.9897131963888213E-4,3.8112308112732252E-2,6.6397086794630342E-2,0,1.8863322414987689E-4,3.5125742770656491E-3,1.4784036867016156E-3,0.10024606578196274,4.1367115939227943E-7,4.9692945958622914E-6,0.12030724509105312,0.33111007220412425,0.70265232319916981,70.265232319916976,2.1,11.516667783884284,0.11516667783884284,17.159042004456605,null,4.2643141944315788E-2,null,1.1108049337214971E-2,6.8316277063989236E-3,5.7764853498732264E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR9, IF(MODE_ILIM=4,#REF!,#REF!))","v":70.265232319916976},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ9, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.1108049337214971E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA9, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.8316277063989236E-3},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB9, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.7764853498732264E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S9, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":17.159042004456605},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P9, IF(MODE_ILIM=4,#REF!,#REF!))","v":244.9824309539168}]
["Iout",{"$f":"Iout","v":7.0000000000000007E-2},"A",{"$f":"B10","v":7.0000000000000007E-2},"Iout(max)",null,null,4,2.8000000000000004E-3,7.3615061321327738E-2,7.3615061321327738E-2,0,206.80439969633073,240.04154909054776,1,240.04154909054776,1.8170476072160916E-6,3.449966117298154E-2,22878.722672608808,8.3249841151525998E-6,3.5383749729382983E-5,1.3380225183589248E-4,1.1683559245390638E-2,1.119345564452535E-4,7.5899424559203099E-3,7.7020149518259428E-3,5.8483937221605851E-3,3.7624080042348077E-7,3.7624080042348077E-7,3.971537019867695E-3,3.1546212600359144E-8,3.1546212600359144E-8,7.8770452158896317E-3,4.2626866995887614E-5,9.185807153052437E-5,35,91.485596098664772,1.7373953983820414E-3,3.2286453435585545E-3,5.0578988134711202E-3,5.1005658925075735E-3,8.6288884166724113E-3,2.2635145453444525E-5,2.5166594939869696E-4,0,1.4540761421176572E-5,2.6620671081987351E-4,2.8884306547730587E-4,6.224993034518617E-3,8.7670707893948551E-3,3.4352402092922135E-4,1.4500003768308956E-2,2.2202426507147922E-2,5.3200000000000011E-2,0.70554758599123868,5.6585816946366557E-4,3.0020724406377693E-4,3.8269349004728816E-2,6.7078727406625918E-2,0,1.928420887064974E-4,3.5304793645419075E-3,1.4844954152058016E-3,0.10065912739825164,4.1837131855920652E-7,4.9897704603420718E-6,0.11627040661037298,0.32835690084373992,0.70554758599123868,70.554758599123872,2.8000000000000003,12.603144523181673,0.12603144523181672,22.878722672608809,null,4.2818852033262994E-2,null,1.4500003768308956E-2,8.7670707893948551E-3,7.7020149518259428E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR10, IF(MODE_ILIM=4,#REF!,#REF!))","v":70.554758599123872},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ10, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.4500003768308956E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA10, IF(MODE_ILIM=4,#REF!,#REF!))","v":8.7670707893948551E-3},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB10, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.7020149518259428E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S10, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":22.878722672608809},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P10, IF(MODE_ILIM=4,#REF!,#REF!))","v":240.04154909054776}]
["Rt",{"$f":"Vout*2500/(Fsw/1000)","v":158.33333333333334},"kW",{"$f":"B11*1000","v":158333.33333333334},"RT pin resistance to get Fsw",null,null,5,3.5000000000000005E-3,7.3615061321327738E-2,7.3615061321327738E-2,0,203.82567629207543,235.10066838504204,1,235.10066838504204,1.8170476072160916E-6,4.3124576466226923E-2,28598.403340761011,8.3249841151525998E-6,2.6642002960475865E-5,1.6475281479486561E-4,1.3062616345919806E-2,1.3991819555656684E-4,9.4874280699003884E-3,9.6275617968288318E-3,6.5387029609670442E-3,4.7030100052935112E-7,4.7030100052935112E-7,4.4604310102173165E-3,3.979088959381654E-8,3.979088959381654E-8,8.8068042822843605E-3,5.3283583744859496E-5,1.1482258941315546E-4,35,91.485596098664772,2.2102044750409149E-3,4.0358066794481933E-3,6.3608337439022642E-3,6.4141805381058813E-3,9.6473905349700184E-3,2.8293931816805643E-5,3.1458243674837113E-4,0,1.8499447073221749E-5,3.3308188382159289E-4,3.6137770671445461E-4,7.5249166787954899E-3,1.0702513872390787E-2,4.2940502616152661E-4,1.7907477143372649E-2,2.7535549032091603E-2,6.6500000000000004E-2,0.70717936657450131,5.6730454336382239E-4,3.0090559564027405E-4,3.8357857819555655E-2,6.7642862825541605E-2,0,1.9672822952209728E-4,3.5420847461412885E-3,1.4879287354276714E-3,0.10089193041944812,4.2314730975024208E-7,5.0013107316345979E-6,0.11381348843657338,0.32680651580925529,0.70717936657450131,70.717936657450124,3.5000000000000004,13.76888730592373,0.1376888730592373,28.59840334076101,null,4.2917882875027291E-2,null,1.7907477143372649E-2,1.0702513872390787E-2,9.6275617968288318E-3,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR11, IF(MODE_ILIM=4,#REF!,#REF!))","v":70.717936657450124},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ11, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7907477143372649E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA11, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.0702513872390787E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB11, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.6275617968288318E-3},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S11, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":28.59840334076101},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P11, IF(MODE_ILIM=4,#REF!,#REF!))","v":235.10066838504204}]
["Tamb",{"$f":"'Design Converter'!E56","v":25},"°C",{"$f":"B12","v":25},"Ambient temperature",null,null,6,4.2000000000000006E-3,7.3615061321327738E-2,7.3615061321327738E-2,0,200.84695288782012,230.15978891196781,1,230.15978891196781,1.8170476072160916E-6,5.1749491759472306E-2,34318.084008913211,8.3249841151525998E-6,2.0814171781204452E-5,1.9570337775383871E-4,1.4309379265391966E-2,1.679018346678802E-4,1.1384913683880464E-2,1.1553125885113506E-2,7.1627902170949423E-3,5.6436120063522115E-7,5.6436120063522115E-7,4.9125921304323892E-3,4.8267122879972487E-8,4.8267122879972487E-8,9.6473707298804778E-3,6.3940300493831411E-5,1.3778710729578654E-4,35,91.485596098664772,2.6983976425251346E-3,4.8429680153378313E-3,7.6791527651587522E-3,7.7431846346846861E-3,1.0568186834129823E-2,3.3952718180166775E-5,3.7749892409804536E-4,0,2.2587598107411999E-5,4.0008652220545733E-4,4.3404196597612052E-4,8.8248403230723593E-3,1.2637956955386715E-2,5.1528603139383187E-4,2.1330469587441354E-2,3.2884208100878373E-2,7.980000000000001E-2,0.70817376582671265,5.6824173151761041E-4,3.0133276297478369E-4,3.8411794666323329E-2,6.8147550527081283E-2,0,2.0045043123692081E-4,3.5505110161247041E-3,1.4900209842852983E-3,0.10103379946272807,4.2833972651041098E-7,5.0083433175479883E-6,0.11215375400315922,0.32586289226847531,0.70817376582671265,70.817376582671272,4.2,15.015319606822954,0.15015319606822955,34.31808400891321,null,4.2978231794487627E-2,null,2.1330469587441354E-2,1.2637956955386715E-2,1.1553125885113506E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR12, IF(MODE_ILIM=4,#REF!,#REF!))","v":70.817376582671272},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ12, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.1330469587441354E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA12, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.2637956955386715E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB12, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.1553125885113506E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S12, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":34.31808400891321},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P12, IF(MODE_ILIM=4,#REF!,#REF!))","v":230.15978891196781}]
["VDD",5,"V",{"$f":"B13","v":5},"Gate drive rail",null,null,7,4.9000000000000007E-3,7.3615061321327738E-2,7.3615061321327738E-2,0,197.86822948356482,225.21891075243673,1,225.21891075243673,1.8170476072160916E-6,6.0374407052717696E-2,40037.764677065417,8.3249841151525998E-6,1.6651435224582011E-5,2.2665394071281185E-4,1.5455896095696548E-2,1.9588547377919358E-4,1.3282399297860544E-2,1.3478707216911594E-2,7.7366976790141451E-3,6.584214007410914E-7,6.584214007410914E-7,5.3392885283771677E-3,5.7016003978520046E-8,5.7016003978520046E-8,1.0420351353627526E-2,7.4597017242803299E-5,1.6075162517841765E-4,35,91.485596098664772,3.2019749008346996E-3,5.650129351227471E-3,9.0128558772405876E-3,9.0875782732412116E-3,1.1414946420720546E-2,3.9611504543527919E-5,4.4041541144771964E-4,0,2.6805248155469655E-5,4.672206596031893E-4,5.0683587730124702E-4,1.0124763967349232E-2,1.4573400038382648E-2,6.0116703662613734E-4,2.4768981225551243E-2,3.8248403879867554E-2,9.3100000000000016E-2,0.70880191346025123,5.6888697383004146E-4,3.0160410425915911E-4,3.844586579276707E-2,6.8617932239845303E-2,0,2.0407745631980406E-4,3.5571095331353515E-3,1.4913426276451155E-3,0.10112341608664499,4.3408219890260256E-7,5.0127857004131512E-6,0.11095224310233423,0.32526792478468036,0.70880191346025123,70.880191346025128,4.9000000000000004,16.343061169118954,0.16343061169118955,40.037764677065418,null,4.3016353334564536E-2,null,2.4768981225551243E-2,1.4573400038382648E-2,1.3478707216911594E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR13, IF(MODE_ILIM=4,#REF!,#REF!))","v":70.880191346025128},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ13, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.4768981225551243E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA13, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.4573400038382648E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB13, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.3478707216911594E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S13, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":40.037764677065418},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P13, IF(MODE_ILIM=4,#REF!,#REF!))","v":225.21891075243673}]
["K1",400,"pC",4,"RT constant",null,null,8,5.6000000000000008E-3,7.3615061321327738E-2,7.3615061321327738E-2,0,194.88950607930946,220.27803399483784,1,220.27803399483784,1.8170476072160916E-6,6.8999322345963079E-2,45757.445345217617,8.3249841151525998E-6,1.3529382807115188E-5,2.5760450367178498E-4,1.6523047941621002E-2,2.2386911289050694E-4,1.517988491184062E-2,1.540430579245472E-2,8.2708777199771676E-3,7.5248160084696175E-7,7.5248160084696175E-7,5.7479072181107526E-3,6.6076874776019382E-8,6.6076874776019382E-8,1.1139824175737221E-2,8.5253733991775215E-5,1.8371614306104874E-4,35,91.485596098664772,3.7209362499696095E-3,6.4572906871171089E-3,1.0361943080147767E-2,1.0447361544773394E-2,1.2203091027062225E-2,4.5270290906889044E-5,5.0333189879739392E-4,0,3.1152430849117033E-5,5.3448432964651094E-4,5.7975947472892013E-4,1.1424687611626103E-2,1.650884312137858E-2,6.8704804185844271E-4,2.8223012182739336E-2,4.3628136533669676E-2,0.10640000000000002,0.70920030374516763,5.6934963400319676E-4,3.0177769402773614E-4,3.8467474734752372E-2,6.9066665223974921E-2,0,2.0764392312588463E-4,3.562560610266332E-3,1.4921808539577884E-3,0.10118025366817718,4.4042988403838662E-7,5.0156031943920596E-6,0.11003831349777261,0.32489167587313644,0.70920030374516763,70.920030374516756,5.6000000000000005,17.75180413241851,0.17751804132418511,45.757445345217619,null,4.3040531171750891E-2,null,2.8223012182739336E-2,1.650884312137858E-2,1.540430579245472E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR14, IF(MODE_ILIM=4,#REF!,#REF!))","v":70.920030374516756},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ14, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.8223012182739336E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA14, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.650884312137858E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB14, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.540430579245472E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S14, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":45.757445345217619},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P14, IF(MODE_ILIM=4,#REF!,#REF!))","v":220.27803399483784}]
["Outputs",null,null,null,null,null,null,9,6.3E-3,7.3615061321327738E-2,7.3615061321327738E-2,0,191.91078267505415,215.33715873567249,1,215.33715873567249,1.8170476072160916E-6,7.7624237639208449E-2,51477.126013369816,8.3249841151525998E-6,1.1101119815752102E-5,2.8855506663075806E-4,1.7525338868085955E-2,2.518527520018203E-4,1.7077370525820697E-2,1.7329921611974511E-2,8.7725905832408777E-3,8.4654180095283178E-7,8.4654180095283178E-7,6.1435872064249906E-3,7.5487327525897638E-8,7.5487327525897638E-8,1.1815567823834446E-2,9.5910450740747103E-5,2.0668066094367983E-4,35,91.485596098664772,4.2552816899298646E-3,7.2644520230067478E-3,1.1726414373880292E-2,1.1822534540279891E-2,1.2943332625008614E-2,5.0929077270250162E-5,5.6624838614706798E-4,0,3.5629179820076473E-5,6.0187756596714447E-4,6.5281279229836831E-4,1.2724611255902973E-2,1.8444286204374508E-2,7.7292904709074786E-4,3.1692562584043515E-2,4.9023406225146504E-2,0.1197,0.70944513673622089,5.6969076520026489E-4,3.0188595329361278E-4,3.8480754631627555E-2,6.9500815780309852E-2,0,2.1116915914163369E-4,3.5672440441606064E-3,1.4926959906543435E-3,0.10121518352369234,4.4740281870060435E-7,5.0173347011688253E-6,0.10931670132217598,0.32466160590777604,0.70944513673622089,70.944513673622083,6.3,19.240199150848532,0.19240199150848533,51.477126013369819,null,4.3055389797625215E-2,null,3.1692562584043515E-2,1.8444286204374508E-2,1.7329921611974511E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR15, IF(MODE_ILIM=4,#REF!,#REF!))","v":70.944513673622083},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ15, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.1692562584043515E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA15, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.8444286204374508E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB15, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.7329921611974511E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S15, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":51.477126013369819},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P15, IF(MODE_ILIM=4,#REF!,#REF!))","v":215.33715873567249}]
["Design","Value","Units","Std Units","Description",null,null,10,7.000000000000001E-3,7.3615061321327738E-2,7.3615061321327738E-2,0,188.93205927079885,210.39628508050683,1,210.39628508050683,1.8170476072160916E-6,8.6249152932453846E-2,57196.806681522023,8.3249841151525998E-6,9.1585094226616294E-6,3.1950562958973119E-4,1.8473329196476269E-2,2.7983639111313368E-4,1.8974856139800777E-2,1.9255554675702603E-2,9.2471224077287067E-3,9.4060200105870192E-7,9.4060200105870192E-7,6.5300537841754868E-3,8.5283204848449195E-8,8.5283204848449195E-8,1.2454702057171994E-2,1.0656716748971902E-4,2.2964517882631091E-4,35,91.485596098664772,4.8050112207154664E-3,8.0716133588963866E-3,1.3106269758438163E-2,1.3213097350760074E-2,1.364347053606443E-2,5.6587863633611307E-5,6.2916487349674226E-4,0,4.0235528700070299E-5,6.6940040219681254E-4,7.2599586404896248E-4,1.4024534900179844E-2,2.0379729287370436E-2,8.5881005232305322E-4,3.5177632554502521E-2,5.443421311541103E-2,0.13300000000000001,0.70958229978059761,5.6994713263011588E-4,3.0194840585107997E-4,3.8488194442237104E-2,6.9924639373965786E-2,0,2.1466480442018136E-4,3.5713885478561745E-3,1.492984586228272E-3,0.10123475231342727,4.5500340322573226E-7,5.0183047450335769E-6,0.10873003892209257,0.32453403183685681,0.70958229978059761,70.958229978059762,7.0000000000000009,20.80575856495858,0.20805758564958579,57.19680668152202,null,4.3063714061244297E-2,null,3.5177632554502521E-2,2.0379729287370436E-2,1.9255554675702603E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR16, IF(MODE_ILIM=4,#REF!,#REF!))","v":70.958229978059762},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ16, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.5177632554502521E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA16, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.0379729287370436E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB16, IF(MODE_ILIM=4,#REF!,#REF!))","v":1.9255554675702603E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S16, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":57.19680668152202},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P16, IF(MODE_ILIM=4,#REF!,#REF!))","v":210.39628508050683}]
["On-Time",{"$f":"(Rt*k_RT/10000)/Vin","v":1.5079365079365079},"µs",{"$f":"B17/1000000","v":1.507936507936508E-6},"On Time - fixed",null,null,11,7.7000000000000011E-3,7.3615061321327738E-2,7.3615061321327738E-2,0,185.95333586654351,205.45541314506167,1,205.45541314506167,1.8170476072160916E-6,9.4874068225699229E-2,62916.487349674222,8.3249841151525998E-6,7.5691009192239705E-6,3.5045619254870432E-4,1.9374991116424309E-2,3.0782003022444712E-4,2.0872341753780853E-2,2.1181204983870633E-2,9.6984638013383438E-3,1.034662201164572E-6,1.034662201164572E-6,6.9100868203965139E-3,9.5498599730835209E-8,9.5498599730835209E-8,1.3062601718884976E-2,1.1722388423869091E-4,2.52609696708942E-4,35,91.485596098664772,5.3701248423264122E-3,8.8787746947860246E-3,1.4501509233821378E-2,1.4619050067214038E-2,1.4309392617973135E-2,6.2246649996972424E-5,6.9208136084641654E-4,0,4.4971511120820845E-5,7.3705287196723743E-4,7.9930872402021638E-4,1.5324458544456715E-2,2.2315172370366367E-2,9.4469105755535859E-4,3.8678222219155983E-2,5.9860557363827512E-2,0.14630000000000001,0.70964107718147595,5.7014219837030384E-4,3.019775113583498E-4,3.849138256577754E-2,7.0340851903254412E-2,0,2.1813828840914576E-4,3.5751400820405385E-3,1.4931082558203082E-3,0.10124313797302077,4.6322439632476074E-7,5.0187204303033747E-6,0.1082417153684012,0.32448107609127919,0.70964107718147595,70.964107718147602,7.7000000000000011,22.444784059665849,0.22444784059665848,62.91648734967422,null,4.3067281192478359E-2,null,3.8678222219155983E-2,2.2315172370366367E-2,2.1181204983870633E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR17, IF(MODE_ILIM=4,#REF!,#REF!))","v":70.964107718147602},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ17, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.8678222219155983E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA17, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.2315172370366367E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB17, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.1181204983870633E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S17, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":62.91648734967422},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P17, IF(MODE_ILIM=4,#REF!,#REF!))","v":205.45541314506167}]
["Off Time",{"$f":"L*Iripple*1000000/(Vout+(Rdcr+RdsonBot)*Iout)","v":1.809531239075107},"µs",{"$f":"B18/1000000","v":1.809531239075107E-6},"Off Time - depends on Vout, L, Iout, DCR, etc.",null,null,12,8.4000000000000012E-3,7.3615061321327738E-2,7.3615061321327738E-2,0,182.97461246228818,200.51454305646382,1,200.51454305646382,1.8170476072160916E-6,0.10349898351894461,68636.168017826421,8.3249841151525998E-6,6.2445938330259254E-6,3.814067555076774E-4,2.0236518226257674E-2,3.358036693357604E-4,2.2769827367760929E-2,2.3106872536710239E-2,1.0129715069448993E-2,1.1287224012704421E-6,1.1287224012704421E-6,7.2858031653031978E-3,1.0616585552708419E-7,1.0616585552708419E-7,1.3643442527438198E-2,1.2788060098766282E-4,2.7557421459157308E-4,35,91.485596098664772,5.9506225547627037E-3,9.6859360306756626E-3,1.5912132800029941E-2,1.6040392780642589E-2,1.4945673150519178E-2,6.7905436360333563E-5,7.5499784819609071E-4,0,4.983716071405043E-5,8.0483500891014113E-4,8.7275140625178542E-4,1.6624382188733584E-2,2.4250615453362295E-2,1.0305720627876637E-3,4.2194331703044333E-2,6.5302439128011369E-2,0.15960000000000002,0.70964103643694987,5.702916389432527E-4,3.0198159524178039E-4,3.849138035576858E-2,7.0751268246463841E-2,0,2.2159457632953372E-4,3.5785961772163799E-3,1.4931081700924797E-3,0.10124313216007699,4.7205293076726498E-7,5.01872014215012E-6,0.10782726744710482,0.32448411114031056,0.70964103643694987,70.964103643694983,8.4,24.152326085424395,0.24152326085424394,68.636168017826421,null,4.3067278719741052E-2,null,4.2194331703044333E-2,2.4250615453362295E-2,2.3106872536710239E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR18, IF(MODE_ILIM=4,#REF!,#REF!))","v":70.964103643694983},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ18, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.2194331703044333E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA18, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.4250615453362295E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB18, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.3106872536710239E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S18, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":68.636168017826421},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P18, IF(MODE_ILIM=4,#REF!,#REF!))","v":200.51454305646382}]
["DIL",{"$f":"(Vin-Vout-(Rdcr+RdsonTop)*Iout)/L*OnTime*1000","v":73.454186085781842},"mA",{"$f":"B19/1000","v":7.3454186085781845E-2},"Inductor pk-pk ripple current in CCM",null,null,13,9.1000000000000004E-3,7.3615061321327738E-2,7.3615061321327738E-2,0,179.99588905803287,195.57367495468654,1,195.57367495468654,1.8170476072160916E-6,0.11212389881218998,74355.848685978621,8.3249841151525998E-6,5.123857067781423E-6,4.1235731846665053E-4,2.1062835969588647E-2,3.6378730844707384E-4,2.4667312981741005E-2,2.503255733445308E-2,1.0543341722175843E-2,1.2227826013763124E-6,1.2227826013763124E-6,7.6588369207762699E-3,1.1731556595809149E-7,1.1731556595809149E-7,1.4200545212519186E-2,1.3853731773663471E-4,2.9853873247420417E-4,35,91.485596098664772,6.5465043580243418E-3,1.0493097366565302E-2,1.7338140457063847E-2,1.7477125582047254E-2,1.5555949818284825E-2,7.3564222723694687E-5,8.1791433554576488E-4,0,5.4832511111481392E-5,8.7274684665724625E-4,9.4632394478346858E-4,1.7924305833010457E-2,2.6186058536358227E-2,1.1164530680199691E-3,4.5725961131208914E-2,7.0759858563829325E-2,0.1729,0.70959574966143624,5.7040632709305346E-4,3.0196643205777788E-4,3.8488923972312898E-2,7.1157147341616531E-2,0,2.250371129437286E-4,3.5818244818878152E-3,1.4930128852216167E-3,0.10123667118225441,4.8147268347592598E-7,5.0183998652202751E-6,0.10746972722837113,0.32453021683630767,0.70959574966143624,70.95957496614362,9.1,25.922181532084487,0.25922181532084487,74.355848685978614,null,4.3064530318671766E-2,null,4.5725961131208914E-2,2.6186058536358227E-2,2.503255733445308E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR19, IF(MODE_ILIM=4,#REF!,#REF!))","v":70.95957496614362},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ19, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.5725961131208914E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA19, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.6186058536358227E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB19, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.503255733445308E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S19, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":74.355848685978614},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P19, IF(MODE_ILIM=4,#REF!,#REF!))","v":195.57367495468654}]
["CCM Freq",{"$f":"'Design Converter'!E12","v":300},"kHz",{"$f":"B20*1000","v":300000},"Frequency in CCM",{"$f":"10000*Vout/(k_RT*Rt/1000+Vin*0.75)","v":285.78591125595386},null,14,9.8000000000000014E-3,7.3615061321327738E-2,7.3615061321327738E-2,0,177.01716565377757,190.63280899421457,1,190.63280899421457,1.8170476072160916E-6,0.12074881410543539,80075.529354130835,8.3249841151525998E-6,4.1632255547147048E-6,4.4330788142562367E-4,2.1857937877163426E-2,3.9177094755838717E-4,2.6564798595721088E-2,2.6958259377330797E-2,1.0941342785642251E-2,1.3168428014821828E-6,1.3168428014821828E-6,8.0304599840737515E-3,1.2897657511161959E-7,1.2897657511161959E-7,1.4736602208992889E-2,1.4919403448560665E-4,3.2150325035683531E-4,35,91.485596098664772,7.1577702521113274E-3,1.1300258702454942E-2,1.8779532204923104E-2,1.8929248562430282E-2,1.6143172041945212E-2,7.9223009087055825E-5,8.8083082289543927E-4,0,5.9957595944836057E-5,9.4078841884027531E-4,1.0200263736552069E-3,1.9224229477287327E-2,2.8121501619354158E-2,1.2023340732522747E-3,4.927311062869192E-2,7.6232815825399314E-2,0.18620000000000003,0.70951492637979319,5.7049404067967778E-4,3.0193615293770963E-4,3.8484540066203207E-2,7.1559389956084685E-2,0,2.28468363440976E-4,3.5848733927627274E-3,1.4928428303685867E-3,0.10122514027893167,4.914651191999926E-7,5.0178282671718119E-6,0.10715695569895432,0.32461015007374999,0.70951492637979319,70.951492637979314,9.8000000000000007,27.746934669307642,0.27746934669307644,80.075529354130836,null,4.3059625248898677E-2,null,4.927311062869192E-2,2.8121501619354158E-2,2.6958259377330797E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR20, IF(MODE_ILIM=4,#REF!,#REF!))","v":70.951492637979314},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ20, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.927311062869192E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA20, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.8121501619354158E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB20, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.6958259377330797E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S20, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":80.075529354130836},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P20, IF(MODE_ILIM=4,#REF!,#REF!))","v":190.63280899421457}]
["Icrit_Skip",{"$f":"1000*Iripple/2","v":36.727093042890921},"mA",{"$f":"Iripple/2","v":3.6727093042890922E-2},"CCM-DCM (critical conduction) boundary",null,null,15,1.0500000000000001E-2,7.3615061321327738E-2,7.3615061321327738E-2,0,174.03844224952226,185.69194534597455,1,185.69194534597455,1.8170476072160916E-6,0.12937372939868075,85795.210022283019,8.3249841151525998E-6,3.3306782433902206E-6,4.7425844438459675E-4,2.2625115190912815E-2,4.1975458666970055E-4,2.846228420970116E-2,2.8883978665575044E-2,1.1325365743995976E-2,1.4109030015880527E-6,1.4109030015880527E-6,8.4016658301285119E-3,1.4117597744229804E-7,1.4117597744229804E-7,1.5253832469231673E-2,1.5985075123457849E-4,3.4446776823946634E-4,35,91.485596098664772,7.7844202370236535E-3,1.2107420038344578E-2,2.0236308043607699E-2,2.0396761812794619E-2,1.6709770567027167E-2,8.4881795450416977E-5,9.4374731024511344E-4,0,6.5212448845836744E-5,1.0089597590909503E-3,1.0938587269070836E-3,2.0524153121564196E-2,3.0056944702350086E-2,1.2882150784845798E-3,5.2835780320536367E-2,8.1721311065090438E-2,0.19950000000000001,0.70940569633367678,5.705604905233599E-4,3.0189379138653884E-4,3.8478615359153485E-2,7.1958657638587983E-2,0,2.3189013876243151E-4,3.5877784484740563E-3,1.4926130067452309E-3,0.10120955663674217,5.0201023851148307E-7,5.0170557709315644E-6,0.10688003902873924,0.32471712360512395,0.70940569633367678,70.940569633367673,10.5,29.618044224570543,0.29618044224570544,85.795210022283015,null,4.3052996206045843E-2,null,5.2835780320536367E-2,3.0056944702350086E-2,2.8883978665575044E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR21, IF(MODE_ILIM=4,#REF!,#REF!))","v":70.940569633367673},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ21, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.2835780320536367E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA21, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.0056944702350086E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB21, IF(MODE_ILIM=4,#REF!,#REF!))","v":2.8883978665575044E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S21, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":85.795210022283015},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P21, IF(MODE_ILIM=4,#REF!,#REF!))","v":185.69194534597455}]
["Tr",null,"ns",{"$f":"B22/1000000000","v":0},"Switch rise time",null,null,16,1.1200000000000002E-2,7.3615061321327738E-2,7.3615061321327738E-2,0,171.05971884526693,180.75108419958238,1,180.75108419958238,1.8170476072160916E-6,0.13799864469192616,91514.890690435233,8.3249841151525998E-6,2.6021993459812935E-6,5.0520900734356993E-4,2.3367118490781276E-2,4.4773822578101399E-4,3.035976982368124E-2,3.0809715199417487E-2,1.169678744432117E-2,1.5049632016939231E-6,1.5049632016939231E-6,8.7732296724645081E-3,1.5393911777162339E-7,1.5393911777162339E-7,1.5754090431779263E-2,1.7050746798355046E-4,3.6743228612209748E-4,35,91.485596098664772,8.4264543127613289E-3,1.2914581374234218E-2,2.1708467973117644E-2,2.1879665424143963E-2,1.7257776833344823E-2,9.0540581813778102E-5,1.0066637975947878E-3,0,7.0597103446205813E-5,1.0772609010409936E-3,1.1678210385793252E-3,2.1824076765841072E-2,3.1992387785346021E-2,1.3740960837168854E-3,5.6413970331786197E-2,8.7225344433523144E-2,0.21280000000000004,0.70927341289045764,5.7060996413338253E-4,3.018416251110981E-4,3.8471440221208693E-2,7.2355447217651983E-2,0,2.353037993490182E-4,3.5905663339041113E-3,1.4923346780132424E-3,0.10119068401039058,5.1308704623696141E-7,5.016120236560144E-6,0.10663228416836164,0.32484604122540656,0.70927341289045764,70.927341289045771,11.200000000000001,31.525976771075946,0.31525976771075948,91.514890690435237,null,4.3044968079674048E-2,null,5.6413970331786197E-2,3.1992387785346021E-2,3.0809715199417487E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR22, IF(MODE_ILIM=4,#REF!,#REF!))","v":70.927341289045771},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ22, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.6413970331786197E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA22, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.1992387785346021E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB22, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.0809715199417487E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S22, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":91.514890690435237},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P22, IF(MODE_ILIM=4,#REF!,#REF!))","v":180.75108419958238}]
["Tf",null,"ns",{"$f":"B23/1000000000","v":0},"Switch fall time",null,null,17,1.1900000000000003E-2,7.3615061321327738E-2,7.3615061321327738E-2,0,168.08099544101159,175.81022576596914,1,175.81022576596914,1.8170476072160916E-6,0.14662355998517154,97234.571358587447,8.3249841151525998E-6,1.959423848267534E-6,5.3615957030254317E-4,2.4086274425953683E-2,4.7572186489232732E-4,3.2257255437661322E-2,3.2735468979089792E-2,1.2056772528333658E-2,1.599023401799793E-6,1.599023401799793E-6,9.1457528746396628E-3,1.6728959128795932E-7,1.6728959128795932E-7,1.6238944721439611E-2,1.8116418473252237E-4,3.9039680400472856E-4,35,91.485596098664772,9.0838724793243491E-3,1.3721742710123859E-2,2.3196011993452937E-2,2.3377959487482693E-2,1.7788909186804543E-2,9.6199368177139226E-5,1.0695802849444622E-3,0,7.6111593377665556E-5,1.1456918783221278E-3,1.2419133427122996E-3,2.3124000410117949E-2,3.392783086834196E-2,1.4599770889491908E-3,6.0007680787486146E-2,9.2744916079569029E-2,0.22610000000000005,0.70912217381435627,5.7064574297415046E-4,3.0178139759380482E-4,3.846323691770176E-2,7.2750139091646279E-2,0,2.3871038721116563E-4,3.5932574757949584E-3,1.4920164660038328E-3,0.10116910702007677,5.2467385506693006E-7,5.0150506442472173E-6,0.10640856779373933,0.32499300201724135,0.70912217381435627,70.912217381435624,11.900000000000002,33.460383546927204,0.33460383546927203,97.234571358587445,null,4.3035789558267694E-2,null,6.0007680787486146E-2,3.392783086834196E-2,3.2735468979089792E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR23, IF(MODE_ILIM=4,#REF!,#REF!))","v":70.912217381435624},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ23, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.0007680787486146E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA23, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.392783086834196E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB23, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.2735468979089792E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S23, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":97.234571358587445},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P23, IF(MODE_ILIM=4,#REF!,#REF!))","v":175.81022576596914}]
[null,null,null,null,null,null,null,18,1.26E-2,7.3615061321327738E-2,7.3615061321327738E-2,0,165.10227203675629,170.86937028046302,1,170.86937028046302,1.8170476072160916E-6,0.1552484752784169,102954.25202673963,8.3249841151525998E-6,1.3880678502997501E-6,5.6711013326151609E-4,2.47845719124315E-2,5.0370550400364049E-4,3.4154741051641395E-2,3.4661240004823596E-2,1.240631657996575E-2,1.6930836019056636E-6,1.6930836019056636E-6,9.5196965168679749E-3,1.8124924354653651E-7,1.8124924354653651E-7,1.6709736263605831E-2,1.9182090148149421E-4,4.1336132188735965E-4,35,91.485596098664772,9.7566747367127116E-3,1.4528904046013496E-2,2.4698940104613567E-2,2.4891644093815928E-2,1.8304636540593337E-2,1.0185815454050032E-4,1.132496772294136E-3,0,8.1755952271938298E-5,1.2142527245660743E-3,1.3161356733465172E-3,2.4423924054394811E-2,3.5863273951337885E-2,1.5458580941814957E-3,6.3616911812681823E-2,9.8280026150350863E-2,0.2394,0.7089551689782444,5.706703810682617E-4,3.0171446603442223E-4,3.8454178469362436E-2,7.3143029471386178E-2,0,2.4211071410998037E-4,3.5958677758021508E-3,1.4916650823148401E-3,0.10114528075887472,5.3674848824441846E-7,5.0138695533973452E-6,0.10620490160519558,0.32515496934219018,0.7089551689782444,70.895516897824436,12.6,35.410314704487,0.35410314704487,102.95425202673964,null,4.3025654231454456E-2,null,6.3616911812681823E-2,3.5863273951337885E-2,3.4661240004823596E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR24, IF(MODE_ILIM=4,#REF!,#REF!))","v":70.895516897824436},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ24, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.3616911812681823E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA24, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.5863273951337885E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB24, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.4661240004823596E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S24, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":102.95425202673964},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P24, IF(MODE_ILIM=4,#REF!,#REF!))","v":170.86937028046302}]
["Components","Input Value","Units","Std Units","Description",null,null,19,1.3300000000000001E-2,7.3615061321327738E-2,7.3615061321327738E-2,0,162.12354863250096,165.92851800642137,1,165.92851800642137,1.8170476072160916E-6,0.16387339057166228,108673.93269489183,8.3249841151525998E-6,8.768545889601517E-7,5.9806069622048922E-4,2.5463727025764056E-2,5.3168914311495393E-4,3.6052226665621474E-2,3.6587028276850612E-2,1.274627860846784E-2,1.7871438020115333E-6,1.7871438020115333E-6,9.8954072798812295E-3,1.9583817046945286E-7,1.9583817046945286E-7,1.7167622034881713E-2,2.0247761823046607E-4,4.3632583976999074E-4,35,91.485596098664772,1.0444861084926422E-2,1.5336065381903134E-2,2.6217252306599548E-2,2.6420719334149498E-2,1.8806226301681862E-2,1.0751694090386148E-4,1.1954132596438103E-3,0,8.7530213760746419E-5,1.2829434734045568E-3,1.3904880645226334E-3,2.5723847698671681E-2,3.7798717034333809E-2,1.6317390994138011E-3,6.724166353241974E-2,0.10383067479124283,0.25270000000000004,0.70877491858999742,5.7068589587441667E-4,3.0164190270878224E-4,3.8444401573865895E-2,7.3534352470374015E-2,0,2.4550542197244996E-4,3.5984097978547019E-3,1.4912858295468418E-3,0.10111956478003163,5.4928841840641265E-7,5.0125947874133079E-6,0.10601813450263668,0.32532954405807124,0.70877491858999742,70.877491858999747,13.3,37.364462120689176,0.37364462120689174,108.67393269489183,null,4.301471504768211E-2,null,6.724166353241974E-2,3.7798717034333809E-2,3.6587028276850612E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR25, IF(MODE_ILIM=4,#REF!,#REF!))","v":70.877491858999747},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ25, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.724166353241974E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA25, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.7798717034333809E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB25, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.6587028276850612E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S25, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":108.67393269489183},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P25, IF(MODE_ILIM=4,#REF!,#REF!))","v":165.92851800642137}]
["L",{"$f":"'Design Converter'!E17","v":470},"µH",{"$f":"B26/1000000","v":4.6999999999999999E-4},"Filter inductance",null,null,20,1.4000000000000002E-2,7.3615061321327738E-2,7.3615061321327738E-2,0,159.14482522824562,160.98766923953224,1,160.98766923953224,1.8170476072160916E-6,0.17249830586490769,114393.61336304405,8.3249841151525998E-6,4.16762653754514E-7,6.2901125917946236E-4,2.6125232691839612E-2,5.5967278222626737E-4,3.7949712279601554E-2,3.851283379540249E-2,1.3077405921934088E-2,1.8812040021174045E-6,1.8812040021174045E-6,1.0273137747194695E-2,2.1107471834567299E-7,2.1107471834567299E-7,1.7613608564568721E-2,2.1313433497943798E-4,4.5929035765262182E-4,35,91.485596098664772,1.1148431523965479E-2,1.6143226717792773E-2,2.7750948599410873E-2,2.7965185299489957E-2,1.9294781069940037E-2,1.1317572726722257E-4,1.2583297469934845E-3,0,9.3434411475812191E-5,1.3517641584692968E-3,1.4649705502814429E-3,2.7023771342948553E-2,3.9734160117329741E-2,1.7176201046461064E-3,7.088193607174724E-2,0.10939686214587019,0.26600000000000001,0.70858344014777297,5.7069390205994144E-4,3.0156456600363598E-4,3.8434015661593136E-2,7.3924295586220212E-2,0,2.4889502523200584E-4,3.6008936002880966E-3,1.490882952582571E-3,0.10109224691615884,5.6227086486315492E-7,5.0112406144364995E-6,0.10584574386210506,0.32551480558372281,0.70858344014777297,70.858344014777302,14.000000000000002,39.311419610679415,0.39311419610679416,114.39361336304404,null,4.3003094446537764E-2,null,7.088193607174724E-2,3.9734160117329741E-2,3.851283379540249E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR26, IF(MODE_ILIM=4,#REF!,#REF!))","v":70.858344014777302},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ26, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.088193607174724E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA26, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.9734160117329741E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB26, IF(MODE_ILIM=4,#REF!,#REF!))","v":3.851283379540249E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S26, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":114.39361336304404},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P26, IF(MODE_ILIM=4,#REF!,#REF!))","v":160.98766923953224}]
["Rdcr",{"$f":"'Design Converter'!E18","v":820},"mW",{"$f":"B27/1000","v":0.82},"Inductor DCR at 25°C",null,null,21,1.4700000000000001E-2,7.3615061321327738E-2,7.3615061321327738E-2,0,156.16610182399032,156.04682431293236,2,312.09364862586472,1.8170476072160916E-6,0.18112322115815307,120113.29403119624,8.3249841151525998E-6,4.8899809227020199E-10,6.599618221384356E-4,2.6770397314251865E-2,5.876564213375808E-4,3.9847197893581633E-2,4.0438656560710919E-2,1.3400353462852706E-2,1.9752642022232736E-6,1.9752642022232736E-6,1.0653062560386773E-2,2.2697548383102877E-7,2.2697548383102877E-7,1.8048577977202E-2,2.237910517284099E-4,4.8225487553525296E-4,35,91.485596098664772,1.186738605382988E-2,1.6950388053682413E-2,2.9300028983047545E-2,2.9525042080844568E-2,1.9771267166364487E-2,1.1883451363058377E-4,1.3212462343431587E-3,0,9.9468579048857966E-5,1.4207148133920167E-3,1.5395831646638845E-3,2.832369498722543E-2,4.1669603200325672E-2,1.8035011098784116E-3,7.4537729555712542E-2,0.11497858835610952,0.27930000000000005,0.70838236781891462,5.7069570715261194E-4,3.0148315120908043E-4,3.8423109370818338E-2,7.4313010770404739E-2,0,2.5227994110351906E-4,3.6033273308487077E-3,1.4904598897640714E-3,0.10106356031079206,5.756728631330752E-7,5.0098185916178361E-6,0.10568568629116118,0.32570919825470901,0.70838236781891462,70.838236781891467,14.700000000000001,41.239947953148963,0.41239947953148964,120.11329403119625,null,4.2990891603712819E-2,null,7.4537729555712542E-2,4.1669603200325672E-2,4.0438656560710919E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR27, IF(MODE_ILIM=4,#REF!,#REF!))","v":70.838236781891467},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ27, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.4537729555712542E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA27, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.1669603200325672E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB27, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.0438656560710919E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S27, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":120.11329403119625},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P27, IF(MODE_ILIM=4,#REF!,#REF!))","v":312.09364862586472}]
["Kcore",0,null,{"$f":"B28","v":0},"Core loss constant - consult inductor vendor",null,null,22,1.5400000000000002E-2,7.3615061321327738E-2,7.3615061321327738E-2,0,153.18737841973498,151.10598360332961,2,302.21196720665921,1.8170476072160916E-6,0.18974813645139846,125832.97469934844,7.9470425171882855E-6,0,6.6E-4,2.7400375207705489E-2,6.1564006044889413E-4,4.1744683507561706E-2,4.2364496573007573E-2,1.3715699042037207E-2,2.0693244023291439E-6,2.0693244023291439E-6,1.1035291431317507E-2,2.4355531394821917E-7,2.4355531394821917E-7,1.8473308510725237E-2,2.3444776847738181E-4,5.0521939341788399E-4,35,91.485596098664772,1.2601724674519628E-2,1.7757549389572049E-2,3.0864493457509561E-2,3.1100289769221311E-2,2.0236537109659055E-2,1.2449329999394485E-4,1.3841627216928331E-3,0,1.056327501116061E-4,1.4897954718044392E-3,1.6143259417110394E-3,2.8325298457411135E-2,4.230672610923044E-2,1.8893821151107172E-3,7.6910723935273512E-2,0.11927753338799738,0.29260000000000003,0.71040534207619577,5.7249131743640155E-4,3.0234829484930879E-4,3.8532836778886366E-2,7.4936093754923397E-2,0,2.5646640457103499E-4,3.6170836014039645E-3,1.494716294391683E-3,0.10135217418678025,5.9132944675276786E-7,5.0241254610500849E-6,0.10271676088090148,0.32378658696905172,0.71040534207619577,71.040534207619572,15.400000000000002,43.139231734149426,0.43139231734149425,125.83297469934844,null,4.3113663528823898E-2,null,7.6910723935273512E-2,4.230672610923044E-2,4.2364496573007573E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR28, IF(MODE_ILIM=4,#REF!,#REF!))","v":71.040534207619572},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ28, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.6910723935273512E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA28, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.230672610923044E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB28, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.2364496573007573E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S28, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":125.83297469934844},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P28, IF(MODE_ILIM=4,#REF!,#REF!))","v":302.21196720665921}]
["Cin",{"$f":"'Design Converter'!E37","v":2.2000000000000002},"µF",{"$f":"B29/1000000","v":2.2000000000000001E-6},"Input capacitance",null,null,23,1.6100000000000003E-2,7.3615061321327738E-2,7.3615061321327738E-2,0,150.20865501547971,146.16514753836722,2,292.33029507673444,1.8170476072160916E-6,0.19837305174464384,131552.65536750064,7.6015189294844481E-6,0,6.6E-4,2.8016190866768091E-2,6.4362369956020736E-4,4.3642169121541778E-2,4.4290353832524144E-2,1.4023955486740972E-2,2.1633846024350138E-6,2.1633846024350138E-6,1.1419879729813497E-2,2.608273060868104E-7,2.608273060868104E-7,1.8888490878461572E-2,2.4510448522635378E-4,5.2818391130051508E-4,35,91.485596098664772,1.3351447386034717E-2,1.8564710725461689E-2,3.2444342022796918E-2,3.269092845562889E-2,2.0691347539912763E-2,1.3015208635730599E-4,1.4470792090425072E-3,0,1.1192695829577886E-4,1.5590061673382862E-3,1.6891989154641312E-3,2.8325298457411135E-2,4.2942245547949502E-2,1.9752631203430225E-3,7.9297636039385541E-2,0.12359041408381821,0.30590000000000006,0.71223941203097818,5.7413722110186258E-4,3.0313307085926472E-4,3.8632317897654624E-2,7.5541481157400545E-2,0,2.606040894638814E-4,3.6298974696884257E-3,1.4985752381299932E-3,0.10161383744649696,6.0729482552760302E-7,5.0370963623248953E-6,9.9984176921743828E-2,0.32204380490372719,0.71223941203097818,71.223941203097823,16.100000000000001,44.999115697666738,0.44999115697666736,131.55265536750065,null,4.3224971074298874E-2,null,7.9297636039385541E-2,4.2942245547949502E-2,4.4290353832524144E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR29, IF(MODE_ILIM=4,#REF!,#REF!))","v":71.223941203097823},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ29, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.9297636039385541E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA29, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.2942245547949502E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB29, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.4290353832524144E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S29, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":131.55265536750065},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P29, IF(MODE_ILIM=4,#REF!,#REF!))","v":292.33029507673444}]
["RCinESR",{"$f":"'Design Converter'!E39","v":2},"mW",{"$f":"B30/1000","v":2E-3},"Input capacitor ESR",null,null,24,1.6800000000000002E-2,7.3615061321327738E-2,7.3615061321327738E-2,0,147.22993161122434,141.22431660553372,2,282.44863321106743,1.8170476072160916E-6,0.20699796703788922,137272.33603565284,7.284788974089263E-6,0,6.6E-4,2.8618758530783932E-2,6.716073386715208E-4,4.5539654735521858E-2,4.6216228339492342E-2,1.4325580434189885E-2,2.2574448025408846E-6,2.2574448025408846E-6,1.180683717180929E-2,2.7880280800323514E-7,2.7880280800323514E-7,1.9294741459760956E-2,2.5576120197532564E-4,5.5114842918314616E-4,35,91.485596098664772,1.4116554188375154E-2,1.9371872061351325E-2,3.4039574678909626E-2,3.4296958231076723E-2,2.1136373668259646E-2,1.358108727206671E-4,1.5099956963921814E-3,0,1.1835123723309862E-4,1.6283469336252801E-3,1.7642021199645258E-3,2.8325298457411135E-2,4.3577764986668557E-2,2.0611441255753275E-3,8.1700069463285133E-2,0.12791883405038801,0.31920000000000004,0.71390416974478821,5.7564909497435945E-4,3.0384581456467013E-4,3.8722615412978993E-2,7.6130934522596144E-2,0,2.6469749923296908E-4,3.6418661206335441E-3,1.5020779433233046E-3,0.10185134525196442,6.2355415780095604E-7,5.0488698543315712E-6,9.7463496654577431E-2,0.32046220073885801,0.71390416974478821,71.390416974478825,16.8,46.810309970062292,0.46810309970062292,137.27233603565284,null,4.3326003259277178E-2,null,8.1700069463285133E-2,4.3577764986668557E-2,4.6216228339492342E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR30, IF(MODE_ILIM=4,#REF!,#REF!))","v":71.390416974478825},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ30, IF(MODE_ILIM=4,#REF!,#REF!))","v":8.1700069463285133E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA30, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.3577764986668557E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB30, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.6216228339492342E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S30, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":137.27233603565284},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P30, IF(MODE_ILIM=4,#REF!,#REF!))","v":282.44863321106743}]
["Cout",{"$f":"'Design Converter'!E24","v":0.47},"µF",{"$f":"B31/1000000","v":4.6999999999999995E-7},"Output capacitance",null,null,25,1.7500000000000002E-2,7.3615061321327738E-2,7.3615061321327738E-2,0,144.25120820696904,136.2834913630106,2,272.56698272602119,1.8170476072160916E-6,0.21562288233113458,142992.01670380504,6.9933974151256924E-6,0,6.6E-4,2.920889811347659E-2,6.9959097778283413E-4,4.7437140349501937E-2,4.8142120094143842E-2,1.4620984305401463E-2,2.351505002646755E-6,2.351505002646755E-6,1.219613499885914E-2,2.9749141782079367E-7,2.9749141782079367E-7,1.9692613039724079E-2,2.6641791872429756E-4,5.7411294706577725E-4,35,91.485596098664772,1.4897045081540937E-2,2.0179033397240965E-2,3.5650191425847674E-2,3.5918379186574943E-2,2.1572221041681026E-2,1.4146965908402826E-4,1.5729121837418556E-3,0,1.2490562055528771E-4,1.6978178042971433E-3,1.8393355892537321E-3,2.8325298457411135E-2,4.4213284425387619E-2,2.1470251308076328E-3,8.4118024332023936E-2,0.13226279342258823,0.33250000000000002,0.71541871403133706,5.7704223428104253E-4,3.0449465180813832E-4,3.8804765256640665E-2,7.670620783413816E-2,0,2.6875133363293249E-4,3.6530846021346477E-3,1.505264594506228E-3,0.10206742239448037,6.4009301525627478E-7,5.0595810076144276E-6,9.5130860411165558E-2,0.3190235929868106,0.71541871403133706,71.541871403133712,17.5,48.564555994658186,0.48564555994658187,142.99201670380504,null,4.3417919168269266E-2,null,8.4118024332023936E-2,4.4213284425387619E-2,4.8142120094143842E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR31, IF(MODE_ILIM=4,#REF!,#REF!))","v":71.541871403133712},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ31, IF(MODE_ILIM=4,#REF!,#REF!))","v":8.4118024332023936E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA31, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.4213284425387619E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB31, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.8142120094143842E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S31, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":142.99201670380504},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P31, IF(MODE_ILIM=4,#REF!,#REF!))","v":272.56698272602119}]
["RCoutESR",{"$f":"'Design Converter'!E26","v":1.0999999999999999E-2},"mW",{"$f":"B32","v":1.0999999999999999E-2},"Output capacitor ESR",null,null,26,1.8200000000000001E-2,7.3615061321327738E-2,7.3615061321327738E-2,0,141.27248480271373,131.34267245296923,2,262.68534490593845,1.8170476072160916E-6,0.22424779762437996,148711.69737195724,6.7244205914670118E-6,0,6.6E-4,2.9787348290232125E-2,7.2757461689414767E-4,4.9334625963482009E-2,5.0068029096710348E-2,1.491053685623518E-2,2.4455652027526245E-6,2.4455652027526245E-6,1.2587711945179974E-2,3.1690098402965326E-7,3.1690098402965326E-7,2.0082603632636958E-2,2.7707463547326937E-4,5.9707746494840834E-4,35,91.485596098664772,1.5692920065532068E-2,2.0986194733130605E-2,3.7276192263611077E-2,3.7555191413134417E-2,2.1999435208613683E-2,1.4712844544738937E-4,1.6358286710915298E-3,0,1.3159014189406844E-4,1.7674188129855983E-3,1.9145993573734007E-3,2.8325298457411135E-2,4.4848803864106682E-2,2.2329061360399382E-3,8.6551500770654433E-2,0.13662229233355155,0.3458,0.71679937991113907,5.7832972057277445E-4,3.050865325395045E-4,3.8879653450523209E-2,7.7268801330262635E-2,0,2.7276961281690878E-4,3.6636342081878492E-3,1.5081695611012423E-3,0.10226439936024258,6.5689539862835524E-7,5.0693453466319847E-6,9.2965861190132934E-2,0.31771243120712489,0.71679937991113907,71.679937991113903,18.2,50.254747979561841,0.50254747979561842,148.71169737195723,null,4.350171015443155E-2,null,8.6551500770654433E-2,4.4848803864106682E-2,5.0068029096710348E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR32, IF(MODE_ILIM=4,#REF!,#REF!))","v":71.679937991113903},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ32, IF(MODE_ILIM=4,#REF!,#REF!))","v":8.6551500770654433E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA32, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.4848803864106682E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB32, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.0068029096710348E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S32, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":148.71169737195723},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P32, IF(MODE_ILIM=4,#REF!,#REF!))","v":262.68534490593845}]
["Controller",null,"Units","Std Units","Description",null,null,27,1.8900000000000004E-2,7.3615061321327738E-2,7.3615061321327738E-2,0,138.2937613984584,126.40186061798502,2,252.80372123597004,1.8170476072160916E-6,0.2328727129176254,154431.37804010947,6.4753679769682329E-6,0,6.6E-4,3.0354777339386515E-2,7.5555825600546111E-4,5.1232111577462103E-2,5.1993955347423584E-2,1.5194572604173491E-2,2.5396254028584952E-6,2.5396254028584952E-6,1.2981479220159154E-2,3.3703760548684786E-7,3.3703760548684786E-7,2.0465163791157297E-2,2.8773135222224139E-4,6.2004198283103953E-4,35,91.485596098664772,1.6504179140348546E-2,2.1793356069020244E-2,3.8917577192199834E-2,3.9207395001766718E-2,2.241850972577877E-2,1.5278723181075054E-4,1.6987451584412044E-3,0,1.3840483488116318E-4,1.8371499933223677E-3,1.989993458365326E-3,2.8325298457411135E-2,4.5484323302825744E-2,2.318787141272244E-3,8.9000498904230035E-2,0.14099733091466196,0.35910000000000009,0.71806022108379919,5.7952280816379485E-4,3.0562743609011567E-4,3.8948042276215622E-2,7.7820005799712683E-2,0,2.7675579597280628E-4,3.6735848798918383E-3,1.5108224125563103E-3,0.10244428116374908,6.739440197979399E-7,5.0782622618953023E-6,9.0950941928916854E-2,0.31651533670755078,0.71806022108379919,71.806022108379921,18.900000000000002,51.875007795911799,0.51875007795911798,154.43137804010948,null,4.3578229120241244E-2,null,8.9000498904230035E-2,4.5484323302825744E-2,5.1993955347423584E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR33, IF(MODE_ILIM=4,#REF!,#REF!))","v":71.806022108379921},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ33, IF(MODE_ILIM=4,#REF!,#REF!))","v":8.9000498904230035E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA33, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.5484323302825744E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB33, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.1993955347423584E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S33, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":154.43137804010948},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P33, IF(MODE_ILIM=4,#REF!,#REF!))","v":252.80372123597004}]
["Deadtime1",20,"ns",{"$f":"B34/1000000000","v":2E-8},"PMOS off to NMOS on deadtime",null,null,28,1.9600000000000003E-2,7.3615061321327738E-2,7.3615061321327738E-2,0,135.31503799420307,121.46105672145906,2,242.92211344291812,1.8170476072160916E-6,0.24149762821087079,160151.05870826167,6.2441048349336527E-6,0,6.6E-4,3.0911792191393096E-2,7.8354189511677433E-4,5.3129597191442175E-2,5.391989884651522E-2,1.547339535802829E-2,2.6336856029643656E-6,2.6336856029643656E-6,1.3377324684261026E-2,3.5790563141627867E-7,3.5790563141627867E-7,2.0840702707255052E-2,2.983880689712132E-4,6.4300650071367062E-4,35,91.485596098664772,1.7330822305990361E-2,2.2600517404909884E-2,4.0574346211613918E-2,4.0874990043484098E-2,2.2829892841441091E-2,1.5844601817411168E-4,1.7616616457908785E-3,0,1.4534973314829416E-4,1.9070113789391727E-3,2.0655179262714434E-3,2.8325298457411135E-2,4.6119842741544799E-2,2.4046681465045494E-3,9.1465018857804878E-2,0.14538790929555448,0.37240000000000006,0.71921339474041923,5.8063123234994643E-4,3.0612253489641615E-4,3.9010591147481705E-2,7.8360937911460551E-2,0,2.8071287594575367E-4,3.6829971204496515E-3,1.5132487280028913E-3,0.10260880224824964,6.9122052676588345E-7,5.086417731436544E-6,8.9070914777230711E-2,0.31542073621432548,0.71921339474041923,71.921339474041929,19.600000000000001,53.420714247122767,0.53420714247122769,160.15105870826167,null,4.3648213871308177E-2,null,9.1465018857804878E-2,4.6119842741544799E-2,5.391989884651522E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR34, IF(MODE_ILIM=4,#REF!,#REF!))","v":71.921339474041929},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ34, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.1465018857804878E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA34, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.6119842741544799E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB34, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.391989884651522E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S34, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":160.15105870826167},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P34, IF(MODE_ILIM=4,#REF!,#REF!))","v":242.92211344291812}]
["Deadtime2",20,"ns",{"$f":"B35/1000000000","v":2E-8},"NMOS off to PMOS on deadtime",null,null,29,2.0300000000000002E-2,7.3615061321327738E-2,7.3615061321327738E-2,0,132.33631458994776,116.52026177323357,2,233.04052354646714,1.8170476072160916E-6,0.25012254350411617,165870.73937641387,6.0287908751083548E-6,0,6.6E-4,3.1458946035174309E-2,8.1152553422808766E-4,5.5027082805422248E-2,5.5845859594216993E-2,1.5747282025422776E-2,2.7277458030702359E-6,2.7277458030702359E-6,1.3775116359013349E-2,3.7950766140871439E-7,3.7950766140871439E-7,2.1209593340408027E-2,3.0904478572018517E-4,6.659710185963017E-4,35,91.485596098664772,1.817284956245753E-2,2.3407678740799524E-2,4.2246499321853356E-2,4.2557976629299603E-2,2.323399311307742E-2,1.6410480453747279E-4,1.8245781331405527E-3,0,1.5242487032718382E-4,1.9770030034677367E-3,2.1411727951338318E-3,2.8325298457411135E-2,4.6755362180263854E-2,2.4905491517368543E-3,9.3945060756434134E-2,0.14979402760411561,0.38570000000000004,0.72026947102600258,5.8166345727485487E-4,3.0657632616486224E-4,3.9067873395697207E-2,7.889256862652759E-2,0,2.8464345533255823E-4,3.6919235351945165E-3,1.5154707473750552E-3,0.1027594706361564,7.087056845557946E-7,5.0938865093876003E-6,8.7312574501446236E-2,0.3144185672733632,0.72026947102600258,72.026947102600261,20.3,54.888490199331855,0.54888490199331852,165.87073937641387,null,4.3712305897283581E-2,null,9.3945060756434134E-2,4.6755362180263854E-2,5.5845859594216993E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR35, IF(MODE_ILIM=4,#REF!,#REF!))","v":72.026947102600261},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ35, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.3945060756434134E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA35, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.6755362180263854E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB35, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.5845859594216993E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S35, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":165.87073937641387},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P35, IF(MODE_ILIM=4,#REF!,#REF!))","v":233.04052354646714}]
["Sleep delay",5,"µs",{"$f":"B36/1000000","v":5.0000000000000004E-6},"Delay time to enter sleep mode",null,null,30,2.1000000000000001E-2,7.3615061321327738E-2,7.3615061321327738E-2,0,129.35759118569246,111.57947696201423,2,223.15895392402845,1.8170476072160916E-6,0.2587474587973615,171590.42004456604,5.8278311792714106E-6,0,6.5999999999999989E-4,3.1996744753242434E-2,8.3950917333940067E-4,5.692456841940232E-2,5.777183759076062E-2,1.6016485833994766E-2,2.8218060031761046E-6,2.8218060031761046E-6,1.4174705383565999E-2,4.0184454542178988E-7,4.0184454542178988E-7,2.1572176756154509E-2,3.1970150246915697E-4,6.8893553647893268E-4,35,91.485596098664772,1.9030260909750032E-2,2.4214840076689156E-2,4.3934036522918121E-2,4.4256354850226914E-2,2.363118416003258E-2,1.6976359090083393E-4,1.8874946204902269E-3,0,1.5963028004955436E-4,2.0471249005397812E-3,2.2169580989947128E-3,2.8325298457411129E-2,4.7390881618982909E-2,2.5764301569691597E-3,9.6440624725173701E-2,0.15421568596648291,0.39900000000000002,0.72123768382115938,5.8262687679524886E-4,3.0699273857036135E-4,3.9120389872408894E-2,7.9415746222314995E-2,0,2.885498081470266E-4,3.7004100795938167E-3,1.5175078990624698E-3,0.10289760370759109,7.2637952179493331E-7,5.1007338995573345E-6,8.5664385195784426E-2,0.31350003951368965,0.72123768382115938,72.123768382115941,21,56.276153038808332,0.5627615303880833,171.59042004456603,null,4.3771065591506446E-2,null,9.6440624725173701E-2,4.7390881618982909E-2,5.777183759076062E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR36, IF(MODE_ILIM=4,#REF!,#REF!))","v":72.123768382115941},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ36, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.6440624725173701E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA36, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.7390881618982909E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB36, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.777183759076062E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S36, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":171.59042004456603},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P36, IF(MODE_ILIM=4,#REF!,#REF!))","v":223.15895392402845}]
["IQ(active)",660,"µA",{"$f":"B37/1000000","v":6.6E-4},"LM5164 quiescent current - active state ",null,null,31,2.1700000000000001E-2,7.3615061321327738E-2,7.3615061321327738E-2,0,126.37886778143714,106.63870369680447,2,213.27740739360894,1.8170476072160916E-6,0.26737237409060688,177310.10071271824,5.6398366251013652E-6,0,6.6E-4,3.2525652398749598E-2,8.67492812450714E-4,5.8822054033382386E-2,5.9697832836377814E-2,1.6281239073022261E-2,2.9158662032819745E-6,2.9158662032819745E-6,1.4575928508674982E-2,4.2491538378000819E-7,4.2491538378000819E-7,2.1928765818715501E-2,3.3035821921812889E-4,7.1190005436156366E-4,35,91.485596098664772,1.9903056347867886E-2,2.5022001412578796E-2,4.5636957814808247E-2,4.5970124797280514E-2,2.4021808708592711E-2,1.7542237726419504E-4,1.9504111078399006E-3,0,1.6696599594712827E-4,2.117377103787029E-3,2.2928738718964491E-3,2.8325298457411135E-2,4.8026401057701971E-2,2.6623111622014642E-3,9.8951710889080405E-2,0.15865288450704529,0.4123,0.72212613542705106,5.8352797842490796E-4,3.0737521934220919E-4,3.916858005157578E-2,7.99312150847801E-2,0,2.9243393015044482E-4,3.7084970778545941E-3,1.5193772305742848E-3,0.10302435740239535,7.442214503336395E-7,5.1070172030035417E-6,8.4116224579839818E-2,0.31265743979359084,0.72212613542705106,72.2126135427051,21.7,57.582635216683897,0.57582635216683897,177.31010071271822,null,4.3824984673091774E-2,null,9.8951710889080405E-2,4.8026401057701971E-2,5.9697832836377814E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR37, IF(MODE_ILIM=4,#REF!,#REF!))","v":72.2126135427051},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ37, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.8951710889080405E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA37, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.8026401057701971E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB37, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.9697832836377814E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S37, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":177.31010071271822},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P37, IF(MODE_ILIM=4,#REF!,#REF!))","v":213.27740739360894}]
["IQ(sleep)",10,"µA",{"$f":"B38/1000000","v":1.0000000000000001E-5},"LM5164 quiescent current - sleep state",null,null,32,{"$f":"IF(PLOT_TYPE=1, H38/100*Iout, min_I*EXP(H38*rr/100))","v":2.2400000000000003E-2},{"$f":"IF(I38<Icrit, (Vin-(Rdcr+RdsonTop)*Iripple/2-Vout)/L*OnTime, (Vin-(Rdcr+RdsonTop)*I38-Vout)/L*OnTime)","v":7.3615061321327738E-2},{"$f":"IF(I38<Icrit, (Vin-(Rdcr+RdsonTop)*Iripple/2-Vout)/L*OnTime, I38+((Vin-(Rdcr+RdsonTop)*J38-Vout)/L*OnTime)/2)","v":7.3615061321327738E-2},{"$f":"IF(I38<Icrit, 0, I38-((Vin-(Rdcr+RdsonTop)*K38-Vout)/L*OnTime)/2)","v":0},123.4001443771818,{"$f":"IF(I38<Icrit, 1000*SQRT((J38*CoutEsr)^2+(((J38/2)-I38)*(OnTime+OffTime)/Cout)^2), 1000*J38*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":101.69794366041749},2,{"$f":"IF(I38<Icrit, 1000*((N38/1000)*O38), 1000*J38*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":203.39588732083499},{"$f":"IF(I38<Icrit, L*J38/(Vout+J38/2*(RdsonBot+Rdcr)), L*J38/(Vout+I38*(RdsonBot+Rdcr)))","v":1.8170476072160916E-6},0.27599728938385232,{"$f":"IF(I38<Icrit,I38/((OnTime+Q38)*J38/2),1/(OnTime+Q38))","v":183029.78138087047},5.463591730566947E-6,0,{"$f":"S38*(T38*Iq_active+U38*Iq_sleep)","v":6.600000000000001E-4},3.3046095883242005E-2,{"$f":"W38^2*Rdcr","v":8.9547645156202776E-4},{"$f":"Core_Loss/1000*S38/$S$106","v":6.0719539647362479E-2},{"$f":"(Y38+X38*(1+Ltc*(Ta-25)))/(1-X38*Ltc*ThetaCa)","v":6.1623845331300331E-2},1.6541755439954335E-2,3.009926403387847E-6,3.009926403387847E-6,1.4978610202130541E-2,4.4871752717473828E-7,4.4871752717473828E-7,2.2279648351474442E-2,3.4101493596710086E-4,7.3486457224419496E-4,{"$f":"20*VIN_nom/24","v":35},{"$f":"IF(I38<Icrit, Csw*Vin/Iripple*1000000000, Csw*Vin/(I38+Iripple/2)*1000000000)","v":91.485596098664772},{"$f":"IF(I38<Icrit, Vin*(I38+Iripple/2)*AK38/1000000000/2*S38, Vin*(I38-Iripple/2)*AJ38/1000000000/2*S38 + Vin*(I38+Iripple/2)*AK38/1000000000/2*S38)","v":2.0791235876811094E-2},{"$f":"IF(I38<Icrit, Csw*(Vin)^2*S38/2, Csw*Vin^2*S38/2)","v":2.5829162748468436E-2},4.7355263197523728E-2,{"$f":"(AI38+AL38+AM38+AH38*(1+RdsonTopTc*(Ta-25)))/(1-AH38*RdsonTopTc*ThetaJA)","v":4.7699286561475575E-2},{"$f":"IF(I38<Icrit,Iripple*SQRT((OffTime)*S38/3), SQRT(OffTime*S38*(I38^2+Iripple^2/12)))","v":2.440618205412445E-2},1.8108116362755618E-4,{"$f":"QgBot*S38*Vdd","v":2.0133275951895757E-3},{"$f":"IF(I38<Icrit, Vin*Idss*R38, QrrBot*(I38-Iripple/2)/1*S38*Vin+Vin*Idss*R38)","v":0},{"$f":"IF(I38<Icrit, dead1*S38*(I38+Iripple/2)*((I38+Iripple/2)*BDserR+VSD), dead1*S38*(I38+Iripple/2)*((I38+Iripple/2)*BDserR+VSD)+dead2*S38*(I38-Iripple/2)*((I38-Iripple/2)*BDserR+VSD))","v":1.744320516516278E-4},2.1877596468412035E-3,{"$f":"(AR38+AS38+AT38+AQ38*(1+RdsonBotTc*(Ta-25)))/(1-AQ38*RdsonBotTc*ThetaJA)","v":2.3689201478815486E-3},{"$f":"Vin*V38+Vout*Ifb/0.8","v":2.8325298457411139E-2},{"$f":"(Vin-Vdd)*(S38*QgBot+S38*QgTop)+AW38","v":4.8661920496421041E-2},{"$f":"AI38+AR38","v":2.7481921674337708E-3},0.10147831937321194,{"$f":"SUM(Z38,AC38,AF38,AZ38)","v":0.16310562334844284},{"$f":"Vout*I38","v":0.42560000000000009},0.72294196474507955,5.8437247803937869E-4,3.0772680581839788E-4,{"$f":"Vin*S38*(QgBot+QgTop)/($BB38+$BA38)","v":3.9212831151742268E-2},8.0439631149055821E-2,0,2.9629758020569306E-4,3.7162200598622667E-3,{"$f":"X38/($BB38+$BA38)","v":1.521093762394747E-3},{"$f":"Y38/($BB38+$BA38)","v":0.10314075021400605},7.6221036351329613E-7,5.1127869074325666E-6,8.2659173900261923E-2,0.31188397209865748,{"$f":"BC38","v":0.72294196474507955},72.294196474507956,{"$f":"I38*1000","v":22.400000000000002},58.807882255999409,0.58807882255999411,{"$f":"S38/1000","v":183.02978138087047},null,{"$f":"AM38/($BB38+$BA38)","v":4.3874496393557769E-2},null,0.10147831937321194,4.8661920496421041E-2,6.1623845331300331E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR38, IF(MODE_ILIM=4,#REF!,#REF!))","v":72.294196474507956},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ38, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10147831937321194},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA38, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.8661920496421041E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB38, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.1623845331300331E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S38, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":183.02978138087047},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P38, IF(MODE_ILIM=4,#REF!,#REF!))","v":203.39588732083499}]
["High-side N-ch MOSFET",null,"Units","Std Units","Description",null,null,33,2.3100000000000002E-2,7.3615061321327738E-2,7.3615061321327738E-2,0,{"$f":"IF(I39<Icrit, 1000*((((J39/2)-I39)*0.000002/Cout+Vout/306)), 1000*J39*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":120.42142097292648},96.757198879382884,2,193.51439775876577,1.8170476072160916E-6,0.2846222046770977,188749.46204902267,{"$f":"IF(1/S39-OnTime-Q39>Tsleep, OnTime+Q39+Tsleep, 1/S39)","v":5.2980283447921912E-6},{"$f":"IF(1/S39-OnTime-Q39>Tsleep, 1/S39-OnTime-Q39-Tsleep, 0)","v":0},6.600000000000001E-4,{"$f":"IF(I39<Icrit,Iripple*SQRT((OnTime+OffTime)*S39/3), SQRT(I39^2+Iripple^2/12))","v":3.3558469009842544E-2},9.2346009067334109E-4,6.2617025261342552E-2,6.3549875075759849E-2,{"$f":"Iripple/SQRT(12)*SQRT((OnTime+Q39)*S39)","v":1.67982320592856E-2},3.1039866034937157E-6,3.1039866034937157E-6,{"$f":"SQRT($R39)*SQRT($I39^2*(1-R39)+(Iripple^2)/12)","v":1.5382564426392254E-2},4.7324657666421698E-7,4.7324657666421698E-7,{"$f":"IF(I39<Icrit,Iripple*SQRT((OnTime)*S39/3), SQRT(OnTime*S39*(I39^2+Iripple^2/12)))","v":2.2625089856145326E-2},{"$f":"RdsonTop*AG39^2","v":3.5167165271607267E-4},{"$f":"QgTop*S39*Vdd","v":7.5782909012682604E-4},35,91.485596098664772,2.1694799496579639E-2,2.6636324084358075E-2,4.9088952671064542E-2,4.9443840233827918E-2,2.4784595039780501E-2,{"$f":"RdsonBot*AP39^2","v":1.8673994999091731E-4},2.0762440825392494E-3,0,1.8202848079477529E-4,2.2582725633340248E-3,2.4450969609926586E-3,2.8325298457411139E-2,4.9297439935140103E-2,2.8340731726660753E-3,0.10402045030262674,0.16757390261156674,0.43890000000000007,0.72369148632782276,5.85165431249683E-4,3.0805018460669151E-4,3.9253485678249198E-2,8.094157466575265E-2,0,3.0014231446882309E-4,3.723610453161409E-3,1.5226707805509594E-3,0.10324768302758672,7.8032471739731388E-7,5.1180876705947075E-6,8.1285344221503991E-2,0.31117362516951808,0.72369148632782276,72.36914863278227,23.1,59.95273560232264,0.59952735602322638,188.74946204902267,null,4.3919983975663421E-2,null,0.10402045030262674,4.9297439935140103E-2,6.3549875075759849E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR39, IF(MODE_ILIM=4,#REF!,#REF!))","v":72.36914863278227},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ39, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10402045030262674},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA39, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.9297439935140103E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB39, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.3549875075759849E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S39, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":188.74946204902267},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P39, IF(MODE_ILIM=4,#REF!,#REF!))","v":193.51439775876577}]
["RdsonTop",687,"mW",{"$f":"B40/1000","v":0.68700000000000006},"Drain-source resistance of high-side MOSFET @ VDD, 25°C",null,null,34,2.3800000000000005E-2,7.3615061321327738E-2,7.3615061321327738E-2,0,117.44269756867115,91.816471816422222,2,183.63294363284444,1.8170476072160916E-6,0.29324711997034308,194469.14271717489,5.1422039817100673E-6,0,6.600000000000001E-4,3.4063135960223929E-2,9.5144372978465453E-4,6.4514510875322645E-2,6.547592206998816E-2,1.7050851228016813E-2,3.1980468035995864E-6,3.1980468035995864E-6,1.5787596138639153E-2,4.9849638367354777E-7,4.9849638367354777E-7,2.2965335863686879E-2,3.6232836946504469E-4,7.8079360800945713E-4,35,91.485596098664772,2.2613747207173539E-2,2.7443485420247719E-2,5.0838026235430711E-2,5.1203785905354182E-2,2.5157316631802332E-2,1.9239873635427848E-4,2.1391605698889244E-3,0,1.8975531700829307E-4,2.3289158868972175E-3,2.5214043452725715E-3,2.8325298457411139E-2,4.9932959373859165E-2,2.9199541778983816E-3,0.10657810380238429,0.17205772241555972,0.4522000000000001,0.72438030602203218,5.8591132602760156E-4,3.0834774078648402E-4,3.9290847695783414E-2,8.1437560818172036E-2,0,3.0396951482480108E-4,3.7306961584479847E-3,1.5241200799295702E-3,0.10334595561859339,7.9854259831119154E-7,5.1229591381341214E-6,7.9987731958915953E-2,0.3105210624132177,0.72438030602203218,72.438030602203213,23.800000000000004,61.018807215515402,0.61018807215515403,194.46914271717489,null,4.3961787631645773E-2,null,0.10657810380238429,4.9932959373859165E-2,6.547592206998816E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR40, IF(MODE_ILIM=4,#REF!,#REF!))","v":72.438030602203213},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ40, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10657810380238429},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA40, IF(MODE_ILIM=4,#REF!,#REF!))","v":4.9932959373859165E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB40, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.547592206998816E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S40, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":194.46914271717489},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P40, IF(MODE_ILIM=4,#REF!,#REF!))","v":183.63294363284444}]
["RdsonTopTc",4500,"ppm/°C",{"$f":"B41/1000000","v":4.4999999999999997E-3},"Drain to Source Resistance Temp Co",null,null,35,2.4500000000000001E-2,7.3615061321327738E-2,7.3615061321327738E-2,0,114.46397416441586,86.875765494478799,2,173.7515309889576,1.8170476072160916E-6,0.30187203526358841,200188.82338532706,4.995283867946923E-6,0,6.6E-4,3.4560434323151069E-2,9.7942736889596754E-4,6.641199648930271E-2,6.7401986314216941E-2,1.7299781931640473E-2,3.2921070037054555E-6,3.2921070037054555E-6,1.6193502554955504E-2,5.2445904999470088E-7,5.2445904999470088E-7,2.3300613976143098E-2,3.729850862140165E-4,8.0375812589208811E-4,35,91.485596098664772,2.3548079008592765E-2,2.8250646756137351E-2,5.2602483890622206E-2,5.2979123667071644E-2,2.5524596156249052E-2,1.9805752271763956E-4,2.2020770572385977E-3,0,1.9761259392390334E-4,2.3996896511625011E-3,2.5978423347642185E-3,2.8325298457411135E-2,5.0568478812578213E-2,3.0058351831306861E-3,0.10915127999754476,0.17655708287781541,0.46550000000000002,0.72501341767548966,5.8661416016356411E-4,3.086215990540302E-4,3.9325188073819128E-2,8.1928048600987943E-2,0,3.0778041266699862E-4,3.737502030826699E-3,1.5254521677511878E-3,0.1034362804497572,8.1684177930719343E-7,5.1274366275185995E-6,7.8760098067793591E-2,0.30992152984122712,0.72501341767548966,72.501341767548965,24.5,62.00835196729512,0.62008351967295117,200.18882338532705,null,4.4000210432245168E-2,null,0.10915127999754476,5.0568478812578213E-2,6.7401986314216941E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR41, IF(MODE_ILIM=4,#REF!,#REF!))","v":72.501341767548965},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ41, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10915127999754476},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA41, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.0568478812578213E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB41, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.7401986314216941E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S41, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":200.18882338532705},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P41, IF(MODE_ILIM=4,#REF!,#REF!))","v":173.7515309889576}]
["QgTop",0.80300000000000005,"nC",{"$f":"B42/1000000000","v":8.0300000000000002E-10},"Gate charge of high-side MOSFET @ VDD",null,null,36,2.52E-2,7.3615061321327738E-2,7.3615061321327738E-2,0,111.48525076016053,81.935083665618436,2,163.87016733123687,1.8170476072160916E-6,0.3104969505568338,205908.50405347926,4.8565259827261753E-6,0,6.6E-4,3.505067773617191E-2,1.0074110080072812E-3,6.830948210328279E-2,6.9328067808677965E-2,1.7545181166481755E-2,3.3861672038113271E-6,3.3861672038113271E-6,1.6600074213486436E-2,5.5112492778651467E-7,5.5112492778651467E-7,2.3631135647668892E-2,3.8364180296298841E-4,8.267226437747193E-4,35,91.485596098664772,2.4497794900837349E-2,2.9057808092026991E-2,5.4382325636639056E-2,5.4769853609998365E-2,2.5886665250017229E-2,2.0371630908100065E-4,2.2649935445882719E-3,0,2.056003451733286E-4,2.4705938897616004E-3,2.6744109635106783E-3,2.8325298457411135E-2,5.1203998251297275E-2,3.0917161883629914E-3,0.1117399790131693,0.18107198411397887,0.4788,0.72559528442913479,5.8727750637822384E-4,3.0887365830926499E-4,3.9356748895954488E-2,8.2413448283698718E-2,0,3.1157610888631922E-4,3.7440502843576668E-3,1.5266764346117056E-3,0.10351929426887713,8.3519976761328845E-7,5.1315517029534004E-6,7.7596866489262672E-2,0.30937077868180679,0.72559528442913479,72.559528442913475,25.2,62.924142868481049,0.62924142868481048,205.90850405347928,null,4.4035523240228781E-2,null,0.1117399790131693,5.1203998251297275E-2,6.9328067808677965E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR42, IF(MODE_ILIM=4,#REF!,#REF!))","v":72.559528442913475},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ42, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.1117399790131693},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA42, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.1203998251297275E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB42, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.9328067808677965E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S42, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":205.90850405347928},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P42, IF(MODE_ILIM=4,#REF!,#REF!))","v":163.87016733123687}]
["Coss",100,"pF",{"$f":"B43/1000000000000","v":1E-10},"Capacitance (Coss)",null,null,37,2.5900000000000003E-2,7.3615061321327738E-2,7.3615061321327738E-2,0,108.50652735590522,76.994431044956173,2,153.98886208991235,1.8170476072160916E-6,0.31912186585007918,211628.18472163146,4.725268523733576E-6,0,6.6E-4,3.553415819919075E-2,1.0353946471185944E-3,7.0206967717262869E-2,7.1254166553602977E-2,1.7787195097794872E-2,3.4802274039171971E-6,3.4802274039171971E-6,1.7007095865765764E-2,5.7848261957469396E-7,5.7848261957469396E-7,2.3957097744339149E-2,3.9429851971196033E-4,8.4968716165735039E-4,35,91.485596098664772,2.5462894883907281E-2,2.9864969427916627E-2,5.617755147348126E-2,5.6575975825153085E-2,2.6243739569529637E-2,2.0937509544436189E-4,2.3279100319379465E-3,0,2.1371860438829115E-4,2.5416286363262376E-3,2.7511102655551701E-3,2.8325298457411135E-2,5.183951769001633E-2,3.1775971935952968E-3,0.11434420097431988,0.18560242623794634,0.49210000000000004,0.7261299073868448,5.8790456732397067E-4,3.0910562087228225E-4,3.9385747184604004E-2,8.2894127715217744E-2,0,3.1535759075658519E-4,3.7503608337885051E-3,1.5278012989657789E-3,0.1035955679058063,8.5359384469959731E-7,5.1353326610273384E-6,7.6493038364621541E-2,0.3088650000084624,0.7261299073868448,72.612990738684474,25.900000000000002,63.769353027551922,0.63769353027551923,211.62818472163147,null,4.4067968877878581E-2,null,0.11434420097431988,5.183951769001633E-2,7.1254166553602977E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR43, IF(MODE_ILIM=4,#REF!,#REF!))","v":72.612990738684474},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ43, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.11434420097431988},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA43, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.183951769001633E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB43, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.1254166553602977E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S43, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":211.62818472163147},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P43, IF(MODE_ILIM=4,#REF!,#REF!))","v":153.98886208991235}]
["Low-side N-ch MOSFET",null,"Units","Std Units","Description",null,null,38,2.6600000000000002E-2,7.3615061321327738E-2,7.3615061321327738E-2,0,105.52780395164989,72.053813640816671,2,144.10762728163334,1.8170476072160916E-6,0.32774678114332456,217347.86538978366,4.6009193520563762E-6,0,6.5999999999999989E-4,3.6011148108401843E-2,1.0633782862299079E-3,7.2104453331242949E-2,7.3180282549223735E-2,1.8025960077881282E-2,3.5742876040230674E-6,3.5742876040230674E-6,1.7414347220780488E-2,6.0651897825181025E-7,6.0651897825181025E-7,2.4278683915424912E-2,4.0495523646093224E-4,8.7265167953998147E-4,35,91.485596098664772,2.6443378957802553E-2,3.0672130763806267E-2,5.7988161401148805E-2,5.8397490403555255E-2,2.6596020292896105E-2,2.1503388180772298E-4,2.3908265192876207E-3,0,2.2196740520051333E-4,2.612793924488134E-3,2.827940274941054E-3,2.8325298457411129E-2,5.2475037128735386E-2,3.2634781988276022E-3,0.11696394600605931,0.19014840936186531,0.50540000000000007,0.7266208838917223,5.8849822226175611E-4,3.0931901727775807E-4,3.9412378061941457E-2,8.3370417674235434E-2,0,3.1912574626424427E-4,3.7564515845636914E-3,1.5288343297420665E-3,0.10366561458661888,8.7200110026599634E-7,5.1388049428541101E-6,7.5444119233740892E-2,0.30840076926268933,0.7266208838917223,72.662088389172226,26.6,64.547447140017496,0.645474471400175,217.34786538978366,null,4.4097765663710708E-2,null,0.11696394600605931,5.2475037128735386E-2,7.3180282549223735E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR44, IF(MODE_ILIM=4,#REF!,#REF!))","v":72.662088389172226},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ44, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.11696394600605931},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA44, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.2475037128735386E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB44, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.3180282549223735E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S44, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":217.34786538978366},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P44, IF(MODE_ILIM=4,#REF!,#REF!))","v":144.10762728163334}]
["RdsonBot",304,"mW",{"$f":"B45/1000","v":0.30399999999999999},"Drain-source resistance of low-side MOSFET @ VDD, 25°C",null,null,39,2.7300000000000005E-2,7.3615061321327738E-2,7.3615061321327738E-2,0,102.54908054739457,67.113239230713404,2,134.22647846142681,1.8170476072160916E-6,0.33637169643657,223067.54605793589,4.482947060978007E-6,0,6.6E-4,3.6481902050816813E-2,1.0913619253412213E-3,7.4001938945223028E-2,7.5106415795771986E-2,1.8261603544369308E-2,3.6683478041289382E-6,3.6683478041289382E-6,1.7821603562492662E-2,6.3521910707730227E-7,6.3521910707730227E-7,2.4596065803262211E-2,4.1561195320990405E-4,8.9561619742261256E-4,35,91.485596098664772,2.7439247122523176E-2,3.147929209969591E-2,5.9814155419641697E-2,6.0234397436225065E-2,2.6943695445261165E-2,2.2069266817108412E-4,2.4537430066372953E-3,0,2.3034678124171738E-4,2.6840897878790126E-3,2.9049010257118347E-3,2.8325298457411135E-2,5.3110556567454448E-2,3.349359204059908E-3,0.11959921423345125,0.19470993359613445,0.51870000000000005,0.72707145719902344,5.8906106684697402E-4,3.0951522740896477E-4,3.9436817444191065E-2,8.3842616429704558E-2,0,3.2288137632257587E-4,3.7623386800196864E-3,1.5297823508567062E-3,0.10372989702035178,8.9039846119791137E-7,5.1419914853689315E-6,7.4446056981203518E-2,0.30797499896685243,0.72707145719902344,72.707145719902343,27.300000000000004,65.262084299350803,0.65262084299350809,223.06754605793589,null,4.4125110427066919E-2,null,0.11959921423345125,5.3110556567454448E-2,7.5106415795771986E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR45, IF(MODE_ILIM=4,#REF!,#REF!))","v":72.707145719902343},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ45, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.11959921423345125},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA45, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.3110556567454448E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB45, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.5106415795771986E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S45, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":223.06754605793589},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P45, IF(MODE_ILIM=4,#REF!,#REF!))","v":134.22647846142681}]
["RdsonBotTc",4500,"ppm/°C",{"$f":"B46/1000000","v":4.4999999999999997E-3},"Drain To Source Resitance Temp Co",null,null,40,2.8000000000000004E-2,7.3615061321327738E-2,7.3615061321327738E-2,0,99.570357143139248,62.172718064250709,2,124.34543612850142,1.8170476072160916E-6,0.34499661172981538,228787.22672608809,4.3708733844535573E-6,0,6.6E-4,3.6946658392952539E-2,1.1193455644525347E-3,7.5899424559203107E-2,7.7032566293479487E-2,1.8494244815457413E-2,3.7624080042348077E-6,3.7624080042348077E-6,1.8228636258336445E-2,6.6456635967747633E-7,6.6456635967747633E-7,2.4909404114343989E-2,4.2626866995887607E-4,9.1858071530524364E-4,35,91.485596098664772,2.8450499378069139E-2,3.2286453435585546E-2,6.165553352895993E-2,6.2086697014183415E-2,2.728694107212886E-2,2.2635145453444523E-4,2.516659493986969E-3,0,2.3885676614362564E-4,2.7555162601305945E-3,2.9819925519111562E-3,2.8325298457411135E-2,5.374607600617351E-2,3.4352402092922129E-3,0.1222500057815603,0.1992869990494037,0.53200000000000003,0.72748455899194719,5.8959544718277762E-4,3.0969549858667951E-4,3.9459224347710792E-2,8.4310993644226742E-2,0,3.2662520522601157E-4,3.7680367129628669E-3,1.5306515306679406E-3,0.1037888334646512,9.0876271633618912E-7,5.1449130220085174E-6,7.3495188723494004E-2,0.30758489825044733,0.72748455899194719,72.748455899194724,28.000000000000004,65.91703305041338,0.65917033050413376,228.78722672608808,null,4.4150181088347729E-2,null,0.1222500057815603,5.374607600617351E-2,7.7032566293479487E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR46, IF(MODE_ILIM=4,#REF!,#REF!))","v":72.748455899194724},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ46, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.1222500057815603},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA46, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.374607600617351E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB46, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.7032566293479487E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S46, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":228.78722672608808},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P46, IF(MODE_ILIM=4,#REF!,#REF!))","v":124.34543612850142}]
["QgBot",2.2000000000000002,"nC",{"$f":"B47/1000000000","v":2.2000000000000003E-9},"Gate charge of low-side MOSFET at VDD",null,null,41,2.87E-2,7.3615061321327738E-2,7.3615061321327738E-2,0,96.591633738883942,57.232263930051303,2,114.46452786010261,1.8170476072160916E-6,0.35362152702306071,234506.90739424026,4.2642667165400563E-6,0,6.6E-4,3.7405640691821708E-2,1.1473292035638477E-3,7.7796910173183173E-2,7.8958734042577972E-2,1.8723995796208277E-2,3.8564682043406772E-6,3.8564682043406772E-6,1.8635213173525875E-2,6.9454234004550466E-7,6.9454234004550466E-7,2.521884957060868E-2,4.3692538670784788E-4,9.4154523318787462E-4,35,91.485596098664772,2.9477135724440443E-2,3.3093614771475183E-2,6.3512295729103496E-2,6.3954389228451924E-2,2.7625922281449333E-2,2.3201024089780634E-4,2.5795759813366428E-3,0,2.4749739353796047E-4,2.8270733748746034E-3,3.0592148875828104E-3,2.8325298457411135E-2,5.4381595444892565E-2,3.5211212145245174E-3,0.12491632077545183,0.20387960582857417,0.54530000000000001,0.72786284591518158,5.9010348908187865E-4,3.0986096111287518E-4,3.9479742870595171E-2,8.4775793728208149E-2,0,3.3035788963346703E-4,3.7735589074771058E-3,1.5314474588439041E-3,0.10384280293794397,9.2707053774823179E-7,5.1475883410834688E-6,7.258819516949859E-2,0.30722793807127391,0.72786284591518158,72.786284591518154,28.7,66.516098897051677,0.66516098897051679,234.50690739424027,null,4.4173138876190385E-2,null,0.12491632077545183,5.4381595444892565E-2,7.8958734042577972E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR47, IF(MODE_ILIM=4,#REF!,#REF!))","v":72.786284591518154},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ47, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.12491632077545183},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA47, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.4381595444892565E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB47, IF(MODE_ILIM=4,#REF!,#REF!))","v":7.8958734042577972E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S47, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":234.50690739424027},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P47, IF(MODE_ILIM=4,#REF!,#REF!))","v":114.46452786010261}]
["VSD",0.8,"V",{"$f":"B48","v":0.8},"Body diode forward voltage",null,null,42,2.9400000000000003E-2,7.3615061321327738E-2,7.3615061321327738E-2,0,93.612910334628609,52.291895827419538,2,104.58379165483908,1.8170476072160916E-6,0.36224644231630615,240226.58806239249,4.1627365566224354E-6,0,6.6E-4,3.7859058951931264E-2,1.1753128426751616E-3,7.9694395787163266E-2,8.088491904329928E-2,1.8950961607759567E-2,3.950528404446548E-6,3.950528404446548E-6,1.9041099003752757E-2,7.2512690254142856E-7,7.2512690254142856E-7,2.5524543756907429E-2,4.475821034568198E-4,9.6450975107050592E-4,35,91.485596098664772,3.0519156161637102E-2,3.3900776107364826E-2,6.5384442020072431E-2,6.5837474170052923E-2,2.7960794171974526E-2,2.3766902726116748E-4,2.6424924686863174E-3,0,2.5626869705644439E-4,2.8987611657427617E-3,3.1365680667707284E-3,2.8325298457411135E-2,5.5017114883611627E-2,3.6070022197568232E-3,0.12759815934019211,0.20848775403879838,0.5586000000000001,0.72820873108573536,5.9058712330529322E-4,3.1001264167741983E-4,3.9498503901842813E-2,8.5237238732878209E-2,0,3.3408002631662737E-4,3.778917275736024E-3,1.5321752126624558E-3,0.10389214971502779,9.4529849906162422E-7,5.1500345086290279E-6,7.1722061255626454E-2,0.30690182121808079,0.72820873108573536,72.820873108573537,29.400000000000002,67.063063929713536,0.6706306392971354,240.22658806239249,null,4.4194130239824117E-2,null,0.12759815934019211,5.5017114883611627E-2,8.088491904329928E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR48, IF(MODE_ILIM=4,#REF!,#REF!))","v":72.820873108573537},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ48, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.12759815934019211},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA48, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.5017114883611627E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB48, IF(MODE_ILIM=4,#REF!,#REF!))","v":8.088491904329928E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S48, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":240.22658806239249},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P48, IF(MODE_ILIM=4,#REF!,#REF!))","v":104.58379165483908}]
["BDserR",100,"mW",{"$f":"B49*0.001","v":0.1},"Series resistance of body diode",null,null,43,3.0100000000000002E-2,7.3615061321327738E-2,7.3615061321327738E-2,0,90.634186930373303,47.351640684317893,2,94.703281368635785,1.8170476072160916E-6,0.37087135760955148,245946.26873054466,4.0659287297242401E-6,0,6.6E-4,3.8307110748344683E-2,1.2032964817864746E-3,8.1591881401143332E-2,8.2811121295875117E-2,1.9175241149490894E-2,4.044588604552417E-6,4.044588604552417E-6,1.9446055536948278E-2,7.5629815189215358E-7,7.5629815189215358E-7,2.5826619878171718E-2,4.5823882020579171E-4,9.8747426895313679E-4,35,91.485596098664772,3.1576560689659097E-2,3.4707937443254455E-2,6.7271972401866692E-2,6.7735951930009461E-2,2.8291702662695477E-2,2.4332781362452859E-4,2.7054089560359916E-3,0,2.6517071033079929E-4,2.9705796663667908E-3,3.2140521235189826E-3,2.8325298457411135E-2,5.5652634322330682E-2,3.6928832249891281E-3,0.13029552160084823,0.21311144378347979,0.57190000000000007,0.72852441136863255,5.9104810740917395E-4,3.1015147496288705E-4,3.9515626600807381E-2,8.5695530854479493E-2,0,3.3779215886684335E-4,3.7841227537392815E-3,1.532839414400136E-3,0.10393718721844242,9.6342309132088781E-7,5.1522670613041234E-6,7.0894042071672866E-2,0.30660445634493311,0.72852441136863255,72.852441136863249,30.1,67.561637846160409,0.67561637846160405,245.94626873054466,null,4.4213288504399845E-2,null,0.13029552160084823,5.5652634322330682E-2,8.2811121295875117E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR49, IF(MODE_ILIM=4,#REF!,#REF!))","v":72.852441136863249},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ49, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.13029552160084823},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA49, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.5652634322330682E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB49, IF(MODE_ILIM=4,#REF!,#REF!))","v":8.2811121295875117E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S49, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":245.94626873054466},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P49, IF(MODE_ILIM=4,#REF!,#REF!))","v":94.703281368635785}]
["QrrBot",3,"nC",{"$f":"B50*0.000000001","v":3.0000000000000004E-9},"Reverse recovery charge of body diode at 100mA",null,null,44,3.0800000000000004E-2,7.3615061321327738E-2,7.3615061321327738E-2,0,87.65546352611797,42.411537974614937,3,127.2346139238448,1.8170476072160916E-6,0.37949627290279692,251665.94939869689,3.9735212585941428E-6,0,6.6E-4,3.8749982232848618E-2,1.2312801208977885E-3,8.3489367015123411E-2,8.473734080053727E-2,1.9396927602676688E-2,4.1386488046582878E-6,4.1386488046582878E-6,1.984984185316668E-2,7.8803244319145524E-7,7.8803244319145524E-7,2.6125203437769952E-2,4.6889553695476363E-4,1.010438786835768E-3,35,91.485596098664772,3.2649349308506451E-2,3.5515098779144098E-2,6.9174886874486308E-2,6.9649822599345337E-2,2.861878523594627E-2,2.489865999878897E-4,2.7683254433856662E-3,0,2.7420346699274796E-4,3.0425289103784142E-3,3.2916670918717913E-3,2.8325298457411135E-2,5.6288153761049745E-2,3.7787642302214344E-3,0.13300840768248831,0.21775067516427343,0.58520000000000005,0.72881189106700184,5.9148804471938936E-4,3.1027831372382441E-4,3.9531219682163062E-2,8.6150854609262278E-2,0,3.4149478352035691E-4,3.7891853192052573E-3,1.5334442811769033E-3,0.10397820139828957,9.8142073674729003E-7,5.1543001739323195E-6,7.0101633265995958E-2,0.30633393541896725,0.72881189106700184,72.881189106700191,30.800000000000004,68.015419380100283,0.68015419380100284,251.66594939869688,null,4.4230735308713909E-2,null,0.13300840768248831,5.6288153761049745E-2,8.473734080053727E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR50, IF(MODE_ILIM=4,#REF!,#REF!))","v":72.881189106700191},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ50, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.13300840768248831},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA50, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.6288153761049745E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB50, IF(MODE_ILIM=4,#REF!,#REF!))","v":8.473734080053727E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S50, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":251.66594939869688},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P50, IF(MODE_ILIM=4,#REF!,#REF!))","v":127.2346139238448}]
["TrrBot",20,"ns",{"$f":"B51*0.000000001","v":2E-8},"Reverse recovery time of body diode (not used)",null,null,45,3.1500000000000007E-2,7.3615061321327738E-2,7.3615061321327738E-2,0,84.676740121862636,37.471647986872235,3,112.4149439606167,1.8170476072160916E-6,0.38812118819604235,257385.63006684912,3.8852207861809393E-6,0,6.5999999999999989E-4,3.9187849037759417E-2,1.2592637600091017E-3,8.5386852629103491E-2,8.6663577557517538E-2,1.9616108882901131E-2,4.2327090047641586E-6,4.2327090047641586E-6,2.0252214470274289E-2,8.2030438189997464E-7,8.2030438189997464E-7,2.6420412846853081E-2,4.7955225370373554E-4,1.0334033047183992E-3,35,91.485596098664772,3.3737522018179159E-2,3.6322260115033742E-2,7.1093185437931306E-2,7.1579086269085032E-2,2.8942171604910059E-2,2.5464538635125086E-4,2.8312419307353403E-3,0,2.8336700067401247E-4,3.1146089314093529E-3,3.3694130058735117E-3,2.8325298457411129E-2,5.6923673199768807E-2,3.8646452354537397E-3,0.13573681771018109,0.22240544828108527,0.59850000000000014,0.72907300256468566,5.9190840086536958E-4,3.1039393756942342E-4,3.9545382535572833E-2,8.6603378728689298E-2,0,3.4518835423417131E-4,3.794114094298084E-3,1.5339936683888575E-3,0.10401545367727449,9.9926780071642935E-7,5.1561468054903702E-6,6.9342545257754989E-2,0.30608851406925375,0.72907300256468566,72.907300256468559,31.500000000000007,68.427867006324419,0.68427867006324417,257.3856300668491,null,4.4246581857983573E-2,null,0.13573681771018109,5.6923673199768807E-2,8.6663577557517538E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR51, IF(MODE_ILIM=4,#REF!,#REF!))","v":72.907300256468559},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ51, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.13573681771018109},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA51, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.6923673199768807E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB51, IF(MODE_ILIM=4,#REF!,#REF!))","v":8.6663577557517538E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S51, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":257.3856300668491},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P51, IF(MODE_ILIM=4,#REF!,#REF!))","v":112.4149439606167}]
["Idss",0,"μA",{"$f":"B52/1000000","v":0},"Leakage current of low-side device",null,null,46,3.2200000000000006E-2,7.3615061321327738E-2,7.3615061321327738E-2,0,81.698016717607317,32.532067624673559,3,97.596202874020676,1.8170476072160916E-6,0.39674610348928768,263105.31073500129,3.8007594647422241E-6,0,6.6E-4,3.9620877089816681E-2,1.2872473991204154E-3,8.7284338243083556E-2,8.858983156704768E-2,1.983286804746566E-2,4.3267692048700277E-6,4.3267692048700277E-6,2.0652927441953829E-2,8.5308682384521912E-7,8.5308682384521912E-7,2.6712359973080847E-2,4.9020897045270746E-4,1.0563678226010302E-3,35,91.485596098664772,3.4841078818677193E-2,3.7129421450923378E-2,7.3026868092201602E-2,7.3523743030253705E-2,2.9261984314719804E-2,2.6030417271461197E-4,2.8941584180850145E-3,0,2.9266134500631512E-4,3.1868197630913297E-3,3.4472898995686458E-3,2.8325298457411135E-2,5.7559192638487869E-2,3.9505262406860451E-3,0.13848075180899627,0.22707576323207268,0.61180000000000012,0.72930942436913304,5.9231051823182006E-4,3.104990606401125E-4,3.9558206204346365E-2,8.7053257815959698E-2,0,3.4887328712267387E-4,3.7989174354173161E-3,1.534491107671091E-3,0.10404918352485119,1.0169406022155094E-6,5.1578188267110997E-6,6.8614680696841485E-2,0.30586659441051067,0.72930942436913304,72.930942436913298,32.200000000000003,68.802277733330541,0.68802277733330541,263.1053107350013,null,4.4260930018849072E-2,null,0.13848075180899627,5.7559192638487869E-2,8.858983156704768E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR52, IF(MODE_ILIM=4,#REF!,#REF!))","v":72.930942436913298},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ52, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.13848075180899627},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA52, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.7559192638487869E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB52, IF(MODE_ILIM=4,#REF!,#REF!))","v":8.858983156704768E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S52, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":263.1053107350013},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P52, IF(MODE_ILIM=4,#REF!,#REF!))","v":97.596202874020676}]
["Csw",160,"pF",{"$f":"B53/1000000000000","v":1.5999999999999999E-10},"Effective SW node capacitance (CossHS + CossLS)",null,null,47,3.2899999999999999E-2,7.3615061321327738E-2,7.3615061321327738E-2,0,78.71929331335204,27.592963172247551,3,82.778889516742652,1.8170476072160916E-6,0.40537101878253301,268824.99140315346,3.7198922420881344E-6,0,6.6E-4,4.0049223344860232E-2,1.3152310382317282E-3,8.9181823857063636E-2,9.0516102829359513E-2,2.00472836631434E-2,4.4208294049758985E-6,4.4208294049758985E-6,2.105173241352792E-2,8.8635087522156412E-7,8.8635087522156412E-7,2.7001150635940392E-2,5.0086568720167932E-4,1.0793323404836611E-3,35,91.485596098664772,3.5960019710000561E-2,3.7936582786813014E-2,7.497593483729724E-2,7.5483792973877306E-2,2.9578339285053743E-2,2.6596295907797309E-4,2.9570749054346882E-3,0,3.0208653362137828E-4,3.2591614390560667E-3,3.5252978070018383E-3,2.8325298457411135E-2,5.8194712077206924E-2,4.0364072459183496E-3,0.14124021010400442,0.23176162011364415,0.62509999999999999,0.72952269692869898,5.9269562862753768E-4,3.1059433833723868E-4,3.9569774243380477E-2,8.7500633798201055E-2,0,3.5254996434700049E-4,3.8036030119120165E-3,1.5349398401778005E-3,0.10407961071384619,1.0344154229991173E-6,5.1593271319464299E-6,6.7916114704132335E-2,0.30566670998551659,0.72952269692869898,72.952269692869891,32.9,69.1417728033842,0.69141772803384205,268.82499140315343,null,4.4273873279306812E-2,null,0.14124021010400442,5.8194712077206924E-2,9.0516102829359513E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR53, IF(MODE_ILIM=4,#REF!,#REF!))","v":72.952269692869891},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ53, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.14124021010400442},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA53, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.8194712077206924E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB53, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.0516102829359513E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S53, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":268.82499140315343},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P53, IF(MODE_ILIM=4,#REF!,#REF!))","v":82.778889516742652}]
["ThetaJA",41.1,"°C/W",null,"Thermal resistance",null,null,48,3.3600000000000005E-2,7.3615061321327738E-2,7.3615061321327738E-2,0,75.740569909096678,22.654645901405846,4,90.618583605623385,1.8170476072160916E-6,0.41399593407577845,274544.67207130569,3.6423944870446315E-6,0,6.6E-4,4.0473036452515349E-2,1.3432146773430416E-3,9.1079309471043715E-2,9.2442391344684807E-2,2.0259430138897985E-2,4.5148896050817684E-6,4.5148896050817684E-6,2.1448378640240535E-2,9.2006589259025293E-7,9.2006589259025293E-7,2.7286885054876395E-2,5.1152240395065129E-4,1.1022968583662923E-3,35,91.485596098664772,3.7094344692149291E-2,3.874374412270265E-2,7.6940385673218231E-2,7.7459236190982494E-2,2.9891346301038357E-2,2.7162174544133425E-4,3.0199913927843628E-3,0,3.1164260015092445E-4,3.3316339929352875E-3,3.6034367622178763E-3,2.8325298457411135E-2,5.8830231515925979E-2,4.122288251150655E-3,0.14401519272027699,0.23646301902045946,0.63840000000000008,0.72971423653817791,5.9306486442322628E-4,3.1068037323935899E-4,3.9580163473403956E-2,8.7945637203141289E-2,0,3.5621873753431145E-4,3.8081778752810371E-3,1.5353428458399945E-3,0.10410693730433442,1.0516685156270575E-6,5.1606817375100211E-6,6.7245077500012795E-2,0.30548751252746353,0.72971423653817791,72.971423653817794,33.6,69.449289175978407,0.69449289175978413,274.54467207130568,null,4.4285497592619794E-2,null,0.14401519272027699,5.8830231515925979E-2,9.2442391344684807E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR54, IF(MODE_ILIM=4,#REF!,#REF!))","v":72.971423653817794},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ54, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.14401519272027699},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA54, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.8830231515925979E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB54, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.2442391344684807E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S54, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":274.54467207130568},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P54, IF(MODE_ILIM=4,#REF!,#REF!))","v":90.618583605623385}]
["Inductor",null,"Units","Std Units","Description",null,null,49,3.4300000000000004E-2,7.3615061321327738E-2,7.3615061321327738E-2,0,72.761846504841373,17.717774036700202,5,88.588870183501015,1.8170476072160916E-6,0.42262084936902383,280264.35273945791,3.5680599056763731E-6,0,6.6E-4,4.0892457358867228E-2,1.371198316454355E-3,9.2976795085023808E-2,9.4368697113255393E-2,2.0469378027562046E-2,4.6089498051876383E-6,4.6089498051876383E-6,2.1842612971888165E-2,9.5419948287939419E-7,9.5419948287939419E-7,2.7569658255613711E-2,5.2217912069962326E-4,1.1252613762489235E-3,35,91.485596098664772,3.8244053765123374E-2,3.9550905458592293E-2,7.8920220599964591E-2,7.945007277259665E-2,3.0201109458353439E-2,2.7728053180469542E-4,3.0829078801340374E-3,0,3.2132957822667588E-4,3.4042374583607132E-3,3.6817067992616884E-3,2.8325298457411135E-2,5.9465750954645048E-2,4.2081692563829612E-3,0.14680569978288635,0.2411799600454298,0.65170000000000006,0.72988534759682755,5.9341926836962479E-4,3.1075772031758622E-4,3.958944464586072E-2,8.8388388284522737E-2,0,3.5987993079195844E-4,3.8126485201745433E-3,1.535702869156777E-3,0.10413134939246832,1.0686761105388057E-6,5.1618918683684358E-6,6.6599939091050303E-2,0.30532776029069147,0.72988534759682755,72.98853475968275,34.300000000000004,69.727575757335345,0.69727575757335347,280.26435273945793,null,4.4295882121242747E-2,null,0.14680569978288635,5.9465750954645048E-2,9.4368697113255393E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR55, IF(MODE_ILIM=4,#REF!,#REF!))","v":72.98853475968275},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ55, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.14680569978288635},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA55, IF(MODE_ILIM=4,#REF!,#REF!))","v":5.9465750954645048E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB55, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.4368697113255393E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S55, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":280.26435273945793},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P55, IF(MODE_ILIM=4,#REF!,#REF!))","v":88.588870183501015}]
["Ltc",4000,"ppm",{"$f":"Ltc","v":4.0000000000000001E-3},"Inductor DCR Temp Co",null,null,50,3.5000000000000003E-2,7.3615061321327738E-2,7.3615061321327738E-2,0,69.783123100586053,12.784022227665892,6,76.704133365995347,1.8170476072160916E-6,0.43124576466226916,285984.03340761008,3.4966987075628462E-6,0,6.6E-4,4.1307619854052499E-2,1.3991819555656678E-3,9.4874280699003874E-2,9.6295020135303E-2,2.0677194299942914E-2,4.7030100052935082E-6,4.7030100052935082E-6,2.2234179807044428E-2,9.8871750338396429E-7,9.8871750338396429E-7,2.784956043934305E-2,5.3283583744859501E-4,1.1482258941315545E-3,35,91.485596098664772,3.9409146928922792E-2,4.035806679448193E-2,8.0915439617536278E-2,8.1456302809747777E-2,3.0507727567655563E-2,2.8293931816805653E-4,3.1458243674837112E-3,0,3.311475014803547E-4,3.4769718689640658E-3,3.7601079521783452E-3,2.8325298457411135E-2,6.0101270393364103E-2,4.2940502616152657E-3,0.14961173141690551,0.24591244327971717,0.66500000000000004,0.7300372334422004,5.9375980227488717E-4,3.1082689154498226E-4,3.9597683030543562E-2,8.8828998016760294E-2,0,3.6353384337145127E-4,3.8170209383080952E-3,1.5360224419900871E-3,0.1041530186561196,1.085414422295201E-6,5.1629660347600916E-6,6.5979195735839324E-2,0.30518630773720934,0.7300372334422004,73.003723344220035,35,69.979193442852676,0.69979193442852672,285.98403340761007,null,4.4305099894314463E-2,null,0.14961173141690551,6.0101270393364103E-2,9.6295020135303E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR56, IF(MODE_ILIM=4,#REF!,#REF!))","v":73.003723344220035},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ56, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.14961173141690551},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA56, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.0101270393364103E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB56, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.6295020135303E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S56, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":285.98403340761007},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P56, IF(MODE_ILIM=4,#REF!,#REF!))","v":76.704133365995347}]
["ThetaCA",20,"°C/W",{"$f":"ThetaCa","v":40},"Inductor Core-to-Ambient thermal resistance",null,null,51,3.5700000000000003E-2,7.3615061321327738E-2,7.3615061321327738E-2,0,66.804399696330734,7.8592686316061515,9,70.733417684455375,1.8170476072160916E-6,0.4398706799555146,291703.71407576231,3.4281359878067117E-6,0,6.600000000000001E-4,4.1718651070798675E-2,1.4271655946769819E-3,9.6771766312983953E-2,9.82213604110595E-2,2.0882942594374568E-2,4.7970702053993799E-6,4.7970702053993799E-6,2.2622821019556861E-2,1.0235840617658075E-6,1.0235840617658075E-6,2.8126677318835832E-2,5.4349255419756698E-4,1.1711904120141857E-3,35,91.485596098664772,4.0589624183547557E-2,4.1165228130371573E-2,8.2926042725933319E-2,8.3477926393464741E-2,3.0811294522774226E-2,2.8859810453141764E-4,3.2087408548333858E-3,0,3.4109640354368348E-4,3.5498372583770694E-3,3.8386402550130636E-3,2.8325298457411139E-2,6.0736789832083166E-2,4.3799312668475719E-3,0.15243328774740855,0.25066046881273518,0.67830000000000001,0.73017100594916207,5.9408735469310234E-4,3.1088835998059307E-4,3.9604938936251138E-2,8.9267568976231643E-2,0,3.6718075202879654E-4,3.8213006662317561E-3,1.5363039037613532E-3,0.10417210372435312,1.1018596550981407E-6,5.1639121000814067E-6,6.5381457953435057E-2,0.30506209639872173,0.73017100594916207,73.017100594916201,35.700000000000003,70.206518151218702,0.702065181512187,291.70371407576232,null,4.4313218390211045E-2,null,0.15243328774740855,6.0736789832083166E-2,9.82213604110595E-2,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR57, IF(MODE_ILIM=4,#REF!,#REF!))","v":73.017100594916201},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ57, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15243328774740855},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA57, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.0736789832083166E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB57, IF(MODE_ILIM=4,#REF!,#REF!))","v":9.82213604110595E-2},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S57, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":291.70371407576232},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P57, IF(MODE_ILIM=4,#REF!,#REF!))","v":70.733417684455375}]
[null,null,null,null,null,null,null,52,3.6400000000000002E-2,7.3615061321327738E-2,7.3615061321327738E-2,0,63.825676292075414,2.9883363489483847,22,65.743399676864456,1.8170476072160916E-6,0.44849559524875993,297423.39474391448,3.3622102957335059E-6,0,6.6E-4,4.2125671939177295E-2,1.4551492337882953E-3,9.8669251926964019E-2,0.10014771794075665,2.1086683444351686E-2,4.8911304055052498E-6,4.8911304055052498E-6,2.3008275859499275E-2,1.0587615160536342E-6,1.0587615160536342E-6,2.8401090425038373E-2,5.5414927094653884E-4,1.1941549298968167E-3,35,91.485596098664772,4.1785485528997655E-2,4.1972389466261209E-2,8.4952029925155687E-2,8.5514943614776989E-2,3.111189963656965E-2,2.9425689089477875E-4,3.2716573421830595E-3,0,3.5117631804838431E-4,3.622833660231444E-3,3.9173037418111963E-3,2.8325298457411135E-2,6.1372309270802221E-2,4.4658122720798764E-3,0.15527036889947027,0.25542403673214847,0.69159999999999999,0.73028769405523408,5.9440274775255189E-4,3.1094256339666562E-4,3.9611268173207835E-2,8.9704196123992455E-2,0,3.7082091312082424E-4,3.8254928277560792E-3,1.5365494193890904E-3,0.10418875139372109,1.1179880076825219E-6,5.1647373411796859E-6,6.4805439873075216E-2,0.3049541467607606,0.73028769405523408,73.028769405523406,36.4,70.411746141009829,0.70411746141009823,297.42339474391446,null,4.4320300053938826E-2,null,0.15527036889947027,6.1372309270802221E-2,0.10014771794075665,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR58, IF(MODE_ILIM=4,#REF!,#REF!))","v":73.028769405523406},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ58, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15527036889947027},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA58, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.1372309270802221E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB58, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10014771794075665},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S58, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":297.42339474391446},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P58, IF(MODE_ILIM=4,#REF!,#REF!))","v":65.743399676864456}]
[null,null,null,null,null,null,null,53,3.7100000000000008E-2,7.3613258308004054E-2,7.3818357951272118E-2,3.8213787936667437E-4,65.265004239363137,65.265004239363137,1,65.265004239363137,1.8169717345601083E-6,0.45352725487673134,300760.17954983236,3.3249082424966169E-6,0,6.600000000000001E-4,4.2732147786653428E-2,1.4973498926575193E-3,9.9776219524199128E-2,0.10129783794594061,2.1204397054865508E-2,4.9458909990642792E-6,4.9458909990642792E-6,2.3346256591962142E-2,1.0900953937154716E-6,1.0900953937154716E-6,2.8777722295141077E-2,5.689440654409305E-4,1.207552120892577E-3,35,91.023494533313368,4.2525710877153337E-2,4.2443276538072339E-2,8.6176539536118257E-2,8.6754612460186231E-2,3.1524480025815503E-2,3.0211302363300437E-4,3.3083619750481565E-3,1.4131600985314292E-5,3.6034111923458415E-4,3.6828346952680548E-3,3.9851703934997611E-3,2.8325298457411139E-2,6.174306276737257E-2,4.5159140959407339E-3,0.15699875971699931,0.2583026336493327,0.70490000000000019,0.73182939432932315,6.0015712568995034E-4,3.1388587164284663E-4,3.9382864083522047E-2,8.9468754056056712E-2,1.4671472535091816E-5,3.7410728194268132E-4,3.8235305496567415E-3,1.5545533622395079E-3,0.10358798454087702,1.1317404621137444E-6,5.134839571945044E-6,6.4101841720930114E-2,0.30322861664512679,0.73182939432932315,73.182939432932315,37.100000000000009,70.596901007914624,0.70596901007914625,300.76017954983234,null,4.4064743030514171E-2,null,0.15699875971699931,6.174306276737257E-2,0.10129783794594061,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR59, IF(MODE_ILIM=4,#REF!,#REF!))","v":73.182939432932315},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ59, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15699875971699931},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA59, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.174306276737257E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB59, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10129783794594061},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S59, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":300.76017954983234},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P59, IF(MODE_ILIM=4,#REF!,#REF!))","v":65.265004239363137}]
[null,null,null,null,null,null,null,54,3.7800000000000007E-2,7.3609873792637628E-2,7.4518366133375175E-2,1.0838301568302164E-3,65.262003551514027,65.262003551514027,1,65.262003551514027,1.8168131252591671E-6,0.45354889068357096,300774.52750594704,3.3247496331956753E-6,0,6.6E-4,4.3341278874306298E-2,1.540342492657519E-3,9.9780979412363718E-2,0.10134629918679901,2.1204397054865508E-2,4.9458909990642792E-6,4.9458909990642792E-6,2.3623178525228626E-2,1.1161091272696459E-6,1.1161091272696459E-6,2.9188634373790257E-2,5.8530777072887858E-4,1.2076097279363775E-3,35,90.168551135257445,4.2682488087704758E-2,4.2445301321639241E-2,8.6335399137280375E-2,8.6930117325504069E-2,3.1974612579145807E-2,3.1080225827428667E-4,3.308519802565418E-3,4.0660588468373382E-5,3.6715873738745396E-4,3.7163391284212454E-3,4.0273728916787868E-3,2.8325298457411135E-2,6.1744656983124424E-2,4.5161295305017959E-3,0.15721827673080907,0.25857063791773438,0.71820000000000017,0.73528008738166872,6.0886165609104113E-4,3.184307054116601E-4,3.8837662173266597E-2,8.8388610166793016E-2,4.1627570373176891E-5,3.7589043234362329E-4,3.8047203551733323E-3,1.5769746067932579E-3,0.10215395051705829,1.1426522091705696E-6,5.0635131801339335E-6,6.3213055948068614E-2,0.29932599029676188,0.73528008738166872,73.528008738166875,37.800000000000004,70.763841860106652,0.70763841860106647,300.77452750594705,null,4.3454726907151422E-2,null,0.15721827673080907,6.1744656983124424E-2,0.10134629918679901,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR60, IF(MODE_ILIM=4,#REF!,#REF!))","v":73.528008738166875},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ60, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15721827673080907},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA60, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.1744656983124424E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB60, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10134629918679901},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S60, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":300.77452750594705},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P60, IF(MODE_ILIM=4,#REF!,#REF!))","v":65.262003551514027}]
[null,null,null,null,null,null,null,55,3.8500000000000006E-2,7.3606489277271189E-2,7.5218374315478204E-2,1.7855224342937445E-3,65.259002863664918,65.259002863664918,1,65.259002863664918,1.8166545290645638E-6,0.45357052676672482,300788.87564530171,3.3245910370010718E-6,0,6.6E-4,4.3953116550028502E-2,1.5841386926575191E-3,9.9785739361317599E-2,0.10139557799931481,2.1204397054865508E-2,4.9458909990642792E-6,4.9458909990642792E-6,2.3901977479374031E-2,1.1426090548490068E-6,1.1426090548490068E-6,2.9601388837313555E-2,6.0197840589421025E-4,1.2076673357158865E-3,35,89.329518504305,4.2839280088400614E-2,4.2447326131064972E-2,8.6494273555181467E-2,8.7105949980949615E-2,3.2426763368129663E-2,3.1965447468993341E-4,3.3086776320983193E-3,6.7192106971824414E-5,3.7397818366708313E-4,3.7498479227372266E-3,4.0697430010203876E-3,2.8325298457411135E-2,6.1746251219236256E-2,4.5163449678142058E-3,0.15743828916902045,0.25883995566838913,0.73150000000000015,0.73863524925267132,6.1764288340292455E-4,3.2301542157537298E-4,3.8307348413540589E-2,8.733796214129895E-2,6.784751699377398E-5,3.7762606822692708E-4,3.7864249556672897E-3,1.5995908108023065E-3,0.1007590765071892,1.1537543732423173E-6,4.9941345603149507E-6,6.2348540888227777E-2,0.29553122349585859,0.73863524925267132,73.863524925267129,38.500000000000007,70.914272258910415,0.70914272258910416,300.78887564530169,null,4.286136885431114E-2,null,0.15743828916902045,6.1746251219236256E-2,0.10139557799931481,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR61, IF(MODE_ILIM=4,#REF!,#REF!))","v":73.863524925267129},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ61, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15743828916902045},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA61, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.1746251219236256E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB61, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10139557799931481},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S61, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":300.78887564530169},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P61, IF(MODE_ILIM=4,#REF!,#REF!))","v":65.259002863664918}]
[null,null,null,null,null,null,null,56,3.9200000000000006E-2,7.3603104761904764E-2,7.591838249758126E-2,2.4872147117572865E-3,65.256002175815809,65.256002175815809,1,65.256002175815809,1.8164959459746756E-6,0.45359216312619788,300803.22396789963,3.324432453911184E-6,0,6.6E-4,4.456754934322045E-2,1.6287384926575192E-3,9.9790499371061825E-2,0.10144567441969389,2.1204397054865508E-2,4.9458909990642792E-6,4.9458909990642792E-6,2.418258865359469E-2,1.1695951879779334E-6,1.1695951879779334E-6,3.0015910741200101E-2,6.1895601466747615E-4,1.207724944231117E-3,35,88.505956578686565,4.299608687952422E-2,4.244935096634999E-2,8.665316279010532E-2,8.7282110504228294E-2,3.2880850295000208E-2,3.2866969610115346E-4,3.3088354636468965E-3,9.3726156544153674E-5,3.807994582546408E-4,3.7833610784456908E-3,4.1122807496496308E-3,2.8325298457411135E-2,6.1747845475708434E-2,4.5165604078780137E-3,0.15765879713746436,0.25911058704334528,0.74480000000000013,0.74189874039832415,6.2649774017755028E-4,3.2763841267244097E-4,3.7791321175236529E-2,8.6315618052510826E-2,9.3361059992593646E-5,3.7931610959114154E-4,3.7686235480275283E-3,1.6223939797809861E-3,9.9401780057882014E-2,1.1650392007743956E-6,4.9266250031595028E-6,6.1507315763612298E-2,0.29183995756368786,0.74189874039832415,74.189874039832418,39.200000000000003,71.049749591014816,0.71049749591014821,300.80322396789961,null,4.2283995720544358E-2,null,0.15765879713746436,6.1747845475708434E-2,0.10144567441969389,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR62, IF(MODE_ILIM=4,#REF!,#REF!))","v":74.189874039832418},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ62, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15765879713746436},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA62, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.1747845475708434E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB62, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10144567441969389},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S62, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":300.80322396789961},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P62, IF(MODE_ILIM=4,#REF!,#REF!))","v":65.256002175815809}]
[null,1500,null,null,null,"Eff (%)","Iout (mA)",57,3.9899999999999998E-2,7.3599720246538325E-2,7.6618390679684303E-2,3.1889069892208216E-3,65.253001487966685,65.253001487966685,1,65.253001487966685,1.8163373759878766E-6,0.45361379976199578,300817.57247374457,3.3242738839243847E-6,0,6.5999999999999989E-4,4.5184471386311348E-2,1.6741418926575187E-3,9.9795259441597658E-2,0.10149658848477425,2.1204397054865508E-2,4.9458909990642792E-6,4.9458909990642792E-6,2.4464949807531652E-2,1.197067538170086E-6,1.197067538170086E-6,3.0432128907462025E-2,6.3624064078034507E-4,1.2077825534820845E-3,35,87.697441376753986,4.3152908461358948E-2,4.2451375827494829E-2,8.6812066842335861E-2,8.7458598973165144E-2,3.3336795388018252E-2,3.3784794572974891E-4,3.3089932972111906E-3,1.202627372338486E-4,3.8762256133130182E-4,3.8168785957763411E-3,4.1549861657234283E-3,2.8325298457411129E-2,6.1749439752541366E-2,4.5167758506932752E-3,0.15787980074212321,0.25938253218543467,0.7581,0.7450742160375855,6.3542332214844722E-4,3.3229815672694774E-4,3.7289010814102935E-2,8.5320449340661991E-2,1.1819636547031248E-4,3.8096237436011158E-4,3.7512964351123826E-3,1.6453765442652425E-3,9.8080562844896219E-2,1.1764993504103934E-6,4.8609099838216175E-6,6.0688451938246762E-2,0.28824806554532556,0.7450742160375855,74.507421603758544,39.9,71.171694607053283,0.71171694607053282,300.81757247374458,null,4.172197014165363E-2,null,0.15787980074212321,6.1749439752541366E-2,0.10149658848477425,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR63, IF(MODE_ILIM=4,#REF!,#REF!))","v":74.507421603758544},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ63, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15787980074212321},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA63, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.1749439752541366E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB63, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10149658848477425},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S63, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":300.81757247374458},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P63, IF(MODE_ILIM=4,#REF!,#REF!))","v":65.253001487966685}]
[null,null,null,null,null,{"$f":"BR56","v":73.003723344220035},{"$f":"I56*1000","v":35},58,4.0600000000000004E-2,7.35963357311719E-2,7.7318398861787346E-2,3.8905992666843567E-3,65.25000080011759,65.25000080011759,1,65.25000080011759,1.8161788191025441E-6,0.45363543667412382,300831.92116283998,3.3241153270390515E-6,0,6.6E-4,4.5803782097774304E-2,1.7203488926575195E-3,9.9800019572926266E-2,0.10154832023202576,2.1204397054865508E-2,4.9458909990642792E-6,4.9458909990642792E-6,2.4749001160939792E-2,1.2250261169283983E-6,1.2250261169283983E-6,3.084997571158745E-2,6.5383232796560305E-4,1.2078401634688027E-3,35,86.903564269157584,4.3309744834188139E-2,4.2453400714499975E-2,8.6970985712156917E-2,8.7635415465704775E-2,3.3794524568090532E-2,3.4718924679811544E-4,3.3091511327912404E-3,1.4680184908939879E-4,3.9444749307824509E-4,3.8504004749588842E-3,4.1978592774305481E-3,2.8325298457411135E-2,6.1751034049735455E-2,4.5169912962600431E-3,0.15810130008913081,0.25965579123827254,0.77140000000000009,0.74816513961244302,6.4441687752890022E-4,3.3699321164218913E-4,3.6799877573080779E-2,8.4351386657463917E-2,1.423801217517952E-4,3.8256658507734425E-4,3.7344249532167881E-3,1.668531331938326E-3,9.6794005155694737E-2,1.1881278659588073E-6,4.7969188875069376E-6,5.9891069498357589E-2,0.28475163701250583,0.74816513961244302,74.816513961244297,40.6,71.281400919850697,0.71281400919850701,300.83192116283999,null,4.1174688193656807E-2,null,0.15810130008913081,6.1751034049735455E-2,0.10154832023202576,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR64, IF(MODE_ILIM=4,#REF!,#REF!))","v":74.816513961244297},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ64, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15810130008913081},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA64, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.1751034049735455E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB64, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10154832023202576},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S64, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":300.83192116283999},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P64, IF(MODE_ILIM=4,#REF!,#REF!))","v":65.25000080011759}]
[null,null,null,null,null,{"$f":"BR81","v":79.041056223318691},{"$f":"I81*1000","v":52.500000000000007},59,4.1300000000000003E-2,7.3592951215805474E-2,7.8018407043890403E-2,4.5922915441478987E-3,65.247000112268466,65.247000112268466,1,65.247000112268466,1.816020275317054E-6,0.45365707386258686,300846.27003518917,3.3239567832535626E-6,0,6.600000000000001E-4,4.6425385883807034E-2,1.7673594926575192E-3,9.9804779765048701E-2,0.10160086969955034,2.1204397054865508E-2,4.9458909990642792E-6,4.9458909990642792E-6,2.5034685296055525E-2,1.2534709357450774E-6,1.2534709357450774E-6,3.1269386882035052E-2,6.7173111995715105E-4,1.2078977741912845E-3,35,86.123931290200233,4.3466595998295103E-2,4.2455425627365893E-2,8.712991939985229E-2,8.781256005991131E-2,3.4253967429126543E-2,3.5669362252924126E-4,3.3093089703870814E-3,1.733434921592935E-4,4.0127425367665403E-4,3.883926716223029E-3,4.2409001129916253E-3,2.8325298457411139E-2,6.1752628367291049E-2,4.5172067445783661E-3,0.15832329528477235,0.25993036434625749,0.78470000000000006,0.75117479520239194,6.5347579714114903E-4,3.4172221002975978E-4,3.6323409647588054E-2,8.3407416033114509E-2,1.659376350483302E-4,3.8413037508035327E-4,3.7179914051738653E-3,1.6918515419217729E-3,9.5540760800599311E-2,1.1999181514597413E-6,4.7345847563597083E-6,5.9114334098393354E-2,0.28134696404699827,0.75117479520239194,75.1174795202392,41.300000000000004,71.3800443047935,0.713800443047935,300.84627003518915,null,4.064157722807054E-2,null,0.15832329528477235,6.1752628367291049E-2,0.10160086969955034,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR65, IF(MODE_ILIM=4,#REF!,#REF!))","v":75.1174795202392},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ65, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15832329528477235},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA65, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.1752628367291049E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB65, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10160086969955034},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S65, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":300.84627003518915},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P65, IF(MODE_ILIM=4,#REF!,#REF!))","v":65.247000112268466}]
[null,null,null,null,null,{"$f":"BR106","v":83.004583597587057},{"$f":"I106*1000","v":70},60,4.2000000000000003E-2,7.3589566700439049E-2,7.8718415225993446E-2,5.2939838216114407E-3,65.243999424419371,65.243999424419371,1,65.243999424419371,1.8158617446297823E-6,0.45367871132739085,300860.61909079604,3.3237982525662897E-6,0,6.6E-4,4.7049191857675823E-2,1.8151736926575188E-3,9.9809540017966283E-2,0.10165423692608226,2.1204397054865508E-2,4.9458909990642792E-6,4.9458909990642792E-6,2.5321947062791273E-2,1.2824020061016074E-6,1.2824020061016074E-6,3.1690301311597065E-2,6.8993706049000998E-4,1.2079553856495461E-3,35,85.358162485929839,4.3623461953963279E-2,4.2457450566093131E-2,8.7288867905705947E-2,8.7990032833968806E-2,3.4715057031396615E-2,3.6636109614670832E-4,3.3094668099987569E-3,1.9988766649202446E-4,4.081028433077172E-4,3.9174573197984985E-3,4.2841087006591921E-3,2.8325298457411135E-2,6.1754222705208577E-2,4.5174221956483032E-3,0.15854578643548486,0.26020625165457228,0.79800000000000004,0.75410629898687209,6.6259760530288302E-4,3.464838544351926E-4,3.5859121399173598E-2,8.2487575337250457E-2,1.8889291778373778E-4,3.8565529420150625E-4,3.7019789985868129E-3,1.7153307210379641E-3,9.4319552414198801E-2,1.2118639481636881E-6,4.6738440557604588E-6,5.8357454048917165E-2,0.27803052829889208,0.75410629898687209,75.410629898687205,42,71.468691685531624,0.71468691685531627,300.86061909079604,null,4.012209387320121E-2,null,0.15854578643548486,6.1754222705208577E-2,0.10165423692608226,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR66, IF(MODE_ILIM=4,#REF!,#REF!))","v":75.410629898687205},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ66, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15854578643548486},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA66, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.1754222705208577E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB66, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10165423692608226},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S66, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":300.86061909079604},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P66, IF(MODE_ILIM=4,#REF!,#REF!))","v":65.243999424419371}]
[null,null,null,null,null,null,null,61,4.2700000000000002E-2,7.358618218507261E-2,7.9418423408096489E-2,5.9956760990749758E-3,65.240998736570262,65.240998736570262,1,65.240998736570262,1.8157032270391067E-6,0.45370034906854056,300874.96832966374,3.3236397349756144E-6,0,6.5999999999999989E-4,4.7675113575747143E-2,1.863791492657519E-3,9.9814300331680067E-2,0.1017084219509878,2.1204397054865508E-2,4.9458909990642792E-6,4.9458909990642792E-6,2.5610733486848263E-2,1.3118193394687421E-6,1.3118193394687421E-6,3.211266087997549E-2,7.0845019330031587E-4,1.2080129978435999E-3,35,84.605891296703703,4.3780342701475974E-2,4.2459475530682141E-2,8.7447831230001716E-2,8.8167833866180989E-2,3.5177729707173526E-2,3.761916908746915E-4,3.3096246516263017E-3,2.2643437213608407E-4,4.1493326215262706E-4,3.9509922859150125E-3,4.3274850687176764E-3,2.8325298457411129E-2,6.17558170634884E-2,4.5176376494699012E-3,0.15876877364785699,0.26048345330918332,0.81130000000000002,0.75696260983976926,6.717799514036443E-4,3.5127691292511005E-4,3.5406551704432833E-2,8.1590951007875973E-2,2.1126877023241677E-4,3.8714281403720167E-4,3.6863717887378575E-3,1.7389627418700785E-3,9.3129167112534314E-2,1.2239593132534714E-6,4.6146364583196361E-6,5.7619677625003744E-2,0.27479898902482475,0.75696260983976926,75.696260983976927,42.7,71.54830972155635,0.71548309721556347,300.87496832966372,null,3.9615722186777981E-2,null,0.15876877364785699,6.17558170634884E-2,0.1017084219509878,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR67, IF(MODE_ILIM=4,#REF!,#REF!))","v":75.696260983976927},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ67, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15876877364785699},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA67, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.17558170634884E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB67, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.1017084219509878},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S67, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":300.87496832966372},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P67, IF(MODE_ILIM=4,#REF!,#REF!))","v":65.240998736570262}]
[null,null,null,null,null,null,null,62,4.3400000000000001E-2,7.3582797669706185E-2,8.0118431590199546E-2,6.6973683765385109E-3,65.237998048721138,65.237998048721138,1,65.237998048721138,1.8155447225434043E-6,0.4537219870860415,300889.31775179593,3.3234812304799123E-6,0,6.600000000000001E-4,4.83030687892642E-2,1.9132128926575189E-3,9.9819060706191232E-2,0.10176342481426565,2.1204397054865508E-2,4.9458909990642792E-6,4.9458909990642792E-6,2.5900993680807997E-2,1.3417229473065117E-6,1.3417229473065117E-6,3.2536410286938593E-2,7.2727056212532233E-4,1.2080706107734608E-3,35,83.866763972117113,4.3937238241116575E-2,4.2461500521133434E-2,8.7606809373023467E-2,8.8345963234971403E-2,3.56419248779642E-2,3.8618542993795876E-4,3.3097824952697556E-3,2.529836091399662E-4,4.2176551039258144E-4,3.9845316148023032E-3,4.3710292454834324E-3,2.8325298457411139E-2,6.1757411442130941E-2,4.5178531060432164E-3,0.15899225702862899,0.26076196945684099,0.8246,0.75974653913169921,6.8102060211105281E-4,3.5610021500435312E-4,3.4965262427386061E-2,8.0716675024890966E-2,2.330868560527963E-4,3.8859433282303961E-4,3.6711546257662997E-3,1.762741782462645E-3,9.1968452475025192E-2,1.236198600157295E-6,4.5569046440234152E-6,5.6900290575905142E-2,0.27164917202067168,0.75974653913169921,75.974653913169917,43.4,71.619772941093288,0.71619772941093285,300.88931775179594,null,3.9121971946725648E-2,null,0.15899225702862899,6.1757411442130941E-2,0.10176342481426565,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR68, IF(MODE_ILIM=4,#REF!,#REF!))","v":75.974653913169917},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ68, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15899225702862899},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA68, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.1757411442130941E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB68, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10176342481426565},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S68, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":300.88931775179594},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P68, IF(MODE_ILIM=4,#REF!,#REF!))","v":65.237998048721138}]
[null,null,null,null,null,null,null,63,4.4100000000000007E-2,7.3579413154339759E-2,8.0818439772302603E-2,7.3990606540020598E-3,65.234997360872043,65.234997360872043,1,65.234997360872043,1.8153862311410525E-6,0.45374362537989882,300903.66735719604,3.3233227390775607E-6,0,6.5999999999999989E-4,4.8932979210961493E-2,1.9634378926575193E-3,9.9823821141500971E-2,0.10181924555654689,2.1204397054865508E-2,4.9458909990642792E-6,4.9458909990642792E-6,2.6192678758235249E-2,1.3721128410642162E-6,1.3721128410642162E-6,3.2961496895448306E-2,7.4639821070340145E-4,1.2081282244391421E-3,35,83.140439016333659,4.4094148573168471E-2,4.2463525537447498E-2,8.7765802335055113E-2,8.8524421018883664E-2,3.6107584882664037E-2,3.9634233656187174E-4,3.3099403409291572E-3,2.7953537755216615E-4,4.2859958820878229E-4,4.0180753066901059E-3,4.4147412593047502E-3,2.8325298457411129E-2,6.1759005841136541E-2,4.5180685653682991E-3,0.15921623668469326,0.26104180024508028,0.83790000000000009,0.76246075980833194,6.9031743415289937E-4,3.6095264783465506E-4,3.4534837004680234E-2,7.9863922107141647E-2,2.5436777224219302E-4,3.900111799489274E-4,3.6563131057477435E-3,1.7866623075213294E-3,9.0836312823152937E-2,1.2485764403157788E-6,4.500594115139921E-6,5.6198613818642044E-2,0.26857805937162005,0.76246075980833194,76.246075980833197,44.100000000000009,71.68387138413388,0.71683871384133879,300.90366735719601,null,3.8640377068173672E-2,null,0.15921623668469326,6.1759005841136541E-2,0.10181924555654689,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR69, IF(MODE_ILIM=4,#REF!,#REF!))","v":76.246075980833197},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ69, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15921623668469326},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA69, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.1759005841136541E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB69, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10181924555654689},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S69, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":300.90366735719601},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P69, IF(MODE_ILIM=4,#REF!,#REF!))","v":65.234997360872043}]
[null,null,null,null,null,null,null,64,{"$f":"IF(PLOT_TYPE=1, H70/100*Iout, min_I*EXP(H70*rr/100))","v":4.4800000000000006E-2},{"$f":"IF(I70<Icrit, (Vin-(Rdcr+RdsonTop)*Iripple/2-Vout)/L*OnTime, (Vin-(Rdcr+RdsonTop)*I70-Vout)/L*OnTime)","v":7.3576028638973334E-2},{"$f":"IF(I70<Icrit, (Vin-(Rdcr+RdsonTop)*Iripple/2-Vout)/L*OnTime, I70+((Vin-(Rdcr+RdsonTop)*J70-Vout)/L*OnTime)/2)","v":8.1518447954405632E-2},{"$f":"IF(I70<Icrit, 0, I70-((Vin-(Rdcr+RdsonTop)*K70-Vout)/L*OnTime)/2)","v":8.1007529314655949E-3},65.231996673022934,{"$f":"IF(I70<Icrit, 1000*SQRT((J70*CoutEsr)^2+(((J70/2)-I70)*(OnTime+OffTime)/Cout)^2), 1000*J70*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":65.231996673022934},1,{"$f":"IF(I70<Icrit, 1000*((N70/1000)*O70), 1000*J70*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":65.231996673022934},{"$f":"IF(I70<Icrit, L*J70/(Vout+J70/2*(RdsonBot+Rdcr)), L*J70/(Vout+I70*(RdsonBot+Rdcr)))","v":1.8152277528304286E-6},0.45376526395011807,{"$f":"IF(I70<Icrit,I70/((OnTime+Q70)*J70/2),1/(OnTime+Q70))","v":300918.01714586775},3.3231642607669368E-6,0,{"$f":"S70*(T70*Iq_active+U70*Iq_sleep)","v":6.6E-4},4.9564770295648396E-2,{"$f":"W70^2*Rdcr","v":2.0144664926575193E-3},{"$f":"Core_Loss/1000*S70/$S$106","v":9.982858163761045E-2},{"$f":"(Y70+X70*(1+Ltc*(Ta-25)))/(1-X70*Ltc*ThetaCa)","v":0.10187588421909503},2.1204397054865508E-2,4.9458909990642792E-6,4.9458909990642792E-6,2.6485741750802712E-2,1.4029890321804277E-6,1.4029890321804277E-6,3.3387870584175021E-2,7.6583318277404075E-4,1.2081858388406589E-3,{"$f":"20*VIN_nom/24","v":35},{"$f":"IF(I70<Icrit, Csw*Vin/Iripple*1000000000, Csw*Vin/(I70+Iripple/2)*1000000000)","v":82.426586661990356},{"$f":"IF(I70<Icrit, Vin*(I70+Iripple/2)*AK70/1000000000/2*S70, Vin*(I70-Iripple/2)*AJ70/1000000000/2*S70 + Vin*(I70+Iripple/2)*AK70/1000000000/2*S70)","v":4.4251073697915075E-2},{"$f":"IF(I70<Icrit, Csw*(Vin)^2*S70/2, Csw*Vin^2*S70/2)","v":4.2465550579624853E-2},8.7924810116380592E-2,{"$f":"(AI70+AL70+AM70+AH70*(1+RdsonTopTc*(Ta-25)))/(1-AH70*RdsonTopTc*ThetaJA)","v":8.8703207296581404E-2},{"$f":"IF(I70<Icrit,Iripple*SQRT((OffTime)*S70/3), SQRT(OffTime*S70*(I70^2+Iripple^2/12)))","v":3.6574654815994652E-2},4.066624339723849E-4,{"$f":"QgBot*S70*Vdd","v":3.3100981886045452E-3},{"$f":"IF(I70<Icrit, Vin*Idss*R70, QrrBot*(I70-Iripple/2)/1*S70*Vin+Vin*Idss*R70)","v":3.060896774211797E-4},{"$f":"IF(I70<Icrit, dead1*S70*(I70+Iripple/2)*((I70+Iripple/2)*BDserR+VSD), dead1*S70*(I70+Iripple/2)*((I70+Iripple/2)*BDserR+VSD)+dead2*S70*(I70-Iripple/2)*((I70-Iripple/2)*BDserR+VSD))","v":4.354354957824365E-4},4.0516233618081614E-3,{"$f":"(AR70+AS70+AT70+AQ70*(1+RdsonBotTc*(Ta-25)))/(1-AQ70*RdsonBotTc*ThetaJA)","v":4.4586211385618689E-3},{"$f":"Vin*V70+Vout*Ifb/0.8","v":2.8325298457411135E-2},{"$f":"(Vin-Vdd)*(S70*QgBot+S70*QgTop)+AW70","v":6.1760600260505651E-2},{"$f":"AI70+AR70","v":4.5182840274452041E-3},0.15944071272309412,{"$f":"SUM(Z70,AC70,AF70,AZ70)","v":0.26132294582222038},{"$f":"Vout*I70","v":0.85120000000000018},0.7651078148063839,6.9966842762558118E-4,3.6583315272918881E-4,{"$f":"Vin*S70*(QgBot+QgTop)/($BB70+$BA70)","v":3.4114879134011719E-2},7.9031907113968722E-2,2.7513111398791082E-4,3.9139462014477715E-4,3.6418335253425005E-3,{"$f":"X70/($BB70+$BA70)","v":1.8107190509843451E-3},{"$f":"Y70/($BB70+$BA70)","v":8.9731705770644751E-2},1.2610877262792414E-6,4.4456530246295025E-6,5.5514001299866132E-2,0.26558277995005652,{"$f":"BC70","v":0.7651078148063839},76.510781480638386,{"$f":"I70*1000","v":44.800000000000004},71.741317737155555,0.71741317737155552,{"$f":"S70/1000","v":300.91801714586774},null,{"$f":"AM70/($BB70+$BA70)","v":3.8170494135957161E-2},null,0.15944071272309412,6.1760600260505651E-2,0.10187588421909503,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR70, IF(MODE_ILIM=4,#REF!,#REF!))","v":76.510781480638386},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ70, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15944071272309412},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA70, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.1760600260505651E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB70, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10187588421909503},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S70, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":300.91801714586774},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P70, IF(MODE_ILIM=4,#REF!,#REF!))","v":65.231996673022934}]
[null,null,null,null,null,null,null,65,4.5500000000000006E-2,7.3572644123606895E-2,8.2218456136508689E-2,8.8024452089291369E-3,{"$f":"IF(I71<Icrit, 1000*((((J71/2)-I71)*0.000002/Cout+Vout/306)), 1000*J71*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":65.22899598517381},65.22899598517381,{"$f":"ROUNDUP(M71/N71,0)","v":1},65.22899598517381,1.8150692876099102E-6,0.45378690279670447,300932.36711781455,{"$f":"IF(1/S71-OnTime-Q71>Tsleep, OnTime+Q71+Tsleep, 1/S71)","v":3.3230057955464177E-6},{"$f":"IF(1/S71-OnTime-Q71>Tsleep, 1/S71-OnTime-Q71-Tsleep, 0)","v":0},6.6E-4,{"$f":"IF(I71<Icrit,Iripple*SQRT((OnTime+OffTime)*S71/3), SQRT(I71^2+Iripple^2/12))","v":5.0198371033932855E-2},2.0662986926575188E-3,9.9833342194520849E-2,0.10193334084380617,{"$f":"Iripple/SQRT(12)*SQRT((OnTime+Q71)*S71)","v":2.1204397054865508E-2},{"$f":"RCoutEsr*AA71^2","v":4.9458909990642792E-6},4.9458909990642792E-6,{"$f":"SQRT($R71)*SQRT($I71^2*(1-R71)+(Iripple^2)/12)","v":2.6780137528427561E-2},{"$f":"RCinEsr*AD71^2","v":1.4343515320829886E-6},1.4343515320829886E-6,{"$f":"IF(I71<Icrit,Iripple*SQRT((OnTime)*S71/3), SQRT(OnTime*S71*(I71^2+Iripple^2/12)))","v":3.3815483608842872E-2},{"$f":"RdsonTop*AG71^2","v":7.8557552207784574E-4},{"$f":"QgTop*S71*Vdd","v":1.2082434539780254E-3},35,81.724888370974554,4.4408013615639758E-2,4.2467575647665984E-2,{"$f":"AI71+AL71+AM71","v":8.8083832717283761E-2},8.8882322146848228E-2,3.7043082376614918E-2,{"$f":"RdsonBot*AP71^2","v":4.1714574539604632E-4},3.3102560382959607E-3,3.3264650879550472E-4,4.4227323329475539E-4,{"$f":"AR71+AS71+AT71","v":4.0851757803862208E-3},4.5026689116670019E-3,2.8325298457411135E-2,6.176219470023863E-2,4.5184994922739859E-3,0.15966568525102784,0.26160540633736518,0.86450000000000016,0.76769012486297228,{"$f":"(AO71-AN71)/($BB71+$BA71)","v":7.0907165978497267E-4},{"$f":"(AV71-AU71)/($BB71+$BA71)","v":3.7074072189979877E-4},3.370501155708916E-2,{"$f":"AN71/($BB71+$BA71)","v":7.8219882634055202E-2},{"$f":"AS71/(BA71+BB71)","v":2.9539553484378574E-4},{"$f":"AT71/($BB71+$BA71)","v":3.9274585736448947E-4},{"$f":"AU71/($BB71+$BA71)","v":3.6277028397129988E-3},1.8349069998501407E-3,8.8653639022324496E-2,{"$f":"(AF71)/($BB71+$BA71)","v":1.2737275960233486E-6},{"$f":"(AC71)/($BB71+$BA71)","v":4.3920320169234308E-6},{"$f":"AX71/($BB71+$BA71)","v":5.4845838011841973E-2},{"$f":"SUM(BD71:BO71)","v":0.26266060059837998},0.76769012486297228,76.769012486297228,45.500000000000007,71.792753953912452,{"$f":"BT71/100","v":0.71792753953912447},300.93236711781452,null,3.7711901042896949E-2,null,{"$f":"AZ71","v":0.15966568525102784},{"$f":"AX71","v":6.176219470023863E-2},{"$f":"Z71","v":0.10193334084380617},null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR71, IF(MODE_ILIM=4,#REF!,#REF!))","v":76.769012486297228},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ71, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15966568525102784},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA71, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.176219470023863E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB71, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10193334084380617},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S71, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":300.93236711781452},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P71, IF(MODE_ILIM=4,#REF!,#REF!))","v":65.22899598517381}]
[null,null,null,null,null,null,null,66,4.6200000000000005E-2,7.356925960824047E-2,8.2918464318611732E-2,9.5041374863926789E-3,65.225995297324715,65.225995297324715,1,65.225995297324715,1.8149108354778767E-6,{"$f":"OnTime*S72","v":0.45380854191966313},300946.71727303974,3.3228473434143847E-6,0,6.6E-4,5.0833713758296172E-2,2.1189344926575192E-3,9.9838102812233265E-2,0.10199161547320887,2.1204397054865508E-2,4.9458909990642792E-6,{"$f":"AB72","v":4.9458909990642792E-6},2.7075822722393963E-2,1.4662003521890106E-6,{"$f":"AE72","v":1.4662003521890106E-6},3.4244290471875494E-2,8.0562527235653947E-4,1.2083010698512547E-3,35,81.035036360485137,4.4564968326625938E-2,4.2469600741571363E-2,8.8242870138048546E-2,8.9061765648587962E-2,3.7512817724324729E-2,4.2779229405999708E-4,3.310413890003438E-3,3.5920587172363975E-4,4.4911280092695474E-4,4.1187325626540327E-3,4.5468846070643434E-3,2.8325298457411135E-2,6.1763789160335855E-2,4.5187149598546923E-3,{"$f":"AO72+AV72+AX72+AY72","v":0.15989115437584286},0.261889181940403,0.87780000000000014,0.77020999576874305,7.185252992795699E-4,3.7567439543591258E-4,3.3304874929280748E-2,7.7427136746010594E-2,3.1517880262061081E-4,3.9406603839329927E-4,3.6139086234385355E-3,1.8592213791569735E-3,8.7601167400967767E-2,1.2864914183818948E-6,4.339684080043247E-6,5.4193538149742322E-2,0.25980891793982475,0.77020999576874305,{"$f":"100*BQ72","v":77.020999576874303},46.2,71.838757366287027,0.71838757366287032,300.94671727303972,null,3.7264195725069359E-2,null,0.15989115437584286,6.1763789160335855E-2,0.10199161547320887,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR72, IF(MODE_ILIM=4,#REF!,#REF!))","v":77.020999576874303},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ72, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.15989115437584286},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA72, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.1763789160335855E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB72, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10199161547320887},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S72, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":300.94671727303972},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P72, IF(MODE_ILIM=4,#REF!,#REF!))","v":65.225995297324715}]
[null,null,null,null,null,null,null,67,4.6900000000000004E-2,7.3565875092874045E-2,8.3618472500714774E-2,1.0205829763856221E-2,65.222994609475606,65.222994609475606,1,65.222994609475606,1.814752396432706E-6,0.45383018131899949,300961.06761154701,3.3226889043692136E-6,0,6.6E-4,5.147073396077026E-2,2.1723738926575191E-3,9.9842863490748932E-2,0.10205070815046458,2.1204397054865508E-2,4.9458909990642792E-6,4.9458909990642792E-6,2.7372755651421693E-2,1.4985355039048765E-6,1.4985355039048765E-6,3.4674247799839318E-2,8.2598247735296267E-4,1.2083586864603613E-3,35,80.356733152896098,4.4721937831157015E-2,4.2471625861341511E-2,8.8401922378958886E-2,8.9241537880824715E-2,3.7983813345810621E-2,4.386021031919718E-4,3.3105717437270175E-3,3.8576776625408494E-4,4.5595419886025547E-4,4.1522937088413576E-3,4.5912682532300887E-3,2.8325298457411135E-2,6.1765383640797741E-2,4.5189304301873788E-3,0.16011712020503993,0.26217427278200744,0.89110000000000011,{"$f":"BB73/(BB73+BA73)","v":0.77266962511044956},7.2802760078957652E-4,3.8063325849609607E-4,3.2914126768827184E-2,7.6652990936587603E-2,3.3449785134242994E-4,3.9535625620119955E-4,3.6004390341812698E-3,1.8836576380197654E-3,8.6573390083437049E-2,1.2993747795049706E-6,4.2885644081294389E-6,5.3556543398651416E-2,0.25702525076572119,0.77266962511044956,77.266962511044952,46.900000000000006,71.879846296152991,0.71879846296152994,300.96106761154704,null,3.6826994986100342E-2,null,0.16011712020503993,6.1765383640797741E-2,0.10205070815046458,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR73, IF(MODE_ILIM=4,#REF!,#REF!))","v":77.266962511044952},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ73, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.16011712020503993},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA73, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.1765383640797741E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB73, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10205070815046458},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S73, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":300.96106761154704},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P73, IF(MODE_ILIM=4,#REF!,#REF!))","v":65.222994609475606}]
[null,null,null,null,null,null,null,68,4.760000000000001E-2,7.3562490577507619E-2,8.4318480682817831E-2,1.0907522041319756E-2,65.219993921626497,65.219993921626497,1,65.219993921626497,1.8145939704727768E-6,0.45385182099471871,300975.41813333979,3.3225304784092848E-6,0,6.5999999999999989E-4,5.2109370121508757E-2,2.2266168926575194E-3,9.984762423006896E-2,0.10211061891936737,2.1204397054865508E-2,4.9458909990642792E-6,4.9458909990642792E-6,2.7670896250629795E-2,1.5313569986262362E-6,1.5313569986262362E-6,3.5105314228208249E-2,8.4664718081107224E-4,1.2084163038053593E-3,35,79.68969114803987,4.4878922129516406E-2,4.2473651006976906E-2,8.8560989440298665E-2,8.9421638922702829E-2,3.8456023928411548E-2,4.495751960202987E-4,3.3107295994667381E-3,4.1233219243534176E-4,4.6279742727588279E-4,4.1858592191779623E-3,4.6358198786724536E-3,2.8325298457411129E-2,6.176697814162465E-2,4.5191459032720973E-3,0.16034358284627204,0.26246067901363712,0.9044000000000002,0.77507110854442485,7.3757690003889887E-4,3.8561643869501963E-4,3.2532440479161921E-2,7.5896798163736595E-2,3.5336882958802898E-4,3.9661755306305422E-4,3.5872827788801008E-3,1.9082114366384408E-3,8.5569448029109582E-2,1.3123734702592878E-6,4.238630273534546E-6,5.2934321339748194E-2,0.25430723295240365,0.77507110854442485,77.507110854442487,47.600000000000009,71.916485184007442,0.71916485184007439,300.97541813333976,null,3.6399933403258082E-2,null,0.16034358284627204,6.176697814162465E-2,0.10211061891936737,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR74, IF(MODE_ILIM=4,#REF!,#REF!))","v":77.507110854442487},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ74, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.16034358284627204},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA74, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.176697814162465E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB74, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10211061891936737},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S74, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":300.97541813333976},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P74, IF(MODE_ILIM=4,#REF!,#REF!))","v":65.219993921626497}]
[null,null,null,null,null,null,null,69,4.8300000000000003E-2,7.355910606214118E-2,8.5018488864920874E-2,1.1609214318783291E-2,65.216993233777387,65.216993233777387,1,65.216993233777387,1.8144355575964675E-6,0.45387346094682646,300989.76883842173,3.3223720655329755E-6,0,6.6E-4,5.2749563547581972E-2,2.2816634926575187E-3,9.9852385030194571E-2,0.10217134782434432,2.1204397054865508E-2,4.9458909990642792E-6,4.9458909990642792E-6,2.7970206003335104E-2,1.5646648477380061E-6,1.5646648477380061E-6,3.5537450292999768E-2,8.6761942647594411E-4,1.2084739218862633E-3,35,79.033632216617988,4.5035921221987553E-2,4.247567617847807E-2,8.8720071322351879E-2,8.9602068853487135E-2,3.8929406241411862E-2,4.6071159577389857E-4,3.3108874572226393E-3,4.3889915031591193E-4,4.6964248635506667E-4,4.2194290938936179E-3,4.6805395119316855E-3,2.8325298457411135E-2,6.1768572662817017E-2,4.5193613791089026E-3,0.16057054240734475,0.26274840078753586,0.91770000000000007,0.7774164456385867,7.4717160915024471E-4,3.906231036701289E-4,3.2159504438472715E-2,7.5157941052876431E-2,3.7180714550767355E-4,3.9785092346412157E-4,3.5744290822696074E-3,1.9328786341997728E-3,8.4588521585168872E-2,1.325483474495065E-6,4.1898409077132292E-6,5.2326363966106543E-2,0.25165260686526836,0.7774164456385867,77.741644563858671,48.300000000000004,71.94908925319227,0.71949089253192267,300.98976883842175,null,3.5982662308780652E-2,null,0.16057054240734475,6.1768572662817017E-2,0.10217134782434432,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR75, IF(MODE_ILIM=4,#REF!,#REF!))","v":77.741644563858671},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ75, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.16057054240734475},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA75, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.1768572662817017E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB75, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10217134782434432},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S75, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":300.98976883842175},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P75, IF(MODE_ILIM=4,#REF!,#REF!))","v":65.216993233777387}]
[null,null,null,null,null,null,null,70,4.9000000000000002E-2,7.3555721546774755E-2,8.5718497047023917E-2,1.2310906596246833E-2,65.213992545928264,65.213992545928264,1,65.213992545928264,1.814277157802159E-6,0.4538951011753275,301004.11972679611,3.3222136657386674E-6,0,6.6E-4,5.3391258221364188E-2,2.3375136926575188E-3,9.9857145891126875E-2,0.1022328949104553,2.1204397054865508E-2,4.9458909990642792E-6,4.9458909990642792E-6,2.8270647875618032E-2,1.5984590626143727E-6,1.5984590626143727E-6,3.597061832885784E-2,8.8889925809376984E-4,1.2085315407030864E-3,35,78.388287313531734,4.5192935108853888E-2,4.2477701375845459E-2,8.8879168025402439E-2,8.9782827752562841E-2,3.9403919024396605E-2,4.7201132568228625E-4,3.3110453169947576E-3,4.6546863994429978E-4,4.7648937627904121E-4,4.2530033332180989E-3,4.7254271815800808E-3,2.8325298457411135E-2,6.1770167204375177E-2,4.5195768576978441E-3,0.16079799899621594,0.26303743825673293,0.93100000000000005,0.77970754531720421,7.5681021231606004E-4,3.9565245881377866E-4,3.1795021151170187E-2,7.4435830215812973E-2,3.8982750877884802E-4,3.9905731680800954E-4,3.5618676575396042E-3,1.9576552776018772E-3,8.3629828254728769E-2,1.3387009581107323E-6,4.1421573902114539E-6,5.1732186299416366E-2,0.24905921721133481,0.77970754531720421,77.970754531720416,49,71.978028730187987,0.71978028730187982,301.00411972679609,null,3.557484884047013E-2,null,0.16079799899621594,6.1770167204375177E-2,0.1022328949104553,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR76, IF(MODE_ILIM=4,#REF!,#REF!))","v":77.970754531720416},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ76, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.16079799899621594},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA76, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.1770167204375177E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB76, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.1022328949104553},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S76, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.00411972679609},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P76, IF(MODE_ILIM=4,#REF!,#REF!))","v":65.213992545928264}]
[null,null,null,null,null,null,null,71,4.9700000000000001E-2,7.3552337031408302E-2,8.6418505229126946E-2,1.3012598873710361E-2,65.21099185807914,65.21099185807914,1,65.21099185807914,1.814118771088229E-6,0.45391674168022766,301018.47079846676,3.3220552790247363E-6,0,6.5999999999999989E-4,5.4034400657917814E-2,2.3941674926575189E-3,9.9861906812867121E-2,0.1022952602233934,2.1204397054865508E-2,4.9458909990642792E-6,4.9458909990642792E-6,2.8572186253582245E-2,1.6327396546187884E-6,1.6327396546187884E-6,3.6404782373182877E-2,9.1048671941186033E-4,1.2085891602558441E-3,35,77.753396110003209,4.5349963790398864E-2,4.2479726599079622E-2,8.9038279549734339E-2,8.9963915699435751E-2,3.9879522882230858E-2,4.8347440897556989E-4,3.3112031787831345E-3,4.9204066136901057E-4,4.8333809722904641E-4,4.286581937381192E-3,4.770482916222004E-3,2.8325298457411129E-2,6.1771761766299574E-2,4.5197923390389791E-3,0.16102595272099632,0.26332779157504338,0.94430000000000003,0.78194623093958515,7.6649126176050867E-4,4.0070374515784063E-4,3.1438706456407485E-2,7.3729902682685491E-2,4.0744396974109771E-4,4.0023763994256444E-4,3.5495886789674129E-3,1.9825375909368038E-3,8.2692620615018031E-2,1.3520222588528662E-6,4.095542545119488E-6,5.1151325099709759E-2,0.246525005305131,0.78194623093958515,78.194623093958512,49.7,72.003632642003467,0.72003632642003468,301.01847079846675,null,3.5176175056120251E-2,null,0.16102595272099632,6.1771761766299574E-2,0.1022952602233934,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR77, IF(MODE_ILIM=4,#REF!,#REF!))","v":78.194623093958512},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ77, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.16102595272099632},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA77, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.1771761766299574E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB77, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.1022952602233934},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S77, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.01847079846675},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P77, IF(MODE_ILIM=4,#REF!,#REF!))","v":65.21099185807914}]
[null,null,null,null,null,null,null,72,5.04E-2,7.3548952516041877E-2,8.7118513411230003E-2,1.3714291151173903E-2,65.207991170230045,65.207991170230045,1,65.207991170230045,1.8139603974530592E-6,0.45393838246153173,301032.82205343683,3.321896905389567E-6,0,6.6E-4,5.4678939770814769E-2,2.451624892657519E-3,9.986666779541635E-2,0.1023584438094846,2.1204397054865508E-2,4.9458909990642792E-6,4.9458909990642792E-6,2.8874786883230572E-2,1.6675066351039686E-6,1.6675066351039686E-6,3.6839908075932369E-2,9.3238185417864202E-4,1.208646780544549E-3,35,77.128706643430405,4.5507007266905888E-2,4.2481751848181003E-2,8.9197405895631438E-2,9.0145332773732115E-2,4.035618018625111E-2,4.9510086888445066E-4,3.3113610425878053E-3,5.186152146385496E-4,4.9018864938632511E-4,4.3201649066126804E-3,4.8157067444938974E-3,2.8325298457411135E-2,6.1773356348590561E-2,4.5200078231323543E-3,0.16125440368994895,0.26361946089706773,0.95760000000000001,0.78413424504108253,7.762133739699507E-4,4.0577623739897521E-4,3.1090288789225227E-2,7.303962043817247E-2,4.2466995592879914E-4,4.0139275951780909E-4,3.5375827563697924E-3,2.00752196567244E-3,8.1776184373984331E-2,1.3654438767943257E-6,4.0499608444097268E-6,5.0583337660877012E-2,0.24404800371583801,0.78413424504108253,78.413424504108249,50.4,72.026192211331946,0.72026192211331941,301.0328220534368,null,3.4786337106825424E-2,null,0.16125440368994895,6.1773356348590561E-2,0.1023584438094846,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR78, IF(MODE_ILIM=4,#REF!,#REF!))","v":78.413424504108249},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ78, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.16125440368994895},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA78, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.1773356348590561E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB78, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.1023584438094846},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S78, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.0328220534368},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P78, IF(MODE_ILIM=4,#REF!,#REF!))","v":65.207991170230045}]
[null,null,null,null,null,null,null,73,5.1100000000000007E-2,7.3545568000675438E-2,8.781852159333306E-2,1.4415983428637452E-2,65.204990482380907,65.204990482380907,1,65.204990482380907,1.8138020368950282E-6,0.4539600235192453,301047.17349171004,3.3217385448315364E-6,0,6.5999999999999989E-4,5.5324826745868708E-2,2.509885892657519E-3,9.9871428838775811E-2,0.10242244571568826,2.1204397054865508E-2,4.9458909990642792E-6,4.9458909990642792E-6,2.91784168128764E-2,1.7027600154118964E-6,1.7027600154118964E-6,3.7275962614738763E-2,9.5458470614366109E-4,1.2087044015692159E-3,35,76.513974983986358,4.5664065538658434E-2,4.2483777123150115E-2,8.9356547063377756E-2,9.0327079055199114E-2,4.0833854981281337E-2,5.0689072864022364E-4,3.3115189084088107E-3,5.4519229980142523E-4,4.9704103293212636E-4,4.353752241142362E-3,4.8610986950643068E-3,2.8325298457411129E-2,6.1774950951248526E-2,4.5202233099780262E-3,0.16148335201148997,0.26391244637819272,0.9709000000000001,0.7862732537623266,7.859752261713984E-4,4.1086924205374994E-4,3.0749508490284669E-2,7.2364469053958685E-2,4.4151830620149592E-4,4.0252350418882546E-4,3.5258409112349635E-3,2.0326049514800583E-3,8.0879836554698631E-2,1.3789624654385631E-6,4.005378317631141E-6,5.0027800685391186E-2,0.24162633126644673,0.7862732537623266,78.627325376232662,51.100000000000009,72.045963869077937,0.72045963869077934,301.04717349171005,null,3.4405044464654165E-2,null,0.16148335201148997,6.1774950951248526E-2,0.10242244571568826,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR79, IF(MODE_ILIM=4,#REF!,#REF!))","v":78.627325376232662},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ79, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.16148335201148997},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA79, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.1774950951248526E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB79, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10242244571568826},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S79, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.04717349171005},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P79, IF(MODE_ILIM=4,#REF!,#REF!))","v":65.204990482380907}]
[null,null,null,null,null,null,null,74,5.1800000000000006E-2,7.3542183485309012E-2,8.8518529775436103E-2,1.5117675706100987E-2,65.201989794531812,65.201989794531812,1,65.201989794531812,1.8136436894125172E-6,0.45398166485337366,301061.52511328988,3.3215801973490256E-6,0,6.6E-4,5.5972014922284062E-2,2.5689504926575193E-3,9.9876189942946655E-2,0.102487265989597,2.1204397054865508E-2,4.9458909990642792E-6,4.9458909990642792E-6,2.9483044338007386E-2,1.7384998068738188E-6,1.7384998068738188E-6,3.7712914615012368E-2,9.7709531905757971E-4,1.208762023329859E-3,35,75.90896491703613,4.582113860593999E-2,4.2485802423987466E-2,8.9515703053257317E-2,9.0509154623704541E-2,4.1312512898109978E-2,5.1884401147477704E-4,3.3116767762461892E-3,5.7177191690614541E-4,5.038952480477029E-4,4.3873439412000373E-3,4.9066587966338894E-3,2.8325298457411135E-2,6.1776545574273888E-2,4.5204387995760485E-3,0.16171279779418837,0.26420674817459133,0.98420000000000007,0.78836485099034281,7.9577555303977584E-4,4.1598209573377384E-4,3.0416117160501296E-2,7.1703956410157463E-2,4.580013026541109E-4,4.0363066667533943E-4,3.5143545544071841E-3,2.0577832476585175E-3,8.0002923797860503E-2,1.3925748234025785E-6,3.9617624674779394E-6,4.9484309232229781E-2,0.23925818835820861,0.78836485099034281,78.836485099034277,51.800000000000004,72.063171902227168,0.72063171902227163,301.06152511328986,null,3.4032019200560884E-2,null,0.16171279779418837,6.1776545574273888E-2,0.102487265989597,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR80, IF(MODE_ILIM=4,#REF!,#REF!))","v":78.836485099034277},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ80, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.16171279779418837},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA80, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.1776545574273888E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB80, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.102487265989597},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S80, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.06152511328986},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P80, IF(MODE_ILIM=4,#REF!,#REF!))","v":65.201989794531812}]
[null,null,null,null,null,null,null,75,5.2500000000000005E-2,7.3538798969942587E-2,8.9218537957539146E-2,1.5819367983564522E-2,65.198989106682703,65.198989106682703,1,65.198989106682703,1.8134853550039069E-6,0.45400330646392201,301075.87691817986,3.3214218629404149E-6,0,6.6E-4,5.6620459680758413E-2,2.6288186926575188E-3,9.9880951107930036E-2,0.10255290467943678,2.1204397054865508E-2,4.9458909990642792E-6,4.9458909990642792E-6,2.9788638948517309E-2,1.7747260208102449E-6,1.7747260208102449E-6,3.8150734074718036E-2,9.999137366721784E-4,1.2088196458264922E-3,35,75.313447640502389,4.5978226469033989E-2,4.2487827750693534E-2,8.9674873865554006E-2,9.0691559559237009E-2,4.1792121071086721E-2,5.3096074062059266E-4,3.3118346460999787E-3,5.9835406600122017E-4,5.1075129491431242E-4,4.4209400070155114E-3,4.9523870779354358E-3,2.8325298457411135E-2,6.1778140217667019E-2,4.5206542919264707E-3,0.16194274114676593,0.26450236644322256,0.99750000000000005,0.79041056223318695,8.0561314361746379E-4,4.211141635318274E-4,3.008987705720818E-2,7.1057611499010187E-2,4.7413070047372212E-4,4.0471500568877187E-4,3.5031154652073377E-3,2.0830536951103166E-3,7.914482077353828E-2,1.4062778866350799E-6,3.919082190791434E-6,4.8952475732498085E-2,0.23694185259596162,0.79041056223318695,79.041056223318691,52.500000000000007,72.078010752951272,0.72078010752951271,301.07587691817986,null,3.3666995308764387E-2,null,0.16194274114676593,6.1778140217667019E-2,0.10255290467943678,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR81, IF(MODE_ILIM=4,#REF!,#REF!))","v":79.041056223318691},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ81, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.16194274114676593},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA81, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.1778140217667019E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB81, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10255290467943678},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S81, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.07587691817986},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P81, IF(MODE_ILIM=4,#REF!,#REF!))","v":65.198989106682703}]
[null,null,null,null,null,null,null,76,5.3200000000000004E-2,7.3535414454576162E-2,8.9918546139642203E-2,1.6521060261028064E-2,65.195988418833593,65.195988418833593,1,65.195988418833593,1.8133270336675778E-6,0.45402494835089569,301090.22890638345,3.3212635416040857E-6,0,6.6E-4,5.7270118338103589E-2,2.6894904926575186E-3,9.9885712333727131E-2,0.1026193618340671,2.1204397054865508E-2,4.9458909990642792E-6,4.9458909990642792E-6,3.0095171278221276E-2,1.8114386685309497E-6,1.8114386685309497E-6,3.8589392293533385E-2,1.0230400027403551E-3,1.2088772690591295E-3,35,74.727201476365764,4.6135329128223934E-2,4.2489853103268825E-2,8.9834059500551885E-2,9.0874293941906159E-2,4.2272648060519065E-2,5.4324093931074589E-4,3.3119925179702185E-3,6.2493874713516093E-4,5.1760917371321746E-4,4.4545404388185977E-3,4.9982835677338817E-3,2.8325298457411135E-2,6.1779734881428308E-2,4.5208697870293482E-3,0.1621731821780977,0.26479930134183238,1.0108000000000001,0.79241184824789113,8.1548683842961244E-4,4.2626483751073555E-4,2.9770560528764332E-2,7.0424983304752012E-2,4.8991775589542371E-4,4.0577724773659904E-4,3.4921157718828815E-3,2.1084132688285271E-3,7.8304928694030357E-2,1.4200687211301035E-6,3.8773077045915451E-6,4.8431929067725865E-2,0.23467567469198208,0.79241184824789113,79.241184824789116,53.2,72.090646982404948,0.72090646982404949,301.09022890638346,null,3.3309718074141903E-2,null,0.1621731821780977,6.1779734881428308E-2,0.1026193618340671,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR82, IF(MODE_ILIM=4,#REF!,#REF!))","v":79.241184824789116},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ82, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.1621731821780977},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA82, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.1779734881428308E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB82, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.1026193618340671},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S82, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.09022890638346},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P82, IF(MODE_ILIM=4,#REF!,#REF!))","v":65.195988418833593}]
[null,null,null,null,null,null,null,77,5.3900000000000003E-2,7.3532029939209723E-2,9.0618554321745232E-2,1.7222752538491599E-2,65.192987730984484,65.192987730984484,1,65.192987730984484,1.813168725401911E-6,0.45404659051430002,301104.58107790421,3.321105233338419E-6,0,6.6E-4,5.7920950047978231E-2,2.7509658926575193E-3,9.9890473620339107E-2,0.10268663750298102,2.1204397054865508E-2,4.9458909990642792E-6,4.9458909990642792E-6,3.0402613056569393E-2,1.8486377613349675E-6,1.8486377613349675E-6,3.9028861806115006E-2,1.0464741610161253E-3,1.2089348930277855E-3,35,74.150011595535091,4.6292446583793313E-2,4.2491878481713839E-2,8.9993259958534938E-2,9.1057357851942508E-2,4.2754063779568981E-2,5.5568463077890543E-4,3.3121503918569469E-3,6.515259603564798E-4,5.2446888462568471E-4,4.4881452368391115E-3,5.0443482948263263E-3,2.8325298457411135E-2,6.1781329565558152E-2,4.5210852848847323E-3,0.16240412099721172,0.2650975530289531,1.0241,0.79437010843985101,8.2539552678135783E-4,4.3143353528745293E-4,2.9457949484782225E-2,6.9805639754044621E-2,5.0537325239698757E-4,4.0681808881303866E-4,3.4813479332894111E-3,2.1338590708570308E-3,7.7482673920414857E-2,1.4339445160996598E-6,3.8364104767682594E-6,4.792231370623045E-2,0.23245807462789031,0.79437010843985101,79.437010843985107,53.900000000000006,72.101220909974245,0.7210122090997424,301.10458107790419,null,3.295994347947661E-2,null,0.16240412099721172,6.1781329565558152E-2,0.10268663750298102,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR83, IF(MODE_ILIM=4,#REF!,#REF!))","v":79.437010843985107},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ83, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.16240412099721172},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA83, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.1781329565558152E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB83, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10268663750298102},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S83, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.10458107790419},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P83, IF(MODE_ILIM=4,#REF!,#REF!))","v":65.192987730984484}]
[null,null,null,null,null,null,null,78,5.460000000000001E-2,7.3528645423843297E-2,9.1318562503848288E-2,1.7924444815955148E-2,65.189987043135375,65.189987043135375,1,65.189987043135375,1.8130104302052884E-6,0.45406823295414023,301118.93343274563,3.3209469381417963E-6,0,6.6E-4,5.8572915707350522E-2,2.813244892657519E-3,9.9895234967767116E-2,0.10275473173630521,2.1204397054865508E-2,4.9458909990642792E-6,4.9458909990642792E-6,3.071093706247496E-2,1.8863233105105962E-6,1.8863233105105962E-6,3.9469116319216332E-2,1.0702162552546225E-3,1.2089925177324737E-3,35,73.581669755370541,4.6449578836025587E-2,4.2493903886029055E-2,9.0152475239787117E-2,9.1240751369697615E-2,4.3236339425368836E-2,5.6829183825933386E-4,3.312308267760202E-3,6.7811570571369101E-4,5.3133042783298583E-4,4.5217544013068794E-3,5.0905812880420514E-3,2.8325298457411135E-2,6.1782924270056938E-2,4.5213007854926759E-3,0.16263555771328927,0.26539712166390406,1.0374000000000001,0.79628668405028047,8.3533814422354221E-4,4.3661969870541207E-4,2.9151834899383732E-2,6.9199166731844119E-2,5.2050752526043066E-4,4.0783819598433108E-4,3.4708047217143008E-3,2.1593883236896497E-3,7.667750665597349E-2,1.4479025775720359E-6,3.7963631610941035E-6,4.7423288893322951E-2,0.23028753805584065,0.79628668405028047,79.628668405028051,54.600000000000009,72.109847935853821,0.72109847935853821,301.11893343274562,null,3.261743764966011E-2,null,0.16263555771328927,6.1782924270056938E-2,0.10275473173630521,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR84, IF(MODE_ILIM=4,#REF!,#REF!))","v":79.628668405028051},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ84, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.16263555771328927},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA84, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.1782924270056938E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB84, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10275473173630521},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S84, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.11893343274562},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P84, IF(MODE_ILIM=4,#REF!,#REF!))","v":65.189987043135375}]
[null,null,null,null,null,null,null,79,5.5300000000000009E-2,7.3525260908476872E-2,9.2018570685951345E-2,1.862613709341869E-2,65.186986355286265,65.186986355286265,1,65.186986355286265,1.812852148076091E-6,0.45408987567042175,301133.28597091127,3.3207886560125987E-6,0,6.6E-4,5.9225977868334008E-2,2.8763274926575191E-3,9.9899996376012337E-2,0.10282364458480019,2.1204397054865508E-2,4.9458909990642792E-6,4.9458909990642792E-6,3.1020117080173909E-2,1.9244953273353942E-6,1.9244953273353942E-6,3.9910130652417199E-2,1.0942663292120985E-3,1.2090501431732087E-3,35,73.021974049185928,4.66067258852043E-2,4.2495929316214993E-2,9.0311705344592499E-2,9.1424474575644288E-2,4.3719447414093726E-2,5.8106258498688676E-4,3.3124661456800245E-3,7.0470798325530861E-4,5.3819380351639715E-4,4.5553679324517298E-3,5.136982576242532E-3,2.8325298457411135E-2,6.1784518994925063E-2,4.5215162888532327E-3,0.16286749243566512,0.26569800740679173,1.0507000000000002,0.79816286114698887,8.4531367017476918E-4,4.4182279258880115E-4,2.8852016345107083E-2,6.8605167157993474E-2,5.3533048461804642E-4,4.0883820887620427E-4,3.4604792067601743E-3,2.1849983640765866E-3,7.5888899720235853E-2,1.461940322385104E-6,3.7571395362465821E-6,4.6934527891481739E-2,0.22816261292177137,0.79816286114698887,79.816286114698883,55.300000000000011,72.116619551864289,0.72116619551864292,301.13328597091129,null,3.2281976330189734E-2,null,0.16286749243566512,6.1784518994925063E-2,0.10282364458480019,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR85, IF(MODE_ILIM=4,#REF!,#REF!))","v":79.816286114698883},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ85, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.16286749243566512},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA85, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.1784518994925063E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB85, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10282364458480019},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S85, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.13328597091129},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P85, IF(MODE_ILIM=4,#REF!,#REF!))","v":65.186986355286265}]
[null,null,null,null,null,null,null,80,5.6000000000000008E-2,7.3521876393110447E-2,9.2718578868054388E-2,1.9327829370882225E-2,65.183985667437156,65.183985667437156,1,65.183985667437156,1.8126938790127016E-6,0.45411151866314975,301147.63869240455,3.3206303869492092E-6,0,6.6E-4,5.9880100655062274E-2,2.9402136926575191E-3,9.9904757845075923E-2,0.10289337609986025,2.1204397054865508E-2,4.9458909990642792E-6,4.9458909990642792E-6,3.133012785703386E-2,1.9631538230761779E-6,1.9631538230761779E-6,4.0351880682240486E-2,1.1186244266459221E-3,1.2091077693500043E-3,35,72.470728667096935,4.676388773161292E-2,4.2497954772272126E-2,9.047095027323504E-2,9.160852755037642E-2,4.4203361319744235E-2,5.939968941970137E-4,3.3126240256164509E-3,7.3130279302984901E-4,5.4505901185719912E-4,4.5889858305034987E-3,5.1835521883214601E-3,2.8325298457411135E-2,6.1786113740162907E-2,4.5217317949664548E-3,0.16309992527382725,0.26600021041850963,1.0640000000000001,0.79999987343249535,8.5532112568870926E-4,4.4704230357292183E-4,2.8558301555280424E-2,6.8023260120212037E-2,5.4985163709089238E-4,4.0981874107048899E-4,3.4503647402127006E-3,2.2106866372091213E-3,7.5116347397899283E-2,1.4760552725464865E-6,3.718714448554832E-6,4.6455717266932414E-2,0.22608190629489006,0.79999987343249535,79.999987343249529,56.000000000000007,72.121604042494241,0.72121604042494236,301.14763869240454,null,3.1953344397516549E-2,null,0.16309992527382725,6.1786113740162907E-2,0.10289337609986025,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR86, IF(MODE_ILIM=4,#REF!,#REF!))","v":79.999987343249529},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ86, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.16309992527382725},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA86, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.1786113740162907E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB86, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10289337609986025},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S86, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.14763869240454},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P86, IF(MODE_ILIM=4,#REF!,#REF!))","v":65.183985667437156}]
[null,null,null,null,null,null,null,81,5.6700000000000007E-2,7.3518491877744008E-2,9.3418587050157431E-2,2.0029521648345767E-2,65.180984979588047,65.180984979588047,1,65.180984979588047,1.8125356230135019E-6,0.4541331619323295,301161.99159722903,3.3204721309500098E-6,0,6.6E-4,6.0535249685289887E-2,3.0049034926575191E-3,9.9909519374959038E-2,0.10296392633351371,2.1204397054865508E-2,4.9458909990642792E-6,4.9458909990642792E-6,3.1640945063232756E-2,2.0022988089890268E-6,2.0022988089890268E-6,4.0794343289445728E-2,1.1432905913145793E-3,1.2091653962628746E-3,35,71.927743667620604,4.6921064375534963E-2,4.2499980254200959E-2,9.0630210025998803E-2,9.1792910374609266E-2,4.4688055816409361E-2,6.0709478912575755E-4,3.3127819075695194E-3,7.5790013508582972E-4,5.5192605303667759E-4,4.6226080956920266E-3,5.2302901532047504E-3,2.8325298457411135E-2,6.1787708505770852E-2,4.5219473038323943E-3,0.16333285633741726,0.266303730860739,1.0773000000000001,0.80179890488236472,8.6535957135636544E-4,4.522777390052576E-4,2.8270506012854392E-2,6.7453080059504816E-2,5.6408010611901462E-4,4.1078038141729691E-4,3.4404549418232803E-3,2.2364506912559094E-3,7.435936435734293E-2,1.4902450499347114E-6,3.6810637582078189E-6,4.5986556219361215E-2,0.22404408138884863,0.80179890488236472,80.179890488236467,56.70000000000001,72.124846875437001,0.72124846875436999,301.16199159722902,null,3.1631335398997908E-2,null,0.16333285633741726,6.1787708505770852E-2,0.10296392633351371,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR87, IF(MODE_ILIM=4,#REF!,#REF!))","v":80.179890488236467},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ87, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.16333285633741726},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA87, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.1787708505770852E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB87, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10296392633351371},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S87, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.16199159722902},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P87, IF(MODE_ILIM=4,#REF!,#REF!))","v":65.180984979588047}]
[null,null,null,null,null,"Eff (%)","Iout (mA)",82,5.74E-2,7.3515107362377582E-2,9.4118595232260488E-2,2.0731213925809296E-2,65.177984291738937,65.177984291738937,1,65.177984291738937,1.8123773800768747E-6,0.45415480547796633,301176.34468538821,3.3203138880133829E-6,0,6.600000000000001E-4,6.1191391996426987E-2,3.0703968926575186E-3,9.9914280965662836E-2,0.10303529533842294,2.1204397054865508E-2,4.9458909990642792E-6,4.9458909990642792E-6,3.1952545253228853E-2,2.0419302963192756E-6,2.0419302963192756E-6,4.1237496309303137E-2,1.1682648669776757E-3,1.2092230239118336E-3,35,71.392834759466069,4.7078255817253972E-2,4.2502005762001978E-2,9.0789484603167783E-2,9.1977623129179412E-2,4.5173506623794255E-2,6.2035629300975488E-4,3.3129397915392707E-3,7.8450000947176868E-4,5.5879492723612235E-4,4.6562347282471618E-3,5.2771964998505685E-3,2.8325298457411139E-2,6.1789303291749309E-2,4.5221628154511039E-3,0.16356628573623039,0.26660856889594869,1.0906,0.80356109222562055,8.7542810533398408E-4,4.5752862591233256E-4,2.798845256384578E-2,6.6894276004330344E-2,5.7802465107476995E-4,4.1172369526865457E-4,3.4307436859427423E-3,2.2622881722263225E-3,7.3617484633876365E-2,1.5045073713175337E-6,3.6441642886823382E-6,4.5526755951749688E-2,0.22204785476122099,0.80356109222562055,80.356109222562054,57.4,72.126370778645395,0.72126370778645399,301.17634468538819,null,3.1315751120386877E-2,null,0.16356628573623039,6.1789303291749309E-2,0.10303529533842294,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR88, IF(MODE_ILIM=4,#REF!,#REF!))","v":80.356109222562054},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ88, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.16356628573623039},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA88, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.1789303291749309E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB88, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10303529533842294},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S88, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.17634468538819},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P88, IF(MODE_ILIM=4,#REF!,#REF!))","v":65.177984291738937}]
[null,null,null,null,null,{"$f":"BT51","v":68.427867006324419},{"$f":"I56*1000","v":35},83,5.8100000000000006E-2,7.3511722847011143E-2,9.4818603414363517E-2,2.1432906203272831E-2,65.174983603889814,65.174983603889814,1,65.174983603889814,1.8122191502012023E-6,0.45417644930006562,301190.69795688562,3.3201556581377105E-6,0,6.6E-4,6.1848495975734039E-2,3.1366938926575194E-3,9.9919042617188522E-2,0.10310748316788443,2.1204397054865508E-2,4.9458909990642792E-6,4.9458909990642792E-6,3.2264905828946117E-2,2.0820482963015226E-6,2.0820482963015226E-6,4.1681318484663984E-2,1.1935472973959344E-3,1.2092806522968958E-3,35,70.865823092989885,4.7235462057053458E-2,4.250403129567569E-2,9.0948774005026045E-2,9.2162665895044904E-2,4.5659690455811412E-2,6.3378142908623674E-4,3.3130976775257422E-3,8.1110241623618697E-4,5.6566563463682847E-4,4.6898657283987576E-3,5.324271257249341E-3,2.8325298457411135E-2,6.1790898098098651E-2,4.5223783298226385E-3,0.16380021358021554,0.2669147246873953,1.1039000000000001,0.80528752727815689,8.8552586148772097E-4,4.6279451002779023E-4,2.7711971053690752E-2,6.634651085015611E-2,5.9169368524338917E-4,4.1264922563902609E-4,3.4212250889471942E-3,2.2881968191382101E-3,7.2890260673246235E-2,1.5188400436655062E-6,3.6079937791681911E-6,4.5076039077556328E-2,0.22009199367895557,0.80528752727815689,80.528752727815686,58.100000000000009,72.126175499523185,0.72126175499523182,301.19069795688563,null,3.1006401178954677E-2,null,0.16380021358021554,6.1790898098098651E-2,0.10310748316788443,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR89, IF(MODE_ILIM=4,#REF!,#REF!))","v":80.528752727815686},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ89, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.16380021358021554},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA89, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.1790898098098651E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB89, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10310748316788443},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S89, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.19069795688563},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P89, IF(MODE_ILIM=4,#REF!,#REF!))","v":65.174983603889814}]
[null,null,null,null,null,{"$f":"BT81","v":72.078010752951272},{"$f":"I81*1000","v":52.500000000000007},84,5.8800000000000005E-2,7.3508338331644718E-2,9.5518611596466574E-2,2.213459848073638E-2,65.171982916040719,65.171982916040719,1,65.171982916040719,1.8120609333848679E-6,0.45419809339863271,301205.05141172482,3.3199974413213761E-6,0,6.5999999999999989E-4,6.2506531294420659E-2,3.2037944926575192E-3,9.992380432953725E-2,0.10318048987582899,2.1204397054865508E-2,4.9458909990642792E-6,4.9458909990642792E-6,3.2578005004600986E-2,2.122652820159614E-6,2.122652820159614E-6,4.2125789421655527E-2,1.2191379263311957E-3,1.2093382814180752E-3,35,70.346535060820628,4.7392683095216978E-2,4.2506056855222601E-2,9.1108078231857653E-2,9.2348038753285316E-2,4.614658497204667E-2,6.4737022059302635E-4,3.3132555655289737E-3,8.3770735542760492E-4,5.7253817542009516E-4,4.7235010963766737E-3,5.3715144544237712E-3,2.8325298457411129E-2,6.1792492924819288E-2,4.5225938469470491E-3,0.16403463997947543,0.26722219839912364,1.1172000000000002,0.8069792591392092,8.956520076472995E-4,4.6807495487751312E-4,2.744089798493891E-2,6.5809460681293938E-2,6.050952927483304E-4,4.1355749429772905E-4,3.411893497401799E-3,2.3141744594692469E-3,7.2177262431275743E-2,1.5332409597405639E-6,3.5725308397853332E-6,4.4634139062688406E-2,0.21817531363843845,0.8069792591392092,80.697925913920926,58.800000000000004,72.124237241864293,0.72124237241864297,301.20505141172481,null,3.0703102640491076E-2,null,0.16403463997947543,6.1792492924819288E-2,0.10318048987582899,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR90, IF(MODE_ILIM=4,#REF!,#REF!))","v":80.697925913920926},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ90, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.16403463997947543},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA90, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.1792492924819288E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB90, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10318048987582899},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S90, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.20505141172481},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P90, IF(MODE_ILIM=4,#REF!,#REF!))","v":65.171982916040719}]
[null,null,null,null,null,{"$f":"BT106","v":71.049894896969974},{"$f":"I106*1000","v":70},85,5.9500000000000004E-2,7.3504953816278279E-2,9.6218619778569617E-2,2.2836290758199922E-2,65.168982228191595,65.168982228191595,1,65.168982228191595,1.8119027296262551E-6,0.4542197377736728,301219.40504990931,3.3198392375627631E-6,0,6.6E-4,6.3165468845409425E-2,3.2716986926575181E-3,9.992856610271017E-2,0.10325431551682171,2.1204397054865508E-2,4.9458909990642792E-6,4.9458909990642792E-6,3.2891821773099343E-2,2.1637438791066641E-6,2.1637438791066641E-6,4.257088954783949E-2,1.2450367975464182E-3,1.2093959112753859E-3,35,69.834802107185354,4.7549918932028049E-2,4.2508082440643198E-2,9.126739728394663E-2,9.253374178510175E-2,4.6634168731924122E-2,6.6112269076854121E-4,3.3134134555490033E-3,8.643148270945448E-4,5.7941254976722628E-4,4.757140832410774E-3,5.4189261204288597E-3,2.8325298457411135E-2,6.1794087771911616E-2,4.5228093668243895E-3,0.16426956504426662,0.26753099019596649,1.1305000000000001,0.808637296260174,9.0580574396109236E-4,4.7336954091791713E-4,2.7175076194841333E-2,6.5282814132148384E-2,6.182372444929787E-4,4.1444900279786231E-4,3.4027434769124472E-3,2.3402190048726415E-3,7.1478076525830714E-2,1.5477080939410115E-6,3.5377549094036879E-6,4.4200799699904897E-2,0.21629667602968361,0.808637296260174,80.863729626017403,59.500000000000007,72.120507778355574,0.72120507778355569,301.21940504990931,null,3.0405679658563726E-2,null,0.16426956504426662,6.1794087771911616E-2,0.10325431551682171,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR91, IF(MODE_ILIM=4,#REF!,#REF!))","v":80.863729626017403},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ91, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.16426956504426662},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA91, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.1794087771911616E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB91, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10325431551682171},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S91, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.21940504990931},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P91, IF(MODE_ILIM=4,#REF!,#REF!))","v":65.168982228191595}]
[null,null,null,null,null,null,null,86,6.0200000000000004E-2,7.3501569300911854E-2,9.691862796067266E-2,2.3537983035663464E-2,65.165981540342486,65.165981540342486,1,65.165981540342486,1.8117445389237476E-6,0.45424138242519102,301233.75887144246,3.3196810468602558E-6,0,6.6E-4,6.3825280684540589E-2,3.34040649265752E-3,9.9933327936708435E-2,0.10332896014606217,2.1204397054865508E-2,4.9458909990642792E-6,4.9458909990642792E-6,3.3206335873934012E-2,2.2053214843450337E-6,2.2053214843450337E-6,4.3016600072683729E-2,1.2712439548056779E-3,1.2094535418688416E-3,35,69.330460545498383,4.770716956777022E-2,4.2510108051937952E-2,9.1426731161577013E-2,9.2719775071816946E-2,4.7122421151404886E-2,6.750388628517926E-4,3.3135713475858672E-3,8.9092483128552986E-4,5.8628875785953047E-4,4.7907849367309274E-3,5.4665062843519139E-3,2.8325298457411135E-2,6.179568263937598E-2,4.5230248894547083E-3,0.16450498888499956,0.26784110024354513,1.1438000000000001,0.81026260839434638,9.1598630134589337E-4,4.7867786472383572E-4,2.6914354551496617E-2,6.4766271785231727E-2,6.3112701318474062E-4,4.1532423344600847E-4,3.3937698016191157E-3,2.3663284471394405E-3,7.0792305437598332E-2,1.5622394983856431E-6,3.5036462158908396E-6,4.3775774613472637E-2,0.21445498593497259,0.81026260839434638,81.026260839434642,60.2,72.229662267470047,0.72229662267470052,301.23375887144249,null,3.011396313454166E-2,null,0.16450498888499956,6.179568263937598E-2,0.10332896014606217,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR92, IF(MODE_ILIM=4,#REF!,#REF!))","v":81.026260839434642},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ92, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.16450498888499956},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA92, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.179568263937598E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB92, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10332896014606217},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S92, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.23375887144249},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P92, IF(MODE_ILIM=4,#REF!,#REF!))","v":65.165981540342486}]
[null,null,null,null,null,null,null,87,6.0900000000000003E-2,7.3498184785545428E-2,9.7618636142775717E-2,2.4239675313126992E-2,65.162980852493391,65.162980852493391,1,65.162980852493391,1.811586361275729E-6,0.45426302735319296,301248.11287632794,3.3195228692122372E-6,0,6.6E-4,6.4485939975008427E-2,3.4099178926575197E-3,9.9938089831533239E-2,0.10340442381938462,2.1204397054865508E-2,4.9458909990642792E-6,4.9458909990642792E-6,3.3521527762516629E-2,2.247385647066346E-6,2.247385647066346E-6,4.3462902950206335E-2,1.2977594418741706E-3,1.2095111731984566E-3,35,68.833351383797464,4.7864435002727058E-2,4.2512133689107397E-2,9.1586079865032921E-2,9.2906138694875531E-2,4.7611322462065626E-2,6.8911876008238566E-4,3.3137292416396077E-3,9.1753736804908552E-4,5.9316679987832103E-4,4.8244334095670135E-3,5.5142549753125743E-3,2.8325298457411135E-2,6.1797277527212813E-2,4.5232404148380645E-3,0.164740911612239,0.26815252870826978,1.1571,0.81185612843549848,9.2619294002516291E-4,4.83999538222716E-4,2.6658587667320571E-2,6.4259545603500112E-2,6.4377178750257326E-4,4.1618365021665177E-4,3.3849674442882611E-3,2.3925008543910359E-3,7.0119566756432133E-2,1.5768332992211487E-6,3.4701857386261386E-6,4.33588267920638E-2,0.21264919005300084,0.81185612843549848,81.185612843549848,60.900000000000006,72.361493645121143,0.72361493645121144,301.24811287632792,null,2.9827790397002035E-2,null,0.164740911612239,6.1797277527212813E-2,0.10340442381938462,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR93, IF(MODE_ILIM=4,#REF!,#REF!))","v":81.185612843549848},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ93, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.164740911612239},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA93, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.1797277527212813E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB93, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10340442381938462},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S93, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.24811287632792},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P93, IF(MODE_ILIM=4,#REF!,#REF!))","v":65.162980852493391}]
[null,null,null,null,null,null,null,88,6.1600000000000009E-2,7.3494800270179003E-2,9.8318644324878759E-2,2.4941367590590534E-2,65.159980164644267,65.159980164644267,1,65.159980164644267,1.8114281966805835E-6,0.45428467255768379,301262.46706456924,3.3193647046170913E-6,0,6.600000000000001E-4,6.5147420934833555E-2,3.4802328926575189E-3,9.9942851787185732E-2,0.10348070659325785,2.1204397054865508E-2,4.9458909990642792E-6,4.9458909990642792E-6,3.3837378580879117E-2,2.2899363784514736E-6,2.2899363784514736E-6,4.3909780843660505E-2,1.3245833025182089E-3,1.2095688052642455E-3,35,68.343320157636413,4.8021715237182142E-2,4.2514159352152005E-2,9.1745443394598392E-2,9.3092832735843831E-2,4.8100853672412777E-2,7.033624057005191E-4,3.3138871377102618E-3,9.4415243743373775E-4,6.0004667600491591E-4,4.8580862511489152E-3,5.5621722224628248E-3,2.8325298457411139E-2,6.1798872435422494E-2,4.5234559429745075E-3,0.16497733333670367,0.26846527575733903,1.1704000000000001,0.81341875415261955,9.364249481496785E-4,4.8933418797205861E-4,2.6407635628697992E-2,6.3762358394748711E-2,6.5617848546437973E-4,4.1702769961495147E-4,3.3763315669647301E-3,2.4187343674867104E-3,6.945949247026019E-2,1.5914876931380374E-6,3.4373551731318528E-6,4.2949728148033169E-2,0.21087827474025886,0.81341875415261955,81.341875415261953,61.600000000000009,72.477313046906502,0.724773130469065,301.26246706456925,null,2.9547004899242498E-2,null,0.16497733333670367,6.1798872435422494E-2,0.10348070659325785,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR94, IF(MODE_ILIM=4,#REF!,#REF!))","v":81.341875415261953},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ94, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.16497733333670367},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA94, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.1798872435422494E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB94, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10348070659325785},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S94, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.26246706456925},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P94, IF(MODE_ILIM=4,#REF!,#REF!))","v":65.159980164644267}]
[null,null,null,null,null,null,null,89,6.2300000000000008E-2,7.3491415754812564E-2,9.9018652506981816E-2,2.5643059868054083E-2,65.156979476795158,65.156979476795158,1,65.156979476795158,1.8112700451366946E-6,0.45430631803866883,301276.82143616985,3.3192065530732021E-6,0,6.6E-4,6.5809698787187815E-2,3.5513514926575188E-3,9.9947613803667096E-2,0.10355780852478555,2.1204397054865508E-2,4.9458909990642792E-6,4.9458909990642792E-6,3.4153870129683295E-2,2.3329736896705453E-6,2.3329736896705453E-6,4.435721709213717E-2,1.3517155805052234E-3,1.2096264380662221E-3,35,67.860216770065264,4.8179010271419034E-2,4.2516185041072282E-2,9.190482175055753E-2,9.3279857276410069E-2,4.8590996531297406E-2,7.1776982294698513E-4,3.3140450357978684E-3,9.7077003948801337E-4,6.0692838642063753E-4,4.891743461706519E-3,5.6102580549870079E-3,2.8325298457411135E-2,6.1800467364005407E-2,4.5236714738640903E-3,0.16521425416926658,0.26877934155874084,1.1837000000000002,0.81495134982760031,9.4668164049542156E-4,4.9468145447728617E-4,2.6161363740760384E-2,6.3274443305974357E-2,6.6835376704650607E-4,4.178568114912443E-4,3.3678575121467136E-3,2.4450271966321769E-3,6.881172829377899E-2,1.6062009440815136E-6,3.4051368976832072E-6,4.254825910135402E-2,0.20914126416199885,0.81495134982760031,81.495134982760035,62.300000000000011,72.230234640211876,0.72230234640211877,301.27682143616983,null,2.92714559337179E-2,null,0.16521425416926658,6.1800467364005407E-2,0.10355780852478555,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR95, IF(MODE_ILIM=4,#REF!,#REF!))","v":81.495134982760035},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ95, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.16521425416926658},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA95, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.1800467364005407E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB95, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10355780852478555},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S95, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.27682143616983},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P95, IF(MODE_ILIM=4,#REF!,#REF!))","v":65.156979476795158}]
[null,null,null,null,null,null,null,90,6.3000000000000014E-2,7.3488031239446139E-2,9.9718660689084859E-2,2.6344752145517618E-2,65.153978788946063,65.153978788946063,1,65.153978788946063,1.8111119066424483E-6,0.45432796379615326,301291.1759911332,3.3190484145789563E-6,0,6.5999999999999989E-4,6.6472749713400545E-2,3.6232736926575214E-3,9.9952375880978467E-2,0.1036357296717062,2.1204397054865508E-2,4.9458909990642792E-6,4.9458909990642792E-6,3.4470984841478952E-2,2.3764975918829432E-6,2.3764975918829432E-6,4.480519567897015E-2,1.3791563196037635E-3,1.2096840716043999E-3,35,67.383895338349447,4.8336320105721295E-2,4.2518210755868716E-2,9.2064214933194416E-2,9.3467212398384528E-2,4.9081733493304781E-2,7.323410350631701E-4,3.3142029359024658E-3,9.9739017426044106E-4,6.1381193130681305E-4,4.9254050414697208E-3,5.6585125021018472E-3,2.8325298457411129E-2,6.1802062312961932E-2,4.5238870075068657E-3,0.16545167422095516,0.26909472628125231,1.1970000000000003,0.81645474780213512,9.5696235723377382E-4,5.000409915474238E-4,2.5919642286311387E-2,6.2795543345766744E-2,6.8030404610370577E-4,4.1867139981039715E-4,3.3595407944498955E-3,2.4713776181761126E-3,6.817593303435962E-2,1.6209713801446694E-6,3.3735139417693194E-6,4.2154208186617512E-2,0.20743721854569852,0.81645474780213512,81.645474780213505,63.000000000000014,72.8349974854723,0.72834997485472297,301.29117599113323,null,2.9000998362306442E-2,null,0.16545167422095516,6.1802062312961932E-2,0.1036357296717062,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR96, IF(MODE_ILIM=4,#REF!,#REF!))","v":81.645474780213505},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ96, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.16545167422095516},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA96, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.1802062312961932E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB96, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.1036357296717062},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S96, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.29117599113323},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P96, IF(MODE_ILIM=4,#REF!,#REF!))","v":65.153978788946063}]
[null,null,null,null,null,null,null,91,6.3700000000000007E-2,7.3484646724079714E-2,0.1004186688711879,2.7046444422981153E-2,65.150978101096939,65.150978101096939,1,65.150978101096939,1.810953781196229E-6,0.4543496098301425,301305.53072946292,3.3188902891327372E-6,0,6.6E-4,6.7136550808485768E-2,3.6959994926575204E-3,9.9957138019121025E-2,0.10371447009239337,2.1204397054865508E-2,4.9458909990642792E-6,4.9458909990642792E-6,3.4788705755153512E-2,2.4205080962373019E-6,2.4205080962373019E-6,4.5253701201836076E-2,1.4069055635834965E-3,1.2097417058787936E-3,35,66.914214047099691,4.8493644740372516E-2,4.2520236496541804E-2,9.2223622942793113E-2,9.3654898183699375E-2,4.9573047686000356E-2,7.4707606529105343E-4,3.3143608380240925E-3,1.0240128417995501E-3,6.2069731084477421E-4,4.9590709906684174E-3,5.706935593056451E-3,2.8325298457411135E-2,6.1803657282292493E-2,4.5241025439028866E-3,0.16568959360295121,0.26941143009443991,1.2103000000000002,0.81792974993965872,9.6726646276896989E-4,5.0541246568616585E-4,2.5682346297993253E-2,6.2325410932932444E-2,6.9203550163439247E-4,4.1947186337890172E-4,3.3513770927294339E-3,2.4977839715826411E-3,6.7551777992781628E-2,1.6357973906323189E-6,3.34246995628642E-6,4.1767371681617663E-2,0.20576523253045242,0.81792974993965872,81.792974993965871,63.70000000000001,73.305168165960453,0.73305168165960455,301.30553072946293,null,2.8735492361391047E-2,null,0.16568959360295121,6.1803657282292493E-2,0.10371447009239337,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR97, IF(MODE_ILIM=4,#REF!,#REF!))","v":81.792974993965871},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ97, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.16568959360295121},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA97, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.1803657282292493E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB97, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10371447009239337},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S97, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.30553072946293},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P97, IF(MODE_ILIM=4,#REF!,#REF!))","v":65.150978101096939}]
[null,null,null,null,null,null,null,92,6.4400000000000013E-2,7.3481262208713288E-2,0.10111867705329097,2.7748136700444702E-2,65.147977413247844,65.147977413247844,1,65.147977413247844,1.8107956687964219E-6,0.45437125614064183,301319.88565116248,3.3187321767329299E-6,0,6.6E-4,6.7801080039040618E-2,3.7695288926575211E-3,9.9961900218095937E-2,0.10379402984585576,2.1204397054865508E-2,4.9458909990642792E-6,4.9458909990642792E-6,3.5107016491518525E-2,2.4650052138715074E-6,2.4650052138715074E-6,4.570271884444823E-2,1.4349633562152078E-3,1.2097993408894175E-3,35,66.451035007501432,4.865098417565631E-2,4.2522262263092046E-2,9.2383045779637768E-2,9.3842914714409073E-2,5.0064922878921919E-2,7.6197493687320944E-4,3.3145187421627876E-3,1.0506380421538726E-3,6.2758452521585761E-4,4.9927413095325179E-3,5.7555273571323531E-3,2.8325298457411135E-2,6.180525227199745E-2,4.5243180830522051E-3,0.16592801242659108,0.26972945316865976,1.2236000000000002,0.81937712900771675,9.7759334463915111E-4,5.1079555551609708E-4,2.5449355342853627E-2,6.1863807469686206E-2,7.0355408843276275E-4,4.2025858653239645E-4,3.3433622426307466E-3,2.5242446565686143E-3,6.6938946396583265E-2,1.6506774232846421E-6,3.3119891853533803E-6,4.1387553256151455E-2,0.20412443360620294,0.81937712900771675,81.937712900771672,64.400000000000006,73.638455592594738,0.73638455592594743,301.31988565116245,null,2.8474803180815241E-2,null,0.16592801242659108,6.180525227199745E-2,0.10379402984585576,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR98, IF(MODE_ILIM=4,#REF!,#REF!))","v":81.937712900771672},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ98, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.16592801242659108},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA98, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.180525227199745E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB98, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10379402984585576},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S98, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.31988565116245},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P98, IF(MODE_ILIM=4,#REF!,#REF!))","v":65.147977413247844}]
[null,null,null,null,null,null,null,93,6.5100000000000005E-2,7.3477877693346849E-2,0.101818685235394,2.844982897790823E-2,65.14497672539872,65.14497672539872,1,65.14497672539872,1.8106375694414118E-6,0.45439290272765664,301334.24075623543,3.31857407737792E-6,0,6.6E-4,6.846631620337397E-2,3.8438618926575187E-3,9.9966662477904394E-2,0.10387440899173722,2.1204397054865508E-2,4.9458909990642792E-6,4.9458909990642792E-6,3.5425901229980711E-2,2.5099889559126979E-6,2.5099889559126979E-6,4.6152234349749924E-2,1.4633297412708006E-3,1.2098569766362853E-3,35,65.994224122350687,4.8808338411856264E-2,4.2524288055519936E-2,9.2542483444012488E-2,9.4031262072690205E-2,5.0557343454214303E-2,7.7703767305280528E-4,3.3146766483185901E-3,1.0772657753719398E-3,6.3447357460140398E-4,5.0264159982919337E-3,5.8042878236435023E-3,2.8325298457411135E-2,6.1806847282077214E-2,4.524533624954875E-3,0.16616693080336578,0.27004879567505796,1.2369000000000001,0.82079762998577144,9.8794241247646282E-4,5.1618995123395045E-4,2.5220553318532377E-2,6.1410502937863154E-2,7.1486554716636145E-4,4.2103193978610466E-4,3.3354922295420683E-3,2.5507581303952725E-3,6.6337132863975634E-2,1.6656099816505805E-6,3.2820564396474406E-6,4.1014563639761893E-2,0.20251398063715459,0.82079762998577144,82.079762998577138,65.100000000000009,73.832411821820315,0.73832411821820321,301.33424075623543,null,2.8218800915840413E-2,null,0.16616693080336578,6.1806847282077214E-2,0.10387440899173722,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR99, IF(MODE_ILIM=4,#REF!,#REF!))","v":82.079762998577138},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ99, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.16616693080336578},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA99, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.1806847282077214E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB99, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10387440899173722},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S99, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.33424075623543},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P99, IF(MODE_ILIM=4,#REF!,#REF!))","v":65.14497672539872}]
[null,null,null,null,null,null,null,94,6.5799999999999997E-2,7.3474493177980424E-2,0.10251869341749703,2.9151521255371765E-2,65.141976037549611,65.141976037549611,1,65.141976037549611,1.8104794831295851E-6,0.4544145495911921,301348.59604468528,3.3184159910660931E-6,0,6.6E-4,6.9132238893734585E-2,3.918998492657518E-3,9.9971424798547537E-2,0.10395560759031701,2.1204397054865508E-2,4.9458909990642792E-6,4.9458909990642792E-6,3.5745344686247314E-2,2.5554593334772583E-6,2.5554593334772583E-6,4.6602233994519099E-2,1.4920047625232994E-3,1.2099146131194114E-3,35,65.543650956618578,4.8965707449255977E-2,4.252631387382598E-2,9.2701935936201366E-2,9.4219940340841621E-2,5.1050294378810063E-2,7.9226429707360258E-4,3.3148345564915386E-3,1.1038960415022856E-3,6.4136445918275926E-4,5.0600950571765835E-3,5.8532170219363008E-3,2.8325298457411135E-2,6.1808442312532165E-2,4.5247491696109501E-3,0.16640634884492103,0.27036945778557059,1.2502,0.82219197130309718,9.9831309702284117E-4,5.2159535409500692E-4,2.4995828260343647E-2,6.0965275516716391E-2,7.2597541391493348E-4,4.2179228045050206E-4,3.3277631819237513E-3,2.5773229053047122E-3,6.5746042896414281E-2,1.6805936226016365E-6,3.2526570711653375E-6,4.0648220307242508E-2,0.20093306246412235,0.82219197130309718,82.219197130309723,65.8,73.8844086186851,0.73884408618685105,301.34859604468528,null,2.7967360291293583E-2,null,0.16640634884492103,6.1808442312532165E-2,0.10395560759031701,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR100, IF(MODE_ILIM=4,#REF!,#REF!))","v":82.219197130309723},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ100, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.16640634884492103},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA100, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.1808442312532165E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB100, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10395560759031701},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S100, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.34859604468528},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P100, IF(MODE_ILIM=4,#REF!,#REF!))","v":65.141976037549611}]
[null,null,null,null,null,null,null,95,6.6500000000000004E-2,7.3471108662613999E-2,0.10321870159960009,2.9853213532835307E-2,65.138975349700516,65.138975349700516,1,65.138975349700516,1.810321409859328E-6,0.45443619673125346,301362.95151651546,3.3182579177958359E-6,0,6.6E-4,6.9798828460514939E-2,3.9949386926575198E-3,9.9976187180026502E-2,0.10403762570250981,2.1204397054865508E-2,4.9458909990642792E-6,4.9458909990642792E-6,3.6065332091018032E-2,2.6014163576708303E-6,2.6014163576708303E-6,4.7052704565301279E-2,1.5209884637468428E-3,1.2099722503388095E-3,35,65.099188613282323,4.912309128813909E-2,4.2528339718010656E-2,9.2861403256488562E-2,9.4408949601284584E-2,5.1543761178065334E-2,8.0765483217995634E-4,3.3149924666816704E-3,1.1305288405934449E-3,6.4825717914127382E-4,5.0937784864163891E-3,5.902314981389602E-3,2.8325298457411135E-2,6.1810037363362685E-2,4.5249647170204797E-3,0.16664626666305735,0.27069143967292386,1.2635000000000001,0.82356084601108659,1.0087048491979236E-3,5.2701147592479445E-4,2.4775072158579745E-2,6.0527911220965874E-2,7.3688902920385452E-4,4.2253995321436322E-4,3.3201713649910194E-3,2.6039375460921652E-3,6.516539239805727E-2,1.6956269539774184E-6,3.2237769493217218E-6,4.0288347180805574E-2,0.19938089658093591,0.82356084601108659,82.356084601108662,66.5,73.791636151568156,0.73791636151568152,301.36295151651547,null,2.7720360457152156E-2,null,0.16664626666305735,6.1810037363362685E-2,0.10403762570250981,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR101, IF(MODE_ILIM=4,#REF!,#REF!))","v":82.356084601108662},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ101, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.16664626666305735},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA101, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.1810037363362685E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB101, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10403762570250981},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S101, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.36295151651547},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P101, IF(MODE_ILIM=4,#REF!,#REF!))","v":65.138975349700516}]
[null,null,null,null,null,null,null,96,{"$f":"IF(PLOT_TYPE=1, H102/100*Iout, min_I*EXP(H102*rr/100))","v":6.720000000000001E-2},{"$f":"IF(I102<Icrit, (Vin-(Rdcr+RdsonTop)*Iripple/2-Vout)/L*OnTime, (Vin-(Rdcr+RdsonTop)*I102-Vout)/L*OnTime)","v":7.3467724147247573E-2},{"$f":"IF(I102<Icrit, (Vin-(Rdcr+RdsonTop)*Iripple/2-Vout)/L*OnTime, I102+((Vin-(Rdcr+RdsonTop)*J102-Vout)/L*OnTime)/2)","v":0.10391870978170314},{"$f":"IF(I102<Icrit, 0, I102-((Vin-(Rdcr+RdsonTop)*K102-Vout)/L*OnTime)/2)","v":3.0554905810298849E-2},65.135974661851407,{"$f":"IF(I102<Icrit, 1000*SQRT((J102*CoutEsr)^2+(((J102/2)-I102)*(OnTime+OffTime)/Cout)^2), 1000*J102*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":65.135974661851407},1,{"$f":"IF(I102<Icrit, 1000*((N102/1000)*O102), 1000*J102*SQRT(CoutEsr^2+(1/(8*Fsw*Cout))^2))","v":65.135974661851407},1.8101633496290261E-6,0.45445784414784612,301377.30717172951,3.3180998575655345E-6,0,{"$f":"S102*(T102*Iq_active+U102*Iq_sleep)","v":6.600000000000001E-4},7.0466065978316048E-2,{"$f":"W102^2*Rdcr","v":4.0716824926575199E-3},{"$f":"Core_Loss/1000*S102/$S$106","v":9.9980949622342496E-2},{"$f":"(Y102+X102*(1+Ltc*(Ta-25)))/(1-X102*Ltc*ThetaCa)","v":0.10412046338986591},2.1204397054865508E-2,4.9458909990642792E-6,4.9458909990642792E-6,3.6385849169617415E-2,2.6478600395882967E-6,2.6478600395882967E-6,4.7503633335593584E-2,1.5502808887166901E-3,1.210029888294494E-3,{"$f":"20*VIN_nom/24","v":35},64.660713614174128,{"$f":"IF(I102<Icrit, Vin*(I102+Iripple/2)*AK102/1000000000/2*S102, Vin*(I102-Iripple/2)*AJ102/1000000000/2*S102 + Vin*(I102+Iripple/2)*AK102/1000000000/2*S102)","v":4.9280489928789188E-2},4.2530365588074465E-2,9.3020885405158155E-2,{"$f":"(AI102+AL102+AM102+AH102*(1+RdsonTopTc*(Ta-25)))/(1-AH102*RdsonTopTc*ThetaJA)","v":9.4598289936562663E-2},5.2037729910766099E-2,8.2320930161681549E-4,3.3151503788890254E-3,{"$f":"IF(I102<Icrit, Vin*Idss*R102, QrrBot*(I102-Iripple/2)/1*S102*Vin+Vin*Idss*R102)","v":1.1571641726939531E-3},6.5515173465830216E-4,5.1274662862412813E-3,{"$f":"(AR102+AS102+AT102+AQ102*(1+RdsonBotTc*(Ta-25)))/(1-AQ102*RdsonBotTc*ThetaJA)","v":5.9515817314147422E-3},{"$f":"Vin*V102+Vout*Ifb/0.8","v":2.8325298457411139E-2},{"$f":"(Vin-Vdd)*(S102*QgBot+S102*QgTop)+AW102","v":6.1811632434569178E-2},4.5251802671835194E-3,0.16688668436973009,{"$f":"SUM(Z102,AC102,AF102,AZ102)","v":0.27101474151063465},1.2768000000000002,0.82490492289398276,1.019117139215895E-3,5.3243803865644891E-4,2.4558180785410482E-2,6.0098203557857131E-2,7.4761154656311456E-4,4.2327529069718494E-4,3.3127131747285087E-3,2.6306006678057884E-3,6.4594907220461781E-2,1.7107086323548259E-6,3.1954024383029152E-6,3.9934774347892769E-2,0.1978567278803598,0.82490492289398276,82.490492289398276,67.2,73.551124384272143,0.73551124384272137,301.37730717172951,null,2.7477684794864864E-2,null,0.16688668436973009,6.1811632434569178E-2,0.10412046338986591,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR102, IF(MODE_ILIM=4,#REF!,#REF!))","v":82.490492289398276},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ102, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.16688668436973009},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA102, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.1811632434569178E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB102, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10412046338986591},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S102, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.37730717172951},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P102, IF(MODE_ILIM=4,#REF!,#REF!))","v":65.135974661851407}]
[null,null,null,null,null,null,null,97,{"$f":"IF(PLOT_TYPE=1, H103/100*Iout, min_I*EXP(H103*rr/100))","v":6.7900000000000002E-2},7.3464339631881134E-2,0.10461871796380617,3.1256598087762384E-2,65.132973974002283,65.132973974002283,1,65.132973974002283,1.810005302437066E-6,0.45447949184097541,301391.66301033105,{"$f":"IF(1/S103-OnTime-Q103>Tsleep, OnTime+Q103+Tsleep, 1/S103)","v":3.3179418103735744E-6},0,6.6E-4,7.1133933213765072E-2,4.149229892657519E-3,9.9985712125496687E-2,0.10420412071457133,2.1204397054865508E-2,4.9458909990642792E-6,4.9458909990642792E-6,3.6706882122524355E-2,2.6947903903137966E-6,2.6947903903137966E-6,4.7955008044207111E-2,{"$f":"RdsonTop*AG103^2","v":1.5798820812092187E-3},1.2100875269864793E-3,35,64.228105785613266,4.9437903371489941E-2,4.2532391484017912E-2,9.3180382382494334E-2,9.4787961429342135E-2,5.2532187145425284E-2,{"$f":"RdsonBot*AP103^2","v":8.3892772862972356E-4},3.3153082931136417E-3,1.1838020378523476E-3,6.6204812591520419E-4,5.1611584568811934E-3,6.0010173014555497E-3,2.8325298457411135E-2,6.181322752615203E-2,4.5253958201001213E-3,0.16712760207704982,0.27133936347301052,1.2901,0.82622484752178427,1.0295494557484226E-3,5.3787477389215525E-4,2.434505353079507E-2,5.9675953202075756E-2,7.5814794064067389E-4,4.239986139728491E-4,3.3053851322164414E-3,2.6573109335662256E-3,6.4034322730986373E-2,1.7258373609334052E-6,3.1675203755997591E-6,3.9587337793678255E-2,0.19635982746530878,0.82622484752178427,82.622484752178423,67.900000000000006,73.159788011658193,0.73159788011658189,301.39166301033106,null,2.723922073375671E-2,null,0.16712760207704982,6.181322752615203E-2,0.10420412071457133,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR103, IF(MODE_ILIM=4,#REF!,#REF!))","v":82.622484752178423},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ103, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.16712760207704982},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA103, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.181322752615203E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB103, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10420412071457133},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S103, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.39166301033106},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P103, IF(MODE_ILIM=4,#REF!,#REF!))","v":65.132973974002283}]
[null,null,null,null,null,null,null,98,{"$f":"IF(PLOT_TYPE=1, H104/100*Iout, min_I*EXP(H104*rr/100))","v":6.8600000000000008E-2},7.3460955116514709E-2,0.10531872614590923,3.1958290365225933E-2,65.129973286153188,65.129973286153188,1,65.129973286153188,1.8098472682818347E-6,0.45450113981064666,301406.01903232356,{"$f":"IF(1/S104-OnTime-Q104>Tsleep, OnTime+Q104+Tsleep, 1/S104)","v":3.3177837762183425E-6},0,6.6E-4,7.1802412594984516E-2,4.2275808926575207E-3,9.9990474689490239E-2,0.10428859773944782,2.1204397054865508E-2,4.9458909990642792E-6,4.9458909990642792E-6,3.7028417606756493E-2,2.7422074209207083E-6,2.7422074209207083E-6,4.840681687473964E-2,{"$f":"RdsonTop*AG104^2","v":1.6097920850019255E-3},1.210145166414779E-3,35,63.801248148598432,4.9595331616524983E-2,4.2534417405841497E-2,9.3339894188781261E-2,9.4977964162411707E-2,5.3027119937796227E-2,{"$f":"RdsonBot*AP104^2","v":8.5481013646481754E-4},3.3154662093555594E-3,1.2104424361171675E-3,6.689463530933444E-4,5.1948549985660715E-3,6.0506217209883679E-3,2.8325298457411135E-2,6.1814822638111638E-2,4.5256113757703382E-3,0.16736901989728206,0.27166530573514985,1.3034000000000001,0.82752124324879839,1.0400013051305762E-3,5.4332142248722428E-4,2.413559324686386E-2,5.9260967687441733E-2,7.6850301489702515E-4,4.2471023306625289E-4,3.2981838782496775E-3,2.6840670524987081E-3,6.3483383403471275E-2,1.7410118875298339E-6,3.1401180516485449E-6,3.9245879147379245E-2,0.19488949152142476,0.82752124324879839,82.752124324879844,68.600000000000009,72.614496083320674,0.72614496083320679,301.40601903232357,null,2.7004859576910605E-2,null,0.16736901989728206,6.1814822638111638E-2,0.10428859773944782,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR104, IF(MODE_ILIM=4,#REF!,#REF!))","v":82.752124324879844},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ104, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.16736901989728206},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA104, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.1814822638111638E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB104, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10428859773944782},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S104, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.40601903232357},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P104, IF(MODE_ILIM=4,#REF!,#REF!))","v":65.129973286153188}]
[null,null,null,null,null,null,null,99,{"$f":"IF(PLOT_TYPE=1, H105/100*Iout, min_I*EXP(H105*rr/100))","v":6.93E-2},7.3457570601148256E-2,0.10601873432801227,3.2659982642689454E-2,65.12697259830405,65.12697259830405,1,65.12697259830405,1.809689247161719E-6,0.45452278805686502,301420.37523771048,{"$f":"IF(1/S105-OnTime-Q105>Tsleep, OnTime+Q105+Tsleep, 1/S105)","v":3.3176257550982263E-6},0,6.6E-4,7.2471487182618172E-2,4.3067354926575197E-3,9.9995237314324303E-2,0.10437389452795309,2.1204397054865508E-2,4.9458909990642792E-6,4.9458909990642792E-6,3.7350442718070045E-2,2.7901111424716637E-6,2.7901111424716637E-6,4.8859048436094961E-2,{"$f":"RdsonTop*AG105^2","v":1.6400109438734227E-3},1.2102028065794077E-3,35,63.38002681335017,4.9752774664177921E-2,4.25364433535457E-2,9.3499420824303028E-2,9.5168298218682779E-2,5.3522515809532614E-2,{"$f":"RdsonBot*AP105^2","v":8.7085654836882717E-4},3.3156241276148155E-3,1.2370853675369511E-3,6.7584641637409137E-4,5.2285559115258584E-3,6.10039501952206E-3,2.8325298457411135E-2,6.1816417770448391E-2,4.525826934194223E-3,0.16761093794284745,0.27199256847294206,1.3167,0.82879471216109324,1.0504722106076711E-3,5.4877773415546154E-4,2.3929706100264271E-2,5.8853061114382287E-2,7.7868140890596771E-4,4.2541044742452455E-4,3.2911061682321385E-3,2.7108677777709831E-3,6.2941842429866807E-2,1.7562310026750677E-6,3.1131831905138766E-6,3.8910245441549834E-2,0.19344504024735312,0.82879471216109324,82.879471216109323,69.3,71.912167665597565,0.71912167665597559,301.42037523771046,null,2.6774496335960019E-2,null,0.16761093794284745,6.1816417770448391E-2,0.10437389452795309,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR105, IF(MODE_ILIM=4,#REF!,#REF!))","v":82.879471216109323},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ105, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.16761093794284745},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA105, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.1816417770448391E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB105, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10437389452795309},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S105, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.42037523771046},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P105, IF(MODE_ILIM=4,#REF!,#REF!))","v":65.12697259830405}]
[null,null,null,null,null,null,null,100,{"$f":"IF(PLOT_TYPE=1, H106/100*Iout, min_I*EXP(H106*rr/100))","v":7.0000000000000007E-2},7.3454186085781831E-2,0.10671874251011532,3.3361674920153003E-2,65.123971910454941,65.123971910454941,1,65.123971910454941,1.809531239075107E-6,0.45454443657963572,301434.73162649525,{"$f":"IF(1/S106-OnTime-Q106>Tsleep, OnTime+Q106+Tsleep, 1/S106)","v":3.3174677470116149E-6},0,6.6E-4,7.3141140642325159E-2,4.3866936926575187E-3,0.1,0.10446001114418089,2.1204397054865508E-2,4.9458909990642792E-6,4.9458909990642792E-6,3.7672944973936792E-2,2.8385015660185386E-6,2.8385015660185386E-6,4.9311691743989194E-2,{"$f":"RdsonTop*AG106^2","v":1.6705387016034438E-3},1.2102604474803786E-3,35,62.964330878003025,4.9910232514732415E-2,4.2538469327131005E-2,9.3658962289343797E-2,9.5358963681189499E-2,5.4018362727929634E-2,{"$f":"RdsonBot*AP106^2","v":8.8706698758907795E-4},3.3157820478914479E-3,1.26373083216024E-3,6.8274831593881813E-4,5.2622611959905058E-3,6.1503372265980351E-3,2.8325298457411135E-2,6.1818012923162649E-2,4.5260424953718261E-3,0.16785335632632201,0.27232115186306799,1.33,0.83004583597587056,1.0609617116200817E-3,5.542434670945559E-4,2.3727301431999304E-2,5.8452053872248798E-2,7.8868760528490894E-4,4.2609954636432633E-4,3.2841488673303184E-3,2.7377119047308184E-3,6.2409461351569211E-2,1.7714935378080265E-6,3.0867039315517615E-6,3.8580288883589255E-2,{"$f":"SUM(BD106:BO106)","v":0.19202581683930095},0.83004583597587056,83.004583597587057,70,71.049894896969974,0.71049894896969978,301.43473162649525,null,2.6548029574264949E-2,null,0.16785335632632201,6.1818012923162649E-2,0.10446001114418089,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR106, IF(MODE_ILIM=4,#REF!,#REF!))","v":83.004583597587057},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ106, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.16785335632632201},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA106, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.1818012923162649E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB106, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.10446001114418089},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S106, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":301.43473162649525},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P106, IF(MODE_ILIM=4,#REF!,#REF!))","v":65.123971910454941}]
[null,null,null,null,null,null,null,null,{"$f":"Losses!$E$5/1000","v":0.5},7.1375126646403234E-2,0.53672376865912985,0.46440121679061269,63.280692231715626,63.280692231715626,1,63.280692231715626,{"$f":"IF(I107<Icrit, L*J107/(Vout+J107/2*(RdsonBot+Rdcr)), L*J107/(Vout+I107*(RdsonBot+Rdcr)))","v":1.7148711544734443E-6},{"$f":"OnTime*S107","v":0.46789528445172646},{"$f":"IF(I107<Icrit,I107/((OnTime+Q107)*J107/2),1/(OnTime+Q107))","v":310288.45179430279},{"$f":"IF(1/S107-OnTime-Q107>Tsleep, OnTime+Q107+Tsleep, 1/S107)","v":3.222807662409952E-6},{"$f":"IF(1/S107-OnTime-Q107>Tsleep, 1/S107-OnTime-Q107-Tsleep, 0)","v":0},6.6E-4,{"$f":"IF(I107<Icrit,Iripple*SQRT((OnTime+OffTime)*S107/3), SQRT(I107^2+Iripple^2/12))","v":0.50044942447210428},0.20536869369265751,0.10293719310977678,0.31878069891616972,{"$f":"Iripple/SQRT(12)*SQRT((OnTime+Q107)*S107)","v":2.1204397054865508E-2},{"$f":"RCoutEsr*AA107^2","v":4.9458909990642792E-6},{"$f":"AB107","v":4.9458909990642792E-6},{"$f":"SQRT($R107)*SQRT($I107^2*(1-R107)+(Iripple^2)/12)","v":0.24990538191022993},{"$f":"RCinEsr*AD107^2","v":1.2490539981539574E-4},{"$f":"AE107","v":1.2490539981539574E-4},{"$f":"IF(I107<Icrit,Iripple*SQRT((OnTime)*S107/3), SQRT(OnTime*S107*(I107^2+Iripple^2/12)))","v":0.34232177729548319},{"$f":"RdsonTop*AG107^2","v":8.0505544857777278E-2},{"$f":"QgTop*S107*Vdd","v":1.2458081339541257E-3},35,{"$f":"IF(I107<Icrit, Csw*Vin/Iripple*1000000000, Csw*Vin/(I107+Iripple/2)*1000000000)","v":12.520329394780509},0.1494428576148181,{"$f":"IF(I107<Icrit, Csw*(Vin)^2*S107/2, Csw*Vin^2*S107/2)","v":4.3787906317212001E-2},0.1944765720659842,0.27913834749433392,{"$f":"IF(I107<Icrit,Iripple*SQRT((OffTime)*S107/3), SQRT(OffTime*S107*(I107^2+Iripple^2/12)))","v":0.37499548852673431},{"$f":"RdsonBot*AP107^2","v":4.2748971390282858E-2},{"$f":"QgBot*S107*Vdd","v":3.4131729697373311E-3},1.8112277365303901E-2,{"$f":"IF(I107<Icrit, dead1*S107*(I107+Iripple/2)*((I107+Iripple/2)*BDserR+VSD), dead1*S107*(I107+Iripple/2)*((I107+Iripple/2)*BDserR+VSD)+dead2*S107*(I107-Iripple/2)*((I107-Iripple/2)*BDserR+VSD))","v":5.2765778472604313E-3},2.6802028182301665E-2,7.0105281530928376E-2,2.8325298457411135E-2,6.2801758624727921E-2,{"$f":"AI107+AR107","v":4.6589811036914569E-3},{"$f":"AO107+AV107+AX107+AY107","v":0.41670436875368166},0.73561491896066589,{"$f":"Vout*I107","v":9.5},{"$f":"BB107/(BB107+BA107)","v":0.92813182942257844},8.2712935274187067E-3,4.23064502635898E-3,{"$f":"Vin*S107*(QgBot+QgTop)/($BB107+$BA107)","v":3.8234577581179748E-3},1.8999989116993035E-2,{"$f":"AS107/(BA107+BB107)","v":1.7695348553756493E-3},{"$f":"AT107/($BB107+$BA107)","v":5.1551156320720783E-4},2.6185068893763317E-3,{"$f":"X107/($BB107+$BA107)","v":2.0064128566641196E-2},{"$f":"Y107/($BB107+$BA107)","v":1.0056766879642354E-2},{"$f":"(AF107)/($BB107+$BA107)","v":1.2203018656360194E-5},{"$f":"(AC107)/($BB107+$BA107)","v":4.8320409064065199E-7},6.1356116971919917E-3,{"$f":"SUM(BD107:BO107)","v":7.6498132103070424E-2},{"$f":"BC107","v":0.92813182942257844},{"$f":"100*BQ107","v":92.813182942257839},{"$f":"I107*1000","v":500},72.049894896970002,{"$f":"BT107/100","v":0.72049894896970001},{"$f":"S107/1000","v":310.28845179430277},null,{"$f":"AM107/($BB107+$BA107)","v":4.2779946943977323E-3},null,0.41670436875368166,6.2801758624727921E-2,0.31878069891616972,null,null,{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BR107, IF(MODE_ILIM=4,#REF!,#REF!))","v":92.813182942257839},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), BZ107, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.41670436875368166},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CA107, IF(MODE_ILIM=4,#REF!,#REF!))","v":6.2801758624727921E-2},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), CB107, IF(MODE_ILIM=4,#REF!,#REF!))","v":0.31878069891616972},{"$f":"(IF(OR(MODE=1,MODE=2,MODE=3), S107, IF(MODE_ILIM=4,#REF!,#REF!)))/1000","v":310.28845179430277},{"$f":"IF(OR(MODE=1,MODE=2,MODE=3), P107, IF(MODE_ILIM=4,#REF!,#REF!))","v":63.280692231715626}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(OR(MODE=1, MODE=2,MODE=3),Efficiency!BD107,IF(AND(MODE=4,MODE_ILIM=4),#REF!,#REF!))","v":8.2712935274187067E-3},{"$f":"IF(OR(MODE=1, MODE=2,MODE=3),Efficiency!BE107,IF(AND(MODE=4,MODE_ILIM=4),#REF!,#REF!))","v":4.23064502635898E-3},null,{"$f":"IF(OR(MODE=1, MODE=2,MODE=3),Efficiency!BG107,IF(AND(MODE=4,MODE_ILIM=4),#REF!,#REF!))","v":1.8999989116993035E-2},null,null,{"$f":"IF(OR(MODE=1, MODE=2,MODE=3),Efficiency!BJ107,IF(AND(MODE=4,MODE_ILIM=4),#REF!,#REF!))","v":2.6185068893763317E-3},{"$f":"IF(OR(MODE=1, MODE=2,MODE=3),Efficiency!BK107,IF(AND(MODE=4,MODE_ILIM=4),#REF!,#REF!))","v":2.0064128566641196E-2},{"$f":"IF(OR(MODE=1, MODE=2,MODE=3),Efficiency!BL107,IF(AND(MODE=4,MODE_ILIM=4),#REF!,#REF!))","v":1.0056766879642354E-2},null,null,{"$f":"IF(OR(MODE=1, MODE=2,MODE=3),Efficiency!BO107,IF(AND(MODE=4,MODE_ILIM=4),#REF!,#REF!))","v":6.1356116971919917E-3}]
[null,null,null,null,null,null,null,1.0000000000000001E-5,"A","min_I",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Load (A)","High-side MOSFET Rdson %","Low-side MOSFET Rdson %","Gate Drive (Qg) Loss from Vin %","High-side MOSFET Switching Loss %","Reverse Recovery & Leakage Loss %","Deadtime Loss %",null,"Inductor Cu Loss %","Inductor Core Loss %","Cin ESR %","Cout ESR %","Quiescent Current Loss %","Total Loss %","Overall Eff %"]
[null,null,null,null,null,null,null,{"$f":"Iout","v":7.0000000000000007E-2},"A","max_I",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"I107","v":0.5},{"$f":"BD107","v":8.2712935274187067E-3},{"$f":"BE107","v":4.23064502635898E-3},3.8234577581179748E-3,1.8999989116993035E-2,1.7695348553756493E-3,5.1551156320720783E-4,null,2.0064128566641196E-2,1.0056766879642354E-2,1.2203018656360194E-5,4.8320409064065199E-7,6.1356116971919917E-3,7.6498132103070424E-2,0.92813182942257844]
[null,null,null,null,null,null,null,{"$f":"LOG(max_I/min_I,EXP(1))","v":8.8536654280374503},null,"rr",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"10mA",{"$f":"BD70","v":6.9966842762558118E-4},{"$f":"BE70","v":3.6583315272918881E-4},3.4114879134011719E-2,7.9031907113968722E-2,2.7513111398791082E-4,3.9139462014477715E-4,null,1.8107190509843451E-3,8.9731705770644751E-2,1.2610877262792414E-6,4.4456530246295025E-6,5.5514001299866132E-2,0.26558277995005652,0.7651078148063839]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"50ma",{"$f":"BD85","v":8.4531367017476918E-4},{"$f":"BE85","v":4.4182279258880115E-4},2.8852016345107083E-2,6.8605167157993474E-2,5.3533048461804642E-4,4.0883820887620427E-4,null,2.1849983640765866E-3,7.5888899720235853E-2,1.461940322385104E-6,3.7571395362465821E-6,4.6934527891481739E-2,0.22816261292177137,0.79816286114698887]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"100mA",{"$f":"BD91","v":9.0580574396109236E-4},{"$f":"BE91","v":4.7336954091791713E-4},2.7175076194841333E-2,6.5282814132148384E-2,6.182372444929787E-4,4.1444900279786231E-4,null,2.3402190048726415E-3,7.1478076525830714E-2,1.5477080939410115E-6,3.5377549094036879E-6,4.4200799699904897E-2,0.21629667602968361,0.808637296260174]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"500mA",{"$f":"BD106","v":1.0609617116200817E-3},{"$f":"BE106","v":5.542434670945559E-4},2.3727301431999304E-2,5.8452053872248798E-2,7.8868760528490894E-4,4.2609954636432633E-4,null,2.7377119047308184E-3,6.2409461351569211E-2,1.7714935378080265E-6,3.0867039315517615E-6,3.8580288883589255E-2,0.19202581683930095,0.83004583597587056]

{"sheet":"Schematic Mgmt","index":10,"n_rows":2,"n_cols":1,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
[]
[{"$f":"'Variable Mgmt'!K27","v":"SCH_COT3_LM5163"}]

{"sheet":"Efficiency Plots","index":11,"n_rows":2,"n_cols":1,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
[]
[{"$f":"IF(PLOT_TYPE=1, \"EFF_LINEAR\", \"EFF_LOG\")","v":"EFF_LINEAR"}]