Eval Board:
Timestamp	Message
25.09.2016 09:20:55	Click one of the scan buttons to find a device in ROM or program mode ...
25.09.2016 09:21:00	
25.09.2016 09:21:00	Looking for device in ROM mode at address 11d ...
25.09.2016 09:21:00	Reading ROM version ...
25.09.2016 09:21:00	SAA: BlockRead (Address 11d, Cmd 0xEC): ACK 0x00030002
25.09.2016 09:21:00	Reading PKGID version ...
25.09.2016 09:21:00	SAA: BlockWrite (Address 11d, Cmd 0xFD, 0xFFF7F010): ACK
25.09.2016 09:21:00	SAA: BlockRead (Address 11d, Cmd 0xFA): ACK 0x00000000
25.09.2016 09:21:00	Found ROM v2 IC v3 - UCD31xx 1p0

Own board:
Timestamp	Message	
25.09.2016 09:23:14	Looking for device in ROM mode at address 11d ...
25.09.2016 09:23:14	Reading ROM version ...
25.09.2016 09:23:14	SAA: BlockRead (Address 11d, Cmd 0xEC): ACK 0x00030002
25.09.2016 09:23:14	Reading PKGID version ...
25.09.2016 09:23:14	SAA: BlockWrite (Address 11d, Cmd 0xFD, 0xFFF7F010): ACK
25.09.2016 09:23:14	SAA: BlockRead (Address 11d, Cmd 0xFA): ACK 0x00000001
25.09.2016 09:23:14	Found ROM v2 IC v3 - UCD31xx 1p0

Differences:
Eval board: SAA: BlockRead (Address 11d, Cmd 0xFA): ACK 0x00000000
Own board: SAA: BlockRead (Address 11d, Cmd 0xFA): ACK 0x00000001

Flash program on eval board:
Timestamp	Message
25.09.2016 09:30:56	USB Adapter v1.0.10 [PEC; 400 kHz] Found (Adapter #1)
25.09.2016 09:30:56	Looking for device in ROM mode ...
25.09.2016 09:30:56	ROM v2 IC v3 detected
25.09.2016 09:30:56	Ready to download firmware
25.09.2016 09:31:03	
25.09.2016 09:31:03	Firmware download options:
25.09.2016 09:31:03	   File: W:\CCS\First Steps\UCD3138_lab_ClosedLoop_3Phase_unbalanced\Debug\UCD3138_Lab_ClosedLoop_3Phase_unbalanced.x0
25.09.2016 09:31:03	   Download program flash: Download
25.09.2016 09:31:03	   Download data flash: Download
25.09.2016 09:31:03	   Send to program mode when done: False
25.09.2016 09:31:03	
25.09.2016 09:31:03	Starting download ...
25.09.2016 09:31:03	Parsing firmware file ...
25.09.2016 09:31:03	Firmware is in Tektronix Extended format
25.09.2016 09:31:03	Mass erasing program flash
25.09.2016 09:31:03	Downloading program flash ...
25.09.2016 09:31:09	Mass erasing data flash
25.09.2016 09:31:09	Downloading data flash ...
25.09.2016 09:31:10	Verifying program flash ...
25.09.2016 09:31:10	Having ROM calculate checksum for program flash 0x10000 through 0x17FFB ...
25.09.2016 09:31:11	Program Flash checksum match between GUI calculation and Rom calculation (0x0067B676)
25.09.2016 09:31:11	Verifying data flash ...
25.09.2016 09:31:11	Reading data flash ...
25.09.2016 09:31:11	Data Flash verified!
25.09.2016 09:31:11	Download completed without error; 9,0 sec elapsed
25.09.2016 09:31:11	Sending ROM execute flash command (SendByte 0xF0 to address 11)
25.09.2016 09:31:11	Executing program ...

Flash same program on own board:
Timestamp	Message
25.09.2016 09:35:03	USB Adapter v1.0.10 [PEC; 400 kHz] Found (Adapter #1)
25.09.2016 09:35:03	Looking for device in ROM mode ...
25.09.2016 09:35:03	ROM v2 IC v3 detected
25.09.2016 09:35:03	Ready to download firmware
25.09.2016 09:35:09	
25.09.2016 09:35:09	Firmware download options:
25.09.2016 09:35:09	   File: W:\CCS\First Steps\UCD3138_lab_ClosedLoop_3Phase_unbalanced\Debug\UCD3138_Lab_ClosedLoop_3Phase_unbalanced.x0
25.09.2016 09:35:09	   Download program flash: Download
25.09.2016 09:35:09	   Download data flash: Download
25.09.2016 09:35:09	   Send to program mode when done: False
25.09.2016 09:35:09	
25.09.2016 09:35:09	Starting download ...
25.09.2016 09:35:09	Parsing firmware file ...
25.09.2016 09:35:09	Firmware is in Tektronix Extended format
25.09.2016 09:35:09	Mass erasing program flash
25.09.2016 09:35:09	Downloading program flash ...
25.09.2016 09:35:15	Mass erasing data flash
25.09.2016 09:35:15	Downloading data flash ...
25.09.2016 09:35:16	Verifying program flash ...
25.09.2016 09:35:16	Having ROM calculate checksum for program flash 0x10000 through 0x17FFB ...
25.09.2016 09:35:17	Program Flash checksum match between GUI calculation and Rom calculation (0x0067B676)
25.09.2016 09:35:17	Verifying data flash ...
25.09.2016 09:35:17	Reading data flash ...
25.09.2016 09:35:17	Data Flash verified!
25.09.2016 09:35:17	Download completed without error; 8,9 sec elapsed
25.09.2016 09:35:17	Sending ROM execute flash command (SendByte 0xF0 to address 11)
25.09.2016 09:35:17	Executing program ...

Flashing eval board with different options:
Timestamp	Message
25.09.2016 09:38:08	USB Adapter v1.0.10 [PEC; 400 kHz] Found (Adapter #1)
25.09.2016 09:38:08	Looking for device in ROM mode ...
25.09.2016 09:38:08	ROM v2 IC v3 detected
25.09.2016 09:38:08	Ready to download firmware
25.09.2016 09:38:24	
25.09.2016 09:38:24	Firmware download options:
25.09.2016 09:38:24	   File: W:\CCS\First Steps\UCD3138_lab_ClosedLoop_3Phase_unbalanced\Debug\UCD3138_Lab_ClosedLoop_3Phase_unbalanced.x0
25.09.2016 09:38:24	   Download program flash: Download
25.09.2016 09:38:24	   Download data flash: Download
25.09.2016 09:38:24	   Send to program mode when done: False
25.09.2016 09:38:24	
25.09.2016 09:38:24	Starting download ...
25.09.2016 09:38:24	Parsing firmware file ...
25.09.2016 09:38:24	Firmware is in Tektronix Extended format
25.09.2016 09:38:25	Mass erasing program flash
25.09.2016 09:38:25	Downloading program flash ...
25.09.2016 09:38:30	Mass erasing data flash
25.09.2016 09:38:30	Downloading data flash ...
25.09.2016 09:38:31	Verifying program flash ...
25.09.2016 09:38:31	Having ROM calculate checksum for program flash 0x10000 through 0x17FFB ...
25.09.2016 09:38:32	Program Flash checksum match between GUI calculation and Rom calculation (0x0067B676)
25.09.2016 09:38:32	Verifying data flash ...
25.09.2016 09:38:32	Reading data flash ...
25.09.2016 09:38:33	Data Flash verified!
25.09.2016 09:38:33	Download completed without error; 8,8 sec elapsed
25.09.2016 09:38:33	Sending ROM execute flash command (SendByte 0xF0 to address 11)
25.09.2016 09:38:33	Executing program ...
25.09.2016 09:38:35	Scanning for programs that respond to a DEVICE_ID read ...
25.09.2016 09:38:35	Looking for device in program mode ...
25.09.2016 09:38:36	Found DC-DC LLC Firmware v0.0.35.68 @ Address 88d in program mode
25.09.2016 09:38:36	Click a scan button to perform more programming ...

Flashing own board with same options than above:
Timestamp	Message
25.09.2016 09:40:09	USB Adapter v1.0.10 [PEC; 400 kHz] Found (Adapter #1)
25.09.2016 09:40:09	Looking for device in ROM mode ...
25.09.2016 09:40:09	ROM v2 IC v3 detected
25.09.2016 09:40:09	Ready to download firmware
25.09.2016 09:40:18	
25.09.2016 09:40:18	Firmware download options:
25.09.2016 09:40:18	   File: W:\CCS\First Steps\UCD3138_lab_ClosedLoop_3Phase_unbalanced\Debug\UCD3138_Lab_ClosedLoop_3Phase_unbalanced.x0
25.09.2016 09:40:18	   Download program flash: Download
25.09.2016 09:40:18	   Download data flash: Download
25.09.2016 09:40:18	   Send to program mode when done: False
25.09.2016 09:40:18	
25.09.2016 09:40:18	Starting download ...
25.09.2016 09:40:18	Parsing firmware file ...
25.09.2016 09:40:18	Firmware is in Tektronix Extended format
25.09.2016 09:40:19	Mass erasing program flash
25.09.2016 09:40:19	Downloading program flash ...
25.09.2016 09:40:25	Mass erasing data flash
25.09.2016 09:40:25	Downloading data flash ...
25.09.2016 09:40:25	Verifying program flash ...
25.09.2016 09:40:25	Having ROM calculate checksum for program flash 0x10000 through 0x17FFB ...
25.09.2016 09:40:26	Program Flash checksum match between GUI calculation and Rom calculation (0x0067B676)
25.09.2016 09:40:26	Verifying data flash ...
25.09.2016 09:40:26	Reading data flash ...
25.09.2016 09:40:27	Data Flash verified!
25.09.2016 09:40:27	Download completed without error; 9,0 sec elapsed
25.09.2016 09:40:27	Sending ROM execute flash command (SendByte 0xF0 to address 11)
25.09.2016 09:40:27	Executing program ...
25.09.2016 09:40:29	Scanning for programs that respond to a DEVICE_ID read ...
25.09.2016 09:40:29	Looking for device in program mode ...
25.09.2016 09:40:30	No PMBus devices responded to a DEVICE_ID request
25.09.2016 09:40:30	Checking if ROM is still present ...
25.09.2016 09:40:30	ROM v2 IC v3 detected
There is adifference, but for what reason?

Memory debugger after flashing on eval board:
Timestamp	Message
25.09.2016 09:44:09	0x0001904C: read  4 byte(s) 0x00000064

Memory debugger after flashing on own board:
Timestamp	Message
25.09.2016 09:46:19	0x0001904C: read  4 byte(s) 0xE12FFF1E

==> program not running, but why???????